-- *****************************************************************
-- CISCO-ENHANCED-SLB-MIB: Cisco Enhanced SLB MIB
--   
-- February 2006, Subra Hegde
--   
-- Copyright (c) 2006, 2008-2009, 2012 by cisco Systems Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-ENHANCED-SLB-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    NOTIFICATION-TYPE,
    OBJECT-TYPE,
    Unsigned32,
    Counter64,
    Counter32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    TEXTUAL-CONVENTION,
    DateAndTime,
    RowStatus,
    StorageType,
    TruthValue
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    InetAddressType,
    InetAddress,
    InetPortNumber
        FROM INET-ADDRESS-MIB
    SlbServerString,
    SlbRealServerState,
    slbEntity,
    slbServerFarmName
        FROM CISCO-SLB-MIB
    SlbUrlString
        FROM CISCO-SLB-EXT-MIB
    CiscoHTTPResponseStatusCode
        FROM CISCO-TC
    CiscoProbeHealthMonState,
    cslbxProbeName
        FROM CISCO-SLB-HEALTH-MON-MIB
    ciscoMgmt
        FROM CISCO-SMI;


ciscoEnhancedSlbMIB MODULE-IDENTITY
    LAST-UPDATED    "201212030000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W. Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-slb@cisco.com"
    DESCRIPTION
        "The MIB for managing Server Load Balancing
        Manager(s), and products supporting Server
        Load Balancing(SLB) features.

        This MIB extends the tables(as appropriate)
        that  are defined in CISCO-SLB-MIB  and 
        CISCO-SLB-EXT-MIB.
        Some of the functionalities supported are:  
           * Real Server Configuration with real server 
             identified by a name
           * Real Server configuration in a Server Farm.
           * Health Probe Configuration in a real server.
           * Sticky Configuration for HTTP Header, HTTP Cookie
             and Client IP Address, SSL(Secure Socket Layer).

        Acronyms and terminology:

        SLB       : Server Load Balancing
                    When a client initiates a connection to 
                    virtual server, the system load balances 
                    the connection to the chosen real server 
                    based on the user configuration.
                    SLB is important for Scaling of Web 
                    Services and for traditional serverices 
                    such as DNS, FTP etc.
        Server Farm    : Contains cluster of Real Server
        Virtual Server : Group of Real Servers
        RServer                   : RServers are physical devices that
                                         do not belong to any server farm.                  
        Real Server    : Real Servers are physical devices
                         assigned to a server farms.
                         Real  servers provide services that
                         are load balanced.
        Health Probe   : The mechanisms to monitor the health 
                         of real servers.
        sticky ConnectIons : Sticky connections limit traffic
                    to the individual real servers by allowing
                    multiple connections from the same client 
                    to stick (or attach) to the same real 
                    server using source IP addresses, 
                    source IP subnets, cookies, and the 
                    secure socket layer (SSL) or by 
                    redirecting these connections using 
                    Hypertext Transfer Protocol (HTTP)
                    redirect messages. Sticky connection
                    feature also permits coupling of the
                    services that are handled by more
                    than one virtual server.
        cookie : A cookie is a small data structure used by a 
                 server to deliver data to a Web client and 
                 request that the client store the information.
                 In certain applications, the client returns 
                 the information to the server to maintain 
                 the state between the client and the server.
        BuddyGroup : Contains buddy group name of real server."
    REVISION        "201212030000Z"
    DESCRIPTION
        "-Added SlbRserverLocalityState new TEXTUAL-CONVENTION.

        -Added cesRealServerGroupRev2 & cesRealServerNotifGroupRev3. 

        -Added ciscoEnhancedSlbMIBComplianceRev6. 

        -Deprecated ciscoEnhancedSlbMIBComplianceRev5."
    REVISION        "201204090000Z"
    DESCRIPTION
        "-Added the object cesServerFarmRserverBuddyGroup to
        cesServerFarmRserverTable.

        -Added cesRealServerFarmBuddyGroup OBJECT-GROUP.

        -Deprecated ciscoEnhancedSlbMIBComplianceRev4
        MODULE-COMPLIANCE.

        -Added ciscoEnhancedSlbMIBComplianceRev5 MODULE-COMPLIANCE 
        statement"
    REVISION        "200909190000Z"
    DESCRIPTION
        "-Added cesServerFarmRserverDescr to cesServerFarmRserverTable.

        -Deprecated cesRealServerStateUp NOTIFICATION-TYPE.

        -Deprecated cesRealServerStateDown NOTIFICATION-TYPE.

        -Deprecated cesRealServerStateChange NOTIFICATION-TYPE.

        -Added cesRealServerStateUpRev1 NOTIFICATION-TYPE.

        -Added cesRealServerStateDownRev1 NOTIFICATION-TYPE.

        -Added cesRealServerStateChangeRev1 NOTIFICATION-TYPE.

        -Deprecated cesRealServerFarmGroup OBJECT-GROUP.

        -Deprecated cesRealServerNotifGroupRev1 NOTIFICATION-GROUP.

        -Added cesRealServerFarmGroupRev1 OBJECT-GROUP.

        -Added cesRealServerNotifGroupRev2 NOTIFICATION-GROUP

        -Deprecated ciscoEnhancedSlbMIBComplianceRev3
        MODULE-COMPLIANCE.

        -Added ciscoEnhancedSlbMIBComplianceRev4 MODULE-COMPLIANCE."
    REVISION        "200805210000Z"
    DESCRIPTION
        "-Added the following objects to the cesRserverProbeTable
        cesRserverProbeLastProbeTime  
        cesRserverProbeLastActiveTime 
        cesRserverProbeLastFailedTime 

        -Deprecated cesRserverProbeGroup OBJECT-GROUP.

        -Deprecated ciscoEnhancedSlbMIBComplianceRev2 MODULE-COMPLIANCE
        statement.

        -Added cesRserverProbeGroupRev1 OBJECT-GROUP.

        -Added ciscoEnhancedSlbMIBComplianceRev3 MODULE-COMPLIANCE
        statement."
    REVISION        "200803120000Z"
    DESCRIPTION
        "-Added the following objects to the cesRserverTable
        cesRserverTotalConns
        cesRserverFailedConns
        cesRserverCurrConns

                -Added the following objects to the cesRserverProbeTable
        cesRserverProbesPassed
        cesRserverProbesFailed
        cesRserverHealthMonState

        -Added cesRealServerProbeTable

        -Deprecated cesRealServerGroup OBJECT-GROUP

        -Deprecated ciscoEnhancedSlbMIBComplianceRev1 MODULE-COMPLIANCE
        statement

        - Added the following OBJECT-GROUP's  
        cesRealServerGroupRev1
        cesRserverProbeGroup
        cesRealserverProbeGroup

        - Added ciscoEnhancedSlbMIBComplianceRev2 MODULE-COMPLIANCE
        statement"
    REVISION        "200603310000Z"
    DESCRIPTION
        "-Added the following Notifications:
        cesRserverStateUp
        cesRserverStateDown
        cesRserverStateChange.

        -Added OBJECT-GROUP cesRealServerNotifGroupRev1

        -Added MODULE-COMPLIANCE ciscoEnhancedSlbMIBComplianceRev1"
    REVISION        "200602270000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 470 }


ciscoEnhancedSlbMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoEnhancedSlbMIB 0 }

ciscoEnhancedSlbMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoEnhancedSlbMIB 1 }

ciscoEnhancedSlbMIBConformance  OBJECT IDENTIFIER
    ::= { ciscoEnhancedSlbMIB 2 }

cesRealServer  OBJECT IDENTIFIER
    ::= { ciscoEnhancedSlbMIBObjects 1 }

cesDfpAgent  OBJECT IDENTIFIER
    ::= { ciscoEnhancedSlbMIBObjects 2 }

cesStickyConfig  OBJECT IDENTIFIER
    ::= { ciscoEnhancedSlbMIBObjects 3 }

cesNotifControl  OBJECT IDENTIFIER
    ::= { ciscoEnhancedSlbMIBObjects 4 }

cesNotificationObjects  OBJECT IDENTIFIER
    ::= { ciscoEnhancedSlbMIBObjects 5 }


CiscoRserverAdminStatus ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This is the textual convention for
        administrative status of the real server.
        The possible value(s) are :
          'inService'        : Places the real server into service state.
          'outOfService'     : Places the real server out of service. 
          'inserviceStandby' : Places the real server into standby 
                               state."
    SYNTAX          INTEGER  {
                        inService(1),
                        outOfService(2),
                        inServiceStandby(3)
                    }

SlbRserverLocalityState ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This is the textual convention for
        locality status of the real server.
        The possible value(s) are :
          'unknown'        : The locality of the real server is not
        known.
          'local'          : The locality of the real server is local.
          'remote'         : The locality of the real server is remote.
                               state."
    SYNTAX          INTEGER  {
                        unknown(1),
                        local(2),
                        remote(3)
                    }
-- *************************************************************
-- *                                                           *
-- * SLB - Real Server(identified by Name) Table               *
-- *                                                           *
-- *************************************************************

cesRserverTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CesRserverEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table of real servers. A real server
        is identified by a name."
    ::= { cesRealServer 1 }

cesRserverEntry OBJECT-TYPE
    SYNTAX          CesRserverEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in real server table.
        Each entry refers to real server and contains
        real server IP Address, maximum connections supported,
        minimum connections supported, redirect code, 
        redirect port etc. The 'slbEntity' is used
        in identifying the module in which configuration 
        is applied."
    INDEX           {
                        slbEntity,
                        cesRserverName
                    } 
    ::= { cesRserverTable 1 }

CesRserverEntry ::= SEQUENCE {
        cesRserverName                  SnmpAdminString,
        cesRserverType                  INTEGER,
        cesRserverIpAddressType         InetAddressType,
        cesRserverIpAddress             InetAddress,
        cesRserverDescription           SnmpAdminString,
        cesRserverMaxConns              Unsigned32,
        cesRserverMinConns              Unsigned32,
        cesRserverAdminWeight           Unsigned32,
        cesRserverRedirectRelocationStr SlbUrlString,
        cesRserverRedirectCode          CiscoHTTPResponseStatusCode,
        cesRserverRedirectPort          InetPortNumber,
        cesRserverAdminStatus           CiscoRserverAdminStatus,
        cesRserverOperStatus            SlbRealServerState,
        cesRserverStatechangeDescr      SnmpAdminString,
        cesRserverStorageType           StorageType,
        cesRserverRowStatus             RowStatus,
        cesRserverTotalConns            Counter64,
        cesRserverFailedConns           Counter64,
        cesRserverCurrConns             Counter64,
        cesRserverLocality              SlbRserverLocalityState
}

cesRserverName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..255))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object identifies the name(unique identifier)
        of the real server." 
    ::= { cesRserverEntry 1 }

cesRserverType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        redirect(1),
                        host(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The type of the real server.
        The possible values are :
          redirect(1): Specifies that this real server is just used for
                       redirecting traffic to new virtual server 
                       equivalent pointed to by the redirection string
                       (cesRserverRedirectRelocationStr).
          host   (2): Specifies typical server offering services.

        The real server type redirect(1) implies that the following
        objects are applicable for a real server entry:
            cesRserverRedirectRelocationStr.
            cesRserverRedirectCode.
            cesRserverRedirectPort.
        This means that only the above objects will be
        used to create the real server entry, and all 
        other objects will be ignored during row creation.

        The real server type host(2) implies that the following
        objects are applicable for a real server entry:
            cesRserverIpAddressType
            cesRserverIpAddress
        This means that only the above objects will be
        used to create the real server entry, and all 
        other objects will be ignored during row creation.

        This object cannot be changed when the cesRserverRowStatus
        value is 'active'."
    DEFVAL          { host } 
    ::= { cesRserverEntry 2 }

cesRserverIpAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The type of the internet Address configured in
        'cesRserverIpAddress'.  This object is applicable 
        only for cesRserverType value 'host'." 
    ::= { cesRserverEntry 3 }

cesRserverIpAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the internet address of real server.
        This object is applicable only for cesRserverType value 'host'.
        This object contains zero length octet string
        for cesRserverType value other than 'host'."
    DEFVAL          { "" } 
    ::= { cesRserverEntry 4 }

cesRserverDescription OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used for configuring
        the description of the real server."
    DEFVAL          { "" } 
    ::= { cesRserverEntry 5 }

cesRserverMaxConns OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used for configuring the
        maximum number of concurrent active connections
        this real server can handle."
    DEFVAL          { 4294967295 } 
    ::= { cesRserverEntry 6 }

cesRserverMinConns OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used for configuring the minimum number
        of concurrent active connections this real server can handle.
        The value for this object must to be less than or equal
        to value specified in cesRserverMaxConns object."
    DEFVAL          { 4294967295 } 
    ::= { cesRserverEntry 7 }

cesRserverAdminWeight OBJECT-TYPE
    SYNTAX          Unsigned32 (0..65535)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The user configured weight of the real server for the
        load-balancing algorithms. This is applicable only
        in case of weighted Round Robin Predictor algorithms
        (SlbPredictor values: 'roundRobin', 'leastConns').

        A weight of zero indicates that no new connections will 
        be assigned to this real server.  
        Higher weight values indicate to the load-balancing algorithms 
        a higher availability of this real server to accept more work.

        This object is applicable only for cesRserverType value 'host'."
    DEFVAL          { 8 } 
    ::= { cesRserverEntry 8 }

cesRserverRedirectRelocationStr OBJECT-TYPE
    SYNTAX          SlbUrlString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The relocation URL string used for redirection.
        This value is sent in the reply of the Redirect Server.
        This object is applicable only for 
        cesRserverType value 'redirect'."
    DEFVAL          { "" } 
    ::= { cesRserverEntry 9 }

cesRserverRedirectCode OBJECT-TYPE
    SYNTAX          CiscoHTTPResponseStatusCode (300..399)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The HTTP response code sent in the reply by
        the redirect server.
        meaning of few Redirect Codes:
          301 : If page is permanently moved.
                The requested resource has been assigned a 
                new permanent URL.
          302 : The requested resource resides temporarily 
                under a different URL.
        This object is applicable only for 
        cesRserverType value 'redirect'."
    REFERENCE
        "RFC 2616 Section 6.1.1 Status Code and Reason Phrase.
         RFC 2616 Section 10.3 Redirection 3xxx."
    DEFVAL          { 302 } 
    ::= { cesRserverEntry 10 }

cesRserverRedirectPort OBJECT-TYPE
    SYNTAX          InetPortNumber
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The TCP or UDP port of redirect server.  This is used
        for redirecting the URL string identified by
        'cesRserverRedirectRelocationStr'.
        This object is applicable only for 
        cesRserverType = 'redirect'." 
    ::= { cesRserverEntry 11 }

cesRserverAdminStatus OBJECT-TYPE
    SYNTAX          CiscoRserverAdminStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is  used for setting the administrative
        status of the Real server.
        If set to 'inService', the real server
        is placed into service. If set to 'outOfService'
        the real server is taken out of service."
    DEFVAL          { outOfService } 
    ::= { cesRserverEntry 12 }

cesRserverOperStatus OBJECT-TYPE
    SYNTAX          SlbRealServerState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides the current state of the
        real server." 
    ::= { cesRserverEntry 13 }

cesRserverStatechangeDescr OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object contains the descriptive
        text qualifying the reason for the
        value in cesRserverOperStatus.

         Examples:
           ARP failure
           Health probe failed." 
    ::= { cesRserverEntry 14 }

cesRserverStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The storage type for this conceptual row."
    DEFVAL          { nonVolatile } 
    ::= { cesRserverEntry 15 }

cesRserverRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The object is used for adding/deleting entries in
        the table.

        An entry MUST NOT exist in the active state unless all
        objects in the entry have an appropriate value, as described
        in the description clause for each writeable object.

        This object may be modified if the associated
        instance of this object is equal to active(1),
        notInService(2), or notReady(3).  All other writeable objects
        may be modified if the associated instance of this object is
        equal to notInService(2) or notReady(3).

        This object may not be set to 'destroy' if the real server
        identified by cesRserverName is referenced and being used in 
        other tables." 
    ::= { cesRserverEntry 16 }

cesRserverTotalConns OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "connections"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of connections loadbalanced to
        this real server." 
    ::= { cesRserverEntry 17 }

cesRserverFailedConns OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "connections"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of failed attempts to establish a connection
        to the real server." 
    ::= { cesRserverEntry 18 }

cesRserverCurrConns OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "connections"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of active connections loadbalanced to
        this real server." 
    ::= { cesRserverEntry 19 }

cesRserverLocality OBJECT-TYPE
    SYNTAX          SlbRserverLocalityState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the current locality state of the
        real server."
    DEFVAL          { 1 } 
    ::= { cesRserverEntry 20 }
 

-- Probes configured in RServers.

cesRserverProbeTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CesRserverProbeEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The Rserver health probe table.
        This table contains list of health probes configured 
        in a Rserver."
    ::= { cesRealServer 2 }

cesRserverProbeEntry OBJECT-TYPE
    SYNTAX          CesRserverProbeEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in Rserver probe table.
        Each entry is for a health probe configured in a
        Rserver. There can be multiple health probes 
        configured in a Rserver. The 'slbEntity' is used
        in identifying the module in which configuration 
        is applied. The 'cesRserverName' identifies the 
        Rserver in which probe is configured."
    INDEX           {
                        slbEntity,
                        cesRserverName,
                        cesRserverProbeName
                    } 
    ::= { cesRserverProbeTable 1 }

CesRserverProbeEntry ::= SEQUENCE {
        cesRserverProbeName           SlbServerString,
        cesRserverProbeStorageType    StorageType,
        cesRserverProbeRowStatus      RowStatus,
        cesRserverProbesPassed        Counter32,
        cesRserverProbesFailed        Counter32,
        cesRserverProbeHealthMonState CiscoProbeHealthMonState,
        cesRserverProbeLastProbeTime  DateAndTime,
        cesRserverProbeLastActiveTime DateAndTime,
        cesRserverProbeLastFailedTime DateAndTime
}

cesRserverProbeName OBJECT-TYPE
    SYNTAX          SlbServerString
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The name of the health probe configured in a Rserver.
        This value must correspond to an entry in cslbxProbeCfgTable."
    REFERENCE
        "cslbxProbeCfgTable defined in CISCO-SLB-HEALTH-MON-MIB" 
    ::= { cesRserverProbeEntry 1 }

cesRserverProbeStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The storage type for this conceptual row."
    DEFVAL          { nonVolatile } 
    ::= { cesRserverProbeEntry 2 }

cesRserverProbeRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The object is used for adding/deleting entries from
        this table." 
    ::= { cesRserverProbeEntry 3 }

cesRserverProbesPassed OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object contains the number of probes
        passed for this Rserver. The probe is identified as pass 
        if the Rserver returns a valid response." 
    ::= { cesRserverProbeEntry 4 }

cesRserverProbesFailed OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object contains the number of probes
        failed for this Rserver. The probe is identified as failed 
        if the Rserver fails to provide a valid response for a 
        specified number of retries." 
    ::= { cesRserverProbeEntry 5 }

cesRserverProbeHealthMonState OBJECT-TYPE
    SYNTAX          CiscoProbeHealthMonState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object contains the health monitor state
        of the probe for this Rserver."
    DEFVAL          { init } 
    ::= { cesRserverProbeEntry 6 }

cesRserverProbeLastProbeTime OBJECT-TYPE
    SYNTAX          DateAndTime
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the date and time of the last probe." 
    ::= { cesRserverProbeEntry 7 }

cesRserverProbeLastActiveTime OBJECT-TYPE
    SYNTAX          DateAndTime
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the last date and time that the
        probe's state transitioned to 'active'" 
    ::= { cesRserverProbeEntry 8 }

cesRserverProbeLastFailedTime OBJECT-TYPE
    SYNTAX          DateAndTime
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the last date and time that the
        probe's state transitioned to 'failed'" 
    ::= { cesRserverProbeEntry 9 }
 

-- Real Server configuration in a Server Farm

cesServerFarmRserverTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CesServerFarmRserverEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table of real servers configured in a server farm.
        This table is used for configuring real server
        (cesRserverName) in a server farm(slbServerFarmName)
        and configuring attributes of real server specific to 
        a server farm.  The real server identified by 
        'cesRserverName' should have been configured prior to 
        creating of an entry in this table.  The probes
        configured for the real server identifeid by
        'cesRserverName' will be inherited by the server farm."
    ::= { cesRealServer 3 }

cesServerFarmRserverEntry OBJECT-TYPE
    SYNTAX          CesServerFarmRserverEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Information about a real server in a system.
        Each entry refers to real server and contains
        information such as real server IP Address,
        maximum connections supported, minimum connections
        supported etc.
        The 'slbEntity' refers to the module in which this 
        configuration is applied.  The 'cesRserverName' refers 
        to the Real Server.  The 'slbServerFarmName' refers to 
        the Server Farm."
    INDEX           {
                        slbEntity,
                        slbServerFarmName,
                        cesRserverName,
                        cesServerFarmRserverPort
                    } 
    ::= { cesServerFarmRserverTable 1 }

CesServerFarmRserverEntry ::= SEQUENCE {
        cesServerFarmRserverPort         InetPortNumber,
        cesServerFarmRserverAdminWeight  Unsigned32,
        cesServerFarmRserverOperWeight   Unsigned32,
        cesServerFarmRserverMaxConns     Unsigned32,
        cesServerFarmRserverMinConns     Unsigned32,
        cesServerFarmRserverAdminStatus  CiscoRserverAdminStatus,
        cesServerFarmRserverOperStatus   SlbRealServerState,
        cesServerFarmRserverStateDescr   SnmpAdminString,
        cesServerFarmRserverBackupName   SnmpAdminString,
        cesServerFarmRserverBackupPort   InetPortNumber,
        cesServerFarmRserverTotalConns   Counter64,
        cesServerFarmRserverFailedConns  Counter64,
        cesServerFarmRserverDroppedConns Counter64,
        cesServerFarmRserverCurrentConns Counter64,
        cesServerFarmRserverStorageType  StorageType,
        cesServerFarmRserverRowStatus    RowStatus,
        cesServerFarmRserverDescr        SnmpAdminString,
        cesServerFarmRserverBuddyGroup   SnmpAdminString
}

cesServerFarmRserverPort OBJECT-TYPE
    SYNTAX          InetPortNumber
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The port  number of the real server.
        The value zero specifies that 
        port number is not used in conjunction
        with real server IP Address." 
    ::= { cesServerFarmRserverEntry 1 }

cesServerFarmRserverAdminWeight OBJECT-TYPE
    SYNTAX          Unsigned32 (0..65535)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies user configured weight of
        the real server under the serverfarm  for the 
        load-balancing algorithms. 

        If value is not specified, then the value
        specified in the object cesRserverAdminWeight is used." 
    ::= { cesServerFarmRserverEntry 2 }

cesServerFarmRserverOperWeight OBJECT-TYPE
    SYNTAX          Unsigned32 (0..65535)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The actual operating weight of the real server used
        by the load-balancing algorithms.  This can be adjusted
        dynamically by DFP/SASP.  A weight of zero indicates that no
        new connections will be assigned to this real server.
        Higher weight values indicate to the load-balancing
        algorithms availability of this real server to
        accept more work." 
    ::= { cesServerFarmRserverEntry 3 }

cesServerFarmRserverMaxConns OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specfies the maximum number of
        connections that can be supported by the 
        real server.

        If value is not specified, then the value
        specified in the object cesRserverMaxConns is used." 
    ::= { cesServerFarmRserverEntry 4 }

cesServerFarmRserverMinConns OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the minimum number of
        connections that needs to be supported by the 
        real server.  The value of this object must be 
        less than or equal to value specified in 
        cesServerFarmRserverMaxConns object.
        The value in this object is relevant only if 
        the cesServerFarmMaxConns object is configured.

        If value is not specified, then the value
        specified in the object cesRserverMinConns is used." 
    ::= { cesServerFarmRserverEntry 5 }

cesServerFarmRserverAdminStatus OBJECT-TYPE
    SYNTAX          CiscoRserverAdminStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is  used for setting the administrative status
        of the Real server a server farm." 
    ::= { cesServerFarmRserverEntry 6 }

cesServerFarmRserverOperStatus OBJECT-TYPE
    SYNTAX          SlbRealServerState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides the current state of the
        real server in a server farm." 
    ::= { cesServerFarmRserverEntry 7 }

cesServerFarmRserverStateDescr OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object contains the descriptive
        text qualifying the reason for the
        value in cesServerFarmRserverOperStatus.

         Examples:
           ARP failure
           Health probe failed." 
    ::= { cesServerFarmRserverEntry 8 }

cesServerFarmRserverBackupName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the backup real server.
        The value of this object cannot be same as
        the value specified in the INDEX cesRserverName.
        This value must correspond to an entry in cesRserverTable.
        The zero length value is not considered as a valid
        real server name."
    DEFVAL          { "" } 
    ::= { cesServerFarmRserverEntry 9 }

cesServerFarmRserverBackupPort OBJECT-TYPE
    SYNTAX          InetPortNumber
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the port number of the backup real server
        configured in 'cesServerFarmRserverBackupName'.
        This object can be configured only if the value
        specified in cesServerFarmRserverBackupName is valid.
        The value of this object is of signficance for the valid
        value of cesServerFarmRserverBackupName."
    DEFVAL          { 0 } 
    ::= { cesServerFarmRserverEntry 10 }

cesServerFarmRserverTotalConns OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of connections loadbalanced to
        this real server." 
    ::= { cesServerFarmRserverEntry 11 }

cesServerFarmRserverFailedConns OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of failed connections after which the real
        server goes to Failed state.  A failed connection is
        when a SYN timeouts or a RST is received from the
        real server." 
    ::= { cesServerFarmRserverEntry 12 }

cesServerFarmRserverDroppedConns OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of connections that were not
        connected to this server due to the current 
        connection count being at the max number of allowed 
        connections(cevServerFarmRserverMaxConns value) to 
        this real server." 
    ::= { cesServerFarmRserverEntry 13 }

cesServerFarmRserverCurrentConns OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of connections currently assigned
        to this real server.  This object represents the
        connections that are still active." 
    ::= { cesServerFarmRserverEntry 14 }

cesServerFarmRserverStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The storage type for this conceptual row."
    DEFVAL          { nonVolatile } 
    ::= { cesServerFarmRserverEntry 15 }

cesServerFarmRserverRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used for adding/deleting
        entries in the table." 
    ::= { cesServerFarmRserverEntry 16 }

cesServerFarmRserverDescr OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object contains the descriptive text
        qualifying the real server." 
    ::= { cesServerFarmRserverEntry 17 }

cesServerFarmRserverBuddyGroup OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object contains the buddy group
        of the real server." 
    ::= { cesServerFarmRserverEntry 18 }
 

-- Probes configured in Real Servers.

cesRealServerProbeTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CesRealServerProbeEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The real server health probe table.
        This table can be used for configuring probes 
        in a real server."
    ::= { cesRealServer 4 }

cesRealServerProbeEntry OBJECT-TYPE
    SYNTAX          CesRealServerProbeEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in real server probe table.
        An entry in the table is created when a probe is
        associated with a real server. An entry is deleted when a 
        probe is dissociated with a real server.
        The 'slbEntity' is used in identifying the module 
        in which configuration is applied. 
        The 'cesRserverName' identifies the real server to which 
        probe is configured. The 'cslbxProbeName' represents
        the probe associated with the real server. The 
        'cesServerFarmRserverPort' represents the port of the 
        real server through which it is attached to the server farm."
    INDEX           {
                        slbEntity,
                        cslbxProbeName,
                        slbServerFarmName,
                        cesRserverName,
                        cesServerFarmRserverPort
                    } 
    ::= { cesRealServerProbeTable 1 }

CesRealServerProbeEntry ::= SEQUENCE {
        cesRealServerProbeStorageType StorageType,
        cesRealServerProbeRowStatus   RowStatus
}

cesRealServerProbeStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The storage type for this conceptual row."
    DEFVAL          { nonVolatile } 
    ::= { cesRealServerProbeEntry 1 }

cesRealServerProbeRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The object is used for adding/deleting entries from
        this table." 
    ::= { cesRealServerProbeEntry 2 }
 


-- Notification related objects

cesRealServerNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object is used for enabling/disabling
        notifications related to real servers." 
    ::= { cesNotifControl 1 }

cesRealServerName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object identifies the real server name
        that are sent in notifications.  This object
        contains the value of object cesRserverName.
        This object is set to zero length octet string 
        value if the real server name is not available
        or applicable." 
    ::= { cesNotificationObjects 1 }

cesProbeName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object identifies the probe name
        that are sent in notification.  This
        object must correspond to an entry in
        cslbxProbeCfgTable.  This object is set to
        zero length octet string value if the probe
        is not available/applicable." 
    ::= { cesNotificationObjects 2 }

cesServerFarmName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object identifies the server farm name
        that are sent in notifications.  This object
        contains the value of object slbServerFarmName.
        This object is set to zero length octet string 
        value if the server farm name is not available
        or applicable." 
    ::= { cesNotificationObjects 3 }

-- Notifications

cesRealServerStateUp NOTIFICATION-TYPE
    OBJECTS         {
                        cesRealServerName,
                        cesServerFarmRserverBackupPort,
                        cesServerFarmName,
                        cesServerFarmRserverAdminStatus,
                        cesServerFarmRserverOperStatus,
                        cesRserverIpAddressType,
                        cesRserverIpAddress
                    }
    STATUS          deprecated
    DESCRIPTION
        "This notification is generated when a real server
        changes to 'inservice' state by the user intervention.

        The cesServerFarmName refers to the server farm
        to which the real server identified by the 
        cesRealServerName is associated.

        The cesServerFarmRserverBackupPort refers to the
        real server port.  This object contains the value
        of cesServerFarmRserverPort.
        cesRealServerStateUp object is superseded by cesRealServerStateUpRev1."
   ::= { ciscoEnhancedSlbMIBNotifs 1 }

cesRealServerStateDown NOTIFICATION-TYPE
    OBJECTS         {
                        cesRealServerName,
                        cesServerFarmRserverBackupPort,
                        cesServerFarmName,
                        cesServerFarmRserverAdminStatus,
                        cesServerFarmRserverOperStatus,
                        cesServerFarmRserverStateDescr,
                        cesRserverIpAddressType,
                        cesRserverIpAddress
                    }
    STATUS          deprecated
    DESCRIPTION
        "This notification is generated when a real server
        changes to 'outOfService' state by the user intervention.

        The cesServerFarmName refers to the server farm
        to which the real server identified by the 
        cesRealServerName is associated.

        The cesServerFarmRserverBackupPort refers to the
        real server port.  This object contains the value
        of cesServerFarmRserverPort.
        cesRealServerStateDown object is superseded by cesRealServerStateDownRev1."
   ::= { ciscoEnhancedSlbMIBNotifs 2 }

cesRealServerStateChange NOTIFICATION-TYPE
    OBJECTS         {
                        cesRealServerName,
                        cesServerFarmRserverBackupPort,
                        cesServerFarmName,
                        cesServerFarmRserverAdminStatus,
                        cesServerFarmRserverOperStatus,
                        cesServerFarmRserverStateDescr,
                        cesRserverIpAddressType,
                        cesRserverIpAddress,
                        cesProbeName
                    }
    STATUS          deprecated
    DESCRIPTION
        "This notification generated when a real server
        changes to a new state other than that is initiated
        by the user.  This notification is sent for the 
        reasons that are specified in objects:
           cesServerFarmRserverOperStatus 
           cesRserverStatechangeDescr.

        The cesServerFarmName refers to the server farm
        to which the real server identified by the 
        cesRealServerName is associated.

        The cesServerFarmRserverBackupPort refers to the
        real server port.  This object contains the value
        of cesServerFarmRserverPort.

        The cesProbeName object with zero length
        octet string specifies that real server state
        change is not due to probe failure.
        cesRealServerStateChange object is superseded by cesRealServerStateChangeRev1."
   ::= { ciscoEnhancedSlbMIBNotifs 3 }

cesRserverStateUp NOTIFICATION-TYPE
    OBJECTS         {
                        cesRealServerName,
                        cesRserverAdminStatus,
                        cesRserverOperStatus,
                        cesRserverIpAddressType,
                        cesRserverIpAddress
                    }
    STATUS          current
    DESCRIPTION
        "This notification is generated when the real server
        identified in cesRserverTable changes state to 
        'inservice' by the user intervention."
   ::= { ciscoEnhancedSlbMIBNotifs 4 }

cesRserverStateDown NOTIFICATION-TYPE
    OBJECTS         {
                        cesRealServerName,
                        cesRserverAdminStatus,
                        cesRserverOperStatus,
                        cesRserverIpAddressType,
                        cesRserverIpAddress
                    }
    STATUS          current
    DESCRIPTION
        "This notification is generated when the real server
        identified in cesRserverTable changes to 
        'outOfService' state by the user intervention."
   ::= { ciscoEnhancedSlbMIBNotifs 5 }

cesRserverStateChange NOTIFICATION-TYPE
    OBJECTS         {
                        cesRealServerName,
                        cesRserverAdminStatus,
                        cesRserverOperStatus,
                        cesRserverStatechangeDescr,
                        cesRserverIpAddressType,
                        cesRserverIpAddress,
                        cesProbeName
                    }
    STATUS          current
    DESCRIPTION
        "This notification generated when the real server
        identified in cesRserverTable changes to a new 
        state other than that is initiated by the user.  
        This notification is sent for the reasons that 
        are specified in objects:
           cesRserverOperStatus 
           cesRserverStatechangeDescr.

        The cesProbeName object with zero length
        octet string specifies that real server state
        change is not due to probe failure."
   ::= { ciscoEnhancedSlbMIBNotifs 6 }

cesRealServerStateUpRev1 NOTIFICATION-TYPE
    OBJECTS         {
                        cesRealServerName,
                        cesServerFarmRserverBackupPort,
                        cesServerFarmName,
                        cesServerFarmRserverAdminStatus,
                        cesServerFarmRserverOperStatus,
                        cesRserverIpAddressType,
                        cesRserverIpAddress,
                        cesServerFarmRserverDescr
                    }
    STATUS          current
    DESCRIPTION
        "This notification is generated when a real server
        changes to 'inservice' state by the user intervention.

        The cesServerFarmName refers to the server farm
        to which the real server identified by the 
        cesRealServerName is associated.

        The cesServerFarmRserverBackupPort refers to the
        real server port. This object contains the value
        of cesServerFarmRserverPort.

        The cesServerFarmRserverAdminStatus refers to the
        administrative state of the real server.

        The cesServerFarmRserverOperStatus refers to the 
        current state of the real server.

        The cesRserverIpAddress refers to the internet
        address of the real server.

        The cesRserverIpAddressType refers to the type of
        internet address in cesRserverIpAddress.

        The cesServerFarmRserverDescr refers to the
        description configured for the real server."
   ::= { ciscoEnhancedSlbMIBNotifs 7 }

cesRealServerStateDownRev1 NOTIFICATION-TYPE
    OBJECTS         {
                        cesRealServerName,
                        cesServerFarmRserverBackupPort,
                        cesServerFarmName,
                        cesServerFarmRserverAdminStatus,
                        cesServerFarmRserverOperStatus,
                        cesServerFarmRserverStateDescr,
                        cesRserverIpAddressType,
                        cesRserverIpAddress,
                        cesServerFarmRserverDescr
                    }
    STATUS          current
    DESCRIPTION
        "This notification is generated when a real server
        changes to 'outOfService' state by the user intervention.

        The cesServerFarmName refers to the server farm
        to which the real server identified by the 
        cesRealServerName is associated.

        The cesServerFarmRserverBackupPort refers to the
        real server port. This object contains the value
        of cesServerFarmRserverPort.

        The cesServerFarmRserverAdminStatus refers to the
        administrative state of the real server.

        The cesServerFarmRserverOperStatus refers to the 
        current state of the real server.

        The cesRserverIpAddress refers to the internet
        address of the real server.

        The cesRserverIpAddressType refers to the type of
        internet address in cesRserverIpAddress.

        The cesServerFarmRserverDescr refers to the
        description configured for the real server."
   ::= { ciscoEnhancedSlbMIBNotifs 8 }

cesRealServerStateChangeRev1 NOTIFICATION-TYPE
    OBJECTS         {
                        cesRealServerName,
                        cesServerFarmRserverBackupPort,
                        cesServerFarmName,
                        cesServerFarmRserverAdminStatus,
                        cesServerFarmRserverOperStatus,
                        cesServerFarmRserverStateDescr,
                        cesRserverIpAddressType,
                        cesRserverIpAddress,
                        cesProbeName,
                        cesServerFarmRserverDescr
                    }
    STATUS          current
    DESCRIPTION
        "This notification is generated when a real server
        changes to a new state other than that is initiated
        by the user.  This notification is sent for the 
        reasons that are specified in objects:
                   cesServerFarmRserverOperStatus 
                   cesRserverStatechangeDescr.

        The cesServerFarmName refers to the server farm
        to which the real server identified by the 
        cesRealServerName is associated.

        The cesServerFarmRserverBackupPort refers to the
        real server port. This object contains the value
        of cesServerFarmRserverPort.

        The cesServerFarmRserverAdminStatus refers to the
        administrative state of the real server.

        The cesRserverIpAddress refers to the internet
        address of the real server.

        The cesRserverIpAddressType refers to the type of
        internet address in cesRserverIpAddress.

        The cesProbeName object with zero length
        octet string specifies that real server state
        change is not due to probe failure.

        The cesServerFarmRserverDescr refers to the
        description configured for the real server."
   ::= { ciscoEnhancedSlbMIBNotifs 9 }

cesRserverLocalityChange NOTIFICATION-TYPE
    OBJECTS         { cesRserverLocality }
    STATUS          current
    DESCRIPTION
        "This notification is generated when the system detects the
        change of cesRserverLocality object value."
   ::= { ciscoEnhancedSlbMIBNotifs 10 }
-- Conformance Information

ciscoEnhancedSlbMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoEnhancedSlbMIBConformance 1 }

ciscoEnhancedSlbMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoEnhancedSlbMIBConformance 2 }


-- Compliance

ciscoEnhancedSlbMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which implement
        the Cisco Enhanced SLB MIB"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cesRealServerGroup,
                        cesRealServerFarmGroup
                    }

    GROUP           cesNotificationObjectGroup
    DESCRIPTION
        "This group is mandatory for those systems
        which support real server notifications."

    GROUP           cesRealServerNotifGroup
    DESCRIPTION
        "This group is mandatory for those systems
        which support real server notifications."
    ::= { ciscoEnhancedSlbMIBCompliances 1 }

ciscoEnhancedSlbMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which implement
        the Cisco Enhanced SLB MIB"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cesRealServerGroup,
                        cesRealServerFarmGroup
                    }

    GROUP           cesNotificationObjectGroup
    DESCRIPTION
        "This group is mandatory for those systems
        which support Enabling/disabling of notifications."

    GROUP           cesRealServerNotifGroupRev1
    DESCRIPTION
        "This group is mandatory for those systems
        which support real server notifications."
    ::= { ciscoEnhancedSlbMIBCompliances 2 }

ciscoEnhancedSlbMIBComplianceRev2 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which implement
        the Cisco Enhanced SLB MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cesRealServerFarmGroup,
                        cesRealServerGroupRev1,
                        cesRserverProbeGroup,
                        cesRealserverProbeGroup
                    }

    GROUP           cesNotificationObjectGroup
    DESCRIPTION
        "This group is mandatory for those systems
        which support Enabling/disabling of notifications."

    GROUP           cesRealServerNotifGroupRev1
    DESCRIPTION
        "This group is mandatory for those systems
        which support real server notifications."
    ::= { ciscoEnhancedSlbMIBCompliances 3 }

ciscoEnhancedSlbMIBComplianceRev3 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which implement
        the Cisco Enhanced SLB MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cesRealServerFarmGroup,
                        cesRealServerGroupRev1,
                        cesRserverProbeGroupRev1,
                        cesRealserverProbeGroup
                    }

    GROUP           cesNotificationObjectGroup
    DESCRIPTION
        "This group is mandatory for those systems
        which support Enabling/disabling of notifications."

    GROUP           cesRealServerNotifGroupRev1
    DESCRIPTION
        "This group is mandatory for those systems
        which support real server notifications."
    ::= { ciscoEnhancedSlbMIBCompliances 4 }

ciscoEnhancedSlbMIBComplianceRev4 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which implement the Cisco
        Enhanced SLB MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cesRealServerFarmGroupRev1,
                        cesRealServerGroupRev1,
                        cesRserverProbeGroupRev1,
                        cesRealserverProbeGroup
                    }

    GROUP           cesNotificationObjectGroup
    DESCRIPTION
        "This group is mandatory for those systems which support
        enabling/disabling of notifications."

    GROUP           cesRealServerNotifGroupRev2
    DESCRIPTION
        "This group is mandatory for those systems which supports
        real server notifications."
    ::= { ciscoEnhancedSlbMIBCompliances 5 }

ciscoEnhancedSlbMIBComplianceRev5 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which implement the Cisco
        Enhanced SLB MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cesRealServerFarmGroupRev1,
                        cesRealServerGroupRev1,
                        cesRserverProbeGroupRev1,
                        cesRealserverProbeGroup,
                        cesRealServerFarmBuddyGroup
                    }

    GROUP           cesNotificationObjectGroup
    DESCRIPTION
        "This group is mandatory for those systems which support
        enabling/disabling of notifications."

    GROUP           cesRealServerNotifGroupRev2
    DESCRIPTION
        "This group is mandatory for those systems which supports
        real server notifications."
    ::= { ciscoEnhancedSlbMIBCompliances 6 }

ciscoEnhancedSlbMIBComplianceRev6 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for entities which implement the Cisco
        Enhanced SLB MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cesRealServerFarmGroupRev1,
                        cesRealServerGroupRev2,
                        cesRserverProbeGroupRev1,
                        cesRealserverProbeGroup,
                        cesRealServerFarmBuddyGroup
                    }

    GROUP           cesNotificationObjectGroup
    DESCRIPTION
        "This group is mandatory for those systems which support
        enabling/disabling of notifications."

    GROUP           cesRealServerNotifGroupRev3
    DESCRIPTION
        "This group is mandatory for those systems which supports
        real server notifications."
    ::= { ciscoEnhancedSlbMIBCompliances 7 }

-- Units of Conformance

cesRealServerGroup OBJECT-GROUP
    OBJECTS         {
                        cesRealServerName,
                        cesRserverType,
                        cesRserverIpAddressType,
                        cesRserverIpAddress,
                        cesRserverDescription,
                        cesRserverMaxConns,
                        cesRserverMinConns,
                        cesRserverAdminWeight,
                        cesRserverRedirectRelocationStr,
                        cesRserverRedirectPort,
                        cesRserverRedirectCode,
                        cesRserverAdminStatus,
                        cesRserverOperStatus,
                        cesRserverStatechangeDescr,
                        cesRserverStorageType,
                        cesRserverRowStatus,
                        cesRserverProbeStorageType,
                        cesRserverProbeRowStatus
                    }
    STATUS          deprecated
    DESCRIPTION
        "This group contains objects applicable for
        Rserver configuration.
        cesRealServerGroup object is superseded by cesRealServerGroupRev1."
    ::= { ciscoEnhancedSlbMIBGroups 1 }

cesRealServerFarmGroup OBJECT-GROUP
    OBJECTS         {
                        cesServerFarmRserverAdminWeight,
                        cesServerFarmRserverOperWeight,
                        cesServerFarmRserverMaxConns,
                        cesServerFarmRserverMinConns,
                        cesServerFarmRserverAdminStatus,
                        cesServerFarmRserverOperStatus,
                        cesServerFarmRserverStateDescr,
                        cesServerFarmRserverBackupName,
                        cesServerFarmRserverBackupPort,
                        cesServerFarmRserverTotalConns,
                        cesServerFarmRserverFailedConns,
                        cesServerFarmRserverDroppedConns,
                        cesServerFarmRserverCurrentConns,
                        cesServerFarmRserverStorageType,
                        cesServerFarmRserverRowStatus
                    }
    STATUS          deprecated
    DESCRIPTION
        "The group contains obbjects for
        real server configuration in a server farm.
        cesRealServerFarmGroup object is superseded by cesRealServerFarmGroup2."
    ::= { ciscoEnhancedSlbMIBGroups 3 }

cesNotificationObjectGroup OBJECT-GROUP
    OBJECTS         {
                        cesRealServerName,
                        cesServerFarmName,
                        cesProbeName,
                        cesRealServerNotifEnable
                    }
    STATUS          current
    DESCRIPTION
        "This group contains objects related to
        notification."
    ::= { ciscoEnhancedSlbMIBGroups 9 }

cesRealServerNotifGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        cesRealServerStateUp,
                        cesRealServerStateDown,
                        cesRealServerStateChange
                    }
    STATUS          deprecated
    DESCRIPTION
        "This group contains real server Notifications.
        cesRealServerNotifGroup object is superseded by cesRealServerNotifGroupRev1."
    ::= { ciscoEnhancedSlbMIBGroups 10 }

cesRealServerNotifGroupRev1 NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        cesRealServerStateUp,
                        cesRealServerStateDown,
                        cesRealServerStateChange,
                        cesRserverStateUp,
                        cesRserverStateDown,
                        cesRserverStateChange
                    }
    STATUS          current
    DESCRIPTION
        "This group contains real server Notifications.
        cesRealServerNotifGroupRev1 object is superseded by cesRealServerNotifGroupRev2."
    ::= { ciscoEnhancedSlbMIBGroups 11 }

cesRealServerGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        cesRealServerName,
                        cesRserverType,
                        cesRserverIpAddressType,
                        cesRserverIpAddress,
                        cesRserverDescription,
                        cesRserverMaxConns,
                        cesRserverMinConns,
                        cesRserverAdminWeight,
                        cesRserverRedirectRelocationStr,
                        cesRserverRedirectCode,
                        cesRserverRedirectPort,
                        cesRserverAdminStatus,
                        cesRserverOperStatus,
                        cesRserverStatechangeDescr,
                        cesRserverStorageType,
                        cesRserverRowStatus,
                        cesRserverTotalConns,
                        cesRserverFailedConns,
                        cesRserverCurrConns
                    }
    STATUS          current
    DESCRIPTION
        "This group contains objects applicable for
        Rserver configuration.
        cesRealServerGroupRev1 object is superseded by NA."
    ::= { ciscoEnhancedSlbMIBGroups 12 }

cesRserverProbeGroup OBJECT-GROUP
    OBJECTS         {
                        cesRserverProbeStorageType,
                        cesRserverProbeRowStatus,
                        cesRserverProbesPassed,
                        cesRserverProbesFailed,
                        cesRserverProbeHealthMonState
                    }
    STATUS          deprecated
    DESCRIPTION
        "This group contains objects applicable for
        Rserver probe configuration and Rserver probe statistics.
        cesRserverProbeGroup object is superseded by NA."
    ::= { ciscoEnhancedSlbMIBGroups 13 }

cesRealserverProbeGroup OBJECT-GROUP
    OBJECTS         {
                        cesRealServerProbeStorageType,
                        cesRealServerProbeRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "This group contains objects applicable for
        real server probe configuration."
    ::= { ciscoEnhancedSlbMIBGroups 14 }

cesRserverProbeGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        cesRserverProbeStorageType,
                        cesRserverProbeRowStatus,
                        cesRserverProbesPassed,
                        cesRserverProbesFailed,
                        cesRserverProbeHealthMonState,
                        cesRserverProbeLastProbeTime,
                        cesRserverProbeLastActiveTime,
                        cesRserverProbeLastFailedTime
                    }
    STATUS          current
    DESCRIPTION
        "This group contains objects applicable for
        Rserver probe configuration and Rserver probe statistics."
    ::= { ciscoEnhancedSlbMIBGroups 15 }

cesRealServerFarmGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        cesServerFarmRserverAdminWeight,
                        cesServerFarmRserverOperWeight,
                        cesServerFarmRserverMaxConns,
                        cesServerFarmRserverMinConns,
                        cesServerFarmRserverAdminStatus,
                        cesServerFarmRserverOperStatus,
                        cesServerFarmRserverStateDescr,
                        cesServerFarmRserverBackupName,
                        cesServerFarmRserverBackupPort,
                        cesServerFarmRserverTotalConns,
                        cesServerFarmRserverFailedConns,
                        cesServerFarmRserverDroppedConns,
                        cesServerFarmRserverCurrentConns,
                        cesServerFarmRserverStorageType,
                        cesServerFarmRserverRowStatus,
                        cesServerFarmRserverDescr
                    }
    STATUS          deprecated
    DESCRIPTION
        "The group contains objects for real server configuration in a
        server farm.
        cesRealServerFarmGroupRev1 object is superseded by NA."
    ::= { ciscoEnhancedSlbMIBGroups 19 }

cesRealServerNotifGroupRev2 NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        cesRealServerStateUpRev1,
                        cesRealServerStateDownRev1,
                        cesRealServerStateChangeRev1,
                        cesRserverStateUp,
                        cesRserverStateDown,
                        cesRserverStateChange
                    }
    STATUS          current
    DESCRIPTION
        "This group contains real server Notifications.
        cesRealServerNotifGroupRev2 object is superseded by NA."
    ::= { ciscoEnhancedSlbMIBGroups 21 }

cesRealServerFarmBuddyGroup OBJECT-GROUP
    OBJECTS         { cesServerFarmRserverBuddyGroup }
    STATUS          current
    DESCRIPTION
        "The group contains objects for buddy group configuration of
        real server in a server farm."
    ::= { ciscoEnhancedSlbMIBGroups 22 }

cesRealServerGroupRev2 OBJECT-GROUP
    OBJECTS         { cesRserverLocality }
    STATUS          current
    DESCRIPTION
        "This group contains object indicates the current locality state
        of the real server."
    ::= { ciscoEnhancedSlbMIBGroups 23 }

cesRealServerNotifGroupRev3 NOTIFICATION-GROUP
   NOTIFICATIONS    { cesRserverLocalityChange }
    STATUS          current
    DESCRIPTION
        "This group contain real server Locality state change
        Notification."
    ::= { ciscoEnhancedSlbMIBGroups 24 }

END
































































































































































































































