-- *****************************************************************
-- CISCO-TRUSTSEC-SXP-MIB.my
--   
-- February 2010, Dipesh Gorashia
--   
-- Copyright (c) 2010-2012 by Cisco Systems Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-TRUSTSEC-SXP-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Unsigned32,
    Gauge32,
    NOTIFICATION-TYPE
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    RowStatus,
    StorageType,
    TruthValue
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    InetAddressType,
    InetAddress,
    InetAddressPrefixLength
        FROM INET-ADDRESS-MIB
    InterfaceIndexOrZero
        FROM IF-MIB
    CtsSecurityGroupTag,
    CtsPasswordEncryptionType,
    CtsPassword
        FROM CISCO-TRUSTSEC-TC-MIB
    CiscoVrfName
        FROM CISCO-TC
    ciscoMgmt
        FROM CISCO-SMI;


ciscoTrustSecSxpMIB MODULE-IDENTITY
    LAST-UPDATED    "201204170000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "This MIB module is for the configuration and status query
        of SGT Exchange Protocol over TCP (SXPoTCP) feature of the
        device on the Cisco's Trusted Security (TrustSec) system.

        Security Group Tag (SGT) identifying its source, assigned to a
        packet on ingress to a TrustSec cloud, and used to determine
        security and other policy to be applied to it along its path
        through the cloud.

        SXPoTCP protocol extends the original SGT Exchange Protocol
        (SXP) protocol to enable a much wider array of deployment
        scenarios.  This MIB uses the term SXP to refer to SXPoTCP.

        TrustSec secures a network fabric by authenticating and
        authorizing each device connecting to the network, allowing
        for the encryption, authentication and replay protection of data
        traffic on a hop by hop basis.  SXP allows the deployment
        of RBACL, a key component of the TrustSec architecture, in the
        absence of TrustSec capable hardware."
    REVISION        "201204170000Z"
    DESCRIPTION
        "Added following OBJECT-GROUP
        - ctsxSxpBindingLogGroup
        - ctsxSxpBindingNotifInfoGroup
        - ctsxSxpNotifErrMsgGroup
        - ctsxSxpNodeIdInfoGroup
        - ctsxSxpSgtMapGroup
        - ctsxNotifsControlGroup
        - ctsxNotifsGroup
        - ctsxSxpGlobalHoldTimeGroup
        - ctsxSxpConnHoldTimeGroup
        - ctsxSxpConnCapbilityGroup
        - ctsxSxpVersionSupportGroup
        - ctsxSgtMapPeerSeqGroup
        Added new compliance
        - ciscoTrustSecSxpMIBCompliance3.
        Added enumerations three(4) and four(5)
        for the object ctsxSxpConnVersion."
    REVISION        "201011240000Z"
    DESCRIPTION
        "Added ctsxSxpVersionGroup."
    REVISION        "201002030000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 720 }


ciscoTrustSecSxpMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoTrustSecSxpMIB 0 }

ciscoTrustSecSxpMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoTrustSecSxpMIB 1 }

ciscoTrustSecSxpMIBConform  OBJECT IDENTIFIER
    ::= { ciscoTrustSecSxpMIB 2 }

ctsxSxpGlobalObjects  OBJECT IDENTIFIER
    ::= { ciscoTrustSecSxpMIBObjects 1 }

ctsxSxpConnectionObjects  OBJECT IDENTIFIER
    ::= { ciscoTrustSecSxpMIBObjects 2 }

ctsxSxpSgtObjects  OBJECT IDENTIFIER
    ::= { ciscoTrustSecSxpMIBObjects 3 }

ciscoTrustSecSxpMIBNotifsControl  OBJECT IDENTIFIER
    ::= { ciscoTrustSecSxpMIBObjects 4 }

ciscoTrustSecSxpMIBNotifsOnlyInfo  OBJECT IDENTIFIER
    ::= { ciscoTrustSecSxpMIBObjects 5 }


-- Objects to manage SXP functionality of TrustSec

ctsxSxpEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies if the SXP (Security Group Tag Exchange
        Protocol) functionality is enabled on the device." 
    ::= { ctsxSxpGlobalObjects 1 }

ctsxSxpConfigDefaultPasswordType OBJECT-TYPE
    SYNTAX          CtsPasswordEncryptionType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the type of encryption used
        to configure ctsxSxpConfigDefaultPassword string.

        When read, this object will always return 'other'.

        Value of this object must be set in the same PDU as
        ctsxSxpConfigDefaultPassword.

        Value of this object must be specified as 'clearText',
        'typeSix' or 'typeSeven' to configure a non zero length
        password in ctsxSxpConfigDefaultPassword.

        Value for this object must be 'none' if 
        ctsxSxpConfigDefaultPassword is a zero length string." 
    ::= { ctsxSxpGlobalObjects 2 }

ctsxSxpConfigDefaultPassword OBJECT-TYPE
    SYNTAX          CtsPassword
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the default password for SXP
        connections.

        The type of encryption used to configure this password 
        is determined by ctsxSxpConfigDefaultPasswordType.

        When read, this object will always return a zero length
        string.

        The value of this object must be set in the same PDU as
        ctsxSxpConfigDefaultPasswordType.

        A non zero length password must be specified for this object
        if the value of ctsxSxpConfigDefaultPasswordType is other than
        'none' or 'other'.

        Value for this object must be a zero length string if the value
        of ctsxSxpConfigDefaultPasswordType is 'none'.

        The purpose of this object is to only allow configuration of
        the default password. The ctsxSxpViewDefaultPassword object is
        used to display the default password." 
    ::= { ctsxSxpGlobalObjects 3 }

ctsxSxpViewDefaultPasswordType OBJECT-TYPE
    SYNTAX          CtsPasswordEncryptionType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the type of encryption in use
        for ctsxSxpViewDefaultPassword." 
    ::= { ctsxSxpGlobalObjects 4 }

ctsxSxpViewDefaultPassword OBJECT-TYPE
    SYNTAX          CtsPassword
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the default password for SXP connections.

        The type of encryption used to display this password is 
        determined by the object ctsxSxpViewDefaultPasswordType.

        The purpose of this object is to only display the password.
        The ctsxSxpConfigDefaultPassword object is used to configure the
        password." 
    ::= { ctsxSxpGlobalObjects 5 }

ctsxSxpDefaultSourceAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The type of Internet address of the default source address
        for SXP connections." 
    ::= { ctsxSxpGlobalObjects 6 }

ctsxSxpDefaultSourceAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The Internet address to be used as default source address for
        SXP connections. The type of this address is determined by the
        ctsxSxpDefaultSourceAddrType object.

        This address will be used as source address for SXP connections
        that do not have specific source-IP address configured via
        ctsxSxpConnSourceAddr object." 
    ::= { ctsxSxpGlobalObjects 7 }

ctsxSxpRetryPeriod OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the amount of time after which the device
        will make the retry attempt for the SXP connections that are not
        setup successfully.

        A value of zero for this object indicates that the device will
        never try to establish connections that were not setup
        successfully." 
    ::= { ctsxSxpGlobalObjects 8 }

ctsxSxpReconPeriod OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the amount of time after which system
        will initiate removal of SGT mappings for a reconciled
        connection.

        A value of zero for this object indicates that SGT
        mappings for a reconciled connection will never be deleted." 
    ::= { ctsxSxpGlobalObjects 9 }

ctsxSxpBindingChangesLogEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies if the system will generate system
        logging messages for SXP binding changes.

        A value of 'false' will prevent system from generating 
        logging messages for SXP binding changes." 
    ::= { ctsxSxpGlobalObjects 10 }

ctsxSgtMapExpansionLimit OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the maximum number of SGT
        mapping entries that can be expanded on the system.

        Value of zero for this object indicates that SGT mapping
        expansion functionality is disabled." 
    ::= { ctsxSxpGlobalObjects 11 }

ctsxSgtMapExpansionCount OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of SGT mapping
        entries currently expanded on the system." 
    ::= { ctsxSxpGlobalObjects 12 }

ctsxSxpAdminNodeId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the administrative SXP node ID for
        this system.

        Setting this object to a non-zero value will clear the values
        in ctsxSxpNodeIdInterface and ctsxSxpNodeIdIpAddrType.

        This object can be set only if ctsxSxpEnable is 'false'." 
    ::= { ctsxSxpGlobalObjects 13 }

ctsxSxpNodeIdInterface OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the interface to be used to select
        SXP node ID.

        Setting this object to a non-zero value will clear the values
        in ctsxSxpAdminNodeId and ctsxSxpNodeIdIpAddrType.

        This object can be set only if ctsxSxpEnable is 'false'." 
    ::= { ctsxSxpGlobalObjects 14 }

ctsxSxpNodeIdIpAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the type of Internet address to be
        used to select the SXP node ID." 
    ::= { ctsxSxpGlobalObjects 15 }

ctsxSxpNodeIdIpAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the Internet address to be used to
        select the SXP node ID.

        The type of this address is determined by
        ctsxSxpOperNodeIdIpAddrType object.

        Setting this object to a non-zero length value will clear the
        values in ctsxSxpAdminNodeId and ctsxSxpNodeIdInterface.

        This object can be set only if ctsxSxpEnable is 'false'." 
    ::= { ctsxSxpGlobalObjects 16 }

ctsxSxpOperNodeId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the operational SXP node ID of
        the system." 
    ::= { ctsxSxpGlobalObjects 17 }

ctsxSxpSpeakerMinHoldTime OBJECT-TYPE
    SYNTAX          Unsigned32 (1..65534)
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the global minimum hold-time for SXP
        connections in 'speaker' mode." 
    ::= { ctsxSxpGlobalObjects 18 }

ctsxSxpListenerMinHoldTime OBJECT-TYPE
    SYNTAX          Unsigned32 (1..65534)
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the global minimum hold-time for
        SXP connections in 'listener' mode.

        Value of this object must be lesser than
        ctsxSxpListenerMaxHoldTime." 
    ::= { ctsxSxpGlobalObjects 19 }

ctsxSxpListenerMaxHoldTime OBJECT-TYPE
    SYNTAX          Unsigned32 (1..65534)
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the global maximum hold-time for
        SXP connections in 'listener' mode.

        Value of this object must be greater than
        ctsxSxpListenerMinHoldTime." 
    ::= { ctsxSxpGlobalObjects 20 }

ctsxSxpVersionSupport OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        one(2),
                        two(3),
                        three(4),
                        four(5)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The highest version of SXP protocol that this device supports.

        'unknown' - The SXP protocol version capability for the
                    device is unknown. 

        'one'     - The device supports SXP protocol up to version 1.

        'two'     - The device supports SXP protocol up to version 2.

        'three'   - The device supports SXP protocol up to version 3.

        'four'    - The device supports SXP protocol up to version 4." 
    ::= { ctsxSxpGlobalObjects 21 }

ctsxSxpConnectionTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CtsxSxpConnectionEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A list of SXP peers configured on this device."
    ::= { ctsxSxpConnectionObjects 1 }

ctsxSxpConnectionEntry OBJECT-TYPE
    SYNTAX          CtsxSxpConnectionEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing management information of a
        particular SXP peers."
    INDEX           {
                        ctsxSxpConnVrfName,
                        ctsxSxpConnPeerAddrType,
                        ctsxSxpConnPeerAddr
                    } 
    ::= { ctsxSxpConnectionTable 1 }

CtsxSxpConnectionEntry ::= SEQUENCE {
        ctsxSxpConnVrfName             CiscoVrfName,
        ctsxSxpConnPeerAddrType        InetAddressType,
        ctsxSxpConnPeerAddr            InetAddress,
        ctsxSxpConnSourceAddrType      InetAddressType,
        ctsxSxpConnSourceAddr          InetAddress,
        ctsxSxpConnOperSourceAddrType  InetAddressType,
        ctsxSxpConnOperSourceAddr      InetAddress,
        ctsxSxpConnPasswordUsed        INTEGER,
        ctsxSxpConnConfigPasswordType  CtsPasswordEncryptionType,
        ctsxSxpConnConfigPassword      CtsPassword,
        ctsxSxpConnViewPasswordType    CtsPasswordEncryptionType,
        ctsxSxpConnViewPassword        CtsPassword,
        ctsxSxpConnModeLocation        INTEGER,
        ctsxSxpConnMode                INTEGER,
        ctsxSxpConnInstance            Unsigned32,
        ctsxSxpConnStatusLastChange    Unsigned32,
        ctsxSxpConnStatus              INTEGER,
        ctsxSxpVrfId                   Unsigned32,
        ctsxSxpConnStorageType         StorageType,
        ctsxSxpConnRowStatus           RowStatus,
        ctsxSxpConnVersion             INTEGER,
        ctsxSxpConnSpeakerMinHoldTime  Unsigned32,
        ctsxSxpConnListenerMinHoldTime Unsigned32,
        ctsxSxpConnListenerMaxHoldTime Unsigned32,
        ctsxSxpConnHoldTime            Unsigned32,
        ctsxSxpConnCapability          BITS
}

ctsxSxpConnVrfName OBJECT-TYPE
    SYNTAX          CiscoVrfName
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The name of the Virtual Routing and Forwarding (VRF) table
        associated with this SXP connection.

        A zero length string implies that connection will be setup
        in the default virtual routing and forwarding domain." 
    ::= { ctsxSxpConnectionEntry 1 }

ctsxSxpConnPeerAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The type of Internet address of the peer SXP device." 
    ::= { ctsxSxpConnectionEntry 2 }

ctsxSxpConnPeerAddr OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (1..64))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The Internet address of the SXP peer device. The type of this
        address is determined by the value of ctsxSxpConnPeerAddrType
        object." 
    ::= { ctsxSxpConnectionEntry 3 }

ctsxSxpConnSourceAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The type of source Internet address that is configured
        for this SXP connection."
    DEFVAL          { unknown } 
    ::= { ctsxSxpConnectionEntry 4 }

ctsxSxpConnSourceAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The source Internet address configured for this SXP connection.
        The type of this address is determined by the value
        of ctsxSxpConnSourceAddrType object.

        When specified, value of this object takes precedence over
        the ctsxSxpDefaultSourceAddr object."
    DEFVAL          { "" } 
    ::= { ctsxSxpConnectionEntry 5 }

ctsxSxpConnOperSourceAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The type of source Internet address that is in
        in use for this SXP connection." 
    ::= { ctsxSxpConnectionEntry 6 }

ctsxSxpConnOperSourceAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The source Internet address that is in use for
        this SXP connection.

        The type of this address is determined by the value
        of ctsxSxpConnSourceAddrType object." 
    ::= { ctsxSxpConnectionEntry 7 }

ctsxSxpConnPasswordUsed OBJECT-TYPE
    SYNTAX          INTEGER  {
                        none(1),
                        default(2),
                        connectionSpecific(3)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the type of password to be used for this
        SXP connection.

        'none'    - No password required for the SXP connection. 

        'default' - The default password which is specified by the
                   object ctsxSxpViewDefaultPassword, will be used
                   for the SXP connection.

        'connectionSpecific' - The password specified by the 
                   ctsxSxpConnViewPassword object will be used for
                   the connection."
    DEFVAL          { none } 
    ::= { ctsxSxpConnectionEntry 8 }

ctsxSxpConnConfigPasswordType OBJECT-TYPE
    SYNTAX          CtsPasswordEncryptionType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the type of encryption used
        to configure ctsxSxpConnConfigPassword string.

        When read, this object will always return 'other'. 

        Value for this object may be specified as 'clearText',
        'typeSix' or 'typeSeven' if the value of the object
        ctsxSxpConnPasswordUsed is 'connectionSpecific'.

        Value for this object may not be specified if the value of 
        ctsxSxpConnPasswordUsed is other than 'connectionSpecific'."
    DEFVAL          { none } 
    ::= { ctsxSxpConnectionEntry 9 }

ctsxSxpConnConfigPassword OBJECT-TYPE
    SYNTAX          CtsPassword
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to specify the password for this
        connection.

        The type of encryption used to configure this password 
        is determined by ctsxSxpConnConfigPasswordType.

        When read, this object will always return a zero length string.

        A non zero length password must be specified for this object if
        the value of ctsxSxpConnConfigPasswordType is other than 'none'
        or 'other'.

        A value for this object may not be specified if the value of
        ctsxSxpConnPasswordUsed is other than 'connectionSpecific'.

        The purpose of this object is to only allow configuration of
        the password. The ctsxSxpConnViewPassword object is used to
        display the password."
    DEFVAL          { "" } 
    ::= { ctsxSxpConnectionEntry 10 }

ctsxSxpConnViewPasswordType OBJECT-TYPE
    SYNTAX          CtsPasswordEncryptionType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the type of encryption in use
        for ctsxSxpConnViewPassword." 
    ::= { ctsxSxpConnectionEntry 11 }

ctsxSxpConnViewPassword OBJECT-TYPE
    SYNTAX          CtsPassword
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the password associated with this
        connection.

        The type of encryption used to display this password is 
        determined by the object ctsxSxpConnViewPasswordType.

        The purpose of this object is to only display the password.
        The ctsxSxpConnConfigPassword object is used to configure the
        password." 
    ::= { ctsxSxpConnectionEntry 12 }

ctsxSxpConnModeLocation OBJECT-TYPE
    SYNTAX          INTEGER  {
                        local(1),
                        peer(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies if ctsxSxpConnMode is applicable
        for local or the peer device.

        A value of 'local' indicates that ctsxSxpConnMode applies to 
        the local device in this SXP connection.

        A value of 'peer' indicates that ctsxSxpConnMode applies to 
        the peer device in this SXP connection."
    DEFVAL          { local } 
    ::= { ctsxSxpConnectionEntry 13 }

ctsxSxpConnMode OBJECT-TYPE
    SYNTAX          INTEGER  {
                        speaker(1),
                        listener(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the device mode of this SXP connection.

        A value of 'speaker' indicates that device will acts as
        the speaker in this SXP connection.

        A value of 'listener' indicates that device will acts as
        the listener in this SXP connection."
    DEFVAL          { speaker } 
    ::= { ctsxSxpConnectionEntry 14 }

ctsxSxpConnInstance OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the instance number associated
        with this SXP connection.

        The instance number is used to identify stale SGT
        mappings which need to be removed from the system." 
    ::= { ctsxSxpConnectionEntry 15 }

ctsxSxpConnStatusLastChange OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The amount of time elapsed since change in status of this SXP
        connection." 
    ::= { ctsxSxpConnectionEntry 16 }

ctsxSxpConnStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        off(2),
                        on(3),
                        pendingOn(4),
                        deleteHoldDown(5)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the status of this SXP connection.

        'other'      - Any other state not covered by below
                       enumerations.

        'off'        - The SXP connection has been disconnected.
                       SGT mappings are no longer learnt through SXP
                       connection in this state. SGT mappings
                       already learnt through this connection will be
                       deleted.

        'on'         - The SXP connection has been successfully
                       established. SGT mappings are learnt
                       through this SXP connection.

        'pendingOn'  - A request to establish SXP connection has been
                       sent to the peer and is pending.

        'deleteHoldDown' - The SXP connection is not operational and
                       delete hold-down timer has been started. If the
                       SXP connection does not recover before the
                       expiration of the hold-down timer, the SGT
                       mappings learnt on this connection will be
                       deleted. If the SXP connection recovers
                       before the expiration of the hold-down timer,
                       the SGT mappings learnt on this connection
                       will not be deleted." 
    ::= { ctsxSxpConnectionEntry 17 }

ctsxSxpVrfId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The numerical identifier associated with ctsxSxpConnVrfName." 
    ::= { ctsxSxpConnectionEntry 18 }

ctsxSxpConnStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The storage type of this conceptual row."
    DEFVAL          { volatile } 
    ::= { ctsxSxpConnectionEntry 19 }

ctsxSxpConnRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The status of this conceptual row.

        Once a row becomes active, only the value in
        ctsxSxpConnModeLocation, ctsxSxpConnMode
        ctsxSxpConnSpeakerMinHoldTime, ctsxSxpConnListenerMinHoldTime,
        and ctsxSxpConnListenerMaxHoldTime within each a row can
        be modified." 
    ::= { ctsxSxpConnectionEntry 20 }

ctsxSxpConnVersion OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        one(2),
                        two(3),
                        three(4),
                        four(5)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The version of SXP protocol in use for this connection.
        'unknown'    - Version of SXP protocol for this connection
                       is unknown.
        'one' - Connection is using version 1 of the SXP protocol.

        'two' - Connection is using version 2 of the SXP protocol.

        'three' - Connection is using version 3 of the SXP protocol.

        'four' - Connection is using version 4 of the SXP protocol." 
    ::= { ctsxSxpConnectionEntry 21 }

ctsxSxpConnSpeakerMinHoldTime OBJECT-TYPE
    SYNTAX          Unsigned32 (0 | 1..65534 | 65535)
    UNITS           "seconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the minimum hold-time for this SXP
        connection when the device is acting as 'speaker'.

        Setting the object to zero indicates that the global value 
        ctsxSxpSpeakerMinHoldTime will be used for the connection.

        Setting the object to 65535 indicates that the hold-time
        functionality has been disabled for the connection. Value of
        this object must be 65535 if the corresponding instance value
        of ctsxSxpConnListenerMinHoldTime is 65535.

        Value of this object should be ignored and can not be set
        if the corresponding instance values of ctsxSxpConnModeLocation
        is 'local' and ctsSxpConnMode is 'listener' or
        ctsxSxpConnModeLocation is 'peer' and ctsSxpConnMode is
        'speaker'."
    DEFVAL          { 0 } 
    ::= { ctsxSxpConnectionEntry 22 }

ctsxSxpConnListenerMinHoldTime OBJECT-TYPE
    SYNTAX          Unsigned32 (0 | 1..65534 | 65535)
    UNITS           "seconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the minimum hold-time for this SXP
        connection when the device is acting as 'listener'.

        Value of this object must be lesser than
        ctsxSxpConnListenerMaxHoldTime.

        Setting the object to zero indicates that the global value
        ctsxSxpListenerMinHoldTime will be used for the connection.
        Value of this object must be zero if the value of corresponding
        instance value of ctsxSxpConnListenerMaxHoldTime is zero.

        Setting the object to 65535 indicates that hold-time
        functionality has been disabled for the connection. Value of
        this object must be 65535 if the corresponding instance value
        of ctsxSxpConnListenerMaxHoldTime is 65535.

        Value of this object should be ignored and can not be set
        if the corresponding instance value of ctsxSxpConnModeLocation
        is 'local' and ctsSxpConnMode is 'speaker' or
        ctsxSxpConnModeLocation is 'peer' and ctsSxpConnMode is
        'listener'."
    DEFVAL          { 0 } 
    ::= { ctsxSxpConnectionEntry 23 }

ctsxSxpConnListenerMaxHoldTime OBJECT-TYPE
    SYNTAX          Unsigned32 (0 | 1..65534 | 65535)
    UNITS           "seconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the maximum hold-time for this SXP
        connection when the device is acting as 'listener'.

        Value of this object must be greater than
        ctsxSxpConnListenerMinHoldTime.

        Setting the object to zero indicates that the global value
        ctsxSxpListenerMaxHoldTime will be used for the connection.
        Value of this object must be zero if the corresponding
        instance value of ctsxSxpConnListenerMinHoldTime is zero.

        Setting the object to 65535 indicates that hold-time
        functionality has been disabled for the connection. Value of
        this object must be 65535 if the corresponding instance value
        ctsxSxpConnListenerMinHoldTime is 65535.

        Value of this object should be ignored and can not be set
        if the corresponding instance value of ctsxSxpConnModeLocation
        is 'local' and ctsSxpConnMode is 'speaker' or
        ctsxSxpConnModeLocation is 'peer' and ctsSxpConnMode is
        'listener'."
    DEFVAL          { 0 } 
    ::= { ctsxSxpConnectionEntry 24 }

ctsxSxpConnHoldTime OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the hold-time in use for this
        SXP connection.

        A value of 0 indicates that hold-time functionality has been
        disabled for this connection." 
    ::= { ctsxSxpConnectionEntry 25 }

ctsxSxpConnCapability OBJECT-TYPE
    SYNTAX          BITS {
                        ipv4(0),
                        ipv6(1),
                        subnet(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the capability of SXP connection." 
    ::= { ctsxSxpConnectionEntry 26 }
 


ctsxIpSgtMappingTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CtsxIpSgtMappingEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A list of SGT mappings learnt by this device.

        If the value of ctsxSxpConnVersion is 'three' or above,
        this table populates entries for all mapping addresses
        without prefix.
        Addresses with prefix are not populated in this table.
        ctsxSxpSgtMapTable should be used in such case."
    ::= { ctsxSxpSgtObjects 1 }

ctsxIpSgtMappingEntry OBJECT-TYPE
    SYNTAX          CtsxIpSgtMappingEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing management information about SGT
        mapping learnt by this device.

        An entry will be created for each SGT mappings the device
        learns via SXP.

        An entry will be deleted if SXP connection from where the
        SGT mappings was learnt is disconnected."
    INDEX           {
                        ctsxIpSgtMappingVrfId,
                        ctsxIpSgtMappingAddrType,
                        ctsxIpSgtMappingAddr,
                        ctsxIpSgtMappingPeerAddrType,
                        ctsxIpSgtMappingPeerAddr
                    } 
    ::= { ctsxIpSgtMappingTable 1 }

CtsxIpSgtMappingEntry ::= SEQUENCE {
        ctsxIpSgtMappingVrfId        Unsigned32,
        ctsxIpSgtMappingAddrType     InetAddressType,
        ctsxIpSgtMappingAddr         InetAddress,
        ctsxIpSgtMappingPeerAddrType InetAddressType,
        ctsxIpSgtMappingPeerAddr     InetAddress,
        ctsxIpSgtMappingSgt          CtsSecurityGroupTag,
        ctsxIpSgtMappingInstance     Unsigned32,
        ctsxIpSgtMappingVrfName      CiscoVrfName,
        ctsxIpSgtMappingStatus       INTEGER
}

ctsxIpSgtMappingVrfId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The VRF number identifying the VRF where this SGT mapping
        was learnt." 
    ::= { ctsxIpSgtMappingEntry 1 }

ctsxIpSgtMappingAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The type of IP address in this SGT mapping." 
    ::= { ctsxIpSgtMappingEntry 2 }

ctsxIpSgtMappingAddr OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (1..48))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP address in this SGT mapping.

        The type of this address is determined by the value of
        ctsxIpSgtMappingAddrType object." 
    ::= { ctsxIpSgtMappingEntry 3 }

ctsxIpSgtMappingPeerAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The type of IP address of the SXP peer device from where
        this SGT mapping was learnt." 
    ::= { ctsxIpSgtMappingEntry 4 }

ctsxIpSgtMappingPeerAddr OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (1..48))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP address of the peer SXP device from where this SGT
        mapping was learnt.

        The type of this address is determined by the value of
        ctsxIpSgtMappingPeerAddrType object." 
    ::= { ctsxIpSgtMappingEntry 5 }

ctsxIpSgtMappingSgt OBJECT-TYPE
    SYNTAX          CtsSecurityGroupTag
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The Security Group Tag (SGT) in this SGT mapping.

        ctsxIpSgtMappingAddr represents the IP address associated
        with this SGT." 
    ::= { ctsxIpSgtMappingEntry 6 }

ctsxIpSgtMappingInstance OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the instance number of the SXP
        connection from where this SGT mapping was learnt.

        The instance number is used to determine if an SGT
        mapping entry is stale and needs to be removed 
        from the system." 
    ::= { ctsxIpSgtMappingEntry 7 }

ctsxIpSgtMappingVrfName OBJECT-TYPE
    SYNTAX          CiscoVrfName
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The name of the VRF identified by ctsxIpSgtMappingVrfId." 
    ::= { ctsxIpSgtMappingEntry 8 }

ctsxIpSgtMappingStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        active(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the status of this SGT mapping.

        'other'  - Any other state no covered by below
                   enumerations.
        'active' - The SGT mapping is currently active." 
    ::= { ctsxIpSgtMappingEntry 9 }
 


ctsxSxpSgtMapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CtsxSxpSgtMapEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A list of SGT mappings learnt by this device."
    ::= { ctsxSxpSgtObjects 2 }

ctsxSxpSgtMapEntry OBJECT-TYPE
    SYNTAX          CtsxSxpSgtMapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing management information about SGT
        mapping learnt by this device.

        An entry will be created for each of the SGT mappings
        the device learns via SXP.

        An entry will be deleted if SXP connection from where the
        SGT mappings was learnt is disconnected."
    INDEX           {
                        ctsxSxpSgtMapVrfId,
                        ctsxSxpSgtMapAddrType,
                        ctsxSxpSgtMapAddr,
                        ctsxSxpSgtMapAddrPrefixLength,
                        ctsxSxpSgtMapPeerAddrType,
                        ctsxSxpSgtMapPeerAddr
                    } 
    ::= { ctsxSxpSgtMapTable 1 }

CtsxSxpSgtMapEntry ::= SEQUENCE {
        ctsxSxpSgtMapVrfId            Unsigned32,
        ctsxSxpSgtMapAddrType         InetAddressType,
        ctsxSxpSgtMapAddr             InetAddress,
        ctsxSxpSgtMapAddrPrefixLength InetAddressPrefixLength,
        ctsxSxpSgtMapPeerAddrType     InetAddressType,
        ctsxSxpSgtMapPeerAddr         InetAddress,
        ctsxSxpSgtMapSgt              CtsSecurityGroupTag,
        ctsxSxpSgtMapInstance         Unsigned32,
        ctsxSxpSgtMapVrfName          CiscoVrfName,
        ctsxSxpSgtMapPeerSeq          OCTET STRING,
        ctsxSxpSgtMapStatus           INTEGER
}

ctsxSxpSgtMapVrfId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The VRF number identifying the VRF where this SGT mapping
        was learnt." 
    ::= { ctsxSxpSgtMapEntry 1 }

ctsxSxpSgtMapAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The type of address in this SGT mapping." 
    ::= { ctsxSxpSgtMapEntry 2 }

ctsxSxpSgtMapAddr OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (1..48))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The address in this SGT mapping.

        The type of this address is determined by the value of
        ctsxSxpSgtMapAddrType object." 
    ::= { ctsxSxpSgtMapEntry 3 }

ctsxSxpSgtMapAddrPrefixLength OBJECT-TYPE
    SYNTAX          InetAddressPrefixLength
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the length of the prefix associated
        with ctsxSxpSgtMapAddr.

        This object is always interpreted with the value of
        ctsxSxpSgtMapAddrType object." 
    ::= { ctsxSxpSgtMapEntry 4 }

ctsxSxpSgtMapPeerAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The type of address of the SXP peer device from where
        this SGT mapping was learnt." 
    ::= { ctsxSxpSgtMapEntry 5 }

ctsxSxpSgtMapPeerAddr OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (1..48))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The address of the peer SXP device from where this SGT
        mapping was learnt.

        The type of this address is determined by the value of
        ctsxSxpSgtMapPeerAddrType object." 
    ::= { ctsxSxpSgtMapEntry 6 }

ctsxSxpSgtMapSgt OBJECT-TYPE
    SYNTAX          CtsSecurityGroupTag
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The Security Group Tag (SGT) in this SGT mapping.

        ctsxSxpSgtMapAddr represents the address associated
        with this SGT." 
    ::= { ctsxSxpSgtMapEntry 7 }

ctsxSxpSgtMapInstance OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the instance number of the SXP
        connection from where this SGT binding was learnt.

        The instance number is used to determine if an SGT
        mapping entry is stale and needs to be removed 
        from the system." 
    ::= { ctsxSxpSgtMapEntry 8 }

ctsxSxpSgtMapVrfName OBJECT-TYPE
    SYNTAX          CiscoVrfName
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The name of the VRF identified by ctsxEnahncedSgtMapVrfId." 
    ::= { ctsxSxpSgtMapEntry 9 }

ctsxSxpSgtMapPeerSeq OBJECT-TYPE
    SYNTAX          OCTET STRING
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The Peer Sequence associated with this SGT
        mapping entry.

        It is a sequence of node IDs though which SGT 
        mapping has traversed.

        Each node ID is 4 octets long. The octets 1 to 4
        represent the first node ID in the sequence, octets
        5 to 8 represent the second node ID in the sequence
        and so on." 
    ::= { ctsxSxpSgtMapEntry 10 }

ctsxSxpSgtMapStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        active(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the status of this SGT mapping.

        'other'  - Any other state no covered by below
                   enumerations.
        'active' - The SGT mapping is currently active." 
    ::= { ctsxSxpSgtMapEntry 11 }
 


-- Notifications Control

ctsxSxpConnSourceAddrErrNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the system generates the
        ctsxSxpConnSourceAddrErrNotif.

        A value of 'false' will prevent ctsxSxpConnSourceAddrErrNotif
        notifications from being generated by this system." 
    ::= { ciscoTrustSecSxpMIBNotifsControl 1 }

ctsxSxpMsgParseErrNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the system generates the
        ctsxSxpMsgParseErrNotif.

        A value of 'false' will prevent ctsxSxpMsgParseErrNotif
        notifications from being generated by this system." 
    ::= { ciscoTrustSecSxpMIBNotifsControl 2 }

ctsxSxpConnConfigErrNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the system generates the
        ctsxSxpConnConfigErrNotif.

        A value of 'false' will prevent ctsxSxpConnConfigErrNotif
        notifications from being generated by this system." 
    ::= { ciscoTrustSecSxpMIBNotifsControl 3 }

ctsxSxpBindingErrNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the system generates the
        ctsxSxpBindingErrNotif.

        A value of 'false' will prevent ctsxSxpBindingErrNotif
        notifications from being generated by this system." 
    ::= { ciscoTrustSecSxpMIBNotifsControl 4 }

ctsxSxpConnUpNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the system generates the
        ctsxSxpConnUpNotif.

        A value of 'false' will prevent ctsxSxpConnUpNotif
        notifications from being generated by this system." 
    ::= { ciscoTrustSecSxpMIBNotifsControl 5 }

ctsxSxpConnDownNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the system generates the
        ctsxSxpConnDownNotif.

        A value of 'false' will prevent ctsxSxpConnDownNotif
        notifications from being generated by this system." 
    ::= { ciscoTrustSecSxpMIBNotifsControl 6 }

ctsxSxpExpansionFailNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the system generates the
        ctsxSxpExpansionFailNotif.

        A value of 'false' will prevent ctsxSxpExpansionFailNotif
        notifications from being generated by this system." 
    ::= { ciscoTrustSecSxpMIBNotifsControl 7 }

ctsxSxpOperNodeIdChangeNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the system generates the
        ctsxSxpOperNodeIdChangeNotif.

        A value of 'false' will prevent ctsxSxpOperNodeIdChangeNotif
        notifications from being generated by this system." 
    ::= { ciscoTrustSecSxpMIBNotifsControl 8 }

ctsxSxpBindingConflictNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the system generates the
        ctsxSxpBindingConflictNotif.

        A value of 'false' will prevent ctsxSxpBindingConflictNotif
        notifications from being generated by this system." 
    ::= { ciscoTrustSecSxpMIBNotifsControl 9 }

ctsxSgtMapExpansionVrf OBJECT-TYPE
    SYNTAX          CiscoVrfName
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object indicates the VRF name for which
        host SGT bindings cannot be expanded." 
    ::= { ciscoTrustSecSxpMIBNotifsOnlyInfo 1 }

ctsxSgtMapExpansionAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object indicates the type of subnet address for
        which host SGT binding cannot be expanded." 
    ::= { ciscoTrustSecSxpMIBNotifsOnlyInfo 2 }

ctsxSgtMapExpansionAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object indicates the subnet address for which
        host SGT binding cannot be expanded.

        The type of this address is determined by the value of
        ctsxSgtMapExpansionAddrType object." 
    ::= { ciscoTrustSecSxpMIBNotifsOnlyInfo 3 }

ctsxSgtMapExpansionAddrPrefixLength OBJECT-TYPE
    SYNTAX          InetAddressPrefixLength
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object indicates the length of the prefix associated
        with ctsxSgtMapExpansionAddr.

        This object is always interpreted with the value of
        ctsxSgtMapExpansionAddrType object." 
    ::= { ciscoTrustSecSxpMIBNotifsOnlyInfo 4 }

ctsxSxpNotifErrMsg OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object indicates error message associated with
        notifications." 
    ::= { ciscoTrustSecSxpMIBNotifsOnlyInfo 5 }

ctsxSgtMapConflictingVrfName OBJECT-TYPE
    SYNTAX          CiscoVrfName
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object indicates the VRF name of the SXP connection
        on which conflicting SGT mapping was received." 
    ::= { ciscoTrustSecSxpMIBNotifsOnlyInfo 6 }

ctsxSgtMapConflictingAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object indicates the type of Internet address
        in the conflicting SGT mapping." 
    ::= { ciscoTrustSecSxpMIBNotifsOnlyInfo 7 }

ctsxSgtMapConflictingAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object indicates the Internet address
        in the conflicting SGT mapping.

        The type of this address is determined by the value of
        ctsxSgtMapConflictingAddrType object." 
    ::= { ciscoTrustSecSxpMIBNotifsOnlyInfo 8 }

ctsxSgtMapConflictingOldSgt OBJECT-TYPE
    SYNTAX          CtsSecurityGroupTag
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "The existing value of Security Group Tag (SGT) in
        SGT mapping for which conflict has occurred." 
    ::= { ciscoTrustSecSxpMIBNotifsOnlyInfo 9 }

ctsxSgtMapConflictingNewSgt OBJECT-TYPE
    SYNTAX          CtsSecurityGroupTag
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "The new value of Security Group Tag (SGT) in
        SGT mapping that conflicts with the existing SGT." 
    ::= { ciscoTrustSecSxpMIBNotifsOnlyInfo 10 }

ctsxSxpOldOperNodeId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "The SXP node ID that was in use by this SXP node and
        now replaced by a new SXP node ID represented by
        ctsxSxpOperNodeId." 
    ::= { ciscoTrustSecSxpMIBNotifsOnlyInfo 11 }

-- Notifications

ctsxSxpConnSourceAddrErrNotif NOTIFICATION-TYPE
    OBJECTS         {
                        ctsxSxpConnOperSourceAddrType,
                        ctsxSxpConnOperSourceAddr
                    }
    STATUS          current
    DESCRIPTION
        "A ctsxSxpConnSourceAddrErrNotif is generated if the
        system is not able to establish SXP connection using
        ctsxSxpConnOperSourceAddr."
   ::= { ciscoTrustSecSxpMIBNotifs 1 }

ctsxSxpMsgParseErrNotif NOTIFICATION-TYPE
    OBJECTS         {
                        ctsxSxpConnOperSourceAddrType,
                        ctsxSxpConnOperSourceAddr,
                        ctsxSxpNotifErrMsg
                    }
    STATUS          current
    DESCRIPTION
        "A ctsxSxpMsgParseErrNotif is generated if the system is
        not able to parse a received SXP message."
   ::= { ciscoTrustSecSxpMIBNotifs 2 }

ctsxSxpConnConfigErrNotif NOTIFICATION-TYPE
    OBJECTS         {
                        ctsxSxpConnOperSourceAddrType,
                        ctsxSxpConnOperSourceAddr,
                        ctsxSxpNotifErrMsg
                    }
    STATUS          current
    DESCRIPTION
        "A ctsxSxpConnConfigErrNotif is generated if the system
        detects a configuration error for an SXP connection."
   ::= { ciscoTrustSecSxpMIBNotifs 3 }

ctsxSxpBindingErrNotif NOTIFICATION-TYPE
    OBJECTS         {
                        ctsxSxpSgtMapSgt,
                        ctsxSxpSgtMapInstance,
                        ctsxSxpSgtMapVrfName,
                        ctsxSxpNotifErrMsg
                    }
    STATUS          current
    DESCRIPTION
        "A ctsxSxpBindingErrNotif is generated if the address in the
        SGT mapping is not found in routing and forwarding table of
        the system."
   ::= { ciscoTrustSecSxpMIBNotifs 4 }

ctsxSxpConnUpNotif NOTIFICATION-TYPE
    OBJECTS         {
                        ctsxSxpConnOperSourceAddrType,
                        ctsxSxpConnOperSourceAddr,
                        ctsxSxpConnInstance,
                        ctsxSxpConnStatus
                    }
    STATUS          current
    DESCRIPTION
        "A ctsxSxpConnUpNotif is generated if the ctsxSxpConnStatus
        for an SXP connection transitioned into 'on' state."
   ::= { ciscoTrustSecSxpMIBNotifs 5 }

ctsxSxpConnDownNotif NOTIFICATION-TYPE
    OBJECTS         {
                        ctsxSxpConnOperSourceAddrType,
                        ctsxSxpConnOperSourceAddr,
                        ctsxSxpConnInstance,
                        ctsxSxpConnStatus
                    }
    STATUS          current
    DESCRIPTION
        "A ctsxSxpConnDownNotif is generated if ctsxSxpConnStatus
        for an SXP connection left the 'on' state and transitioned
        into some other state."
   ::= { ciscoTrustSecSxpMIBNotifs 6 }

ctsxSxpExpansionFailNotif NOTIFICATION-TYPE
    OBJECTS         {
                        ctsxSgtMapExpansionLimit,
                        ctsxSgtMapExpansionCount,
                        ctsxSgtMapExpansionVrf,
                        ctsxSgtMapExpansionAddrType,
                        ctsxSgtMapExpansionAddr,
                        ctsxSgtMapExpansionAddrPrefixLength
                    }
    STATUS          current
    DESCRIPTION
        "A ctsxSxpExpansionFailNotif is generated if the number of
        expanded SGT maps reaches the configured limit and the received
        SGT mapping can not be expanded."
   ::= { ciscoTrustSecSxpMIBNotifs 7 }

ctsxSxpOperNodeIdChangeNotif NOTIFICATION-TYPE
    OBJECTS         {
                        ctsxSxpOldOperNodeId,
                        ctsxSxpOperNodeId
                    }
    STATUS          current
    DESCRIPTION
        "A ctsxSxpOperNodeIdChangeNotif is generated if the value of
        ctsxSxpOperNodeId changes."
   ::= { ciscoTrustSecSxpMIBNotifs 8 }

ctsxSxpBindingConflictNotif NOTIFICATION-TYPE
    OBJECTS         {
                        ctsxSgtMapConflictingVrfName,
                        ctsxSgtMapConflictingAddrType,
                        ctsxSgtMapConflictingAddr,
                        ctsxSgtMapConflictingOldSgt,
                        ctsxSgtMapConflictingNewSgt
                    }
    STATUS          current
    DESCRIPTION
        "A ctsxSxpBindingConflictNotif is generated if the
        device receives conflicting SGT mapping information."
   ::= { ciscoTrustSecSxpMIBNotifs 9 }
-- Conformance

ciscoTrustSecSxpMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoTrustSecSxpMIBConform 1 }

ciscoTrustSecSxpMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoTrustSecSxpMIBConform 2 }


ciscoTrustSecSxpMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the CISCO-TRUSTSEC-SXP-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ctsxSxpGlobalGroup,
                        ctsxSxpConnectionGroup,
                        ctsxIpSgtMappingGroup
                    }

    OBJECT          ctsxSxpEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConfigDefaultPasswordType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConfigDefaultPassword
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpDefaultSourceAddrType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpDefaultSourceAddr
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpRetryPeriod
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpReconPeriod
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnSourceAddrType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnSourceAddr
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnPasswordUsed
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnConfigPasswordType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnConfigPassword
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnModeLocation
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnMode
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnRowStatus
    SYNTAX          INTEGER  {
                        active(1)
                    }
    WRITE-SYNTAX    INTEGER  {
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required.
        Support for createAndWait and notInService is not required."
    ::= { ciscoTrustSecSxpMIBCompliances 1 }

ciscoTrustSecSxpMIBCompliance2 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the CISCO-TRUSTSEC-SXP-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ctsxSxpGlobalGroup,
                        ctsxSxpConnectionGroup,
                        ctsxIpSgtMappingGroup
                    }

    GROUP           ctsxSxpVersionGroup
    DESCRIPTION
        "This group is mandatory for platforms which support
        displaying SXP protocol version."

    OBJECT          ctsxSxpEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConfigDefaultPasswordType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConfigDefaultPassword
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpDefaultSourceAddrType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpDefaultSourceAddr
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpRetryPeriod
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpReconPeriod
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnSourceAddrType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnSourceAddr
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnPasswordUsed
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnConfigPasswordType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnConfigPassword
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnModeLocation
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnMode
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnRowStatus
    SYNTAX          INTEGER  {
                        active(1)
                    }
    WRITE-SYNTAX    INTEGER  {
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required.
        Support for createAndWait and notInService is not required."
    ::= { ciscoTrustSecSxpMIBCompliances 2 }

ciscoTrustSecSxpMIBCompliance3 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for the CISCO-TRUSTSEC-SXP-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ctsxSxpGlobalGroup,
                        ctsxSxpConnectionGroup
                    }

    GROUP           ctsxSxpVersionGroup
    DESCRIPTION
        "This group is mandatory for platforms which support
        displaying SXP protocol version."

    GROUP           ctsxSxpBindingLogGroup
    DESCRIPTION
        "This group is mandatory for platforms which support
        controlling logging functionality for SXP bindings."

    GROUP           ctsxSxpBindingNotifInfoGroup
    DESCRIPTION
        "This group is mandatory for platforms which support
        binding expansion functionality in SXP."

    GROUP           ctsxSxpNodeIdInfoGroup
    DESCRIPTION
        "This group is mandatory for platforms which support
        loop detection functionality for SXP."

    GROUP           ctsxIpSgtMappingGroup
    DESCRIPTION
        "This group is mandatory for platforms which support
        SGT mapping functionality but do not support
        SGT mapping expansion functionality ."

    GROUP           ctsxSxpSgtMapGroup
    DESCRIPTION
        "This group is mandatory for platforms which support
        SGT mapping and SGT mapping expansion functionality in SXP."

    GROUP           ctsxNotifsControlGroup
    DESCRIPTION
        "This group is mandatory for platforms which support
        SXP notifications."

    GROUP           ctsxNotifsGroup
    DESCRIPTION
        "This group is mandatory for platforms which support
        SXP notifications."

    GROUP           ctsxSxpNotifErrMsgGroup
    DESCRIPTION
        "This group is mandatory for platforms which support
        ctsxNotifsGroup."

    GROUP           ctsxSxpGlobalHoldTimeGroup
    DESCRIPTION
        "This group is mandatory for platforms which support
        global hold-time configuration for SXP connections."

    GROUP           ctsxSxpConnHoldTimeGroup
    DESCRIPTION
        "This group is mandatory for platforms which support
        hold-time configuration for individual SXP connections."

    GROUP           ctsxSxpConnCapbilityGroup
    DESCRIPTION
        "This group is mandatory for platforms which provide
        capability information for SXP connections."

    GROUP           ctsxSxpVersionSupportGroup
    DESCRIPTION
        "This group is mandatory for platforms which provide
        version support information for SXP protocol."

    GROUP           ctsxSgtMapPeerSeqGroup
    DESCRIPTION
        "This group is mandatory for platforms which provide
        Peer Sequence information for the SGT mapping."

    OBJECT          ctsxSxpEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConfigDefaultPasswordType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConfigDefaultPassword
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpDefaultSourceAddrType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpDefaultSourceAddr
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpRetryPeriod
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpReconPeriod
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnSourceAddrType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnSourceAddr
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnPasswordUsed
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnConfigPasswordType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnConfigPassword
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnModeLocation
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnMode
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnRowStatus
    SYNTAX          INTEGER  {
                        active(1)
                    }
    WRITE-SYNTAX    INTEGER  {
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required.
        Support for createAndWait and notInService is not required."

    OBJECT          ctsxSxpBindingChangesLogEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSgtMapExpansionLimit
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpAdminNodeId
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpNodeIdInterface
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpNodeIdIpAddrType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpNodeIdIpAddr
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnSourceAddrErrNotifEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpMsgParseErrNotifEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnConfigErrNotifEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpBindingErrNotifEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnUpNotifEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpConnDownNotifEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpExpansionFailNotifEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpOperNodeIdChangeNotifEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ctsxSxpBindingConflictNotifEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."
    ::= { ciscoTrustSecSxpMIBCompliances 3 }

-- Units of Conformance

ctsxSxpGlobalGroup OBJECT-GROUP
    OBJECTS         {
                        ctsxSxpEnable,
                        ctsxSxpConfigDefaultPasswordType,
                        ctsxSxpConfigDefaultPassword,
                        ctsxSxpViewDefaultPasswordType,
                        ctsxSxpViewDefaultPassword,
                        ctsxSxpDefaultSourceAddrType,
                        ctsxSxpDefaultSourceAddr,
                        ctsxSxpRetryPeriod,
                        ctsxSxpReconPeriod
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing management functionality
        of global SXP configuration."
    ::= { ciscoTrustSecSxpMIBGroups 1 }

ctsxSxpConnectionGroup OBJECT-GROUP
    OBJECTS         {
                        ctsxSxpConnSourceAddrType,
                        ctsxSxpConnSourceAddr,
                        ctsxSxpConnOperSourceAddrType,
                        ctsxSxpConnOperSourceAddr,
                        ctsxSxpConnPasswordUsed,
                        ctsxSxpConnConfigPasswordType,
                        ctsxSxpConnConfigPassword,
                        ctsxSxpConnViewPasswordType,
                        ctsxSxpConnViewPassword,
                        ctsxSxpConnModeLocation,
                        ctsxSxpConnMode,
                        ctsxSxpConnInstance,
                        ctsxSxpConnStatusLastChange,
                        ctsxSxpConnStatus,
                        ctsxSxpVrfId,
                        ctsxSxpConnStorageType,
                        ctsxSxpConnRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing management functionality
        of SXP connections."
    ::= { ciscoTrustSecSxpMIBGroups 2 }

ctsxIpSgtMappingGroup OBJECT-GROUP
    OBJECTS         {
                        ctsxIpSgtMappingSgt,
                        ctsxIpSgtMappingInstance,
                        ctsxIpSgtMappingVrfName,
                        ctsxIpSgtMappingStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing management functionality
        of SGT mapping for SXP."
    ::= { ciscoTrustSecSxpMIBGroups 3 }

ctsxSxpVersionGroup OBJECT-GROUP
    OBJECTS         { ctsxSxpConnVersion }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) providing version information
        for SXP."
    ::= { ciscoTrustSecSxpMIBGroups 4 }

ctsxSxpBindingLogGroup OBJECT-GROUP
    OBJECTS         { ctsxSxpBindingChangesLogEnable }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) providing logging control
        for SXP binding."
    ::= { ciscoTrustSecSxpMIBGroups 5 }

ctsxSxpBindingNotifInfoGroup OBJECT-GROUP
    OBJECTS         {
                        ctsxSgtMapExpansionVrf,
                        ctsxSgtMapExpansionAddrType,
                        ctsxSgtMapExpansionAddr,
                        ctsxSgtMapExpansionAddrPrefixLength,
                        ctsxSgtMapConflictingVrfName,
                        ctsxSgtMapConflictingAddrType,
                        ctsxSgtMapConflictingAddr,
                        ctsxSgtMapConflictingOldSgt,
                        ctsxSgtMapConflictingNewSgt,
                        ctsxSxpOldOperNodeId
                    }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) providing variable binding
        information for SXP notifications."
    ::= { ciscoTrustSecSxpMIBGroups 6 }

ctsxSxpNotifErrMsgGroup OBJECT-GROUP
    OBJECTS         { ctsxSxpNotifErrMsg }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) providing detailed error messages
        for SXP notifications."
    ::= { ciscoTrustSecSxpMIBGroups 7 }

ctsxSxpNodeIdInfoGroup OBJECT-GROUP
    OBJECTS         {
                        ctsxSxpAdminNodeId,
                        ctsxSxpNodeIdInterface,
                        ctsxSxpNodeIdIpAddrType,
                        ctsxSxpNodeIdIpAddr,
                        ctsxSxpOperNodeId
                    }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) providing SXP node ID information
        for the system."
    ::= { ciscoTrustSecSxpMIBGroups 8 }

ctsxSxpSgtMapGroup OBJECT-GROUP
    OBJECTS         {
                        ctsxSxpSgtMapSgt,
                        ctsxSxpSgtMapInstance,
                        ctsxSxpSgtMapVrfName,
                        ctsxSxpSgtMapStatus,
                        ctsxSgtMapExpansionLimit,
                        ctsxSgtMapExpansionCount
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing management functionality
        of SGT mapping and expansion for SXP."
    ::= { ciscoTrustSecSxpMIBGroups 9 }

ctsxNotifsControlGroup OBJECT-GROUP
    OBJECTS         {
                        ctsxSxpConnSourceAddrErrNotifEnable,
                        ctsxSxpMsgParseErrNotifEnable,
                        ctsxSxpConnConfigErrNotifEnable,
                        ctsxSxpBindingErrNotifEnable,
                        ctsxSxpConnUpNotifEnable,
                        ctsxSxpConnDownNotifEnable,
                        ctsxSxpExpansionFailNotifEnable,
                        ctsxSxpOperNodeIdChangeNotifEnable,
                        ctsxSxpBindingConflictNotifEnable
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing notification control
        for SXP."
    ::= { ciscoTrustSecSxpMIBGroups 10 }

ctsxNotifsGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        ctsxSxpConnSourceAddrErrNotif,
                        ctsxSxpMsgParseErrNotif,
                        ctsxSxpConnConfigErrNotif,
                        ctsxSxpBindingErrNotif,
                        ctsxSxpConnUpNotif,
                        ctsxSxpConnDownNotif,
                        ctsxSxpExpansionFailNotif,
                        ctsxSxpOperNodeIdChangeNotif,
                        ctsxSxpBindingConflictNotif
                    }
    STATUS          current
    DESCRIPTION
        "A collection of notifications for SXP."
    ::= { ciscoTrustSecSxpMIBGroups 11 }

ctsxSxpGlobalHoldTimeGroup OBJECT-GROUP
    OBJECTS         {
                        ctsxSxpSpeakerMinHoldTime,
                        ctsxSxpListenerMinHoldTime,
                        ctsxSxpListenerMaxHoldTime
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing global
        hold-time information for SXP connections."
    ::= { ciscoTrustSecSxpMIBGroups 12 }

ctsxSxpConnHoldTimeGroup OBJECT-GROUP
    OBJECTS         {
                        ctsxSxpConnSpeakerMinHoldTime,
                        ctsxSxpConnListenerMinHoldTime,
                        ctsxSxpConnListenerMaxHoldTime,
                        ctsxSxpConnHoldTime
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing hold-time
        information for each SXP connection."
    ::= { ciscoTrustSecSxpMIBGroups 13 }

ctsxSxpConnCapbilityGroup OBJECT-GROUP
    OBJECTS         { ctsxSxpConnCapability }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) providing capability
        information for each SXP connection."
    ::= { ciscoTrustSecSxpMIBGroups 14 }

ctsxSxpVersionSupportGroup OBJECT-GROUP
    OBJECTS         { ctsxSxpVersionSupport }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) providing SXP version
        capability information."
    ::= { ciscoTrustSecSxpMIBGroups 15 }

ctsxSgtMapPeerSeqGroup OBJECT-GROUP
    OBJECTS         { ctsxSxpSgtMapPeerSeq }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) providing Peer Sequence
        information."
    ::= { ciscoTrustSecSxpMIBGroups 16 }

END



