-- *****************************************************************
-- CISCO-CAS-IF-CAPABILITY
--
-- Agent capabilities for Voice Interface (DS1) or Voice Port 
-- (DS0 Group) of the media gateway in CISCO Products
--
-- August 2004,  Margaret Hsieh
--
-- Copyright(c) 2003, 2004 by Cisco Systems, Inc.
--
-- *****************************************************************

CISCO-CAS-IF-CAPABILITY DEFINITIONS ::= BEGIN
IMPORTS
        MODULE-IDENTITY, Integer32
                FROM SNMPv2-SMI
        AGENT-CAPABILITIES
                FROM SNMPv2-CONF
        ciscoAgentCapability
                FROM CISCO-SMI;

ciscoCasIfCapability MODULE-IDENTITY
    LAST-UPDATED "200912040000Z"
    ORGANIZATION "Cisco Systems, Inc."
    CONTACT-INFO
        "        Cisco Systems
                 Customer Service
        Postal: 170 W Tasman Drive
                San Jose, CA 95134
                USA
           Tel: +1 800 553-NETS
        E-mail: cs-voice-gateway@cisco.com"
    DESCRIPTION
            "The agent capabilities for CISCO-CAS-IF-MIB." 
    REVISION        "200912040000Z"
    DESCRIPTION
        "Added capability statement ciscoCasIfCapabilityV12R04TPC3xxx."
 
    REVISION "200408100000Z"
    DESCRIPTION
        "Added ciscoCasIfCapabilityV5R015 for 
         MGX8850 release 5.0.15."

    REVISION "200312030000Z"
    DESCRIPTION
        "Initial version of this MIB module."

        ::= { ciscoAgentCapability 122 }


    ciscoCasIfCapabilityV5R000 AGENT-CAPABILITIES

        PRODUCT-RELEASE "MGX8850 Release 5.0"
        STATUS          current
        DESCRIPTION     "CISCO-CAS-IF-MIB Capabilities for Voice 
                         Switch Service Module(VXSM) in 
                         Release 5.0.0." 

        SUPPORTS        CISCO-CAS-IF-MIB
        INCLUDES        { 
                            ccasGeneralInfoGroupRev1,
                            ccasVoiceGroup
                        }

        VARIATION    ccasGrpCfgServiceType
        SYNTAX       INTEGER {
                        trunkingService  (8), 
                        h248             (9),
                        ds0xconn        (10)
                     }
        DESCRIPTION  "VXSM supports trunkingService(8), h248(9)
                      and ds0xconn(10) only."

        VARIATION    ccasGrpCfgType
        ACCESS       not-implemented
        DESCRIPTION  "Not supported."

        VARIATION    ccasVoiceCfgConnectionMode
        ACCESS       not-implemented
        DESCRIPTION  "Not supported."

        VARIATION    ccasVoiceCfgConnectionNumber
        ACCESS       not-implemented
        DESCRIPTION  "Not supported."

        VARIATION    ccasVoiceCfgNoiseRegEnable
        DEFVAL       { true } 
        DESCRIPTION  "The initial value is 'true'."

        VARIATION    ccasVoiceCfgNonLinearProcEnable
        DEFVAL       { true } 
        DESCRIPTION  "The initial value is 'true'."

        VARIATION    ccasVoiceCfgMusicOnHoldThreshold
        SYNTAX       Integer32 (-60..-30)
        DEFVAL       { -38 } 
        DESCRIPTION  "Limited data range supported by VXSM.
                      The initial value is -38."

        VARIATION    ccasVoiceCfgInGain
        DEFVAL       { 0 } 
        DESCRIPTION  "The initial value is 0."

        VARIATION    ccasVoiceCfgOutAttn
        DEFVAL       { 0 } 
        DESCRIPTION  "The initial value is 0."

        VARIATION    ccasVoiceCfgEchoCancelEnable
        DEFVAL       { true } 
        DESCRIPTION  "The initial value is 'true'."

        VARIATION    ccasVoiceCfgEchoCancelCoverage
        DEFVAL       { echoCanceller8ms }
        DESCRIPTION  "The initial value is 'echoCanceller8ms'."

        VARIATION    ccasVoiceCfgInitialDigitTimeOut
        DEFVAL       { 10 }
        DESCRIPTION  "The initial value is 10."

        VARIATION    ccasVoiceCfgInterDigitTimeOut
        DEFVAL       { 10 }
        DESCRIPTION  "The initial value is 10."

        VARIATION    ccasVoiceCfgRegionalTone
        ACCESS       not-implemented
        DESCRIPTION  "Not supported."

    ::= { ciscoCasIfCapability 1 }

    ciscoCasIfCapabilityV5R015 AGENT-CAPABILITIES

        PRODUCT-RELEASE "MGX8850 Release 5.0.15"
        STATUS          current
        DESCRIPTION     "CISCO-CAS-IF-MIB Capabilities for Voice 
                         Switch Service Module(VXSM) in 
                         Release 5.0.15." 

        SUPPORTS        CISCO-CAS-IF-MIB
        INCLUDES        { 
                            ccasGeneralInfoGroupRev1,
                            ccasVoiceGroup
                        }

        VARIATION    ccasGrpCfgServiceType
        SYNTAX       INTEGER {
                        mgcp             (6),
                        trunkingService  (8), 
                        h248             (9),
                        ds0xconn        (10),
                        tgcp            (11)
                     }
        DESCRIPTION  "VXSM supports mgcp(6),trunkingService(8),
                      h248(9), ds0xconn(10) and tgcp(11)."

        VARIATION    ccasGrpCfgType
        ACCESS       not-implemented
        DESCRIPTION  "Not supported."

        VARIATION    ccasVoiceCfgConnectionMode
        ACCESS       not-implemented
        DESCRIPTION  "Not supported."

        VARIATION    ccasVoiceCfgConnectionNumber
        ACCESS       not-implemented
        DESCRIPTION  "Not supported."

        VARIATION    ccasVoiceCfgNoiseRegEnable
        DEFVAL       { true } 
        DESCRIPTION  "The initial value is 'true'."

        VARIATION    ccasVoiceCfgNonLinearProcEnable
        DEFVAL       { true } 
        DESCRIPTION  "The initial value is 'true'."

        VARIATION    ccasVoiceCfgMusicOnHoldThreshold
        SYNTAX       Integer32 (-60..-30)
        DEFVAL       { -38 } 
        DESCRIPTION  "Limited data range supported by VXSM.
                      The initial value is -38."

        VARIATION    ccasVoiceCfgInGain
        DEFVAL       { 0 } 
        DESCRIPTION  "The initial value is 0."

        VARIATION    ccasVoiceCfgOutAttn
        DEFVAL       { 0 } 
        DESCRIPTION  "The initial value is 0."

        VARIATION    ccasVoiceCfgEchoCancelEnable
        DEFVAL       { true } 
        DESCRIPTION  "The initial value is 'true'."

        VARIATION    ccasVoiceCfgEchoCancelCoverage
        DEFVAL       { echoCanceller128ms }
        DESCRIPTION  "The initial value is 'echoCanceller128ms'."

        VARIATION    ccasVoiceCfgInitialDigitTimeOut
        DEFVAL       { 10 }
        DESCRIPTION  "The initial value is 10."

        VARIATION    ccasVoiceCfgInterDigitTimeOut
        DEFVAL       { 10 }
        DESCRIPTION  "The initial value is 10."

        VARIATION    ccasVoiceCfgRegionalTone
        DESCRIPTION  "Support the following regional tones -
                         AR: Argentina
                         AU: Australia
                         BE: Belgium
                         BR: Brazil
                         CA: Canada
                         CH: Switzerland
                         CN: China
                         CY: Cyprus
                         CZ: Czech
                         DK: Denmark
                         DE: Germany
                         EG: Egypt
                         ES: Spain
                         FI: Finland
                         FR: France
                         GB: United Kingdom
                         GH: Ghana
                         GR: Greece
                         HK: Hong Kong
                         HU: Hungary
                         ID: Indonesia
                         IE: Ireland
                         IL: Israel
                         IN: India
                         IS: Iceland
                         IT: Italy
                         JP: Japan
                         JO: Jordan
                         KE: Kenya
                         KR: Korea
                         LB: Lebanon
                         LU: Luxembourg
                         MY: Malaysia
                         MX: Mexico
                         NG: Nigeria
                         NL: Netherlands
                         NO: Norway
                         NP: Nepal
                         NZ: New Zealand
                         PA: Panama
                         PK: Pakistan
                         PH: Philippines
                         PL: Poland
                         PT: Portugal
                         RU: Russian
                         SA: Saudi Arab
                         SG: Singapore
                         SK: Slovakia
                         SI: Slovenia
                         SE: Sweden
                         ZA: S. Africa
                         TH: Thailand
                         TR: Turkey
                         US: USA
                         ZW: Zimbabwe"

    ::= { ciscoCasIfCapability 2 }

ciscoCasIfCapabilityV12R04TPC3xxx AGENT-CAPABILITIES
    PRODUCT-RELEASE "CISCO IOS 12.4T for Integrate Service
                     Router (ISR) c2xxx and c3xxx platforms."
    STATUS          current
    DESCRIPTION
        "CISCO-CAS-IF-MIB Capabilities"

    SUPPORTS        CISCO-CAS-IF-MIB
    INCLUDES        {
                        ccasGeneralInfoGroupRev1,
                        ccasIfDS1Group, ccasEMGroupRev2,
                        ccasLineGroup,
                        ccasCustomABCDGroup, ccasChannelInfoGroup
                    }
    VARIATION  ccasGrpCfgServiceType
    ACCESS      read-only
    DESCRIPTION "create/write access is not implemented."

                       
    VARIATION   ccasGrpCfgType
    SYNTAX      INTEGER {
                emWinkStart(1), emWinkStartFgd(2),emImmedStart(3),
                fxsLoopStart(5), fxsGroundStart(6),
                sasLoopStart(7), sasGroundStart(8),
                r2Analog(9), r2Digital(10), r2Pulse(11),p7(12),
                fxoLoopStart(13), fxoGroundStart(14),
                extsig(26), emLmr(27)
                }
    ACCESS      read-only
    DESCRIPTION "create/write access is not implemented. Only a
                 limited set of enumerated values is supported"

    VARIATION   ccasGrpCfgDs0Channels
    ACCESS      read-only
    DESCRIPTION "create/write access is not implemented"

    VARIATION   ccasGrpCfgRowStatus
    ACCESS      read-only
    DESCRIPTION "create/write access is not implemented"

    VARIATION   ccasGrpEMCfgDialType
    ACCESS      read-only
    DESCRIPTION "write access is not implemented"

    VARIATION   ccasGrpEMCfgDnisAni
    ACCESS      read-only
    DESCRIPTION "write access is not implemented"

    VARIATION   ccasGrpEMTmClearWaitDuration
    ACCESS      not-implemented
    DESCRIPTION "this object is not supported"

    VARIATION   ccasGrpEMTmMaxWinkWaitDuration
    ACCESS      read-only
    DESCRIPTION "write access is not supported"

    VARIATION   ccasGrpEMTmMaxWinkDuration
    ACCESS      read-only
    DESCRIPTION "write access is not supported"

    VARIATION   ccasGrpEMTmDelayStart
    ACCESS      not-implemented
    DESCRIPTION "this object is not supported"

    VARIATION   ccasGrpEMTmMaxDelayDuration
    ACCESS       not-implemented
    DESCRIPTION "this object is not supported"

    VARIATION   ccasGrpEMTmMinDelayPulseWidth
    ACCESS      not-implemented
    DESCRIPTION "this object is not supported"

    VARIATION   ccasGrpEMTmDigitDuration
    ACCESS      read-only
    DESCRIPTION "write access is not supported"

    VARIATION   ccasGrpEMTmInterDigitDuration
    ACCESS      read-only
    DESCRIPTION "write access is not supported"

    VARIATION   ccasGrpEMTmPulseRate
    ACCESS      not-implemented
    DESCRIPTION "this object is not supported"

    VARIATION   ccasGrpEMTmPulseInterDigitDuration
    ACCESS      not-implemented
    DESCRIPTION "this object is not supported"

    VARIATION   ccasGrpLineCfgNumberRings
    ACCESS      read-only
    DESCRIPTION "write access is not supported"

    VARIATION   ccasGrpLineCfgSupDisconnect
    ACCESS      read-only
    DESCRIPTION "write access is not supported"

    VARIATION   ccasGrpLineCfgDialType
    ACCESS      read-only
    DESCRIPTION "write access is not supported"

    VARIATION   ccasGrpLineTmDigitDuration
    ACCESS      read-only
    DESCRIPTION "write access is not supported"

    VARIATION   ccasGrpLineTmInterDigitDuration
    ACCESS      read-only
    DESCRIPTION "write access is not supported"

    VARIATION   ccasGrpLineTmPulseRate
    ACCESS      not-implemented
    DESCRIPTION "this object is not supported"

    VARIATION   ccasGrpLineTmPulseInterDigitDuration
    ACCESS      not-implemented
    DESCRIPTION "this object is not supported"

    VARIATION   ccasGrpABCDCfgInvertBits
    ACCESS      read-only
    DESCRIPTION "write access is not supported"

    VARIATION   ccasGrpABCDCfgUnusedBits
    ACCESS      read-only
    DESCRIPTION "write access is not supported"

    VARIATION   ccasChannelCfgBusyOut
    ACCESS      read-only
    DESCRIPTION "write access is not supported"

    VARIATION   ccasGrpEMCfgLmrMCap
    ACCESS      read-only
    DESCRIPTION "write access is not supported"

    VARIATION   ccasGrpEMCfgLmrECap
    ACCESS      read-only
    DESCRIPTION "write access is not supported"


    ::= { ciscoCasIfCapability 3 }

END








