-- ****
-- *------------------------------------------------------------------
-- * CISCO-SCAS-BB-MIB.my:  Main SNMP MIB for Cisco SCAS BB.
-- *
-- * PCube was acquired by Cisco Systems on August 23, 2004 
-- *
-- * Copyright (c) May 2006 by Cisco Systems, Inc.
-- * All rights reserved.
-- * Author: Guy Keinan
-- *------------------------------------------------------------------
-- ****


CISCO-SCAS-BB-MIB DEFINITIONS ::= BEGIN


IMPORTS
    pcubeWorkgroup, pcubeModules
        FROM PCUBE-SMI
    linkModuleIndex, linkIndex, spvIndex, pmoduleIndex
                FROM PCUBE-SE-MIB
    MODULE-IDENTITY, OBJECT-TYPE, Counter32,Integer32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,OBJECT-GROUP
        FROM SNMPv2-CONF
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB;

        
pcubeEngageMIB  MODULE-IDENTITY
    LAST-UPDATED "200605100000Z"
    ORGANIZATION "Cisco Systems, Inc."
    CONTACT-INFO
                 "Cisco Systems
                  Customer Service
                  
           Postal: 170 W Tasman Drive
                   San Jose, CA  95134
                   USA

              Tel: +1 800 553-NETS

           E-mail: cs-sce@cisco.com"
    DESCRIPTION 
        "Main SNMP MIB for Cisco SCAS BB application
        which runs over Service Control Engine devices."
        
    REVISION    "200605100000Z"     
    DESCRIPTION 
        "MIB revised as a part of integration into
         Cisco SNMP MIB standard.
         Changed contacts,
         Added OBJECT-GROUPS,
         Added MODULE-COMPLIANCE."
        
    REVISION    "200412210000Z"     
    DESCRIPTION 
        "Main SNMP MIB for P-cube's Engage Applictaion, 
        revised for Engage 2.5."
        
    REVISION    "200407010000Z"     
    DESCRIPTION 
        "Main SNMP MIB for P-cube's Engage Applictaion."
        
    REVISION    "200207032000Z"     
    DESCRIPTION 
        "This MIB provides runtime status and monitoring 
        capabilities for the SCAS BB application."
    ::= { pcubeModules 4 }


pcubeEngageObjs           OBJECT IDENTIFIER ::= { pcubeWorkgroup 2 }
pcubeEngageConformance    OBJECT IDENTIFIER ::= { pcubeEngageMIB 3 }
pcubeEngageGroups         OBJECT IDENTIFIER 
                               ::= { pcubeEngageConformance 1 }
-- Compliances to the SNMP agents running SCABB application
pcubeEngageCompliances    OBJECT IDENTIFIER 
                                ::= { pcubeEngageConformance 2 }

--
-- GenericApp Objects
--
serviceGrp              OBJECT IDENTIFIER ::= { pcubeEngageObjs 1 }
linkGrp                 OBJECT IDENTIFIER ::= { pcubeEngageObjs 2 }
packageGrp              OBJECT IDENTIFIER ::= { pcubeEngageObjs 3 }
subscriberGrp           OBJECT IDENTIFIER ::= { pcubeEngageObjs 4 }
serviceCounterGrp       OBJECT IDENTIFIER ::= { pcubeEngageObjs 5 }
             
--
-- Service group
--

--  OBJECT-TYPE which is a leaf cannot have 'not-accessible' 
-- access according to SMICNG
--  Thus we removed it and declared an OBJECT IDENTIFIER instead.
--serviceTable OBJECT-TYPE
--        SYNTAX        Counter32 
--        MAX-ACCESS    not-accessible
--        STATUS        deprecated
--        DESCRIPTION   "The Service table is no longer supported, the 
--                       Tables in the Counter group are used instead."
--        ::= { serviceGrp 1 }
serviceTable OBJECT IDENTIFIER ::= { serviceGrp 1 }

--
-- Link group
--

-- Link counter table
linkServiceUsageTable OBJECT-TYPE
        SYNTAX        SEQUENCE OF LinkServiceUsageEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "The Link Service-usage table provides
            information per link per global-scope
            service-counter."
        ::= { linkGrp 1 }

linkServiceUsageEntry OBJECT-TYPE
        SYNTAX        LinkServiceUsageEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "A linkServiceUsageTable entry."
        INDEX         { linkModuleIndex,
                        linkIndex,
                        globalScopeServiceCounterIndex 
                       }
        ::= { linkServiceUsageTable 1 }
     
LinkServiceUsageEntry ::=
    SEQUENCE {
            linkServiceUsageUpVolume            Counter32,
            linkServiceUsageDownVolume          Counter32,
            linkServiceUsageNumSessions         Counter32,
            linkServiceUsageDuration            Counter32,
            linkServiceUsageConcurrentSessions  Counter32,
            linkServiceUsageActiveSubscribers   Counter32,
            linkServiceUpDroppedPackets         Counter32,
            linkServiceDownDroppedPackets       Counter32,
            linkServiceUpDroppedBytes           Counter32,
            linkServiceDownDroppedBytes         Counter32
            }

        
linkServiceUsageUpVolume OBJECT-TYPE
        SYNTAX        Counter32 
        UNITS         "KBytes"  
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The link service-counter upstream volume."
        ::= { linkServiceUsageEntry 1 }

linkServiceUsageDownVolume OBJECT-TYPE
        SYNTAX        Counter32 
        UNITS         "KBytes" 
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The link service-counter downstream volume."
        ::= { linkServiceUsageEntry 2 }

linkServiceUsageNumSessions OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "sessions"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The link service-counter."
        ::= { linkServiceUsageEntry 3 }

linkServiceUsageDuration OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "seconds"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The link service-counter aggregated 
            session duration."
        ::= { linkServiceUsageEntry 4 }

linkServiceUsageConcurrentSessions OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "sessions"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The link service-counter concurrent sessions."
        ::= { linkServiceUsageEntry 5 }

linkServiceUsageActiveSubscribers OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "subscribers"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The link service-counter amount of active
            subscribers."
        ::= { linkServiceUsageEntry 6 }

linkServiceUpDroppedPackets  OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "packets"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The link service-counter number of dropped
            packets on the upstream, when accelerate 
            packet drop is enabled this counter will 
            always return 0xFFFFFFFF."
        ::= { linkServiceUsageEntry 7 }

linkServiceDownDroppedPackets  OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "packets"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The link service-counter number of dropped
            packets on the downstream when accelerate 
            packet drop is enabled this counter will 
            always return 0xFFFFFFFF."
        ::= { linkServiceUsageEntry 8 }

linkServiceUpDroppedBytes  OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "bytes"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The link service-counter number of dropped
            bytes on the upstream when accelerate packet 
            drop is enabled this counter will always 
            return 0xFFFFFFFF."
        ::= { linkServiceUsageEntry 9 }

linkServiceDownDroppedBytes  OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "bytes"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The link service-counter number of dropped 
            bytes on the downstream when accelerate packet
            drop is enabled this counter will always 
            return 0xFFFFFFFF."
        ::= { linkServiceUsageEntry 10 }

--
-- Package group
--

-- Package table
packageCounterTable OBJECT-TYPE
        SYNTAX        SEQUENCE OF PackageCounterEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "This table provides information per each
            package-counter configured into the system."
        ::= { packageGrp 1 }

packageCounterEntry OBJECT-TYPE
        SYNTAX        PackageCounterEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "A packageCounterTable entry."
        INDEX         { pmoduleIndex, packageCounterIndex }
        ::= { packageCounterTable 1 }
     
PackageCounterEntry ::=
    SEQUENCE {
            packageCounterIndex             Integer32,
            packageCounterStatus            INTEGER,
            packageCounterName              SnmpAdminString,
            packageCounterActiveSubscribers Counter32 
              }

packageCounterIndex OBJECT-TYPE
        SYNTAX        Integer32 (1..255)
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "The package-counter index."
        ::= { packageCounterEntry 1 }

packageCounterStatus OBJECT-TYPE
        SYNTAX        INTEGER {
                                disabled(0),     
                                enabled(1) 
                                }
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The package-counter status."   
    ::= { packageCounterEntry 2 }


packageCounterName OBJECT-TYPE
        SYNTAX        SnmpAdminString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The name of the package-counter."
        ::= { packageCounterEntry 3 }

packageCounterActiveSubscribers OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The total amount of active subscribers of the
            package-counter."
        ::= { packageCounterEntry 4 }


-- Package service-usage table
packageServiceUsageTable OBJECT-TYPE
        SYNTAX        SEQUENCE OF PackageServiceUsageEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "The Package Service Usage table contains 
            counters per package-counter per global-scope
            service-counter."
        ::= { packageGrp 2 }

packageServiceUsageEntry OBJECT-TYPE
        SYNTAX        PackageServiceUsageEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "A packageServiceUsageTable entry."
        INDEX         {  pmoduleIndex,
                         packageCounterIndex,
                         globalScopeServiceCounterIndex }
        ::= { packageServiceUsageTable 1 }
     
PackageServiceUsageEntry ::=
    SEQUENCE {
            packageServiceUsageUpVolume             Counter32,
            packageServiceUsageDownVolume           Counter32,
            packageServiceUsageNumSessions          Counter32,
            packageServiceUsageDuration             Counter32,
            packageServiceUsageConcurrentSessions   Counter32,
            packageServiceUsageActiveSubscribers    Counter32,
            packageServiceUpDroppedPackets          Counter32,
            packageServiceDownDroppedPackets        Counter32,
            packageServiceUpDroppedBytes            Counter32,
            packageServiceDownDroppedBytes          Counter32 
            }

packageServiceUsageUpVolume OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "KBytes"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The package-counter service-counter upstream
            volume."
        ::= { packageServiceUsageEntry 1 }

packageServiceUsageDownVolume OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "KBytes"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The package-counter service-counter downstream
            volume."
        ::= { packageServiceUsageEntry 2 }

packageServiceUsageNumSessions OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "sessions"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The package-counter service-counter 
            number of sessions."
        ::= { packageServiceUsageEntry 3 }

packageServiceUsageDuration OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "seconds"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The package-counter service-counter aggregated 
            session duration."
        ::= { packageServiceUsageEntry 4 }

packageServiceUsageConcurrentSessions OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "sessions"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The package-counter service-counter 
            concurrent sessions."
        ::= { packageServiceUsageEntry 5 }

packageServiceUsageActiveSubscribers OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "subscribers"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The package-counter service-counter amount of 
            active subscribers."
        ::= { packageServiceUsageEntry 6 }

packageServiceUpDroppedPackets  OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "packets"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The package-counter service number of dropped
            packets on the upstream when accelerate packet
            drop is enabled this counter will always return
            0xFFFFFFFF."
        ::= { packageServiceUsageEntry 7 }

packageServiceDownDroppedPackets  OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "packets"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The package-counter service number of dropped
            packets on the downstream when accelerate
            packet drop is enabled this counter will always
            return 0xFFFFFFFF."
        ::= { packageServiceUsageEntry 8 }

packageServiceUpDroppedBytes  OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "bytes"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The package-counter service number of dropped
            bytes on the upstream when accelerate packet 
            drop is enabled this counter will always return
            0xFFFFFFFF."
        ::= { packageServiceUsageEntry 9 }

packageServiceDownDroppedBytes  OBJECT-TYPE
        SYNTAX        Counter32
        UNITS         "bytes"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The package-counter service number of dropped 
            bytes on the downstream when accelerate packet
            drop is enabled this counter will always return
            0xFFFFFFFF."
        ::= { packageServiceUsageEntry 10 }

--
-- Subscriber group
--


-- Subscribers table
subscribersTable OBJECT-TYPE
        SYNTAX        SEQUENCE OF SubscribersEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "This table provides information for 
            each subscriber."
        ::= { subscriberGrp 1 }

subscribersEntry OBJECT-TYPE
        SYNTAX        SubscribersEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "A subscribersTable entry."
        INDEX         { pmoduleIndex, spvIndex }
        ::= { subscribersTable 1 }
     
SubscribersEntry ::=
    SEQUENCE {
            subscriberPackageIndex              Integer32
            }

subscriberPackageIndex OBJECT-TYPE
        SYNTAX        Integer32 (1..255)
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The subscriber package index."
        ::= { subscribersEntry 1 }



-- Subscribers service-usage table
subscriberServiceUsageTable OBJECT-TYPE
        SYNTAX        SEQUENCE OF SubscriberServiceUsageEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "This table provides information for each 
            subscriber for each subscriber-scope 
            service-counter."
        ::= { subscriberGrp 2 }

subscriberServiceUsageEntry OBJECT-TYPE
        SYNTAX        SubscriberServiceUsageEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "A subscriberServiceUsageTable entry."
        INDEX         { pmoduleIndex,
                        spvIndex, 
                        subscriberScopeServiceCounterIndex }
        ::= { subscriberServiceUsageTable 1 }
     
SubscriberServiceUsageEntry ::=
    SEQUENCE {
            subscriberServiceUsageUpVolume              Counter32,
            subscriberServiceUsageDownVolume            Counter32,
            subscriberServiceUsageNumSessions           Integer32,
            subscriberServiceUsageDuration              Integer32
            }

subscriberServiceUsageUpVolume OBJECT-TYPE
        SYNTAX        Counter32 
        UNITS         "KBytes"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The upstream volume."
        ::= { subscriberServiceUsageEntry 1 }

subscriberServiceUsageDownVolume OBJECT-TYPE
        SYNTAX        Counter32 
        UNITS         "KBytes"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The downstream volume."
        ::= { subscriberServiceUsageEntry 2 }

subscriberServiceUsageNumSessions OBJECT-TYPE
        SYNTAX        Integer32 (0..65535)
        UNITS         "sessions"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The number of sessions."
        ::= { subscriberServiceUsageEntry 3 }

subscriberServiceUsageDuration OBJECT-TYPE
        SYNTAX        Integer32 (0..65535)
        UNITS         "seconds"
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "Aggregated session duration."
        ::= { subscriberServiceUsageEntry 4 }

--
-- Service Counter group
--
globalScopeServiceCounterTable OBJECT-TYPE
        SYNTAX        SEQUENCE OF GlobalScopeServiceCounterEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "The Global-scope Service-counter table 
            consists of data regarding each service-counter
            configured into the system, used by the link 
            and package entries."
        ::= { serviceCounterGrp 1 }

globalScopeServiceCounterEntry OBJECT-TYPE
        SYNTAX        GlobalScopeServiceCounterEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "A globalScopeServiceCounterEntry entry."
        INDEX         { pmoduleIndex, globalScopeServiceCounterIndex }
        ::= { globalScopeServiceCounterTable 1 }
     
GlobalScopeServiceCounterEntry ::=
    SEQUENCE {
            globalScopeServiceCounterIndex       Integer32,
            globalScopeServiceCounterStatus      INTEGER,
            globalScopeServiceCounterName        SnmpAdminString
            }

globalScopeServiceCounterIndex OBJECT-TYPE
        SYNTAX        Integer32 (1..255)
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "The global-scope service-counter index."
        ::= { globalScopeServiceCounterEntry 1 }

globalScopeServiceCounterStatus OBJECT-TYPE
        SYNTAX        INTEGER {
                                disabled(0),     
                                enabled(1) 
                              }
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The global-scope service-counter status."   
    ::= { globalScopeServiceCounterEntry 2 }

globalScopeServiceCounterName OBJECT-TYPE
        SYNTAX        SnmpAdminString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The name of the global-scope service-counter."
        ::= { globalScopeServiceCounterEntry 3 }


subscriberScopeServiceCounterTable OBJECT-TYPE
        SYNTAX        SEQUENCE OF SubscriberScopeServiceCounterEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "The Subscriber-Scope Service-counter table
            consists of data regarding each service-counter
            definition configured into the system,
            used by the subscriber entries."
        ::= { serviceCounterGrp 2 }

subscriberScopeServiceCounterEntry OBJECT-TYPE
        SYNTAX        SubscriberScopeServiceCounterEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "A subscriberScopeServiceCounterEntry entry."
        INDEX         { pmoduleIndex, 
                        subscriberScopeServiceCounterIndex }
        ::= { subscriberScopeServiceCounterTable 1 }
     
SubscriberScopeServiceCounterEntry ::=
    SEQUENCE {
            subscriberScopeServiceCounterIndex          Integer32,
            subscriberScopeServiceCounterStatus         INTEGER,
            subscriberScopeServiceCounterName           SnmpAdminString 
            }

subscriberScopeServiceCounterIndex OBJECT-TYPE
        SYNTAX        Integer32 (1..255)
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   
            "The subscriber-scope service-counter index."
        ::= { subscriberScopeServiceCounterEntry 1 }

subscriberScopeServiceCounterStatus OBJECT-TYPE
        SYNTAX        INTEGER {
                disabled(0),     
                enabled(1) 
                                }
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The subscriber-scope service-counter status."
    ::= { subscriberScopeServiceCounterEntry 2 }

subscriberScopeServiceCounterName OBJECT-TYPE
        SYNTAX        SnmpAdminString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   
            "The name of the subscriber-scope 
            service-counter."
        ::= { subscriberScopeServiceCounterEntry 3 }


--Compliances
pcubeEngageCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "A compliance statement defined in this MIB module,
             for SCABB SNMP agents."
    MODULE  -- this module
    -- Currently all groups are mandatory.
    MANDATORY-GROUPS {  
        pcubeLinkGroup,
        pcubePackageGroup,
        pcubeSubscriberGroup,
        pcubeServiceCounterGroup }
    ::= { pcubeEngageCompliances 1 }     
    
pcubeLinkGroup        OBJECT-GROUP
    OBJECTS { 
        linkServiceUsageUpVolume,
        linkServiceUsageDownVolume,
        linkServiceUsageNumSessions,
        linkServiceUsageDuration,
        linkServiceUsageConcurrentSessions,
        linkServiceUsageActiveSubscribers,
        linkServiceUpDroppedPackets,
        linkServiceDownDroppedPackets,
        linkServiceUpDroppedBytes,
        linkServiceDownDroppedBytes }
    STATUS current
    DESCRIPTION 
        "Link related inforamtion."
    ::= { pcubeEngageGroups 2 }
                
pcubePackageGroup OBJECT-GROUP
    OBJECTS { 
        packageCounterStatus,
        packageCounterName,
        packageCounterActiveSubscribers,
        packageServiceUsageUpVolume,
        packageServiceUsageDownVolume,
        packageServiceUsageNumSessions,
        packageServiceUsageDuration,
        packageServiceUsageConcurrentSessions,
        packageServiceUsageActiveSubscribers,
        packageServiceUpDroppedPackets,
        packageServiceDownDroppedPackets,
        packageServiceUpDroppedBytes,
        packageServiceDownDroppedBytes }
    STATUS  current
    DESCRIPTION 
        "Package related information."
    ::= { pcubeEngageGroups 3 }

pcubeSubscriberGroup OBJECT-GROUP
    OBJECTS { 
        subscriberPackageIndex,
        subscriberServiceUsageUpVolume,
        subscriberServiceUsageDownVolume,
        subscriberServiceUsageNumSessions,
        subscriberServiceUsageDuration }
    STATUS  current
    DESCRIPTION 
        "Subscriber related information."
    ::= { pcubeEngageGroups 4 }

pcubeServiceCounterGroup OBJECT-GROUP
    OBJECTS { 
        globalScopeServiceCounterStatus,
        globalScopeServiceCounterName,
        subscriberScopeServiceCounterStatus,
        subscriberScopeServiceCounterName }
    STATUS current
    DESCRIPTION 
        "Service related information."
    ::= { pcubeEngageGroups 5 }
    
END


