-- *****************************************************************
-- CISCO-IP-RAN-BACKHAUL-MIB: MIB for providing information and
-- measurements on backhaul traffic used by the Cisco IP Radio
-- Access Network Transport optimization.
--   
-- July 2005 John Linton
--   
-- Copyright (c) 2004-2007, 2009-2010 by Cisco Systems Inc.
-- All rights reserved.
-- ****************************************************************

CISCO-IP-RAN-BACKHAUL-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-COMPLIANCE,
    NOTIFICATION-GROUP,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    Counter32,
    Integer32,
    Unsigned32,
    MODULE-IDENTITY,
    NOTIFICATION-TYPE,
    OBJECT-TYPE
        FROM SNMPv2-SMI
    InetAddressType,
    InetAddress,
    InetPortNumber
        FROM INET-ADDRESS-MIB
    ifDescr,
    ifIndex,
    InterfaceIndex,
    InterfaceIndexOrZero
        FROM IF-MIB
    PerfIntervalCount,
    PerfCurrentCount
        FROM PerfHist-TC-MIB
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    AutonomousType,
    TimeStamp,
    TruthValue,
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    ciscoMgmt
        FROM CISCO-SMI;


ciscoIpRanBackHaulMIB MODULE-IDENTITY
    LAST-UPDATED    "201005040000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems, Inc
            Customer Service

            Postal: 170 W. Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-ran-o@cisco.com"
    DESCRIPTION
        "This MIB provides information on the IP-RAN traffic
        from cell site to aggregation site in the following
        situations.  In an GSM environment the cell site will
        be the Base station Transceiver System(BTS) and the
        aggregation site will be the Base Station
        Controller(BSC).  In the UMTS environment the cell
        site will be the B-Node and the aggregation site will
        Radio Network Controller(RNC).



        There are two typical type backhaul, also know
        as longhaul, links.  The traditional backhaul
        connection consists of a PPP multilink containing two
        or more E1 or T1 links or ATM or ATM/IMA.  The
        alternate backhaul is traffic transported using
        IP cloud.


        Simple back-to-back configuration
        ---------------------------------
           This setup consists of two devices that
           support a limited number of GSM and UMTS links.
           They are deployed in pairs and inserted between
           the existing BTS device and BSC device.

               BTS site               BSC site

           GSM-Abis                           GSM-Abis
           ----||||||||    Backhaul   ||||||||----
           ----|      |---------------|      |----
           ----|      |---------------|      |----
               ||||||||               ||||||||

               RNC  B-Node site       RNC

           UMTS                                UMTS
           ----||||||||    Backhaul   ||||||||----
           ----|      |---------------|      |----
           ----|      |---------------|      |----
               ||||||||               ||||||||
                  |                       |
                  |-----------------------|
                   Alternate backhaul over
                   IP cloud


        Aggregate node configuration
        ----------------------------
        This configuration consists of one aggregate node
        located at BSC site and several devices at BTS
        sites. The aggregate device has a seperate backhaul
        link to each BTS site.

            BTS site                BSC site

                                   Aggregate
        GSM                                GSM
        ----||||||||    Backhaul   ||||||||----
        ----|      |---------------|      |----
        ----|      |---------------|      |----
            ||||||||               |      |
               .                   |      | .
               .                   |      | .
        GSM    .                   |      | .
        ----||||||||    Backhaul   |      |----
        ----|      |---------------|      |----
        ----|      |---------------|      |----
            ||||||||               ||||||||


             RNC                   B-Node
        UMTS                                UMTS
        ----||||||||    Backhaul   ||||||||----
        ----|      |---------------|      |----
        ----|      |---------------|      |----
            ||||||||               |      |
               |     Alternate     |      |
               |        ....       |      |
               -------.      .     |      |
                      . IP   .     |      |
                      . Cloud.-----|      |
                      .      .     |      |
               -------.      .     |      |
               |       ......      |      |
               |    Backhaul       |      |
        UMTS   |                   |      |
        ----||||||||    Backhaul   |      |----
        ----|      |---------------|      |----
        ----|      |---------------|      |----
            ||||||||               ||||||||


                           Compression
                           Multiplexing
                               |
        BSC <---------->||||||||  V   ||||||||<---------->BTS
             . GSM    . |      |<---->|      | . GSM    .
             . A(bis) . |      |<---->|      | . A(bis) .
            <---------->||||||||      ||||||||<---------->
                 A                A
                 |                |
            ShortHaul         BackHaul

            Multiple E1/T1 Back Haul Links

        Entries in these tables cannot be created or deleted
        by the network management system.  All entries are
        created or deleted by the agent.

        Shorthaul interfaces support the following protocols.

        Protocol    ifType
        --------    ----------------------------
        GSM-Abis    propPointToPointSerial(22)
        UMTS-iub    atm(37)
        UMTS/IMA    atmSubInterface(134)
                   aal5(49)
        ifType.44 = atmIma(107)


        The following list provides the currently allowed
        backhaul interfaces types.  Additional interfaces
        types will be added as they are supported.

        ifType
        ---------------------------
        ethernetCsmacd(6)
        ppp(23) as Multilink bundle
        pppMultilinkBundle(108)


        In order to manage the IP-RAN optimization solution, two
        key factors must be monitored. The first and most
        important is the amount of traffic sent over the backhaul
        interface.  The second is compression efficiency which has
        a direct impact amount of traffic placed backhaul link.

        MIB Structure
        -------------
        The MIB has the following structure.

        Shorthaul information tables:
         cirbhInfoTable

        Shorthaul Alarm Information tables
         cirbhGsmAlarmTable
         cirbhUmtsConnectionTable
         cirbhUmtsAlarmTable

        Shorthaul statistics tables
         cirbhStatsTable
         cirbhErrorsTable(deprecated)
         cirbhShortHaulHistoryTable(obsolete)
         cirbhCongestionTable
         cirbhGsmErrorsTable(replaces cirbhErrorsTable)
         cirbhUmtsErrorsTable(replaces cirbhErrorsTable)

        Backhaul information tables
         cirbhBackHaulTable(obsolete)

        Backhaul statistics tables
         cirbhBackHaulHistoryTable(obsolete)
         cirbhBackHaulStatsTable(obsolete)
         cirbhBackHaulStatsHistoryTable(deprecated)

        Abbreviations:
            A-bis   Interface between BSC and BTS
            AAL2    ATM Adaptation Layer type 2
            AAL5    ATM Adaptation Layer type 5
            AIM     Advanced Interface Module
            AgNode  Aggregation Node
            ALCAP   Access Link Control Application Part
            AMR     Adaptive Multi-Rate speech codec
            ATM     Asynchronous Transfer Mode
            BCH     Broadcast Channel
            BSC     Base Station Controller.
            BTS     Base Station Transceiver System
            CDF     CID Definition Field
            CID     Channel IDentification
            CPCH    Common Packet Channel
            DCH     Dedicated Channel
            DSCH    Downlink Shared Channel
            DTX     Discontinuous Transmission (mechanism)
            FACH    Forward Link Access Channel
            GSM     Global System for Mobile communications
            IMA     Inverse Multiplexing for ATM
            Iub     Node B to RNC interface
            OC3     Optical Carrier 3
            OSF     OffSet Field
            LAPD    Link Access Protocol on Dm Channel
            O&M     Operations and Maintenance
            MLPPP   Multi-Link PPP
            MS      Mobile Station (Handset)
            NBAP    Node B Application Part
            NNI     Network to Network Interface
            Node-B  Node B
            PCH     Paging Channel
            PVC     Permanent Virtual Circuit
            RAN     Radio Access Network
            SVC     Switched Virtual Circuit
            RACH    Random Access Channel
            RNC     Radio Network Controller
            SAR     Segment Assembly Reassembly
            SDC     Traffic Channel
            SDH     Signaling Channel
            SPVC    Soft Permanent Virtual Circuit
            SSCOP   Service Specific Connection Oriented Protocol
            STC     Signaling Transport Converter
            STM-1   Synchronous Transport Module type 1
            TRAU    Transcoder Unit
            UMTS    Universal Mobile Telecommunications System
            UNI     User to Network Interface
            USCH    Uplink Shared Channel
            UTRAN   UMTS Terrestrial Radio Access Network
            VCI     Virtual Channel Identifier
            VPI     Virtual Path Identifier"
    REVISION        "201003240000Z"
    DESCRIPTION
        "The following tables are now obsolete and the
        information provided in them can be calculated using
        the objects in the cirbhShortHaulBulkTable.

        cirbhShortHaulHistoryTable
        cirbhBackHaulTable
        cirbhBackHaulShortHaulTable
        cirbhBackHaulHistoryTable
        cirbhBackHaulStatsTable
        cirbhBackHaulStatsHistoryTable

        The following scalars are no longer used
        in implementation of MIB.
        cirbhBackHaulStatsInterval
        cirbhBackHaulStatsEntries
        cirbhBackHaulAcceptableThreshold
        cirbhBackHaulWarningThreshold
        cirbhBackHaulOverloadedThreshold
        cirbhBackHaulUtilInterval
        cirbhUtilNotifEnabled

        The following notifications are now obsolete
        and not supported.

        ciscoIpRanBackHaulRcvdUtil
        ciscoIpRanBackHaulSentUtil

        Changes to Compliance and Conformance Statements

        Changed status to obsolete
        ciscoIpRanBackHaulMIBCompliance
        ciscoIpRanBackHaulMIBComplianceRev1
        ciscoIpRanBackHaulMIBComplianceRev2
        ciscoIpRanBackHaulShortHaulGroup
        ciscoIpRanBackHaulHistoryGroup
        ciscoIpRanBackHaulNotifGroup
        ciscoIpRanBackHaulHistoryGroupRev2

        Added following as active
        ciscoIpRanBackHaulMIBComplianceRev3
        ciscoIpRanBackHaulHistoryGroupRev3"
    REVISION        "200705300000Z"
    DESCRIPTION
        "Added the cirbhInfoOptimizeTraffic object to the
        cirbhInfoTable.
        Added OBJECT-GROUP ciscoIpRanBackHaulConfigGroupSup3 and
        MODULE-COMPLIANCE ciscoIpRanBackHaulMIBComplianceRev2."
    REVISION        "200608250000Z"
    DESCRIPTION
        "The following tables, objects and notifications have been
        deprecated.

        Scalars
          cirbhBackHaulStatsInterval
          cirbhBackHaulStatsEntries
          cirbhBackHaulAcceptableThreshold
          cirbhBackHaulWarningThreshold
          cirbhBackHaulOverloadedThreshold
          cirbhBackHaulUtilInterval
          cirbhUtilNotifEnabled

        cirbhErrorsTable
        cirbhBackHaulTable
        cirbhBackHaulShortHaulTable
        cirbhBackHaulHistoryTable
        cirbhBackHaulStatsTable
        cirbhBackHaulStatsHistoryTable

        The following tables and objects have been added.

        cirbhInfoTable
          cirbhInfoAdjectSerialNum
          cirbhInfoAdjectVendorType
          cirbhInfoBackhaulRxIfIndex
          cirbhInfoBackhaulTxIfIndex
          cirbhInfoShBulkLastIndex

        cirbhGsmErrorsTable
        cirbhUmtsErrorsTable
        cirbhCongestionTable
        cirbhShortHaulBulkTable"
    REVISION        "200510180000Z"
    DESCRIPTION
        "Added cirbhUmtsConnectionRootIfIndex object
        and cirbhBackHaulShortHaulTable."
    REVISION        "200509130000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 483 }


ciscoIpRanBackHaulMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoIpRanBackHaulMIB 0 }

ciscoIpRanBackHaulMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoIpRanBackHaulMIB 1 }

ciscoIpRanBackHaulMIBConform  OBJECT IDENTIFIER
    ::= { ciscoIpRanBackHaulMIB 2 }

cirbhScalars  OBJECT IDENTIFIER
    ::= { ciscoIpRanBackHaulMIBObjects 1 }

cirbhObjects  OBJECT IDENTIFIER
    ::= { ciscoIpRanBackHaulMIBObjects 2 }

cirbhNotifEnables  OBJECT IDENTIFIER
    ::= { ciscoIpRanBackHaulMIBObjects 3 }

cirbhShortHaul  OBJECT IDENTIFIER
    ::= { cirbhObjects 1 }

cirbhShortHaulInfo  OBJECT IDENTIFIER
    ::= { cirbhShortHaul 1 }

cirbhShortHaulAlarmInfo  OBJECT IDENTIFIER
    ::= { cirbhShortHaul 2 }

cirbhShortHaulStats  OBJECT IDENTIFIER
    ::= { cirbhShortHaul 3 }

cirbhBackHaul  OBJECT IDENTIFIER
    ::= { cirbhObjects 2 }

cirbhBackHaulInfo  OBJECT IDENTIFIER
    ::= { cirbhBackHaul 1 }

cirbhBackHaulStats  OBJECT IDENTIFIER
    ::= { cirbhBackHaul 2 }


-- *************************************************************
-- *                                                           *
-- * Textual Conventions                                       *
-- *                                                           *
-- *************************************************************

CirbhAlarmState ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Alarm states of local and remote interfaces.
        These states apply to both GSM and UMTS interfaces.

          'blue' - Indicates a problem at the remote end. The alarm
                   generate by the remote interface in the E1/T1 data
                   stream is sent and no other action is required.

          'green' - No alarm.

          'red' - Indicates local interface problem.
                  A-bis:
                  The interface has not received synchronization
                  from the GSM device. Device stops transmitting
                  backhaul samples.

          'yellow' - Indicates receive problem in the local device.
                  The remote device stops transmitting
                  backhaul data and indicates a blue alarm.

          'unavailable' - Indicates the alarms state is not available.
                  This state only applies to remote and occurs when
                  peer connection is inactive."
    SYNTAX          INTEGER  {
                        blue(1),
                        green(2),
                        red(3),
                        yellow(4),
                        unavailable(5)
                    }

CirbhBackHaulUtilization ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d"
    STATUS          current
    DESCRIPTION
        "A percentage representing the average utilization of
        backhaul interface."
    SYNTAX          Integer32 (0..100)

CirbhBackHaulUtilizationState ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "BackHaul Utilization State:

        'acceptable' - traffic for a specified direction is
                       at the acceptable level.

        'warning'    - traffic for a specified direction is
                       above acceptable level but below the
                       overloaded level.

        'overloaded' - traffic for a specified direction
                       has reached or exceeds overloaded level"
    SYNTAX          INTEGER  {
                        acceptable(1),
                        warning(2),
                        overloaded(3)
                    }

CirbhCommpressInterfaceRate ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d"
    STATUS          current
    DESCRIPTION
        "The traffic rate of data received from GSM or UMTS interface
        after data has been compressed. The transmission compressed
        interface rate is calculated after data compression and prior
        to transmission on backhaul. The receive compression
        interface rate is calculated after data is received and prior
        to decompression."
    SYNTAX          Unsigned32 (0..4294967295)

CirbhConnectGsmState ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The state of the GSM connection:

        'connected'      - The device is monitoring local and
                           remote alarm status.

        'disconnected'   - The system ignores the local alarm
                           status. The local transmitter on the
                           short-haul is disabled. Capability
                           messages are transmitted to the remote
                           describing the provisioning. The system
                           stays disconnected until the remote
                           capabilities are known and the peer
                           state is transitioned to connected.

        'sendConnect'    - One or more attempts have been made to
                           connect to remote peer.

        'recConnect'     - The local-peer has received a connect
                           request from the remote-peer.

        'connectedRej'   - Connection was rejected.

        'ackConnect'     - The initial connect request was sent
                           and acknowledged by remote-peer. The
                           local-peer is now waiting for a connect
                           request from the remote-peer.

        'connectedCheck' - The local-peer has reason to believe its
                           remote-peer has failed. Additional tests
                           are being processed to verify peer's
                           state."
    SYNTAX          INTEGER  {
                        connected(1),
                        disconnected(2),
                        sendConnect(3),
                        recConnect(4),
                        connectedRej(5),
                        ackConnect(6),
                        connectedCheck(7)
                    }

CirbhConnectUmtsState ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The state of the UMTS connection:

        'init'        - The connection is starting initialization
                        process.

        'starting'    - The shorthaul interface is administratively
                        active but the backhaul interface is down.

        'closed'      - The backhaul interface is active but
                        shorthaul is administratively closed.

        'stopped'     - Unable to connect to peer in specified time
                        interval. Additional attempts will be tried
                        based on peer request or restart timers.

        'closing'     - Connection closed by administration
                        request.

        'stopping'    - Connection shutdown by peer's Term-Request.
                        Will transition to stopped state.

        'connectSent' - Connection request sent to peer.

        'ackReceived' - Connection request sent and acknowledgement
                        has been received from peer. Now waiting
                        for peer's connection request.

        'ackSent'     - Connection request received and
                        acknowledgement has been sent to peer.
                        Connection request sent and waiting for
                        peer's acknowledgement.

        'open'        - Connection open and available for traffic."
    SYNTAX          INTEGER  {
                        init(1),
                        starting(2),
                        closed(3),
                        stopped(4),
                        closing(5),
                        stopping(6),
                        connectSent(7),
                        ackReceived(8),
                        ackSent(9),
                        open(10)
                    }

CirbhHistoryIndex ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d"
    STATUS          current
    DESCRIPTION
        "The system maintains a system wide counter that
        is incremented once a second. All tables that store
        historical informations should use the provided integer
        to that data from different tables can be easily compared
        and referenced. The implementations should ensure that
        the counters will not wrap and is only reset when device
        is reloaded."
    SYNTAX          Unsigned32 (1..4294967295)

CirbhProtocol ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The protocol used between BSC and BTS.

        'undefined' : Protocol not defined.

        'gsmAbis'   : Global System for Mobile communications
                      A-bis Interface between BSC and BTS.

        'umtsIub'   : Universal Mobile Telecommunications System
                      Node B to RNC interface."
    SYNTAX          INTEGER  {
                        undefined(1),
                        gsmAbis(2),
                        umtsIub(3)
                    }

CirbhRawInterfaceRate ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d"
    STATUS          current
    DESCRIPTION
        "The rate of traffic, in bits per second, on an interface in
        a particular direction prior to optimization for the
        following flows:

        Traffic received on UMTS or GSM-Abis interface
        prior to compression and placement on backhaul
        interface(Multilink).

        Traffic received from backhaul
        interface(Multilink) after decompression prior to
        transmittion on UMTS or GSM-Abis interface."
    SYNTAX          Unsigned32 (0..4294967295)

CirbhRedundancyState ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The Redundancy State of an interface. Used to
        indicate which device was current owner of
        interface.

           'active'       - Active owner of interface.

           'standby'      - Standby owner of interface."
    SYNTAX          INTEGER  {
                        active(1),
                        standby(2)
                    }

CirbhShortHaulUtilization ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d"
    STATUS          current
    DESCRIPTION
        "A percentage representing the average load over one
        second as a percent of E1 or T1."
    SYNTAX          Integer32 (0..255)

CirbhTrafficDirection ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Direction of traffic on an interface."
    SYNTAX          INTEGER  {
                        receive(1),
                        transmit(2)
                    }

CirbhTrafficType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The types of traffic on backhaul interface.

        'all'  - All types of traffic

        'gsm'  - Only GSM based traffic

        'umts' - Only UMTS based traffic"
    SYNTAX          INTEGER  {
                        all(1),
                        gsm(2),
                        umts(3)
                    }

-- *************************************************************
-- *                                                           *
-- * Scalars                                                   *
-- *                                                           *
-- *************************************************************

cirbhSnmpTrafficMode OBJECT-TYPE
    SYNTAX          INTEGER  {
                        undefined(1),
                        inBand(2),
                        outOfBand(3)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object describes the mode of SNMP traffic for this
        device in relationship to connectivity to network management
        station. This will be used to define default behavior for
        the device based on the on available bandwidth for
        management.

        'undefined' : Traffic mode is not defined.

        'inBand'    : SNMP traffic uses same physical interfaces as
                      voice traffic.

        'outOfBand' : SNMP traffic does not use same physical
                      interfaces as voice traffic." 
    ::= { cirbhScalars 1 }

cirbhLocation OBJECT-TYPE
    SYNTAX          INTEGER  {
                        undefined(1),
                        aggSite(2),
                        cellSite(3)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object provides information on location of
        the device to aid in topology display.

          'undefined' : not defined.

          'aggSite'   : Located at Base Station Controller or
                        or Radio Network Controller site.

          'cellSite'  : Located at Base Station Transceiver System
                        or Node B site." 
    ::= { cirbhScalars 2 }

cirbhBackHaulStatsInterval OBJECT-TYPE
    SYNTAX          Unsigned32 (60..3600)
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "The length of the interval used to collect statistics in the
        cirbhBackHaulStatsTable."
    DEFVAL          { 900 } 
    ::= { cirbhScalars 3 }

cirbhBackHaulStatsEntries OBJECT-TYPE
    SYNTAX          Unsigned32 (4..100)
    UNITS           "entries"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "The maximum number of entries in the cirbhBackHaulStatsTable
        table."
    DEFVAL          { 100 } 
    ::= { cirbhScalars 4 }

cirbhBackHaulAcceptableThreshold OBJECT-TYPE
    SYNTAX          Unsigned32 (20..100)
    UNITS           "percent"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object is used to specify a level of
        traffic below which the instances of the
        cirbhBackHaulRcvdUtilState and cirbhBackHaulSentUtilState
        objects are marked as 'acceptable'. All changes to this
        threshold will take effect at the end of the current
        interval. The value for this object must be less than
        the values specified by cirbhBackHaulOverloadedThreshold
        and cirbhBackHaulWarningThreshold objects."
    DEFVAL          { 60 } 
    ::= { cirbhScalars 5 }

cirbhBackHaulWarningThreshold OBJECT-TYPE
    SYNTAX          Unsigned32 (30..100)
    UNITS           "percent"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object is used to specify a level of
        traffic were the instances of the
        cirbhBackHaulRcvdUtilState and cirbhBackHaulSentUtilState
        objects are marked as 'warning'.  All changes to this
        threshold will take effect at the end of the current
        interval. The value for this object must be greater than
        the value specified for the cirbhBackHaulAcceptableThreshold
        object. Also, the value for this object must be less than or
        equal to value of the cirbhBackHaulOverloadedThreshold
        object."
    DEFVAL          { 70 } 
    ::= { cirbhScalars 6 }

cirbhBackHaulOverloadedThreshold OBJECT-TYPE
    SYNTAX          Unsigned32 (40..100)
    UNITS           "percent"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object is used to specify a level of
        traffic were the instances of the
        cirbhBackHaulRcvdUtilState and cirbhBackHaulSentUtilState
        objects are marked as 'overloaded'. Changes to this
        threshold will take effect at the end of the current
        interval. The value for this object must be greater than
        the value specified for the cirbhBackHaulAcceptableThreshold
        object. Also, the value for this object must be greater than
        or equal to value of the cirbhBackHaulWarningThreshold
        object.

        This object will be used to determine the state of the
        cirbhBackHaulRcvdUtilState and cirbhBackHaulSentUtilState
        objects."
    DEFVAL          { 80 } 
    ::= { cirbhScalars 7 }

cirbhBackHaulUtilInterval OBJECT-TYPE
    SYNTAX          Unsigned32 (0 | 60..3600)
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "The length of the interval used to suppress
        generation of the ciscoIpRanBackHaulRcvdUtil
        and ciscoIpRanBackHaulSentUtil notifications.
        Notification will not be suppressed when
        zero value is specified."
    DEFVAL          { 0 } 
    ::= { cirbhScalars 8 }
-- *************************************************************
-- *                                                           *
-- * Information Table                                         *
-- *                                                           *
-- *************************************************************

cirbhInfoTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhInfoTableEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides information on interface used to
        establish shorthaul connection to BTS or BSC or node
        B site."
    ::= { cirbhShortHaulInfo 1 }

cirbhInfoTableEntry OBJECT-TYPE
    SYNTAX          CirbhInfoTableEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry describes the information used to route
        GSM and UMTS packets across backhaul for a single
        GSM or UMTS link."
    INDEX           { ifIndex } 
    ::= { cirbhInfoTable 1 }

CirbhInfoTableEntry ::= SEQUENCE {
        cirbhInfoProtocol          CirbhProtocol,
        cirbhInfoLocalAddrType     InetAddressType,
        cirbhInfoLocalAddr         InetAddress,
        cirbhInfoLocalPortNumber   InetPortNumber,
        cirbhInfoRemoteAddrType    InetAddressType,
        cirbhInfoRemoteAddr        InetAddress,
        cirbhInfoRemotePortNumber  InetPortNumber,
        cirbhInfoAdjectSerialNum   SnmpAdminString,
        cirbhInfoAdjectVendorType  AutonomousType,
        cirbhInfoBackhaulRxIfIndex InterfaceIndexOrZero,
        cirbhInfoBackhaulTxIfIndex InterfaceIndexOrZero,
        cirbhInfoShBulkLastIndex   CirbhHistoryIndex,
        cirbhInfoOptimizeTraffic   TruthValue
}

cirbhInfoProtocol OBJECT-TYPE
    SYNTAX          CirbhProtocol
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Protocol used to indicate type of shorthaul."
    REFERENCE
        "GSM-Abis - 3GPP TS 08.60 V8.2.1 (Rel99) GSM A-bis
         specification for FR, EFR and AMR
              UMTS-Iub - 3GPP TS 25.302" 
    ::= { cirbhInfoTableEntry 1 }

cirbhInfoLocalAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The type of address specified in the corresponding instance
        of cirbhConfigLocalIpAddr object." 
    ::= { cirbhInfoTableEntry 2 }

cirbhInfoLocalAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The local address used to route traffic across backhaul." 
    ::= { cirbhInfoTableEntry 3 }

cirbhInfoLocalPortNumber OBJECT-TYPE
    SYNTAX          InetPortNumber
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The local port number used to distinguish traffic from this
        interface when transported over backhaul connection." 
    ::= { cirbhInfoTableEntry 4 }

cirbhInfoRemoteAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The type of address in the in the corresponding instance of
        the cirbhInfoRemoteAddr object." 
    ::= { cirbhInfoTableEntry 5 }

cirbhInfoRemoteAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The remote IP address used to route traffic across backhaul." 
    ::= { cirbhInfoTableEntry 6 }

cirbhInfoRemotePortNumber OBJECT-TYPE
    SYNTAX          InetPortNumber
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The remote port number used to distinguish traffic
        from this interface when transported over backhaul
        connection." 
    ::= { cirbhInfoTableEntry 7 }

cirbhInfoAdjectSerialNum OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides the serial number of the adjacent
        device supporting the other side of this shorthaul.  This object
        contains the same value as the corresponding
        entPhysicalSerialNum object on the adjacent device. The type of
        object like chassis or module is provided by the
        cirbhInfoAdjectVendorType object." 
    ::= { cirbhInfoTableEntry 8 }

cirbhInfoAdjectVendorType OBJECT-TYPE
    SYNTAX          AutonomousType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides the vendor type of the adjacent
        device supporting other end of this shorthaul.  This
        objectcontains the same value as the corresponding
        entPhysicalVendorType object on the adjacent device." 
    ::= { cirbhInfoTableEntry 9 }

cirbhInfoBackhaulRxIfIndex OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides the ifIndex of the interface
        used to receive traffic from destination." 
    ::= { cirbhInfoTableEntry 10 }

cirbhInfoBackhaulTxIfIndex OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides the ifIndex of the interface
        used to sent traffic to destination." 
    ::= { cirbhInfoTableEntry 11 }

cirbhInfoShBulkLastIndex OBJECT-TYPE
    SYNTAX          CirbhHistoryIndex
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The latest value of the cirbhShortHaulBulkHistory object
        from the cirbhShortHaulBulkHistory table." 
    ::= { cirbhInfoTableEntry 12 }

cirbhInfoOptimizeTraffic OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicate whether the traffic received and sent for
        this shorthaul interface is optimized." 
    ::= { cirbhInfoTableEntry 13 }
 

-- *************************************************************
-- *                                                           *
-- * GSM Alarm information                                     *
-- *                                                           *
-- *************************************************************

cirbhGsmAlarmTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhGsmAlarmTableEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides alarm information for GSM-Abis
        interfaces."
    ::= { cirbhShortHaulAlarmInfo 1 }

cirbhGsmAlarmTableEntry OBJECT-TYPE
    SYNTAX          CirbhGsmAlarmTableEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents the set of alarms that apply to
        GSM interface."
    INDEX           { ifIndex } 
    ::= { cirbhGsmAlarmTable 1 }

CirbhGsmAlarmTableEntry ::= SEQUENCE {
        cirbhGsmAlarmConnectState    CirbhConnectGsmState,
        cirbhGsmAlarmLocalState      CirbhAlarmState,
        cirbhGsmAlarmRemoteState     CirbhAlarmState,
        cirbhGsmAlarmRedundancyState CirbhRedundancyState
}

cirbhGsmAlarmConnectState OBJECT-TYPE
    SYNTAX          CirbhConnectGsmState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The state of the connection for GSM interface." 
    ::= { cirbhGsmAlarmTableEntry 1 }

cirbhGsmAlarmLocalState OBJECT-TYPE
    SYNTAX          CirbhAlarmState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The local alarm state." 
    ::= { cirbhGsmAlarmTableEntry 2 }

cirbhGsmAlarmRemoteState OBJECT-TYPE
    SYNTAX          CirbhAlarmState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The remote alarm state." 
    ::= { cirbhGsmAlarmTableEntry 3 }

cirbhGsmAlarmRedundancyState OBJECT-TYPE
    SYNTAX          CirbhRedundancyState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The redundancy state of the interface" 
    ::= { cirbhGsmAlarmTableEntry 4 }
 

-- *************************************************************
-- *                                                           *
-- * UMTS Connection information                               *
-- *                                                           *
-- *************************************************************

cirbhUmtsConnectionTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhUmtsConnectionTableEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides information associated with
        UMTS connection between BTS and BSC."
    ::= { cirbhShortHaulAlarmInfo 2 }

cirbhUmtsConnectionTableEntry OBJECT-TYPE
    SYNTAX          CirbhUmtsConnectionTableEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each Entry represents the set of alarms that apply to
        UMTS interfaces."
    INDEX           { ifIndex } 
    ::= { cirbhUmtsConnectionTable 1 }

CirbhUmtsConnectionTableEntry ::= SEQUENCE {
        cirbhUmtsConnectionState       CirbhConnectUmtsState,
        cirbhUmtsConnectionRedundState CirbhRedundancyState,
        cirbhUmtsConnectionRootIfIndex InterfaceIndexOrZero
}

cirbhUmtsConnectionState OBJECT-TYPE
    SYNTAX          CirbhConnectUmtsState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The state of the connection between the UMTS
        interfaces." 
    ::= { cirbhUmtsConnectionTableEntry 1 }

cirbhUmtsConnectionRedundState OBJECT-TYPE
    SYNTAX          CirbhRedundancyState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The redundancy state of the interface." 
    ::= { cirbhUmtsConnectionTableEntry 2 }

cirbhUmtsConnectionRootIfIndex OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The root interface used to transport
        and receive UMTS traffic as follows.

        ATM:
        ATM0/0.0-aal5 layer -> ATM0/0-atm layer.

        IMA
        ATM0/IMA0.1-aal5 layer -> ATM0/IMA0" 
    ::= { cirbhUmtsConnectionTableEntry 3 }
 

-- *************************************************************
-- *                                                           *
-- * UMTS Alarm information                                    *
-- *                                                           *
-- *************************************************************

cirbhUmtsAlarmTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhUmtsAlarmTableEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides information on alarm states for
        UMTS-ATM interfaces."
    ::= { cirbhShortHaulAlarmInfo 3 }

cirbhUmtsAlarmTableEntry OBJECT-TYPE
    SYNTAX          CirbhUmtsAlarmTableEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry provides information about the alarms for
        each ATM interface used to configure the shorthaul
        UMTS interface."
    INDEX           { ifIndex } 
    ::= { cirbhUmtsAlarmTable 1 }

CirbhUmtsAlarmTableEntry ::= SEQUENCE {
        cirbhUmtsAlarmRxLocalState  CirbhAlarmState,
        cirbhUmtsAlarmRxRemoteState CirbhAlarmState,
        cirbhUmtsAlarmTxLocalState  CirbhAlarmState,
        cirbhUmtsAlarmTxRemoteState CirbhAlarmState
}

cirbhUmtsAlarmRxLocalState OBJECT-TYPE
    SYNTAX          CirbhAlarmState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The local receive alarm state." 
    ::= { cirbhUmtsAlarmTableEntry 1 }

cirbhUmtsAlarmRxRemoteState OBJECT-TYPE
    SYNTAX          CirbhAlarmState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The remote receive alarm state." 
    ::= { cirbhUmtsAlarmTableEntry 2 }

cirbhUmtsAlarmTxLocalState OBJECT-TYPE
    SYNTAX          CirbhAlarmState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The local transmit alarm state." 
    ::= { cirbhUmtsAlarmTableEntry 3 }

cirbhUmtsAlarmTxRemoteState OBJECT-TYPE
    SYNTAX          CirbhAlarmState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The remote transmit alarm state." 
    ::= { cirbhUmtsAlarmTableEntry 4 }
 

-- *************************************************************
-- *                                                           *
-- *  Statistics                                               *
-- *                                                           *
-- *************************************************************

cirbhStatsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhStatsTableEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides measurements on bytes and
        packets sent or received on a per interface basis.
        It is important to note that this table shares the
        same index with the cirbhInfoTable table the ifIndex
        can be used to associate information from both tables."
    ::= { cirbhShortHaulStats 1 }

cirbhStatsTableEntry OBJECT-TYPE
    SYNTAX          CirbhStatsTableEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry provides measurements on shorthaul
        interfaces to allow compression efficency to be
        calculated."
    INDEX           { ifIndex } 
    ::= { cirbhStatsTable 1 }

CirbhStatsTableEntry ::= SEQUENCE {
        cirbhStatsRcvdSamples         Counter32,
        cirbhStatsSentSamples         Counter32,
        cirbhStatsRcvdBackHaulPackets Counter32,
        cirbhStatsSentBackHaulPackets Counter32,
        cirbhStatsRcvdBackHaulBytes   Counter32,
        cirbhStatsSentBackHaulBytes   Counter32
}

cirbhStatsRcvdSamples OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "For GSM-Abis interfaces, the count of samples received on
        interface. For UMTS interfaces, the number of packets received
        on interface." 
    ::= { cirbhStatsTableEntry 1 }

cirbhStatsSentSamples OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "For GSM-Abis interfaces, the count of samples sent on
        interface. For UMTS interfaces, the number of packets sent
        on this interface." 
    ::= { cirbhStatsTableEntry 2 }

cirbhStatsRcvdBackHaulPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The count of packets received from backhaul that contained
        data for this interface." 
    ::= { cirbhStatsTableEntry 3 }

cirbhStatsSentBackHaulPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The count of packets transmitted on backhaul that contained
        data from this interface." 
    ::= { cirbhStatsTableEntry 4 }

cirbhStatsRcvdBackHaulBytes OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The count of bytes received from backhaul that contained
        data for this interface." 
    ::= { cirbhStatsTableEntry 5 }

cirbhStatsSentBackHaulBytes OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The count of bytes transmitted on backhaul that contained
        data from this interface." 
    ::= { cirbhStatsTableEntry 6 }
 

-- *************************************************************
-- *                                                           *
-- * Error information                                         *
-- *                                                           *
-- *************************************************************

cirbhErrorsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhErrorsTableEntry 
    MAX-ACCESS      not-accessible
    STATUS          deprecated
    DESCRIPTION
        "This table provides information on the errors that
        can be encountered during the compression and
        decompression of UMTS and GSM-Abis traffic.

          UMTS
        -------------------
                          |
          GSM Links    --------
         --------------|      | IP based Multi-link(backhaul)
         --------------|      |-----------------------------
         --------------|      |-----------------------------
                       --------"
    ::= { cirbhShortHaulStats 2 }

cirbhErrorsTableEntry OBJECT-TYPE
    SYNTAX          CirbhErrorsTableEntry
    MAX-ACCESS      not-accessible
    STATUS          deprecated
    DESCRIPTION
        "Each entry provides account of various types of
        errors encountered on GSM and UMTS interfaces."
    INDEX           { ifIndex } 
    ::= { cirbhErrorsTable 1 }

CirbhErrorsTableEntry ::= SEQUENCE {
        cirbhErrorsBhPeerNotReadyDrops  Counter32,
        cirbhErrorsBhPeerNotActiveDrops Counter32,
        cirbhErrorsBhInvalidPackets     Counter32,
        cirbhErrorsBhLostRcvdPackets    Counter32,
        cirbhErrorsBhLostSentPackets    Counter32,
        cirbhErrorsBhMissedPackets      Counter32,
        cirbhErrorsBhMissedLatePackets  Counter32,
        cirbhErrorsBhMissedLostPackets  Counter32,
        cirbhErrorsBhMissedNoMemPackets Counter32,
        cirbhErrorsBhMissedResetPackets Counter32,
        cirbhErrorsDecompFailures       Counter32,
        cirbhErrorsCompFailures         Counter32,
        cirbhErrorsCompNoPacketFailures Counter32,
        cirbhErrorsCompNoIntFailures    Counter32,
        cirbhErrorsCompIntDownFailures  Counter32,
        cirbhErrorsCompEncapFailures    Counter32,
        cirbhErrorsCompQosDrops         Counter32
}


cirbhErrorsBhPeerNotReadyDrops OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The count of packets dropped on backhaul because peer was
        not ready." 
    ::= { cirbhErrorsTableEntry 1 }

cirbhErrorsBhPeerNotActiveDrops OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The count of packets dropped on backhaul because peer was
        reachable but not in active state." 
    ::= { cirbhErrorsTableEntry 2 }

cirbhErrorsBhInvalidPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of backhaul packets that were received and dropped
        because they contained invalid information." 
    ::= { cirbhErrorsTableEntry 3 }

cirbhErrorsBhLostRcvdPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of backhaul packets expected to be received but
        never arrived." 
    ::= { cirbhErrorsTableEntry 4 }

cirbhErrorsBhLostSentPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of backhaul packets sent but never were
        received by peer." 
    ::= { cirbhErrorsTableEntry 5 }

cirbhErrorsBhMissedPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The value of this object is the sum total of the values of
        the corresponding instances of the following objects:

        cirbhErrorsBhMissedLatePackets
        cirbhErrorsBhMissedLostPackets
        cirbhErrorsBhMissedNoMemPackets
        cirbhErrorsBhMissedResetPackets" 
    ::= { cirbhErrorsTableEntry 6 }

cirbhErrorsBhMissedLatePackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of packets missed on backhaul because they
        arrived past the allowed time frame." 
    ::= { cirbhErrorsTableEntry 7 }

cirbhErrorsBhMissedLostPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of packets missed on backhaul because they
        were lost on backhaul." 
    ::= { cirbhErrorsTableEntry 8 }

cirbhErrorsBhMissedNoMemPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of packets missed on backhaul for lack of
        available memory to allocate packet." 
    ::= { cirbhErrorsTableEntry 9 }

cirbhErrorsBhMissedResetPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of packets missed on backhaul because the of a
        reset event." 
    ::= { cirbhErrorsTableEntry 10 }

cirbhErrorsDecompFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of times information contained in
        packet could not be decompressed." 
    ::= { cirbhErrorsTableEntry 11 }

cirbhErrorsCompFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of times the information contained in the
        packet could not be compressed.  This counter is
        incremented for all types of compression errors." 
    ::= { cirbhErrorsTableEntry 12 }

cirbhErrorsCompNoPacketFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of times compression failed because
        packet was unavailable." 
    ::= { cirbhErrorsTableEntry 13 }

cirbhErrorsCompNoIntFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of times compression failed because
        route to peer was not available." 
    ::= { cirbhErrorsTableEntry 14 }

cirbhErrorsCompIntDownFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of times compression failed because
        interface was down." 
    ::= { cirbhErrorsTableEntry 15 }

cirbhErrorsCompEncapFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of times compression failed because of
        encapsulation errors." 
    ::= { cirbhErrorsTableEntry 16 }

cirbhErrorsCompQosDrops OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "drops"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of times compression failed because
        of quality of service errors or traffic load." 
    ::= { cirbhErrorsTableEntry 17 }
 

-- *************************************************************
-- *
-- * ShortHaul traffic history
-- *
-- *************************************************************

cirbhShortHaulHistoryTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhShortHaulHistoryTableEntry 
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "This table provides historical information on the amount of
        backhaul traffic contributed by each interface."
    ::= { cirbhShortHaulStats 3 }

cirbhShortHaulHistoryTableEntry OBJECT-TYPE
    SYNTAX          CirbhShortHaulHistoryTableEntry
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "Each entry represents the average traffic for last second.
        Each entry provides information on traffic rates for raw
        and compressed data."
    INDEX           {
                        ifIndex,
                        cirbhShortHaulHistory
                    } 
    ::= { cirbhShortHaulHistoryTable 1 }

CirbhShortHaulHistoryTableEntry ::= SEQUENCE {
        cirbhShortHaulHistory          CirbhHistoryIndex,
        cirbhShortHaulRcvdRate         CirbhRawInterfaceRate,
        cirbhShortHaulSentRate         CirbhRawInterfaceRate,
        cirbhShortHaulRcvdCompressRate CirbhCommpressInterfaceRate,
        cirbhShortHaulSentCompressRate CirbhCommpressInterfaceRate,
        cirbhShortHaulTimeStamp        TimeStamp,
        cirbhShortHaulRcvdUtilization  CirbhShortHaulUtilization,
        cirbhShortHaulSentUtilization  CirbhShortHaulUtilization
}

cirbhShortHaulHistory OBJECT-TYPE
    SYNTAX          CirbhHistoryIndex
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "An index used to access history of
        cirbhShortHaulHistoryTable objects." 
    ::= { cirbhShortHaulHistoryTableEntry 1 }

cirbhShortHaulRcvdRate OBJECT-TYPE
    SYNTAX          CirbhRawInterfaceRate
    UNITS           "bytes/second"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The rate of traffic received from this interface to be sent
        on backhaul prior to compression." 
    ::= { cirbhShortHaulHistoryTableEntry 2 }

cirbhShortHaulSentRate OBJECT-TYPE
    SYNTAX          CirbhRawInterfaceRate
    UNITS           "bytes/second"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The rate of traffic sent out from this interface after
        traffic was decompressed." 
    ::= { cirbhShortHaulHistoryTableEntry 3 }

cirbhShortHaulRcvdCompressRate OBJECT-TYPE
    SYNTAX          CirbhCommpressInterfaceRate
    UNITS           "bytes/second"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The rate of traffic received into this interface to be sent
        on backhaul after compression." 
    ::= { cirbhShortHaulHistoryTableEntry 4 }

cirbhShortHaulSentCompressRate OBJECT-TYPE
    SYNTAX          CirbhCommpressInterfaceRate
    UNITS           "bytes/second"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The rate of traffic received from backhaul and prior to
        decompression." 
    ::= { cirbhShortHaulHistoryTableEntry 5 }

cirbhShortHaulTimeStamp OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "Time when sample was collected." 
    ::= { cirbhShortHaulHistoryTableEntry 6 }

cirbhShortHaulRcvdUtilization OBJECT-TYPE
    SYNTAX          CirbhShortHaulUtilization
    UNITS           "percent of DS load"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "Amount of traffic that was receive from backhaul before
        decompression express as load on E1 or T1." 
    ::= { cirbhShortHaulHistoryTableEntry 7 }

cirbhShortHaulSentUtilization OBJECT-TYPE
    SYNTAX          CirbhShortHaulUtilization
    UNITS           "percent of DS load"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "Amount of traffic that was send on after
        compression express as load on E1 or T1." 
    ::= { cirbhShortHaulHistoryTableEntry 8 }
 

-- *************************************************************
-- *                                                           *
-- * Congestion information                                    *
-- *                                                           *
-- *************************************************************

cirbhCongestionTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhCongestionTableEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides information on congestion
        mechanism for shorthaul interfaces."
    ::= { cirbhShortHaulStats 4 }

cirbhCongestionTableEntry OBJECT-TYPE
    SYNTAX          CirbhCongestionTableEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents single shorthaul interface."
    INDEX           { ifIndex } 
    ::= { cirbhCongestionTable 1 }

CirbhCongestionTableEntry ::= SEQUENCE {
        cirbhCongestionEnabled      TruthValue,
        cirbhCongestionDrops        Counter32,
        cirbhCongestionDroppedBytes Counter32,
        cirbhCongestionEvents       Counter32,
        cirbhCongestionActive       TruthValue,
        cirbhCongestionDuration     Counter32
}

cirbhCongestionEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates congestion mechanisms have been
        enabled for shorthaul interface." 
    ::= { cirbhCongestionTableEntry 1 }

cirbhCongestionDrops OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provide the number packets or cells
        that were dropped due to congestion.  When the
        cirbhInfoProtocol is 'gsmAbis' object indicates the
        number of packets dropped.  When the cirbhInfoProtocol
        is 'umtsIub' object indicates the number of cells
        dropped." 
    ::= { cirbhCongestionTableEntry 2 }

cirbhCongestionDroppedBytes OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of bytes dropped due to congestion
        control mechanisms." 
    ::= { cirbhCongestionTableEntry 3 }

cirbhCongestionEvents OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "occurences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times congestion mechanism was engaged." 
    ::= { cirbhCongestionTableEntry 4 }

cirbhCongestionActive OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates whether congestion mechanism is
        active." 
    ::= { cirbhCongestionTableEntry 5 }

cirbhCongestionDuration OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides number of seconds interface was
        congested." 
    ::= { cirbhCongestionTableEntry 6 }
 

-- *************************************************************
-- *                                                           *
-- * GSM Shorthaul Error information                           *
-- *                                                           *
-- *************************************************************

cirbhGsmErrorsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhGsmErrorsTableEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides information on the errors that
        can be encountered during the compression and
        decompression of GSM-Abis traffic."
    ::= { cirbhShortHaulStats 5 }

cirbhGsmErrorsTableEntry OBJECT-TYPE
    SYNTAX          CirbhGsmErrorsTableEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents single shorthaul interface."
    INDEX           { ifIndex } 
    ::= { cirbhGsmErrorsTable 1 }

CirbhGsmErrorsTableEntry ::= SEQUENCE {
        cirbhGsmErrorsPeerNotReadyDrops    Counter32,
        cirbhGsmErrorsPeerNotActiveDrops   Counter32,
        cirbhGsmErrorsInvalidPackets       Counter32,
        cirbhGsmErrorsLostRcvdPackets      Counter32,
        cirbhGsmErrorsLostSentPackets      Counter32,
        cirbhGsmErrorsMissedPackets        Counter32,
        cirbhGsmErrorsMissedLatePackets    Counter32,
        cirbhGsmErrorsMissedLostPackets    Counter32,
        cirbhGsmErrorsMissedNoMemPackets   Counter32,
        cirbhGsmErrorsMissedResetPackets   Counter32,
        cirbhGsmErrorsDecompFailures       Counter32,
        cirbhGsmErrorsCompFailures         Counter32,
        cirbhGsmErrorsCompNoPacketFailures Counter32,
        cirbhGsmErrorsCompNoIntFailures    Counter32,
        cirbhGsmErrorsCompIntDownFailures  Counter32,
        cirbhGsmErrorsCompEncapFailures    Counter32,
        cirbhGsmErrorsCompQosDrops         Counter32,
        cirbhGsmErrorsFastSendFailures     Counter32,
        cirbhGsmErrorsTxPacketFailures     Counter32,
        cirbhGsmErrorsTxNoBuffers          Counter32,
        cirbhGsmErrorsTxResets             Counter32,
        cirbhGsmErrorsOverruns             Counter32,
        cirbhGsmErrorsInterruptFailures    Counter32,
        cirbhGsmErrorsLateArrivals         Counter32,
        cirbhGsmErrorsEarlyArrivals        Counter32
}

cirbhGsmErrorsPeerNotReadyDrops OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The count of packets dropped on backhaul because peer was
        not ready." 
    ::= { cirbhGsmErrorsTableEntry 1 }

cirbhGsmErrorsPeerNotActiveDrops OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The count of packets dropped on backhaul because peer was
        reachable but not in active state." 
    ::= { cirbhGsmErrorsTableEntry 2 }

cirbhGsmErrorsInvalidPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of backhaul packets that were received and dropped
        because they contained invalid information." 
    ::= { cirbhGsmErrorsTableEntry 3 }

cirbhGsmErrorsLostRcvdPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of backhaul packets expected to be received but
        never arrived." 
    ::= { cirbhGsmErrorsTableEntry 4 }

cirbhGsmErrorsLostSentPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of backhaul packets sent but never were
        received by peer." 
    ::= { cirbhGsmErrorsTableEntry 5 }

cirbhGsmErrorsMissedPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The value of this object is the sum total of the values of
        the corresponding instances of the following objects:

        cirbhGsmErrorsMissedLatePackets
        cirbhGsmErrorsMissedLostPackets
        cirbhGsmErrorsMissedNoMemPackets
        cirbhGsmErrorsMissedResetPackets" 
    ::= { cirbhGsmErrorsTableEntry 6 }

cirbhGsmErrorsMissedLatePackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of packets missed on backhaul because they
        arrived past the allowed time frame." 
    ::= { cirbhGsmErrorsTableEntry 7 }

cirbhGsmErrorsMissedLostPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of packets missed on backhaul because they
        were lost on backhaul." 
    ::= { cirbhGsmErrorsTableEntry 8 }

cirbhGsmErrorsMissedNoMemPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of packets missed on backhaul for lack of
        available memory to allocate packet." 
    ::= { cirbhGsmErrorsTableEntry 9 }

cirbhGsmErrorsMissedResetPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of packets missed on backhaul because the of a
        reset event." 
    ::= { cirbhGsmErrorsTableEntry 10 }

cirbhGsmErrorsDecompFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times information contained in
        packet could not be decompressed." 
    ::= { cirbhGsmErrorsTableEntry 11 }

cirbhGsmErrorsCompFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times the information contained in the
        packet could not be compressed." 
    ::= { cirbhGsmErrorsTableEntry 12 }

cirbhGsmErrorsCompNoPacketFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times compression failed because
        packet was unavailable." 
    ::= { cirbhGsmErrorsTableEntry 13 }

cirbhGsmErrorsCompNoIntFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times compression failed because
        route to peer was not available." 
    ::= { cirbhGsmErrorsTableEntry 14 }

cirbhGsmErrorsCompIntDownFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times compression failed because
        interface was down." 
    ::= { cirbhGsmErrorsTableEntry 15 }

cirbhGsmErrorsCompEncapFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times compression failed because of
        encapsulation errors." 
    ::= { cirbhGsmErrorsTableEntry 16 }

cirbhGsmErrorsCompQosDrops OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "drops"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times compression failed because
        of quality of service errors or traffic load." 
    ::= { cirbhGsmErrorsTableEntry 17 }

cirbhGsmErrorsFastSendFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "occurences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Fast send failures." 
    ::= { cirbhGsmErrorsTableEntry 18 }

cirbhGsmErrorsTxPacketFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "occurences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Unable to transmit GSM packet." 
    ::= { cirbhGsmErrorsTableEntry 19 }

cirbhGsmErrorsTxNoBuffers OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "occurences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Unable to allocate buffer for transmission." 
    ::= { cirbhGsmErrorsTableEntry 20 }

cirbhGsmErrorsTxResets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "occurences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Transmission interface resets." 
    ::= { cirbhGsmErrorsTableEntry 21 }

cirbhGsmErrorsOverruns OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "occurences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Packet was missed because backhaul jitter buffer was
        ran out of available space." 
    ::= { cirbhGsmErrorsTableEntry 22 }

cirbhGsmErrorsInterruptFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "Failures"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Packet was lost because of interrupt failure." 
    ::= { cirbhGsmErrorsTableEntry 23 }

cirbhGsmErrorsLateArrivals OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of GSM packets that arrived later than the allowed
        time." 
    ::= { cirbhGsmErrorsTableEntry 24 }

cirbhGsmErrorsEarlyArrivals OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of GSM packets that arrived earlier than the
        allowed time." 
    ::= { cirbhGsmErrorsTableEntry 25 }
 

-- *************************************************************
-- *                                                           *
-- * UMTS Shorthaul Error information                          *
-- *                                                           *
-- *************************************************************

cirbhUmtsErrorsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhUmtsErrorsTableEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides information on the errors that
        can be encountered during the compression and
        decompression of UMTS-Iub traffic."
    ::= { cirbhShortHaulStats 6 }

cirbhUmtsErrorsTableEntry OBJECT-TYPE
    SYNTAX          CirbhUmtsErrorsTableEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents single shorthaul interface."
    INDEX           { ifIndex } 
    ::= { cirbhUmtsErrorsTable 1 }

CirbhUmtsErrorsTableEntry ::= SEQUENCE {
        cirbhUmtsErrorsPeerNotReadyDrops    Counter32,
        cirbhUmtsErrorsInvalidPackets       Counter32,
        cirbhUmtsErrorsDecompFailures       Counter32,
        cirbhUmtsErrorsCompFailures         Counter32,
        cirbhUmtsErrorsCompNoPacketFailures Counter32,
        cirbhUmtsErrorsCompNoIntFailures    Counter32,
        cirbhUmtsErrorsCompIntDownFailures  Counter32,
        cirbhUmtsErrorsCompEncapFailures    Counter32,
        cirbhUmtsErrorsCompQosDrops         Counter32,
        cirbhUmtsErrorsShorthaulPakFailures Counter32,
        cirbhUmtsErrorsUmtsEncapFailures    Counter32,
        cirbhUmtsErrorsLocalPvcDrops        Counter32,
        cirbhUmtsErrorsRemotePvcDrops       Counter32,
        cirbhUmtsErrorsBackhaulDrops        Counter32
}

cirbhUmtsErrorsPeerNotReadyDrops OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The count of packets dropped on backhaul because peer was
        not ready." 
    ::= { cirbhUmtsErrorsTableEntry 1 }

cirbhUmtsErrorsInvalidPackets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of backhaul packets that were received and dropped
        because they contained invalid information." 
    ::= { cirbhUmtsErrorsTableEntry 2 }

cirbhUmtsErrorsDecompFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times information contained in
        packet could not be decompressed." 
    ::= { cirbhUmtsErrorsTableEntry 3 }

cirbhUmtsErrorsCompFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times the information contained int the
        packet could not be compressed." 
    ::= { cirbhUmtsErrorsTableEntry 4 }

cirbhUmtsErrorsCompNoPacketFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times compression failed because
        packet was unavailable." 
    ::= { cirbhUmtsErrorsTableEntry 5 }

cirbhUmtsErrorsCompNoIntFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times compression failed because
        route to peer was not available." 
    ::= { cirbhUmtsErrorsTableEntry 6 }

cirbhUmtsErrorsCompIntDownFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times compression failed because
        interface was down." 
    ::= { cirbhUmtsErrorsTableEntry 7 }

cirbhUmtsErrorsCompEncapFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "failures"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times compression failed because of
        encapsulation errors." 
    ::= { cirbhUmtsErrorsTableEntry 8 }

cirbhUmtsErrorsCompQosDrops OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "drops"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times compression failed because
        of quality of service errors or traffic load." 
    ::= { cirbhUmtsErrorsTableEntry 9 }

cirbhUmtsErrorsShorthaulPakFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "occurrences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Unable to allocate packet used to send data on shorthaul
        interface." 
    ::= { cirbhUmtsErrorsTableEntry 10 }

cirbhUmtsErrorsUmtsEncapFailures OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "occurences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The UMTS encapsulate failures." 
    ::= { cirbhUmtsErrorsTableEntry 11 }

cirbhUmtsErrorsLocalPvcDrops OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Packet dropped because local PVC was unavailable." 
    ::= { cirbhUmtsErrorsTableEntry 12 }

cirbhUmtsErrorsRemotePvcDrops OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Packet dropped because remote PVC was unavailable." 
    ::= { cirbhUmtsErrorsTableEntry 13 }

cirbhUmtsErrorsBackhaulDrops OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Packets dropped on backhaul." 
    ::= { cirbhUmtsErrorsTableEntry 14 }
 

-- *************************************************************
-- *
-- * ShortHaul Bulk Traffic History
-- *
-- *************************************************************

cirbhShortHaulBulkTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhShortHaulBulkTableEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides historical information on the amount of
        backhaul traffic contributed by each interface."
    ::= { cirbhShortHaulStats 7 }

cirbhShortHaulBulkTableEntry OBJECT-TYPE
    SYNTAX          CirbhShortHaulBulkTableEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents the average traffic for last second.
        Each entry provides information on traffic rates for raw
        and compressed data."
    INDEX           {
                        ifIndex,
                        cirbhShortHaulBulkHistory
                    } 
    ::= { cirbhShortHaulBulkTable 1 }

CirbhShortHaulBulkTableEntry ::= SEQUENCE {
        cirbhShortHaulBulkHistory   CirbhHistoryIndex,
        cirbhShortHaulBulkTimeStamp TimeStamp,
        cirbhShortHaulBulkBaseUnit  Unsigned32,
        cirbhShortHaulBulkUtil      OCTET STRING
}

cirbhShortHaulBulkHistory OBJECT-TYPE
    SYNTAX          CirbhHistoryIndex
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An index used to access history of
        cirbhShortHaulBulkDataTable objects." 
    ::= { cirbhShortHaulBulkTableEntry 1 }

cirbhShortHaulBulkTimeStamp OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Time when sample was collected." 
    ::= { cirbhShortHaulBulkTableEntry 2 }

cirbhShortHaulBulkBaseUnit OBJECT-TYPE
    SYNTAX          Unsigned32 (256..2147483647)
    UNITS           "Bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The Base Unit is an integer used to provide a range of bytes
        rates provided in the cirbhShortHaulBulkUtil object.  All
        values in the cirbhShortHaulBulkUtil object share the same
        base unit." 
    ::= { cirbhShortHaulBulkTableEntry 3 }

cirbhShortHaulBulkUtil OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (0..256))
    UNITS           "Bytes/Second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides the amount of traffic transmitted
        in a particular shorthaul.  The object contains 1 to
        128 pairs.  The length of the octet string can be used
        to calculate number of pairs.  The information is in
        the following format were each rate is stored as single
        byte.

        [rx,tx] * 128

        The approximated rate can be calculated by multiplying
        value from cirbhShortHaulBulkUtil times value in the
        cirbhShortHaulBulkBaseUnit." 
    ::= { cirbhShortHaulBulkTableEntry 4 }
 

-- *************************************************************
-- *
-- * BackHaul Table
-- *
-- *************************************************************

cirbhBackHaulTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhBackHaulEntry 
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "This table provides information on backHaul links."
    ::= { cirbhBackHaulInfo 1 }

cirbhBackHaulEntry OBJECT-TYPE
    SYNTAX          CirbhBackHaulEntry
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "Each entry represents a backhaul link between BSC and
        a particular BTS site."
    INDEX           { ifIndex } 
    ::= { cirbhBackHaulTable 1 }

CirbhBackHaulEntry ::= SEQUENCE {
        cirbhBackHaulAdjectSerialNum  SnmpAdminString,
        cirbhBackHaulAdjectVendorType AutonomousType,
        cirbhBackHaulRcvdUtilState    CirbhBackHaulUtilizationState,
        cirbhBackHaulSentUtilState    CirbhBackHaulUtilizationState,
        cirbhBackHaulRcvdUtil         CirbhBackHaulUtilization,
        cirbhBackHaulSentUtil         CirbhBackHaulUtilization
}

cirbhBackHaulAdjectSerialNum OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "This object provides the serial number of the adjacent
        device supporting the backhaul connection. This object
        contains the same value as the corresponding
        entPhysicalSerialNum object. The type of object like chassis
        or module is provided by the cirbhBackHaulAdjectVendorType
        object." 
    ::= { cirbhBackHaulEntry 1 }

cirbhBackHaulAdjectVendorType OBJECT-TYPE
    SYNTAX          AutonomousType
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "This object provides the vendor type of the adjacent
        device supporting backhaul connection. This object
        contains the same value as the corresponding
        entPhysicalVendorType object." 
    ::= { cirbhBackHaulEntry 2 }

cirbhBackHaulRcvdUtilState OBJECT-TYPE
    SYNTAX          CirbhBackHaulUtilizationState
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The utilization state for traffic received on
        backhaul multilink.

        The following objects will be used to calculate
        link utilization state:

        cirbhBackHaulAcceptableThreshold
        cirbhBackHaulWarningThreshold
        cirbhBackHaulOverloadedThreshold" 
    ::= { cirbhBackHaulEntry 3 }

cirbhBackHaulSentUtilState OBJECT-TYPE
    SYNTAX          CirbhBackHaulUtilizationState
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The utilization state for traffic transmitted on
        backhaul multilink.

        The following objects will be used to calculate
        link utilization state:

        cirbhBackHaulAcceptableThreshold
        cirbhBackHaulWarningThreshold
        cirbhBackHaulOverloadedThreshold" 
    ::= { cirbhBackHaulEntry 4 }

cirbhBackHaulRcvdUtil OBJECT-TYPE
    SYNTAX          CirbhBackHaulUtilization
    UNITS           "percent"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The average receive utilization of the link over the last
        second." 
    ::= { cirbhBackHaulEntry 5 }

cirbhBackHaulSentUtil OBJECT-TYPE
    SYNTAX          CirbhBackHaulUtilization
    UNITS           "percent"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The average transmit utilization of the link over the last
        second." 
    ::= { cirbhBackHaulEntry 6 }
 

-- *************************************************************
-- *
-- * BackHaul to ShortHaul Table
-- *
-- *************************************************************

cirbhBackHaulShortHaulTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhBackHaulShortHaulEntry 
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "This table lists the associations between shorthaul and
        backhaul interfaces."
    ::= { cirbhBackHaulInfo 2 }

cirbhBackHaulShortHaulEntry OBJECT-TYPE
    SYNTAX          CirbhBackHaulShortHaulEntry
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "An entry indicates a single association between a backhaul and
        shorthaul interface."
    INDEX           {
                        cirbhBackHaulShortHaulBhIndex,
                        cirbhBackHaulShortHaulShIndex
                    } 
    ::= { cirbhBackHaulShortHaulTable 1 }

CirbhBackHaulShortHaulEntry ::= SEQUENCE {
        cirbhBackHaulShortHaulBhIndex   InterfaceIndex,
        cirbhBackHaulShortHaulShIndex   InterfaceIndex,
        cirbhBackHaulShortHaulTimestamp TimeStamp
}

cirbhBackHaulShortHaulBhIndex OBJECT-TYPE
    SYNTAX          InterfaceIndex
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "This object indicates the backhaul interface." 
    ::= { cirbhBackHaulShortHaulEntry 1 }

cirbhBackHaulShortHaulShIndex OBJECT-TYPE
    SYNTAX          InterfaceIndex
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "This object indicates the shorthaul interface." 
    ::= { cirbhBackHaulShortHaulEntry 2 }

cirbhBackHaulShortHaulTimestamp OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "This object indicates the value of sysUpTime when the
        entry was created." 
    ::= { cirbhBackHaulShortHaulEntry 3 }
 

-- *************************************************************
-- *
-- * BackHaul History Table
-- *
-- *************************************************************

cirbhBackHaulHistoryTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhBackHaulHistoryEntry 
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "This table provides historical information on traffic
        distribution on backhaul interface."
    ::= { cirbhBackHaulStats 1 }

cirbhBackHaulHistoryEntry OBJECT-TYPE
    SYNTAX          CirbhBackHaulHistoryEntry
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "Each entry provides information on the utilization of
        backhaul interface. The utilization is broken down
        by protocol and by direction.  An entry is updated in
        this table every second."
    INDEX           {
                        ifIndex,
                        cirbhBackHaulHistoryIndex
                    } 
    ::= { cirbhBackHaulHistoryTable 1 }

CirbhBackHaulHistoryEntry ::= SEQUENCE {
        cirbhBackHaulHistoryIndex        CirbhHistoryIndex,
        cirbhBackHaulHistoryRcvdUtil     CirbhBackHaulUtilization,
        cirbhBackHaulHistorySentUtil     CirbhBackHaulUtilization,
        cirbhBackHaulHistoryRcvdAbisUtil CirbhBackHaulUtilization,
        cirbhBackHaulHistorySentAbisUtil CirbhBackHaulUtilization,
        cirbhBackHaulHistoryRcvdUmtsUtil CirbhBackHaulUtilization,
        cirbhBackHaulHistorySentUmtsUtil CirbhBackHaulUtilization,
        cirbhBackHaulHistoryTimeStamp    TimeStamp
}

cirbhBackHaulHistoryIndex OBJECT-TYPE
    SYNTAX          CirbhHistoryIndex
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "An index used to access history of
        cirbhBackHaulHistoryTable objects." 
    ::= { cirbhBackHaulHistoryEntry 1 }

cirbhBackHaulHistoryRcvdUtil OBJECT-TYPE
    SYNTAX          CirbhBackHaulUtilization
    UNITS           "percent"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The average receive utilization of link over the last
        second." 
    ::= { cirbhBackHaulHistoryEntry 2 }

cirbhBackHaulHistorySentUtil OBJECT-TYPE
    SYNTAX          CirbhBackHaulUtilization
    UNITS           "percent"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The average transmit utilization of link over the last
        second." 
    ::= { cirbhBackHaulHistoryEntry 3 }

cirbhBackHaulHistoryRcvdAbisUtil OBJECT-TYPE
    SYNTAX          CirbhBackHaulUtilization
    UNITS           "percent"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The average receive utilization of link over the last
        second that consisted of GSM-Abis traffic." 
    ::= { cirbhBackHaulHistoryEntry 4 }

cirbhBackHaulHistorySentAbisUtil OBJECT-TYPE
    SYNTAX          CirbhBackHaulUtilization
    UNITS           "percent"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The average transmit utilization of link over the last
        second that consisted of GSM-Abis traffic." 
    ::= { cirbhBackHaulHistoryEntry 5 }

cirbhBackHaulHistoryRcvdUmtsUtil OBJECT-TYPE
    SYNTAX          CirbhBackHaulUtilization
    UNITS           "percent"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The average receive utilization of link over the last
        second that consisted of UMTS traffic." 
    ::= { cirbhBackHaulHistoryEntry 6 }

cirbhBackHaulHistorySentUmtsUtil OBJECT-TYPE
    SYNTAX          CirbhBackHaulUtilization
    UNITS           "percent"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The average transmit utilization of link over the last
        second that consisted of UMTS traffic." 
    ::= { cirbhBackHaulHistoryEntry 7 }

cirbhBackHaulHistoryTimeStamp OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "Time when sample was collected." 
    ::= { cirbhBackHaulHistoryEntry 8 }
 

-- *************************************************************
-- *
-- * BackHaul Statistics Table
-- *
-- *************************************************************

cirbhBackHaulStatsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhBackHaulStatsEntry 
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "This table provides current information on the utilization of
        backhaul interface. One second load samples are collected
        and the corresponding entry is incremented. The provides
        a distribution of the traffic load. At the end of an
        interval the information is collected and used to
        populate entry in the cirbhBackHaulStatsHistoryTable.
        The interval is specified by the cirbhBackHaulStatsInterval
        object. The counters in this table increase until the
        interval ends at which time they are reset."
    ::= { cirbhBackHaulStats 2 }

cirbhBackHaulStatsEntry OBJECT-TYPE
    SYNTAX          CirbhBackHaulStatsEntry
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "Each entry contains the distribution of traffic in the
        current window specified by the cirbhBackHaulStatsInterval
        object."
    INDEX           {
                        ifIndex,
                        cirbhStatsDirection,
                        cirbhStatsTrafficType
                    } 
    ::= { cirbhBackHaulStatsTable 1 }

CirbhBackHaulStatsEntry ::= SEQUENCE {
        cirbhStatsDirection       CirbhTrafficDirection,
        cirbhStatsTrafficType     CirbhTrafficType,
        cirbhStats000to009Seconds PerfCurrentCount,
        cirbhStats010to019Seconds PerfCurrentCount,
        cirbhStats020to029Seconds PerfCurrentCount,
        cirbhStats030to039Seconds PerfCurrentCount,
        cirbhStats040to049Seconds PerfCurrentCount,
        cirbhStats050to059Seconds PerfCurrentCount,
        cirbhStats060to069Seconds PerfCurrentCount,
        cirbhStats070to079Seconds PerfCurrentCount,
        cirbhStats080to089Seconds PerfCurrentCount,
        cirbhStats090to100Seconds PerfCurrentCount,
        cirbhStatsTimeStamp       TimeStamp,
        cirbhStatsMaxUtilization  CirbhBackHaulUtilization,
        cirbhStatsMaxTimeStamp    TimeStamp
}

cirbhStatsDirection OBJECT-TYPE
    SYNTAX          CirbhTrafficDirection
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "The direction of traffic on backhaul." 
    ::= { cirbhBackHaulStatsEntry 1 }

cirbhStatsTrafficType OBJECT-TYPE
    SYNTAX          CirbhTrafficType
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "The type of traffic." 
    ::= { cirbhBackHaulStatsEntry 2 }

cirbhStats000to009Seconds OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 0 to 9 percent." 
    ::= { cirbhBackHaulStatsEntry 3 }

cirbhStats010to019Seconds OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 10 to 19 percent." 
    ::= { cirbhBackHaulStatsEntry 4 }

cirbhStats020to029Seconds OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 20 to 29 percent." 
    ::= { cirbhBackHaulStatsEntry 5 }

cirbhStats030to039Seconds OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 30 to 39 percent." 
    ::= { cirbhBackHaulStatsEntry 6 }

cirbhStats040to049Seconds OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 40 to 49 percent." 
    ::= { cirbhBackHaulStatsEntry 7 }

cirbhStats050to059Seconds OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 50 to 59 percent." 
    ::= { cirbhBackHaulStatsEntry 8 }

cirbhStats060to069Seconds OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 60 to 69 percent." 
    ::= { cirbhBackHaulStatsEntry 9 }

cirbhStats070to079Seconds OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 70 to 79 percent." 
    ::= { cirbhBackHaulStatsEntry 10 }

cirbhStats080to089Seconds OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 80 to 89 percent." 
    ::= { cirbhBackHaulStatsEntry 11 }

cirbhStats090to100Seconds OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 90 to 100 percent." 
    ::= { cirbhBackHaulStatsEntry 12 }

cirbhStatsTimeStamp OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "Time when sample was collected." 
    ::= { cirbhBackHaulStatsEntry 13 }

cirbhStatsMaxUtilization OBJECT-TYPE
    SYNTAX          CirbhBackHaulUtilization
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The maximum utilization encountered within interval." 
    ::= { cirbhBackHaulStatsEntry 14 }

cirbhStatsMaxTimeStamp OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "Time when cirbhStatsMaxUtilization was recorded." 
    ::= { cirbhBackHaulStatsEntry 15 }
 

-- *************************************************************
-- *
-- * BackHaul Statistics History Table
-- *
-- *************************************************************

cirbhBackHaulStatsHistoryTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CirbhBackHaulStatsHistoryEntry 
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "This table provides historical information of distribution
        of load on backhaul interfaces."
    ::= { cirbhObjects 12 }

cirbhBackHaulStatsHistoryEntry OBJECT-TYPE
    SYNTAX          CirbhBackHaulStatsHistoryEntry
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "Each entry in this table is the data collected from the
        cirbhBackHaulStatsTable table."
    INDEX           {
                        ifIndex,
                        cirbhStatsHistoryIndex,
                        cirbhStatsHistoryDirection,
                        cirbhStatsHistoryTrafficType
                    } 
    ::= { cirbhBackHaulStatsHistoryTable 1 }

CirbhBackHaulStatsHistoryEntry ::= SEQUENCE {
        cirbhStatsHistoryIndex           CirbhHistoryIndex,
        cirbhStatsHistoryDirection       CirbhTrafficDirection,
        cirbhStatsHistoryTrafficType     CirbhTrafficType,
        cirbhStatsHistory000to009Seconds PerfIntervalCount,
        cirbhStatsHistory010to019Seconds PerfIntervalCount,
        cirbhStatsHistory020to029Seconds PerfIntervalCount,
        cirbhStatsHistory030to039Seconds PerfIntervalCount,
        cirbhStatsHistory040to049Seconds PerfIntervalCount,
        cirbhStatsHistory050to059Seconds PerfIntervalCount,
        cirbhStatsHistory060to069Seconds PerfIntervalCount,
        cirbhStatsHistory070to079Seconds PerfIntervalCount,
        cirbhStatsHistory080to089Seconds PerfIntervalCount,
        cirbhStatsHistory090to100Seconds PerfIntervalCount,
        cirbhStatsHistoryTimeStamp       TimeStamp,
        cirbhStatsHistoryMaxUtilization  CirbhBackHaulUtilization,
        cirbhStatsHistoryMaxTimeStamp    TimeStamp,
        cirbhStatsHistoryAverage         CirbhBackHaulUtilization
}

cirbhStatsHistoryIndex OBJECT-TYPE
    SYNTAX          CirbhHistoryIndex
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "An index used to access each 15 minute entry." 
    ::= { cirbhBackHaulStatsHistoryEntry 1 }

cirbhStatsHistoryDirection OBJECT-TYPE
    SYNTAX          CirbhTrafficDirection
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "The direction of traffic on backhaul." 
    ::= { cirbhBackHaulStatsHistoryEntry 2 }

cirbhStatsHistoryTrafficType OBJECT-TYPE
    SYNTAX          CirbhTrafficType
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "The type of traffic in backhaul history table." 
    ::= { cirbhBackHaulStatsHistoryEntry 3 }

cirbhStatsHistory000to009Seconds OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 0 to 9 percent." 
    ::= { cirbhBackHaulStatsHistoryEntry 4 }

cirbhStatsHistory010to019Seconds OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 10 to 19 percent." 
    ::= { cirbhBackHaulStatsHistoryEntry 5 }

cirbhStatsHistory020to029Seconds OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 20 to 29 percent." 
    ::= { cirbhBackHaulStatsHistoryEntry 6 }

cirbhStatsHistory030to039Seconds OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 30 to 39 percent." 
    ::= { cirbhBackHaulStatsHistoryEntry 7 }

cirbhStatsHistory040to049Seconds OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 40 to 49 percent." 
    ::= { cirbhBackHaulStatsHistoryEntry 8 }

cirbhStatsHistory050to059Seconds OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 50 to 59 percent." 
    ::= { cirbhBackHaulStatsHistoryEntry 9 }

cirbhStatsHistory060to069Seconds OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 60 to 69 percent." 
    ::= { cirbhBackHaulStatsHistoryEntry 10 }

cirbhStatsHistory070to079Seconds OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 70 to 79 percent." 
    ::= { cirbhBackHaulStatsHistoryEntry 11 }

cirbhStatsHistory080to089Seconds OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 80 to 89 percent." 
    ::= { cirbhBackHaulStatsHistoryEntry 12 }

cirbhStatsHistory090to100Seconds OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The total numbers of seconds during which the backhaul link
        was utilized from 90 to 100 percent." 
    ::= { cirbhBackHaulStatsHistoryEntry 13 }

cirbhStatsHistoryTimeStamp OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "End time when sample was collected." 
    ::= { cirbhBackHaulStatsHistoryEntry 14 }

cirbhStatsHistoryMaxUtilization OBJECT-TYPE
    SYNTAX          CirbhBackHaulUtilization
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The maximum utilization encountered within interval." 
    ::= { cirbhBackHaulStatsHistoryEntry 15 }

cirbhStatsHistoryMaxTimeStamp OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "Time when cirbhStatsHistoryMaxUtilization was recorded." 
    ::= { cirbhBackHaulStatsHistoryEntry 16 }

cirbhStatsHistoryAverage OBJECT-TYPE
    SYNTAX          CirbhBackHaulUtilization
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The average utilization over the specified time period." 
    ::= { cirbhBackHaulStatsHistoryEntry 17 }
 


-- *************************************************************
-- *                                                           *
-- * Notification Enable Objects                               *
-- *                                                           *
-- *************************************************************

cirbhGsmAlarmNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the agent should
        generate the ciscoIpRanBackHaulGsmAlarm defined in
        this MIB module.

        'true'  Indicates that ciscoIpRanBackHaulGsmAlarm
               notification is to be generated.

        'false' Indicates that ciscoIpRanBackHaulGsmAlarm
               notification generation is disabled."
    DEFVAL          { false } 
    ::= { cirbhNotifEnables 1 }

cirbhUmtsAlarmNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the agent should
        generate the ciscoIpRanBackHaulUmtsAlarm defined in
        this MIB module.

        'true'  Indicates that ciscoIpRanBackHaulUmtsAlarm
               notification is to be generated.

        'false' Indicates that ciscoIpRanBackHaulUmtsAlarm
               notification generation is disabled."
    DEFVAL          { false } 
    ::= { cirbhNotifEnables 2 }

cirbhUtilNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object specifies whether the agent should
        generate the ciscoIpRanBackHaulRcvdUtil or
        ciscoIpRanBackHaulSentUtil defined in this MIB module.

        'true'  Indicates that ciscoIpRanBackHaulRcvdUtil and
               ciscoIpRanBackHaulSentUtil notifications
               are to be generated.

        'false' Indicates that ciscoIpRanBackHaulRcvdUtil and
               ciscoIpRanBackHaulSentUtil notifications
               generation is disabled."
    DEFVAL          { false } 
    ::= { cirbhNotifEnables 3 }

-- *************************************************************
-- *                                                           *
-- * Notifications                                             *
-- *                                                           *
-- *************************************************************

ciscoIpRanBackHaulGsmAlarm NOTIFICATION-TYPE
    OBJECTS         {
                        ifDescr,
                        cirbhGsmAlarmConnectState,
                        cirbhGsmAlarmLocalState,
                        cirbhGsmAlarmRemoteState,
                        cirbhGsmAlarmRedundancyState
                    }
    STATUS          current
    DESCRIPTION
        "This notification is generated whenever the
        values of the specified objects change."
   ::= { ciscoIpRanBackHaulMIBNotifs 1 }

ciscoIpRanBackHaulUmtsAlarm NOTIFICATION-TYPE
    OBJECTS         {
                        ifDescr,
                        cirbhUmtsConnectionState,
                        cirbhUmtsAlarmRxLocalState,
                        cirbhUmtsAlarmRxRemoteState,
                        cirbhUmtsAlarmTxLocalState,
                        cirbhUmtsAlarmTxRemoteState,
                        cirbhUmtsConnectionRedundState
                    }
    STATUS          current
    DESCRIPTION
        "This notification is generated whenever the
        values of the specified objects change."
   ::= { ciscoIpRanBackHaulMIBNotifs 2 }

ciscoIpRanBackHaulRcvdUtil NOTIFICATION-TYPE
    OBJECTS         {
                        ifDescr,
                        cirbhBackHaulRcvdUtilState,
                        cirbhBackHaulRcvdUtil
                    }
    STATUS          obsolete
    DESCRIPTION
        "This notification is generated once for the interval
        specified by the cirbhBackHaulStatsInterval object
        for the following state transitions.

        'acceptable' ->  'warning'
        'acceptable' ->  'overloaded'
        'warning'    ->  'overloaded'

        At the end of the interval specified by the
        cirbhBackHaulUtilInterval object another notification
        will be generated if the current state is
        different from state sent in last notification."
   ::= { ciscoIpRanBackHaulMIBNotifs 3 }

ciscoIpRanBackHaulSentUtil NOTIFICATION-TYPE
    OBJECTS         {
                        ifDescr,
                        cirbhBackHaulSentUtilState,
                        cirbhBackHaulSentUtil
                    }
    STATUS          obsolete
    DESCRIPTION
        "This notification is generated once for the interval
        specified by the cirbhBackHaulStatsInterval object
        for the following state transitions.

        'acceptable' ->  'warning'
        'acceptable' ->  'overloaded'
        'warning'    ->  'overloaded'

        At the end of the interval specified by the
        cirbhBackHaulUtilInterval object another notification
        will be generated if the current state is
        different from state sent in last notification."
   ::= { ciscoIpRanBackHaulMIBNotifs 4 }
-- *************************************************************
-- *                                                           *
-- * Conformance Information                                   *
-- *                                                           *
-- *************************************************************

ciscoIpRanBackHaulMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoIpRanBackHaulMIBConform 1 }

ciscoIpRanBackHaulMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoIpRanBackHaulMIBConform 2 }


-- ********************************************************************
-- Compliance Statements
-- ********************************************************************

ciscoIpRanBackHaulMIBCompliance MODULE-COMPLIANCE
    STATUS          obsolete
    DESCRIPTION
        "The compliance statement for entities which implement
        the CISCO-IP-RAN-BACKHAUL-MIB.my managment information
        base."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoIpRanBackHaulScalarsGroup,
                        ciscoIpRanBackHaulConfigGroup,
                        ciscoIpRanBackHaulStatsGroup,
                        ciscoIpRanBackHaulAlarmGroup,
                        ciscoIpRanBackHaulErrorsGroup,
                        ciscoIpRanBackHaulHistoryGroup,
                        ciscoIpRanBackHaulNotifGroup
                    }
    ::= { ciscoIpRanBackHaulMIBCompliances 1 }

ciscoIpRanBackHaulMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          obsolete
    DESCRIPTION
        "The compliance statement for entities which implement
        the CISCO-IP-RAN-BACKHAUL-MIB.my managment information
        base."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoIpRanBackHaulScalarsGroup,
                        ciscoIpRanBackHaulConfigGroup,
                        ciscoIpRanBackHaulStatsGroup,
                        ciscoIpRanBackHaulAlarmGroup,
                        ciscoIpRanBackHaulErrorsGroup,
                        ciscoIpRanBackHaulHistoryGroup,
                        ciscoIpRanBackHaulNotifGroup,
                        ciscoIpRanBackHaulShortHaulGroup,
                        ciscoIpRanBackHaulAlarmGroupSup1
                    }
    ::= { ciscoIpRanBackHaulMIBCompliances 2 }

ciscoIpRanBackHaulMIBComplianceRev2 MODULE-COMPLIANCE
    STATUS          obsolete
    DESCRIPTION
        "The compliance statement for entities which implement
        the CISCO-IP-RAN-BACKHAUL-MIB.my managment information
        base."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoIpRanBackHaulScalarsGroupRev2,
                        ciscoIpRanBackHaulConfigGroup,
                        ciscoIpRanBackHaulConfigGroupSup2,
                        ciscoIpRanBackHaulConfigGroupSup3,
                        ciscoIpRanBackHaulStatsGroup,
                        ciscoIpRanBackHaulAlarmGroup,
                        ciscoIpRanBackHaulHistoryGroupRev2,
                        ciscoIpRanBackHaulNotifGroupRev2,
                        ciscoIpRanBackHaulAlarmGroupSup1,
                        ciscoIpRanBackHaulCongestionGroup,
                        ciscoIpRanBackHaulGsmErrorsGroup,
                        ciscoIpRanBackHaulUmtsErrorsGroup
                    }
    ::= { ciscoIpRanBackHaulMIBCompliances 3 }

ciscoIpRanBackHaulMIBComplianceRev3 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for entities which implement
        the CISCO-IP-RAN-BACKHAUL-MIB.my managment information
        base."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoIpRanBackHaulScalarsGroupRev2,
                        ciscoIpRanBackHaulConfigGroup,
                        ciscoIpRanBackHaulConfigGroupSup2,
                        ciscoIpRanBackHaulConfigGroupSup3,
                        ciscoIpRanBackHaulStatsGroup,
                        ciscoIpRanBackHaulAlarmGroup,
                        ciscoIpRanBackHaulHistoryGroupRev3,
                        ciscoIpRanBackHaulNotifGroupRev2,
                        ciscoIpRanBackHaulAlarmGroupSup1,
                        ciscoIpRanBackHaulCongestionGroup,
                        ciscoIpRanBackHaulGsmErrorsGroup,
                        ciscoIpRanBackHaulUmtsErrorsGroup
                    }
    ::= { ciscoIpRanBackHaulMIBCompliances 4 }

-- ****************************************************************
-- Units of Conformance
-- ****************************************************************

ciscoIpRanBackHaulScalarsGroup OBJECT-GROUP
    OBJECTS         {
                        cirbhSnmpTrafficMode,
                        cirbhLocation,
                        cirbhBackHaulStatsInterval,
                        cirbhBackHaulStatsEntries,
                        cirbhBackHaulAcceptableThreshold,
                        cirbhBackHaulWarningThreshold,
                        cirbhBackHaulOverloadedThreshold,
                        cirbhBackHaulUtilInterval,
                        cirbhGsmAlarmNotifEnabled,
                        cirbhUmtsAlarmNotifEnabled,
                        cirbhUtilNotifEnabled
                    }
    STATUS          deprecated
    DESCRIPTION
        "Cisco IP RAN Input Scalars Group."
    ::= { ciscoIpRanBackHaulMIBGroups 1 }

ciscoIpRanBackHaulConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cirbhInfoProtocol,
                        cirbhInfoLocalAddrType,
                        cirbhInfoLocalAddr,
                        cirbhInfoLocalPortNumber,
                        cirbhInfoRemoteAddrType,
                        cirbhInfoRemoteAddr,
                        cirbhInfoRemotePortNumber
                    }
    STATUS          current
    DESCRIPTION
        "Cisco IP RAN Configuration Group."
    ::= { ciscoIpRanBackHaulMIBGroups 2 }

ciscoIpRanBackHaulStatsGroup OBJECT-GROUP
    OBJECTS         {
                        cirbhStatsRcvdSamples,
                        cirbhStatsSentSamples,
                        cirbhStatsRcvdBackHaulPackets,
                        cirbhStatsSentBackHaulPackets,
                        cirbhStatsRcvdBackHaulBytes,
                        cirbhStatsSentBackHaulBytes
                    }
    STATUS          current
    DESCRIPTION
        "Cisco IP RAN Backhaul Statistics Group."
    ::= { ciscoIpRanBackHaulMIBGroups 3 }

ciscoIpRanBackHaulAlarmGroup OBJECT-GROUP
    OBJECTS         {
                        cirbhGsmAlarmConnectState,
                        cirbhGsmAlarmLocalState,
                        cirbhGsmAlarmRemoteState,
                        cirbhGsmAlarmRedundancyState,
                        cirbhUmtsConnectionState,
                        cirbhUmtsConnectionRedundState,
                        cirbhUmtsAlarmRxLocalState,
                        cirbhUmtsAlarmRxRemoteState,
                        cirbhUmtsAlarmTxLocalState,
                        cirbhUmtsAlarmTxRemoteState
                    }
    STATUS          current
    DESCRIPTION
        "Cisco IP RAN Alarm Group."
    ::= { ciscoIpRanBackHaulMIBGroups 4 }

ciscoIpRanBackHaulErrorsGroup OBJECT-GROUP
    OBJECTS         {
                        cirbhErrorsBhPeerNotReadyDrops,
                        cirbhErrorsBhPeerNotActiveDrops,
                        cirbhErrorsBhInvalidPackets,
                        cirbhErrorsBhLostRcvdPackets,
                        cirbhErrorsBhLostSentPackets,
                        cirbhErrorsBhMissedPackets,
                        cirbhErrorsBhMissedLatePackets,
                        cirbhErrorsBhMissedLostPackets,
                        cirbhErrorsBhMissedNoMemPackets,
                        cirbhErrorsBhMissedResetPackets,
                        cirbhErrorsDecompFailures,
                        cirbhErrorsCompFailures,
                        cirbhErrorsCompNoPacketFailures,
                        cirbhErrorsCompNoIntFailures,
                        cirbhErrorsCompIntDownFailures,
                        cirbhErrorsCompEncapFailures,
                        cirbhErrorsCompQosDrops
                    }
    STATUS          deprecated
    DESCRIPTION
        "Cisco protocol errors Group."
    ::= { ciscoIpRanBackHaulMIBGroups 5 }

ciscoIpRanBackHaulHistoryGroup OBJECT-GROUP
    OBJECTS         {
                        cirbhShortHaulRcvdRate,
                        cirbhShortHaulSentRate,
                        cirbhShortHaulRcvdCompressRate,
                        cirbhShortHaulSentCompressRate,
                        cirbhShortHaulTimeStamp,
                        cirbhShortHaulRcvdUtilization,
                        cirbhShortHaulSentUtilization,
                        cirbhBackHaulRcvdUtilState,
                        cirbhBackHaulSentUtilState,
                        cirbhBackHaulRcvdUtil,
                        cirbhBackHaulSentUtil,
                        cirbhBackHaulAdjectSerialNum,
                        cirbhBackHaulAdjectVendorType,
                        cirbhBackHaulHistoryRcvdUtil,
                        cirbhBackHaulHistorySentUtil,
                        cirbhBackHaulHistoryRcvdAbisUtil,
                        cirbhBackHaulHistorySentAbisUtil,
                        cirbhBackHaulHistoryRcvdUmtsUtil,
                        cirbhBackHaulHistorySentUmtsUtil,
                        cirbhBackHaulHistoryTimeStamp,
                        cirbhStats000to009Seconds,
                        cirbhStats010to019Seconds,
                        cirbhStats020to029Seconds,
                        cirbhStats030to039Seconds,
                        cirbhStats040to049Seconds,
                        cirbhStats050to059Seconds,
                        cirbhStats060to069Seconds,
                        cirbhStats070to079Seconds,
                        cirbhStats080to089Seconds,
                        cirbhStats090to100Seconds,
                        cirbhStatsTimeStamp,
                        cirbhStatsMaxUtilization,
                        cirbhStatsMaxTimeStamp,
                        cirbhStatsHistory000to009Seconds,
                        cirbhStatsHistory010to019Seconds,
                        cirbhStatsHistory020to029Seconds,
                        cirbhStatsHistory030to039Seconds,
                        cirbhStatsHistory040to049Seconds,
                        cirbhStatsHistory050to059Seconds,
                        cirbhStatsHistory060to069Seconds,
                        cirbhStatsHistory070to079Seconds,
                        cirbhStatsHistory080to089Seconds,
                        cirbhStatsHistory090to100Seconds,
                        cirbhStatsHistoryTimeStamp,
                        cirbhStatsHistoryMaxUtilization,
                        cirbhStatsHistoryMaxTimeStamp,
                        cirbhStatsHistoryAverage
                    }
    STATUS          obsolete
    DESCRIPTION
        "Cisco IP RAN Utilization History Group."
    ::= { ciscoIpRanBackHaulMIBGroups 6 }

ciscoIpRanBackHaulNotifGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        ciscoIpRanBackHaulGsmAlarm,
                        ciscoIpRanBackHaulUmtsAlarm,
                        ciscoIpRanBackHaulRcvdUtil,
                        ciscoIpRanBackHaulSentUtil
                    }
    STATUS          obsolete
    DESCRIPTION
        "Cisco IP RAN Notifications."
    ::= { ciscoIpRanBackHaulMIBGroups 7 }

ciscoIpRanBackHaulShortHaulGroup OBJECT-GROUP
    OBJECTS         { cirbhBackHaulShortHaulTimestamp }
    STATUS          obsolete
    DESCRIPTION
        "Cisco IP RAN Backhaul to Shorthaul Group."
    ::= { ciscoIpRanBackHaulMIBGroups 8 }

ciscoIpRanBackHaulAlarmGroupSup1 OBJECT-GROUP
    OBJECTS         { cirbhUmtsConnectionRootIfIndex }
    STATUS          current
    DESCRIPTION
        "Additional objects for Cisco IP RAN Alarm Group."
    ::= { ciscoIpRanBackHaulMIBGroups 9 }

ciscoIpRanBackHaulScalarsGroupRev2 OBJECT-GROUP
    OBJECTS         {
                        cirbhSnmpTrafficMode,
                        cirbhLocation,
                        cirbhGsmAlarmNotifEnabled,
                        cirbhUmtsAlarmNotifEnabled
                    }
    STATUS          current
    DESCRIPTION
        "Cisco IP RAN Input Scalars Group."
    ::= { ciscoIpRanBackHaulMIBGroups 10 }

ciscoIpRanBackHaulConfigGroupSup2 OBJECT-GROUP
    OBJECTS         {
                        cirbhInfoAdjectSerialNum,
                        cirbhInfoAdjectVendorType,
                        cirbhInfoBackhaulRxIfIndex,
                        cirbhInfoBackhaulTxIfIndex,
                        cirbhInfoShBulkLastIndex
                    }
    STATUS          current
    DESCRIPTION
        "Cisco IP RAN Configuration Group Sup2."
    ::= { ciscoIpRanBackHaulMIBGroups 11 }

ciscoIpRanBackHaulHistoryGroupRev2 OBJECT-GROUP
    OBJECTS         {
                        cirbhShortHaulRcvdRate,
                        cirbhShortHaulSentRate,
                        cirbhShortHaulRcvdCompressRate,
                        cirbhShortHaulSentCompressRate,
                        cirbhShortHaulTimeStamp,
                        cirbhShortHaulRcvdUtilization,
                        cirbhShortHaulSentUtilization,
                        cirbhShortHaulBulkTimeStamp,
                        cirbhShortHaulBulkBaseUnit,
                        cirbhShortHaulBulkUtil
                    }
    STATUS          obsolete
    DESCRIPTION
        "Cisco IP RAN Utilization History Group."
    ::= { ciscoIpRanBackHaulMIBGroups 12 }

ciscoIpRanBackHaulNotifGroupRev2 NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        ciscoIpRanBackHaulGsmAlarm,
                        ciscoIpRanBackHaulUmtsAlarm
                    }
    STATUS          current
    DESCRIPTION
        "Cisco IP RAN Notifications."
    ::= { ciscoIpRanBackHaulMIBGroups 13 }

ciscoIpRanBackHaulCongestionGroup OBJECT-GROUP
    OBJECTS         {
                        cirbhCongestionEnabled,
                        cirbhCongestionDrops,
                        cirbhCongestionDroppedBytes,
                        cirbhCongestionEvents,
                        cirbhCongestionActive,
                        cirbhCongestionDuration
                    }
    STATUS          current
    DESCRIPTION
        "Cisco IP RAN congestion object group."
    ::= { ciscoIpRanBackHaulMIBGroups 14 }

ciscoIpRanBackHaulGsmErrorsGroup OBJECT-GROUP
    OBJECTS         {
                        cirbhGsmErrorsPeerNotReadyDrops,
                        cirbhGsmErrorsPeerNotActiveDrops,
                        cirbhGsmErrorsInvalidPackets,
                        cirbhGsmErrorsLostRcvdPackets,
                        cirbhGsmErrorsLostSentPackets,
                        cirbhGsmErrorsMissedPackets,
                        cirbhGsmErrorsMissedLatePackets,
                        cirbhGsmErrorsMissedLostPackets,
                        cirbhGsmErrorsMissedNoMemPackets,
                        cirbhGsmErrorsMissedResetPackets,
                        cirbhGsmErrorsDecompFailures,
                        cirbhGsmErrorsCompFailures,
                        cirbhGsmErrorsCompNoPacketFailures,
                        cirbhGsmErrorsCompNoIntFailures,
                        cirbhGsmErrorsCompIntDownFailures,
                        cirbhGsmErrorsCompEncapFailures,
                        cirbhGsmErrorsCompQosDrops,
                        cirbhGsmErrorsFastSendFailures,
                        cirbhGsmErrorsTxPacketFailures,
                        cirbhGsmErrorsTxNoBuffers,
                        cirbhGsmErrorsTxResets,
                        cirbhGsmErrorsOverruns,
                        cirbhGsmErrorsInterruptFailures,
                        cirbhGsmErrorsLateArrivals,
                        cirbhGsmErrorsEarlyArrivals
                    }
    STATUS          current
    DESCRIPTION
        "Cisco GSM-Abis protocol errors Group."
    ::= { ciscoIpRanBackHaulMIBGroups 15 }

ciscoIpRanBackHaulUmtsErrorsGroup OBJECT-GROUP
    OBJECTS         {
                        cirbhUmtsErrorsPeerNotReadyDrops,
                        cirbhUmtsErrorsInvalidPackets,
                        cirbhUmtsErrorsDecompFailures,
                        cirbhUmtsErrorsCompFailures,
                        cirbhUmtsErrorsCompNoPacketFailures,
                        cirbhUmtsErrorsCompNoIntFailures,
                        cirbhUmtsErrorsCompIntDownFailures,
                        cirbhUmtsErrorsCompEncapFailures,
                        cirbhUmtsErrorsCompQosDrops,
                        cirbhUmtsErrorsShorthaulPakFailures,
                        cirbhUmtsErrorsUmtsEncapFailures,
                        cirbhUmtsErrorsLocalPvcDrops,
                        cirbhUmtsErrorsRemotePvcDrops,
                        cirbhUmtsErrorsBackhaulDrops
                    }
    STATUS          current
    DESCRIPTION
        "Cisco UMTS-Iub protocol errors Group."
    ::= { ciscoIpRanBackHaulMIBGroups 16 }

ciscoIpRanBackHaulConfigGroupSup3 OBJECT-GROUP
    OBJECTS         { cirbhInfoOptimizeTraffic }
    STATUS          current
    DESCRIPTION
        "Cisco IP RAN Configuration Group for Optimization."
    ::= { ciscoIpRanBackHaulMIBGroups 17 }

ciscoIpRanBackHaulHistoryGroupRev3 OBJECT-GROUP
    OBJECTS         {
                        cirbhShortHaulBulkTimeStamp,
                        cirbhShortHaulBulkBaseUnit,
                        cirbhShortHaulBulkUtil
                    }
    STATUS          current
    DESCRIPTION
        "Cisco IP RAN Utilization History Group."
    ::= { ciscoIpRanBackHaulMIBGroups 18 }

END

























































































































































































































































































































































































































































































































