-- *****************************************************************
-- IEEE8021-SECY-MIB
--
-- Definitions of managed objects supporting IEEE 802.1AE MACsec.
--
-- January 2006
--
-- *****************************************************************

IEEE8021-SECY-MIB DEFINITIONS ::= BEGIN

-- -----------------------------------------------------------------
-- IEEEE802.1AE MIB
-- -----------------------------------------------------------------

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Unsigned32, Integer32, Counter32,
    Counter64
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, RowPointer, TimeStamp, TruthValue, RowStatus
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    InterfaceIndex
        FROM IF-MIB
    ;

ieee8021SecyMIB MODULE-IDENTITY
    LAST-UPDATED   "200610020000Z"    -- 2 oct 2006
    ORGANIZATION   "IEEE 802.1 Working Group"
    CONTACT-INFO
        "http:/grouper.ieee.org/groups/8021/index.html"
    DESCRIPTION
        "The MAC security entity (SecY) module for managing IEEE
         802.1AE.  An SecY is the entity that operates the MAC Security
         protocol within the system.

         Each SecY transmits frames conveying secure MAC Service
         requests on a single Secure Channel (SC), and receives frames
         conveying secure service indications on separate SCs (one for
         each of the other SecYs participating in the Secure
         Connectivity Association (CA)).  A CA is a security
         relationship, established and maintained by key agreement
         protocols that comprise a fully connected subset of the
         service access points in stations attached to a single MACsec
         supported LAN.  An SC is a security relationship used to
         provide security guarantees for frames transmitted from one
         member of a CA to the others.  It is a unidirectional point to
         multipoint communication, and can be long lived, persisting
         through Secure Association Key (SAK) changes.  Each SC is
         supported by a sequence of Secure Associations (SAs) thus
         allowing the periodic use of fresh keys without terminating
         the relationship.  Each SA is supported by a single secret
         key, or a set of keys where the cryptographic operations used
         to protect one frame require more than one key.

         Two different interfaces 'Controlled Port' and
         'Uncontrolled Port', are associated with a SecY, and that for
         each instance of a SecY, two ifTable rows (one for each
         interface) run on top of an ifTable row representing the
         'Common Port' interface, such as a row with ifType =
         'ethernetCsmacd(6)'.

         For example :

         -----------------------------------------------------------
         |                            |                            |
         |   Controlled Port          |   Uncontrolled Port        |
         |      Interface             |      Interface             |
         |    (ifEntry = j)           |     (ifEntry = k)          |
         | (ifType =                  | (ifType =                  |
         |  macSecControlledIF(231))  |  macSecUncontrolledIF(232))|
         |                            |                            |
         |---------------------------------------------------------|
         |                                                         |
         |                    Physical Interface                   |
         |                      (ifEntry = i)                      |
         |                (ifType = ethernetCsmacd(6))             |
         |_________________________________________________________|
         i, j, k are ifIndex to indicate an interface row in the ifTable.

                         Figure : MACsec Interface Stack

         The 'Controlled Port' is the service point to provide one
         instance of the secure MAC service in a SecY.  The
         'Uncontrolled Port' is the service point to provide one instance
         of the insecure MAC service in a SecY."

    REVISION        "200610020000Z"  -- 2 Oct 2006
    DESCRIPTION
         "Fixed a SYNTAX error in the SEQUENCE of SecyCipherSuiteEntry,
	  the syntax for secyCipherSuiteProtectionOffset is Integer32
	  instead of INTEGER.
	  This error was uncovered after publication of 802.1AE."
    REVISION        "200601100000Z"
    DESCRIPTION
         "Initial version of this MIB module.  Published as part of
          IEEE standard 802.1AE"
    ::= { iso(1) std(0) iso8802(8802) ieee802dot1(1)
          ieee802dot1mibs(1) 3 }

secyMIBNotifications OBJECT IDENTIFIER ::= { ieee8021SecyMIB 0 }

secyMIBObjects OBJECT IDENTIFIER ::= { ieee8021SecyMIB 1 }

secyMIBConformance OBJECT IDENTIFIER ::= { ieee8021SecyMIB 2 }

--
-- Textual Convention
--

SecySCI ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "This textual convention indicates a Secure Channel
         Identifier (SCI).
         
         Each SC is identified by an SCI, comprised of a unique 48-bit
         Universally Administered MAC Address, identifying the system
         to which the transmitting SecY belongs, concatenated with a
         16-bit Port number, identifying the SecY within that system."
    REFERENCE
        "IEEE 802.1AE Clause 7.1.2, 10.7.1 and figure 7.7"
    SYNTAX OCTET STRING (SIZE (8))

SecyAN ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS current
    DESCRIPTION
        "This textual convention indicates an Association Number (AN).

         Each SC is comprised of a succession of SAs, each with a
         different SAK.  Each SA is identified by the SC identifier
         concatenated with a two-bit AN.  The Secure Association
         Identifier (SAI) thus created allows the receiving SecY to
         identify the SA, and the SAK used to decrypt and authenticate
         the received frame. The AN, and the SAI, is only unique for
         the SAs that can be used or recorded by participating SecYs
         at any instant."
    REFERENCE
         "IEEE 802.1AE Clause 8.1.3 and figure 7.7"
    SYNTAX Unsigned32 (0..3)

secyMgmtMIBObjects OBJECT IDENTIFIER ::= { secyMIBObjects 1 }

secyStatsMIBObjects OBJECT IDENTIFIER ::= { secyMIBObjects 2 }

--
-- SecY Management Table
-- 

secyIfTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF SecyIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of system level information for each interface
        supported by the MAC security entity.  An entry appears in this
        table for each interface with MAC security capability in this
        system.

        For the writeable objects in this table, the configured value
        shall be stored in persistent memory and remain unchanged across
        a re-initialization of the management system of the entity."
    REFERENCE
        "IEEE 802.1AE Clause 10.7"
    ::= { secyMgmtMIBObjects 1 }
    
secyIfEntry    OBJECT-TYPE
    SYNTAX      SecyIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
         "An entry containing SecY management information applicable to
          a particular interface."
    INDEX   { secyIfInterfaceIndex }
    ::= { secyIfTable 1 }

SecyIfEntry ::= SEQUENCE {
    secyIfInterfaceIndex               InterfaceIndex,
    secyIfMaxPeerSCs                   Unsigned32,
    secyIfRxMaxKeys                    Unsigned32,
    secyIfTxMaxKeys                    Unsigned32,
    secyIfProtectFramesEnable          TruthValue,
    secyIfValidateFrames               INTEGER,
    secyIfReplayProtectEnable          TruthValue,
    secyIfReplayProtectWindow          Unsigned32,
    secyIfCurrentCipherSuite           Unsigned32,
    secyIfAdminPt2PtMAC                INTEGER,
    secyIfOperPt2PtMAC                 TruthValue,
    secyIfIncludeSCIEnable             TruthValue,
    secyIfUseESEnable                  TruthValue,
    secyIfUseSCBEnable                 TruthValue
}
 
secyIfInterfaceIndex    OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An interface index for a port with SecY management ability.

         This interface index should be aligned with ifIndex in the
         ifTable to point to the SecY Controlled Port entity."
    REFERENCE
        "IEEE 802.1AE Clause 10.1"
    ::= { secyIfEntry 1 }

secyIfMaxPeerSCs    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "security connections"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum number of peer SCs that this SecY can support."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.7"
    ::= { secyIfEntry 2 }

secyIfRxMaxKeys    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "keys"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum number of keys in simultaneous use for reception
         that this SecY can support."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.7"
    ::= { secyIfEntry 3 }

secyIfTxMaxKeys    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "keys"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum number of keys in simultaneous use for transmission
         that this SecY can support."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.16"
    ::= { secyIfEntry 4 }

secyIfProtectFramesEnable    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "An object to enable or disable the protection function for
         egress frames."
    REFERENCE
        "IEEE 802.1AE Clause 10.5"
    DEFVAL { true }
    ::= { secyIfEntry 5 }

secyIfValidateFrames    OBJECT-TYPE
    SYNTAX      INTEGER {
                    disabled(1),
                    check(2),
                    strict(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "An object to control the validation function for ingress
         frames.

         disabled(1) : means to disable the validation function.

         check(2) : means to enable the validation function but only
                    for checking without filtering out invalid frames.

         strict(3) : means to enable the validation function and also
                     strictly filter out those invalid frames."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.8"
    DEFVAL { strict }
    ::= { secyIfEntry 6 }

secyIfReplayProtectEnable    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "An object to enable or disable the replay protection function."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.8, 10.7.17"
    DEFVAL { true }
    ::= { secyIfEntry 7 }

secyIfReplayProtectWindow    OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "Packets"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "An object to indicate the replay protection window size.  This
         object only takes effect if the object secyReplayProtectEnable
         is true."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.8"
    DEFVAL { 0 }
    ::= { secyIfEntry 8 }

secyIfCurrentCipherSuite    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "An object that points to an entry of the secyCipherSuiteTable
         with 'active' row status to indicate the cipher Suite which this
         SecY is currently using.  By default, this object should point
         to the default cipher suite which system provides."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.25"
    ::= { secyIfEntry 9 }

secyIfAdminPt2PtMAC    OBJECT-TYPE
    SYNTAX      INTEGER {
                    forceTrue(1),
                    forceFalse(2),
                    auto(3)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "An object to control the service connectivity to at most one
         other system.  The secyOperPt2PtMAC indicates operational
         status of the service connectivity for this SecY. 

         forceTrue(1) : allows only one service connection to the
                        other system.

         forceFalse(2) : no restriction on the number of service
                         connections to the other systems.

         auto(3) : means the service connectivity is determined by the
                   service providing entity."
    REFERENCE
        "IEEE 802.1AE Clause 6.5"
    DEFVAL { auto }
    ::= { secyIfEntry 10 }

secyIfOperPt2PtMAC    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An object to reflect the current service connectivity status.

         true(1) : means the service connectivity of this SecY provides
                   at most one other system.

         false(2) : means the service connectivity of this SecY could
                    provide more than one other system."
    REFERENCE
        "IEEE 802.1AE Clause 6.5"
    ::= { secyIfEntry 11 }

secyIfIncludeSCIEnable    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "An object indicates to include the SCI information in
         security TAG (SecTAG) field while transmitting MACsec
         frames."
    REFERENCE
        "IEEE 802.1AE Clause 9.3, 10.5.3, 10.7.17"
    DEFVAL { false }
    ::= { secyIfEntry 12 }

secyIfUseESEnable    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "An object indicates to enable the ES bit in
         security TAG (SecTAG) field while transmitting MACsec
         frames."
    REFERENCE
        "IEEE 802.1AE Clause 9.3, 10.5.3, 10.7.17"
    DEFVAL { false }
    ::= { secyIfEntry 13 }

secyIfUseSCBEnable    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "An object indicates to enable the SCB bit in
         security TAG (SecTAG) field while transmitting MACsec
         frames."
    REFERENCE
        "IEEE 802.1AE Clause 9.3, 10.5.3, 10.7.17"
    DEFVAL { false }
    ::= { secyIfEntry 14 }

--
-- Tx SC Management Table
--

secyTxSCTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF SecyTxSCEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table for providing information about the status of each
         transmitting SC supported by the MAC security entity."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.17, 10.7.20"
    ::= { secyMgmtMIBObjects 2 }

secyTxSCEntry    OBJECT-TYPE
    SYNTAX      SecyTxSCEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry containing transmitting SC management information
         applicable to a particular SecY."
    INDEX { secyIfInterfaceIndex }
    ::= { secyTxSCTable 1 }

SecyTxSCEntry ::= SEQUENCE {
    secyTxSCI              SecySCI,
    secyTxSCState          INTEGER,
    secyTxSCEncodingSA     RowPointer,
    secyTxSCEncipheringSA  RowPointer,
    secyTxSCCreatedTime    TimeStamp,
    secyTxSCStartedTime    TimeStamp,
    secyTxSCStoppedTime    TimeStamp
}

secyTxSCI    OBJECT-TYPE
    SYNTAX      SecySCI
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The SCI information for transmitting MACsec frames of the
         transmitting SC in the SecY."
    REFERENCE
        "IEEE 802.1AE Clause 7.1.2, 8.2.1, 10.7.1"
    ::= { secyTxSCEntry 1 }

secyTxSCState    OBJECT-TYPE
    SYNTAX      INTEGER {
                    inUse(1),
                    notInUse(2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The state of the current transmitting SC in the SecY.

         inUse(1) : means any of SAs for this SC is in use.

         notInUse(2) : means no SAs for this SC is in use."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.20"
    ::= { secyTxSCEntry 2 }

secyTxSCEncodingSA    OBJECT-TYPE
    SYNTAX      RowPointer
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current transmitting SA in use.  The row pointer will point
         to an entry in the secyTxSATable.  If no such information is
         available, the value shall be the OBJECT IDENTIFIER { 0 0 }."
    REFERENCE
        "IEEE 802.1AE Clause 10.5.1, 10.7.20"
    ::= { secyTxSCEntry 3 }

secyTxSCEncipheringSA    OBJECT-TYPE
    SYNTAX      RowPointer
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The previous transmitting SA in use.  The row pointer will point
         to an entry in the secyTxSATable.  If no such information is
         available, the value shall be the OBJECT IDENTIFIER { 0 0 }."
    REFERENCE
        "IEEE 802.1AE Clause 10.5.4, 10.7.20"
    ::= { secyTxSCEntry 4 }

secyTxSCCreatedTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system time when this transmitting SC was created."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.20"
    ::= { secyTxSCEntry 5 }

secyTxSCStartedTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system time when this transmitting SC last started
         transmitting MACsec frames."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.20"
    ::= { secyTxSCEntry 6 }

secyTxSCStoppedTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system time when this transmitting SC last stopped
         transmitting MACsec frames."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.20"
    ::= { secyTxSCEntry 7 }

--
-- Tx SA Management Table
--

secyTxSATable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF SecyTxSAEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table for providing information about the status of each
         transmitting SA supported by the MAC security entity."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.21"
    ::= { secyMgmtMIBObjects 3 }

secyTxSAEntry    OBJECT-TYPE
    SYNTAX      SecyTxSAEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry containing transmitting SA management information
         applicable to a particular SA."
    INDEX   { secyIfInterfaceIndex, secyTxSA } 
    ::= { secyTxSATable 1 }

SecyTxSAEntry ::= SEQUENCE {
    secyTxSA                   SecyAN,
    secyTxSAState              INTEGER,
    secyTxSANextPN             Unsigned32,
    secyTxSAConfidentiality    TruthValue,
    secyTxSASAKUnchanged       TruthValue,
    secyTxSACreatedTime        TimeStamp,
    secyTxSAStartedTime        TimeStamp,
    secyTxSAStoppedTime        TimeStamp
}

secyTxSA    OBJECT-TYPE
    SYNTAX      SecyAN
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The association number (AN) for identifying a transmitting
         SA."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.21"
    ::= { secyTxSAEntry 1 }

secyTxSAState    OBJECT-TYPE
    SYNTAX      INTEGER {
                    inUse(1),
                    notInUse(2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current status of the transmitting SA.

         inUse(1) : means this SA is in use.

         notInUse(2) : means this SA is not in use."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.22"
    ::= { secyTxSAEntry 2 }

secyTxSANextPN    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The next packet number (PN) that will be used in transmitting
         MACsec frames in the SA."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.21"
    ::= { secyTxSAEntry 3 }

secyTxSAConfidentiality    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Whether this SA supports the confidentiality as well as
         integrity function in transmitting frames."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.21"
    ::= { secyTxSAEntry 4 }

secyTxSASAKUnchanged    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A reference to an SAK that is unchanged for the life
         of the transmitting SA."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.21"
    ::= { secyTxSAEntry 5 }

secyTxSACreatedTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system time when this transmitting SA was created."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.22"
    ::= { secyTxSAEntry 6 }

secyTxSAStartedTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system time when this transmitting SA last started
         transmitting MACsec frames."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.22"
    ::= { secyTxSAEntry 7 }

secyTxSAStoppedTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system time when this transmitting SA last stopped
         transmitting MACsec frames."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.22"
    ::= { secyTxSAEntry 8 }

--
-- Rx SC Management Table
--

secyRxSCTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF SecyRxSCEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table for providing information about the status of each 
         receiving SC supported by the MAC security entity."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.11"
    ::= { secyMgmtMIBObjects 4 }

secyRxSCEntry    OBJECT-TYPE
    SYNTAX      SecyRxSCEntry  
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry containing receiving SC management information
         applicable to a particular SC."
    INDEX    { secyIfInterfaceIndex, secyRxSCI } 
    ::= { secyRxSCTable 1 }

SecyRxSCEntry ::= SEQUENCE {
    secyRxSCI              SecySCI,
    secyRxSCState          INTEGER,
    secyRxSCCurrentSA      RowPointer,
    secyRxSCCreatedTime    TimeStamp, 
    secyRxSCStartedTime    TimeStamp, 
    secyRxSCStoppedTime    TimeStamp
}

secyRxSCI    OBJECT-TYPE
    SYNTAX      SecySCI
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The SCI for identifying the receiving SC in the SecY."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.11"
    ::= { secyRxSCEntry 1 }

secyRxSCState    OBJECT-TYPE
    SYNTAX      INTEGER {
                    inUse(1),
                    notInUse(2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The state of the receiving SC in the SecY.

         inUse(1) : means any of SAs for this SC is in use.

         notInUse(2) : means no SAs for this SC is in use."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.12"
    ::= { secyRxSCEntry 2 }

secyRxSCCurrentSA    OBJECT-TYPE
    SYNTAX      RowPointer
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current receiving association number of the SC in use.
         The row pointer will point to an entry in the
         secyRxSATable.  If no such information can be identified,
         the value of this object shall be set to the
         OBJECT IDENTIFIER { 0 0 }."
    REFERENCE
        "IEEE 802.1AE Clause 10.6.1, 10.7.13"
    ::= { secyRxSCEntry 3 }

secyRxSCCreatedTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system time when this receiving SC was created."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.12"
    ::= { secyRxSCEntry 4 }

secyRxSCStartedTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system time when this receiving SC last started
         receiving MACsec frames."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.12"
    ::= { secyRxSCEntry 5 }

secyRxSCStoppedTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system time when this receiving SC last stopped
         receiving MACsec frames."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.12"
    ::= { secyRxSCEntry 6 }

--
-- Rx SA Management Table
--

secyRxSATable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF SecyRxSAEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table for providing information about the status of each
         receiving SA supported by the MAC security entity."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.13"
    ::= { secyMgmtMIBObjects 5 }

secyRxSAEntry    OBJECT-TYPE
    SYNTAX      SecyRxSAEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry containing receiving SA management information
         applicable to a particular SA."
    INDEX    { secyIfInterfaceIndex, secyRxSCI, secyRxSA }
    ::= { secyRxSATable 1 }

SecyRxSAEntry ::= SEQUENCE {
    secyRxSA               SecyAN,
    secyRxSAState          INTEGER,
    secyRxSANextPN         Unsigned32,
    secyRxSASAKUnchanged   TruthValue,
    secyRxSACreatedTime    TimeStamp,
    secyRxSAStartedTime    TimeStamp,
    secyRxSAStoppedTime    TimeStamp
}

secyRxSA    OBJECT-TYPE
    SYNTAX      SecyAN
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The association number (AN) for identifying a receiving
         SA."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.13"
    ::= { secyRxSAEntry 1 }

secyRxSAState    OBJECT-TYPE
    SYNTAX      INTEGER {
                    inUse(1),
                    notInUse(2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current state for the receiving SA."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.14"
    ::= { secyRxSAEntry 2 }

secyRxSANextPN    OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The stored packet number (PN) for replay protection
         in the SA.  If the PN of any receiving frames is less
         than the value of this object minus the value of
         secyReplayProtectWindow and secyReplayProtectEnable
         is true, the receiving frames should be discarded."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.14, Clause 10.7.15"
    ::= { secyRxSAEntry 3 }

secyRxSASAKUnchanged    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A reference to an SAK that is unchanged for the life
         of the receiving SA."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.13"
    ::= { secyRxSAEntry 4 }

secyRxSACreatedTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system time when this receiving SA was created."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.14"
    ::= { secyRxSAEntry 5 }

secyRxSAStartedTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system time when this receiving SA last started
         receiving MACsec frames."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.14"
    ::= { secyRxSAEntry 6 }

secyRxSAStoppedTime    OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The system time when this receiving SA last stopped
         receiving MACsec frames."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.14"
    ::= { secyRxSAEntry 7 }

--
--  SecY Selectable Cipher Suites
--

secyCipherSuiteTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF SecyCipherSuiteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table of selectable cipher suites for the MAC security
         entity.

        For the writeable objects in this table, the configured value
        shall be stored in persistent memory and remain unchanged across
        a re-initialization of the management system of the entity."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.24"
    ::= { secyMgmtMIBObjects 6 }

secyCipherSuiteEntry    OBJECT-TYPE
    SYNTAX      SecyCipherSuiteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry containing the management information for a cipher
         suite."
    INDEX { secyCipherSuiteIndex }
    ::= { secyCipherSuiteTable 1 }

SecyCipherSuiteEntry ::= SEQUENCE {
    secyCipherSuiteIndex               Unsigned32,
    secyCipherSuiteId                  OCTET STRING,
    secyCipherSuiteName                SnmpAdminString,
    secyCipherSuiteCapability          BITS,
    secyCipherSuiteProtection          BITS,
    secyCipherSuiteProtectionOffset    Integer32,
    secyCipherSuiteDataLengthChange    TruthValue,
    secyCipherSuiteICVLength           Unsigned32,
    secyCipherSuiteRowStatus           RowStatus
}

secyCipherSuiteIndex    OBJECT-TYPE
    SYNTAX      Unsigned32 (1..4294967295)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index to recognize a Cipher Suite in the system."
    ::= { secyCipherSuiteEntry 1 }

secyCipherSuiteId    OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (8))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The identifier for the cipher suite.  This is a global
         unique 64-bit (EUI-64) identifier."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.24"
    ::= { secyCipherSuiteEntry 2 }

secyCipherSuiteName    OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE (1..128))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The name of the cipher suite.  If the name is composed of
         multi-byte characters, the total length must fit within 128
         octets."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.24"
    ::= { secyCipherSuiteEntry 3 }

secyCipherSuiteCapability    OBJECT-TYPE
    SYNTAX      BITS {
                    integrity(0),
                    confidentiality(1),
                    offsetConfidentiality(2)
                }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The capability of this cipher suite.

         integrity(0) : integrity protection capability for this
             cipher suite..

         confidentiality(1) : confidentiality protection
             capability for this cipher suite.

         offsetConfidentiality(2) : offset confidentiality protection
             capability for this cipher suite."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.24, 10.7.25"
    ::= { secyCipherSuiteEntry 4 }

secyCipherSuiteProtection    OBJECT-TYPE
    SYNTAX      BITS {
                    integrity(0),
                    confidentiality(1),
                    offsetConfidentiality(2)
                }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The protection options of this cipher suite.  The options
         should depend on the object secyCipherSuiteCapability.

         If the value of secyCipherSuiteCapability is only integerity
         bit on, users can only choose to turn on integrity bit for
         this object.

         If the value of secyCipherSuiteCapability is integrity and
         confidentiality bits on, users can choose to turn on
         integrity or confidentiality bits, but if confidentiality
         bit is on, the integrity bit has to be on.

         If the value of secyCipherSuiteCapability is integrity and
         offsetConfidentiality bits on, users can choose to turn on
         integrity or offsetConfidentiality bits, but if
         offsetConfidentiality bit is on, the integrity bit has to be
         on.

         If the value of secyCipherSuiteCapability is integrity and
         confidentiality and offsetConfidentiality bits on, users can
         choose to turn on integrity or confidentiality or 
         offsetConfidentiality bits, but if confidentiality or
         offsetConfidentiality bits are on, the integrity bit has to
         be on.

         integrity(0) : on or off the function of supporting integrity
             protection for this cipher suite.

         confidentiality(1) : on or off the function of supporting
             confidentiality for this cipher suite.

         offsetConfidentiality(2) : on or off the function of
             supporting offset confidentiality for this cipher suite."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.24, 10.7.25"
    DEFVAL { { integrity } }
    ::= { secyCipherSuiteEntry 5 }

secyCipherSuiteProtectionOffset    OBJECT-TYPE
    SYNTAX      Integer32 (0 | 30 | 50)
    UNITS       "bytes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The confidentiality protection offset options of this
         cipher suite.  The options should depend on the choice of
         secyCipherSuiteProtection.

         If the value of secyCipherSuiteProtection only turns on
         integrity bit, users can only choose 0 byte for this
         object.

         If the value of secyCipherSuiteProtection only turns on
         integrity and confidentiality bits, users can only choose
         0 byte for this object.

         If the value of secyCipherSuiteProtection only turns on
         integrity and offsetConfidentiality bits, users can choose
         30 or 50 bytes for this object.

         If the value of secyCipherSuiteProtection turns on
         integrity and confidentiality and offsetConfidentiality
         bits, users can choose 0 or 30 or 50 bytes for this object."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.24, 10.7.25"
    DEFVAL { 0 }
    ::= { secyCipherSuiteEntry 6 }

secyCipherSuiteDataLengthChange    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This indicates whether the data length will be
         changed after encryption by the cipher suite."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.24"
    ::= { secyCipherSuiteEntry 7 }

secyCipherSuiteICVLength    OBJECT-TYPE
    SYNTAX      Unsigned32 (8..16)
    UNITS       "octets"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The length of integrity check value (ICV) field."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.24"
    ::= { secyCipherSuiteEntry 8 }

secyCipherSuiteRowStatus    OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object to create the paramaters for the supported
         Cipher Suites in the system.  If the specified
         secyCipherSuiteId object information is not supported
         in the system or the secyCipherSuiteCapability object
         is not matched the capability of the corresponding
         specified Cipher Suite in the same entry, the corresponding
         entry should not be active, i.e., this object should not be
         'active' or 'notInService'."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.24"
    ::= { secyCipherSuiteEntry 9 }

--
-- Statistics Information
--

--
-- TX SA Statistics Information
--

secyTxSAStatsTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF SecyTxSAStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains the statistics objects for each
         transmitting SA in the MAC security entity."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.18, figure 10.4"
    ::= { secyStatsMIBObjects 1 }

secyTxSAStatsEntry    OBJECT-TYPE
    SYNTAX      SecyTxSAStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The entry holds the statistics for a transmitting SA.  An SA
         may be reused once a while.

         When starting using the SA, the counters of the SA should
         start at 0.

         When stopping using the SA, the counters will be stopped
         incrementing.

         The timestamps of starting and stopping time are recorded in
         the secyTxSATable."
    AUGMENTS { secyTxSAEntry }
    ::= { secyTxSAStatsTable 1 }

SecyTxSAStatsEntry ::= SEQUENCE {
    secyTxSAStatsProtectedPkts    Counter32,
    secyTxSAStatsEncryptedPkts    Counter32
}

secyTxSAStatsProtectedPkts    OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of integrity protected but not encrypted packets
         for this transmitting SA."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.18, figure 10.4"
    ::= { secyTxSAStatsEntry 1 }

secyTxSAStatsEncryptedPkts    OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of integrity protected and encrypted packets for
         this transmitting SA."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.18, figure 10.4"
    ::= { secyTxSAStatsEntry 2 }

--
-- TX SC Statistics Information
--

secyTxSCStatsTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF SecyTxSCStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains statistics information for each
         transmitting SC in the MAC security entity."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.18, 10.7.19, figure 10.4"
    ::= { secyStatsMIBObjects 2 }

secyTxSCStatsEntry    OBJECT-TYPE
    SYNTAX      SecyTxSCStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The entry contains the counters of a transmitting SC.  Since some
         counters in the transmitting SA will be reset while the SA is
         reused, in order to maintain complete statistics information
         for the SC, the counters information on the SAs need to be kept
         in the SC.

         Those counters that may be reset are :
         secyTxSAStatsProtectedPkts,
         secyTxSAStatsEncryptedPkts

         Each counter for a SC is in the summation of the corresponding
         counter information for all the SAs, current and prior SAs,
         belonging to this SC."
    AUGMENTS { secyTxSCEntry }
    ::= { secyTxSCStatsTable 1 }

SecyTxSCStatsEntry ::= SEQUENCE {
    secyTxSCStatsProtectedPkts      Counter64,
    secyTxSCStatsEncryptedPkts      Counter64,
    secyTxSCStatsOctetsProtected    Counter64,
    secyTxSCStatsOctetsEncrypted    Counter64
}

secyTxSCStatsProtectedPkts    OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of integrity protected but not encrypted packets
         for this transmitting SC."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.18, figure 10.4"
    ::= { secyTxSCStatsEntry 1 }

secyTxSCStatsEncryptedPkts    OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of integrity protected and encrypted packets for
         this transmitting SC."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.18, figure 10.4"
    ::= { secyTxSCStatsEntry 4 }

secyTxSCStatsOctetsProtected    OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Octets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of plain text octets that are integrity protected
         but not encrypted on the transmitting SC."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.19, figure 10.4"
    ::= { secyTxSCStatsEntry 10 }

secyTxSCStatsOctetsEncrypted    OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Octets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of plain text octets that are integrity protected
         and encrypted on the transmitting SC."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.19, figure 10.4"
    ::= { secyTxSCStatsEntry 11 }

--
-- RX SA Statistics Information
--

secyRxSAStatsTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF SecyRxSAStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table that contains the statistics objects for each
         receiving SA in the MAC security entity."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyStatsMIBObjects 3 }

secyRxSAStatsEntry    OBJECT-TYPE
    SYNTAX      SecyRxSAStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The entry holds the statistics for a receiving SA.  An SA
         may be reused once a while.

         When starting using the SA, the counters of the SA should
         start at 0.

         When stopping using the SA, the counters will be stopped
         incrementing.

         The timestamps of starting and stopping time are recorded in
         the secyRxSATable."
    AUGMENTS { secyRxSAEntry }
    ::= { secyRxSAStatsTable 1 }    

SecyRxSAStatsEntry ::= SEQUENCE {
    secyRxSAStatsUnusedSAPkts    Counter32,
    secyRxSAStatsNoUsingSAPkts   Counter32,
    secyRxSAStatsNotValidPkts    Counter32,
    secyRxSAStatsInvalidPkts     Counter32,
    secyRxSAStatsOKPkts          Counter32
}

secyRxSAStatsUnusedSAPkts    OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "For this SA which is not currently in use, the number of
         received, unencrypted, packets with secyValidateFrames
         not in the strict mode."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyRxSAStatsEntry 1 }

secyRxSAStatsNoUsingSAPkts   OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "For this SA which is not currently in use, the number of
         received packets that have been discarded, and have
         either the packets encrypted or the secyValidateFrames set to
         strict mode."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyRxSAStatsEntry 4 }

secyRxSAStatsNotValidPkts     OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "For this SA, the number discarded packets with the
         condition that the packets are not valid and one of the
         following conditions are true: either secyValidateFrames in
         strict mode or the packets encrypted."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyRxSAStatsEntry 13 }

secyRxSAStatsInvalidPkts     OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "For this SA, the number of packets with the condition
         that the packets are not valid and secyValidateFrames is in
         check mode."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyRxSAStatsEntry 16 }

secyRxSAStatsOKPkts          OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "For this SA, the number of validated packets."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyRxSAStatsEntry 25 }

--
-- RX SC Statistics Information
--

secyRxSCStatsTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF SecyRxSCStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table for the statistics information of each receiving SC
         supported by the MAC security entity."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, 10.7.10, figure 10.5"
    ::= { secyStatsMIBObjects 4 }

secyRxSCStatsEntry    OBJECT-TYPE
    SYNTAX      SecyRxSCStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The entry contains the counters of a receiving SC.  Since some
         counters in the receiving SA will be reset while the SA is
         reused, in order to maintain complete statistics information
         for the SC, the counters information on the SAs need to be kept
         in the SC.

         Those counters that may be reset are :
         secyRxSAStatsUnusedSAPkts,
         secyRxSAStatsNoUsingSAPkts,
         secyRxSAStatsNotValidPkts,
         secyRxSAStatsInvalidPkts,
         secyRxSAStatsOKPkts

         Each counter for a SC is in the summation of the corresponding
         counter information for all the SAs, current and prior SAs,
         belonging to this SC."
    AUGMENTS { secyRxSCEntry }
    ::= { secyRxSCStatsTable 1 }

SecyRxSCStatsEntry ::= SEQUENCE {
    secyRxSCStatsUnusedSAPkts         Counter64,
    secyRxSCStatsNoUsingSAPkts        Counter64,
    secyRxSCStatsLatePkts             Counter64,
    secyRxSCStatsNotValidPkts         Counter64,
    secyRxSCStatsInvalidPkts          Counter64,
    secyRxSCStatsDelayedPkts          Counter64,
    secyRxSCStatsUncheckedPkts        Counter64,
    secyRxSCStatsOKPkts               Counter64,
    secyRxSCStatsOctetsValidated      Counter64,
    secyRxSCStatsOctetsDecrypted      Counter64
}

secyRxSCStatsUnusedSAPkts    OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The summation of counter secyRxSAStatsUnusedSAPkts
         information for all the SAs which belong to this SC.

         Since the secyRxSAStatsUnusedSAPkts counters in the SAs
         will be reset, in order to maintain complete statistics
         information for the SC, the counter information on the SAs
         need to be kept in the SC."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyRxSCStatsEntry 1 }

secyRxSCStatsNoUsingSAPkts    OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The summation of counter secyRxSAStatsNoUsingSAPkts 
         information for all the SAs which belong to this SC.

         Since the secyRxSAStatsNoUsingSAPkts counters in the SAs
         will be reset, in order to maintain complete statistics        
         information for the SC, the counter information on the SAs     
         need to be kept in the SC."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyRxSCStatsEntry 2 }

secyRxSCStatsLatePkts        OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "For this SC, the number of received packets that have
         been discarded with the condition : secyReplayProtect is equal
         to true and the PN of the packet is lower than the lower bound
         replay check PN."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyRxSCStatsEntry 3 }

secyRxSCStatsNotValidPkts     OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The summation of counter secyRxSAStatsNotValidPkts
         information for all the SAs which belong to this SC.

         Since the secyRxSAStatsNotValidPkts counters in the SAs
         will be reset, in order to maintain complete statistics        
         information for the SC, the counter information on the SAs     
         need to be kept in the SC."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyRxSCStatsEntry 4 }

secyRxSCStatsInvalidPkts     OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The summation of counter secyRxSAStatsInvalidPkts
         information for all the SAs which belong to this SC.

         Since the secyRxSAStatsInvalidPkts counters in the SAs
         will be reset, in order to maintain complete statistics        
         information for the SC, the counter information on the SAs     
         need to be kept in the SC."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyRxSCStatsEntry 5 }

secyRxSCStatsDelayedPkts     OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "For this SC, the number of packets with the condition
         that the PN of the packets is lower than the lower bound
         replay protection PN."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyRxSCStatsEntry 6 }

secyRxSCStatsUncheckedPkts   OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "For this SC, the number of packets with the following
         condition:
         -secyValidateFrames is disabled or
         -secyValidateFrames is not disabled and the packet is not
         encrypted and the integrity check has failed or
         -secyValidateFrames is not disable and the packet is
         encrypted and integrity check has failed."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyRxSCStatsEntry 7 }

secyRxSCStatsOKPkts          OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The summation of counter secyRxSAStatsOKPkts
         information for all the SAs which belong to this SC.

         Since the secyRxSAStatsOKPkts counters in the SAs
         will be reset, in order to maintain complete statistics        
         information for the SC, the counter information on the SAs     
         need to be kept in the SC."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, figure 10.5"
    ::= { secyRxSCStatsEntry 8 }

secyRxSCStatsOctetsValidated     OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Octets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of octets of plaintext recovered from received
         packets that were integrity protected but not encrypted."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.10, figure 10.5"
    ::= { secyRxSCStatsEntry 9 }

secyRxSCStatsOctetsDecrypted    OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Octets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of octets of plaintext recovered from received
         packets that were integrity protected and encrypted."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.10, figure 10.5"
    ::= { secyRxSCStatsEntry 10 }

--
-- SecY statistics table
--

secyStatsTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF SecyStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table for the statistics information of each SecY supported by
         the MAC security entity."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9, 10.7.18, figure 10.4, 10.5"
    ::= { secyStatsMIBObjects 5 }

secyStatsEntry    OBJECT-TYPE
    SYNTAX      SecyStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry containing counters for statistics or diagnosis for
         a SecY."
    AUGMENTS { secyIfEntry }
    ::= { secyStatsTable 1 }

SecyStatsEntry ::= SEQUENCE {
    secyStatsTxUntaggedPkts     Counter64,
    secyStatsTxTooLongPkts      Counter64,
    secyStatsRxUntaggedPkts     Counter64,
    secyStatsRxNoTagPkts        Counter64,
    secyStatsRxBadTagPkts       Counter64,
    secyStatsRxUnknownSCIPkts   Counter64,
    secyStatsRxNoSCIPkts        Counter64,
    secyStatsRxOverrunPkts      Counter64
}

secyStatsTxUntaggedPkts    OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of transmitted packets without the MAC
         security tag (SecTAG) because secyProtectFramesEnable is
         configured as false."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.18, figure 10.4"
    ::= { secyStatsEntry 1 }

secyStatsTxTooLongPkts    OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of transmitted packets discarded because the packet
         length is greater than the ifMtu of the Common Port interface."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.18, figure 10.4"
    ::= { secyStatsEntry 2 }

secyStatsRxUntaggedPkts    OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of received packets without the MAC security tag
         (SecTAG) with secyValidateFrames which is not in the 
         strict mode."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9 , figure 10.5"
    ::= { secyStatsEntry 3 }

secyStatsRxNoTagPkts       OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of received packets discarded without the
         MAC security tag (SecTAG) with secyValidateFrames which is
         in the strict mode."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9 , figure 10.5"
    ::= { secyStatsEntry 4 }

secyStatsRxBadTagPkts      OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of received packets discarded with an invalid
         SecTAG or a zero value PN or an invalid ICV."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9 , figure 10.5"
    ::= { secyStatsEntry 5 }

secyStatsRxUnknownSCIPkts  OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of received packets with unknown SCI with the
         condition :
         secyValidateFrames is not in the strict mode and the
         C bit in the SecTAG is not set."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9 , figure 10.5"
    ::= { secyStatsEntry 6 }

secyStatsRxNoSCIPkts       OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of received packets discarded with unknown SCI
         information with the condition :
         secyValidateFrames is in the strict mode or the C bit
         in the SecTAG is set."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9 , figure 10.5"
    ::= { secyStatsEntry 7 }

secyStatsRxOverrunPkts       OBJECT-TYPE
    SYNTAX      Counter64
    UNITS       "Packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets discarded because the number of
         received packets exceeded the cryptographic performance
         capabilities."
    REFERENCE
        "IEEE 802.1AE Clause 10.7.9 , figure 10.5"
    ::= { secyStatsEntry 8 }

--
-- Conformance
--

secyMIBCompliances  OBJECT IDENTIFIER ::= { secyMIBConformance 1 }

secyMIBGroups  OBJECT IDENTIFIER ::= { secyMIBConformance 2 }

-- Compliance

secyMIBCompliance MODULE-COMPLIANCE
    STATUS current
    DESCRIPTION
        "The compliance statement for entities which implement
         the IEEE8021-SECY-MIB."
    MODULE  -- this module
        MANDATORY-GROUPS {
            secyIfCtrlGroup,
            secyTxSCGroup,
            secyTxSAGroup,
            secyRxSCGroup,
            secyRxSAGroup,
            secyCipherSuiteGroup,
            secyTxSAStatsGroup,
            secyTxSCStatsGroup,
            secyRxSAStatsGroup,
            secyRxSCStatsGroup, 
            secyStatsGroup
        }

        OBJECT secyIfCurrentCipherSuite
            MIN-ACCESS    read-only
            DESCRIPTION
                "write access is not required.  This may be
                 read-only."

        OBJECT    secyCipherSuiteId
            MIN-ACCESS    read-only
            DESCRIPTION
                "read-create access is not required.  This may be
                 read-only."

        OBJECT    secyCipherSuiteName
            MIN-ACCESS    read-only
            DESCRIPTION
                "read-create access is not required.  This may be
                 read-only."

        OBJECT    secyCipherSuiteCapability
            MIN-ACCESS    read-only
            DESCRIPTION
                "read-create access is not required.  This may be
                 read-only."

        OBJECT    secyCipherSuiteProtection
            MIN-ACCESS    read-only
            DESCRIPTION
                "read-create access is not required.  This may be
                 read-only."

        OBJECT    secyCipherSuiteProtectionOffset
            MIN-ACCESS    read-only
            DESCRIPTION
                "read-create access is not required.  This may be
                 read-only."

        OBJECT    secyCipherSuiteDataLengthChange
            MIN-ACCESS    read-only
            DESCRIPTION
                "read-create access is not required.  This may be
                 read-only."

        OBJECT    secyCipherSuiteICVLength
            MIN-ACCESS    read-only
            DESCRIPTION
                "read-create access is not required.  This may be
                 read-only."

        OBJECT    secyCipherSuiteRowStatus
            MIN-ACCESS    read-only
            DESCRIPTION
                "read-create access is not required.  This may be
                 read-only."

    ::= { secyMIBCompliances 1 }

-- Units of Conformance

secyIfCtrlGroup    OBJECT-GROUP
    OBJECTS {
        secyIfMaxPeerSCs,
        secyIfRxMaxKeys,
        secyIfTxMaxKeys,
        secyIfProtectFramesEnable,
        secyIfValidateFrames,
        secyIfReplayProtectEnable,
        secyIfReplayProtectWindow,
        secyIfCurrentCipherSuite,
        secyIfAdminPt2PtMAC,
        secyIfOperPt2PtMAC,
        secyIfIncludeSCIEnable,
        secyIfUseESEnable,
        secyIfUseSCBEnable
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing a SecY control management
         information."
    ::= { secyMIBGroups 1 }

secyTxSCGroup    OBJECT-GROUP
    OBJECTS {
        secyTxSCI,
        secyTxSCState,
        secyTxSCEncodingSA,
        secyTxSCEncipheringSA,
        secyTxSCCreatedTime,
        secyTxSCStartedTime,
        secyTxSCStoppedTime
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing a transmitting SC control
         management information."
    ::= { secyMIBGroups 2 }

secyTxSAGroup    OBJECT-GROUP
    OBJECTS {
        secyTxSAState,
        secyTxSANextPN,
        secyTxSAConfidentiality,
        secyTxSASAKUnchanged,
        secyTxSACreatedTime,
        secyTxSAStartedTime,
        secyTxSAStoppedTime
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing a transmitting SA control
         management information."
    ::= { secyMIBGroups 3 }

secyRxSCGroup    OBJECT-GROUP
    OBJECTS {
        secyRxSCState,
        secyRxSCCurrentSA,
        secyRxSCCreatedTime,
        secyRxSCStartedTime,
        secyRxSCStoppedTime
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing a receiving SC control
         management information."
    ::= { secyMIBGroups 4 }

secyRxSAGroup    OBJECT-GROUP
    OBJECTS {
        secyRxSAState,
        secyRxSANextPN,
        secyRxSASAKUnchanged,
        secyRxSACreatedTime,
        secyRxSAStartedTime,
        secyRxSAStoppedTime
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing a receiving SA control
         management information."
    ::= { secyMIBGroups 5 }

secyCipherSuiteGroup    OBJECT-GROUP
    OBJECTS {
        secyCipherSuiteId,
        secyCipherSuiteName,
        secyCipherSuiteCapability,
        secyCipherSuiteProtection,
        secyCipherSuiteProtectionOffset,
        secyCipherSuiteDataLengthChange,
        secyCipherSuiteICVLength,
        secyCipherSuiteRowStatus
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing a cipher suite information."
    ::= { secyMIBGroups 6 }

secyTxSAStatsGroup    OBJECT-GROUP
    OBJECTS {
        secyTxSAStatsProtectedPkts,
        secyTxSAStatsEncryptedPkts
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing a transmitting SA statistics
         information."
    ::= { secyMIBGroups 7 }

secyRxSAStatsGroup    OBJECT-GROUP
    OBJECTS {
        secyRxSAStatsUnusedSAPkts,
        secyRxSAStatsNoUsingSAPkts,
        secyRxSAStatsNotValidPkts,
        secyRxSAStatsInvalidPkts,
        secyRxSAStatsOKPkts
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing a receiving SA statistics
         information."
    ::= { secyMIBGroups 8 }

secyTxSCStatsGroup    OBJECT-GROUP
    OBJECTS {
        secyTxSCStatsProtectedPkts,
        secyTxSCStatsEncryptedPkts,
        secyTxSCStatsOctetsProtected,
        secyTxSCStatsOctetsEncrypted
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing a transmitting SC statistics
         information."
    ::= { secyMIBGroups 9 }

secyRxSCStatsGroup    OBJECT-GROUP
    OBJECTS {
        secyRxSCStatsUnusedSAPkts,
        secyRxSCStatsNoUsingSAPkts,
        secyRxSCStatsLatePkts,
        secyRxSCStatsNotValidPkts,
        secyRxSCStatsInvalidPkts,
        secyRxSCStatsDelayedPkts,
        secyRxSCStatsUncheckedPkts,
        secyRxSCStatsOKPkts,
        secyRxSCStatsOctetsValidated,
        secyRxSCStatsOctetsDecrypted
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing a receiving SC statistics
         information."
    ::= { secyMIBGroups 10 }

secyStatsGroup    OBJECT-GROUP
    OBJECTS {
        secyStatsTxUntaggedPkts,
        secyStatsTxTooLongPkts,
        secyStatsRxUntaggedPkts,
        secyStatsRxNoTagPkts,
        secyStatsRxBadTagPkts,
        secyStatsRxUnknownSCIPkts,
        secyStatsRxNoSCIPkts,
        secyStatsRxOverrunPkts
    }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing a SecY statistics
         information."
    ::= { secyMIBGroups 11 }

END


