-- *****************************************************************
-- CISCO-ENTITY-DIAG-MIB
-- Definitions of managed objects supporting the Online
-- Diagnostic Feature
--   
-- November 2002, Patrick Gili
-- October  2005, Jayakumar Kadirvelu
--   
-- Copyright (c) 2002-2010, 2016 by Cisco Systems Inc.
-- All rights reserved.
-- ****************************************************************

CISCO-ENTITY-DIAG-MIB DEFINITIONS ::= BEGIN

IMPORTS
    OBJECT-GROUP,
    MODULE-COMPLIANCE,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    Unsigned32,
    Gauge32,
    Integer32,
    Counter32,
    OBJECT-TYPE,
    MODULE-IDENTITY,
    NOTIFICATION-TYPE
        FROM SNMPv2-SMI
    entPhysicalIndex,
    PhysicalIndex,
    entPhysicalDescr
        FROM ENTITY-MIB
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    DateAndTime,
    TruthValue,
    RowStatus
        FROM SNMPv2-TC
    EntPhysicalIndexOrZero
        FROM CISCO-TC
    CeDiagDiagnosticLevel,
    CeDiagDiagnosticMethod,
    CeDiagTestIdentifier,
    CeDiagErrorIdentifier,
    CeDiagErrorIdentifierOrZero,
    CeDiagJobIdentifier,
    CeDiagPortList,
    CeDiagTestList,
    CeDiagJobSuite
        FROM CISCO-ENTITY-DIAG-TC-MIB
    ciscoMgmt
        FROM CISCO-SMI;


ciscoEntityDiagMIB MODULE-IDENTITY
    LAST-UPDATED    "201603110000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
            San Jose, CA 95134

            Tel: +1 800 553-NETS

            E-mail: cs-snmp@cisco.com"
    DESCRIPTION
        "This MIB module defines the managed objects that describe the
        online diagnostics capabilities supported by the
        physical entities contained by the system, including chassis,
        modules, ports, power supplies, fans, and sensors.  In order to
        manage the online diagnostic capabilities supported by
        a physical entity, it must be represented by a conceptual row
        in the entPhysicalTable of the ENTITY-MIB (RFC-2737).

        GLOSSARY

        Boot-up Diagnostic - a diagnostic consisting of tests intended
        to be executed in a reasonable timeframe when a physical entity
        boots.

        Diagnostic - a suite of tests intended to exercise the
        functional integrity of a physical entity.

        Diagnostic Level - the degree of completeness that a diagnostic
        will exercise a physical entity.

        Field Diagnostic - a special suite of tests intended to
        exercise the functional integrity of a physical entity in a
        manner that is possible when a physical entity is
        operational or running an operational image.

        Field Diagnostic Image - an image supporting field diagnostics.
        A physical entity has to be loaded with a field diagnostic
        image before field diagnostics can be executed on the physical
        entity.

        Health Monitoring - the process of running special
        non-intrusive online tests periodically on a physical entity
        for the purpose of tracking the overall condition of a physical
        entity.

        On-Demand Diagnostic - a diagnostic intended to be executed
        immediately upon request.

        Offline Diagnostic - a diagnostic that consists of tests that
        are disruptive in nature, and thus requires the physical entity
        being evaluated to be taken offline for the duration.

        Online Diagnostic - a diagnostic that consists of tests that
        are not disruptive in nature, and thus can be done without
        taking the physical entity offline.

        Physical Entity - an identifiable physical resource, such as a
        chassis, line card, power supply, or communication port.  See
        RFC-2737, 'Entity MIB (Version 2)', K. McCloghrie and A.
        Bierman.

        Scheduled Diagnostic - a diagnostic intended to execute at some
        time in the future.  There exist two types of scheduled
        diagnostics: 1) one-shot, which execute only once; and 2)
        periodic, which executes at a specific interval.

        Test - an exercise intended to determine the functional
        integrity of a component comprising a physical entity (e.g., a
        port might support an internal loopback test).

        Diagnostic Job - Consists of a diagnostic suite 
        (i.e., a collection of tests) to be executed by a physical
        entity."
    REVISION        "201603110000Z"
    DESCRIPTION
        "Added one new enumaration value disruptive(15)
        to ceDiagTestAttributes"
    REVISION        "201005260000Z"
    DESCRIPTION
        "Added ceDiagHMTestThreshWindowGroup."
    REVISION        "200906300000Z"
    DESCRIPTION
        "Added ceDiagTestPerfLastTestMethodGroup.
        Updated Description of ceDiagTestPerfLastErrorID object."
    REVISION        "200803120000Z"
    DESCRIPTION
        "Added ceDiagNotifControlGroup, ceDiagNotifErrorMsgGroup
        and ceDiagNotificationGroup."
    REVISION        "200701090000Z"
    DESCRIPTION
        "Initial version of this MIB."
    ::= { ciscoMgmt 350 }


ciscoEntityDiagMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIB 0 }

ciscoEntityDiagMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIB 1 }

ciscoEntityDiagMIBConform  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIB 2 }

ceDiagDescriptions  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIBObjects 1 }

ceDiagGlobalConfig  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIBObjects 2 }

ceDiagEntity  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIBObjects 3 }

ceDiagOnDemand  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIBObjects 4 }

ceDiagScheduled  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIBObjects 5 }

ceDiagTest  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIBObjects 6 }

ceDiagHealthMonitor  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIBObjects 7 }

ceDiagEvents  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIBObjects 8 }

ceDiagNotificationControl  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIBObjects 9 }

-- DiagDescriptions

ceDiagTestInfoTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeDiagTestInfoEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table describes the tests supported by each physical
        entity supporting online diagnostics.  The table
        organizes tests into sets associated with the physical entity
        supporting those tests.

        The SNMP entity adds a set of tests corresponding to a physical
        entity upon detection of a physical entity supporting
        online diagnostics.

        The SNMP entity deletes a set of tests corresponding to a
        physical entity upon removal of the physical entity.

        The SNMP entity replaces a set of tests corresponding to a
        physical entity when the physical entity has been successfully
        loaded with a different image (e.g., the field diagnostic
        image)."
    ::= { ceDiagDescriptions 1 }

ceDiagTestInfoEntry OBJECT-TYPE
    SYNTAX          CeDiagTestInfoEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The description of a single test supported by a corresponding
        physical entity."
    INDEX           {
                        entPhysicalIndex,
                        ceDiagTestId
                    } 
    ::= { ceDiagTestInfoTable 1 }

CeDiagTestInfoEntry ::= SEQUENCE {
        ceDiagTestId         CeDiagTestIdentifier,
        ceDiagTestText       SnmpAdminString,
        ceDiagTestAttributes BITS
}

ceDiagTestId OBJECT-TYPE
    SYNTAX          CeDiagTestIdentifier
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates an arbitrary positive integer
        arbitrarily identifying the test." 
    ::= { ceDiagTestInfoEntry 1 }

ceDiagTestText OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates a human-readable description of the
        test.  Examples include:

        'Marching Pattern DRAM Test'

        'Data Pins DRAM Test'

        'Internal Loopback Test'

        'External Loopback Test'" 
    ::= { ceDiagTestInfoEntry 2 }

ceDiagTestAttributes OBJECT-TYPE
    SYNTAX          BITS {
                        minimal(0),
                        complete(1),
                        perPort(2),
                        fatal(3),
                        basicOnDemand(4),
                        standby(5),
                        parallel(6),
                        nonDisruptive(7),
                        hmAlwaysEnable(8),
                        hmFixedInterval(9),
                        nonHM(10),
                        proxy(11),
                        activeToStandby(12),
                        offline(13),
                        perDevice(14),
                        disruptive(15)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates a set of attributes characterizing the
        test:

        'minimal'         - indicates that this test will be executed
                            during boot-up if ceDiagBootupLevel is set
                            to 'minimal' or 'complete'. This test is 
                            also included in the minimal or complete
                            test suites.

        'complete'        - indicates that this test will be executed
                            during boot-up if ceDiagBootupLevel is set
                            to 'complete'. This test is also included
                            in the complete test suites.

        'perPort'         - indicates that this test is a executed for
                            each port contained by the module. This
                            test is also included in the perPort test
                            suites.

        'fatal'           - indicates that if this test fails, then the
                            diagnostic should fail indicating that a
                            major error occurred.

        'basicOnDemand'   - indicates that this test will be
                            run during the basic on demand job is run.

        'standby'         - indicates that this test can only be run
                            if the physical entity is a standby unit
                            and can only be executed from the standby
                            unit.

        'parallel'        - indicates that this test can be executed in
                            parallel with other tests without checking
                            for resource availability.

        'nonDisruptive'   - indicates this test can be executed without
                            disrupting the physical entity's normal
                            operation. This test is also included in 
                            the nonDisruptive test suites.

        'hmAlwaysEnabled' - indicates that a management application can
                            not disable the use of this test for the
                            purpose of health monitoring.

        'hmFixedInterval' - indicates that a management application can
                            not change the interval at which health
                            monitoring executes this test.

        'nonHM'           - indicates that this test can not be used for
                            health monitoring.

        'proxy'           - indicates that the test must be executed
                            through a proxy.

        'activeToStandby' - indicates that this test can only be run if
                            the physical entity is a standby unit and
                            can only be executed from the active unit.

        'offline'         - indicates that this test will not get a user
                            confirmation when it is run.

        'perDevice'       - indicates that this test is a per device test.

        'disruptive'      - indicates that this test can be executed with
                            disrupting the physical entity's normal
                            operation. This test is also included in 
                            the disruptive test suites." 
    ::= { ceDiagTestInfoEntry 3 }
 


ceDiagTestCustomAttributeTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeDiagTestCustomAttributeEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table describes the additional custom based attributes
        of the tests listed in ceDiagTestInfoTable. These are attributes
        which have been customized by the platform supporting the tests."
    ::= { ceDiagDescriptions 2 }

ceDiagTestCustomAttributeEntry OBJECT-TYPE
    SYNTAX          CeDiagTestCustomAttributeEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The description of a single custom based attribute for a test
        supported by a corresponding physical entity."
    INDEX           {
                        entPhysicalIndex,
                        ceDiagTestId,
                        ceDiagTestCustomAttributeIndex
                    } 
    ::= { ceDiagTestCustomAttributeTable 1 }

CeDiagTestCustomAttributeEntry ::= SEQUENCE {
        ceDiagTestCustomAttributeIndex Unsigned32,
        ceDiagTestCustomAttributeDesc  SnmpAdminString
}

ceDiagTestCustomAttributeIndex OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An arbitrary integer which identifies the custom based attribute
        of a test." 
    ::= { ceDiagTestCustomAttributeEntry 1 }

ceDiagTestCustomAttributeDesc OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides a textual description of the custom based
        attribute of this test." 
    ::= { ceDiagTestCustomAttributeEntry 2 }
 


ceDiagErrorInfoTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeDiagErrorInfoEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table describes the errors indicated by a system
        supporting online diagnostics."
    ::= { ceDiagDescriptions 3 }

ceDiagErrorInfoEntry OBJECT-TYPE
    SYNTAX          CeDiagErrorInfoEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The description of a single online error."
    INDEX           { ceDiagErrorId } 
    ::= { ceDiagErrorInfoTable 1 }

CeDiagErrorInfoEntry ::= SEQUENCE {
        ceDiagErrorId   CeDiagErrorIdentifier,
        ceDiagErrorText SnmpAdminString
}

ceDiagErrorId OBJECT-TYPE
    SYNTAX          CeDiagErrorIdentifier
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates an arbitrary positive integer
        arbitrarily identifying the error." 
    ::= { ceDiagErrorInfoEntry 1 }

ceDiagErrorText OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates a human-readable description of the
        error.  Examples include:

        'DIAG_SUCCESS'

        'DIAG_FAILURE'

        'DIAG_NOT_SUPPORT'

        'DIAG_SKIPPED'" 
    ::= { ceDiagErrorInfoEntry 2 }
 


-- DiagGlobalConfig

ceDiagBootupLevel OBJECT-TYPE
    SYNTAX          CeDiagDiagnosticLevel
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the level that physical entities will
        execute their boot-up diagnostic."
    DEFVAL          { minimal } 
    ::= { ceDiagGlobalConfig 1 }
-- DiagEntity

ceDiagEntityTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeDiagEntityEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table supports online diagnostic control and
        status for each physical entity that supporting the feature.

        The SNMP entity adds a conceptual row to this table
        corresponding to a physical entity upon detection of a physical
        entity supporting online diagnostics.

        The SNMP entity deletes a conceptual row from this table
        corresponding to a physical entity upon removal of the physical
        entity."
    ::= { ceDiagEntity 1 }

ceDiagEntityEntry OBJECT-TYPE
    SYNTAX          CeDiagEntityEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Online diagnostic control and status for a single
        physical entity supporting the feature.  Observe that this data
        may not be accurate if the corresponding cefcModuleOperStatus
        (see the CISCO-ENTITY-FRU-CONTROL-MIB for further details) has
        a value of 'boot'."
    INDEX           { entPhysicalIndex } 
    ::= { ceDiagEntityTable 1 }

CeDiagEntityEntry ::= SEQUENCE {
        ceDiagEntityBootLevel          CeDiagDiagnosticLevel,
        ceDiagEntityImageAdminStatus   INTEGER,
        ceDiagEntityImageOperStatus    INTEGER,
        ceDiagEntityFieldDiagnosticUrl SnmpAdminString
}

ceDiagEntityBootLevel OBJECT-TYPE
    SYNTAX          CeDiagDiagnosticLevel
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the level that the physical entity
        executed its boot-up diagnostic." 
    ::= { ceDiagEntityEntry 1 }

ceDiagEntityImageAdminStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        operational(1),
                        fieldDiagnostic(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the desired image the physical entity
        should be running:

        'operational'     - the physical entity should be running the
                            operational image.

        'fieldDiagnostic' - the physical entity should be running the
                            field diagnostic image."
    DEFVAL          { operational } 
    ::= { ceDiagEntityEntry 2 }

ceDiagEntityImageOperStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        operational(1),
                        fieldDiagnostic(2),
                        booting(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the actual image the physical entity is
        running:

        'operational'     - the physical entity is running the
                            operational image.

        'fieldDiagnostic' - the physical entity is running the field
                            diagnostic image.

        'booting'         - the physical entity is booting; that is,
                            there is no way of determining what image
                            the physical entity is running because it
                            is currently booting." 
    ::= { ceDiagEntityEntry 3 }

ceDiagEntityFieldDiagnosticUrl OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies a URL (see RFC-1630) that specifies the
        location of the field diagnostic image.  The following list
        provides some examples of URLs for the field diagnostic:

        file://disk0:/images/fd001
            Describes a file with the path '/images/fd001' on 'disk0:'
            accessed locally.

        ftp://pop-server/usr/bin/fd001
            Describes a file with the path '/usr/bin/fd001' on the host
           'pop-server' accessed via FTP.

        tftp://pop-server/tftpout/fd001
            Describes a file with the path '/tftpout/fd001' on the host
            'pop-server' accessed via TFTP."
    REFERENCE
        "RFC-1630, 'Universal Resource Identifiers in WWW', T.
        Berners-Lee." 
    ::= { ceDiagEntityEntry 4 }
 


ceDiagEntityCurrentTestTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeDiagEntityCurrentTestEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the current test
        executing on a physical entity."
    ::= { ceDiagEntity 2 }

ceDiagEntityCurrentTestEntry OBJECT-TYPE
    SYNTAX          CeDiagEntityCurrentTestEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A test which is currently executing on a particular physical
        entity."
    INDEX           {
                        entPhysicalIndex,
                        ceDiagTestId
                    } 
    ::= { ceDiagEntityCurrentTestTable 1 }

CeDiagEntityCurrentTestEntry ::= SEQUENCE {
        ceDiagEntityCurrentTestMethod CeDiagDiagnosticMethod
}

ceDiagEntityCurrentTestMethod OBJECT-TYPE
    SYNTAX          CeDiagDiagnosticMethod
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the method used to invoke the diagnostic
        that is executing this test." 
    ::= { ceDiagEntityCurrentTestEntry 1 }
 


-- DiagOnDemand

ceDiagOnDemandErrorAllowed OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the number of errors the physical
        entities will allow before aborting an on demand diagnostic job.
        A value of '0' indicates that the an unlimited number of
        errors are allowed for the on demand diagnostic job." 
    ::= { ceDiagOnDemand 1 }

ceDiagOnDemandErrorAction OBJECT-TYPE
    SYNTAX          INTEGER  {
                        continue(1),
                        stop(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies how the physical entities in the
        system are to proceed when they encounter an error during
        an on demand diagnostic job.

        'continue' - indicates that the physical entities will continue
                     executing the on demand job.

        'stop'     - indicates that the physical entities will abort
                     the on demand job." 
    ::= { ceDiagOnDemand 2 }

ceDiagOnDemandIterations OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the maximum number of iterations of an
        on demand job." 
    ::= { ceDiagOnDemand 3 }

ceDiagOnDemandJobTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeDiagOnDemandJobEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains a list of on demand jobs currently in the
        system.

        A row in this table can be created by setting the corresponding
        instance of ceDiagOnDemandJobRowStatus to 'createAndGo'.
        A row can be deleted by setting the corresponding instance of
        ceDiagOnDemandJobRowStatus to 'destroy'.  Once the job is
        completed the corresponding row is deleted from the table.

        The individual results of the tests executed by this job are
        updated in ceDiagTestPerfTable."
    ::= { ceDiagOnDemand 4 }

ceDiagOnDemandJobEntry OBJECT-TYPE
    SYNTAX          CeDiagOnDemandJobEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A on demand job currently executing on a particular physical
        entity which supports on demand diagnostics."
    INDEX           { entPhysicalIndex } 
    ::= { ceDiagOnDemandJobTable 1 }

CeDiagOnDemandJobEntry ::= SEQUENCE {
        ceDiagOnDemandJobSuite     CeDiagJobSuite,
        ceDiagOnDemandJobTestList  CeDiagTestList,
        ceDiagOnDemandJobPortList  CeDiagPortList,
        ceDiagOnDemandJobRowStatus RowStatus
}

ceDiagOnDemandJobSuite OBJECT-TYPE
    SYNTAX          CeDiagJobSuite
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates the various system predefined test
        suites the on demand job can choose from. 

        If the value of this object is 'none', this job will run
        the tests specified by ceDiagOnDemandJobTestList.
        If the value of this object is 'complete', 'minimal', 
        'nonDisruptive' or 'perPort' the value of  
        ceDiagOnDemandJobTestList is ignored." 
    ::= { ceDiagOnDemandJobEntry 1 }

ceDiagOnDemandJobTestList OBJECT-TYPE
    SYNTAX          CeDiagTestList
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the user specified diagnostic suite
        (i.e., a set of tests) to be executed by the corresponding
        physical entity.

        The set of tests supported by this physical entity are
        specified in ceDiagTestInfoTable." 
    ::= { ceDiagOnDemandJobEntry 2 }

ceDiagOnDemandJobPortList OBJECT-TYPE
    SYNTAX          CeDiagPortList
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the list of ports to be exercised by the
        corresponding physical entity when executing the diagnostic
        suite specified for the job." 
    ::= { ceDiagOnDemandJobEntry 3 }

ceDiagOnDemandJobRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The status object used to manage the rows in this table.
        When set to active(1) the on demand job is submitted.
        When set to destroy(6) the on demand job is stopped.
        When the value of this object is 'active', values within
        this row cannot be modified, except by deleting and 
        re-creating the row." 
    ::= { ceDiagOnDemandJobEntry 4 }
 

-- DiagScheduled

ceDiagScheduledJobTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeDiagScheduledJobEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains a list of scheduled jobs on the system.
        A row in this table can be created by setting the corresponding
        instance of ceDiagScheduledJobRowStatus to 'createAndGo'.
        A row can be deleted by setting the corresponding instance of
        ceDiagScheduledJobRowStatus to 'destroy'.  Once the job is
        completed the corresponding row is deleted from the table.
        The individual results of the tests executed by this job are
        updated in ceDiagTestPerfTable."
    ::= { ceDiagScheduled 1 }

ceDiagScheduledJobEntry OBJECT-TYPE
    SYNTAX          CeDiagScheduledJobEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A job currently scheduled on a particular physical
        entity."
    INDEX           {
                        entPhysicalIndex,
                        ceDiagScheduledJobIndex
                    } 
    ::= { ceDiagScheduledJobTable 1 }

CeDiagScheduledJobEntry ::= SEQUENCE {
        ceDiagScheduledJobIndex     CeDiagJobIdentifier,
        ceDiagScheduledJobType      INTEGER,
        ceDiagScheduledJobStart     DateAndTime,
        ceDiagScheduledJobDayOfWeek INTEGER,
        ceDiagScheduledJobTestList  CeDiagTestList,
        ceDiagScheduledJobPortList  CeDiagPortList,
        ceDiagScheduledJobRowStatus RowStatus,
        ceDiagScheduledJobSuite     CeDiagJobSuite
}

ceDiagScheduledJobIndex OBJECT-TYPE
    SYNTAX          CeDiagJobIdentifier
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An arbitrary non-zero integer value that uniquely identifies a
        single scheduled job with respect to a physical entity." 
    ::= { ceDiagScheduledJobEntry 1 }

ceDiagScheduledJobType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        scheduledOneShot(1),
                        scheduledPeriodicDaily(2),
                        scheduledPeriodicWeekly(3)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the type of the scheduled job.

        'scheduledOneShot'        - the physical entity will invoke
                                    this job at the time specified
                                    by ceDiagScheduledJobStart.

        'scheduledPeriodicDaily'  - the physical entity will
                                    first invoke this job at the time
                                    specified by 
                                    ceDiagScheduledJobStart and 
                                    continue invoking it daily at the
                                    same time.

        'scheduledPeriodicWeekly' - the corresponding physical entity 
                                    will first invoke this job at the
                                    time and day of the week specified 
                                    by ceDiagScheduledJobStart and
                                    ceDiagScheduledJobDayOfWeek, and
                                    continue to invoke it weekly at
                                    the same time and day." 
    ::= { ceDiagScheduledJobEntry 2 }

ceDiagScheduledJobStart OBJECT-TYPE
    SYNTAX          DateAndTime
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies when a scheduled job will be executed.

        If the value of ceDiagScheduledJobType is 'scheduledOneShot',
        then this object only applies to the first execution of the job.

        If the value of ceDiagScheduledJobType is
        'scheduledPeriodicDaily' or 'scheduledPeriodicWeekly', then the
         first four octets of this objects should be zero.

        If the physical entity's job queue already contains a job
        scheduled for execution at this time, then the process of
        submitting the job will fail." 
    ::= { ceDiagScheduledJobEntry 3 }

ceDiagScheduledJobDayOfWeek OBJECT-TYPE
    SYNTAX          INTEGER  {
                        sunday(1),
                        monday(2),
                        tuesday(3),
                        wednesday(4),
                        thursday(5),
                        friday(6),
                        saturday(7),
                        notApplicable(8)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the day of the week for a
        weekly periodic scheduled job.  The value of
        of this object must be specified if the value of
        ceDiagScheduledJobType is 'scheduledPeriodicWeekly'. 

        This value of this object is set to 'notApplicable' 
        if the value of ceDiagScheduledJobType is 'scheduledOneShot'
        or  'scheduledPeriodicDaily'." 
    ::= { ceDiagScheduledJobEntry 4 }

ceDiagScheduledJobTestList OBJECT-TYPE
    SYNTAX          CeDiagTestList
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the diagnostic suite (i.e., a set of
        tests) to be executed by the corresponding physical entity.

        The set of tests supported by this physical entity are
        specified in ceDiagTestInfoTable." 
    ::= { ceDiagScheduledJobEntry 5 }

ceDiagScheduledJobPortList OBJECT-TYPE
    SYNTAX          CeDiagPortList
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the list of ports to be tested by the
        corresponding physical entity when executing the diagnostic
        suite specified for the job." 
    ::= { ceDiagScheduledJobEntry 6 }

ceDiagScheduledJobRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The status object used to manage the rows in this table.
        When set to 'active' the scheduled job is submitted.
        When set to destroy(6) the scheduled job is cleared.
        When the value of this object is 'active', values within
        this row cannot be modified, except by deleting and 
        re-creating the row." 
    ::= { ceDiagScheduledJobEntry 7 }

ceDiagScheduledJobSuite OBJECT-TYPE
    SYNTAX          CeDiagJobSuite
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates the various system predefined test
        suites the on scheduled job can choose from. 

        If the value of this object is 'none', this job will run
        the tests specified by ceDiagScheduledJobTestList.
        If the value of this object is 'complete', 'minimal', 
        'nonDisruptive' or 'perPort' the value of  
        ceDiagScheduledJobTestList is ignored." 
    ::= { ceDiagScheduledJobEntry 8 }
 

-- DiagTest

ceDiagTestPerfTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeDiagTestPerfEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table maintains data concerning the performance of tests
        executed by each physical entity supporting the online
        diagnostic feature.  The table organizes tests into sets
        associated with the physical entity supporting those tests.

        The SNMP entity adds a set of tests corresponding to a physical
        entity upon detection of a physical entity supporting
        online diagnostics.

        The SNMP entity deletes a set of tests corresponding to a
        physical entity upon removal of the physical entity.

        The SNMP entity replaces a set of tests corresponding to a
        physical entity when the physical entity has been successfully
        loaded with a different image (e.g., the field diagnostic
        image)."
    ::= { ceDiagTest 1 }

ceDiagTestPerfEntry OBJECT-TYPE
    SYNTAX          CeDiagTestPerfEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Data concerning the performance of a single test."
    INDEX           {
                        entPhysicalIndex,
                        ceDiagTestId
                    } 
    ::= { ceDiagTestPerfTable 1 }

CeDiagTestPerfEntry ::= SEQUENCE {
        ceDiagTestPerfLastResult       INTEGER,
        ceDiagTestPerfLastErrorID      CeDiagErrorIdentifierOrZero,
        ceDiagTestPerfLastRun          DateAndTime,
        ceDiagTestPerfFirstFail        DateAndTime,
        ceDiagTestPerfLastSuccess      DateAndTime,
        ceDiagTestPeffLastFail         DateAndTime,
        ceDiagTestPerfTotalRuns        Counter32,
        ceDiagTestPerfTotalFails       Counter32,
        ceDiagTestPerfConsecutiveFails Gauge32,
        ceDiagTestPerfLastTestMethod   CeDiagDiagnosticMethod
}

ceDiagTestPerfLastResult OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        fail(2),
                        pass(3),
                        skipped(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the result the last time this test was
        executed by the corresponding physical entity:

        'unknown' - the corresponding physical entity has not executed
                    the test.

        'fail'    - the test executed and detected at least one
                    failure.

        'pass'    - the test executed without detecting a failure.

        'skipped' - the test was skipped due to insufficient resources." 
    ::= { ceDiagTestPerfEntry 1 }

ceDiagTestPerfLastErrorID OBJECT-TYPE
    SYNTAX          CeDiagErrorIdentifierOrZero
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the last error code of this test.
        Details of the non-zero error code can be found in the
        corresponding entry in ceDiagErrorInfoTable." 
    ::= { ceDiagTestPerfEntry 2 }

ceDiagTestPerfLastRun OBJECT-TYPE
    SYNTAX          DateAndTime
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the last time the
        corresponding physical entity executed this test.  If the value
        of ceDiagTestPerfLastResult is 'unknown', then the value of
        this object is irrelevant." 
    ::= { ceDiagTestPerfEntry 3 }

ceDiagTestPerfFirstFail OBJECT-TYPE
    SYNTAX          DateAndTime
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the first time
        the corresponding physical entity executed this test and it
        failed.  The value of this object is irrelevant if the value of 
        ceDiagTestPerfTotalFails is 0." 
    ::= { ceDiagTestPerfEntry 4 }

ceDiagTestPerfLastSuccess OBJECT-TYPE
    SYNTAX          DateAndTime
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the last time the
        corresponding physical entity executed this test and 
        it passed. The value 0x0000010100000000 indicates 
        that the corresponding physical entity has not 
        passed this test yet." 
    ::= { ceDiagTestPerfEntry 5 }

ceDiagTestPeffLastFail OBJECT-TYPE
    SYNTAX          DateAndTime
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the last time the
        corresponding physical entity executed this test and it failed.
        If the value of ceDiagTestPerfTotalFails is 0, then the value 
        of this object is irrelevant." 
    ::= { ceDiagTestPerfEntry 6 }

ceDiagTestPerfTotalRuns OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of times the
        corresponding physical entity has executed the test." 
    ::= { ceDiagTestPerfEntry 7 }

ceDiagTestPerfTotalFails OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of times the
        corresponding physical entity has executed the test and the
        test resulted with a failure." 
    ::= { ceDiagTestPerfEntry 8 }

ceDiagTestPerfConsecutiveFails OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the consecutive number of times the
        corresponding physical entity has executed the test and it has
        failed.  The value of this object will be reset to '0' when the
        physical entity executes the test and it succeeds." 
    ::= { ceDiagTestPerfEntry 9 }

ceDiagTestPerfLastTestMethod OBJECT-TYPE
    SYNTAX          CeDiagDiagnosticMethod
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the testing method used for the
        last time this test was executed by the corresponding 
        physical entity." 
    ::= { ceDiagTestPerfEntry 10 }
 


-- DiagHealthMonitor

ceDiagHMSyslogEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the system will generate
        syslog messages due to the tests run by health
        monitor." 
    ::= { ceDiagHealthMonitor 1 }

ceDiagHMTestTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeDiagHMTestEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table describes attributes specific to the health monitor
        for tests supported by a physical entity."
    ::= { ceDiagHealthMonitor 2 }

ceDiagHMTestEntry OBJECT-TYPE
    SYNTAX          CeDiagHMTestEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The attributes of a single test specific to the health
        monitor."
    INDEX           {
                        entPhysicalIndex,
                        ceDiagTestId
                    } 
    ::= { ceDiagHMTestTable 1 }

CeDiagHMTestEntry ::= SEQUENCE {
        ceDiagHMTestEnabled           TruthValue,
        ceDiagHMTestIntervalMin       Unsigned32,
        ceDiagHMTestIntervalDefault   Unsigned32,
        ceDiagHMTestInterval          Unsigned32,
        ceDiagHMTestThresholdDefault  Unsigned32,
        ceDiagHMTestThreshold         Unsigned32,
        ceDiagHMTestThreshWindowSuite INTEGER,
        ceDiagHMTestThreshWindowSize  Unsigned32
}

ceDiagHMTestEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether this test is enabled for
        health monitor." 
    ::= { ceDiagHMTestEntry 1 }

ceDiagHMTestIntervalMin OBJECT-TYPE
    SYNTAX          Unsigned32 (0..2147483647)
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the minimum interval which the health
        monitor can periodically invoke this test." 
    ::= { ceDiagHMTestEntry 2 }

ceDiagHMTestIntervalDefault OBJECT-TYPE
    SYNTAX          Unsigned32 (0..2147483647)
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the default interval which the health
        monitor will periodically invoke this test.  A value of '0'
        indicates that the health monitor will not invoke the test." 
    ::= { ceDiagHMTestEntry 3 }

ceDiagHMTestInterval OBJECT-TYPE
    SYNTAX          Unsigned32 (0..2147483647)
    UNITS           "milliseconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the interval at which the health monitor
        periodically invokes this test.  A value of '0' indicates that
        the health monitor will not invoke the test.  A value of '0'
        cannot be set." 
    ::= { ceDiagHMTestEntry 4 }

ceDiagHMTestThresholdDefault OBJECT-TYPE
    SYNTAX          Unsigned32 (0..2147483647)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the default consecutive failure
        count threshold.  When the specified failure count threshold
        is reached, the diagnostic test result is set to failure. 
        A value of '0' indicates that the health monitor will not
        invoke this test." 
    ::= { ceDiagHMTestEntry 5 }

ceDiagHMTestThreshold OBJECT-TYPE
    SYNTAX          Unsigned32 (0..2147483647)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the consecutive failure count threshold
        for this test.  When the specified failure count threshold is
        reached, the diagnostic test result is set to failure.

        A value of '0' indicates that there is no failure count
        threshold for this test.

        This object is used in combination with
        ceDiagHMTestThreshWindowSuite and ceDiagHMTestThreshWindowSize
        to specify a sliding history window for which the threshold
        is monitored. 

        When the value of ceDiagHMTestThreshWindowSuite is
        'default', the sliding history window is in number of test
        runs, with a window size the same as the value of this
        object.

        If ceDiagHMTestThreshWindowSuite and 
        ceDiagHMTestThreshWindowSize are not supported, the failure
        count threshold will be the consecutive failure count threshold." 
    ::= { ceDiagHMTestEntry 6 }

ceDiagHMTestThreshWindowSuite OBJECT-TYPE
    SYNTAX          INTEGER  {
                        default(1),
                        milliseconds(2),
                        seconds(3),
                        minutes(4),
                        hours(5),
                        days(6),
                        runs(7)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies a sliding history window
        parameter which is used in combination with 
        ceDiagHMTestThreshold. When the specified failure count
        threshold is reached in this sliding history window, 
        the diagnostic test result is set to failure.

        'default'      - The sliding history window is in number
                         of test runs or executions, with a window
                         size the same as ceDiagHMTestThreshold.

        'milliseconds' - The sliding history window is in milli-seconds
                         specified by ceDiagHMTestThreshWindowSize.

        'seconds'      - The sliding history window is in seconds
                         specified by ceDiagHMTestThreshWindowSize.

        'minutes'      - The sliding history window is in minutes
                         specified by ceDiagHMTestThreshWindowSize.

        'hours'        - The sliding history window is in hours
                         specified by ceDiagHMTestThreshWindowSize.

        'days'         - The sliding history window is in days
                         specified by ceDiagHMTestThreshWindowSize.

        'runs'         - The sliding history window is in number
                         of test runs or executions specified by
                         ceDiagHMTestThreshWindowSize.

        When the value of this object is 'default' the user cannot set
        any value for ceDiagHMTestThreshWindowSize.
        When the value of this object is not 'default', 
        then the value of ceDiagHMTestThreshWindowSize cannot be zero (0)." 
    ::= { ceDiagHMTestEntry 7 }

ceDiagHMTestThreshWindowSize OBJECT-TYPE
    SYNTAX          Unsigned32 (0..2147483647)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates the sliding history window size.

        When the value of ceDiagHMTestThreshWindowSuite is 'default', the
        user cannot set any value for this object.

        The value of zero (0) cannot be set." 
    ::= { ceDiagHMTestEntry 8 }
 


-- DiagEvents

ceDiagEventLogSize OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the maximum number of entries which the
        event log buffer can contain." 
    ::= { ceDiagEvents 1 }

ceDiagEventCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the number of entries currently stored
        in the event log buffer." 
    ::= { ceDiagEvents 2 }

ceDiagEventMaxQueries OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Maximum number of query entries allowed in the
        ceDiagEventQueryTable." 
    ::= { ceDiagEvents 3 }

ceDiagEventQueryTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeDiagEventQueryEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A control table used to query the event log buffer. Each row
        instance in the table represents a query with its parameters.
        The resulting data for each instance of a query in this table
        is stored in the ceDiagEventResultTable.

        A row in this table can be created by setting the corresponding
        instance of ceDiagEventQueryStatus to 'createAndGo'.
        A row can be deleted by setting the corresponding instance of
        ceDiagEventQueryStatus to 'destroy'."
    ::= { ceDiagEvents 4 }

ceDiagEventQueryEntry OBJECT-TYPE
    SYNTAX          CeDiagEventQueryEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A conceptual row of the ceDiagEventQueryTable used to setup
        a event log buffer query to search for diagnostic events.
        The actual search is started by when the value of
        ceDiagEventQueryStatus is set to 'active'."
    INDEX           { ceDiagEventQueryIndex } 
    ::= { ceDiagEventQueryTable 1 }

CeDiagEventQueryEntry ::= SEQUENCE {
        ceDiagEventQueryIndex         Unsigned32,
        ceDiagEventQueryPhysicalIndex EntPhysicalIndexOrZero,
        ceDiagEventQuerySeverity      INTEGER,
        ceDiagEventQueryOwner         SnmpAdminString,
        ceDiagEventQueryResultingRows Integer32,
        ceDiagEventQueryStatus        RowStatus
}

ceDiagEventQueryIndex OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An arbitrary integer in the range of 1 to
        ceDiagEventMaxQueries to identify this control query." 
    ::= { ceDiagEventQueryEntry 1 }

ceDiagEventQueryPhysicalIndex OBJECT-TYPE
    SYNTAX          EntPhysicalIndexOrZero
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the physical entity for the event
        log buffer query. A value of zero indicates that the 
        query will return events of all physical entities." 
    ::= { ceDiagEventQueryEntry 2 }

ceDiagEventQuerySeverity OBJECT-TYPE
    SYNTAX          INTEGER  {
                        all(0),
                        info(1),
                        warning(2),
                        error(3)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the severity of the event log buffer
        query. A value of 'all' indicates that the search will return
        events of all severities." 
    ::= { ceDiagEventQueryEntry 3 }

ceDiagEventQueryOwner OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The manager entity that configured this entry and is therefore
        using the resources assigned to it.  It is used to model an
        administratively assigned name of the owner of a resource.
        It is recommended that this object have one or more the following
        information: IP address, management station name, network
        manager's name, location, or phone number." 
    ::= { ceDiagEventQueryEntry 4 }

ceDiagEventQueryResultingRows OBJECT-TYPE
    SYNTAX          Integer32 (-1..2147483647)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The result status of the query. Possible values are:

        -1            - Either the query has not been initiated or 
                        the agent is busy processing this query instance.
                        Time to completion of the query processing
                        depends on the complexity of the query and
                        the number of matches that satisfy this query.

        0..2147483647 - The search has ended and this is the number of 
                        rows in the ceDiagEventResultTable, resulting 
                        from this query." 
    ::= { ceDiagEventQueryEntry 5 }

ceDiagEventQueryStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The status object used to manage rows in this table.
        When set to 'active', the query to search for diagnostic 
        events is initiated. Once a row becomes active, values
        within the row cannot be modified, except by deleting
        and re-creating the row." 
    ::= { ceDiagEventQueryEntry 6 }
 


ceDiagEventResultTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeDiagEventResultEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table containing event log information corresponding
        to all the completed queries set up in ceDiagEventQueryTable.
        The query result will not become available until the current
        search is completed."
    ::= { ceDiagEvents 5 }

ceDiagEventResultEntry OBJECT-TYPE
    SYNTAX          CeDiagEventResultEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A conceptual row in ceDiagEventResultTable, containing
        information about an event that matches the search criteria
        set in the corresponding row of ceDiagEventQueryTable."
    INDEX           {
                        ceDiagEventQueryIndex,
                        ceDiagEventResultIndex
                    } 
    ::= { ceDiagEventResultTable 1 }

CeDiagEventResultEntry ::= SEQUENCE {
        ceDiagEventResultIndex         Unsigned32,
        ceDiagEventResultPhysicalIndex PhysicalIndex,
        ceDiagEventResultPhysicalDescr SnmpAdminString,
        ceDiagEventResultTime          DateAndTime,
        ceDiagEventResultSeverity      INTEGER,
        ceDiagEventResultLogText       SnmpAdminString
}

ceDiagEventResultIndex OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A positive integer which uniquely identifies a result
        entry matching a particular query." 
    ::= { ceDiagEventResultEntry 1 }

ceDiagEventResultPhysicalIndex OBJECT-TYPE
    SYNTAX          PhysicalIndex
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the physical entity corresponding
        to this event." 
    ::= { ceDiagEventResultEntry 2 }

ceDiagEventResultPhysicalDescr OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies a textual description of physical
        entity corresponding to this event." 
    ::= { ceDiagEventResultEntry 3 }

ceDiagEventResultTime OBJECT-TYPE
    SYNTAX          DateAndTime
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the time at which this event occurred." 
    ::= { ceDiagEventResultEntry 4 }

ceDiagEventResultSeverity OBJECT-TYPE
    SYNTAX          INTEGER  {
                        info(1),
                        warning(2),
                        error(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the severity of this event." 
    ::= { ceDiagEventResultEntry 5 }

ceDiagEventResultLogText OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The text message of this event." 
    ::= { ceDiagEventResultEntry 6 }
 


ceDiagEventErrorMsg OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "The error message related to the notification." 
    ::= { ceDiagEvents 6 }

-- Notification Control

ceDiagEnableBootUpFailedNotif OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This variable specifies whether the system produces the
        ceDiagBootUpFailedNotif.  A 'false' value will prevent
        ceDiagBootUpFailedNotif notifications from being
        generated by this system." 
    ::= { ceDiagNotificationControl 1 }

ceDiagEnableHMThreshReachedNotif OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This variable specifies whether the system produces the
        ceDiagHMThresholdReachedNotif.  A 'false' value will prevent
        ceDiagHMThresholdReachedNotif notifications from being
        generated by this system." 
    ::= { ceDiagNotificationControl 2 }

ceDiagEnableHMTestRecoverNotif OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This variable specifies whether the system produces the
        ceDiagHMTestRecoverNotif.  A 'false' value will prevent
        ceDiagHMTestRecoverNotif notifications from being
        generated by this system." 
    ::= { ceDiagNotificationControl 3 }

ceDiagEnableSchedTestFailedNotif OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This variable specifies whether the system produces the
        ceDiagScheduledTestFailedNotif.  A 'false' value will prevent
        ceDiagScheduledTestFailedNotif notifications from being
        generated by this system." 
    ::= { ceDiagNotificationControl 4 }

-- Notifications

ceDiagBootUpFailedNotif NOTIFICATION-TYPE
    OBJECTS         {
                        entPhysicalDescr,
                        ceDiagEntityBootLevel,
                        ceDiagEventErrorMsg
                    }
    STATUS          current
    DESCRIPTION
        "A ceDiagBootUpFailedNotif is sent if the online diagnostic
        discovers a boot up failure for a physical entity."
   ::= { ciscoEntityDiagMIBNotifs 1 }

ceDiagHMThresholdReachedNotif NOTIFICATION-TYPE
    OBJECTS         {
                        entPhysicalDescr,
                        ceDiagHMTestThreshold,
                        ceDiagTestText,
                        ceDiagTestAttributes
                    }
    STATUS          current
    DESCRIPTION
        "A ceDiagHMThresholdReachedNotif is sent if the number of
        consecutive failure of a Health Monitoring test reaches
        the configured threshold."
   ::= { ciscoEntityDiagMIBNotifs 2 }

ceDiagHMTestRecoverNotif NOTIFICATION-TYPE
    OBJECTS         {
                        entPhysicalDescr,
                        ceDiagTestText,
                        ceDiagTestAttributes
                    }
    STATUS          current
    DESCRIPTION
        "A ceDiagHMTestRecoverNotif is sent when no error is
        detected for the first time on the same Health Monitoring test 
        which previously triggered ceDiagHMThresholdReachedNotif."
   ::= { ciscoEntityDiagMIBNotifs 3 }

ceDiagScheduledTestFailedNotif NOTIFICATION-TYPE
    OBJECTS         {
                        entPhysicalDescr,
                        ceDiagTestText,
                        ceDiagEventErrorMsg
                    }
    STATUS          current
    DESCRIPTION
        "A ceDiagScheduledTestFailedNotif is sent if a scheduled
        test failed."
   ::= { ciscoEntityDiagMIBNotifs 4 }
-- Conformance

ciscoEntityDiagMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIBConform 1 }

ciscoEntityDiagMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoEntityDiagMIBConform 2 }


ciscoEntityDiagMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for SNMP entities that implement the
        CISCO-ENTITY-DIAG-MIB.  Implementation of this MIB module is
        strongly recommended for any platform implementing the
        online diagnostic feature."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ceDiagDescrGroup,
                        ceDiagGlobalConfigGroup,
                        ceDiagEntityGroup,
                        ceDiagOnDemandGroup,
                        ceDiagScheduledGroup,
                        ceDiagTestPerfGroup,
                        ceDiagEventGroup
                    }

    GROUP           ceDiagEntityImageGroup
    DESCRIPTION
        "The objects defined by this group only need to be
        implemented if the physical entities in the system
        are capable of running their own diagnostic image."

    GROUP           ceDiagHealthMonitorGroup
    DESCRIPTION
        "The objects defined by this group only need to be
        implemented if the online diagnostic feature
        supports a health monitor."

    GROUP           ceDiagScheduledJobSuiteGroup
    DESCRIPTION
        "The objects defined by this group only need to be
        implemented if the online diagnostic feature
        supports scheduled job test suites."
    ::= { ciscoEntityDiagMIBCompliances 1 }

ciscoEntityDiagMIBComplianceRev2 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for SNMP entities that implement the
        CISCO-ENTITY-DIAG-MIB.  Implementation of this MIB module is
        strongly recommended for any platform implementing the
        online diagnostic feature.

        This statement is deprecated and superceded by 
        ciscoEntityDiagMIBComplianceRev3."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ceDiagDescrGroup,
                        ceDiagGlobalConfigGroup,
                        ceDiagEntityGroup,
                        ceDiagOnDemandGroup,
                        ceDiagScheduledGroup,
                        ceDiagTestPerfGroup,
                        ceDiagEventGroup
                    }

    GROUP           ceDiagEntityImageGroup
    DESCRIPTION
        "The objects defined by this group only need to be
        implemented if the physical entities in the system
        are capable of running their own diagnostic image."

    GROUP           ceDiagHealthMonitorGroup
    DESCRIPTION
        "The objects defined by this group only need to be
        implemented if the online diagnostic feature
        supports a health monitor."

    GROUP           ceDiagScheduledJobSuiteGroup
    DESCRIPTION
        "The objects defined by this group only need to be
        implemented if the online diagnostic feature
        supports scheduled job test suites."

    GROUP           ceDiagNotifControlGroup
    DESCRIPTION
        "This group is mandatory for devices which can provide
        online diagnostic notifications."

    GROUP           ceDiagNotifErrorMsgGroup
    DESCRIPTION
        "This group is mandatory for devices which can provide
        online diagnostic notifications."

    GROUP           ceDiagNotificationGroup
    DESCRIPTION
        "This group is mandatory for devices which can provide
        online diagnostic notifications."
    ::= { ciscoEntityDiagMIBCompliances 2 }

ciscoEntityDiagMIBComplianceRev3 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for SNMP entities that implement the
        CISCO-ENTITY-DIAG-MIB.  Implementation of this MIB module is
        strongly recommended for any platform implementing the
        online diagnostic feature.

        This statement is deprecated and superceded by 
        ciscoEntityDiagMIBComplianceRev4."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ceDiagDescrGroup,
                        ceDiagGlobalConfigGroup,
                        ceDiagEntityGroup,
                        ceDiagOnDemandGroup,
                        ceDiagScheduledGroup,
                        ceDiagTestPerfGroup,
                        ceDiagEventGroup
                    }

    GROUP           ceDiagEntityImageGroup
    DESCRIPTION
        "The objects defined by this group only need to be
        implemented if the physical entities in the system
        are capable of running their own diagnostic image."

    GROUP           ceDiagHealthMonitorGroup
    DESCRIPTION
        "The objects defined by this group only need to be
        implemented if the online diagnostic feature
        supports a health monitor."

    GROUP           ceDiagScheduledJobSuiteGroup
    DESCRIPTION
        "The objects defined by this group only need to be
        implemented if the online diagnostic feature
        supports scheduled job test suites."

    GROUP           ceDiagNotifControlGroup
    DESCRIPTION
        "This group is mandatory for devices which can provide
        online diagnostic notifications."

    GROUP           ceDiagNotifErrorMsgGroup
    DESCRIPTION
        "This group is mandatory for devices which can provide
        online diagnostic notifications."

    GROUP           ceDiagNotificationGroup
    DESCRIPTION
        "This group is mandatory for devices which can provide
        online diagnostic notifications."

    GROUP           ceDiagTestPerfLastTestMethodGroup
    DESCRIPTION
        "This group is mandatory for devices which can provide
        the last testing method for a diagnostic test."
    ::= { ciscoEntityDiagMIBCompliances 3 }

ciscoEntityDiagMIBComplianceRev4 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for SNMP entities that implement the
        CISCO-ENTITY-DIAG-MIB.  Implementation of this MIB module is
        strongly recommended for any platform implementing the
        online diagnostic feature."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ceDiagDescrGroup,
                        ceDiagGlobalConfigGroup,
                        ceDiagEntityGroup,
                        ceDiagOnDemandGroup,
                        ceDiagScheduledGroup,
                        ceDiagTestPerfGroup,
                        ceDiagEventGroup
                    }

    GROUP           ceDiagEntityImageGroup
    DESCRIPTION
        "The objects defined by this group only need to be
        implemented if the physical entities in the system
        are capable of running their own diagnostic image."

    GROUP           ceDiagHealthMonitorGroup
    DESCRIPTION
        "The objects defined by this group only need to be
        implemented if the online diagnostic feature
        supports a health monitor."

    GROUP           ceDiagScheduledJobSuiteGroup
    DESCRIPTION
        "The objects defined by this group only need to be
        implemented if the online diagnostic feature
        supports scheduled job test suites."

    GROUP           ceDiagNotifControlGroup
    DESCRIPTION
        "This group is mandatory for devices which can provide
        online diagnostic notifications."

    GROUP           ceDiagNotifErrorMsgGroup
    DESCRIPTION
        "This group is mandatory for devices which can provide
        online diagnostic notifications."

    GROUP           ceDiagNotificationGroup
    DESCRIPTION
        "This group is mandatory for devices which can provide
        online diagnostic notifications."

    GROUP           ceDiagTestPerfLastTestMethodGroup
    DESCRIPTION
        "This group is mandatory for devices which support sliding
        history window parameters for Health Monitor diagnostic test."

    GROUP           ceDiagHMTestThreshWindowGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        sliding window parameters for health monitor tests."

    OBJECT          ceDiagBootupLevel
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagEntityImageAdminStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagEntityFieldDiagnosticUrl
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagOnDemandErrorAllowed
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagOnDemandErrorAction
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagOnDemandIterations
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagOnDemandJobSuite
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagOnDemandJobTestList
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagOnDemandJobPortList
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagOnDemandJobRowStatus
    SYNTAX          INTEGER  {
                        active(1)
                    }
    WRITE-SYNTAX    INTEGER  {
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagScheduledJobType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagScheduledJobStart
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagScheduledJobDayOfWeek
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagScheduledJobTestList
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagScheduledJobPortList
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagScheduledJobRowStatus
    SYNTAX          INTEGER  {
                        active(1)
                    }
    WRITE-SYNTAX    INTEGER  {
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagScheduledJobSuite
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagHMSyslogEnabled
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagHMTestEnabled
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagHMTestInterval
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagHMTestThreshold
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagHMTestThreshWindowSuite
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagHMTestThreshWindowSize
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagEventLogSize
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagEventQueryPhysicalIndex
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagEventQuerySeverity
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagEventQueryOwner
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagEventQueryStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagEnableBootUpFailedNotif
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagEnableHMThreshReachedNotif
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagEnableHMTestRecoverNotif
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ceDiagEnableSchedTestFailedNotif
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."
    ::= { ciscoEntityDiagMIBCompliances 4 }

-- Units of Conformance

ceDiagDescrGroup OBJECT-GROUP
    OBJECTS         {
                        ceDiagTestText,
                        ceDiagTestAttributes,
                        ceDiagTestCustomAttributeDesc,
                        ceDiagErrorText
                    }
    STATUS          current
    DESCRIPTION
        "A collection of managed objects that describe tests and errors
        supported by each physical entity."
    ::= { ciscoEntityDiagMIBGroups 1 }

ceDiagGlobalConfigGroup OBJECT-GROUP
    OBJECTS         { ceDiagBootupLevel }
    STATUS          current
    DESCRIPTION
        "A collection of managed objects that describe global
        configuration of the online diagnostic feature."
    ::= { ciscoEntityDiagMIBGroups 2 }

ceDiagEntityGroup OBJECT-GROUP
    OBJECTS         {
                        ceDiagEntityBootLevel,
                        ceDiagEntityCurrentTestMethod
                    }
    STATUS          current
    DESCRIPTION
        "A collection of managed objects that describe the state of a
        physical entity with respect ot the online diagnostic
        feature."
    ::= { ciscoEntityDiagMIBGroups 3 }

ceDiagEntityImageGroup OBJECT-GROUP
    OBJECTS         {
                        ceDiagEntityImageAdminStatus,
                        ceDiagEntityImageOperStatus,
                        ceDiagEntityFieldDiagnosticUrl
                    }
    STATUS          current
    DESCRIPTION
        "A collection of managed objects that describe the diagnostic
        image which the physical entity is running."
    ::= { ciscoEntityDiagMIBGroups 4 }

ceDiagOnDemandGroup OBJECT-GROUP
    OBJECTS         {
                        ceDiagOnDemandErrorAllowed,
                        ceDiagOnDemandErrorAction,
                        ceDiagOnDemandIterations,
                        ceDiagOnDemandJobSuite,
                        ceDiagOnDemandJobTestList,
                        ceDiagOnDemandJobPortList,
                        ceDiagOnDemandJobRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of managed objects that describe the diagnostic
        on demand diagnostic jobs on the system."
    ::= { ciscoEntityDiagMIBGroups 5 }

ceDiagScheduledGroup OBJECT-GROUP
    OBJECTS         {
                        ceDiagScheduledJobType,
                        ceDiagScheduledJobStart,
                        ceDiagScheduledJobDayOfWeek,
                        ceDiagScheduledJobTestList,
                        ceDiagScheduledJobPortList,
                        ceDiagScheduledJobRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of managed objects that describe the diagnostic
        on demand diagnostic jobs on the system."
    ::= { ciscoEntityDiagMIBGroups 6 }

ceDiagTestPerfGroup OBJECT-GROUP
    OBJECTS         {
                        ceDiagTestPerfLastResult,
                        ceDiagTestPerfLastErrorID,
                        ceDiagTestPerfLastRun,
                        ceDiagTestPerfFirstFail,
                        ceDiagTestPerfLastSuccess,
                        ceDiagTestPeffLastFail,
                        ceDiagTestPerfTotalRuns,
                        ceDiagTestPerfTotalFails,
                        ceDiagTestPerfConsecutiveFails
                    }
    STATUS          current
    DESCRIPTION
        "A collection of managed objects that describe the performance
        of tests supported by each physical entity."
    ::= { ciscoEntityDiagMIBGroups 7 }

ceDiagHealthMonitorGroup OBJECT-GROUP
    OBJECTS         {
                        ceDiagHMSyslogEnabled,
                        ceDiagHMTestEnabled,
                        ceDiagHMTestIntervalMin,
                        ceDiagHMTestInterval,
                        ceDiagHMTestIntervalDefault,
                        ceDiagHMTestThresholdDefault,
                        ceDiagHMTestThreshold
                    }
    STATUS          current
    DESCRIPTION
        "A collection of managed objects that describe tests and test
        configuration with relating to the health monitor."
    ::= { ciscoEntityDiagMIBGroups 8 }

ceDiagEventGroup OBJECT-GROUP
    OBJECTS         {
                        ceDiagEventLogSize,
                        ceDiagEventCount,
                        ceDiagEventMaxQueries,
                        ceDiagEventQueryPhysicalIndex,
                        ceDiagEventQuerySeverity,
                        ceDiagEventQueryOwner,
                        ceDiagEventQueryResultingRows,
                        ceDiagEventQueryStatus,
                        ceDiagEventResultPhysicalIndex,
                        ceDiagEventResultPhysicalDescr,
                        ceDiagEventResultTime,
                        ceDiagEventResultSeverity,
                        ceDiagEventResultLogText
                    }
    STATUS          current
    DESCRIPTION
        "A collection of managed objects that describe online
        diagnostic event history."
    ::= { ciscoEntityDiagMIBGroups 9 }

ceDiagScheduledJobSuiteGroup OBJECT-GROUP
    OBJECTS         { ceDiagScheduledJobSuite }
    STATUS          current
    DESCRIPTION
        "A collection of managed objects that describe the test suite information
        for a diagnostic scheduled job."
    ::= { ciscoEntityDiagMIBGroups 10 }

ceDiagNotifControlGroup OBJECT-GROUP
    OBJECTS         {
                        ceDiagEnableBootUpFailedNotif,
                        ceDiagEnableHMThreshReachedNotif,
                        ceDiagEnableHMTestRecoverNotif,
                        ceDiagEnableSchedTestFailedNotif
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing enabling/disabling
        of the boot up failed, health monitoring, and 
        scheduled job notifications for online diagnostics."
    ::= { ciscoEntityDiagMIBGroups 11 }

ceDiagNotifErrorMsgGroup OBJECT-GROUP
    OBJECTS         { ceDiagEventErrorMsg }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing error message used by
        various notifications."
    ::= { ciscoEntityDiagMIBGroups 12 }

ceDiagNotificationGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        ceDiagBootUpFailedNotif,
                        ceDiagHMThresholdReachedNotif,
                        ceDiagHMTestRecoverNotif,
                        ceDiagScheduledTestFailedNotif
                    }
    STATUS          current
    DESCRIPTION
        "A collection of notifications providing for boot up failed, health
        monitoring, and scheduled job within online diagnostics."
    ::= { ciscoEntityDiagMIBGroups 13 }

ceDiagTestPerfLastTestMethodGroup OBJECT-GROUP
    OBJECTS         { ceDiagTestPerfLastTestMethod }
    STATUS          current
    DESCRIPTION
        "A collection of managed objects that describe the last testing method
        for a diagnostic test."
    ::= { ciscoEntityDiagMIBGroups 14 }

ceDiagHMTestThreshWindowGroup OBJECT-GROUP
    OBJECTS         {
                        ceDiagHMTestThreshWindowSuite,
                        ceDiagHMTestThreshWindowSize
                    }
    STATUS          current
    DESCRIPTION
        "A collection of managed objects that describe the sliding
        history window parameters for a Health Monitor diagnostic test."
    ::= { ciscoEntityDiagMIBGroups 15 }

END



