-- *****************************************************************
-- DOCS-IF3-MIB.my:
--
-- Aug 2007 Bo Wu
--
-- Initial Version: Aug 2007: Annex Q.6 from CM-SP-OSSIv3.0-I04-070803 
-- Reversion May 2008: Annex Q.6 from CM-SP-OSSIv3.0-I07-080522  
--
-- Copyright (c) 2007-2008 by cisco Systems, Inc.
-- All rights reserved.
-- *****************************************************************


DOCS-IF3-MIB DEFINITIONS ::= BEGIN
  IMPORTS
    NOTIFICATION-TYPE,
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Integer32,
    Unsigned32,
    Counter32
             FROM SNMPv2-SMI         -- RFC 2578
    sysName
             FROM SNMPv2-MIB         -- RFC 3418
    TEXTUAL-CONVENTION,
    RowStatus,
    TruthValue,
    MacAddress,
    DateAndTime
             FROM SNMPv2-TC          -- RFC 2579
    OBJECT-GROUP,
    NOTIFICATION-GROUP,
    MODULE-COMPLIANCE
             FROM SNMPv2-CONF        -- RFC 2580
    SnmpAdminString
             FROM SNMP-FRAMEWORK-MIB -- RFC 3411
    SnmpTagList
             FROM SNMP-TARGET-MIB    -- RFC 3413
    InetAddressIPv6,
    InetAddressIPv4
             FROM INET-ADDRESS-MIB   --  RFC 4001
    ifIndex,
    InterfaceIndex,
    InterfaceIndexOrZero
             FROM IF-MIB             --  RFC 2863
    TenthdB,
    TenthdBmV,
    DocsisUpstreamType,
    DocsEqualizerData,
    DocsisQosVersion
             FROM DOCS-IF-MIB        -- RFC 4546
    NodeName
             FROM CLAB-TOPO-MIB

    docsDevEvLevel,
    docsDevEvId,
    docsDevEvText, 
    docsDevEvLastTime
             FROM DOCS-CABLE-DEVICE-MIB -- RFC 4639 
    clabProjDocsis
              FROM CLAB-DEF-MIB;

docsIf3Mib MODULE-IDENTITY
     LAST-UPDATED    "200805220000Z" -- May 22, 2008
     ORGANIZATION    "Cable Television Laboratories, Inc."
     CONTACT-INFO
         "
         Postal: Cable Television Laboratories, Inc.
         858 Coal Creek Circle
         Louisville, Colorado 80027-9750
         U.S.A.
         Phone: +1 303-661-9100
         Fax:   +1 303-661-9199
         E-mail: mibs@cablelabs.com"
     DESCRIPTION
        "This MIB module contains the management objects for the
        management of DOCSIS 3.0 features, primarly channel bonding,
        interface topology and enhanced signal quality montoring.
        Copyright 1999-2008 Cable Television Laboratories, Inc.
        All rights reserved."
    REVISION        "200805220000Z" -- May 22, 2008
    DESCRIPTION
        "Revised Version includes ECN OSSIv3.0-N-08.0645-4
        and published as I07"
    REVISION "200802150000Z"
    DESCRIPTION
            "Revised Version includes ECN OSSIv3.0-N-07.0605-1
             and published as I06"
    REVISION "200712060000Z"  -- December 6, 2007
    DESCRIPTION
            "Revised Version includes ECNs
            OSSIv3.0-N-07.0522-6
            OSSIv3.0-N-07.0554-4
            and published as I05"
    REVISION "200708030000Z"  -- August 3, 2007
    DESCRIPTION
            "Revised Version includes ECNs
            OSSIv3.0-N-07.0481-2
            OSSIv3.0-N-07.0480-3
            and published as I04"
    REVISION "200705180000Z"  -- May 18, 2007
    DESCRIPTION
            "Revised Version includes ECNs
            OSSIv3.0-N-07.0447-2
            OSSIv3.0-N-07.0446-4
            OSSIv3.0-N-07.0445-3
            OSSIv3.0-N-07.0441-4
            OSSIv3.0-N-07.0422-5
            OSSIv3.0-N-07.0413-3
            OSSIv3.0-N-07.0410-4
            OSSIv3.0-N-07.0392-1
            OSSIv3.0-N-07.0384-1
            OSSIv3.0-N-06.0357-1
            and published as I03"
    REVISION "200702230000Z" -- February 23, 2007
    DESCRIPTION
            "Revised Version includes ECN OSSIv3.0-N-06.0357-1
            and published as IO2"
     REVISION "200612071700Z" -- December 7, 2006
     DESCRIPTION
        "Initial version, published as part of the CableLabs
        OSSIv3.0 specification CM-SP-OSSIv3.0-I01-061207"
     ::= {  clabProjDocsis 20 }

-- Textual Conventions

CmRegState ::= TEXTUAL-CONVENTION
     STATUS      current
     DESCRIPTION
         "This data type defines the CM connectivity state as reported
         by the CM.
         The enumerated values associated with the CmRegState are:
         'other'
          indicates any state not described below.
         'notReady'
          indicates that the CM has not started the registration process
          yet.
         'notSynchronized'
          indicates that the CM has not initiated or completed the
          synchronization of the downstream physical layer
         'phySynchronized'
          indicates that the CM has completed the synchronization of
          the downstream physical layer
         'dsTopologyResolutionInProgress'
          indicates that the CM is attempting to determine its MD-DS-SG
         'usParametersAcquired'
          indicates that the CM has completed the upstream parameters
          acquisition or have completed the downstream and upstream
          service groups resolution, wheater the CM is registering in
          a pre-3.0 or a 3.0 CMTS.
         'rangingInProgress'
          indicates that the CM has initiated the ranging process. 
         'rangingComplete'
          indicates that the CM has completed initial ranging and
          received a Ranging Status of success from the CMTS in the
          RNG-RSP message.
         'eaeInProgress'
          indicates that the CM has sent an Auth Info message for EAE.
         'dhcpv4InProgress'
          indicates that the CM has sent a DHCPv4 DISCOVER to gain 
          IP connectivity.
         'dhcpv6InProgress'
          indicates that the CM has sent an DHCPv6 Solicit message.
         'dhcpv4Complete'
          indicates that the CM has received a DHCPv4 ACK message from
          the CMTS.
         'dhcpv6Complete'
          indicates that the CM has received a DHCPv6 Reply message from
          the CMTS.
         'todEstablished'
          indicates that the CM has successfully acquired time of day.
          If the ToD is acquired after the CM is operational, this
          value should not be reported.
         'securityEstablished'
          indicates that the CM has successfully completed the BPI
          initialization process.
         'configFileDownloadComplete'
          indicates that the CM has completed the config file download
          process.
         'registrationInProgress'
          indicates that the CM has sent a Registration Request
          (REG-REQ or REG-REQ-MP)
         'registrationComplete'
          indicates that the CM has successfully completed the
          Registration process with the CMTS.
         'accessDenied'
          indicates that the CM has received a registration aborted
          notification from the CMTS
         'operational'
          indicates that the CM has completed all necessary
          initialization steps and is operational.
         'bpiInit'
          indicates that the CM has started the BPI initialization
          process as indicated in the CM config file. If the CM already
          performed EAE, this state is skipped by the CM.
         'forwardingDisabled'
          indicates that the registration process was completed, but 
          the network access option in the received configuration file
          prohibits forwarding.
         'rfMuteAll'
          indicates that the CM is instructed to mute all channels 
          in the CM-CTRL-REQ message from CMTS."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Cable Modem -
         CMTS Interaction section."
     SYNTAX      INTEGER {other(1),
                          notReady(2),
                          notSynchronized(3),
                          phySynchronized(4),
                          dsTopologyResolutionInProgress(21),
                          usParametersAcquired(5),
                          rangingInProgress(22),
                          rangingComplete(6),
                          eaeInProgress(14),
                          dhcpv4InProgress(15),
                          dhcpv6InProgress(16),
                          dhcpv4Complete(7),
                          dhcpv6Complete(17),
                          todEstablished(8),
                          securityEstablished(9),
                          configFileDownloadComplete(10),
                          registrationInProgress(18),
                          registrationComplete(11),
                          accessDenied(13),
                          operational(12),
                          bpiInit (19),
                          forwardingDisabled(20),
                          rfMuteAll(23)
                         }

CmtsCmRegState ::= TEXTUAL-CONVENTION
     STATUS      current
     DESCRIPTION
        "This data type defines the CM connectivity states as reported
        by the CMTS.
        The enumerated values associated with the CmtsCmRegState are:

        'other'
         indicates any state not described below.
        'initialRanging'
         indicates that the CMTS has received an Initial Ranging
         Request message from the CM, and the ranging process is not yet
         complete.
        'rangingAutoAdjComplete'
         indicates that the CM has completed initial ranging and the
         CMTS sends  a Ranging Status of success in the RNG-RSP.
        'startEae'
         indicates that the CMTS has received an Auth Info message for
         EAE from the CM.
        'startDhcpv4'
         indicates that the CMTS has received a DHCPv4 DISCOVER message
         from the CM.
        'startDhcpv6'
         indicates that the CMTS has received a DHCPv6 Solicit message
         from the CM.
        'dhcpv4Complete'
         indicates that the CMTS has sent a DHCPv4 ACK message to the
         CM.
        'dhcpv6Complete'
         indicates that the CMTS has sent a DHCPv6 Reply message to the
         CM.
        'startConfigFileDownload'
         indicates that the CM has started the config file download.
         If the TFTP Proxy feature is not enabled, the CMTS may not
         report this state.
        'configFileDownloadComplete'
         indicates that the CM has completed the config file download
         process.  If the TFTP Proxy feature is not enabled, the CMTS
         is not required to report this state.
        'startRegistration'
         indicates that the CMTS has received a Registration
         Request (REG-REQ or REG-REQ-MP) from the CM.
        'registrationComplete'
         indicates that the CMTS has received a Registration Acknowledge
         (REG-ACK) with a confirmation code of okay/success.
        'operational'
         indicates that the CM has completed all necessary
         initialization steps and is operational.
        'bpiInit'
         indicates that the CMTS has received an Auth Info or Auth
         Request message as part of BPI Initialization.
        'forwardingDisabled'
         indicates that the registration process was completed, but 
         the network access option in the received configuration 
         file prohibits forwarding.
        'rfMuteAll'
         indicates that the CM is instructed to mute all channels 
         in the CM-CTRL-REQ message from CMTS."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Cable Modem -
         CMTS Interaction section."
     SYNTAX      INTEGER {other (1),
                          initialRanging(2),
                          rangingAutoAdjComplete(4),
                          startEae(10),
                          startDhcpv4 (11),
                          startDhcpv6(12),
                          dhcpv4Complete(5),
                          dhcpv6Complete(13),
                          startConfigFileDownload(14),
                          configFileDownloadComplete(15),
                          startRegistration(16),
                          registrationComplete(6),
                          operational (8),
                          bpiInit(9),
                          forwardingDisabled(17),
                          rfMuteAll(18)
                         }

ScdmaSelectionString  ::= TEXTUAL-CONVENTION
     STATUS      current
     DESCRIPTION
        "This data type represents the S-CDMA selection string
         for active codes used with Selectable Active Codes Mode 2.
         A 128-bit string indicating which codes are active.
         The first element in the string corresponds to code 0
         (the all-ones code), and the last element in the string
         corresponds to code 127.  A '1' element in the string
         indicates an active code, and a '0' indicates an unused
         code."
     REFERENCE
         "DOCSIS 3.0 Physical Layer Specification
         CM-SP-PHYv3.0-I05-070803, Mini-slot Numbering Parameters
         in UCD section."
     SYNTAX      OCTET STRING (SIZE(16))

AmplitudeData  ::= TEXTUAL-CONVENTION
     STATUS      current
     DESCRIPTION
        "This data type represents a sequence of spectral amplitudes.
        Each spectral amplitude value corresponds to a bin.
        The format of the bin measurement is as follows.
        Sequence of:
          4 bytes: ChCenterFreq
                   The center frequency of the upstream channel.
          4 bytes: FreqSpan
                   The width in Hz of the band across which the spectral
                   amplitudes characterizing the channel are measured.
          4 bytes: NumberOfBins
                   The number of data points or bins that compose the
                   spectral data. The leftmost bin corresponds to the
                   lower band edge, the rightmost bin corresponds to the
                   upper band edge, and the middle bin center is aligned
                   with the center frequency of the analysis span.
          4 bytes: BinSpacing
                   The frequency separation between adjacent bin
                   centers. It is derived from the frequency span and
                   the number of bins or data points.
                   The bin spacing is computed as:

                            BinSpacing = FrequencySpan/(NumberOfBins -1)

                   The larger the number of bins the finer the
                   resolution.
          4 bytes: ResolutionBW
                   The resolution bandwidth or equivalent noise
                   bandwidth of each bin. If spectral windowing is used
                   (based on vendor implementation), the bin spacing and
                   resolution bandwidth would not generally be the same.
          n bytes: Amplitude (2 bytes * NumberOfBins)
                   A sequence of two byte elements. Each element
                   represents the spectral amplitudes in relation to the
                   expected received signal power of a bin, in units of
                   0.01dB. That is, a test CMTS input signal with
                   square-root raised-cosine spectrum, bandwidth equal
                   to the expected received signal bandwidth, and power
                   equal to the expected received signal power, which
                   is present for the entire spectrum sampling period,
                   will exhibit a spectrum measurement of 0 dB average
                   power in each bin of the signal passband.
                   Each bin element amplitude value format is 2's
                   complement which provides a range of -327.68 dB to
                   327.67 dB amplitude value for the bin measurement."
     SYNTAX      OCTET STRING (SIZE(0 | 2..255))

Tlv8 ::= TEXTUAL-CONVENTION
     STATUS      current
     DESCRIPTION
        "This data type represents a single TLV encoding.
        This first octet represents the Type of the TLV.
        The second octet represents an unsigned 8-bit Length of the
        subsequent Value part of the TLV.  The remaining octets
        represent the value. The Value could be an atomic value or a
        sequence of one or more sub-TLVs."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Common Radio
         Frequency Interface Encodings Annex."
     SYNTAX      OCTET STRING (SIZE(0 | 2..255))

ChId ::= TEXTUAL-CONVENTION
     DISPLAY-HINT "d"
     STATUS      current
     DESCRIPTION
        "This data type is an 8-bit number that represents a provisioned
        Downstream Channel ID (DCID) or a provisioned Upstream Channel
        ID (UCID). A Channel Id is unique per direction within a MAC
        Domain. The value zero is reserved for use when the channel ID
        is unknown."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Upstream Channel
         Descriptor (UCD) section."
     SYNTAX      Unsigned32 (0..255)

ChSetId ::= TEXTUAL-CONVENTION
     DISPLAY-HINT "d"
     STATUS      current
     DESCRIPTION
        "This data type is a CMTS-derived unique number within a MAC
        Domain used to reference a Channel Set within the CMTS.
        Values in the range of 1 to 255 define a single-channel Channel
        Set and correspond to either the Downstream Channel ID (DCID)
        or an Upstream Channel ID (UCID) of that channel.
        Values greater than 255 indicate a Channel Set consisting of two
        or more channels in the same direction within the MAC Domain.
        The value zero is reserved for use when the Channel Set is
        unknown."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Channel
         Bonding section."
     SYNTAX      Unsigned32

ChannelList ::= TEXTUAL-CONVENTION
     DISPLAY-HINT "1d,"
     STATUS      current
     DESCRIPTION
        "This data type represents a unique set of channel IDs in
        either the upstream or the downstream direction.  Each octet
        represents a UCID or DCID depending on the direction of the
        channels within the list.  The CMTS must ensure that this
        combination of channels is unique per direction within the MAC
        Domain.

        In order to facilitate Channel ID combinatorial uniqueness
        across all channel lists, a query to retrieve the value of
        an attribute of this type, returns the set of channels in
        the channel list in ascending order of Channel Ids."
     SYNTAX      OCTET STRING (SIZE (0..255))

AttributeMask ::= TEXTUAL-CONVENTION
     STATUS      current
     DESCRIPTION
        "This data type consists of a sequence of 32-bit positions used
        to select the bonding group or the channel to which a service
        flow is assigned. DOCSIS defines three types of Attribute Masks
        for which this type applies: The Provisionied Attribute Mask
        that is configured to a Bonding Group or a single-channel,
        whereas the Required Attribute and the Forbidden Attribute
        Mask are part of the Service Flow QOS Parameter Set to be
        matched with the Provisioned Attribute Mask of CMTS-configured
        Bonding Groups or single-channels. DOCSIS reserves the
        assignment of the meaning of the first 8 bit positions
        (left to right) as follows:
            Bit 0: 'bonding'
            Bit 1: 'lowLatency'
            Bit 2: 'highAvailability'
            Bit positions 3-15 are reserved.

        Bit positions 16-31 are freely assigned by operators to
        represent their own constraints on the channel(s) selection
        for a particular service flow."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Service Flow
         Assignment section."
     SYNTAX      BITS {
                       bonding(0),
                       lowLatency(1),
                       highAvailability(2)
                      }

AttrAggrRuleMask ::= TEXTUAL-CONVENTION
     STATUS      current
     DESCRIPTION
        "This data type represents a sequence of 32-bit positions that
        defines logical (e.g. AND, OR) operations to match against the
        channel list Provisioned Mask and Service Flow Required Mask
        bit positions when the CMTS is determining the service flow
        for assignment to a bonding group not configured by the
        management system."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Service Flow
         Assignment section."
     SYNTAX      OCTET STRING (SIZE (4))

RcpId ::= TEXTUAL-CONVENTION
     STATUS      current
     DESCRIPTION
        "This data type defines a 'Receive Channel Profile Identifier'
        (RCP-ID). An RCP-ID consists of 5-octet length string where the
        first 3-bytes (from left to right corresponds to the
        Organizational Unique ID (OUI) followed by a two-byte
        vendor-maintained identifier to represent multiple versions or
        models of RCP-IDs."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, RCP-ID section in
         the Common Radio Frequency Interface Encodings Annex."
     SYNTAX      OCTET STRING (SIZE (5))

Dsid ::= TEXTUAL-CONVENTION
     DISPLAY-HINT "d"
     STATUS      current
     DESCRIPTION
        "This data type defines the 20-bit Downstream Service Identifier
        (DSID) used by the CM for downstream resequencing, filtering,
        and forwarding. The value zero is reserved for use when the
        DSID is unknown or does not apply."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, DSID Definition
         section."
     SYNTAX      Unsigned32 (0..1048575)

RangingState ::= TEXTUAL-CONVENTION
     STATUS      current
     DESCRIPTION
        "This data type defines the CM ranging state as reported
        by the CMTS.
        The enumerated values associated with the RangingState are:

        'other'
         indicates any state not described below.
        'aborted'
         indicates that the CMTS has sent a ranging abort.
        'retriesExceeded'
         indicates that the CM ranging retry limit has exceeded. 
        'success'
         indicates that the CMTS has sent a ranging success in the
         ranging response.
        'continue'
         indicates that the CMTS has sent a ranging continue in the
         ranging response.
        'timeoutT4'
         indicates that the T4 timer expired on the CM."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Cable Modem - 
         CMTS Interaction section."
     SYNTAX      INTEGER {other(1),
                          aborted(2),
                          retriesExceeded(3), 
                          success(4),
                          continue(5),
                          timeoutT4(6)
                         }
                        
IfDirection ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "Indicates a direction on an RF MAC interface.

       The value downstream(1) is from Cable Modem
       Termination System to Cable Modem.

       The value upstream(2) is from Cable Modem to
       Cable Modem Termination System."
    SYNTAX      INTEGER {
                         downstream(1),
                         upstream(2)
                        }

-- Object Definitions
docsIf3Notifications  OBJECT IDENTIFIER ::= { docsIf3Mib 0 }
docsIf3MibObjects  OBJECT IDENTIFIER ::= { docsIf3Mib 1 }


-- Notifications

-- CMTS Notifications
docsIf3CmtsEventNotif NOTIFICATION-TYPE
    OBJECTS {
        docsDevEvLevel,
        docsDevEvId,
        docsDevEvText, 
        docsDevEvLastTime,
        sysName
    }
    STATUS current
    DESCRIPTION
        "A notification to report a DOCSIS event detected on the 
         CMTS.

         This notification includes the following information:
         - docsDevEvLevel: the DOCSIS priority level associated with 
           the event.
         - docsDevEvId: the numeric identifier of the event.
         - docsDevEvText: The text description of the event.
         - docsDevEvLastTime: The local date and time when this event
           was generated.
         - sysName: the administratively-assigned name of the CMTS.
           e.g. The fully-qualified domain name as indicated in RFC 3418
           or in the absence the IP address of the CMTS administrative
           interface in dot '.' notation for IPv4 and colon ':' notation
           for and IPv6 Address as indicated in  RFC 3164"
     REFERENCE
        "DOCSIS 3.0 Operations Support System Interface
         Specification CM-SP-OSSIv3.0-I07-080522, Format and Content
         for Event, Syslog, and SNMP Notification Annex.
         RFC 3418, RFC 3164"
    ::= { docsIf3Notifications 1 }

-- CM Notifications

docsIf3CmEventNotif NOTIFICATION-TYPE
    OBJECTS {
        docsDevEvLevel,
        docsDevEvId,
        docsDevEvText,
        docsDevEvLastTime
    }
    STATUS current
    DESCRIPTION
        "A notification to report a DOCSIS event detected on the  
         CM.

         This notification includes the following information:
         - docsDevEvLevel: the priority level associated with the
           event.
         - docsDevEvId: the unique identifier of the event that
           occurred.
         - docsDevEvText: a textual description of the event.
         - docsDevEvLastTime: The local date and time when this event
           was generated."
     REFERENCE
        "DOCSIS 3.0 Operations Support System Interface
         Specification CM-SP-OSSIv3.0-I07-080522, Format and Content
         for Event, Syslog, and SNMP Notification Annex."
    ::= { docsIf3Notifications 2 }

docsIf3CmStatusTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3CmStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object defines attributes of the CM connectivity
        status.This object provides CM connectivity status
        information of the CM previously available in
        the SNMP table docsIfCmStatusTable."
     REFERENCE
        "RFC 4546"
     ::= { docsIf3MibObjects 1}

docsIf3CmStatusEntry OBJECT-TYPE
     SYNTAX      DocsIf3CmStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3CmStatusTable.
         An instance exist for the CM MAC Domain Interface."
     INDEX {
             ifIndex
           }
     ::= { docsIf3CmStatusTable 1 }

DocsIf3CmStatusEntry ::= SEQUENCE {
     docsIf3CmStatusValue
                  CmRegState,
     docsIf3CmStatusCode
                  OCTET STRING,
     docsIf3CmStatusResets
                  Counter32,
     docsIf3CmStatusLostSyncs
                  Counter32,
     docsIf3CmStatusInvalidMaps
                  Counter32,
     docsIf3CmStatusInvalidUcds
                  Counter32,
     docsIf3CmStatusInvalidRangingRsps
                  Counter32,
     docsIf3CmStatusInvalidRegRsps
                  Counter32,
     docsIf3CmStatusT1Timeouts
                  Counter32,
     docsIf3CmStatusT2Timeouts
                  Counter32,
     docsIf3CmStatusUCCsSuccesses
                  Counter32,
     docsIf3CmStatusUCCFails
                  Counter32
     }

docsIf3CmStatusValue OBJECT-TYPE
     SYNTAX      CmRegState
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the current CM connectivity
        state. For the case of IP acquisition related states,
        this attribute reflects states for the current CM
        provisioning mode, not the other DHCP process associated
        with dual stack operation."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Establishing
         IP Connectivity section."
     ::= { docsIf3CmStatusEntry 1 }

docsIf3CmStatusCode OBJECT-TYPE
     SYNTAX      OCTET STRING (SIZE( 0 | 5 | 6 ))
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the status code for CM as defined
        in the OSSI Specification. The status code consists
        of a single character indicating error groups,
        followed by a two- or three-digit number indicating
        the status condition, followed by a decimal. An example
        of a returned value could be 'T101.0'. The zero-length
        hex string indicates no status code yet registered."
     REFERENCE
        "DOCSIS 3.0 Operations Support System Interface
         Specification CM-SP-OSSIv3.0-I07-080522, Format and Content
         for Event, Syslog, and SNMP Notification Annex."
     ::= { docsIf3CmStatusEntry 2 }

docsIf3CmStatusResets OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "resets"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of times the CM reset
        or initialized this interface. Discontinuities
        in the value of this counter can occur at re-initialization
        of the managed system, and at other times as
        indicated by the value of ifCounterDiscontinuityTime
        for the CM MAC Domain interface."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusEntry 3 }

docsIf3CmStatusLostSyncs OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "messages"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of times the CM lost
        synchronization with the downstream channel. Discontinuities
        in the value of this counter can occur
        at re-initialization of the managed system, and at
        other times as indicated by the value of
        ifCounterDiscontinuityTime for the CM MAC Domain interface."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusEntry 4 }

docsIf3CmStatusInvalidMaps OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "maps"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of times the CM received
        invalid MAP messages. Discontinuities in the
        value of this counter can occur at re-initialization
        of the managed system, and at other times as indicated
        by the value of ifCounterDiscontinuityTime for
        the CM MAC Domain interface."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusEntry 5 }

docsIf3CmStatusInvalidUcds OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "messages"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of times the CM received
        invalid UCD messages. Discontinuities in the
        value of this counter can occur at re-initialization
        of the managed system, and at other times as indicated
        by the value of ifCounterDiscontinuityTime for
        the CM MAC Domain interface."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusEntry 6 }

docsIf3CmStatusInvalidRangingRsps OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "messages"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of times the CM received
        invalid ranging response messages. Discontinuities
        in the value of this counter can occur at re-initialization
        of the managed system, and at other
        times as indicated by the value of ifCounterDiscontinuityTime
        for the CM MAC Domain interface."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusEntry 7 }

docsIf3CmStatusInvalidRegRsps OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "messages"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of times the CM received
        invalid registration response messages. Discontinuities
        in the value of this counter can occur
        at re-initialization of the managed system, and at
        other times as indicated by the value of
        ifCounterDiscontinuityTime for the CM MAC Domain interface."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusEntry 8 }

docsIf3CmStatusT1Timeouts OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "timeouts"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of times counter
        T1 expired in the CM. Discontinuities in the value of
        this counter can occur at re-initialization of the
        managed system, and at other times as indicated by the
        value of ifCounterDiscontinuityTime for the CM MAC
        Domain interface."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusEntry 9 }

docsIf3CmStatusT2Timeouts OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "timeouts"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of times counter
        T2 expired in the CM. Discontinuities in the value of
        this counter can occur at re-initialization of the
        managed system, and at other times as indicated by the
        value of ifCounterDiscontinuityTime for the CM MAC
        Domain interface."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusEntry 10 }

docsIf3CmStatusUCCsSuccesses OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "attempts"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of successful Upstream
        Channel Change transactions. Discontinuities
        in the value of this counter can occur at re-initialization
        of the managed system, and at other times
        as indicated by the value of ifCounterDiscontinuityTime
         for the CM MAC Domain interface."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusEntry 11 }

docsIf3CmStatusUCCFails OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "attempts"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of failed Upstream
        Channel Change transactions. Discontinuities
        in the value of this counter can occur at re-initialization
        of the managed system, and at other times as indicated
        by the value of ifCounterDiscontinuityTime
        for the CM MAC Domain interface."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusEntry 12 }

docsIf3CmStatusUsTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3CmStatusUsEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object defines PHY and MAC information about
        the CM's upstream channels operating in Multiple Transmit
        Channel (MTC) mode or in a Pre-3.0 DOSCIS transmit
        channel mode. This object provides per-CM Upstream
        channel information previously available in the
        SNMP table docsIfCmStatusTable."
     ::= { docsIf3MibObjects 2}

docsIf3CmStatusUsEntry OBJECT-TYPE
     SYNTAX      DocsIf3CmStatusUsEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3CmStatusUsTable.
         An instance exist for the CM upstream channels configured for
         data transmission."
     INDEX {
             ifIndex
           }
     ::= { docsIf3CmStatusUsTable 1 }

DocsIf3CmStatusUsEntry ::= SEQUENCE {
     docsIf3CmStatusUsTxPower
                  TenthdBmV,
     docsIf3CmStatusUsT3Timeouts
                  Counter32,
     docsIf3CmStatusUsT4Timeouts
                  Counter32,
     docsIf3CmStatusUsRangingAborteds
                  Counter32,
     docsIf3CmStatusUsModulationType
                  DocsisUpstreamType,
     docsIf3CmStatusUsEqData
                  DocsEqualizerData,
     docsIf3CmStatusUsT3Exceededs
                  Counter32,
     docsIf3CmStatusUsIsMuted
                  TruthValue,
     docsIf3CmStatusUsRangingStatus
                  RangingState
     }

docsIf3CmStatusUsTxPower OBJECT-TYPE
     SYNTAX      TenthdBmV
     UNITS       "TenthdBmV"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the operational CM transmit
        power for this upstream channel."
     ::= { docsIf3CmStatusUsEntry 1 }

docsIf3CmStatusUsT3Timeouts OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "timeouts"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of times counter
        T3 expired in the CM for this upstream channel. Discontinuities
        in the value of this counter can occur at
        re-initialization of the managed system, and at other
        times as indicated by the value of ifCounterDiscontinuityTime
        for the associated upstream channel."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusUsEntry 2 }

docsIf3CmStatusUsT4Timeouts OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "timeouts"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of times counter
        T4 expired in the CM for this upstream channel. Discontinuities
        in the value of this counter can occur at
        re-initialization of the managed system, and at other
        times as indicated by the value of ifCounterDiscontinuityTime
        for the associated upstream channel."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusUsEntry 3 }

docsIf3CmStatusUsRangingAborteds OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "attempts"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of times the ranging
        process was aborted by the CMTS. Discontinuities
        in the value of this counter can occur at re-initialization
        of the managed system, and at other times as
        indicated by the value of ifCounterDiscontinuityTime
        ([RFC2863]) for the associated upstream channel."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusUsEntry 4 }

docsIf3CmStatusUsModulationType OBJECT-TYPE
     SYNTAX      DocsisUpstreamType
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute indicates modulation type status
        currently used by the CM for this upstream channel. Since
        this object specifically identifies PHY Layer
        mode, the shared upstream channel type 'tdmaAndAtdma'
        is not permitted."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusUsEntry 5 }

docsIf3CmStatusUsEqData OBJECT-TYPE
     SYNTAX      DocsEqualizerData
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute indicates the pre-equalization data
        for the specified upstream Channel on this CM after
        convolution with data indicated in the RNG-RSP. This
        data is valid when docsIfUpChannelPreEqEnable
        RFC 4546 is set to true."
     REFERENCE
        "RFC 2863.
         RFC 4546."
     ::= { docsIf3CmStatusUsEntry 6 }

docsIf3CmStatusUsT3Exceededs OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "timeouts"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the number of times for excessive
        T3 timeouts. Discontinuities in the value of
        this counter can occur at re-initialization of the managed
        system, and at other times as indicated by the
        value of ifCounterDiscontinuityTime for the associated
        upstream channel."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmStatusUsEntry 7 }

docsIf3CmStatusUsIsMuted OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes whether the upstream
        channel is muted."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522 section
         Media Access Control specification."
     ::= { docsIf3CmStatusUsEntry 8 }

docsIf3CmStatusUsRangingStatus OBJECT-TYPE
     SYNTAX      RangingState
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the ranging state of the CM."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, section
         Media Access Control specification."
     ::= { docsIf3CmStatusUsEntry 9 }

docsIf3CmtsCmRegStatusTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3CmtsCmRegStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object defines attributes that represent the CM's
        registration status as tracked by the CMTS."
     ::= { docsIf3MibObjects 3}

docsIf3CmtsCmRegStatusEntry OBJECT-TYPE
     SYNTAX      DocsIf3CmtsCmRegStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3CmtsCmRegStatusTable."
     INDEX {
             docsIf3CmtsCmRegStatusId
           }
     ::= { docsIf3CmtsCmRegStatusTable 1 }

DocsIf3CmtsCmRegStatusEntry ::= SEQUENCE {
     docsIf3CmtsCmRegStatusId
                  Unsigned32,
     docsIf3CmtsCmRegStatusMacAddr
                  MacAddress,
     docsIf3CmtsCmRegStatusIPv6Addr
                  InetAddressIPv6,
     docsIf3CmtsCmRegStatusIPv6LinkLocal
                  InetAddressIPv6,
     docsIf3CmtsCmRegStatusIPv4Addr
                  InetAddressIPv4,
     docsIf3CmtsCmRegStatusValue
                  CmtsCmRegState,
     docsIf3CmtsCmRegStatusMdIfIndex
                  InterfaceIndexOrZero,
     docsIf3CmtsCmRegStatusMdCmSgId
                  Unsigned32,
     docsIf3CmtsCmRegStatusRcpId
                  RcpId,
     docsIf3CmtsCmRegStatusRccStatusId
                  Unsigned32,
     docsIf3CmtsCmRegStatusRcsId
                  ChSetId,
     docsIf3CmtsCmRegStatusTcsId
                  ChSetId,
     docsIf3CmtsCmRegStatusQosVersion
                  DocsisQosVersion,
     docsIf3CmtsCmRegStatusLastRegTime
                  DateAndTime,
     docsIf3CmtsCmRegStatusAddrResolutionReqs
                  Counter32
     }

docsIf3CmtsCmRegStatusId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..4294967295)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This attribute uniquely identifies a CM.  The CMTS
        must assign a single id value for each CM MAC address seen
        by the CMTS.  The CMTS should ensure that the association
        between an Id and MAC Address remains constant
        during CMTS uptime."
     ::= { docsIf3CmtsCmRegStatusEntry 1 }

docsIf3CmtsCmRegStatusMacAddr OBJECT-TYPE
     SYNTAX      MacAddress
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the MAC address of the CM.
        If the CM has multiple MAC addresses, this is the MAC
        address associated with the MAC Domain interface."
     ::= { docsIf3CmtsCmRegStatusEntry 2 }

docsIf3CmtsCmRegStatusIPv6Addr OBJECT-TYPE
     SYNTAX      InetAddressIPv6
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the IPv6 address of the
        CM. If the CM has no Internet address assigned, or the
        Internet address is unknown, the value of this attribute
        is the all zeros address."
     ::= { docsIf3CmtsCmRegStatusEntry 3 }

docsIf3CmtsCmRegStatusIPv6LinkLocal OBJECT-TYPE
     SYNTAX      InetAddressIPv6
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the IPv6 local scope address
        of the CM. If the CM has no link local address assigned,
        or the Internet address is unknown, the value
        of this attribute is the all zeros address."
     ::= { docsIf3CmtsCmRegStatusEntry 4 }

docsIf3CmtsCmRegStatusIPv4Addr OBJECT-TYPE
     SYNTAX      InetAddressIPv4
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the IPv4 address of this
        CM. If the CM has no IP address assigned, or the IP address
        is unknown, this object returns 0.0.0.0."
     ::= { docsIf3CmtsCmRegStatusEntry 5 }

docsIf3CmtsCmRegStatusValue OBJECT-TYPE
     SYNTAX      CmtsCmRegState
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the current CM connectivity
        state."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Cable Modem
         Initialization and Reinitialization section."
     ::= { docsIf3CmtsCmRegStatusEntry 6 }

docsIf3CmtsCmRegStatusMdIfIndex OBJECT-TYPE
     SYNTAX      InterfaceIndexOrZero
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the interface Index of
        the CMTS MAC Domain where the CM is active. If the interface
        is unknown, the CMTS returns a value of zero."
     ::= { docsIf3CmtsCmRegStatusEntry 7 }

docsIf3CmtsCmRegStatusMdCmSgId OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the ID of the MAC Domain
        CM Service Group Id (MD-CM-SG-ID) in which the CM is registered.
        If the ID is unknown, the CMTS returns a value
        of zero."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Cable Modem
         Service Group (CM-SG) section."
     ::= { docsIf3CmtsCmRegStatusEntry 8 }

docsIf3CmtsCmRegStatusRcpId OBJECT-TYPE
     SYNTAX      RcpId
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the RCP-ID associated
        with the CM. If the RCP-ID is unknown the CMTS returns
        a five octet long string of zeros."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, RCP-ID
         section in the Common Radio Frequency Interface
         Encodings Annex."
     ::= { docsIf3CmtsCmRegStatusEntry 9 }

docsIf3CmtsCmRegStatusRccStatusId OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the RCC Id the CMTS used
        to configure the CM receive channel set during the registration
        process. If unknown, the CMTS returns the
        value zero."
     ::= { docsIf3CmtsCmRegStatusEntry 10 }

docsIf3CmtsCmRegStatusRcsId OBJECT-TYPE
     SYNTAX      ChSetId
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the Receive Channel Set
        (RCS) that the CM is currently using. If the RCS is unknown,
        the CMTS returns the value zero."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Cable Modem
         Physical Receive Channel Configuration section and the
         Receive Channels section in the Common Radio Frequency
         Interface Encodings Annex."
     ::= { docsIf3CmtsCmRegStatusEntry 11 }

docsIf3CmtsCmRegStatusTcsId OBJECT-TYPE
     SYNTAX      ChSetId
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents Transmit Channel Set (TCS)
        the CM is currently using. If the TCS is unknown,
        the CMTS returns the value zero."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Changes to
         the Transmit Channel Set section."
     ::= { docsIf3CmtsCmRegStatusEntry 12 }

docsIf3CmtsCmRegStatusQosVersion OBJECT-TYPE
     SYNTAX      DocsisQosVersion
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the queuing services the CM 
        registered, either DOCSIS 1.1 QoS or DOCSIS 1.0 CoS mode."
     ::= { docsIf3CmtsCmRegStatusEntry 13 }

docsIf3CmtsCmRegStatusLastRegTime OBJECT-TYPE
     SYNTAX      DateAndTime
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the last time the CM registered."
     ::= { docsIf3CmtsCmRegStatusEntry 14 }

docsIf3CmtsCmRegStatusAddrResolutionReqs OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute counts represents the number of upstream
        packets received on the SIDs assigned to a CM that
        are any of the following:
        Upstream IPv4 ARP Requests
        Upstream IPv6 Neighbor Solicitation Requests
        (For routing CMTSs) Upstream IPv4 or IPv6 packets to
        unresolved destinations in locally connected downstream
        subnets in the HFC.
        Discontinuities in the value of this counter can occur
        at re-initialization of the managed system, and at
        other times as indicated by the value of
        ifCounterDiscontinuityTime for the associated MAC Domain
        interface."
     REFERENCE
         "DOCSIS 3.0 Security Specification CM-SP-MULPIv3.0-I08-080522,
         Secure Provisioning section.
         RFC 2863."
     ::= { docsIf3CmtsCmRegStatusEntry 15 }

docsIf3CmtsCmUsStatusTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3CmtsCmUsStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object defines status information of the CM
        currently in use Upstream Logical Channels, as reported
        by the CMTS."
     ::= { docsIf3MibObjects 4}

docsIf3CmtsCmUsStatusEntry OBJECT-TYPE
     SYNTAX      DocsIf3CmtsCmUsStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3CmtsCmUsStatusTable."
     INDEX {
             docsIf3CmtsCmRegStatusId,
             docsIf3CmtsCmUsStatusChIfIndex
           }
     ::= { docsIf3CmtsCmUsStatusTable 1 }

DocsIf3CmtsCmUsStatusEntry ::= SEQUENCE {
     docsIf3CmtsCmUsStatusChIfIndex
                  InterfaceIndex,
     docsIf3CmtsCmUsStatusModulationType
                  DocsisUpstreamType,
     docsIf3CmtsCmUsStatusRxPower
                  TenthdBmV,
     docsIf3CmtsCmUsStatusSignalNoise
                  TenthdB,
     docsIf3CmtsCmUsStatusMicroreflections
                  Unsigned32,
     docsIf3CmtsCmUsStatusEqData
                  DocsEqualizerData,
     docsIf3CmtsCmUsStatusUnerroreds
                  Counter32,
     docsIf3CmtsCmUsStatusCorrecteds
                  Counter32,
     docsIf3CmtsCmUsStatusUncorrectables
                  Counter32,
     docsIf3CmtsCmUsStatusHighResolutionTimingOffset
                  Integer32,
     docsIf3CmtsCmUsStatusIsMuted
                  TruthValue,
     docsIf3CmtsCmUsStatusRangingStatus
                  RangingState

     }

docsIf3CmtsCmUsStatusChIfIndex OBJECT-TYPE
     SYNTAX      InterfaceIndex
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This attribute is a key that represents the ifIndex
        of the upstream interface."
     ::= { docsIf3CmtsCmUsStatusEntry 1 }

docsIf3CmtsCmUsStatusModulationType OBJECT-TYPE
     SYNTAX      DocsisUpstreamType
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the modulation type currently
        used by this upstream channel."
     ::= { docsIf3CmtsCmUsStatusEntry 2 }

docsIf3CmtsCmUsStatusRxPower OBJECT-TYPE
     SYNTAX      TenthdBmV
     UNITS       "TenthdBmV"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the receive power of this
        upstream channel."
     ::= { docsIf3CmtsCmUsStatusEntry 3 }

docsIf3CmtsCmUsStatusSignalNoise OBJECT-TYPE
     SYNTAX      TenthdB
     UNITS       "TenthdB"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents Signal/Noise ratio as
        perceived for upstream data from the CM on this upstream
        channel."
     ::= { docsIf3CmtsCmUsStatusEntry 4 }

docsIf3CmtsCmUsStatusMicroreflections OBJECT-TYPE
     SYNTAX      Unsigned32 (0..65535)
     UNITS       "-dBc"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents microreflections received
        on this upstream channel."
     ::= { docsIf3CmtsCmUsStatusEntry 5 }

docsIf3CmtsCmUsStatusEqData OBJECT-TYPE
     SYNTAX      DocsEqualizerData
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the equalization data
        for the CM on this upstream channel."
     ::= { docsIf3CmtsCmUsStatusEntry 6 }

docsIf3CmtsCmUsStatusUnerroreds OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the codewords received
        without error from the CM on this interface. Discontinuities
        in the value of this counter can occur at re-initialization
        of the managed system, and at other
        times as indicated by the value of ifCounterDiscontinuityTime
        for the associated upstream channel."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmtsCmUsStatusEntry 7 }

docsIf3CmtsCmUsStatusCorrecteds OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the codewords received
        with correctable errors from the CM on this upstream
        channeli. Discontinuities in the value of this counter
        can occur at re-initialization of the managed system,
        and at other times as indicated by the value of
        ifCounterDiscontinuityTime for the associated upstream
        channel."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmtsCmUsStatusEntry 8 }

docsIf3CmtsCmUsStatusUncorrectables OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the codewords received
        with uncorrectable errors from the CM on this upstream
        channel. Discontinuities in the value of this counter
        can occur at re-initialization of the managed
        system, and at other times as indicated by the value of
        ifCounterDiscontinuityTime for the associated upstream
        channel."
     REFERENCE
        "RFC 2863."
     ::= { docsIf3CmtsCmUsStatusEntry 9 }

docsIf3CmtsCmUsStatusHighResolutionTimingOffset OBJECT-TYPE
     SYNTAX      Integer32
     UNITS       "time tick/(64*256)"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the current measured round
        trip time on this CM's upstream channel in units
        of (6.25 microseconds/(64*256)).  This attribute returns
        zero if the value is unknown."
     ::= { docsIf3CmtsCmUsStatusEntry 10 }

docsIf3CmtsCmUsStatusIsMuted OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute has a value 'true' to indicate that 
        the CM's upstream channel has been muted via 
        CM-CTRL-REQ/CM-CTRL-RSP message exchange."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, section
         Media Access Control specification."
     ::= { docsIf3CmtsCmUsStatusEntry 11 }

docsIf3CmtsCmUsStatusRangingStatus OBJECT-TYPE
     SYNTAX      RangingState
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute denotes the ranging state of the CM."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, section
         Media Access Control specification."
     ::= { docsIf3CmtsCmUsStatusEntry 12 }

docsIf3MdChCfgTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3MdChCfgEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object configures the association of downstream
        and upstream channels to a particular MAC Domain
        (MD) on a CMTS.  The creation of channels and MAC domain
        object interface instances is vendor-specific.
        In particular, the assignment of the channel interface
        index is normally vendor-specific. Therefore,
        this object is intended only for associating channels
        to a MAC Domain and assumes that those channels were
        previously configured.
        The CMTS may have restrictions on which channels can
        be configured in the same MAC Domain.  For example, it
        could require the upstream channels to be from the same
        line card.
        This object supports the creation and deletion of multiple
        instances.
        Creation of a new instance of this object requires the
        ChId attribute to be set."
     ::= { docsIf3MibObjects 5}

docsIf3MdChCfgEntry OBJECT-TYPE
     SYNTAX      DocsIf3MdChCfgEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3MdChCfgTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the channel is configured.
         The CMTS persists all instances of MdChCfg across
         reinitializations."
     INDEX {
             ifIndex,
             docsIf3MdChCfgChIfIndex
           }
     ::= { docsIf3MdChCfgTable 1 }

DocsIf3MdChCfgEntry ::= SEQUENCE {
     docsIf3MdChCfgChIfIndex
                  InterfaceIndex,
     docsIf3MdChCfgIsPriCapableDs
                  TruthValue,
     docsIf3MdChCfgChId
                  ChId,
     docsIf3MdChCfgSfProvAttrMask
                  AttributeMask,
     docsIf3MdChCfgRowStatus
                  RowStatus
     }

docsIf3MdChCfgChIfIndex OBJECT-TYPE
     SYNTAX      InterfaceIndex
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents the interface index of an existing
        upstream or downstream channel that is configured
        to be part of the MAC Domain.
        For the case of upstream interfaces the CMTS could reject
        the assignment of upstream logical channels under
        the same physical upstream interface to different
        MAC Domains."
     ::= { docsIf3MdChCfgEntry 1 }

docsIf3MdChCfgIsPriCapableDs OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "If set to 'true', this attribute configures the downstream
        channel as Primary-Capable. 
        The default value for a downstream channel is 'true'.
        This attribute is not relevant for upstream interfaces, 
        therefore it reports the value 'false' for such interfaces.
        A CMTS may restrict the permitted value of this attribute
        based upon physical channel capabilities."
     ::= { docsIf3MdChCfgEntry 2 }

docsIf3MdChCfgChId OBJECT-TYPE
     SYNTAX      ChId (1..255)
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "This attribute contains the 8-bit Downstream Channel
        ID (DCID) or Upstream Channel ID (UCID) configured
        for the channel in the MAC Domain."
     ::= { docsIf3MdChCfgEntry 3 }

docsIf3MdChCfgSfProvAttrMask OBJECT-TYPE
     SYNTAX      AttributeMask
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "This attribute contains Provisioned Attribute Mask
        of non-bonded service flow assignment to this channel."
     DEFVAL { '00000000'H }
     ::= { docsIf3MdChCfgEntry 4 }

docsIf3MdChCfgRowStatus OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "The status of this instance."
     ::= { docsIf3MdChCfgEntry 5 }

docsIf3RccCfgTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3RccCfgEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object identifies the scope of the Receive Channel
        Configuration (RCC) and provides a top level container
        for the Receive Module and Receive Channel
        objects.  The CMTS selects an instance of this object
        to assign to a CM when it registers.
        This object supports the creation and deletion of multiple
        instances."
     ::= { docsIf3MibObjects 6}

docsIf3RccCfgEntry OBJECT-TYPE
     SYNTAX      DocsIf3RccCfgEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3RccCfgTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the RCC is configured.
          The CMTS persists all instances of RccCfg across
          reinitializations."
     INDEX {
             ifIndex,
             docsIf3RccCfgRcpId,
             docsIf3RccCfgRccCfgId
           }
     ::= { docsIf3RccCfgTable 1 }

DocsIf3RccCfgEntry ::= SEQUENCE {
     docsIf3RccCfgRcpId
                  RcpId,
     docsIf3RccCfgRccCfgId
                  Unsigned32,
     docsIf3RccCfgVendorSpecific
                  OCTET STRING,
     docsIf3RccCfgDescription
                  SnmpAdminString,
     docsIf3RccCfgRowStatus
                  RowStatus
     }

docsIf3RccCfgRcpId OBJECT-TYPE
     SYNTAX      RcpId
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents the 'Receive Channel Profile
        Identifier' (RCP-ID) configured for the MAC Domain
        indicated by this instance."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Standard
         Receive Channel Profile Encodings Annex."
     ::= { docsIf3RccCfgEntry 1 }

docsIf3RccCfgRccCfgId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..4294967295)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key denotes an RCC combination assignment for
        a particular RcpId and is unique per combination of
        MAC Domain and RcpId."
     ::= { docsIf3RccCfgEntry 2 }

docsIf3RccCfgVendorSpecific OBJECT-TYPE
     SYNTAX      OCTET STRING (SIZE(0..252))
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "This attribute contains vendor-specific information
        of the CM Receive Channel configuration."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Receive Channel
         Profile/Configuration Vendor Specific Parameters section
         in the Common Radio Frequency Interface Encodings Annex."
     DEFVAL { ''H }
     ::= { docsIf3RccCfgEntry 3 }

docsIf3RccCfgDescription OBJECT-TYPE
     SYNTAX      SnmpAdminString (SIZE (0..15))
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "This attribute contains a human-readable description
        of the CM RCP Configuration."
     DEFVAL { "" }
     ::= { docsIf3RccCfgEntry 4 }

docsIf3RccCfgRowStatus OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "The status of this instance."
     ::= { docsIf3RccCfgEntry 5 }

docsIf3RccStatusTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3RccStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "The RCC Status object provides a read-only view of
        the statically-configured (from the RccCfg object)
        and dynamically-created RCCs.
        The CMTS creates an RCC Status instance for each unique
        MAC Domain Cable Modem Service Group (MD-CM-SG) to
        which it signals an RCC to the CM."
     ::= { docsIf3MibObjects 7}

docsIf3RccStatusEntry OBJECT-TYPE
     SYNTAX      DocsIf3RccStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3RccStatusTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the RCC is configured."
     INDEX {
             ifIndex,
             docsIf3RccStatusRcpId,
             docsIf3RccStatusRccStatusId
            }
     ::= { docsIf3RccStatusTable 1 }

DocsIf3RccStatusEntry ::= SEQUENCE {
     docsIf3RccStatusRcpId
                  RcpId,
     docsIf3RccStatusRccStatusId
                  Unsigned32,
     docsIf3RccStatusRccCfgId
                  Unsigned32,
     docsIf3RccStatusValidityCode
                  INTEGER,
     docsIf3RccStatusValidityCodeText
                  SnmpAdminString
     }

docsIf3RccStatusRcpId OBJECT-TYPE
     SYNTAX      RcpId
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents the RCP-ID to which this instance
        applies."
     ::= { docsIf3RccStatusEntry 1 }

docsIf3RccStatusRccStatusId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..4294967295)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents an RCC combination for a particular
        RcpId either from an RCC configuration object
        or a CMTS-determined RCC and is unique per combination
        of MAC Domain IfIndex and RcpId."
     ::= { docsIf3RccStatusEntry 2 }

docsIf3RccStatusRccCfgId OBJECT-TYPE
     SYNTAX      Unsigned32 (0..65535)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute identifies an RCC-Configured combination
        from which this instance was defined. If nonzero,
        it corresponds to the RccCfg instance from which
        the RCC was created. Zero means that the  RCC was dynamically
        created by the CMTS."
     ::= { docsIf3RccStatusEntry 3 }

docsIf3RccStatusValidityCode OBJECT-TYPE
     SYNTAX      INTEGER {other(1),
                         valid(2),
                         invalid(3),
                         wrongPrimaryDs(4),
                         missingPrimaryDs(5),
                         multiplePrimaryDs(6),
                         duplicateDs(7),
                         wrongFrequencyRange(8),
                         wrongConnectivity(9)
                         }
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute indicates whether the RCC instance
        of this object is valid or not. An RCC Status instance
        from a configured or a dynamic RCC could become invalid,
        for example, due changes in the topology."
     ::= { docsIf3RccStatusEntry 4 }

docsIf3RccStatusValidityCodeText OBJECT-TYPE
     SYNTAX      SnmpAdminString
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute contains the CMTS vendor-specific
        log information from the Receive Channel Configuration
        Status encoding."
     ::= { docsIf3RccStatusEntry 5 }

docsIf3RxChCfgTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3RxChCfgEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "The Receive Channel Configuration object permits
        an operator to configure how CMs registered with certain
        Receive Channel Profiles will configure the Receive
        Channels within their profile. When a CM registers
        with an RCP for which all Receive Channel Indices
        (RcIds) are configured in the Receive Module object
        and all Receive Channels are configured within this
        object, the CMTS should use the configuration within
        these objects to set the Receive Channel Configuration
        returned to the CM in a REG-RSP message.  A CMTS
        may require configuration of all pertinent Receive
        Module and Receive Channel instances in order to register
        a CM that reports a Receive Channel Profile (RCP),
        including any standard Receive Channel Profiles.
        If the CM reports multiple RCPs, and Receive Module
        and Receive Channel objects have instances for more
        than one RCP, the particular RCP selected by the CMTS
        is not specified.  A CMTS is not restricted to assigning
        Receive Modules based only on the contents of this
        object.
        This object supports the creation and deletion of multiple
        instances.
        Creation of a new instance of this object requires the
        ChIfIndex attribute to be set and a valid reference of
        a RccCfg instance."
     ::= { docsIf3MibObjects 8}

docsIf3RxChCfgEntry OBJECT-TYPE
     SYNTAX      DocsIf3RxChCfgEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3RxChCfgTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the RCC is configured.
         The CMTS persists all instances of ReceiveChannelCfg across
         reinitializations."
     INDEX { 
             ifIndex,
             docsIf3RccCfgRcpId,
             docsIf3RccCfgRccCfgId,
             docsIf3RxChCfgRcId
           }
     ::= { docsIf3RxChCfgTable 1 }

DocsIf3RxChCfgEntry ::= SEQUENCE {
     docsIf3RxChCfgRcId
                  Unsigned32,
     docsIf3RxChCfgChIfIndex
                  InterfaceIndex,
     docsIf3RxChCfgPrimaryDsIndicator
                  TruthValue,
     docsIf3RxChCfgRcRmConnectivityId
                  Unsigned32,
     docsIf3RxChCfgRowStatus
                  RowStatus
     }

docsIf3RxChCfgRcId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..255)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents an identifier for the parameters
        of the Receive Channel instance within the Receive
        Channel Profile."
     REFERENCE
        "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
        Specification CM-SP-MULPIv3.0-I08-080522, Receive
        Channel Index section in the Common Radio Frequency
        Interface Encodings Annex."
     ::= { docsIf3RxChCfgEntry 1 }

docsIf3RxChCfgChIfIndex OBJECT-TYPE
     SYNTAX      InterfaceIndex
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "This attribute contains the interface index of a Downstream
        Channel that this Receive Channel Instance
        defines."
     ::= { docsIf3RxChCfgEntry 2 }

docsIf3RxChCfgPrimaryDsIndicator OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "If set to 'true', this attribute indicates the Receive
        Channel is to be the primary-capable downstream
        channel for the CM receiving this RCC. Otherwise, the
        downstream channel is to be a non-primary-capable
        channel."
     REFERENCE
        "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
        Specification CM-SP-MULPIv3.0-I08-080522, Receive Channel
        Primary Downstream Channel Indicator section in the Common
        Radio Frequency Interface Encodings Annex."
     DEFVAL { false }
     ::= { docsIf3RxChCfgEntry 3 }

docsIf3RxChCfgRcRmConnectivityId OBJECT-TYPE
     SYNTAX      Unsigned32 (0..255)
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "This attribute indicates the Receive Module (via
        the RmId from the ReceiveModule object) to which this
        Receive Channel connects.  If this object contains
        a zero value (and thus no Receive Channel Connectivity),
        the Receive Channel Connectivity TLV is omitted
        from the RCC."
     REFERENCE
        "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
        Specification CM-SP-MULPIv3.0-I08-080522, Receive
        Channel Connectivity section in the Common Radio
        Frequency Interface Encodings Annex."
     DEFVAL { 0 }
     ::= { docsIf3RxChCfgEntry 4 }

docsIf3RxChCfgRowStatus OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "The status of this instance."
     ::= { docsIf3RxChCfgEntry 5 }

docsIf3RxChStatusTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3RxChStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "The Receive Channel Status object reports the status
        of the statically-configured and dynamically-created
        Receive Channels within an RCC."
     ::= { docsIf3MibObjects 9}

docsIf3RxChStatusEntry OBJECT-TYPE
     SYNTAX      DocsIf3RxChStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3RxChStatusTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the RCC is configured. When this object is defined
         on the CM, the value of RccStatusId is always 1."
     INDEX {
             ifIndex,
             docsIf3RccStatusRcpId,
             docsIf3RccStatusRccStatusId,
             docsIf3RxChStatusRcId
           }
     ::= { docsIf3RxChStatusTable 1 }

DocsIf3RxChStatusEntry ::= SEQUENCE {
     docsIf3RxChStatusRcId
                  Unsigned32,
     docsIf3RxChStatusChIfIndex
                  InterfaceIndex,
     docsIf3RxChStatusPrimaryDsIndicator
                  TruthValue,
     docsIf3RxChStatusRcRmConnectivityId
                  Unsigned32
     }

docsIf3RxChStatusRcId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..255)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents an identifier for the parameters
        of the Receive Channel instance within the Receive
        Channel Profile."
     ::= { docsIf3RxChStatusEntry 1 }

docsIf3RxChStatusChIfIndex OBJECT-TYPE
     SYNTAX      InterfaceIndex
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute contains the interface index of the
        Downstream Channel that this Receive Channel Instance
        defines."
     ::= { docsIf3RxChStatusEntry 2 }

docsIf3RxChStatusPrimaryDsIndicator OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "If set to 'true', this attribute indicates the Receive
        Channel is to be the primary-capable downstream
        channel for the CM receiving this RCC. Otherwise, the
        downstream channel is to be a non-primary-capable
        channel."
     ::= { docsIf3RxChStatusEntry 3 }

docsIf3RxChStatusRcRmConnectivityId OBJECT-TYPE
     SYNTAX      Unsigned32 (0..255)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute identifies the Receive Module to which
        this Receive Channel connects.  A value a zero indicates
        that the Receive Channel Connectivity TLV is
        omitted from the RCC."
     ::= { docsIf3RxChStatusEntry 4 }

docsIf3RxModuleCfgTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3RxModuleCfgEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "The Receive Module Configuration object permits
        an operator to configure how CMs with certain Receive
        Channel Profiles (RCPs) will configure the Receive
        Modules within their profile upon CM registration.
         When a CM registers with an RCP for which all Receive
        Module Indices (RmIds) are configured in this object
        and all Receive Channels are configured within the
        Receive Channel (ReceiveChannel) object, the CMTS
        should use the configuration within these objects to
        set the Receive Channel Configuration assigned to
        the CM in a REG-RSP message.  A CMTS may require configuration
        of all pertinent Receive Module and Receive
        Channel instances (i.e., MIB table entries) in order
        to register a CM that reports a Receive Channel Profile.
         If the CM reports multiple RCPs, and Receive Module
        and Receive Channel objects have instances (i.e.,
        MIB table entries) for more than one RCP reported by
        the CM, the particular RCP selected by the CMTS is not
        specified.  A CMTS is not restricted to assigning Receive
        Modules based only on the contents of this object.

        This object supports the creation and deletion of multiple
        instances.
        Creation of a new instance of this object requires the
        reference of a valid RccCfg instance."
     ::= { docsIf3MibObjects 10}

docsIf3RxModuleCfgEntry OBJECT-TYPE
     SYNTAX      DocsIf3RxModuleCfgEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3RxModuleCfgTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the RCC is configured."
     INDEX {
             ifIndex,
             docsIf3RccCfgRcpId,
             docsIf3RccCfgRccCfgId,
             docsIf3RxModuleCfgRmId
           }
     ::= { docsIf3RxModuleCfgTable 1 }

DocsIf3RxModuleCfgEntry ::= SEQUENCE {
     docsIf3RxModuleCfgRmId
                  Unsigned32,
     docsIf3RxModuleCfgRmRmConnectivityId
                  Unsigned32,
     docsIf3RxModuleCfgFirstCenterFrequency
                  Unsigned32,
     docsIf3RxModuleCfgRowStatus
                  RowStatus
     }

docsIf3RxModuleCfgRmId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..255)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents an identifier of a Receive Module
        instance within the Receive Channel Profile."
     REFERENCE
        "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
        Specification CM-SP-MULPIv3.0-I08-080522, Receive Module
        Index in the Common Radio Frequency Interface Encodings
        Annex."
     ::= { docsIf3RxModuleCfgEntry 1 }

docsIf3RxModuleCfgRmRmConnectivityId OBJECT-TYPE
     SYNTAX      Unsigned32 (0..255)
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "This attribute represents the higher level (i.e.
        closer to RF) Receive Module to which this Receive Module
        connects.  If this object contains a zero value (and
        thus no Receive Module Connectivity), the Receive
        Module Connectivity TLV is omitted from the RCC.
        Within a single instance of the ReceiveModule object,
        the RmRmConnectivityId attribute cannot contain
        the same value as the RmId attribute.  The RmRmConnectivityId
        attribute points to a separate ReceiveModule
        object instance with the same value of RccCfgId."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Receive Module
         Connectivity section in the Common Radio Frequency Interface
         Encodings Annex."
     DEFVAL { 0 }
     ::= { docsIf3RxModuleCfgEntry 2 }

docsIf3RxModuleCfgFirstCenterFrequency OBJECT-TYPE
     SYNTAX      Unsigned32
     UNITS       "Hz"
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "This attribute represents the center frequency,
        in Hz, and a multiple of 62500, that indicates the lowest
        frequency channel of the Receive Module, or 0 if not
        applicable to the Receive Module."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Receive Module
         First Channel Center Frequency Assignment section in the
         Common Radio Frequency Interface Encodings Annex."
     ::= { docsIf3RxModuleCfgEntry 3 }

docsIf3RxModuleCfgRowStatus OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "The status of this instance."
     ::= { docsIf3RxModuleCfgEntry 4 }

docsIf3RxModuleStatusTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3RxModuleStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "The Receive Module Status object provides a read-only
        view of the statically configured and dynamically
        created Receive Modules within an RCC."
     ::= { docsIf3MibObjects 11}

docsIf3RxModuleStatusEntry OBJECT-TYPE
     SYNTAX      DocsIf3RxModuleStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3RxModuleStatusTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the RCC is configured. When this object is defined
         on the CM, the value of RccStatusId is always 1."
     INDEX {
             ifIndex,
             docsIf3RccStatusRcpId,
             docsIf3RccStatusRccStatusId,
             docsIf3RxModuleStatusRmId
           }
     ::= { docsIf3RxModuleStatusTable 1 }

DocsIf3RxModuleStatusEntry ::= SEQUENCE {
     docsIf3RxModuleStatusRmId
                  Unsigned32,
     docsIf3RxModuleStatusRmRmConnectivityId
                  Unsigned32,
     docsIf3RxModuleStatusFirstCenterFrequency
                  Unsigned32
     }

docsIf3RxModuleStatusRmId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..255)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents an identifier of a Receive Module
        instance within the Receive Channel Profile."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Receive
         Module Index section in the Common Radio Frequency
         Interface Encodings Annex."
     ::= { docsIf3RxModuleStatusEntry 1 }

docsIf3RxModuleStatusRmRmConnectivityId OBJECT-TYPE
     SYNTAX      Unsigned32 (0..255)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the Receive Module to which
        this Receive Module connects. Requirements for
        module connectivity are detailed in the RmRmConnectivityId
        of the RccCfg object."
     ::= { docsIf3RxModuleStatusEntry 2 }

docsIf3RxModuleStatusFirstCenterFrequency OBJECT-TYPE
     SYNTAX      Unsigned32
     UNITS       "Hz"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the low frequency channel
        of the Receive Module, or 0 if not applicable to the
        Receive Module."
     ::= { docsIf3RxModuleStatusEntry 3 }

docsIf3MdNodeStatusTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3MdNodeStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object reports the MD-DS-SG-ID and MD-US-SG-ID
        associated with a MD-CM-SG-ID within a MAC Domain
        and the Fiber Nodes reached by the MD-CM-SG."
     ::= { docsIf3MibObjects 12}

docsIf3MdNodeStatusEntry OBJECT-TYPE
     SYNTAX      DocsIf3MdNodeStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3MdNodeStatusTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the MD-CM-SG-ID is configured."
     INDEX {
             ifIndex,
             docsIf3MdNodeStatusNodeName,
             docsIf3MdNodeStatusMdCmSgId 
           }
     ::= { docsIf3MdNodeStatusTable 1 }

DocsIf3MdNodeStatusEntry ::= SEQUENCE {
     docsIf3MdNodeStatusNodeName
                  NodeName,
     docsIf3MdNodeStatusMdCmSgId
                  Unsigned32,
     docsIf3MdNodeStatusMdDsSgId
                  Unsigned32,
     docsIf3MdNodeStatusMdUsSgId
                  Unsigned32
     }

docsIf3MdNodeStatusNodeName OBJECT-TYPE
     SYNTAX      NodeName (SIZE (1..16))
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents the name of a fiber node associated
        with a MD-CM-SG of a MAC Domain."
     ::= { docsIf3MdNodeStatusEntry 1 }

docsIf3MdNodeStatusMdCmSgId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..4294967295)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This attribute is a key and indicates the MD-CM-SG-ID
        of this instance. A particular MdCmSgId in a MAC Domain
        is associated with one or more Fiber Nodes."
     ::= { docsIf3MdNodeStatusEntry 2 }

docsIf3MdNodeStatusMdDsSgId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..255)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute corresponds to the MD-DS-SG-ID of
        the MD-CM-SG of this object instance. The MdDsSgId values
        are unique within a MAC Domain."
     ::= { docsIf3MdNodeStatusEntry 3 }

docsIf3MdNodeStatusMdUsSgId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..255)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute corresponds to the MD-US-SG-ID of
        the MD-CM-SG of this object instance. The MdUsSgId values
        are unique within a MAC Domain."
     ::= { docsIf3MdNodeStatusEntry 4 }

docsIf3MdDsSgStatusTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3MdDsSgStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object returns the list of downstream channel
        associated with a MAC Domain MD-DS-SG-ID."
     ::= { docsIf3MibObjects 13}

docsIf3MdDsSgStatusEntry OBJECT-TYPE
     SYNTAX      DocsIf3MdDsSgStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3MdDsSgStatusTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the MD-DS-SG-ID is configured.
         The CMTS is not required to persist instances of this
         object across reinitializations."
     INDEX {
             ifIndex,
             docsIf3MdDsSgStatusMdDsSgId
           }
     ::= { docsIf3MdDsSgStatusTable 1 }

DocsIf3MdDsSgStatusEntry ::= SEQUENCE {
     docsIf3MdDsSgStatusMdDsSgId
                  Unsigned32,
     docsIf3MdDsSgStatusChSetId
                  ChSetId
     }

docsIf3MdDsSgStatusMdDsSgId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..255)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents a MD-DS-SG-ID in a Mac Domain."
     ::= { docsIf3MdDsSgStatusEntry 1 }

docsIf3MdDsSgStatusChSetId OBJECT-TYPE
     SYNTAX      ChSetId
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents a reference to the list
        of downstream channels of the MD-DS-SG-ID."
     ::= { docsIf3MdDsSgStatusEntry 2 }

docsIf3MdUsSgStatusTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3MdUsSgStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object returns the list of upstream channels
        associated with a MAC Domain MD-US-SG-ID."
     ::= { docsIf3MibObjects 14}

docsIf3MdUsSgStatusEntry OBJECT-TYPE
     SYNTAX      DocsIf3MdUsSgStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3MdUsSgStatusTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the MD-DS-SG-ID is configured.
         The CMTS is not required to persist instances of this
         object across reinitializations."
     INDEX {
             ifIndex,
             docsIf3MdUsSgStatusMdUsSgId
           }
     ::= { docsIf3MdUsSgStatusTable 1 }

DocsIf3MdUsSgStatusEntry ::= SEQUENCE {
     docsIf3MdUsSgStatusMdUsSgId
                  Unsigned32,
     docsIf3MdUsSgStatusChSetId
                  ChSetId
     }

docsIf3MdUsSgStatusMdUsSgId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..255)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents a MD-US-SG-ID in a Mac Domain."
     ::= { docsIf3MdUsSgStatusEntry 1 }

docsIf3MdUsSgStatusChSetId OBJECT-TYPE
     SYNTAX      ChSetId
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents a reference to the list
        of upstream channels of the MD-US-SG-ID."
     ::= { docsIf3MdUsSgStatusEntry 2 }

docsIf3MdUsToDsChMappingTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3MdUsToDsChMappingEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object returns the set of downstream channels
        that carry UCDs and MAPs for a particular upstream channel
        in a MAC Domain."
     ::= { docsIf3MibObjects 15}

docsIf3MdUsToDsChMappingEntry OBJECT-TYPE
     SYNTAX      DocsIf3MdUsToDsChMappingEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3MdUsToDsChMappingTable."
     INDEX {
             docsIf3MdUsToDsChMappingUsIfIndex,
             docsIf3MdUsToDsChMappingDsIfIndex,
             docsIf3MdUsToDsChMappingMdIfIndex
           }
     ::= { docsIf3MdUsToDsChMappingTable 1 }

DocsIf3MdUsToDsChMappingEntry ::= SEQUENCE {
     docsIf3MdUsToDsChMappingUsIfIndex
                  InterfaceIndex,
     docsIf3MdUsToDsChMappingDsIfIndex
                  InterfaceIndex,
     docsIf3MdUsToDsChMappingMdIfIndex
                  InterfaceIndex
     }

docsIf3MdUsToDsChMappingUsIfIndex OBJECT-TYPE
     SYNTAX      InterfaceIndex
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents the interface index of the upstream
        channel to which this instance applies."
     ::= { docsIf3MdUsToDsChMappingEntry 1 }

docsIf3MdUsToDsChMappingDsIfIndex OBJECT-TYPE
     SYNTAX      InterfaceIndex
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents the interface index of a downstream
        channel carrying in UCDs and Maps associated with
        the upstream channel defined by this instance."
     ::= { docsIf3MdUsToDsChMappingEntry 2 }

docsIf3MdUsToDsChMappingMdIfIndex OBJECT-TYPE
     SYNTAX      InterfaceIndex
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This key represents the MAC domain of the upstream
        and downstream channels of this instance."
     ::= { docsIf3MdUsToDsChMappingEntry 3 }

docsIf3MdCfgTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3MdCfgEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object contains MAC domain level control and
        configuration attributes."
     ::= { docsIf3MibObjects 16}

docsIf3MdCfgEntry OBJECT-TYPE
     SYNTAX      DocsIf3MdCfgEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3MdCfgTable.
         The CMTS persists all instances of MdCfg across
         reinitializations.
         The ifIndex key corresponds to the MAC Domain interface."
     INDEX {
             ifIndex
           }
     ::= { docsIf3MdCfgTable 1 }

DocsIf3MdCfgEntry ::= SEQUENCE {
     docsIf3MdCfgMddInterval
                  Unsigned32,
     docsIf3MdCfgIpProvMode
                  INTEGER,
     docsIf3MdCfgCmStatusEvCtlEnabled
                  TruthValue,
     docsIf3MdCfgUsFreqRange
                  INTEGER,
     docsIf3MdCfgMcastDsidFwdEnabled
                  TruthValue,
     docsIf3MdCfgMultRxChModeEnabled
                  TruthValue,
     docsIf3MdCfgMultTxChModeEnabled
                  TruthValue,
     docsIf3MdCfgEarlyAuthEncrCtrl
                  INTEGER,
     docsIf3MdCfgTftpProxyEnabled
                  TruthValue,
     docsIf3MdCfgSrcAddrVerifEnabled
                  TruthValue,
     docsIf3MdCfgDownChannelAnnex
                  INTEGER,
     docsIf3MdCfgCmUdcEnabled
                  TruthValue,
     docsIf3MdCfgSendUdcRulesEnabled
                  TruthValue,
     docsIf3MdCfgServiceTypeIdList
                  SnmpTagList            
     }

docsIf3MdCfgMddInterval OBJECT-TYPE
     SYNTAX      Unsigned32 (1..2000)
     UNITS       "milliseconds"
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "This attribute configures the interval for the insertion
        of MDD messages in each downstream channel of
        a MAC Domain."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Parameters
         and Constants Annex."
     DEFVAL { 2000 }
     ::= { docsIf3MdCfgEntry 1 }

docsIf3MdCfgIpProvMode OBJECT-TYPE
     SYNTAX      INTEGER {
        ipv4Only(0),
        ipv6Only(1),
        alternate(2),
        dualStack(3)
     }
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "This attribute configures the CMTS IP provisioning
        mode for a MAC Domain. 
        When this attribute is set to 'ipv4Only' the CM will acquire
        a single IPv4 address for the CM management stack.
        When this attribute is set to 'ipv6Only' the CM will acquire
        a single IPv6 address for the CM management stack.
        When this attribute is set to 'alternate' the CM will acquire a
        single IPv6 address for the CM management stack and, if failures
        occur, the CM will fall back to provision and operation with
        an IPv4 address.
        When this attribute is set to 'dualStack' the CM will acquire both
        an IPv6 and IPv4 address for provisioning and operation."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, IP Initialization
         Parameters TLV section."
     DEFVAL { ipv6Only }
     ::= { docsIf3MdCfgEntry 2 }

docsIf3MdCfgCmStatusEvCtlEnabled OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "If set to 'true', this attribute enables the signaling
        of the CM-Status Event reporting mechanism."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, CM-STATUS
         Event Control section "
     DEFVAL { true }
     ::= { docsIf3MdCfgEntry 3 }

docsIf3MdCfgUsFreqRange OBJECT-TYPE
     SYNTAX      INTEGER {
                           standard(0),
                           extended(1)
                         }
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "This attribute indicates in MDD messages the upstream
        frequency upper band edge of an upstream Channel.

        A value 'standard' means Standard Frequency Range and
        a value 'extended' means Extended Frequency Range."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Upstream
         Frequency Upper Band Edge TLV section."
     DEFVAL { standard }
     ::= { docsIf3MdCfgEntry 4 }

docsIf3MdCfgMcastDsidFwdEnabled OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "If set to 'true', this attribute enables the CMTS to
        use IP Multicast DSID Forwarding (MDF) for the MAC domain."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Multicast
         DSID-based Forwarding (MDF) Modes section in the
         Compatibility with Previous Versions of DOCSIS Annex."
     DEFVAL { true }
     ::= { docsIf3MdCfgEntry 5 }

docsIf3MdCfgMultRxChModeEnabled OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "If set to 'true', this attribute enables Downstream
        Channel Bonding for the MAC Domain."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Downstream
         Channel Bonding section."
     DEFVAL { true }
     ::= { docsIf3MdCfgEntry 6 }

docsIf3MdCfgMultTxChModeEnabled OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "If set to 'true', this attribute enables Multiple
        Transmit Channel (MTC) Mode for the MAC Domain."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Upstream
         Channel Bonding section."
     DEFVAL { true }
     ::= { docsIf3MdCfgEntry 7 }

docsIf3MdCfgEarlyAuthEncrCtrl OBJECT-TYPE
     SYNTAX      INTEGER {
                           disableEae(1),
                           enableEaeRangingBasedEnforcement(2),
                           enableEaeCapabilityBasedEnforcement(3),
                           enableEaeTotalEnforcement(4)
                         }
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "This attribute enables or disables early authentication
        and encryption (EAE) signaling for the MAC Domain.
        It also defines the type of EAE enforcement in
        the case that EAE is enabled.
        If set to 'disableEAE', EAE is disabled for the MAC Domain.

        If set to 'enableEaeRangingBasedEnforcement',
        'enableEaeCapabilityBasedEnforcement'
        or 'enableEaeTotalEnforcement',
        EAE is enabled for the MAC Domain.

        The following EAE enforcement methods are defined in
        the case where EAE signaling is enabled:
        The option 'enableEaeRangingBasedEnforcement' indicates
        EAE is enforced on CMs that perform ranging
        with a B-INIT-RNG-REQ message.
        The option 'enableEaeCapabilityBasedEnforcement'
        indicates EAE is enforced on CMs that perform ranging
        with a B-INIT-RNG-REQ message in which the EAE capability
        flag is set.
        The option 'enableEaeTotalEnforcement' indicates
        EAE is enforced on all CMs regardless of their EAE
        capabilities."
     REFERENCE
         "DOCSIS 3.0 Security Specification CM-SP-SECv3.0-I06-071206,
          Early Authentication and Encryption section."
     DEFVAL { enableEaeRangingBasedEnforcement }
     ::= { docsIf3MdCfgEntry 8 }

docsIf3MdCfgTftpProxyEnabled OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "If set to 'true', this attribute enables TFTP Proxy
        functionality for the MAC Domain."
     REFERENCE
         "DOCSIS 3.0 Security Specification CM-SP-SECv3.0-I06-071206,
         TFTP Configuration File Security section."
     DEFVAL { true }
     ::= { docsIf3MdCfgEntry 9 }

docsIf3MdCfgSrcAddrVerifEnabled OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "If set to 'true', this attribute enables Source Address
        Verification (SAV) functionality for the MAC
        Domain."
     REFERENCE
         "DOCSIS 3.0 Security Specification CM-SP-SECv3.0-I06-071206,
         Source Address Verification section."
     DEFVAL { true }
     ::= { docsIf3MdCfgEntry 10 }

docsIf3MdCfgDownChannelAnnex  OBJECT-TYPE
     SYNTAX      INTEGER {
         unknown(1),
         other(2),
         annexA(3),
         annexB(4),
         annexC(5)
        }
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
         "This attribute defines the ITU-J-83 Annex being used 
          for this MAC Domain.  The value of this attribute 
          indicates the conformance of the implementation to 
          important regional cable standards.  
          Valid enumerations for the attribute are:
          unknown
          other
          annexA : Annex A from ITU-J83 is used.
          annexB : Annex B from ITU-J83 is used.
          annexC : Annex C from ITU-J83 is used. 
          Values 6-255 are reserved."
      DEFVAL { unknown }
     ::= { docsIf3MdCfgEntry 11 }

docsIf3MdCfgCmUdcEnabled OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "If set to 'true', this attribute instructs the CMTS MAC 
         Domain to enable Upstream Drop Classifiers (UDC) for the 
         CMs attempting registration in this MAC Domain."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Subscriber Management
         TLVs section in the Common Radio Frequency Interface Encodings
         Annex."
     DEFVAL { false }
     ::= { docsIf3MdCfgEntry 12 }

docsIf3MdCfgSendUdcRulesEnabled OBJECT-TYPE
     SYNTAX      TruthValue
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "If set to 'true' and when the CM signals to the CMTS
        'Upstream Drop Classifier Group ID' encodings, this attribute
        instructs the CMTS MAC Domain to send the Subscriber 
        Management Filters rules associated with the 'Upstream Drop
        Classifier Group ID' encodings to the CM in the form of UDCs 
        when the following conditions occurs:
        - The attribute CmUdcEnabled value for this MAC Domain 
          is set to 'true', and 
        - The CM has the UDC capability advertised as supported. 
        If there is no a single Subscriber Management Filter 
        configured in the CMTS for the CM's signaled UDC Group ID,
        the CMTS does not send UDC encodings to the CM.

        It is vendor specific whether the CMTS maintains enforcement
        of the CM signaled or default Subscriber Management Filter 
        groups in the upstream direction."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Subscriber Management
         TLVs section in the Common Radio Frequency Interface Encodings
         Annex."
     DEFVAL { false }
     ::= { docsIf3MdCfgEntry 13 }

docsIf3MdCfgServiceTypeIdList OBJECT-TYPE
     SYNTAX      SnmpTagList
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "This attribure indicates the list of Service Type IDs 
        associated with the MAC Domain. 
        During the CM registration process the CMTS will attempt to
        redirect the CM to a MAC Domain where the CM' Service Type TLV
        is contained in this attribute."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Service Type 
         Identifier section in the Common Radio Frequency Interface 
         Encodings Annex."
     DEFVAL { "" }
     ::= { docsIf3MdCfgEntry 14 }        
        
docsIf3BondingGrpCfgTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3BondingGrpCfgEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object defines statically configured Downstream
        Bonding Groups and Upstream Bonding Groups on
        the CMTS.
        This object supports the creation and deletion of multiple
        instances.
        Creation of a new instance of this object requires the
        ChList attribute to be set."
     ::= { docsIf3MibObjects 17}

docsIf3BondingGrpCfgEntry OBJECT-TYPE
     SYNTAX      DocsIf3BondingGrpCfgEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3BondingGrpCfgTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the Bonding Group is configured.
         The CMTS persists all instances of BondingGrpCfg
         across reinitializations."
     INDEX {
             ifIndex,
             docsIf3BondingGrpCfgDir,
             docsIf3BondingGrpCfgCfgId
           }
     ::= { docsIf3BondingGrpCfgTable 1 }

DocsIf3BondingGrpCfgEntry ::= SEQUENCE {
     docsIf3BondingGrpCfgDir
                  IfDirection,
     docsIf3BondingGrpCfgCfgId
                  Unsigned32,
     docsIf3BondingGrpCfgChList
                  ChannelList,
     docsIf3BondingGrpCfgSfProvAttrMask
                  AttributeMask,
     docsIf3BondingGrpCfgDsidReseqWaitTime
                  Unsigned32,
     docsIf3BondingGrpCfgDsidReseqWarnThrshld
                  Unsigned32,
     docsIf3BondingGrpCfgRowStatus
                  RowStatus
     }

docsIf3BondingGrpCfgDir OBJECT-TYPE
     SYNTAX      IfDirection
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This attribute defines the ordered list of channels
        that comprise the channel set"
     ::= { docsIf3BondingGrpCfgEntry 1 }

docsIf3BondingGrpCfgCfgId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..65535)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents the configured bonding group
        identifier in the indicated direction for the MAC Domain.
        This attribute is used for the sole purpose of tracking
        bonding groups defined by management systems."
     ::= { docsIf3BondingGrpCfgEntry 2 }

docsIf3BondingGrpCfgChList OBJECT-TYPE
     SYNTAX      ChannelList (SIZE (2..255))
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "This attribute contains the list of channels of the
        bonding group."
     ::= { docsIf3BondingGrpCfgEntry 3 }

docsIf3BondingGrpCfgSfProvAttrMask OBJECT-TYPE
     SYNTAX      AttributeMask
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "This attribute represents the Provisioned Attribute
        Mask encoding for the bonding group."
     DEFVAL { '80000000'H }
     ::= { docsIf3BondingGrpCfgEntry 4 }

docsIf3BondingGrpCfgDsidReseqWaitTime OBJECT-TYPE
     SYNTAX      Unsigned32 (0 | 1..180 | 255)
     UNITS       "hundredMicroseconds"
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "For a Downstream Bonding Group, this attribute provides
        the DSID Resequencing Wait Time that is to be used
        for all DSIDs associated with this Downstream Bonding
        Group.  The value of 255 indicates that the DSID
        Resequencing Wait Time is determined by the CMTS. The
        value zero in not supported for downstream  bonding
        groups.
        For an Upstream Bonding Group, this attribute has no
        meaning and returns the value 0."
     REFERENCE
        "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
        Specification CM-SP-MULPIv3.0-I08-080522, Service Flow
        Assignment section."
     DEFVAL { 255 }
     ::= { docsIf3BondingGrpCfgEntry 5 }

docsIf3BondingGrpCfgDsidReseqWarnThrshld OBJECT-TYPE
     SYNTAX      Unsigned32 (0..179 | 255)
     UNITS       "hundredMicroseconds"
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "For a Downstream Bonding Group, this attribute provides
        the DSID Resequencing Warning Threshold that
        is to be used for all DSIDs associated with this Downstream
        Bonding Group. The value of 255 indicates that
        the DSID Resequencing Warning Threshold is determined
        by the CMTS.  The value of 0 indicates that the threshold
        warnings are disabled.  When 
      the value of DsidReseqWaitTime is not equal to 0 or 255,
      the CMTS must ensure that the value of this object is either 
      255 or less than the value of DsidReseqWaitTime."
     DEFVAL { 255 }
     ::= { docsIf3BondingGrpCfgEntry 6 }

docsIf3BondingGrpCfgRowStatus OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "The status of this instance."
     ::= { docsIf3BondingGrpCfgEntry 7 }

docsIf3DsBondingGrpStatusTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3DsBondingGrpStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object returns administratively-configured
        and CMTS defined downstream bonding groups."
     ::= { docsIf3MibObjects 18}

docsIf3DsBondingGrpStatusEntry OBJECT-TYPE
     SYNTAX      DocsIf3DsBondingGrpStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3DsBondingGrpStatusTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the Bonding Group is configured."
     INDEX {
             ifIndex,
             docsIf3DsBondingGrpStatusChSetId
           }
     ::= { docsIf3DsBondingGrpStatusTable 1 }

DocsIf3DsBondingGrpStatusEntry ::= SEQUENCE {
     docsIf3DsBondingGrpStatusChSetId
                  ChSetId,
     docsIf3DsBondingGrpStatusMdDsSgId
                  Unsigned32,
     docsIf3DsBondingGrpStatusCfgId
                  Unsigned32
     }

docsIf3DsBondingGrpStatusChSetId OBJECT-TYPE
     SYNTAX      ChSetId
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents the identifier for the Downstream
        Bonding Group or the single-downstream channel
        of this instance."
     ::= { docsIf3DsBondingGrpStatusEntry 1 }

docsIf3DsBondingGrpStatusMdDsSgId OBJECT-TYPE
     SYNTAX      Unsigned32 (0..255)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute corresponds to the MD-DS-SG-ID that
        includes all the downstream channels of the Downstream
        Bonding Group. The value zero indicates that the
        bonding group does not contain channels from a single
        MD-DS-SG and therefore the bonding group is not valid
        and usable."
     ::= { docsIf3DsBondingGrpStatusEntry 2 }

docsIf3DsBondingGrpStatusCfgId OBJECT-TYPE
     SYNTAX      Unsigned32 (0..65535)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute provides the BondingGrpCfgId for
        the downstream bonding group if it was configured.
        Otherwise, the zero value indicates that the CMTS will
        define the bonding group."
     ::= { docsIf3DsBondingGrpStatusEntry 3 }

docsIf3UsBondingGrpStatusTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3UsBondingGrpStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object returns administratively-configured
        and CMTS-defined upstream bonding groups."
     ::= { docsIf3MibObjects 19}

docsIf3UsBondingGrpStatusEntry OBJECT-TYPE
     SYNTAX      DocsIf3UsBondingGrpStatusEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3UsBondingGrpStatusTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the Bonding Group is configured."
     INDEX {
             ifIndex,
             docsIf3UsBondingGrpStatusChSetId
           }
     ::= { docsIf3UsBondingGrpStatusTable 1 }

DocsIf3UsBondingGrpStatusEntry ::= SEQUENCE {
     docsIf3UsBondingGrpStatusChSetId
                  ChSetId,
     docsIf3UsBondingGrpStatusMdUsSgId
                  Unsigned32,
     docsIf3UsBondingGrpStatusCfgId
                  Unsigned32
     }

docsIf3UsBondingGrpStatusChSetId OBJECT-TYPE
     SYNTAX      ChSetId
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents the identifier for the Upstream
        Bonding Group or the single-upstream channel of this
        instance."
     ::= { docsIf3UsBondingGrpStatusEntry 1 }

docsIf3UsBondingGrpStatusMdUsSgId OBJECT-TYPE
     SYNTAX      Unsigned32 (0..255)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute corresponds to the MD-US-SG-ID that
        includes all the upstream channels of the Upstream
        Bonding Group. The value zero indicates that the bonding
        group does not contain channels from a single MD-US-SG
        and therefore the bonding group is not valid
        and usable."
     ::= { docsIf3UsBondingGrpStatusEntry 2 }

docsIf3UsBondingGrpStatusCfgId OBJECT-TYPE
     SYNTAX      Unsigned32 (0..65535)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute provides the BondingGrpCfgId for
        the upstream bonding group if it was configured.
        Otherwise, the zero value indicates that the CMTS
        defines the bonding group."
     ::= { docsIf3UsBondingGrpStatusEntry 3 }

docsIf3UsChExtTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3UsChExtEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object defines management extensions for upstream
        channels, in particular SCDMA parameters."
     ::= { docsIf3MibObjects 20}

docsIf3UsChExtEntry OBJECT-TYPE
     SYNTAX      DocsIf3UsChExtEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3UsChExtTable.
         The ifIndex key corresponds to each of the upstream
         channels."
     INDEX {
             ifIndex
           }
     ::= { docsIf3UsChExtTable 1 }

DocsIf3UsChExtEntry ::= SEQUENCE {
     docsIf3UsChExtSacCodeHoppingSelectionMode
                  INTEGER,
     docsIf3UsChExtScdmaSelectionStringActiveCodes
                  ScdmaSelectionString
     }

docsIf3UsChExtSacCodeHoppingSelectionMode OBJECT-TYPE
     SYNTAX      INTEGER {
                           none(0),
                           sac1NoCodeHopping(1),
                           sac1CodeHoppingMode1(2),
                           sac2CodeHoppingMode2(3),
                           sac2NoCodeHopping(4)
                         }
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute indicates the selection mode for active
        codes and code hopping.
        'none'
           Non-SCDMA channel
        'sac1NoCodeHopping'
           Selectable active codes mode 1 and code hopping disabled

        'sac1CodeHoppingMode1'
           Selectable active codes mode 1 and code hopping mode
        1
        'sac2CodeHoppingMode2'
          Selectable active codes mode 2 and code hopping mode
        2
        'sac2NoCodeHopping'
          Selectable active codes mode 2 and code hopping disabled."
     REFERENCE
         "DOCSIS 3.0 Physical Layer Specification
         CM-SP-PHYv3.0-I05-070803, Mini-slot Numbering
         Parameters in UCD section."
     ::= { docsIf3UsChExtEntry 1 }

docsIf3UsChExtScdmaSelectionStringActiveCodes OBJECT-TYPE
     SYNTAX      ScdmaSelectionString
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the active codes of the
        upstream channel and it is applicable only when
        SacCodeHoppingSelectionMode is 'sac2CodeHoppingMode2."
     REFERENCE
         "DOCSIS 3.0 Physical Layer Specification
         CM-SP-PHYv3.0-I05-070803, Mini-slot Numbering
         Parameters in UCD section."
     ::= { docsIf3UsChExtEntry 2 }

docsIf3CmCapabilities OBJECT IDENTIFIER ::= { docsIf3MibObjects 21 }

docsIf3CmCapabilitiesReq OBJECT-TYPE
     SYNTAX      Tlv8
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute contains the TLV encoding for TLV-5
        sent in a REG-REQ.  The first byte of this encoding is
        expected to be '05'H."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Modem Capabilities
         Encoding section in the Common Radio Frequency Interface
         Encodings Annex."
     ::= { docsIf3CmCapabilities 1 }

docsIf3CmCapabilitiesRsp OBJECT-TYPE
     SYNTAX      Tlv8
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute contains the TLV encoding for TLV-5
        received in a REG-RSP.
        The first byte of this encoding is expected to be '05'H."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Modem Capabilities
         Encoding section in the Common Radio Frequency Interface
         Encodings Annex."
     ::= { docsIf3CmCapabilities 2 }

docsIf3UsChSetTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3UsChSetEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object defines a set of upstream channels. These
        channel sets may be associated with channel bonding
        groups, MD-US-SGs, MD-CM-SGs, or any other channel
        set that the CMTS may derive from other CMTS processes."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Partial
         Service Encoding section and Cable Modem Attribute
         Masks section in the Common Radio Frequency Interface
         Encodings Annex."
     ::= { docsIf3MibObjects 22}

docsIf3UsChSetEntry OBJECT-TYPE
     SYNTAX      DocsIf3UsChSetEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3UsChSetTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the upstream channel set is defined."
     INDEX {
             ifIndex,
             docsIf3UsChSetId
           }
     ::= { docsIf3UsChSetTable 1 }

DocsIf3UsChSetEntry ::= SEQUENCE {
     docsIf3UsChSetId
                  ChSetId,
     docsIf3UsChSetChList
                  ChannelList
     }

docsIf3UsChSetId OBJECT-TYPE
     SYNTAX      ChSetId
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key defines a reference identifier for the upstream
        channel set within the MAC Domain."
     ::= { docsIf3UsChSetEntry 1 }

docsIf3UsChSetChList OBJECT-TYPE
     SYNTAX      ChannelList (SIZE (0 | 2..255))
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute defines the ordered list of channels
        that comprise the upstream channel set"
     ::= { docsIf3UsChSetEntry 2 }

docsIf3DsChSetTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3DsChSetEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object defines a set of downstream channels.
        These channel sets may be associated with channel bonding
        groups, MD-DS-SGs, MD-CM-SGs, or any other channel
        set that the CMTS may derive from other CMTS processes."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, Partial
         Service Encoding section and Cable Modem Attribute
         Masks section in the Common Radio Frequency Interface
         Encodings Annex."
     ::= { docsIf3MibObjects 23}

docsIf3DsChSetEntry OBJECT-TYPE
     SYNTAX      DocsIf3DsChSetEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3DsChSetTable.
         The ifIndex key corresponds to the MAC Domain interface
         where the downstream channel set is defined."
     INDEX {
             ifIndex,
             docsIf3DsChSetId
           }
     ::= { docsIf3DsChSetTable 1 }

DocsIf3DsChSetEntry ::= SEQUENCE {
     docsIf3DsChSetId
                  ChSetId,
     docsIf3DsChSetChList
                  ChannelList
     }

docsIf3DsChSetId OBJECT-TYPE
     SYNTAX      ChSetId
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key defines a reference identifier for the downstream
        channel set within the MAC Domain."
     ::= { docsIf3DsChSetEntry 1 }

docsIf3DsChSetChList OBJECT-TYPE
     SYNTAX      ChannelList (SIZE (0 | 2..255))
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute defines the ordered list of channels
        that comprise the downstream channel set."
     ::= { docsIf3DsChSetEntry 2 }

docsIf3SignalQualityExtTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3SignalQualityExtEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object provides an in-channel received modulation
        error ratio metric for CM and CMTS."
     ::= { docsIf3MibObjects 24}

docsIf3SignalQualityExtEntry OBJECT-TYPE
     SYNTAX      DocsIf3SignalQualityExtEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3SignalQualityExtTable.
         The ifIndex key corresponds to each of the upstream
         channels."
     INDEX {
             ifIndex
           }
     ::= { docsIf3SignalQualityExtTable 1 }

DocsIf3SignalQualityExtEntry ::= SEQUENCE {
     docsIf3SignalQualityExtRxMER
                  TenthdB,
     docsIf3SignalQualityExtRxMerSamples
                  Unsigned32
     }

docsIf3SignalQualityExtRxMER OBJECT-TYPE
     SYNTAX      TenthdB (-2147483648..2147483647)
    UNITS     "TenthdB"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "RxMER provides an in-channel received Modulation
        Error Ratio (MER). RxMER is defined as an estimate,
        provided by the demodulator, of the ratio:
        (average constellation energy with equally likely
        symbols) / (average squared magnitude of error vector)

        RxMER is measured just prior to FEC (trellis/Reed-Solomon)
        decoding. RxMER includes the effects of the
        HFC channel as well as implementation effects of the
        modulator and demodulator. Error vector estimation
        may vary among demodulator implementations.  The CMTS
        RxMER is averaged over a given number of bursts at
        the burst receiver, which may correspond to transmissions
        from multiple users. In the case of S-CDMA mode,
        RxMER is measured on the de-spread signal."
     ::= { docsIf3SignalQualityExtEntry 1 }

docsIf3SignalQualityExtRxMerSamples OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "RxMerSamples is a statistically significant number
        of symbols for the CM, or bursts for the CMTS, processed
        to arrive at the RxMER value. For the CMTS, the MER
        measurement includes only valid bursts that are not
        in contention regions."
     ::= { docsIf3SignalQualityExtEntry 2 }

docsIf3CmtsSignalQualityExtTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3CmtsSignalQualityExtEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object provides metrics and parameters associated
        with received carrier, noise and interference
        power levels in the upstream channels of the CMTS."
     ::= { docsIf3MibObjects 25}

docsIf3CmtsSignalQualityExtEntry OBJECT-TYPE
     SYNTAX      DocsIf3CmtsSignalQualityExtEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3CmtsSignalQualityExtTable.
         The ifIndex key corresponds to each of the upstream
         channels.
         The CMTS persists the configured values of all instances of
         CmtsSignalQualityExt across reinitialization."
     INDEX {
             ifIndex
           }
     ::= { docsIf3CmtsSignalQualityExtTable 1 }

DocsIf3CmtsSignalQualityExtEntry ::= SEQUENCE {
     docsIf3CmtsSignalQualityExtCNIR
                  TenthdB,
     docsIf3CmtsSignalQualityExtExpectedRxSignalPower
                  TenthdBmV
     }

docsIf3CmtsSignalQualityExtCNIR OBJECT-TYPE
     SYNTAX      TenthdB
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute provides an upstream in-channel Carrier-to-Noise
        plus Interference Ratio (CNIR). CNIR
        is defined as the ratio of the expected commanded
        received signal power at the CMTS input, assuming
        QPSK0 modulation, to the noise plus
        interference in the channel.
        This measurement occurs prior to the point at which 
        the desired CM signal, when present, is demodulated.
        The measurement includes the effect of the receive matched
        filter but does not include the effect of any ingress filtering.
        Both the signal power and noise/interference power
        are referenced to the same point, e.g., CMTS input."
     ::= { docsIf3CmtsSignalQualityExtEntry 1 }

docsIf3CmtsSignalQualityExtExpectedRxSignalPower OBJECT-TYPE
     SYNTAX      TenthdBmV
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "ExpectedReceivedSignalPower is the power of the
        expected commanded received signal in the channel,
        referenced to the CMTS input."
     ::= { docsIf3CmtsSignalQualityExtEntry 2 }

docsIf3CmtsSpectrumAnalysisMeasTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3CmtsSpectrumAnalysisMeasEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object is used to configure the logical upstream
        interfaces to perform the spectrum measurements.
        This object supports creation and deletion of instances."
     ::= { docsIf3MibObjects 26}

docsIf3CmtsSpectrumAnalysisMeasEntry OBJECT-TYPE
     SYNTAX      DocsIf3CmtsSpectrumAnalysisMeasEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3CmtsSpectrumAnalysisMeasTable.
         The ifIndex key corresponds to each of the upstream
         channels.
         The CMTS is not required to persist instances of this
         object across reinitializations."
     INDEX {
             ifIndex
           }
     ::= { docsIf3CmtsSpectrumAnalysisMeasTable 1 }

DocsIf3CmtsSpectrumAnalysisMeasEntry ::= SEQUENCE {
     docsIf3CmtsSpectrumAnalysisMeasAmplitudeData
                  AmplitudeData,
     docsIf3CmtsSpectrumAnalysisMeasTimeInterval
                  Unsigned32,
     docsIf3CmtsSpectrumAnalysisMeasRowStatus
                  RowStatus
     }

docsIf3CmtsSpectrumAnalysisMeasAmplitudeData OBJECT-TYPE
     SYNTAX      AmplitudeData
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute provides a list of the spectral amplitudes
        corresponding to the frequency bins ordered
        from lowest to highest frequencies covering the frequency
        span. Information about the center frequency,
        frequency span, number of bins and resolution bandwidth
        are included to provide context to the measurement
        point
        The CMTS must support the number of bins as an odd number
        in order to provide a spectrum representation that
        is symmetric about the middle data point or bin. The
        CMTS must support a number of bins greater than or equal
        to 257 for frequency spans greater than or equal to
        6.4 MHz.

        The CMTS must not exceed 25 kHz bin spacing for measurement
        of frequency spans less than or equal to 6.4 MHz.

        The bins measurements are updated periodically at time
        intervals given by the TimeInterval attribute."
     ::= { docsIf3CmtsSpectrumAnalysisMeasEntry 1 }

docsIf3CmtsSpectrumAnalysisMeasTimeInterval OBJECT-TYPE
     SYNTAX      Unsigned32
     UNITS       "milliseconds"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "TimeInterval is the CMTS estimated average repetition
        period of measurements. This attribute defines
        the average rate at which new spectra can be retrieved."
     ::= { docsIf3CmtsSpectrumAnalysisMeasEntry 2 }

docsIf3CmtsSpectrumAnalysisMeasRowStatus OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "The status of this instance."
     ::= { docsIf3CmtsSpectrumAnalysisMeasEntry 3 }

docsIf3CmtsCmCtrl OBJECT IDENTIFIER ::= { docsIf3MibObjects 27 }

docsIf3CmtsCmCtrlCmdMacAddr OBJECT-TYPE
     SYNTAX      MacAddress
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "This attribute represents the MAC Address of the CM which the 
        CMTS is instructed to send the CM-CTRL-REQ message."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522,
         Media Access Control Specification section."
     DEFVAL { '000000000000'H }
     ::= { docsIf3CmtsCmCtrl 1 }  
     
docsIf3CmtsCmCtrlCmdMuteUsChId OBJECT-TYPE
     SYNTAX      ChId
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "This attribute represents the Upstream Channel ID (UCID) to 
        mute or unmute.  A value of zero indicates all upstream 
        channels.  This attribute is only applicable when the 
        docsIf3CmtsCmCtrlCmdCommit attribute is set to 
        'mute'."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, 
         Media Access Control Specification section."
     DEFVAL { 0 }
     ::= { docsIf3CmtsCmCtrl 2 }    
     
docsIf3CmtsCmCtrlCmdMuteInterval OBJECT-TYPE
     SYNTAX      Unsigned32  
     UNITS       "milliseconds"
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "This attribute represents the length of time that the mute 
        operation is in effect.  This attribute is only applicable 
        when the docsIf3CmtsCmCtrlCmdCommit attribute is set to 
        'mute'.  A value of 0 is an indication to unmute the
        channel referenced by the docsIf3CmtsCmCtrlCmdMuteUsChId
        attribute while a value of 0xFFFFFFFF is used to mute
        the channel referenced by the docsIf3CmtsCmCtrlCmdMuteUsChId
        attribute indefinitely."
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, 
         Media Access Control Specification section."
     DEFVAL { 1 }
     ::= { docsIf3CmtsCmCtrl 3 }  
     
docsIf3CmtsCmCtrlCmdDisableForwarding OBJECT-TYPE
     SYNTAX      TruthValue 
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "When set to 'true', this attribute disables data forwarding 
        to the CMCI when the docsIf3CmtsCmCtrlCmdCommit attribute is
        set to 'disableForwarding'. 
        When set to 'false', this attribute enables data forwarding
        to the CMCI when the docsIf3CmtsCmCtrlCmdCommit attribute is
        set to 'disableForwarding'. 
        This attribute is only applicable when the 
        docsIf3CmtsCmCtrlCmdCommit attribute is set to 
        'disableForwarding'." 
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, 
         Media Access Control Specification section."   
     DEFVAL { false }
     ::= { docsIf3CmtsCmCtrl 4 }

docsIf3CmtsCmCtrlCmdCommit OBJECT-TYPE
     SYNTAX      INTEGER {
                         mute(1),
                         cmReinit(2),
                         disableForwarding(3) }
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "This attribute indicates the type of command for the 
        CMTS to trigger in the CM-CTRL-REQ message.
        This attribute will return the value of the last operation 
        performed or the default value if no operation has been 
        performed."  
     REFERENCE
         "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, 
         Media Access Control Specification section."   
     DEFVAL { mute }
     ::= { docsIf3CmtsCmCtrl 5 }       
     
docsIf3CmDpvStatsTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3CmDpvStatsEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object represents the DOCSIS Path Verify Statistics
        collected in the cable modem device.
        The CMTS controls the logging of DPV statistics in the
        cable modem. Therefore the context and nature of the
        measurements are governed by the CMTS and not self-descriptive
        when read from the CM."
     ::= { docsIf3MibObjects 28}

docsIf3CmDpvStatsEntry OBJECT-TYPE
     SYNTAX      DocsIf3CmDpvStatsEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3CmDpvStatsTable."
     INDEX { 
             ifIndex,
             docsIf3CmDpvStatsGrpId
           }
     ::= { docsIf3CmDpvStatsTable 1 }

DocsIf3CmDpvStatsEntry ::= SEQUENCE {
     docsIf3CmDpvStatsGrpId
                  Unsigned32,
     docsIf3CmDpvStatsLastMeasLatency
                  Unsigned32,
     docsIf3CmDpvStatsLastMeasTime
                  DateAndTime,
     docsIf3CmDpvStatsMinLatency
                  Unsigned32,
     docsIf3CmDpvStatsMaxLatency
                  Unsigned32,
     docsIf3CmDpvStatsAvgLatency
                  Unsigned32,
     docsIf3CmDpvStatsNumMeas
                  Unsigned32,
     docsIf3CmDpvStatsLastClearTime
                  DateAndTime
     }

docsIf3CmDpvStatsGrpId OBJECT-TYPE
     SYNTAX      Unsigned32 (1..2)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents the DPV Group ID. The CM reports
        two instance of DPV statistics per downstream normally
        referred as Statistical Group 1 and Statistical
        Group 2."
     ::= { docsIf3CmDpvStatsEntry 1 }

docsIf3CmDpvStatsLastMeasLatency OBJECT-TYPE
     SYNTAX      Unsigned32
     UNITS       "nanoseconds"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attrtibute represents the last latency measurement
        for this statistical group."
     ::= { docsIf3CmDpvStatsEntry 2 }

docsIf3CmDpvStatsLastMeasTime OBJECT-TYPE
     SYNTAX      DateAndTime
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the last measurement time
        of the last latency measurement for this statistical
        group.
        This attribute reports the EPOC time value when no measurements
        are being reported or after the statistics
        were cleared."
     ::= { docsIf3CmDpvStatsEntry 3 }

docsIf3CmDpvStatsMinLatency OBJECT-TYPE
     SYNTAX      Unsigned32
     UNITS       "nanoseconds"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the minimum latency measurement
        for this statistical group since the last
        time statistics were cleared."
     ::= { docsIf3CmDpvStatsEntry 4 }

docsIf3CmDpvStatsMaxLatency OBJECT-TYPE
     SYNTAX      Unsigned32
     UNITS       "nanoseconds"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the maximum latency measurement
        for this statistical group since the last
        time statistics were cleared."
     ::= { docsIf3CmDpvStatsEntry 5 }

docsIf3CmDpvStatsAvgLatency OBJECT-TYPE
     SYNTAX      Unsigned32
     UNITS       "nanoseconds"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the average latency measurement
        for this statistical group since the last
        time statistics were cleared. The averaging mechanism
        is controlled by the CMTS, and can be a simple average
        (mean) or an exponential moving average."
     REFERENCE
        "DOCSIS 3.0 MAC and Upper Layer Protocols Interface
         Specification CM-SP-MULPIv3.0-I08-080522, DOCSIS Path 
         Verification section."
     ::= { docsIf3CmDpvStatsEntry 6 }

docsIf3CmDpvStatsNumMeas OBJECT-TYPE
     SYNTAX      Unsigned32
     UNITS       "measurements"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribure represents the number of latency measurements
        made for this statistical group since the
        last time statistics were cleared."
     ::= { docsIf3CmDpvStatsEntry 7 }

docsIf3CmDpvStatsLastClearTime OBJECT-TYPE
     SYNTAX      DateAndTime
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "This attribute represents the last time statistics
        were cleared for this statistical group."
     ::= { docsIf3CmDpvStatsEntry 8 }

docsIf3CmEventCtrlTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3CmEventCtrlEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object represents the control mechanism to enable the
        dispatching of  events based on the event Id. The following
        rules define the event control behavior:
        
        o	The CmEventCtrl object has no instances 
          Events are sent to Local Log depending on the settings of the
          docsDevEvReporting object. Settings in the DocsDevEvReporting
          for other dispatch mechanisms are treated as disable.

        o	The CmEventCtrl object contains configured instances
          Only events matching the Event Ids configured in the object
          are sent according to the settings of the docsDevEvReporting
          object. 
          
        o The CmEventCtrl object contains an instance with Event Id 0 
          All events matching the Local Log settings of 
          docsDevEvReporting are sent to local log. Events matching 
          the Event Ids configured in the docsDevEvReporting and 
          CmEventCtrl objects are delivered to dispatch mechanisms
          other than Local Log.

          The CM does not persist instances of CmEventCtrl across 
          reinitializations."
     ::= { docsIf3MibObjects 29}

docsIf3CmEventCtrlEntry OBJECT-TYPE
     SYNTAX      DocsIf3CmEventCtrlEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3CmEventCtrlTable."
     INDEX { 
             docsIf3CmEventCtrlEventId
           }
     ::= { docsIf3CmEventCtrlTable 1 }

DocsIf3CmEventCtrlEntry ::= SEQUENCE {
             docsIf3CmEventCtrlEventId
                  Unsigned32,
             docsIf3CmEventCtrlStatus
                  RowStatus
     }

docsIf3CmEventCtrlEventId OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents the Event ID of the event being 
        enabled for delivery to a dispatch mechanism (e.g. syslog)."
     REFERENCE
        "DOCSIS 3.0 Operations Support System Interface
         Specification CM-SP-OSSIv3.0-I07-080522, Format and Content
         for Event, Syslog, and SNMP Notification Annex."
     ::= { docsIf3CmEventCtrlEntry  1 }
     
docsIf3CmEventCtrlStatus OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "The status of this instance."
     ::= { docsIf3CmEventCtrlEntry  2 }     

docsIf3CmtsEventCtrlTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF DocsIf3CmtsEventCtrlEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This object represents the control mechanism to enable the
        dispatching of  events based on the event Id. The following
        rules define the event control behavior:
        
        o	The CmtsEventCtrl object has no instances 
          Events are sent to Local Log depending on the settings of the
          docsDevEvReporting object. Settings in the DocsDevEvReporting
          for other dispatch mechanisms are treated as disable.

        o	The CmtsEventCtrl object contains configured instances
          Only events matching the Event Ids configured in the object
          are sent according to the settings of the docsDevEvReporting
          object. 
          
        o The CmtsEventCtrl object contains an instance with Event Id 0 
          All events matching the Local Log settings of 
          docsDevEvReporting are sent to local log. Events matching 
          the Event Ids configured in the docsDevEvReporting and 
          CmtsEventCtrl objects are delivered to dispatch mechanisms
          other than Local Log. 

          The CMTS persists all instances of CmtsEventCtrl across 
          reinitializations."
     ::= { docsIf3MibObjects 30}

docsIf3CmtsEventCtrlEntry OBJECT-TYPE
     SYNTAX      DocsIf3CmtsEventCtrlEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
         "The conceptual row of docsIf3CmtsEventCtrlTable."
     INDEX { 
             docsIf3CmtsEventCtrlEventId
           }
     ::= { docsIf3CmtsEventCtrlTable 1 }

DocsIf3CmtsEventCtrlEntry ::= SEQUENCE {
             docsIf3CmtsEventCtrlEventId
                  Unsigned32,
             docsIf3CmtsEventCtrlStatus
                  RowStatus
     }

docsIf3CmtsEventCtrlEventId OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
        "This key represents the Event ID of the event being 
        enabled for delivery to a dispatch mechanism (e.g. syslog)."
     REFERENCE
        "DOCSIS 3.0 Operations Support System Interface
         Specification CM-SP-OSSIv3.0-I07-080522, Format and Content
         for Event, Syslog, and SNMP Notification Annex."
     ::= { docsIf3CmtsEventCtrlEntry  1 }
     
docsIf3CmtsEventCtrlStatus OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
        "The status of this instance."
     ::= { docsIf3CmtsEventCtrlEntry  2 }     

     
-- Conformance Definitions
docsIf3MibConformance OBJECT IDENTIFIER ::= { docsIf3Mib 2 }
docsIf3MibCompliances OBJECT IDENTIFIER ::= { docsIf3MibConformance 1 }
docsIf3MibGroups      OBJECT IDENTIFIER ::= { docsIf3MibConformance 2 }

docsIf3CmtsCompliance MODULE-COMPLIANCE
STATUS      current
DESCRIPTION
        "The compliance statement for the CMTS."

    MODULE -- this MODULE
MANDATORY-GROUPS {
     docsIf3CmtsGroup,
     docsIf3CmtsNotificationGroup
     }
OBJECT docsIf3CmtsCmUsStatusRangingStatus
     SYNTAX      INTEGER {other(1),
                          aborted(2),
                          retriesExceeded(3),
                          success(4),
                          continue(5)
                         }
     DESCRIPTION
        "The CMTS does not report 'timeoutT4'."

::= { docsIf3MibCompliances 1 }

docsIf3CmCompliance MODULE-COMPLIANCE
STATUS      current
DESCRIPTION
        "The compliance statement for the CM."

    MODULE -- this MODULE
MANDATORY-GROUPS {
     docsIf3CmGroup,
     docsIf3CmNotificationGroup
     }
::= { docsIf3MibCompliances 2 }

docsIf3CmtsGroup OBJECT-GROUP
    OBJECTS {
     docsIf3SignalQualityExtRxMER,
     docsIf3SignalQualityExtRxMerSamples,
     docsIf3MdNodeStatusMdDsSgId,
     docsIf3MdNodeStatusMdUsSgId,
     docsIf3MdDsSgStatusChSetId,
     docsIf3MdUsSgStatusChSetId,
     docsIf3CmtsSignalQualityExtCNIR,
     docsIf3CmtsSignalQualityExtExpectedRxSignalPower,
     docsIf3CmtsSpectrumAnalysisMeasAmplitudeData,
     docsIf3CmtsSpectrumAnalysisMeasTimeInterval,
     docsIf3CmtsSpectrumAnalysisMeasRowStatus,
     docsIf3CmtsCmRegStatusMacAddr,
     docsIf3CmtsCmRegStatusIPv6Addr,
     docsIf3CmtsCmRegStatusIPv6LinkLocal,
     docsIf3CmtsCmRegStatusIPv4Addr,
     docsIf3CmtsCmRegStatusValue,
     docsIf3CmtsCmRegStatusMdIfIndex,
     docsIf3CmtsCmRegStatusMdCmSgId,
     docsIf3CmtsCmRegStatusRcpId,
     docsIf3CmtsCmRegStatusRccStatusId,
     docsIf3CmtsCmRegStatusRcsId,
     docsIf3CmtsCmRegStatusTcsId,
     docsIf3CmtsCmRegStatusQosVersion,
     docsIf3CmtsCmRegStatusLastRegTime,
     docsIf3CmtsCmRegStatusAddrResolutionReqs,
     docsIf3CmtsCmUsStatusModulationType,
     docsIf3CmtsCmUsStatusRxPower,
     docsIf3CmtsCmUsStatusSignalNoise,
     docsIf3CmtsCmUsStatusMicroreflections,
     docsIf3CmtsCmUsStatusEqData,
     docsIf3CmtsCmUsStatusUnerroreds,
     docsIf3CmtsCmUsStatusCorrecteds,
     docsIf3CmtsCmUsStatusUncorrectables,
     docsIf3CmtsCmUsStatusHighResolutionTimingOffset,
     docsIf3CmtsCmUsStatusIsMuted,
     docsIf3CmtsCmUsStatusRangingStatus,
     docsIf3UsChExtSacCodeHoppingSelectionMode,
     docsIf3UsChExtScdmaSelectionStringActiveCodes,
     docsIf3MdCfgMddInterval,
     docsIf3MdCfgIpProvMode,
     docsIf3MdCfgCmStatusEvCtlEnabled,
     docsIf3MdCfgUsFreqRange,
     docsIf3MdCfgMcastDsidFwdEnabled,
     docsIf3MdCfgMultRxChModeEnabled,
     docsIf3MdCfgMultTxChModeEnabled,
     docsIf3MdCfgEarlyAuthEncrCtrl,
     docsIf3MdCfgTftpProxyEnabled,
     docsIf3MdCfgSrcAddrVerifEnabled,
     docsIf3MdCfgDownChannelAnnex,
     docsIf3MdCfgCmUdcEnabled,
     docsIf3MdCfgSendUdcRulesEnabled,
     docsIf3MdCfgServiceTypeIdList,
     docsIf3MdChCfgIsPriCapableDs,
     docsIf3MdChCfgChId,
     docsIf3MdChCfgSfProvAttrMask,
     docsIf3MdChCfgRowStatus,
     docsIf3MdUsToDsChMappingMdIfIndex,
     docsIf3DsChSetChList,
     docsIf3UsChSetChList,
     docsIf3BondingGrpCfgChList,
     docsIf3BondingGrpCfgSfProvAttrMask,
     docsIf3BondingGrpCfgDsidReseqWaitTime,
     docsIf3BondingGrpCfgDsidReseqWarnThrshld,
     docsIf3BondingGrpCfgRowStatus,
     docsIf3DsBondingGrpStatusMdDsSgId,
     docsIf3DsBondingGrpStatusCfgId,
     docsIf3UsBondingGrpStatusMdUsSgId,
     docsIf3UsBondingGrpStatusCfgId,
     docsIf3RccCfgVendorSpecific,
     docsIf3RccCfgDescription,
     docsIf3RccCfgRowStatus,
     docsIf3RxChCfgChIfIndex,
     docsIf3RxChCfgPrimaryDsIndicator,
     docsIf3RxChCfgRcRmConnectivityId,
     docsIf3RxChCfgRowStatus,
     docsIf3RxModuleCfgRmRmConnectivityId,
     docsIf3RxModuleCfgFirstCenterFrequency,
     docsIf3RxModuleCfgRowStatus,
     docsIf3RccStatusRccCfgId,
     docsIf3RccStatusValidityCode,
     docsIf3RccStatusValidityCodeText,
     docsIf3RxChStatusChIfIndex,
     docsIf3RxChStatusPrimaryDsIndicator,
     docsIf3RxChStatusRcRmConnectivityId,
     docsIf3RxModuleStatusRmRmConnectivityId,
     docsIf3RxModuleStatusFirstCenterFrequency,
     docsIf3CmtsCmCtrlCmdMacAddr,
     docsIf3CmtsCmCtrlCmdMuteUsChId,
     docsIf3CmtsCmCtrlCmdMuteInterval,
     docsIf3CmtsCmCtrlCmdDisableForwarding,
     docsIf3CmtsCmCtrlCmdCommit,
     docsIf3CmtsEventCtrlStatus
     }
    STATUS      current
    DESCRIPTION
         "Group of objects implemented in the CMTS"
    ::= { docsIf3MibGroups 1 }

docsIf3CmGroup OBJECT-GROUP
    OBJECTS {
     docsIf3SignalQualityExtRxMER,
     docsIf3SignalQualityExtRxMerSamples,
     docsIf3CmStatusValue,
     docsIf3CmStatusCode,
     docsIf3CmStatusResets,
     docsIf3CmStatusLostSyncs,
     docsIf3CmStatusInvalidMaps,
     docsIf3CmStatusInvalidUcds,
     docsIf3CmStatusInvalidRangingRsps,
     docsIf3CmStatusInvalidRegRsps,
     docsIf3CmStatusT1Timeouts,
     docsIf3CmStatusT2Timeouts,
     docsIf3CmStatusUCCsSuccesses,
     docsIf3CmStatusUCCFails,
     docsIf3CmStatusUsTxPower,
     docsIf3CmStatusUsT3Timeouts,
     docsIf3CmStatusUsT4Timeouts,
     docsIf3CmStatusUsRangingAborteds,
     docsIf3CmStatusUsModulationType,
     docsIf3CmStatusUsEqData,
     docsIf3CmStatusUsT3Exceededs,
     docsIf3CmStatusUsIsMuted,
     docsIf3CmStatusUsRangingStatus,
     docsIf3CmCapabilitiesReq,
     docsIf3CmCapabilitiesRsp,
     docsIf3UsChExtSacCodeHoppingSelectionMode,
     docsIf3UsChExtScdmaSelectionStringActiveCodes,
     docsIf3RxChStatusChIfIndex,
     docsIf3RxChStatusPrimaryDsIndicator,
     docsIf3RxChStatusRcRmConnectivityId,
     docsIf3RxModuleStatusRmRmConnectivityId,
     docsIf3RxModuleStatusFirstCenterFrequency,
     docsIf3CmDpvStatsLastMeasLatency,
     docsIf3CmDpvStatsLastMeasTime,
     docsIf3CmDpvStatsMinLatency,
     docsIf3CmDpvStatsMaxLatency,
     docsIf3CmDpvStatsAvgLatency,
     docsIf3CmDpvStatsNumMeas,
     docsIf3CmDpvStatsLastClearTime,
     docsIf3CmEventCtrlStatus
     }
    STATUS      current
    DESCRIPTION
         "Group of objects implemented in the CM"
    ::= { docsIf3MibGroups 2 }

docsIf3CmtsNotificationGroup NOTIFICATION-GROUP
        NOTIFICATIONS {
            docsIf3CmtsEventNotif
            }
        STATUS    current
        DESCRIPTION
            "CMTS is required to support notifications in this group"
        ::= { docsIf3MibGroups 3 }

docsIf3CmNotificationGroup NOTIFICATION-GROUP
        NOTIFICATIONS {
            docsIf3CmEventNotif
            }
        STATUS    current
        DESCRIPTION
            "CM is required to support notifications in this group"
        ::= { docsIf3MibGroups 4 }

END


