T11-TC-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, Unsigned32, mib-2
                                     FROM SNMPv2-SMI  -- [RFC2578]
    TEXTUAL-CONVENTION               FROM SNMPv2-TC;  -- [RFC2579]

t11TcMIB MODULE-IDENTITY
    LAST-UPDATED "200603020000Z"
    ORGANIZATION "T11"
    CONTACT-INFO
            "     Claudio DeSanti
                  Cisco Systems, Inc.
                  170 West Tasman Drive
                  San Jose, CA 95134 USA
                  Phone: +1 408 853-9172
                  EMail: cds@cisco.com

                  Keith McCloghrie
                  Cisco Systems, Inc.
                  170 West Tasman Drive
                  San Jose, CA USA 95134
                  Phone: +1 408-526-5260
                  EMail: kzm@cisco.com"
    DESCRIPTION
           "This module defines textual conventions used in T11 MIBs.

           Copyright (C) The Internet Society (2006).  This version
           of this MIB module is part of RFC 4439;  see the RFC
           itself for full legal notices."
    REVISION    "200603020000Z"
    DESCRIPTION
           "Initial version of this MIB module, published as RFC 4439."
    ::= { mib-2 136 }

T11FabricIndex ::= TEXTUAL-CONVENTION
    DISPLAY-HINT  "d"
    STATUS    current
    DESCRIPTION
           "A Fabric Index that is used as a unique
           index value to identify a particular Fabric within
           one (or more) physical infrastructures.

           In an environment that is conformant to FC-SW-3, where

           there is always exactly one Fabric in a single physical
           infrastructure, the value of this Fabric Index will
           always be 1.

           However, the current standard, FC-SW-4, defines
           how multiple Fabrics, each with its own management
           instrumentation, could operate within one (or more)
           physical infrastructures.  When such multiple Fabrics
           are in use, this index value is used to uniquely
           identify a particular Fabric within a physical
           infrastructure.

           Note that the value of this textual convention has a
           range of (0..4095) so as to be consistent with FC-SW-4,
           which says that a 'VF_ID Bitmap' is 512 bytes long, with
           the high-order bit representing VF_ID zero, and the
           low-order bit representing 4095."
    REFERENCE   "Fibre Channel - Switch Fabric - 4 (FC-SW-4),
                 ANSI INCITS 418-2006, section 6.1.27.2.4."
    SYNTAX      Unsigned32 (0..4095)

END



