-- *******************************************************************
-- CISCO-LWAPP-CCX-RM-MIB.my:
-- Light Weight Access Point Wireless client CCX Radio Measurement
-- MIB
-- December 2005, Devesh Pujari, Bharat Biswal, Prasanna Viswakumar
--   
-- Copyright (c) 2005, 2006, 2012 by Cisco Systems Inc.
-- All rights reserved.
-- *******************************************************************

CISCO-LWAPP-CCX-RM-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Integer32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    MacAddress,
    TruthValue,
    TimeInterval,
    TimeStamp
        FROM SNMPv2-TC
    cLWlanConfigEntry
        FROM CISCO-LWAPP-WLAN-MIB
    cLApDot11IfEntry,
    cLApSysMacAddress,
    cLApDot11IfSlotId
        FROM CISCO-LWAPP-AP-MIB
    ciscoMgmt
        FROM CISCO-SMI;


-- ********************************************************************
-- *  MODULE IDENTITY
-- ********************************************************************

ciscoLwappCcxRmMIB MODULE-IDENTITY
    LAST-UPDATED    "201202210000Z"
    ORGANIZATION    "Cisco Systems Inc."
    CONTACT-INFO
            "Cisco Systems,
            Customer Service
            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA
            Tel: +1 800 553-NETS

            Email: cs-aironet@cisco.com"
    DESCRIPTION
        "This MIB is intended to be implemented on all those
        devices operating as Central controllers, that
        terminate the Light Weight Access Point Protocol
        tunnel from Cisco Light-weight LWAPP Access Points.

        Information provided by this MIB is for CCX related 
        features as specified in the CCX specifications. 

        The relationship between CC and the LWAPP APs
        can be depicted as follows:

        +......+     +......+     +......+           +......+
        +      +     +      +     +      +           +      +
        +  CC  +     +  CC  +     +  CC  +           +  CC  +
        +      +     +      +     +      +           +      +
        +......+     +......+     +......+           +......+
        ..            .             .                 .
        ..            .             .                 .
        .  .            .             .                 .
        .    .            .             .                 .
        .      .            .             .                 .
        .        .            .             .                 .
        +......+ +......+     +......+      +......+          +......+
        +      + +      +     +      +      +      +          +      +
        +  AP  + +  AP  +     +  AP  +      +  AP  +          +  AP  +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+
        .              .             .                 .
        .  .              .             .                 .
        .    .              .             .                 .
        .      .              .             .                 .
        .        .              .             .                 .
        +......+ +......+     +......+      +......+          +......+
        +      + +      +     +      +      +      +          +      +
        +  MN  + +  MN  +     +  MN  +      +  MN  +          +  MN  +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+


        The LWAPP tunnel exists between the controller and
        the APs.  The MNs communicate with the APs through
        the protocol defined by the 802.11 standard.

        LWAPP APs, upon bootup, discover and join one of the
        controllers and the controller pushes the configuration,
        that includes the WLAN parameters, to the LWAPP APs.
        The APs then encapsulate all the 802.11 frames from
        wireless clients inside LWAPP frames and forward
        the LWAPP frames to the controller.

                           GLOSSARY

        Access Point ( AP )

        An entity that contains an 802.11 medium access
        control ( MAC ) and physical layer ( PHY ) interface
        and provides access to the distribution services via
        the wireless medium for associated clients.  

        LWAPP APs encapsulate all the 802.11 frames in
        LWAPP frames and sends them to the controller to which
        it is logically connected.

        Central Controller ( CC )

        The central entity that terminates the LWAPP protocol
        tunnel from the LWAPP APs.  Throughout this MIB,
        this entity also referred to as 'controller'.

        Cisco Compatible eXtensions (CCX)

        Wireless LAN Access Points (APs) manufactured by Cisco
        Systems have features and capabilities beyond those in
        related standards (e.g., IEEE 802.11 suite of 
        standards, Wi-Fi recommendations by WECA, 802.1X 
        security suite, etc). A number of features provide 
        higher performance. For example, Cisco AP transmits a 
        specific Information Element, which the clients adapt 
        to for enhanced performance. Similarly, a number of 
        features are implemented by means of proprietary 
        Information Elements, which Cisco clients use in 
        specific ways to carry out tasks above and beyond the
        standard. Other examples of feature categories are 
        roaming and power saving.

        Light Weight Access Point Protocol ( LWAPP ) 

        This is a generic protocol that defines the 
        communication between the Access Points and the
        Central Controller.

        Mobile Node ( MN )

        A roaming 802.11 wireless device in a wireless
        network associated with an access point.  The terms  
        'Mobile node' and 'client' are used interchangeably. 

        Radio Management (RM)

        This term refers to managing the 802.11 radio
        environment to provide the best quality service to
        to the 802.11 wireless clients. 

        Service Set Identifier ( SSID ) 

        SSID is a unique identifier that APs and clients
        use to identify with each other.  SSID is a simple
        means of access control and is not for security.
        The SSID can be any alphanumeric entry up to 32
        characters.

        REFERENCE

        [1] Wireless LAN Medium Access Control ( MAC ) and
        Physical Layer ( PHY ) Specifications

        [2] Draft-obara-capwap-lwapp-00.txt, IETF Light 
        Weight Access Point Protocol"
    REVISION        "201202210000Z"
    DESCRIPTION
        "Added ciscoLwappCcxRmDot11aConfigGroupVer1,
        ciscoLwappCcxRmDot11bConfigGroupVer1,
        and ciscoLwappCcxRmApIfConfigGroupVer1. 
        Deprecated ciscoLwappCcxRmDot11aConfigGroup,
        ciscoLwappCcxRmDot11bConfigGroup,
        and ciscoLwappCcxRmApIfConfigGroup. 
        Added ciscoLwappCcxRmMIBComplianceVer1 and 
        deprecated ciscoLwappCcxRmMIBCompliance."
    REVISION        "200604110000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 520 }


ciscoLwappCcxRmMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoLwappCcxRmMIB 0 }

ciscoLwappCcxRmMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappCcxRmMIB 1 }

ciscoLwappCcxRmMIBConform  OBJECT IDENTIFIER
    ::= { ciscoLwappCcxRmMIB 2 }

clcrDot11aConfigGlobal  OBJECT IDENTIFIER
    ::= { ciscoLwappCcxRmMIBObjects 1 }

clcrDot11bConfigGlobal  OBJECT IDENTIFIER
    ::= { ciscoLwappCcxRmMIBObjects 2 }

clcrApIfConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappCcxRmMIBObjects 3 }

clcrClientMeasurementReport  OBJECT IDENTIFIER
    ::= { ciscoLwappCcxRmMIBObjects 4 }

clcrWlanConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappCcxRmMIBObjects 5 }


-- ********************************************************************
-- Client Measurement request per 802.11a network
-- ********************************************************************

clcrdot11aBeaconEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "When set to 'true', LWAPP APs broadcast radio
        measurement request messages that include a
        beacon measurement request information element
        on 802.11a radio to clients compatible to
        CCX versions 2 and above.  This configuration
        takes higher precedence than that on the radio
        interface of the particular AP when 
        clcrAPIfOverrideGlobal is set to 'false'."
    DEFVAL          { false } 
    ::= { clcrDot11aConfigGlobal 1 }

clcrdot11aBeaconInterval OBJECT-TYPE
    SYNTAX          TimeInterval (6000..3240000)
    UNITS           "hundredths-seconds"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "The interval in hundredths of a second, in
        which the AP issues radio measurement request 
        message to client periodically for every SSID. 

        This configuration takes higher precedence than
        that on the radio interface of the particular AP
        when clcrAPIfOverrideGlobal is set to 'false'.
        clcrdot11aBeaconInterval object is superseded by 
        clcrdot11aBeaconIntvl."
    DEFVAL          { 6000 } 
    ::= { clcrDot11aConfigGlobal 2 }

clcrdot11aBeaconIntvl OBJECT-TYPE
    SYNTAX          TimeInterval
    UNITS           "hundredths-seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The interval in hundredths of a second, in
        which the AP issues radio measurement request 
        message to client periodically for every SSID. 

        This configuration takes higher precedence than
        that on the radio interface of the particular AP
        when clcrAPIfOverrideGlobal is set to 'false'." 
    ::= { clcrDot11aConfigGlobal 3 }

-- ********************************************************************
-- Client Measurement request per 802.11b network
-- ********************************************************************

clcrdot11bBeaconEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "When set to 'true', LWAPP APs broadcast radio
        measurement request messages that include a
        beacon measurement request information element,
        on 802.11b/802.11g radio to clients compatible to
        CCX versions 2 and above.  This configuration
        takes higher precedence than that on the radio
        interface of the particular AP when 
        clcrAPIfOverrideGlobal is set to 'false'."
    DEFVAL          { false } 
    ::= { clcrDot11bConfigGlobal 1 }

clcrdot11bBeaconInterval OBJECT-TYPE
    SYNTAX          TimeInterval (6000..3240000)
    UNITS           "hundredths-seconds"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "The interval in hundredths of a second, at
        which the AP issues radio measurement request 
        message to client periodically for every SSID.

        This configuration takes higher precedence than
        that on the radio interface of the particular AP
        when clcrAPIfOverrideGlobal is set to 'false'.
        clcrdot11bBeaconInterval object is superseded by 
        clcrdot11bBeaconIntvl."
    DEFVAL          { 6000 } 
    ::= { clcrDot11bConfigGlobal 2 }

clcrdot11bBeaconIntvl OBJECT-TYPE
    SYNTAX          TimeInterval
    UNITS           "hundredths-seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The interval in hundredths of a second, at
        which the AP issues radio measurement request 
        message to client periodically for every SSID.

        This configuration takes higher precedence than
        that on the radio interface of the particular AP
        when clcrAPIfOverrideGlobal is set to 'false'." 
    ::= { clcrDot11bConfigGlobal 3 }
-- ********************************************************************
-- Ccx configuration on Cisco AP Radio .
-- ********************************************************************

clcrAPIfTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF ClcrAPIfEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the CCX related parameters on
        the radio interface of the APs.  The values configured
        through the objects of this table are passed onto the
        AP by the controller, when the AP joins the 
        controller. 

        There exists a row in this table for each conceptual row
        in cLApDot11IfTable that represents a dot11 interface
        of an AP."
    ::= { clcrApIfConfig 1 }

clcrAPIfEntry OBJECT-TYPE
    SYNTAX          ClcrAPIfEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row in this table.
        An entry corresponding to each dot11 interface of an
        AP is added to this table when the AP joins the
        controller and deleted when AP disassociates from the
        controller."
    AUGMENTS           { cLApDot11IfEntry  } 
    ::= { clcrAPIfTable 1 }

ClcrAPIfEntry ::= SEQUENCE {
        clcrAPIfOverrideGlobal TruthValue,
        clcrAPIfBeaconEnabled  TruthValue,
        clcrAPIfBeaconInterval TimeInterval,
        clcrAPIfBeaconIntvl    TimeInterval
}

clcrAPIfOverrideGlobal OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "If this object is set to 'true', values populated
        through clcrAPIfBeaconEnabled and
        clcrAPIfBeaconInterval are considered for sending
        beacon measurement requests.

        If this object is set to 'false', the values 
        configured through the objects 
        clcrdot11bBeaconEnabled, clcrdot11aBeaconEnabled,
        clcrdot11bBeaconInterval and clcrdot11aBeaconInterval
        take precedence and are used for sending beacon
        measurement requests."
    DEFVAL          { false } 
    ::= { clcrAPIfEntry 1 }

clcrAPIfBeaconEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "When set to 'true', LWAPP APs broadcast radio
        measurement request messages that include a
        beacon measurement request information element
        to clients compatible with CCX versions 2 and
        above.

        Global configuration at network level takes
        higher precedence if clcrAPIfOverrideGlobal is
        set to 'false'.  Radio measurement frames include 
        a beacon request information element for every
        channel over which the measurement needs
        to be performed.  The measurement requests are
        repeated at every interval configured through
        clcrAPIfBeaconInterval."
    DEFVAL          { false } 
    ::= { clcrAPIfEntry 2 }

clcrAPIfBeaconInterval OBJECT-TYPE
    SYNTAX          TimeInterval (6000..3240000)
    UNITS           "hundredths-seconds"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "The interval at which the AP sends radio measurement
        request messages to the clients associated through
        each and every SSID.
        clcrAPIfBeaconInterval object is superseded by 
        clcrAPIfBeaconIntvl."
    DEFVAL          { 6000 } 
    ::= { clcrAPIfEntry 3 }

clcrAPIfBeaconIntvl OBJECT-TYPE
    SYNTAX          TimeInterval
    UNITS           "hundredths-seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The interval at which the AP sends radio measurement
        request messages to the clients associated through
        each and every SSID." 
    ::= { clcrAPIfEntry 4 }
 

-- ********************************************************************
-- * Beacon report from the CCX clients
-- ********************************************************************

clcrClientBeaconReportTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF ClcrClientBeaconReportEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table reports the received signal power as seen
        by a wireless client when conducting radio
        measurements.  Clients measure the received signal
        power by observing the beacon requests and probe
        response messages on all the specified channels and
        pass them to the APs through beacon reports.

        An entry is added to the table by the agent when the
        beacon report sent by the client arrives at the dot11
        interface of an AP.  An existing entry for a client
        gets over-written when the subsequent reports arrive
        at an AP from that client.  The term 'client' here
        refers to all the wireless CCX compliant devices like
        mobile stations, tags etc.

        An entry is deleted from this table when the particular
        client dissociates from the AP.  The entry also gets
        deleted when the AP dissociates from the controller."
    ::= { clcrClientMeasurementReport 1 }

clcrClientBeaconReportEntry OBJECT-TYPE
    SYNTAX          ClcrClientBeaconReportEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row in this table
        and populates the received signal power as observed
        and reported by the respective client."
    INDEX           {
                        clcrClientMacAddress,
                        cLApSysMacAddress,
                        cLApDot11IfSlotId
                    } 
    ::= { clcrClientBeaconReportTable 1 }

ClcrClientBeaconReportEntry ::= SEQUENCE {
        clcrClientMacAddress    MacAddress,
        clcrClientRxPowerSignal Integer32,
        clcrClientTimeStamp     TimeStamp
}

clcrClientMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object identifies the MAC address of a
        client that has sent a beacon report to the
        AP." 
    ::= { clcrClientBeaconReportEntry 1 }

clcrClientRxPowerSignal OBJECT-TYPE
    SYNTAX          Integer32 (-90..30)
    UNITS           "dBm"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the signal strength of the
        beacon or probe response frame as seen by the
        client." 
    ::= { clcrClientBeaconReportEntry 2 }

clcrClientTimeStamp OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the value of sysUpTime at
        which the beacon measurement report was 
        received." 
    ::= { clcrClientBeaconReportEntry 3 }
 

-- ********************************************************************
-- Table to represent CISCO CCX parameters
-- per each WLAN.
-- ********************************************************************

clcrWlanTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF ClcrWlanEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the CCX parameters of a
        particular WLAN.

        There exist a row in this table corresponding to each
        row representing a WLAN in cLWlanConfigTable."
    ::= { clcrWlanConfig 1 }

clcrWlanEntry OBJECT-TYPE
    SYNTAX          ClcrWlanEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row in this table
        and provides information about the CCX capabilities
        of the WLAN."
    AUGMENTS           { cLWlanConfigEntry  } 
    ::= { clcrWlanTable 1 }

ClcrWlanEntry ::= SEQUENCE {
        clcrVersionIESupport TruthValue,
        clcrAironetIESupport TruthValue
}

clcrVersionIESupport OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the support for the Cisco
        Compatible Extensions Version information element
        on this WLAN.

        A value of 'true' indicates the presence of the
        support and 'false' indicates the absence of the
        same." 
    ::= { clcrWlanEntry 1 }

clcrAironetIESupport OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates the support for the Cisco
        Compatible Extensions Aironet information element
        on this WLAN. 

        The support is enabled or disabled by setting 
        this object to 'true' or 'false' respectively."
    DEFVAL          { false } 
    ::= { clcrWlanEntry 2 }
 

-- ********************************************************************
-- *    Compliance statements
-- ********************************************************************

ciscoLwappCcxRmMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoLwappCcxRmMIBConform 1 }

ciscoLwappCcxRmMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoLwappCcxRmMIBConform 2 }


ciscoLwappCcxRmMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappCcxRmMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappCcxRmDot11aConfigGroup,
                        ciscoLwappCcxRmDot11bConfigGroup,
                        ciscoLwappCcxRmApIfConfigGroup,
                        ciscoLwappCcxRmBeaconReportGroup,
                        ciscoLwappCcxRmD11WlanConfigGroup
                    }
    ::= { ciscoLwappCcxRmMIBCompliances 1 }

ciscoLwappCcxRmMIBComplianceVer1 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappCcxRmMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappCcxRmDot11aConfigGroupVer1,
                        ciscoLwappCcxRmDot11bConfigGroupVer1,
                        ciscoLwappCcxRmApIfConfigGroupVer1,
                        ciscoLwappCcxRmBeaconReportGroup,
                        ciscoLwappCcxRmD11WlanConfigGroup
                    }
    ::= { ciscoLwappCcxRmMIBCompliances 2 }

-- ********************************************************************
-- *    Units of conformance
-- ********************************************************************

ciscoLwappCcxRmDot11aConfigGroup OBJECT-GROUP
    OBJECTS         {
                        clcrdot11aBeaconEnabled,
                        clcrdot11aBeaconInterval
                    }
    STATUS          deprecated
    DESCRIPTION
        "This collection of objects represent the beacon
        request and beacon interval parameters for 802.11a
        networks.
        ciscoLwappCcxRmDot11aConfigGroup object is superseded by 
        ciscoLwappCcxRmDot11aConfigGroupVer1."
    ::= { ciscoLwappCcxRmMIBGroups 1 }

ciscoLwappCcxRmDot11bConfigGroup OBJECT-GROUP
    OBJECTS         {
                        clcrdot11bBeaconEnabled,
                        clcrdot11bBeaconInterval
                    }
    STATUS          deprecated
    DESCRIPTION
        "This collection of objects represent the beacon
        request and beacon interval parameters for 802.11b
        networks.
        ciscoLwappCcxRmDot11bConfigGroup object is superseded by 
        ciscoLwappCcxRmDot11bConfigGroupVer1."
    ::= { ciscoLwappCcxRmMIBGroups 2 }

ciscoLwappCcxRmApIfConfigGroup OBJECT-GROUP
    OBJECTS         {
                        clcrAPIfOverrideGlobal,
                        clcrAPIfBeaconEnabled,
                        clcrAPIfBeaconInterval
                    }
    STATUS          deprecated
    DESCRIPTION
        "This collection of objects represent the beacon
        request and beacon interval parameters for the
        respective 802.11 radio interfaces.
        ciscoLwappCcxRmApIfConfigGroup object is superseded by 
        ciscoLwappCcxRmApIfConfigGroupVer1."
    ::= { ciscoLwappCcxRmMIBGroups 3 }

ciscoLwappCcxRmBeaconReportGroup OBJECT-GROUP
    OBJECTS         {
                        clcrClientRxPowerSignal,
                        clcrClientTimeStamp
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent information
        about the beacon reports received from CCX 
        clients."
    ::= { ciscoLwappCcxRmMIBGroups 4 }

ciscoLwappCcxRmD11WlanConfigGroup OBJECT-GROUP
    OBJECTS         {
                        clcrVersionIESupport,
                        clcrAironetIESupport
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the CCX
        settings on a particular WLAN."
    ::= { ciscoLwappCcxRmMIBGroups 5 }

ciscoLwappCcxRmDot11aConfigGroupVer1 OBJECT-GROUP
    OBJECTS         {
                        clcrdot11aBeaconEnabled,
                        clcrdot11aBeaconIntvl
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the beacon
        request and beacon interval parameters for 802.11a
        networks."
    ::= { ciscoLwappCcxRmMIBGroups 6 }

ciscoLwappCcxRmDot11bConfigGroupVer1 OBJECT-GROUP
    OBJECTS         {
                        clcrdot11bBeaconEnabled,
                        clcrdot11bBeaconIntvl
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the beacon
        request and beacon interval parameters for 802.11b
        networks."
    ::= { ciscoLwappCcxRmMIBGroups 7 }

ciscoLwappCcxRmApIfConfigGroupVer1 OBJECT-GROUP
    OBJECTS         {
                        clcrAPIfOverrideGlobal,
                        clcrAPIfBeaconEnabled,
                        clcrAPIfBeaconIntvl
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the beacon
        request and beacon interval parameters for the
        respective 802.11 radio interfaces."
    ::= { ciscoLwappCcxRmMIBGroups 8 }

END














