-- *******************************************************************
-- CISCO-LWAPP-CLIENT-ROAMING-MIB.my: Wireless client roaming MIB
-- December 2005, Devesh Pujari , Prasanna Viswakumar
--   
-- Copyright (c) 2005, 2006, 2009-2010 by Cisco Systems Inc.
-- *******************************************************************

CISCO-LWAPP-CLIENT-ROAMING-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Counter32,
    Integer32,
    TimeTicks
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    MacAddress,
    TimeInterval
        FROM SNMPv2-TC
    cLApSysMacAddress,
    cLApDot11IfSlotId
        FROM CISCO-LWAPP-AP-MIB
    CLDot11Channel,
    CLDot11RfParamMode
        FROM CISCO-LWAPP-TC-MIB
    ciscoMgmt
        FROM CISCO-SMI;


ciscoLwappClRoamMIB MODULE-IDENTITY
    LAST-UPDATED    "201001290000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems,
            Customer Service
            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA
            Tel: +1 800 553-NETS

            Email: cs-wnbu-snmp@cisco.com"
    DESCRIPTION
        "This MIB is intended to be implemented on all those
        devices operating as Central controllers, that
        terminate the Light Weight Access Point Protocol
        tunnel from Cisco Light-weight LWAPP Access Points.

        Information provided by this MIB is for CCX related 
        features as specified in the CCX specifications.  
        This MIB covers roaming RF parameters for CCX 
        clients.

        The relationship between CC and the LWAPP APs
        can be depicted as follows:

              +......+     +......+     +......+
              +      +     +      +     +      +
              +  CC  +     +  CC  +     +  CC  +
              +      +     +      +     +      +
              +......+     +......+     +......+
                ..            .             .
                ..            .             .
               .  .            .             .
              .    .            .             .
             .      .            .             .
            .        .            .             .
        +......+ +......+     +......+      +......+
        +      + +      +     +      +      +      +
        +  AP  + +  AP  +     +  AP  +      +  AP  +
        +      + +      +     +      +      +      +
        +......+ +......+     +......+      +......+
                   .              .             .
                 .  .              .             .
                .    .              .             .
               .      .              .             .
              .        .              .             .
           +......+ +......+     +......+      +......+
           +      + +      +     +      +      +      +
           +  MN  + +  MN  +     +  MN  +      +  MN  +
           +      + +      +     +      +      +      +
           +......+ +......+     +......+      +......+


        The LWAPP tunnel exists between the controller and
        the APs.  The MNs communicate with the APs through
        the protocol defined by the 802.11 standard.

        LWAPP APs, upon bootup, discover and join one of the
        controllers and the controller pushes the configuration,
        that includes the WLAN parameters, to the LWAPP APs.
        The APs then encapsulate all the 802.11 frames from
        wireless clients inside LWAPP frames and forward
        the LWAPP frames to the controller.

                           GLOSSARY

        Access Point ( AP )

        An entity that contains an 802.11 medium access
        control ( MAC ) and physical layer ( PHY ) interface
        and provides access to the distribution services via
        the wireless medium for associated clients.  

        LWAPP APs encapsulate all the 802.11 frames in
        LWAPP frames and sends them to the controller to which
        it is logically connected.

        Basic Service Set ( BSS )

        The IEEE 802.11 BSS of an AP comprises of the
        stations directly associating with the AP.

        Central Controller ( CC )

        The central entity that terminates the LWAPP protocol
        tunnel from the LWAPP APs.  Throughout this MIB,
        this entity is also referred to as 'controller'.

        Cisco Compatible eXtensions (CCX)

        Wireless LAN Access Points (APs) manufactured by Cisco
        Systems have features and capabilities beyond those in
        related standards (e.g., IEEE 802.11 suite of
        standards ,Wi-Fi recommendations by WECA, 802.1X
        security suite,etc). A number of features provide
        higher performance.For example, Cisco AP transmits a
        specific Information Element, which the clients adapt
        to for enhanced performance. Similarly, a number of
        features are implemented by means of proprietary
        Information Elements, which Cisco clients use in 
        specific ways to carry out tasks above and beyond the
        standard. Other examples of feature categories are
        roaming and power saving.

        Client Roaming

        A client may decide to reassociate with another AP for
        reasons of its own choosing. The decision of whether
        or not to use the information contained in the AP list
        is up to the discretion of the implementor, as long as 
        the roam time requirement is met.

        Light Weight Access Point Protocol ( LWAPP ) 

        This is a generic protocol that defines the 
        communication between the Access Points and the
        Central Controller.

        Mobile Node ( MN )

        A roaming 802.11 wireless device in a wireless
        network associated with an access point. Mobile Node 
        and client are used interchangeably. 

        REFERENCE

        [1] Wireless LAN Medium Access Control ( MAC ) and
        Physical Layer ( PHY ) Specifications

        [2] Draft-obara-capwap-lwapp-00.txt, IETF Light 
        Weight Access Point Protocol"
    REVISION        "201001290000Z"
    DESCRIPTION
        "Deprecated following attributes:-
        clcrDot11aMinRssi, clcrDot11aHysteresis,
        clcrDot11aAdaptiveScanThreshold, clcrDot11aTransitionTime, 
        clcrDot11bMinRssi, clcrDot11bHysteresis,
        clcrDot11bAdaptiveScanThreshold, clcrDot11bTransitionTime.
        clcrMIBCompliance, ciscoLwappClRoamDot11aRfParamsGroup,
        ciscoLwappClRoamDot11bRfParamsGroup

        Added following attributes:-
        clcrDot11aMinRssiV2, clcrDot11aHysteresisV2,
        clcrDot11aAdaptiveScanThresholdV2, clcrDot11aTransitionTimeV2, 
        clcrDot11bMinRssiV2, clcrDot11bHysteresisV2,
        clcrDot11bAdaptiveScanThresholdV2, clcrDot11bTransitionTimeV2.
        clcrMIBComplianceRev1, ciscoLwappClRoamDot11aRfParamsGroupSup1,
        ciscoLwappClRoamDot11bRfParamsGroupSup1"
    REVISION        "200604110000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 523 }


ciscoLwappClRoamMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoLwappClRoamMIB 0 }

ciscoLwappClRoamMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappClRoamMIB 1 }

ciscoLwappClRoamMIBConform  OBJECT IDENTIFIER
    ::= { ciscoLwappClRoamMIB 2 }

clcrRoamDot11aRfParamConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappClRoamMIBObjects 1 }

clcrRoamDot11bRfParamConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappClRoamMIBObjects 2 }

clcrRoamReasonReport  OBJECT IDENTIFIER
    ::= { ciscoLwappClRoamMIBObjects 3 }

clcrRoamDot11Stats  OBJECT IDENTIFIER
    ::= { ciscoLwappClRoamMIBObjects 4 }


-- ********************************************************************
-- Clients Roaming RF Parameters for 802.11a band.
-- ********************************************************************

clcrDot11aMode OBJECT-TYPE
    SYNTAX          CLDot11RfParamMode
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents how the controller chooses
        the values of the RF parameters needed to manage
        roaming in 802.11a networks."
    DEFVAL          { default } 
    ::= { clcrRoamDot11aRfParamConfig 1 }

clcrDot11aMinRssi OBJECT-TYPE
    SYNTAX          Integer32 (-90..-80)
    UNITS           "dBm"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object indicates the Minimum Received Signal
        Strength Indication (RSSI) in dBm required to
        associate with the AP. It also defines the edge of
        coverage for the BSS. If the client's average
        received signal power dips below this threshold,
        clients  must have roamed to another AP with a
        stronger signal.

        This object is superceded by clcrDot11aMinRssiV2"
    DEFVAL          { -85 } 
    ::= { clcrRoamDot11aRfParamConfig 2 }

clcrDot11aHysteresis OBJECT-TYPE
    SYNTAX          Integer32 (2..4)
    UNITS           "dB"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object indicates how much stronger the signal
        strength (dB) of a neighbor AP must be, in order
        for the client to roam to it.  The use of roaming
        hysteresis is intended to reduce the amount of
        clients roaming back and forth between BSSs if the
        client is physically located on or near the border
        between two BSSs.

        This object is superceded by clcrDot11aHysteresisV2"
    DEFVAL          { 2 } 
    ::= { clcrRoamDot11aRfParamConfig 3 }

clcrDot11aAdaptiveScanThreshold OBJECT-TYPE
    SYNTAX          Integer32 (-77..-70)
    UNITS           "dBm"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object configures the threshold for the
        strength of the signals received(RSSI) from an AP,
        as seen by an associated client, below which the
        client must be able to roam to a neighbor AP within
        the specified Transition Time configured through
        clcrDot11aTransitionTime.

        This object is superceded by clcrDot11aAdaptiveScanThresholdV2"
    DEFVAL          { -72 } 
    ::= { clcrRoamDot11aRfParamConfig 4 }

clcrDot11aTransitionTime OBJECT-TYPE
    SYNTAX          TimeInterval (100..10000)
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object configures the maximum time duration
        permitted for the client to detect a suitable
        neighbor AP to roam to and to complete the roam,
        whenever the RSSI from the client?s associated AP
        is below the adaptive scan threshold configured
        through clcrDot11aAdaptiveScanThreshold.  The time
        is expressed in 100th of a second.

        This object is superceded by clcrDot11aTransitionTimeV2"
    DEFVAL          { 500 } 
    ::= { clcrRoamDot11aRfParamConfig 5 }

clcrDot11aMinRssiV2 OBJECT-TYPE
    SYNTAX          Integer32 (-255..255)
    UNITS           "dBm"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates the Minimum Received Signal
        Strength Indication (RSSI) in dBm required to
        associate with the AP. It also defines the edge of
        coverage for the BSS. If the client's average
        received signal power dips below this threshold,
        clients  must have roamed to another AP with a
        stronger signal." 
    ::= { clcrRoamDot11aRfParamConfig 6 }

clcrDot11aHysteresisV2 OBJECT-TYPE
    SYNTAX          Integer32 (0..255)
    UNITS           "dB"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates how much stronger the signal
        strength (dB) of a neighbor AP must be, in order
        for the client to roam to it.  The use of roaming
        hysteresis is intended to reduce the amount of
        clients roaming back and forth between BSSs if the
        client is physically located on or near the border
        between two BSSs." 
    ::= { clcrRoamDot11aRfParamConfig 7 }

clcrDot11aAdaptiveScanThresholdV2 OBJECT-TYPE
    SYNTAX          Integer32 (-255..255)
    UNITS           "dBm"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object configures the threshold for the
        strength of the signals received(RSSI) from an AP,
        as seen by an associated client, below which the
        client must be able to roam to a neighbor AP within
        the specified Transition Time configured through
        clcrDot11aTransitionTime." 
    ::= { clcrRoamDot11aRfParamConfig 8 }

clcrDot11aTransitionTimeV2 OBJECT-TYPE
    SYNTAX          TimeInterval (0..10000)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object configures the maximum time duration
        permitted for the client to detect a suitable
        neighbor AP to roam to and to complete the roam,
        whenever the RSSI from the clients associated AP
        is below the adaptive scan threshold configured
        through clcrDot11aAdaptiveScanThreshold.  The time
        is expressed in 100th of a second." 
    ::= { clcrRoamDot11aRfParamConfig 9 }

-- ********************************************************************
-- Clients Roaming RF Parameters for 802.11b/g band.
-- ********************************************************************

clcrDot11bMode OBJECT-TYPE
    SYNTAX          CLDot11RfParamMode
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents how the controller chooses
        the values of the RF parameters needed to manage
        roaming in 802.11b/g networks."
    DEFVAL          { default } 
    ::= { clcrRoamDot11bRfParamConfig 1 }

clcrDot11bMinRssi OBJECT-TYPE
    SYNTAX          Integer32 (-90..-80)
    UNITS           "dBm"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object indicates the minimum Received Signal
        Strength Indication (RSSI) in dBm required to
        associate with the AP. It also defines the edge of
        coverage for the BSS. If the client's average
        received signal power dips below this threshold,
        clients  must have roamed to another AP with a
        stronger signal.

        This object is superceded by clcrDot11bMinRssiV2"
    DEFVAL          { -85 } 
    ::= { clcrRoamDot11bRfParamConfig 2 }

clcrDot11bHysteresis OBJECT-TYPE
    SYNTAX          Integer32 (2..4)
    UNITS           "dB"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object indicates how much stronger the signal
        strength (dB) of a neighbor AP must be, in order
        for the client to roam to it.  The use of roaming
        hysteresis is intended to reduce the amount of
        clients roaming back and forth between BSSs if the
        client is physically located on or near the border
        between two BSSs.

        This object is superceded by clcrDot11bHysteresisV2"
    DEFVAL          { 2 } 
    ::= { clcrRoamDot11bRfParamConfig 3 }

clcrDot11bAdaptiveScanThreshold OBJECT-TYPE
    SYNTAX          Integer32 (-77..-70)
    UNITS           "dBm"
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object configures the threshold for the
        strength of the signals received(RSSI) from an AP,
        as seen by an associated client, below which the
        client must be able to roam to a neighbor AP within
        the specified Transition Time configured through
        clcrDot11bTransitionTime.

        This object is superceded by clcrDot11bAdaptiveScanThresholdV2"
    DEFVAL          { -72 } 
    ::= { clcrRoamDot11bRfParamConfig 4 }

clcrDot11bTransitionTime OBJECT-TYPE
    SYNTAX          TimeInterval (100..10000)
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object configures the maximum time duration
        permitted for the client to detect a suitable
        neighbor AP to roam to and to complete the roam,
        whenever the RSSI from the client is associated AP
        is below the adaptive scan threshold configured
        through clcrDot11aAdaptiveScanThreshold.  The
        time is expressed in 100th of a second.

        This object is superceded by clcrDot11bTransitionTimeV2"
    DEFVAL          { 500 } 
    ::= { clcrRoamDot11bRfParamConfig 5 }

clcrDot11bMinRssiV2 OBJECT-TYPE
    SYNTAX          Integer32 (-255..255)
    UNITS           "dBm"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates the minimum Received Signal
        Strength Indication (RSSI) in dBm required to
        associate with the AP. It also defines the edge of
        coverage for the BSS. If the client's average
        received signal power dips below this threshold,
        clients  must have roamed to another AP with a
        stronger signal." 
    ::= { clcrRoamDot11bRfParamConfig 6 }

clcrDot11bHysteresisV2 OBJECT-TYPE
    SYNTAX          Integer32 (0..255)
    UNITS           "dB"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates how much stronger the signal
        strength (dB) of a neighbor AP must be, in order
        for the client to roam to it.  The use of roaming
        hysteresis is intended to reduce the amount of
        clients roaming back and forth between BSSs if the
        client is physically located on or near the border
        between two BSSs." 
    ::= { clcrRoamDot11bRfParamConfig 7 }

clcrDot11bAdaptiveScanThresholdV2 OBJECT-TYPE
    SYNTAX          Integer32 (-255..255)
    UNITS           "dBm"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object configures the threshold for the
        strength of the signals received(RSSI) from an AP,
        as seen by an associated client, below which the
        client must be able to roam to a neighbor AP within
        the specified Transition Time configured through
        clcrDot11bTransitionTime." 
    ::= { clcrRoamDot11bRfParamConfig 8 }

clcrDot11bTransitionTimeV2 OBJECT-TYPE
    SYNTAX          TimeInterval (0..10000)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object configures the maximum time duration
        permitted for the client to detect a suitable
        neighbor AP to roam to and to complete the roam,
        whenever the RSSI from the client is associated AP
        is below the adaptive scan threshold configured
        through clcrDot11aAdaptiveScanThreshold.  The
        time is expressed in 100th of a second." 
    ::= { clcrRoamDot11bRfParamConfig 9 }
-- ********************************************************************
-- Client Roam Reason Report
-- ********************************************************************

clcrRoamReasonReportTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF ClcrRoamReasonReportEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides the reasons for CCX clients
        roaming from one AP to another. 

        When a CCX client associates to an AP, it will always 
        send an IAPP information packet to the new AP listing 
        the characteristics of the previous AP.

        An entry is added to this table when a roam reason
        report is sent by a CCX client when it roams to a
        new AP."
    ::= { clcrRoamReasonReport 1 }

clcrRoamReasonReportEntry OBJECT-TYPE
    SYNTAX          ClcrRoamReasonReportEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry corresponds to the roam reason report
        sent by a CCX client to the new AP to which client 
        associates."
    INDEX           {
                        clcrRoamClientMacAddress,
                        clcrRoamClientTimeStamp
                    } 
    ::= { clcrRoamReasonReportTable 1 }

ClcrRoamReasonReportEntry ::= SEQUENCE {
        clcrRoamClientMacAddress     MacAddress,
        clcrRoamClientTimeStamp      TimeTicks,
        clcrRoamNewApMacAddress      MacAddress,
        clcrRoamPrevApMacAddress     MacAddress,
        clcrRoamPrevApChannel        CLDot11Channel,
        clcrRoamPrevApSsid           OCTET STRING,
        clcrRoamDisassocTimeInterval TimeInterval,
        clcrRoamReason               INTEGER
}

clcrRoamClientMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the mac address of the
        client which has roamed to a new AP." 
    ::= { clcrRoamReasonReportEntry 1 }

clcrRoamClientTimeStamp OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the time instance at which
        this report was received by the new AP, to which 
        client roamed to.  This represents number of
        seconds elapsed since 00:00:00 on January 1, 1970,
        Coordinated Universal Time (UTC).  So a value of 
        '1131362704' means 'Mon Nov  7 16:55:04 2005'." 
    ::= { clcrRoamReasonReportEntry 2 }

clcrRoamNewApMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the mac address of the
        current AP to which client has roamed to. This AP
        receives the roam reason report." 
    ::= { clcrRoamReasonReportEntry 3 }

clcrRoamPrevApMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the mac address of the
        previous AP to which client was associated." 
    ::= { clcrRoamReasonReportEntry 4 }

clcrRoamPrevApChannel OBJECT-TYPE
    SYNTAX          CLDot11Channel
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the channel number at which
        the client was associated to the previous AP." 
    ::= { clcrRoamReasonReportEntry 5 }

clcrRoamPrevApSsid OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (1..32))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the SSID at which the client
        was associated to the previous AP." 
    ::= { clcrRoamReasonReportEntry 6 }

clcrRoamDisassocTimeInterval OBJECT-TYPE
    SYNTAX          TimeInterval
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the time elapsed since the
        client disassociated, in hundredth of a second." 
    ::= { clcrRoamReasonReportEntry 7 }

clcrRoamReason OBJECT-TYPE
    SYNTAX          INTEGER  {
                        clcrUnspecified(0),
                        clcrPoorLink(1),
                        clcrLoadBalancing(2),
                        clcrInsufficientCapacity(3),
                        clcrDirectedRoam(4),
                        clcrFirstAssociation(5),
                        clcrRoamingIn(6),
                        clcrRoamingOut(7),
                        clcrBetterAp(8),
                        clcrDisassociated(9)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the reason for a client to
        roam to a new AP.

        The semantics are as follows.

        clcrUnspecified - The reason is not known or can't
        be found.

        clcrPoorLink - Normal roam due to poor link 
        (excessive retries, too much interference, RSSI too 
        low, etc.)

        clcrLoadBalancing - Normal roam due to load 
        balancing

        clcrInsufficientCapacity - Roaming occured due to
        the insufficient capacity on the previous AP
        (TSPEC rejected)

        clcrDirectedRoam - Roaming is directed by the
        802.11 wireless Infrastructure 

        clcrFirstAssociation - This is the first  
        association to a particular WLAN

        clcrRoamingIn - Roaming in from cellular or other 
        WAN

        clcrRoamingOut - Roaming out to cellular or other 
        WAN

        clcrBetterAp - Normal roam due to better AP found

        clcrDisassociated - Deauthenticated or
        Disassociated from the previous AP." 
    ::= { clcrRoamReasonReportEntry 8 }
 

-- ********************************************************************
-- Roaming Stats per 802.11 interface.
-- ********************************************************************

clcrDot11StatsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF ClcrDot11StatsEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table populates the statistics collected when
        the client roamed in the WLAN.

        There exists a row in this table for each conceptual
        row in cLApDot11IfTable that represents a dot11 
        interface of an AP."
    ::= { clcrRoamDot11Stats 1 }

clcrDot11StatsEntry OBJECT-TYPE
    SYNTAX          ClcrDot11StatsEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row in
        clcrDot11StatsTable and corresponds to the roam
        reason report  sent by a CCX client to the new AP
        which the client associates to."
    INDEX           {
                        cLApSysMacAddress,
                        cLApDot11IfSlotId
                    } 
    ::= { clcrDot11StatsTable 1 }

ClcrDot11StatsEntry ::= SEQUENCE {
        clcrDot11NeighborRequestRx  Counter32,
        clcrDot11NeighborReplySent  Counter32,
        clcrDot11RoamReasonReportRx Counter32,
        clcrDot11BcastUpdatesSent   Counter32
}

clcrDot11NeighborRequestRx OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the count of the number
        of requests received from an E2E client for 
        neighbor updates." 
    ::= { clcrDot11StatsEntry 1 }

clcrDot11NeighborReplySent OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the count of the number
        of replies sent to the client in reply to the
        request for neighbor updates received from the
        client." 
    ::= { clcrDot11StatsEntry 2 }

clcrDot11RoamReasonReportRx OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object reports the count of the number
        of roam reason reports received from CCX
        clients." 
    ::= { clcrDot11StatsEntry 3 }

clcrDot11BcastUpdatesSent OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the count of the number of
        broadcast neighbor updates sent by an AP." 
    ::= { clcrDot11StatsEntry 4 }
 

-- ********************************************************************
-- *    Compliance statements
-- ********************************************************************

ciscoLwappClRoamMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoLwappClRoamMIBConform 1 }

ciscoLwappClRoamMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoLwappClRoamMIBConform 2 }


clcrMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappRoamMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappClRoamDot11aRfParamsGroup,
                        ciscoLwappClRoamDot11bRfParamsGroup,
                        ciscoLwappClRoamroamReasonGroup,
                        ciscoLwappClRoamroamingStatsGroup
                    }
    ::= { ciscoLwappClRoamMIBCompliances 1 }

clcrMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappRoamMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappClRoamDot11aRfParamsGroupSup1,
                        ciscoLwappClRoamDot11bRfParamsGroupSup1,
                        ciscoLwappClRoamroamReasonGroup,
                        ciscoLwappClRoamroamingStatsGroup
                    }
    ::= { ciscoLwappClRoamMIBCompliances 2 }

-- ********************************************************************
-- *    Units of conformance
-- ********************************************************************

ciscoLwappClRoamDot11aRfParamsGroup OBJECT-GROUP
    OBJECTS         {
                        clcrDot11aMode,
                        clcrDot11aMinRssi,
                        clcrDot11aHysteresis,
                        clcrDot11aAdaptiveScanThreshold,
                        clcrDot11aTransitionTime
                    }
    STATUS          deprecated
    DESCRIPTION
        "This collection of objects represent the radio
        parameters for the 802.11a networks."
    ::= { ciscoLwappClRoamMIBGroups 1 }

ciscoLwappClRoamDot11bRfParamsGroup OBJECT-GROUP
    OBJECTS         {
                        clcrDot11bMode,
                        clcrDot11bMinRssi,
                        clcrDot11bHysteresis,
                        clcrDot11bAdaptiveScanThreshold,
                        clcrDot11bTransitionTime
                    }
    STATUS          deprecated
    DESCRIPTION
        "This collection of objects represent the radio
        parameters for the 802.11b/g bands."
    ::= { ciscoLwappClRoamMIBGroups 2 }

ciscoLwappClRoamroamReasonGroup OBJECT-GROUP
    OBJECTS         {
                        clcrRoamNewApMacAddress,
                        clcrRoamPrevApMacAddress,
                        clcrRoamPrevApChannel,
                        clcrRoamPrevApSsid,
                        clcrRoamDisassocTimeInterval,
                        clcrRoamReason
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects provide the reasons for
        clients roaming between APs."
    ::= { ciscoLwappClRoamMIBGroups 3 }

ciscoLwappClRoamroamingStatsGroup OBJECT-GROUP
    OBJECTS         {
                        clcrDot11NeighborRequestRx,
                        clcrDot11NeighborReplySent,
                        clcrDot11RoamReasonReportRx,
                        clcrDot11BcastUpdatesSent
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects provide the counters
        related to roaming."
    ::= { ciscoLwappClRoamMIBGroups 4 }

ciscoLwappClRoamDot11aRfParamsGroupSup1 OBJECT-GROUP
    OBJECTS         {
                        clcrDot11aMode,
                        clcrDot11aMinRssiV2,
                        clcrDot11aHysteresisV2,
                        clcrDot11aAdaptiveScanThresholdV2,
                        clcrDot11aTransitionTimeV2
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the radio
        parameters for the 802.11a networks."
    ::= { ciscoLwappClRoamMIBGroups 5 }

ciscoLwappClRoamDot11bRfParamsGroupSup1 OBJECT-GROUP
    OBJECTS         {
                        clcrDot11bMode,
                        clcrDot11bMinRssiV2,
                        clcrDot11bHysteresisV2,
                        clcrDot11bAdaptiveScanThresholdV2,
                        clcrDot11bTransitionTimeV2
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the radio
        parameters for the 802.11b/g bands."
    ::= { ciscoLwappClRoamMIBGroups 6 }

END



















