-- *****************************************************************
-- CISCO-SERVICE-CONTROL-RDR-MIB.my
--   
-- MIB file for Cisco Service Control Raw Data Reporter.
-- March 2007, Zaryab Munir.
--   
-- Copyright (c) 2007 by cisco Systems Inc.
-- All rights reserved.
--   
-- ****************************************************************

CISCO-SERVICE-CONTROL-RDR-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Counter32,
    NOTIFICATION-TYPE,
    Gauge32,
    Unsigned32,
    Integer32,
    TimeTicks
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    NOTIFICATION-GROUP,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    InetAddressType,
    InetAddress,
    InetPortNumber
        FROM INET-ADDRESS-MIB
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    entPhysicalIndex,
    entPhysicalName
        FROM ENTITY-MIB
    TruthValue,
    TimeStamp
        FROM SNMPv2-TC
    ciscoMgmt
        FROM CISCO-SMI;


ciscoServiceControlRdrMIB MODULE-IDENTITY
    LAST-UPDATED    "200708140000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-excelsior-dev@cisco.com"
    DESCRIPTION
        "This MIB module defines objects describing statistics and
        configuration relating to the Raw Data Record Formatter running
        on a service control entity.

        The Raw Data Record (RDR) formatter is a component implemented
        by the service control entity that gathers raw data records
        produced by the entity and delivers them to external entities
        as reports.  The external entities are called RDR destinations
        or RDR collectors.  The RDR formatter can be configured to send
        reports to one or multiple destinations. 

        RDR formatter can group RDRs into potentially four categories.
        RDR mapping to the categories is done by the client application
        or the user and reflects different logical destinations or
        purposes.  For example the application may map Quota related
        RDRs to category 1, and Transaction related RDRs to category 2. 
        The user can configure these categories to different
        destinations and assign them with different priorities.  Each
        category has a separate queue for forwarding the RDRs and has
        seperate counters for gathering of statistics (sent, dropped,
        queued etc.).  An RDR can belong to any one of the category as
        chosen by the user or client application.  

        The RDR formatter supports multiple destinations identified by
        IP address and a port number. Each destination is assigned with
        a priority for each of the categories.  Priority is a number in
        the range of 1-100, with 100 being the highest priority.  The
        priorities are effective only when the formatter is in
        forwarding mode 'Redundancy' and are configured during
        destination configuration (while assigning the destination with
        categories).  For example we have destination A configured with
        category 1 which is configured with priority 100, destination B
        configured with category 1 and priority 80 and destination C
        with category 1 and priority 90.  When in redundancy mode the
        formatter will set the active destination for a category to be
        the destination with the highest priority.  For category 1 the
        active destination will be A. If destination A goes down then
        the next destination selected by the formatter as active is
        destination C."
    REVISION        "200708140000Z"
    DESCRIPTION
        "Initial version of this MIB module"
    ::= { ciscoMgmt 637 }


ciscoSCRdrMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoServiceControlRdrMIB 0 }

ciscoSCRdrMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoServiceControlRdrMIB 1 }

ciscoSCRdrMIBConform  OBJECT IDENTIFIER
    ::= { ciscoServiceControlRdrMIB 2 }


cscRdrFormatterTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CscRdrFormatterEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table lists the operational information and aggregated
        statistics for the RDR formatter of a service control entity."
    ::= { ciscoSCRdrMIBObjects 1 }

cscRdrFormatterEntry OBJECT-TYPE
    SYNTAX          CscRdrFormatterEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry contains the operational data and global counters
        for the RDR formatter associated with the service control entity
        identified by its assigned entPhysicalIndex.  An entry exists
        for each corresponding row in the entPhysicalTable having one of
        the following values assigned to entPhysicalVendorType:
            - cevChassisSCE2000
            - cevChassisSCE1000
            - cevNmeApaModule."
    INDEX           { entPhysicalIndex } 
    ::= { cscRdrFormatterTable 1 }

CscRdrFormatterEntry ::= SEQUENCE {
        cscRdrFormatterEnable              TruthValue,
        cscRdrFormatterNumSentReports      Counter32,
        cscRdrFormatterNumDiscardedReports Counter32,
        cscRdrFormatterReportRate          Gauge32,
        cscRdrFormatterReportRatePeak      Gauge32,
        cscRdrFormatterReportRatePeakTime  TimeTicks,
        cscRdrFormatterProtocol            INTEGER ,
        cscRdrFormatterForwardingMode      INTEGER 
}

cscRdrFormatterEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies whether the RDR formatter is enabled or
        disabled.  When the RDR formatter is enabled, it sends the
        records it gets from the traffic processors to the RDR
        destination as defined in the cscRdrDestTable." 
    ::= { cscRdrFormatterEntry 1 }

cscRdrFormatterNumSentReports OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "reports"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of reports sent by the
        RDR formatter.

        Discontinuities in the value of this counter can occur at
        disabling/enabling of the RDR formatter, and at other times
        as indicated by the value of cscRdrCounterDiscontinuityTime." 
    ::= { cscRdrFormatterEntry 2 }

cscRdrFormatterNumDiscardedReports OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "reports"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of reports discarded by the
        RDR formatter due to insufficient resources or unavailibility
        of
        the destination.

        Discontinuities in the value of this counter can occur at
        disabling/enabling of the RDR formatter, and at other times
        as indicated by the value of cscRdrCounterDiscontinuityTime." 
    ::= { cscRdrFormatterEntry 3 }

cscRdrFormatterReportRate OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "reports per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the rate at which the RDR formatter is
        currently sending reports to all of the destinations." 
    ::= { cscRdrFormatterEntry 4 }

cscRdrFormatterReportRatePeak OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "reports per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the maximum rate at which the RDR
        formatter sent reports to all of the destinations since
        sysUpTime, if cscRdrCounterDiscontinuityTime is zero.  If
        cscRdrCounterDiscontinuityTime has a non zero value, the
        maximum rate is determined from this value." 
    ::= { cscRdrFormatterEntry 5 }

cscRdrFormatterReportRatePeakTime OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the time elapsed since the
        cscRdrFormatterReportRatePeak value occured." 
    ::= { cscRdrFormatterEntry 6 }

cscRdrFormatterProtocol OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        rdrv1(2),
                        netflowV9(3)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the RDR protocol currently used by the
        RDR formatter.
        'other'      : The RDR formatter is using a protocol not 
                       recognized by this revision of the MIB.
        'rdrv1'      : RDR protocol version 1
        'netflowV9'  : NetFlow ver 9"
    DEFVAL          { rdrv1 } 
    ::= { cscRdrFormatterEntry 7 }

cscRdrFormatterForwardingMode OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        redundancy(2),
                        simpleLoadBalancing(3),
                        multicast(4)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the mode by which the RDR formatter
        sends the reports to its destinations.
        'other'                : The RDR formatter is using a protocol 
                                 not recognized by this revision of the 
                                 MIB.
        'redundancy'           : The reports are sent to the primary 
                                 (active destination) and all of the
                                 other destinations are in standby.
        'simpleLoadBalancing'  : The reports are sent to one
        destination
                                 at a time in a round robin manner.
        'multicast'            : The reports are sent to all of the 
                                 destinations."
    DEFVAL          { redundancy } 
    ::= { cscRdrFormatterEntry 8 }
 


cscRdrDestTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CscRdrDestEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table lists the addresses of the configured RDR
        destination servers and the corresponding connection status for
        each destination.  The RDR formatter sends reports to one or
        more configured destinations that have a connection to the RDR
        formatter.
        This table also shows the current connection status of each
        destination."
    ::= { ciscoSCRdrMIBObjects 2 }

cscRdrDestEntry OBJECT-TYPE
    SYNTAX          CscRdrDestEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry contains the operational data and global counters
        for a connection between the RDR formatter destination and the
        RDR formatter associated with the service control entity
        identified by its assigned entPhysicalIndex.  An entry exists
        for each corresponding row in the entPhysicalTable having one
        of
        the following values assigned to entPhysicalVendorType:
            - cevChassisSCE2000
            - cevChassisSCE1000
            - cevNmeApaModule.

        Each connection between RDR formatter and RDR destination is
        uniquely identified by 'cscRdrDestIndex'."
    INDEX           {
                        entPhysicalIndex,
                        cscRdrDestIndex
                    } 
    ::= { cscRdrDestTable 1 }

CscRdrDestEntry ::= SEQUENCE {
        cscRdrDestIndex               Unsigned32,
        cscRdrDestInetAddressType     InetAddressType,
        cscRdrDestInetAddress         InetAddress,
        cscRdrDestPort                InetPortNumber,
        cscRdrDestPriority            Integer32,
        cscRdrDestStatus              INTEGER ,
        cscRdrDestConnectionStatus    INTEGER ,
        cscRdrDestNumSentReports      Counter32,
        cscRdrDestNumDiscardedReports Counter32,
        cscRdrDestReportRate          Gauge32
}

cscRdrDestIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4294967295 )
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A monotonically increasing integer for the sole purpose of
        indexing RDR destinations.  When it reaches the maximum value
        the agent flushes the table and wraps the value back to 1." 
    ::= { cscRdrDestEntry 1 }

cscRdrDestInetAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the type of Internet address by which
        the RDR destination server is reachable." 
    ::= { cscRdrDestEntry 2 }

cscRdrDestInetAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the RDR destination server IP Address." 
    ::= { cscRdrDestEntry 3 }

cscRdrDestPort OBJECT-TYPE
    SYNTAX          InetPortNumber
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the port on which the RDR destination
        server listens." 
    ::= { cscRdrDestEntry 4 }

cscRdrDestPriority OBJECT-TYPE
    SYNTAX          Integer32 (1..100 )
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the priority given to the RDR destination
        server.  The RDR formatter determines the priority of a
        destination by the value of entPhysicalIndex and the RDR
        category of the destination.  RDR formatter assigns the highest
        priority to the destination which has the same value of
        entPhysicalIndex and RDR category as that of the RDR formatter. 
        The RDR formatter activates the destination server which is
        reachable and with the highest priority." 
    ::= { cscRdrDestEntry 5 }

cscRdrDestStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        active(2),
                        standby(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the status of this RDR destination.

        'other'  :    None of the following.
        'active' :    The reports are sent to this destination.
        'standby':    This destination is a backup.

        Only one RDR destination can be 'active' if the
        cscRdrFormatterForwardingMode is set to either 'redundancy' or
        'simpleLoadBalancing'.  Multiple RDR destinations can be in
        'active' state when cscRdrFormatterForwardingMode is set to
        'multicast'." 
    ::= { cscRdrDestEntry 6 }

cscRdrDestConnectionStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        up(2),
                        down(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the status of the connection between the
        RDR formatter and this destination.
        'other'   : The connection is in some unknown state.
        'up'      : The RDR formatter can reach this destination.
        'down'    : The RDR formatter cannot reach this destination." 
    ::= { cscRdrDestEntry 7 }

cscRdrDestNumSentReports OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "reports"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of reports sent by the
        RDR formatter to this destination.

        Discontinuities in the value of this counter can occur at
        disabling/enabling of the RDR formatter, and at other times
        as indicated by the value of cscRdrCounterDiscontinuityTime." 
    ::= { cscRdrDestEntry 8 }

cscRdrDestNumDiscardedReports OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of reports dropped by the RDR
        formatter for this destination. 

        Discontinuities in the value of this counter can occur at
        disabling/enabling of the RDR formatter, and at other times
        as indicated by the value of cscRdrCounterDiscontinuityTime." 
    ::= { cscRdrDestEntry 9 }

cscRdrDestReportRate OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "reports per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the rate at which the RDR formatter is
        currently sending reports to this destinations." 
    ::= { cscRdrDestEntry 10 }
 


cscRdrCategoryTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CscRdrCategoryEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table describes the operational values and aggregated
        statistics of the different categories of the RDR Formatter."
    ::= { ciscoSCRdrMIBObjects 3 }

cscRdrCategoryEntry OBJECT-TYPE
    SYNTAX          CscRdrCategoryEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry contains the operational data and global counters
        for a category configured on a RDR formatter of a service
        control entity identified by the entPhysicalIndex in the
        ENTITY-MIB with the entPhysicalVendorType set to any of the
        following values:
        'cevChassisSCE2000'
        'cevChassisSCE1000'
        'cevNmeApaModule'."
    INDEX           {
                        entPhysicalIndex,
                        cscRdrCategoryIndex
                    } 
    ::= { cscRdrCategoryTable 1 }

CscRdrCategoryEntry ::= SEQUENCE {
        cscRdrCategoryIndex               Unsigned32,
        cscRdrCategoryID                  Unsigned32,
        cscRdrCategoryName                SnmpAdminString,
        cscRdrCategoryNumSentReports      Counter32,
        cscRdrCategoryNumDiscardedReports Counter32,
        cscRdrCategoryReportRate          Gauge32,
        cscRdrCategoryNumQueuedReports    Gauge32
}

cscRdrCategoryIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4 )
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the category number, index to the
        table." 
    ::= { cscRdrCategoryEntry 1 }

cscRdrCategoryID OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the unique id assigned to this RDR
        category by the RDR formatter." 
    ::= { cscRdrCategoryEntry 2 }

cscRdrCategoryName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the human readable name assigned to this
        RDR category by the RDR formatter.  The client application
        provides the RDR formatter with the value of this object." 
    ::= { cscRdrCategoryEntry 3 }

cscRdrCategoryNumSentReports OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "reports"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of RDR reports sent over this
        category.

        Discontinuities in the value of this counter can occur at
        disabling/enabling of the RDR formatter, and at other times
        as indicated by the value of cscRdrCounterDiscontinuityTime." 
    ::= { cscRdrCategoryEntry 4 }

cscRdrCategoryNumDiscardedReports OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "reports"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of RDR reports dropped for
        this category.

        Discontinuities in the value of this counter can occur at
        disabling/enabling of the RDR formatter, and at other times
        as indicated by the value of cscRdrCounterDiscontinuityTime." 
    ::= { cscRdrCategoryEntry 5 }

cscRdrCategoryReportRate OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "reports per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the rate at which the RDR formatter is
        currently sending reports over this category." 
    ::= { cscRdrCategoryEntry 6 }

cscRdrCategoryNumQueuedReports OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "reports"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of pending RDR reports within
        this category." 
    ::= { cscRdrCategoryEntry 7 }
 


cscRdrCategoryDestTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CscRdrCategoryDestEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table lists the operational data for RDR destination
        servers for each RDR category for a service control entity."
    ::= { ciscoSCRdrMIBObjects 4 }

cscRdrCategoryDestEntry OBJECT-TYPE
    SYNTAX          CscRdrCategoryDestEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry contains the operational data for a category of
        RDR formatter for a destination server of the service control
        entity identified by the entPhysicalIndex in the ENTITY-MIB with
        the entPhysicalVendorType set to any of the following values:
        'cevChassisSCE2000'
        'cevChassisSCE1000'
        'cevNmeApaModule'."
    INDEX           {
                        entPhysicalIndex,
                        cscRdrCategoryIndex,
                        cscRdrDestPort,
                        cscRdrDestInetAddress
                    } 
    ::= { cscRdrCategoryDestTable 1 }

CscRdrCategoryDestEntry ::= SEQUENCE {
        cscRdrCategoryDestPriority Integer32,
        cscRdrCategoryDestStatus   INTEGER 
}

cscRdrCategoryDestPriority OBJECT-TYPE
    SYNTAX          Integer32 (1..100 )
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the priority configured for this category
        on the RDR destination server.  The priority is determined by
        entPhysicalIndex and the category of the destination server." 
    ::= { cscRdrCategoryDestEntry 1 }

cscRdrCategoryDestStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        active(2),
                        standby(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the status of this RDR destination for
        this category. 

        'other'  :    None of the following.
        'active' :    The reports are sent to this destination.
        'standby':    This destination is a backup.

        Only one RDR destination can be 'active' if the
        cscRdrFormatterForwardingMode is set to either 'redundancy' or
        'simpleLoadBalancing'.  Multiple RDR destinations can be in
        'active' state when cscRdrFormatterForwardingMode is set to
        'multicast'." 
    ::= { cscRdrCategoryDestEntry 2 }
 

cscRdrNotifsConfig  OBJECT IDENTIFIER
    ::= { ciscoSCRdrMIBObjects 5 }


cscRdrCounterDiscontinuityTime OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The value of service up time on the most recent occasion at
        which any one or more of the RDR counters suffered a
        discontinuity.  If no such discontinuities have occurred since
        the last re-initialization of the local management subsystem,
        then this object contains a zero value." 
    ::= { ciscoSCRdrMIBObjects 6 }

cscRdrReportsEnableNotifs OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object controls whether the system produces notifications
        defined in thi MIB.  A 'false' value will prevent the
        notifications from being generated by this system." 
    ::= { cscRdrNotifsConfig 1 }

cscRdrCategoryStoppedDiscardingReportsTrap NOTIFICATION-TYPE
    OBJECTS         {
                        entPhysicalName,
                        cscRdrCategoryID
                    }
    STATUS          current
    DESCRIPTION
        "The system generates this notification to indicate that the
        system has recovered from congestion or unavailibility of the
        RDR collector identified by the value of cscRdrCategoryID and
        has stopped discarding reports being sent to this RDR
        collector."
   ::= { ciscoSCRdrMIBNotifs 1 }

cscRdrCategoryDiscardingReportsTrap NOTIFICATION-TYPE
    OBJECTS         {
                        entPhysicalName,
                        cscRdrCategoryID
                    }
    STATUS          current
    DESCRIPTION
        "The system generates this notification to indicate that the
        system has either encountered congestion or unavailibility of
        the RDR collector with the category identified by the value of
        cscRdrCategoryID and has started discarding reports destined to
        this collector.  The value of cscRdrCategoryNumReportsDiscarded
        indicates the number of discarded reports."
   ::= { ciscoSCRdrMIBNotifs 2 }

cscRdrNoActiveConnectionTrap NOTIFICATION-TYPE
    OBJECTS         { entPhysicalName }
    STATUS          current
    DESCRIPTION
        "The system generates this notification to indicate that there
        is no active connection between the RDR formatter and any
        collector."
   ::= { ciscoSCRdrMIBNotifs 3 }

cscRdrConnectionStatusDownTrap NOTIFICATION-TYPE
    OBJECTS         {
                        entPhysicalName,
                        cscRdrDestStatus,
                        cscRdrDestInetAddress,
                        cscRdrDestPort
                    }
    STATUS          current
    DESCRIPTION
        "The system generates this notification to indicate that a
        connection to destination has transitioned to the 'down' state."
   ::= { ciscoSCRdrMIBNotifs 4 }

cscRdrActiveConnectionTrap NOTIFICATION-TYPE
    OBJECTS         {
                        entPhysicalName,
                        cscRdrDestInetAddress,
                        cscRdrDestPort
                    }
    STATUS          current
    DESCRIPTION
        "The system generates this notification to indicate that a
        connection to the destination address cscRdrDestInetAddress has
        become active on TCP port cscRdrDestPort."
   ::= { ciscoSCRdrMIBNotifs 5 }

cscRdrConnectionStatusUpTrap NOTIFICATION-TYPE
    OBJECTS         {
                        entPhysicalName,
                        cscRdrDestStatus,
                        cscRdrDestInetAddress,
                        cscRdrDestPort
                    }
    STATUS          current
    DESCRIPTION
        "The system generates this notification to indicate that a
        connection to the destination address cscRdrDestInetAddress has
        become transitioned to 'up' state on TCP port cscRdrDestPort."
   ::= { ciscoSCRdrMIBNotifs 6 }
-- Conformance

cscRdrMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoSCRdrMIBConform 1 }

cscRdrMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoSCRdrMIBConform 2 }


cscRdrCompliance MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for SNMP Agents which implement this
        MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cscRdrObjectGroup,
                        cscRdrNotificationGroup,
                        cscRdrCounterDiscontinuityGroup
                    }

    GROUP           cscRdrNotifsControlGroup
    DESCRIPTION
        "This is optional group."
    ::= { cscRdrMIBCompliances 1 }

-- Units of Conformance

cscRdrObjectGroup OBJECT-GROUP
    OBJECTS         {
                        cscRdrFormatterEnable,
                        cscRdrFormatterNumSentReports,
                        cscRdrFormatterNumDiscardedReports,
                        cscRdrFormatterReportRate,
                        cscRdrFormatterProtocol,
                        cscRdrFormatterForwardingMode,
                        cscRdrDestInetAddressType,
                        cscRdrDestInetAddress,
                        cscRdrDestPort,
                        cscRdrDestPriority,
                        cscRdrDestStatus,
                        cscRdrDestConnectionStatus,
                        cscRdrDestNumSentReports,
                        cscRdrDestNumDiscardedReports,
                        cscRdrDestReportRate,
                        cscRdrCategoryName,
                        cscRdrCategoryNumSentReports,
                        cscRdrCategoryNumDiscardedReports,
                        cscRdrCategoryReportRate,
                        cscRdrCategoryNumQueuedReports,
                        cscRdrCategoryDestPriority,
                        cscRdrCategoryDestStatus,
                        cscRdrFormatterReportRatePeak,
                        cscRdrFormatterReportRatePeakTime,
                        cscRdrCategoryID
                    }
    STATUS          current
    DESCRIPTION
        "This group of objects maintains informative data for RDRs."
    ::= { cscRdrMIBGroups 1 }

cscRdrNotificationGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        cscRdrActiveConnectionTrap,
                        cscRdrCategoryStoppedDiscardingReportsTrap,
                        cscRdrCategoryDiscardingReportsTrap,
                        cscRdrNoActiveConnectionTrap,
                        cscRdrConnectionStatusDownTrap,
                        cscRdrConnectionStatusUpTrap
                    }
    STATUS          current
    DESCRIPTION
        "This group contains notifications for this MIB."
    ::= { cscRdrMIBGroups 2 }

cscRdrNotifsControlGroup OBJECT-GROUP
    OBJECTS         { cscRdrReportsEnableNotifs }
    STATUS          current
    DESCRIPTION
        "This is a collection of objects to control the enable/disable
        state of notification generation."
    ::= { cscRdrMIBGroups 3 }

cscRdrCounterDiscontinuityGroup OBJECT-GROUP
    OBJECTS         { cscRdrCounterDiscontinuityTime }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing information specific to
        RDR counter discontinuities."
    ::= { cscRdrMIBGroups 4 }

END



