LLDP-EXT-DOT1-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Integer32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    TruthValue
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    lldpExtensions,
    lldpLocPortNum,
    lldpRemTimeMark,
    lldpRemLocalPortNum,
    lldpRemIndex,
    lldpPortConfigEntry
        FROM LLDP-MIB
    VlanId
        FROM Q-BRIDGE-MIB;


lldpXdot1MIB MODULE-IDENTITY
    LAST-UPDATED    "200505060000Z"
    ORGANIZATION    "IEEE 802.1 Working Group"
    CONTACT-INFO
            "WG-URL: http://grouper.ieee.org/groups/802/1/index.html
            WG-EMail: stds-802-1@ieee.org

             Contact: Paul Congdon
              Postal: Hewlett-Packard Company
                      8000 Foothills Blvd. 
                      Roseville, CA 95747
                      USA
                 Tel: +1-916-785-5753
              E-mail: paul_congdon@hp.com"
    DESCRIPTION
        "The LLDP Management Information Base extension module for
        IEEE 802.1 organizationally defined discovery information.

        In order to assure the uniqueness of the LLDP-MIB,
        lldpXdot1MIB is branched from lldpExtensions using OUI value
        as the node.  An OUI/'company_id' is a 24 bit globally unique
        assigned number referenced by various standards.

        Copyright (C) IEEE (2005).  This version of this MIB module
        is published as Annex F.7.1 of IEEE Std 802.1AB-2005;
        see the standard itself for full legal notices."
    REVISION        "200505060000Z"
    DESCRIPTION
        "Published as part of IEEE Std 802.1AB-2005 initial version."
    ::= { lldpExtensions 32962 }


-- ----------------------------------------------------------------------------
-- ----------------------------------------------------------------------------
--   
-- Organizationally Defined Information Extension - IEEE 802.1
--   
-- ----------------------------------------------------------------------------
-- ----------------------------------------------------------------------------

lldpXdot1Objects  OBJECT IDENTIFIER
    ::= { lldpXdot1MIB 1 }

-- LLDP IEEE 802.1 extension MIB groups

lldpXdot1Config  OBJECT IDENTIFIER
    ::= { lldpXdot1Objects 1 }

lldpXdot1LocalData  OBJECT IDENTIFIER
    ::= { lldpXdot1Objects 2 }

lldpXdot1RemoteData  OBJECT IDENTIFIER
    ::= { lldpXdot1Objects 3 }

-- ----------------------------------------------------------------------------
-- IEEE 802.1 - Configuration
-- ----------------------------------------------------------------------------
--   
-- lldpXdot1ConfigPortVlanTable : configure the transmission of the
-- Port VLAN-ID TLVs on set of ports.

lldpXdot1ConfigPortVlanTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF LldpXdot1ConfigPortVlanEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table that controls selection of LLDP Port VLAN-ID TLVs
        to be transmitted on individual ports."
    ::= { lldpXdot1Config 1 }

lldpXdot1ConfigPortVlanEntry OBJECT-TYPE
    SYNTAX          LldpXdot1ConfigPortVlanEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "LLDP configuration information that controls the
        transmission of IEEE 802.1 organizationally defined Port
        VLAN-ID TLV on LLDP transmission capable ports.

        This configuration object augments the lldpPortConfigEntry of
        the LLDP-MIB, therefore it is only present along with the port
        configuration defined by the associated lldpPortConfigEntry
        entry.

        Each active lldpConfigEntry must be restored from non-volatile
        storage (along with the corresponding lldpPortConfigEntry)
        after a re-initialization of the management system."
    AUGMENTS           { lldpPortConfigEntry  } 
    ::= { lldpXdot1ConfigPortVlanTable 1 }

LldpXdot1ConfigPortVlanEntry ::= SEQUENCE {
        lldpXdot1ConfigPortVlanTxEnable TruthValue
}

lldpXdot1ConfigPortVlanTxEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The lldpXdot1ConfigPortVlanTxEnable, which is defined as
        a truth value and configured by the network management,
        determines whether the IEEE 802.1 organizationally defined
        port VLAN TLV transmission is allowed on a given LLDP
        transmission capable port.

        The value of this object must be restored from non-volatile
        storage after a re-initialization of the management system."
    REFERENCE       "IEEE 802.1AB-2005 10.2.1.1"
    DEFVAL          { false } 
    ::= { lldpXdot1ConfigPortVlanEntry 1 }
 

-- lldpXdot1ConfigVlanNameTable : configure the transmission of the
-- VLAN name instances on set of ports.

lldpXdot1ConfigVlanNameTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF LldpXdot1ConfigVlanNameEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table that controls selection of LLDP VLAN name TLV
        instances to be transmitted on individual ports."
    ::= { lldpXdot1Config 2 }

lldpXdot1ConfigVlanNameEntry OBJECT-TYPE
    SYNTAX          LldpXdot1ConfigVlanNameEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "LLDP configuration information that specifies the set of
        ports (represented as a PortList) on which the Local System
        VLAN name instance will be transmitted.

        This configuration object augments the lldpLocVlanEntry,
        therefore it is only present along with the VLAN Name instance
        contained in the associated lldpLocVlanNameEntry entry.

        Each active lldpXdot1ConfigVlanNameEntry must be restored
        from non-volatile storage (along with the corresponding
        lldpXdot1LocVlanNameEntry) after a re-initialization of the
        management system."
    AUGMENTS           { lldpXdot1LocVlanNameEntry  } 
    ::= { lldpXdot1ConfigVlanNameTable 1 }

LldpXdot1ConfigVlanNameEntry ::= SEQUENCE {
        lldpXdot1ConfigVlanNameTxEnable TruthValue
}

lldpXdot1ConfigVlanNameTxEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The boolean value that indicates whether the corresponding
        Local System VLAN name instance will be transmitted on the
        port defined by the given lldpXdot1LocVlanNameEntry.

        The value of this object must be restored from non-volatile
        storage after a re-initialization of the management system."
    REFERENCE       "IEEE 802.1AB-2005 10.2.1.1"
    DEFVAL          { false } 
    ::= { lldpXdot1ConfigVlanNameEntry 1 }
 

-- lldpXdot1ConfigProtoVlanTable : configure the transmission of the
-- protocol VLAN instances on set
-- of ports.

lldpXdot1ConfigProtoVlanTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF LldpXdot1ConfigProtoVlanEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table that controls selection of LLDP Port and Protocol
        VLAN ID TLV instances to be transmitted on individual ports."
    ::= { lldpXdot1Config 3 }

lldpXdot1ConfigProtoVlanEntry OBJECT-TYPE
    SYNTAX          LldpXdot1ConfigProtoVlanEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "LLDP configuration information that specifies the set of
        ports (represented as a PortList) on which the Local System
        Protocol VLAN instance will be transmitted.

        This configuration object augments the lldpXdot1LocVlanEntry,
        therefore it is only present along with the Port and
        Protocol VLAN ID instance contained in the associated
        lldpXdot1LocVlanEntry entry.

        Each active lldpXdot1ConfigProtoVlanEntry must be restored
        from non-volatile storage (along with the corresponding
        lldpXdot1LocProtoVlanEntry) after a re-initialization of
        the management system."
    AUGMENTS           { lldpXdot1LocProtoVlanEntry  } 
    ::= { lldpXdot1ConfigProtoVlanTable 1 }

LldpXdot1ConfigProtoVlanEntry ::= SEQUENCE {
        lldpXdot1ConfigProtoVlanTxEnable TruthValue
}

lldpXdot1ConfigProtoVlanTxEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The boolean value that indicates whether the corresponding
        Local System Port and Protocol VLAN instance will
        be transmitted on the port defined by the given
        lldpXdot1LocProtoVlanEntry.

        The value of this object must be restored from non-volatile
        storage after a re-initialization of the management system."
    REFERENCE       "IEEE 802.1AB-2005 10.2.1.1"
    DEFVAL          { false } 
    ::= { lldpXdot1ConfigProtoVlanEntry 1 }
 

-- lldpXdot1ConfigProtocolTable : configure the transmission of the
-- protocol instances on set
-- of ports.

lldpXdot1ConfigProtocolTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF LldpXdot1ConfigProtocolEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table that controls selection of LLDP Protocol
        TLV instances to be transmitted on individual ports."
    ::= { lldpXdot1Config 4 }

lldpXdot1ConfigProtocolEntry OBJECT-TYPE
    SYNTAX          LldpXdot1ConfigProtocolEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "LLDP configuration information that specifies the set of
        ports (represented as a PortList) on which the Local System
        Protocol instance will be transmitted.

        This configuration object augments the lldpXdot1LocProtoEntry,
        therefore it is only present along with the Protocol instance
        contained in the associated lldpXdot1LocProtoEntry entry.

        Each active lldpXdot1ConfigProtocolEntry must be restored
        from non-volatile storage (along with the corresponding
        lldpXdot1LocProtocolEntry) after a re-initialization of the
        management system."
    AUGMENTS           { lldpXdot1LocProtocolEntry  } 
    ::= { lldpXdot1ConfigProtocolTable 1 }

LldpXdot1ConfigProtocolEntry ::= SEQUENCE {
        lldpXdot1ConfigProtocolTxEnable TruthValue
}

lldpXdot1ConfigProtocolTxEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The boolean value that indicates whether the corresponding
        Local System Protocol Identity instance will be transmitted
        on the port defined by the given lldpXdot1LocProtocolEntry.

        The value of this object must be restored from non-volatile
        storage after a re-initialization of the management system."
    REFERENCE       "IEEE 802.1AB-2005 10.2.1.1"
    DEFVAL          { false } 
    ::= { lldpXdot1ConfigProtocolEntry 1 }
 

-- ----------------------------------------------------------------------------
-- IEEE 802.1 - Local System Information
-- ----------------------------------------------------------------------------

lldpXdot1LocTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF LldpXdot1LocEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains one row per port for IEEE 802.1
        organizationally defined LLDP extension on the local system
        known to this agent."
    ::= { lldpXdot1LocalData 1 }

lldpXdot1LocEntry OBJECT-TYPE
    SYNTAX          LldpXdot1LocEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Information about IEEE 802.1 organizationally defined
        LLDP extension."
    INDEX           { lldpLocPortNum } 
    ::= { lldpXdot1LocTable 1 }

LldpXdot1LocEntry ::= SEQUENCE {
        lldpXdot1LocPortVlanId Integer32
}

lldpXdot1LocPortVlanId OBJECT-TYPE
    SYNTAX          Integer32 (0 | 1..4094)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The integer value used to identify the port's VLAN identifier
        associated with the local system.   A value of zero shall
        be used if the system either does not know the PVID or does
        not support port-based VLAN operation."
    REFERENCE       "IEEE 802.1AB-2005 F.2.1" 
    ::= { lldpXdot1LocEntry 1 }
 

-- lldpXdot1LocProtoVlanTable: Port and Protocol VLAN information

lldpXdot1LocProtoVlanTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF LldpXdot1LocProtoVlanEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains one or more rows per Port and Protocol
        VLAN information about the local system."
    ::= { lldpXdot1LocalData 2 }

lldpXdot1LocProtoVlanEntry OBJECT-TYPE
    SYNTAX          LldpXdot1LocProtoVlanEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Port and protocol VLAN ID Information about a particular
        port component.  There may be multiple port and protocol VLANs,
        identified by a particular lldpXdot1LocProtoVlanId, configured
        on the given port."
    INDEX           {
                        lldpLocPortNum,
                        lldpXdot1LocProtoVlanId
                    } 
    ::= { lldpXdot1LocProtoVlanTable 1 }

LldpXdot1LocProtoVlanEntry ::= SEQUENCE {
        lldpXdot1LocProtoVlanId        Integer32,
        lldpXdot1LocProtoVlanSupported TruthValue,
        lldpXdot1LocProtoVlanEnabled   TruthValue
}

lldpXdot1LocProtoVlanId OBJECT-TYPE
    SYNTAX          Integer32 (0 | 1..4094)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The integer value used to identify the port and protocol
        VLANs associated with the given port associated with the
        local system.  A value of zero shall be used if the system
        either does not know the protocol VLAN ID (PPVID) or does
        not support port and protocol VLAN operation."
    REFERENCE       "IEEE 802.1AB-2005 F.3.2" 
    ::= { lldpXdot1LocProtoVlanEntry 1 }

lldpXdot1LocProtoVlanSupported OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The truth value used to indicate whether the given port
        (associated with the local system) supports port and protocol
        VLANs."
    REFERENCE       "IEEE 802.1AB-2005 F.3.1" 
    ::= { lldpXdot1LocProtoVlanEntry 2 }

lldpXdot1LocProtoVlanEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The truth value used to indicate whether the port and
        protocol VLANs are enabled on the given port associated with
        the local system."
    REFERENCE       "IEEE 802.1AB-2005 F.3.1" 
    ::= { lldpXdot1LocProtoVlanEntry 3 }
 

-- lldpXdot1LocVlanNameTable : VLAN name information about the local system

lldpXdot1LocVlanNameTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF LldpXdot1LocVlanNameEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains one or more rows per IEEE 802.1Q VLAN
        name information on the local system known to this agent."
    ::= { lldpXdot1LocalData 3 }

lldpXdot1LocVlanNameEntry OBJECT-TYPE
    SYNTAX          LldpXdot1LocVlanNameEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "VLAN name Information about a particular port component.
        There may be multiple VLANs, identified by a particular
        lldpXdot1LocVlanId, configured on the given port."
    INDEX           {
                        lldpLocPortNum,
                        lldpXdot1LocVlanId
                    } 
    ::= { lldpXdot1LocVlanNameTable 1 }

LldpXdot1LocVlanNameEntry ::= SEQUENCE {
        lldpXdot1LocVlanId   VlanId,
        lldpXdot1LocVlanName SnmpAdminString
}

lldpXdot1LocVlanId OBJECT-TYPE
    SYNTAX          VlanId
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The integer value used to identify the IEEE 802.1Q
        VLAN IDs with which the given port is compatible."
    REFERENCE       "IEEE 802.1AB-2005 F.4.2" 
    ::= { lldpXdot1LocVlanNameEntry 1 }

lldpXdot1LocVlanName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The string value used to identify VLAN name identified by the
        Vlan Id associated with the given port on the local system.

        This object should contain the value of the dot1QVLANStaticName
        object (defined in IETF RFC 2674) identified with the given
        lldpXdot1LocVlanId."
    REFERENCE       "IEEE 802.1AB-2005 F.4.4" 
    ::= { lldpXdot1LocVlanNameEntry 2 }
 

-- lldpXdot1LocProtocolTable : Protocol Identity information

lldpXdot1LocProtocolTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF LldpXdot1LocProtocolEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains one or more rows per protocol identity
        information on the local system known to this agent."
    REFERENCE       "IEEE 802.1AB-2005 F.5"
    ::= { lldpXdot1LocalData 4 }

lldpXdot1LocProtocolEntry OBJECT-TYPE
    SYNTAX          LldpXdot1LocProtocolEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Information about particular protocols that are accessible
        through the given port component.

        There may be multiple protocols, identified by particular
        lldpXdot1ProtocolIndex, and lldpLocPortNum."
    REFERENCE       "IEEE 802.1AB-2005 F.5"
    INDEX           {
                        lldpLocPortNum,
                        lldpXdot1LocProtocolIndex
                    } 
    ::= { lldpXdot1LocProtocolTable 1 }

LldpXdot1LocProtocolEntry ::= SEQUENCE {
        lldpXdot1LocProtocolIndex Integer32,
        lldpXdot1LocProtocolId    OCTET STRING
}

lldpXdot1LocProtocolIndex OBJECT-TYPE
    SYNTAX          Integer32 (1..2147483647)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents an arbitrary local integer value used
        by this agent to identify a particular protocol identity." 
    ::= { lldpXdot1LocProtocolEntry 1 }

lldpXdot1LocProtocolId OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (1..255))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The octet string value used to identify the protocols
        associated with the given port of the local system."
    REFERENCE       "IEEE 802.1AB-2005 F.5.3" 
    ::= { lldpXdot1LocProtocolEntry 2 }
 

-- ----------------------------------------------------------------------------
-- IEEE 802.1 - Remote System Information
-- ----------------------------------------------------------------------------

lldpXdot1RemTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF LldpXdot1RemEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains one or more rows per physical network
        connection known to this agent.  The agent may wish to
        ensure that only one lldpXdot1RemEntry is present for
        each local port, or it may choose to maintain multiple
        lldpXdot1RemEntries for the same local port."
    ::= { lldpXdot1RemoteData 1 }

lldpXdot1RemEntry OBJECT-TYPE
    SYNTAX          LldpXdot1RemEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Information about a particular port component."
    INDEX           {
                        lldpRemTimeMark,
                        lldpRemLocalPortNum,
                        lldpRemIndex
                    } 
    ::= { lldpXdot1RemTable 1 }

LldpXdot1RemEntry ::= SEQUENCE {
        lldpXdot1RemPortVlanId Integer32
}

lldpXdot1RemPortVlanId OBJECT-TYPE
    SYNTAX          Integer32 (0 | 1..4094)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The integer value used to identify the port's VLAN identifier
        associated with the remote system.  if the remote system
        either does not know the PVID or does not support port-based
        VLAN operation, the value of lldpXdot1RemPortVlanId should
        be zero."
    REFERENCE       "IEEE 802.1AB-2005 F.2.1" 
    ::= { lldpXdot1RemEntry 1 }
 


lldpXdot1RemProtoVlanTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF LldpXdot1RemProtoVlanEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains one or more rows per Port and Protocol
        VLAN information about the remote system, received on the
        given port."
    ::= { lldpXdot1RemoteData 2 }

lldpXdot1RemProtoVlanEntry OBJECT-TYPE
    SYNTAX          LldpXdot1RemProtoVlanEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Port and protocol VLAN name Information about a particular
        port component.  There may be multiple protocol VLANs,
        identified by a particular lldpXdot1RemProtoVlanId, configured
        on the remote system."
    INDEX           {
                        lldpRemTimeMark,
                        lldpRemLocalPortNum,
                        lldpRemIndex,
                        lldpXdot1RemProtoVlanId
                    } 
    ::= { lldpXdot1RemProtoVlanTable 1 }

LldpXdot1RemProtoVlanEntry ::= SEQUENCE {
        lldpXdot1RemProtoVlanId        Integer32,
        lldpXdot1RemProtoVlanSupported TruthValue,
        lldpXdot1RemProtoVlanEnabled   TruthValue
}

lldpXdot1RemProtoVlanId OBJECT-TYPE
    SYNTAX          Integer32 (0 | 1..4094)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The integer value used to identify the port and protocol
        VLANs associated with the given port associated with the
        remote system.

        If port and protocol VLANs are not supported on the given
        port associated with the remote system, or if the port is
        not enabled with any port and protocol VLAN, the value of
        lldpXdot1RemProtoVlanId should be zero."
    REFERENCE       "IEEE 802.1AB-2005 F.3.2" 
    ::= { lldpXdot1RemProtoVlanEntry 1 }

lldpXdot1RemProtoVlanSupported OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The truth value used to indicate whether the given port
        (associated with the remote system) is capable of supporting
        port and protocol VLANs."
    REFERENCE       "IEEE 802.1AB-2005 F.3.1" 
    ::= { lldpXdot1RemProtoVlanEntry 2 }

lldpXdot1RemProtoVlanEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The truth value used to indicate whether the port and
        protocol VLANs are enabled on the given port associated with
        the remote system."
    REFERENCE       "IEEE 802.1AB-2005 F.3.1" 
    ::= { lldpXdot1RemProtoVlanEntry 3 }
 

-- lldpXdot1RemVlanNameTable : VLAN name information of the remote
-- systems

lldpXdot1RemVlanNameTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF LldpXdot1RemVlanNameEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains one or more rows per IEEE 802.1Q VLAN
        name information about the remote system, received on the
        given port."
    REFERENCE       "IEEE 802.1AB-2005 F.4"
    ::= { lldpXdot1RemoteData 3 }

lldpXdot1RemVlanNameEntry OBJECT-TYPE
    SYNTAX          LldpXdot1RemVlanNameEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "VLAN name Information about a particular port component.
        There may be multiple VLANs, identified by a particular
        lldpXdot1RemVlanId, received on the given port."
    INDEX           {
                        lldpRemTimeMark,
                        lldpRemLocalPortNum,
                        lldpRemIndex,
                        lldpXdot1RemVlanId
                    } 
    ::= { lldpXdot1RemVlanNameTable 1 }

LldpXdot1RemVlanNameEntry ::= SEQUENCE {
        lldpXdot1RemVlanId   VlanId,
        lldpXdot1RemVlanName SnmpAdminString
}

lldpXdot1RemVlanId OBJECT-TYPE
    SYNTAX          VlanId
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The integer value used to identify the IEEE 802.1Q
        VLAN IDs with which the given port of the remote system
        is compatible."
    REFERENCE       "IEEE 802.1AB-2005 F.4.2" 
    ::= { lldpXdot1RemVlanNameEntry 1 }

lldpXdot1RemVlanName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The string value used to identify VLAN name identified by the
        VLAN Id associated with the remote system."
    REFERENCE       "IEEE 802.1AB-2005 F.4.4" 
    ::= { lldpXdot1RemVlanNameEntry 2 }
 

-- lldpXdot1RemProtocolTable : Protocol information of the remote systems

lldpXdot1RemProtocolTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF LldpXdot1RemProtocolEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains one or more rows per protocol information
        about the remote system, received on the given port."
    ::= { lldpXdot1RemoteData 4 }

lldpXdot1RemProtocolEntry OBJECT-TYPE
    SYNTAX          LldpXdot1RemProtocolEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Protocol information about a particular port component.
        There may be multiple protocols, identified by a particular
        lldpXdot1ProtocolIndex, received on the given port."
    INDEX           {
                        lldpRemTimeMark,
                        lldpRemLocalPortNum,
                        lldpRemIndex,
                        lldpXdot1RemProtocolIndex
                    } 
    ::= { lldpXdot1RemProtocolTable 1 }

LldpXdot1RemProtocolEntry ::= SEQUENCE {
        lldpXdot1RemProtocolIndex Integer32,
        lldpXdot1RemProtocolId    OCTET STRING
}

lldpXdot1RemProtocolIndex OBJECT-TYPE
    SYNTAX          Integer32 (1..2147483647)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents an arbitrary local integer value used
        by this agent to identify a particular protocol identity." 
    ::= { lldpXdot1RemProtocolEntry 1 }

lldpXdot1RemProtocolId OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (1..255))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The octet string value used to identify the protocols
        associated with the given port of remote system."
    REFERENCE       "IEEE 802.1AB-2005 F.5.3" 
    ::= { lldpXdot1RemProtocolEntry 2 }
 

-- ----------------------------------------------------------------------------
-- Conformance Information
-- ----------------------------------------------------------------------------

lldpXdot1Conformance  OBJECT IDENTIFIER
    ::= { lldpXdot1MIB 2 }

lldpXdot1Compliances  OBJECT IDENTIFIER
    ::= { lldpXdot1Conformance 1 }

lldpXdot1Groups  OBJECT IDENTIFIER
    ::= { lldpXdot1Conformance 2 }


-- compliance statements

lldpXdot1Compliance MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for SNMP entities which implement
        the IEEE 802.1 organizationally defined LLDP extension MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        lldpXdot1ConfigGroup,
                        lldpXdot1LocSysGroup,
                        lldpXdot1RemSysGroup
                    }
    ::= { lldpXdot1Compliances 1 }

-- MIB groupings

lldpXdot1ConfigGroup OBJECT-GROUP
    OBJECTS         {
                        lldpXdot1ConfigPortVlanTxEnable,
                        lldpXdot1ConfigVlanNameTxEnable,
                        lldpXdot1ConfigProtoVlanTxEnable,
                        lldpXdot1ConfigProtocolTxEnable
                    }
    STATUS          current
    DESCRIPTION
        "The collection of objects which are used to configure the
        IEEE 802.1 organizationally defined LLDP extension
        implementation behavior.

        This group is mandatory for agents which implement the 
        IEEE 802.1 organizationally defined LLDP extension."
    ::= { lldpXdot1Groups 1 }

lldpXdot1LocSysGroup OBJECT-GROUP
    OBJECTS         {
                        lldpXdot1LocPortVlanId,
                        lldpXdot1LocProtoVlanSupported,
                        lldpXdot1LocProtoVlanEnabled,
                        lldpXdot1LocVlanName,
                        lldpXdot1LocProtocolId
                    }
    STATUS          current
    DESCRIPTION
        "The collection of objects which are used to represent
        IEEE 802.1 organizationally defined LLDP extension associated
        with the Local Device Information.

        This group is mandatory for agents which implement the 
        IEEE 802.1 organizationally defined LLDP extension in the
        TX mode."
    ::= { lldpXdot1Groups 2 }

lldpXdot1RemSysGroup OBJECT-GROUP
    OBJECTS         {
                        lldpXdot1RemPortVlanId,
                        lldpXdot1RemProtoVlanSupported,
                        lldpXdot1RemProtoVlanEnabled,
                        lldpXdot1RemVlanName,
                        lldpXdot1RemProtocolId
                    }
    STATUS          current
    DESCRIPTION
        "The collection of objects which are used to represent LLDP
        802.1 organizational extension Local Device Information.

        This group is mandatory for agents which implement the 
        LLDP 802.1 organizational extension in the RX mode."
    ::= { lldpXdot1Groups 3 }

END



