-- *****************************************************************
-- CISCO-IP-CBR-METRICS-MIB
-- Definitions of managed objects describing MDI flow metrics.
--   
-- October 2009, Patrick R. Gili
--   
-- Copyright (c) 2008-2009 by Cisco Systems Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-IP-CBR-METRICS-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-IDENTITY,
    OBJECT-TYPE,
    Counter64,
    Unsigned32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    TimeStamp
        FROM SNMPv2-TC
    ReportIntervalCount
        FROM CISCO-REPORT-INTERVAL-TC-MIB
    FlowCfgRateType,
    FlowBitRateUnits,
    FlowMetricScale,
    FlowMetricPrecision,
    FlowMetricValue
        FROM CISCO-FLOW-MONITOR-TC-MIB
    cfmFlowMonitorId,
    cfmFlowId,
    cfmFlowMetricsIntNumber
        FROM CISCO-FLOW-MONITOR-MIB
    ciscoMgmt
        FROM CISCO-SMI;


ciscoIpCbrMetricsMIB MODULE-IDENTITY
    LAST-UPDATED    "200906110000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal:  170 W Tasman Drive
            San Jose, CA 95134

            Tel:  +1 800 553-NETS

            E-mail:  cs-snmp@cisco.com"
    DESCRIPTION
        "This MIB module defines objects that describe the a set of
        metrics used to measure the quality of a IP CBR traffic flow. An
        IP CBR traffic flow consists of a stream of IP datagrams sent
        from one application to another with a constant packet rate or
        bit rate.

        GLOSSARY
        ============

        CBR - Constant Bit Rate.

        Delay Factor - the maximum observed value of the flow rate
            imbalance over a measurement interval.

        DF - Delay Factor.

        Flow Monitor - a hardware or software entity that classifies
            traffic flows, collects flow data, and periodically
            computes flow metrics.

        Flow Metric - a measurement that reflects the quality of a
            traffic flow.

        Measurement Interval - the length of time over which a flow
            monitor collects data related to a traffic flow, after which
            the flow monitor computes flow metrics using the collected
            data.

        Media Rate - the effective bit rate of the media content
            carried by a traffic flow.

        Media Rate Variation - a measure of loss (in bytes):

                         N
                   RT - sum [Si]
                        i=1
            MRV = ---------------
                         RT

            where R is the nominal media rate, T is the measurement
            interval, Si is the size of packet[i] received during the
            measurement interval, and N is the number of media packets
            received during the measurement interval.

        MR - Media Rate.

        MRV - Media Rate Variation.

        Traffic Flow - a unidirectional stream of packets conforming to
            a classifier.  For example, packets having a particular 
            source IP address, destination IP address, protocol type,
            source port number, and destination port number.

        VB - Virtual Buffer.

        Virtual Buffer - a virtual buffer is a construct used to
            simulate a real buffer used by a media application for the
            purpose of storing media packets until the the application
            can render their content."
    REVISION        "200906110000Z"
    DESCRIPTION
        "The initial version of the MIB module."
    ::= { ciscoMgmt 697 }


-- **********************************************************************
-- * Top-Level Trees                                                    *
-- **********************************************************************

ciscoIpCbrMetricsMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoIpCbrMetricsMIB 0 }

ciscoIpCbrMetricsMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoIpCbrMetricsMIB 1 }

ciscoIpCbrMetricsMIBConform  OBJECT IDENTIFIER
    ::= { ciscoIpCbrMetricsMIB 2 }

ciscoIpCbrMetricsMIBIds  OBJECT IDENTIFIER
    ::= { ciscoIpCbrMetricsMIB 3 }

-- **********************************************************************
-- * Objects                                                            *
-- **********************************************************************

cfmIpCbrMetrics  OBJECT IDENTIFIER
    ::= { ciscoIpCbrMetricsMIBObjects 1 }


cfmIpCbrMetricsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CfmIpCbrMetricsEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains aggregate data maintained by a flow
        monitor for traffic flows for which it is computing IP CBR
        metrics.

        This table has an sparse dependent relationship on the
        cfmFlowMetricsTable (defined by the CISCO-FLOW-MONITOR-MIB),
        containing a row for each row in the cfmFlowMetricsTable having
        a corresponding instance of cfmFlowMetricsCollected with the
        'ipCbr' bit set to one."
    ::= { cfmIpCbrMetrics 1 }

cfmIpCbrMetricsEntry OBJECT-TYPE
    SYNTAX          CfmIpCbrMetricsEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry describes cumulative and aggregate IP CBR metrics for
        a single traffic flow.

        The devices creates a row in the cfmIpCbrMetricsTable when a
        flow monitor starts monitoring a traffic flow and has been
        configured to compute IP CBR metrics for the same traffic flow.
        Likewise, the device destroys a row in the
        cfmIpCbrMetricsMetricsTable when the corresponding flow monitor
        has ceased monitoring the traffic flow (e.g., when a traffic
        flow has timed out)."
    INDEX           {
                        cfmFlowMonitorId,
                        cfmFlowId
                    } 
    ::= { cfmIpCbrMetricsTable 1 }

CfmIpCbrMetricsEntry ::= SEQUENCE {
        cfmIpCbrMetricsCfgRateType     FlowCfgRateType,
        cfmIpCbrMetricsCfgBitRate      FlowBitRateUnits,
        cfmIpCbrMetricsCfgRate         Unsigned32,
        cfmIpCbrMetricsCfgMediaPktSize Unsigned32,
        cfmIpCbrMetricsValid           BITS,
        cfmIpCbrMetricsLostPkts        Counter64,
        cfmIpCbrMetricsMrvScale        FlowMetricScale,
        cfmIpCbrMetricsMrvPrecision    FlowMetricPrecision,
        cfmIpCbrMetricsMrv             FlowMetricValue
}

cfmIpCbrMetricsCfgRateType OBJECT-TYPE
    SYNTAX          FlowCfgRateType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates how the corresponding flow monitor
        computes the DF for the traffic flow." 
    ::= { cfmIpCbrMetricsEntry 1 }

cfmIpCbrMetricsCfgBitRate OBJECT-TYPE
    SYNTAX          FlowBitRateUnits
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the units for the corresponding instance
        of cfmIpCbrMetricsCfgRate.  The value of this column only has
        relevance if the corresponding instance of
        cfmIpCbrMetricsCfgRateType is 'ipBitRate' or 'mediaRate'." 
    ::= { cfmIpCbrMetricsEntry 2 }

cfmIpCbrMetricsCfgRate OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4294967295)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the configured bit rate used by the flow
        monitor to compute the DF for the traffic flow.  The value of
        this column only has relevance if the corresponding instance of
        cfmIpCbrMetricsCfgRateType is 'ipBitRate' or 'mediaRate'." 
    ::= { cfmIpCbrMetricsEntry 3 }

cfmIpCbrMetricsCfgMediaPktSize OBJECT-TYPE
    SYNTAX          Unsigned32 (64..65535)
    UNITS           "octets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the configured media packet size used by
        the flow monitor to compute the DF for the traffic flow.  The
        value of this column only has relevance if the corresponding
        instance of cfmIpCbrMetricsCfgRateType is 'mediaRate'." 
    ::= { cfmIpCbrMetricsEntry 4 }

cfmIpCbrMetricsValid OBJECT-TYPE
    SYNTAX          BITS {
                        lostPkts(0),
                        mediaRateVariation(1)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates which metrics are valid for the traffic
        flow:

            'lostPkts'
                If this bit is set to '1', then the corresponding
                instance of cfmIpCbrMetricsLostPkts is valid.

            'mediaRateVariation'
                If this bit is set to '1', then the corresponding
                instances of cfmIpCbrMetricsMlrScale,
                cfmIpCbrMetricsMlrPrecision, and cfmIpCbrMetricsMlr are
                valid." 
    ::= { cfmIpCbrMetricsEntry 5 }

cfmIpCbrMetricsLostPkts OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of packets lost for the
        traffic flow.

        The value of this column is valid if and only if the 'lostPkts'
        bit in the corresponding instance of cfmMdiMetricsValid is set
        to '1'." 
    ::= { cfmIpCbrMetricsEntry 6 }

cfmIpCbrMetricsMrvScale OBJECT-TYPE
    SYNTAX          FlowMetricScale
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the scale factor for the corresponding
        instance of cfmIpCbrMetricsMrv.

        The value of this column is valid if and only if the
        'mediaRateVariation' bit in the corresponding instance of
        cfmMdiMetricsValid is set to '1'." 
    ::= { cfmIpCbrMetricsEntry 7 }

cfmIpCbrMetricsMrvPrecision OBJECT-TYPE
    SYNTAX          FlowMetricPrecision
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the precision for the corresponding
        instance of cfmIpCbrMetricsMrv.

        The value of this column is valid if and only if the
        'mediaRateVariation' bit in the corresponding instance of
        cfmMdiMetricsValid is set to '1'." 
    ::= { cfmIpCbrMetricsEntry 8 }

cfmIpCbrMetricsMrv OBJECT-TYPE
    SYNTAX          FlowMetricValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the MRV for the traffic flow since the
        flow monitor started collecting data for the traffic flow.

        The value of this column is valid if and only if the
        'mediaRateVariation' bit in the corresponding instance of
        cfmMdiMetricsValid is set to '1'." 
    ::= { cfmIpCbrMetricsEntry 9 }
 


cfmIpCbrMetricsTableChanged OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the value of sysUpTime the last time the
        device created/destroyed a row in the cfmIpCbrMetricsTable." 
    ::= { cfmIpCbrMetrics 2 }

cfmIpCbrMetricsIntTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CfmIpCbrMetricsIntEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains historic IP CBR metrics for the traffic
        flows monitored by each of the flow monitors supported by the
        device.

        This table has an sparse dependent relationship on the
        cfmFlowMetricsIntTable (defined by the CISCO-FLOW-MONITOR-MIB),
        containing a row for each row in the cfmFlowMetricsIntTable
        having a corresponding instance of cfmFlowMetricsCollected with
        the 'ipCbr' bit set to one."
    ::= { cfmIpCbrMetrics 3 }

cfmIpCbrMetricsIntEntry OBJECT-TYPE
    SYNTAX          CfmIpCbrMetricsIntEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry describes IP CBR metrics collected for a previous
        measurement interval for a corresponding traffic flow."
    INDEX           {
                        cfmFlowMonitorId,
                        cfmFlowId,
                        cfmFlowMetricsIntNumber
                    } 
    ::= { cfmIpCbrMetricsIntTable 1 }

CfmIpCbrMetricsIntEntry ::= SEQUENCE {
        cfmIpCbrMetricsIntValid        BITS,
        cfmIpCbrMetricsIntLostPkts     ReportIntervalCount,
        cfmIpCbrMetricsIntVbMin        ReportIntervalCount,
        cfmIpCbrMetricsIntVbMax        ReportIntervalCount,
        cfmIpCbrMetricsIntMrUnits      FlowBitRateUnits,
        cfmIpCbrMetricsIntMr           ReportIntervalCount,
        cfmIpCbrMetricsIntDfScale      FlowMetricScale,
        cfmIpCbrMetricsIntDfPrecision  FlowMetricPrecision,
        cfmIpCbrMetricsIntDf           FlowMetricValue,
        cfmIpCbrMetricsIntMrvScale     FlowMetricScale,
        cfmIpCbrMetricsIntMrvPrecision FlowMetricPrecision,
        cfmIpCbrMetricsIntMrv          FlowMetricValue
}

cfmIpCbrMetricsIntValid OBJECT-TYPE
    SYNTAX          BITS {
                        lostPkts(0),
                        vbMin(1),
                        vbMax(2),
                        mediaRate(3),
                        delayFactor(4),
                        mediaRateVariation(5)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates which metrics are valid for the
        measurement interval:

            'lostPkts'
                If this bit is set to '1', then the corresponding
                instance of cfmIpCbrMetricsIntLostPkts is valid.

            'vbMin'
                If this bit is set to '1', then the corresponding
                instance of cfmIpCbrMetricsIntVbMin is valid.

            'vbMax'
                If this bit is set to '1', then the corresponding
                instance of cfmIpCbrMetricsIntVbMax is valid.

            'mediaRate'
                If this bit is set to '1', then the corresponding
                instances of cfmIpCbrMetricsIntMrUnits and
                cfmIpCbrMetricsIntMr are valid.

            'delayFactor'
                If this bit is set to '1', then the corresponding
                instances of cfmIpCbrMetricsIntDfScale,
                cfmIpCbrMetricsIntDfPrecision, and cfmIpCbrMetricsIntDf
                are valid.

            'mediaRateVariation'
                If this bit is set to '1', then the corresponding
                instances of cfmIpCbrMetricsIntMrvScale,
                cfmIpCbrMetricsIntMrvPrecision, and
                cfmIpCbrMetricsIntMrv are valid." 
    ::= { cfmIpCbrMetricsIntEntry 1 }

cfmIpCbrMetricsIntLostPkts OBJECT-TYPE
    SYNTAX          ReportIntervalCount
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of lost packets for the
        traffic flow during the measurement interval.

        The value of this column is valid if and only if the 'lostPkts'
        bit in the corresponding instance of cfmIpCbrMetricsIntValid is
        set to '1'." 
    ::= { cfmIpCbrMetricsIntEntry 2 }

cfmIpCbrMetricsIntVbMin OBJECT-TYPE
    SYNTAX          ReportIntervalCount
    UNITS           "bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the minimum virtual buffer size computed
        for the traffic flow over the course of the measurement
        interval.

        The value of this column is valid if and only if the 'vbMin'
        bit in the corresponding instance of cfmIpCbrMetricsIntValid is
        set to '1'." 
    ::= { cfmIpCbrMetricsIntEntry 3 }

cfmIpCbrMetricsIntVbMax OBJECT-TYPE
    SYNTAX          ReportIntervalCount
    UNITS           "bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the maximum virtual buffer size computed
        for the traffic flow over the course of the measurement
        interval.

        The value of this column is valid if and only if the 'vbMax' bit
        in the corresponding instance of cfmIpCbrMetricsIntValid is set
        to '1'." 
    ::= { cfmIpCbrMetricsIntEntry 4 }

cfmIpCbrMetricsIntMrUnits OBJECT-TYPE
    SYNTAX          FlowBitRateUnits
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the units for the corresponding instance
        of cfmIpCbrMetricsMr.

        The value of this column is valid if and only if the 'mediaRate'
        bit in the corresponding instance of cfmIpCbrMetricsIntValid is
        set to '1'." 
    ::= { cfmIpCbrMetricsIntEntry 5 }

cfmIpCbrMetricsIntMr OBJECT-TYPE
    SYNTAX          ReportIntervalCount
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the media rate used by the flow monitor
        to compute the DF for the traffic flow.  If the corresponding
        instance of cfmIpCbrMetricsCfgRateType is 'auto', then the value
        of this column indicates the MR for the traffic flow during the
        measurement interval. Otherwise, the value  of this column
        reflects the configured MR.

        The value of this column is valid if and only if the 'mediaRate'
        bit in the corresponding instance of cfmIpCbrMetricsIntValid is
        set to '1'." 
    ::= { cfmIpCbrMetricsIntEntry 6 }

cfmIpCbrMetricsIntDfScale OBJECT-TYPE
    SYNTAX          FlowMetricScale
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the scaling factor for the corresponding
        instance of cfmIpCbrMetricsIntDf.

        The value of this column is valid if and only if the
        'delayFactor' bit in the corresponding instance of
        cfmIpCbrMetricsIntValid is set to '1'." 
    ::= { cfmIpCbrMetricsIntEntry 7 }

cfmIpCbrMetricsIntDfPrecision OBJECT-TYPE
    SYNTAX          FlowMetricPrecision
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the precision for the corresponding
        instance of cfmIpCbrMetricsIntDf.

        The value of this column is valid if and only if the
        'delayFactor' bit in the corresponding instance of
        cfmIpCbrMetricsIntValid is set to '1'." 
    ::= { cfmIpCbrMetricsIntEntry 8 }

cfmIpCbrMetricsIntDf OBJECT-TYPE
    SYNTAX          FlowMetricValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the DF for the traffic flow during the
        measurement interval.

        The value of this column is valid if and only if the
        'delayFactor' bit in the corresponding instance of
        cfmIpCbrMetricsIntValid is set to '1'." 
    ::= { cfmIpCbrMetricsIntEntry 9 }

cfmIpCbrMetricsIntMrvScale OBJECT-TYPE
    SYNTAX          FlowMetricScale
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the scaling factor for the corresponding
        instance of cfmIpCbrMetricsIntMrv.

        The value of this column is valid if and only if the
        'mediaRateVariation' bit in the corresponding instance of
        cfmIpCbrMetricsIntValid is set to '1'." 
    ::= { cfmIpCbrMetricsIntEntry 10 }

cfmIpCbrMetricsIntMrvPrecision OBJECT-TYPE
    SYNTAX          FlowMetricPrecision
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the precision for for the corresponding
        instance of cfmIpCbrMetricsIntMrv.

        The value of this column is valid if and only if the
        'mediaRateVariation' bit in the corresponding instance of
        cfmIpCbrMetricsIntValid is set to '1'." 
    ::= { cfmIpCbrMetricsIntEntry 11 }

cfmIpCbrMetricsIntMrv OBJECT-TYPE
    SYNTAX          FlowMetricValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the MRV for the traffic flow during the
        measurement interval.

        The value of this column is valid if and only if the
        'mediaRateVariation' bit in the corresponding instance of
        cfmIpCbrMetricsIntValid is set to '1'." 
    ::= { cfmIpCbrMetricsIntEntry 12 }
 

-- **********************************************************************
-- * Object Identifiers                                                 *
-- **********************************************************************

cfmIpCbrMonitoredElements  OBJECT IDENTIFIER
    ::= { ciscoIpCbrMetricsMIBIds 1 }


cfmeIpCbrCumulativeLostPkts OBJECT-IDENTITY
    STATUS          current
    DESCRIPTION
        "This object identifier represents the monitored element
        describing the cumulative number of lost packets for a traffic
        flow (cfmIpCbrMetricsLostPkts).  This obect identifier can be
        used as a value for cfmConditionMonitoredElement."
    REFERENCE
        "The cfmConditionMonitoredElement defined in
        CISCO-FLOW-MONITOR-MIB."
    ::= { cfmIpCbrMonitoredElements 1 }


cfmeIpCbrCumulativeMrv OBJECT-IDENTITY
    STATUS          current
    DESCRIPTION
        "This object identifier represents the monitored element
        describing the cumulative MRV for a traffic flow
        (cfmIpCbrMetricsMrv).  This obect identifier can be used as a
        value for cfmConditionMonitoredElement."
    REFERENCE
        "The cfmConditionMonitoredElement defined in
        CISCO-FLOW-MONITOR-MIB."
    ::= { cfmIpCbrMonitoredElements 2 }


cfmeIpCbrLostPkts OBJECT-IDENTITY
    STATUS          current
    DESCRIPTION
        "This object identifier represents the monitored element
        describing the number of packets lost for a traffic flow during
        the last measurement interval (cfmIpCbrMetricsIntLostPkts). 
        This obect identifier can be used as a value for
        cfmConditionMonitoredElement."
    REFERENCE
        "The cfmConditionMonitoredElement defined in
        CISCO-FLOW-MONITOR-MIB."
    ::= { cfmIpCbrMonitoredElements 3 }


cfmeIpCbrDf OBJECT-IDENTITY
    STATUS          current
    DESCRIPTION
        "This object identifier represents the monitored element
        describing the DF for a traffic flow during the last
        measurement interval (cfmIpCbrMetricsIntDf).  This obect
        identifier can be used as a value for
        cfmConditionMonitoredElement."
    REFERENCE
        "The cfmConditionMonitoredElement defined in
        CISCO-FLOW-MONITOR-MIB."
    ::= { cfmIpCbrMonitoredElements 4 }


cfmeIpCbrMrv OBJECT-IDENTITY
    STATUS          current
    DESCRIPTION
        "This object identifier represents the monitored element
        describing the MRV for a traffic flow during the last
        measurement interval (cfmIpCbrMetricsIntMrv).  This obect
        identifier can be used as a value for
        cfmConditionMonitoredElement."
    REFERENCE
        "The cfmConditionMonitoredElement defined in
        CISCO-FLOW-MONITOR-MIB."
    ::= { cfmIpCbrMonitoredElements 5 }

-- **********************************************************************
-- * Conformance                                                        *
-- **********************************************************************

ciscoIpCbrMetricsMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoIpCbrMetricsMIBConform 1 }

ciscoIpCbrMetricsMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoIpCbrMetricsMIBConform 2 }


ciscoIpCbrMetricsCompliance01 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "This compliance statement specifies the minimal requirements an
        implementation must meet in order to claim full compliance with
        the definition of the CISCO-IP-CBR-METRICS-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS { cfmIpCbrMetricsGroup }
    ::= { ciscoIpCbrMetricsMIBCompliances 1 }

-- **********************************************************************
-- * Units of Conformance                                               *
-- **********************************************************************

cfmIpCbrMetricsGroup OBJECT-GROUP
    OBJECTS         {
                        cfmIpCbrMetricsCfgRateType,
                        cfmIpCbrMetricsCfgBitRate,
                        cfmIpCbrMetricsCfgRate,
                        cfmIpCbrMetricsCfgMediaPktSize,
                        cfmIpCbrMetricsValid,
                        cfmIpCbrMetricsLostPkts,
                        cfmIpCbrMetricsMrvScale,
                        cfmIpCbrMetricsMrvPrecision,
                        cfmIpCbrMetricsMrv,
                        cfmIpCbrMetricsTableChanged,
                        cfmIpCbrMetricsIntValid,
                        cfmIpCbrMetricsIntLostPkts,
                        cfmIpCbrMetricsIntVbMin,
                        cfmIpCbrMetricsIntVbMax,
                        cfmIpCbrMetricsIntMrUnits,
                        cfmIpCbrMetricsIntMr,
                        cfmIpCbrMetricsIntDfScale,
                        cfmIpCbrMetricsIntDfPrecision,
                        cfmIpCbrMetricsIntDf,
                        cfmIpCbrMetricsIntMrvScale,
                        cfmIpCbrMetricsIntMrvPrecision,
                        cfmIpCbrMetricsIntMrv
                    }
    STATUS          current
    DESCRIPTION
        "This group contains objects that describe IP CBR metrics."
    ::= { ciscoIpCbrMetricsMIBGroups 1 }

END






















