-- *****************************************************************
-- CISCO-BRIDGE-CAPABILITY.my:
-- Cisco BRIDGE-MIB AGENT-CAPABILITIES
--   
-- August 1994, Jeffrey T. Johnso
--   
-- Copyright (c) 1994-2014 by Cisco Systems, Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-BRIDGE-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    Integer32,
    Counter32,
    MODULE-IDENTITY
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoBridgeCapability MODULE-IDENTITY
    LAST-UPDATED    "201409180000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "The capabilities description of BRIDGE-MIB."
    REVISION        "201409180000Z"
    DESCRIPTION
        "Added capability statement
        ciscoBridgeCapNxOSV06R0201PMds."
    REVISION        "201307160000Z"
    DESCRIPTION
        "Added VARIATION clauses of dot1dTpPortInFrames and
        dot1dTpPortOutFrames to capability statement
        ciscoBridgeCapNxOSV05R0201PN7k."
    REVISION        "201107260000Z"
    DESCRIPTION
        "Added capability statement
        ciscoBridgeCapNxOSV05R0201PN7k."
    REVISION        "201012010000Z"
    DESCRIPTION
        "Added capability statement
        ciscoBridgeCapV12R4SEPC1861."
    REVISION        "201011180000Z"
    DESCRIPTION
        "Added capability statement
        ciscoBridgeCapNxOSV05R0101PN7k."
    REVISION        "201009090000Z"
    DESCRIPTION
        "Added capability statement
        ciscoBridgeCapV12R2SEPCat3K."
    REVISION        "201006100000Z"
    DESCRIPTION
        "Added the capability statements:

        ciscoBridgeCapNxOSV04R0201N0101PN5k and
        ciscoBridgeCapNxOSV05R0002PN7k."
    REVISION        "201003020000Z"
    DESCRIPTION
        "Added capability statement
        ciscoBridgeCapV12R0233SXHPCat6K."
    REVISION        "200703280000Z"
    DESCRIPTION
        "Added VARIATION clause of dot1dStaticStatus for
        capability statement ciscoBridgeCapCatOSV08R0601."
    REVISION        "200606120000Z"
    DESCRIPTION
        "Added capability statement
        ciscoBridgeCapCatOSV08R0601.
        Commented out ciscoBridgeCapabilityV10R02."
    REVISION        "9408180000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 106 }



ciscoBridgeCapCatOSV08R0601 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.6(1) on Catalyst 6000/6500
                         and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "BRIDGE-MIB capabilities."

    SUPPORTS        BRIDGE-MIB
    INCLUDES        {
                        dot1dBaseBridgeGroup,
                        dot1dBasePortGroup,
                        dot1dStpBridgeGroup,
                        dot1dStpPortGroup2,
                        dot1dStpPortGroup3,
                        dot1dTpBridgeGroup,
                        dot1dTpFdbGroup,
                        dot1dStaticGroup,
                        dot1dNotificationGroup
                    }
    VARIATION       newRoot
    DESCRIPTION
        "Additional VarBinds are appended to notification
        newRoot depends on the value of stpxSpanningTreeType.
        'pvstPlus',
        'rapidPvstPlus' - vtpVlanIndex
        'mistp',
        'mistpPvstPlus' - stpxMISTPInstanceIndex
        'mst' - stpxMSTInstanceIndex"

    VARIATION       topologyChange
    DESCRIPTION
        "Additional VarBinds are appended to notification
        topologyChange depends on the value of
        stpxSpanningTreeType.
        'pvstPlus',
        'rapidPvstPlus' - vtpVlanIndex, ifName
        'mistp',
        'mistpPvstPlus' - stpxMISTPInstanceIndex, ifName
        'mst' - stpxMSTInstanceIndex, ifName"

    VARIATION       dot1dStaticStatus
    DESCRIPTION
        "The default value is deleteOnReset(4)."

    ::= { ciscoBridgeCapability 2 }

ciscoBridgeCapV12R0233SXHPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXH on Catalyst 6000/6500
                         series devices."
    STATUS          current
    DESCRIPTION
        "BRIDGE-MIB capabilities."

    SUPPORTS        BRIDGE-MIB
    INCLUDES        {
                        dot1dBaseBridgeGroup,
                        dot1dBasePortGroup,
                        dot1dStpBridgeGroup,
                        dot1dStpPortGroup,
                        dot1dTpBridgeGroup,
                        dot1dTpFdbGroup,
                        dot1dTpGroup,
                        dot1dStaticGroup,
                        dot1dNotificationGroup
                    }
    VARIATION       dot1dBasePortDelayExceededDiscards
    DESCRIPTION
        "This counter is implemented as a per port
        counter instead of a per port per VLAN
        (Virtual Local Area Network) counter."

    VARIATION       dot1dBasePortMtuExceededDiscards
    DESCRIPTION
        "This counter is implemented as a per port
        counter instead of a per port per VLAN
        counter."

    VARIATION       dot1dTpLearnedEntryDiscards
    DESCRIPTION
        "This counter counts every such discarded
        forwarding database entries on all VLANs."

    VARIATION       dot1dStpPortEnable
    SYNTAX          INTEGER  {
                        enabled(1)
                    }
    DESCRIPTION
        "Only a limited set of enumerated values
        are supported."

    VARIATION       dot1dTpAgingTime
    DESCRIPTION
        "Out of range values 5 to 9 are
        supported as read-only."

    VARIATION       dot1dTpPortInFrames
    DESCRIPTION
        "This counter is implemented as a per port
        counter instead of a per port per VLAN
        counter."

    VARIATION       dot1dTpPortOutFrames
    DESCRIPTION
        "This counter is implemented as a per port
        counter instead of a per port per VLAN
        counter."

    VARIATION       dot1dTpPortInDiscards
    DESCRIPTION
        "Hardcoded to value zero."

    VARIATION       dot1dStaticReceivePort
    SYNTAX          Integer32 (0)
    DESCRIPTION
        "Only supports value zero."

    VARIATION       dot1dStaticAllowedToGoTo
    SYNTAX          OCTET STRING (SIZE (0..256))
    DESCRIPTION
        "The maximum size of the octet string is limited
        to 256."

    VARIATION       dot1dStaticStatus
    SYNTAX          INTEGER  {
                        invalid(2),
                        deleteOnReset(4)
                    }
    DESCRIPTION
        "Only a limited set of enumerated values
        are supported."

    VARIATION       newRoot
    DESCRIPTION
        "Additional VarBinds are appended to notification
        newRoot depends on the value of stpxSpanningTreeType.
        'pvstPlus',
        'rapidPvstPlus' - vtpVlanIndex
        'mst' - stpxMSTInstanceIndex"

    VARIATION       topologyChange
    DESCRIPTION
        "Additional VarBinds are appended to notification
        topologyChange depends on the value of
        stpxSpanningTreeType.
        'pvstPlus',
        'rapidPvstPlus' - vtpVlanIndex, ifName
        'mst' - stpxMSTInstanceIndex, ifName"

    ::= { ciscoBridgeCapability 3 }

ciscoBridgeCapNxOSV04R0201N0101PN5k AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco NX-OS 4.2(1)N1(1) on Nexus 5000
                         series devices."
    STATUS          current
    DESCRIPTION
        "BRIDGE-MIB capabilities."

    SUPPORTS        BRIDGE-MIB
    INCLUDES        {
                        dot1dBaseBridgeGroup,
                        dot1dBasePortGroup,
                        dot1dStpBridgeGroup,
                        dot1dStpPortGroup,
                        dot1dStpPortGroup2,
                        dot1dStpPortGroup3,
                        dot1dTpBridgeGroup,
                        dot1dTpFdbGroup
                    }
    VARIATION       dot1dBaseType
    SYNTAX          INTEGER  {
                        transparent-only(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        are supported."

    VARIATION       dot1dBasePortCircuit
    SYNTAX          OBJECT IDENTIFIER
    DESCRIPTION
        "Always return 0.0"

    VARIATION       dot1dBasePortDelayExceededDiscards
    SYNTAX          Counter32
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dBasePortMtuExceededDiscards
    SYNTAX          Counter32
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dStpPriority
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpBridgeMaxAge
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpBridgeHelloTime
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpBridgeForwardDelay
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpPortPriority
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpPortEnable
    SYNTAX          INTEGER  {
                        enabled(1)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Only limited set of enumerated values
        are supported.
        Write access is not supported."

    VARIATION       dot1dStpPortPathCost
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpPortPathCost32
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dTpLearnedEntryDiscards
    SYNTAX          Counter32
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dTpAgingTime
    SYNTAX          Integer32 (0 | 120..918000)
    DESCRIPTION
        "Only limited set of values
        are supported.
        Setting dot1dTpAgingTime to zero disables
        the aging timeout.
        Only values which are multiple of 5 are supported."

    ::= { ciscoBridgeCapability 4 }

ciscoBridgeCapNxOSV05R0002PN7k AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco NX-OS 5.0(2) on Nexus 7000
                         series devices."
    STATUS          current
    DESCRIPTION
        "BRIDGE-MIB capabilities."

    SUPPORTS        BRIDGE-MIB
    INCLUDES        {
                        dot1dBaseBridgeGroup,
                        dot1dBasePortGroup,
                        dot1dStpBridgeGroup,
                        dot1dStpPortGroup,
                        dot1dStpPortGroup2,
                        dot1dStpPortGroup3,
                        dot1dTpBridgeGroup,
                        dot1dTpFdbGroup,
                        dot1dNotificationGroup
                    }
    VARIATION       dot1dBaseType
    SYNTAX          INTEGER  {
                        transparent-only(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        are supported."

    VARIATION       dot1dBasePortCircuit
    DESCRIPTION
        "Always return 0.0"

    VARIATION       dot1dBasePortDelayExceededDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dBasePortMtuExceededDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dStpPriority
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpBridgeMaxAge
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpBridgeHelloTime
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpBridgeForwardDelay
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpPortPriority
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpPortEnable
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpPortPathCost
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpPortPathCost32
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dTpLearnedEntryDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dTpAgingTime
    SYNTAX          Integer32 (0 | 120..918000)
    DESCRIPTION
        "Only limited set of values
        are supported.
        Setting dot1dTpAgingTime to zero disables
        the aging timeout.
        Only values which are multiple of 5 are supported."

    VARIATION       newRoot
    DESCRIPTION
        "Additional VarBinds are appended to notification
        newRoot depends on the value of stpxSpanningTreeType.
        'rapidPvstPlus' - vtpVlanIndex"

    VARIATION       topologyChange
    DESCRIPTION
        "Additional VarBinds are appended to notification
        topologyChange depends on the value of
        stpxSpanningTreeType.
        'rapidPvstPlus' - vtpVlanIndex, ifName"

    ::= { ciscoBridgeCapability 5 }

ciscoBridgeCapV12R2SEPCat3K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2SE on Catalyst 3K
                        series devices."
    STATUS          current
    DESCRIPTION
        "BRIDGE-MIB capabilities."

    SUPPORTS        BRIDGE-MIB
    INCLUDES        {
                        dot1dBaseBridgeGroup,
                        dot1dBasePortGroup,
                        dot1dStpBridgeGroup,
                        dot1dStpPortGroup,
                        dot1dTpBridgeGroup,
                        dot1dTpFdbGroup,
                        dot1dTpGroup,
                        dot1dStaticGroup,
                        dot1dNotificationGroup
                    }
    VARIATION       dot1dBaseType
    SYNTAX          INTEGER  {
                        transparent-only(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        are supported."

    VARIATION       dot1dBasePortCircuit
    DESCRIPTION
        "Always return 0.0"

    VARIATION       dot1dBasePortDelayExceededDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dStpPortEnable
    SYNTAX          INTEGER  {
                        enabled(1)
                    }
    DESCRIPTION
        "Only a limited set of enumerated values
        are supported."

    VARIATION       dot1dStaticStatus
    SYNTAX          INTEGER  {
                        invalid(2),
                        permanent(3),
                        deleteOnReset(4)
                    }
    DESCRIPTION
        "Only a limited set of enumerated values
        are supported."

    VARIATION       newRoot
    DESCRIPTION
        "Additional VarBinds are appended to notification
        newRoot depends on the value of stpxSpanningTreeType
        as shown in the table below.
        stpxSpanningTreeType        Additional Varbinds
        ------------------------------------------------
        'pvstPlus'                  vtpVlanIndex
        'rapidPvstPlus'             vtpVlanIndex
        'mst'                       stpxMSTInstanceIndex"

    VARIATION       topologyChange
    DESCRIPTION
        "Additional VarBinds are appended to notification
        topologyChange depends on the value of stpxSpanningTreeType
        as shown in the table below.
        stpxSpanningTreeType        Additional Varbinds
        ------------------------------------------------
        'pvstPlus'                  vtpVlanIndex, ifName
        'rapidPvstPlus'             vtpVlanIndex, ifName
        'mst'                       stpxMSTInstanceIndex, ifName"

    ::= { ciscoBridgeCapability 6 }

ciscoBridgeCapNxOSV05R0101PN7k AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco NX-OS 5.1(1) on Nexus 7000
                    series devices."
    STATUS          current
    DESCRIPTION
        "BRIDGE-MIB capabilities."

    SUPPORTS        BRIDGE-MIB
    INCLUDES        {
                        dot1dBaseBridgeGroup,
                        dot1dBasePortGroup,
                        dot1dStpBridgeGroup,
                        dot1dStpPortGroup,
                        dot1dStpPortGroup2,
                        dot1dStpPortGroup3,
                        dot1dTpBridgeGroup,
                        dot1dTpFdbGroup,
                        dot1dTpGroup,
                        dot1dStaticGroup,
                        dot1dNotificationGroup
                    }
    VARIATION       dot1dBaseType
    SYNTAX          INTEGER  {
                        transparent-only(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is supported."

    VARIATION       dot1dBasePortCircuit
    DESCRIPTION
        "Always return 0.0."

    VARIATION       dot1dBasePortDelayExceededDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dBasePortMtuExceededDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dStpPriority
    SYNTAX          Integer32 (0 | 4096 | 8192 | 12288 | 16384 | 20480 | 24576 | 28672 | 32768 | 36864 | 40960 | 45056 | 49152 | 53248 | 57344 | 61440)
    DESCRIPTION
        "Only limited set of values is supported."

    VARIATION       dot1dStpPortPriority
    SYNTAX          Integer32 (0 | 16 | 32 | 48 | 64 | 80 | 96 | 112 | 128 | 144 | 160 | 176 | 192 | 208 | 224)
    DESCRIPTION
        "Only limited set of values is supported."

    VARIATION       dot1dStpPortEnable
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dStpPortPathCost32
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dTpLearnedEntryDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dTpAgingTime
    SYNTAX          Integer32 (0 | 120..918000)
    DESCRIPTION
        "Only limited set of values is supported.
        Setting dot1dTpAgingTime to zero disables
        the aging timeout.
        Only values which are multiple of 5 are supported."

    VARIATION       dot1dTpPortInDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dStaticReceivePort
    SYNTAX          Integer32 (0)
    DESCRIPTION
        "Only limited set of values is supported."

    VARIATION       dot1dStaticStatus
    SYNTAX          INTEGER  {
                        invalid(2),
                        deleteOnReset(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is supported."

    VARIATION       newRoot
    DESCRIPTION
        "Additional VarBinds are appended to notification
        newRoot depends on the value of stpxSpanningTreeType.
        'rapidPvstPlus' - vtpVlanIndex
        'mst'           - stpxMSTInstanceIndex"

    VARIATION       topologyChange
    DESCRIPTION
        "Additional VarBinds are appended to notification
        topologyChange depends on the value of
        stpxSpanningTreeType.
        'rapidPvstPlus' - vtpVlanIndex, ifName
        'mst'           - stpxMSTInstanceIndex, ifName"

    ::= { ciscoBridgeCapability 7 }

ciscoBridgeCapV12R4SEPC1861 AGENT-CAPABILITIES
    PRODUCT-RELEASE "OS=IOS
                     OSVERSION=Cisco IOS 12.4,15.1T
                     PLATFORM=c1861"
    STATUS          current
    DESCRIPTION
        "BRIDGE-MIB capabilities"

    SUPPORTS        BRIDGE-MIB
    INCLUDES        {
                        dot1dBaseBridgeGroup,
                        dot1dBasePortGroup,
                        dot1dStpBridgeGroup,
                        dot1dStpPortGroup,
                        dot1dTpBridgeGroup,
                        dot1dTpFdbGroup,
                        dot1dTpGroup,
                        dot1dStaticGroup
                    }
    VARIATION       dot1dStpPortEnable
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported"

    ::= { ciscoBridgeCapability 8 }

ciscoBridgeCapNxOSV05R0201PN7k AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco NX-OS 5.2(1) on Nexus 7000
                    series devices."
    STATUS          current
    DESCRIPTION
        "BRIDGE-MIB capabilities."

    SUPPORTS        BRIDGE-MIB
    INCLUDES        {
                        dot1dBaseBridgeGroup,
                        dot1dBasePortGroup,
                        dot1dStpBridgeGroup,
                        dot1dStpPortGroup,
                        dot1dStpPortGroup2,
                        dot1dStpPortGroup3,
                        dot1dTpBridgeGroup,
                        dot1dTpFdbGroup,
                        dot1dTpGroup,
                        dot1dStaticGroup,
                        dot1dNotificationGroup
                    }
    VARIATION       dot1dBaseType
    SYNTAX          INTEGER  {
                        transparent-only(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is supported."

    VARIATION       dot1dBasePortCircuit
    DESCRIPTION
        "Always return 0.0."

    VARIATION       dot1dBasePortDelayExceededDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dBasePortMtuExceededDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dStpPriority
    SYNTAX          Integer32 (0 | 4096 | 8192 | 12288 | 16384 | 20480 | 24576 | 28672 | 32768 | 36864 | 40960 | 45056 | 49152 | 53248 | 57344 | 61440)
    DESCRIPTION
        "Only limited set of values is supported."

    VARIATION       dot1dStpPortPriority
    SYNTAX          Integer32 (0 | 16 | 32 | 48 | 64 | 80 | 96 | 112 | 128 | 144 | 160 | 176 | 192 | 208 | 224)
    DESCRIPTION
        "Only limited set of values is supported."

    VARIATION       dot1dStpPortEnable
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       dot1dTpLearnedEntryDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dTpAgingTime
    SYNTAX          Integer32 (0 | 120..918000)
    DESCRIPTION
        "Only limited set of values is supported.
        Setting dot1dTpAgingTime to zero disables
        the aging timeout.
        Only values which are multiple of 5 are supported."

    VARIATION       dot1dTpPortInDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dStaticReceivePort
    SYNTAX          Integer32 (0)
    DESCRIPTION
        "Only limited set of values is supported."

    VARIATION       dot1dStaticStatus
    SYNTAX          INTEGER  {
                        invalid(2),
                        deleteOnReset(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is supported."

    VARIATION       newRoot
    DESCRIPTION
        "Additional VarBinds are appended to notification
        newRoot depends on the value of stpxSpanningTreeType.
        'rapidPvstPlus' - vtpVlanIndex
        'mst'           - stpxMSTInstanceIndex"

    VARIATION       topologyChange
    DESCRIPTION
        "Additional VarBinds are appended to notification
        topologyChange depends on the value of
        stpxSpanningTreeType.
        'rapidPvstPlus' - vtpVlanIndex, ifName
        'mst'           - stpxMSTInstanceIndex, ifName"

    VARIATION       dot1dTpPortInFrames
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dTpPortOutFrames
    DESCRIPTION
        "Always return 0."

    ::= { ciscoBridgeCapability 9 }

ciscoBridgeCapNxOSV06R0201PMds AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco NX-OS 6.2(1) on MDS 9700
                    series devices."
    STATUS          current
    DESCRIPTION
        "BRIDGE-MIB capabilities."

    SUPPORTS        BRIDGE-MIB
    INCLUDES        {
                        dot1dBaseBridgeGroup,
                        dot1dBasePortGroup,
                        dot1dStpBridgeGroup,
                        dot1dTpBridgeGroup,
                        dot1dTpFdbGroup,
                        dot1dTpGroup,
                        dot1dStaticGroup
                    }
    VARIATION       dot1dBaseBridgeAddress
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dBaseType
    SYNTAX          INTEGER  {
                        transparent-only(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is supported."

    VARIATION       dot1dBasePortCircuit
    DESCRIPTION
        "Always return 0.0."

    VARIATION       dot1dBasePortDelayExceededDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dBasePortMtuExceededDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dStpPriority
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dStpTimeSinceTopologyChange
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dStpTopChanges
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dStpDesignatedRoot
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dStpRootCost
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dStpRootPort
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dStpMaxAge
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dStpHelloTime
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dStpHoldTime
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dStpForwardDelay
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dStpBridgeMaxAge
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dStpBridgeHelloTime
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dStpBridgeForwardDelay
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       dot1dTpLearnedEntryDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dTpAgingTime
    SYNTAX          Integer32 (0 | 120..918000)
    DESCRIPTION
        "Only limited set of values is supported.
        Setting dot1dTpAgingTime to zero disables
        the aging timeout.
        Only values which are multiple of 5 are supported."

    VARIATION       dot1dTpPortInDiscards
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dStaticReceivePort
    SYNTAX          Integer32 (0)
    DESCRIPTION
        "Only limited set of values is supported."

    VARIATION       dot1dStaticStatus
    SYNTAX          INTEGER  {
                        invalid(2),
                        deleteOnReset(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is supported."

    VARIATION       dot1dTpPortInFrames
    DESCRIPTION
        "Always return 0."

    VARIATION       dot1dTpPortOutFrames
    DESCRIPTION
        "Always return 0."

    ::= { ciscoBridgeCapability 10 }

END




