-- *****************************************************************
-- CISCO-RTTMON-TC-MIB.my:  IP SLA Textual Conventions MIB file
--   
-- August 2005, Katherine Yang
--   
-- Copyright (c) 2005-2012 by Cisco Systems, Inc.
-- All rights reserved.
--   
-- *****************************************************************

CISCO-RTTMON-TC-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    Unsigned32
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    ciscoMgmt
        FROM CISCO-SMI;


ciscoRttMonTCMIB MODULE-IDENTITY
    LAST-UPDATED    "201205250000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems, Inc.
            Customer Service 

            Postal: 170 W Tasman Drive
            San Jose, CA 95134

            Tel: +1 800 553 NETS
            Email: cs-ipsla@cisco.com"
    DESCRIPTION
        "This MIB contains textual conventions used by
        CISCO-RTTMON-MIB, CISCO-RTTMON-RTP-MIB and 
        CISCO-RTTMON-ICMP-MIB, but they are not limited 
        to only these MIBs. 
        These textual conventions were originally defined in 
        CISCO-RTTMON-MIB.

        Acronyms:
          FEC: Forward Equivalence Class
          LPD: Label Path Discovery
          LSP: Label Switched Path
          MPLS: Multi Protocol Label Switching
          RTT: Round Trip Time
          SAA: Service Assurance Agent
          VPN: Virtual Private Network
          CFM: Connection Fault Management"
    REVISION        "201205250000Z"
    DESCRIPTION
        "Added enumeration y1731slm to RttMonProtocol

        Added the following to RttResopnseSense.
         statsRetrieveOk, statsRetrieveNoConnect,  
         statsRetrieveVersionFail, statsRetrieveInternalError,
         statsRetrieveAbort, statsRetrieveFail,
         statsRetrieveAuthFail, statsRetrieveFormatError,
         statsRetrievePortInUse.

        For enumeration from controlOk to controlPortInUse, changed the
        prefix from control to enable."
    REVISION        "201109150000Z"
    DESCRIPTION
        "Updated following textual conventions to include Y1731
        and Multicast extensions.
        -RttMonRttType, RttMonProtocol."
    REVISION        "201004260000Z"
    DESCRIPTION
        "Added enumeration 'video' to RttMonRttType TC."
    REVISION        "200608110000Z"
    DESCRIPTION
        "Added RttMonIdLst and RttMonCtrlIndex textual conventions."
    REVISION        "200607170000Z"
    DESCRIPTION
        "Added enumeration 'lspPingPseudowire' to RttMonRttType TC."
    REVISION        "200603020000Z"
    DESCRIPTION
        "Added ethernetPing and ethernetJitter in RttMonRttType.
        Added ethernetPingAppl and ethernetJitterAppl 
        in RttMonProtocol"
    REVISION        "200508090000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 485 }



-- Textual Conventions

RttReset ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "When the value set to 'reset', the entire RTT application
        goes through a reset sequence, making a best
        effort to revert to its startup condition. At other times,
        the value is 'ready'."
    SYNTAX          INTEGER  {
                        ready(1),
                        reset(2)
                    }

RttMonOperation ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The following are specific RTT operations for a
        particular probe type:
        notApplicable(0)         - This object is not applicable for the
                                   probe type.
        httpGet(1)               - HTTP get request
        httpRaw(2)               - HTTP request with user defined payload
        ftpGet(3)                - FTP get request
        ftpPassive(4)            - FTP passive mode
        ftpActive(5)             - FTP active mode
        voipDTAlertRinging(6)    - Voip post dial delay detect point:
                                   Alerting / Ringing
        voipDTConnectOK(7)       - Voip post dial delay detect point:
                                   Connect /OK"
    SYNTAX          INTEGER  {
                        notApplicable(0),
                        httpGet(1),
                        httpRaw(2),
                        ftpGet(3),
                        ftpPassive(4),
                        ftpActive(5),
                        voipDTAlertRinging(6),
                        voipDTConnectOK(7)
                    }

-- Operation completion sense code textual convention

RttResponseSense ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "These are the defined values for a completion status
        of a RTT operation.  

        other(0)         - the operation is not started or completed
                            or this object is not applicable for
                            the probe type.  
        ok(1)            - a valid completion occurred and
                            timed successfully
        disconnected(2)  - the operation did not occur because
                            the connection to the target
                            was lost
        overThreshold(3) - a valid completion was received but
                            the completion time exceeded a
                            threshold value
        timeout(4)       - an operation timed out; no completion
                            time recorded
        busy(5)          - the operation did not occur because a
                            previous operation is still
                            outstanding
        notConnected(6)  - the operation did not occur because no
                            connection (session) exists with the
                            target
        dropped(7)       - the operation did not occur due to lack
                            of internal resource
        sequenceError(8) - a completed operation did not contain 
                            the correct sequence id; no completion
                            time recorded
        verifyError(9)   - a completed operation was received, but
                            the data it contained did not match
                            the expected data; no completion time 
                            recorded
        applicationSpecific(10) 
                         - the application generating the operation
                            had a specific error
        dnsServerTimeout(11) 
                         - DNS Server Timeout
        tcpConnectTimeout(12)
                         - TCP Connect Timeout
        httpTransactionTimeout(13)
                         - HTTP Transaction Timeout
        dnsQueryError(14)
                         - DNS Query error (because of unknown address 
                           etc.,)
        httpError(15)
                         - HTTP Response StatusCode is not OK (200),
                           or permenent redirect(301), temporary redirect
                           (302) then HTTP error is set.
        error(16)
                         - if there are socket failures or some other 
                           errors not relavant to the actual probe, they 
                           are recorded under this error
        mplsLspEchoTxError(17)
                         - MPLS echo request transmission failure.
        mplsLspUnreachable(18)
                         - MPLS Target FEC not reachable or unsupported
                           mpls echo reply code.
        mplsLspMalformedReq(19)
                         - MPLS echo request was malformalformed, pointed
                           out by the reply router.
        mplsLspReachButNotFEC(20)
                         - MPLS echo request processed by the downstream
                           router but not the target.
        enableOk(21) 
                         - Control enable request OK
        enableNoConnect(22)
                         - Control enable request fail due to no connection to
                           the target.
        enableVersionFail(23)
                         - Control enable request version fail.
        enableInternalError(24)
                         - Control enable request internal error.
        enableAbort(25)
                         - Control enable request abort.
        enableFail(26)
                         - Control enable request fail.
        enableAuthFail(27)
                         - Control enable request fail due to authentication
                           fail.
        enableFormatError(28)
                         - Control enable request fail due to format error.
        enablePortInUse(29)
                         - Control enable request fail due to port in use.
        statsRetrieveOk(30)
                         - Stats retrieve request OK
        statsRetrieveNoConnect(31)
                         - Stats retrieve request fail due to no connection 
                           to the target.
        statsRetrieveVersionFail(32)
                         - Stats retrieve request version fail.
        statsRetrieveInternalError(33)
                         - Stats retrieve request internal error.
        statsRetrieveAbort(34)
                         - Stats retrieve request abort.
        statsRetrieveFail(35)
                         - Stats retrieve request fail.
        statsRetrieveAuthFail(36)
                         - Stats retrieve request fail due to authentication fail.
        statsRetrieveFormatError(37)
                         - Stats retrieve request fail due to format error.
        statsRetrievePortInUse(38)
                         - Stats retrieve request fail due to port in use."
    SYNTAX          INTEGER  {
                        other(0),
                        ok(1),
                        disconnected(2),
                        overThreshold(3),
                        timeout(4),
                        busy(5),
                        notConnected(6),
                        dropped(7),
                        sequenceError(8),
                        verifyError(9),
                        applicationSpecific(10),
                        dnsServerTimeout(11),
                        tcpConnectTimeout(12),
                        httpTransactionTimeout(13),
                        dnsQueryError(14),
                        httpError(15),
                        error(16),
                        mplsLspEchoTxError(17),
                        mplsLspUnreachable(18),
                        mplsLspMalformedReq(19),
                        mplsLspReachButNotFEC(20),
                        enableOk(21),
                        enableNoConnect(22),
                        enableVersionFail(23),
                        enableInternalError(24),
                        enableAbort(25),
                        enableFail(26),
                        enableAuthFail(27),
                        enableFormatError(28),
                        enablePortInUse(29),
                        statsRetrieveOk(30),
                        statsRetrieveNoConnect(31),
                        statsRetrieveVersionFail(32),
                        statsRetrieveInternalError(33),
                        statsRetrieveAbort(34),
                        statsRetrieveFail(35),
                        statsRetrieveAuthFail(36),
                        statsRetrieveFormatError(37),
                        statsRetrievePortInUse(38)
                    }

-- Operation type textual convention

RttMonRttType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Specifies the type of RTT operation to be performed.

        The value 'echo' will cause the RTT application to
        perform a timed echo request/response operation directed
        at the 'RttMonTargetAddress'.

        The value 'pathEcho' will cause the RTT application
        to perform path discovery to the 'RttMonTargetAddress', 
        then it will perform a timed echo request/response 
        operation directed at the each hop along the path.  
        This operation will provide two types of information, 
        first the path and second the time delay along the path.

        NOTE:  The 'pathEcho' time delay operation is a heuristic
               measurement because an intermediate hop may forward
               the different echo request/response at different
               rates.  Thus the time delay difference between two
               hops along a path may contain very little 'true'
               statistical meaning. 

        The value 'fileIO' will cause the RTT application to 
        write, read, or write/read a file to a preconfigured 
        file server.

        The value 'script' will cause the RTT application to
        execute a preconfigured script.

        The value 'udpEcho' will cause the RTT application
        to perform a timed udp packet send/receive operation 
        directed at the 'RttMonTargetAddress'.

        The value 'tcpConnect' will cause the RTT application
        to perform a timed tcp connect operation directed at the 
        'RttMonTargetAddress'.

        The value 'http' will cause the RTT application
        to perform a download of the object specified in the URL.

        The value 'dns' will cause the RTT application
        to perform a name lookup of an IP Address or a hostname.

        The value 'jitter' will cause the RTT application
        to perform delay variance analysis.

        The value 'dlsw' will cause the RTT application
        to perform a keepalive operation to measure the response 
        time of a DLSw peer.

        The value 'dhcp' will cause the RTT application
        to perform an IP Address lease request/teardown operation.

        The value 'voip' will cause the RTT application
        to perform call set up operation to measure the response.

        The value 'rtp' will cause the RTT application to perform
        delay variance analysis for RTP packet.

        The value 'lspGroup' will cause the RTT application to logically
        group Label Switched Paths discovered as part of LSP Path
        Discovery to the target and perform an RTT operation end to end
        over each path in the Group. The type of operation configured
        is determined by rttMplsVpnMonCtrlRttType.

        The value 'icmpjitter' will cause the RTT application
        to perform delay variance analysis using ICMP timestamp packets.

        The value of 'lspPingIpv4' will cause the RTT application to
        perform ping over LSP path.

        The value of 'lspTraceIpv4' will cause the RTT application to
        perform trace over LSP path.

        The value of 'ethernetPing' will cause the RTT application to
        perform delay variance analysis using regular 802.1ag loopback
        frame.

        The value of 'ethernetJitter' will cause the RTT application to
        perform delay variance analysis using CFM frame.

        The value of 'lspPingPseudowire' will cause the RTT application
        to
        perform LSP Ping over Pseudowire and measure response time.

        The value 'video' will cause the the RTT application to perform
        a video stream analysis directed at the 'RttMonTargetAddress
        The value 'y1731Delay' will cause the RTT application to perform a ITU-T standard Y.1731 delay variance analysis
        The value 'y1731Loss' will cause the RTT application to perform a ITU-T standard Y.1731 loss measure analysis
        The value 'mcastJitter' will cause the RTT application to perform 
        udp jitter stream analysis on a multicast network."
    SYNTAX          INTEGER  {
                        echo(1),
                        pathEcho(2),
                        fileIO(3),
                        script(4),
                        udpEcho(5),
                        tcpConnect(6),
                        http(7),
                        dns(8),
                        jitter(9),
                        dlsw(10),
                        dhcp(11),
                        ftp(12),
                        voip(13),
                        rtp(14),
                        lspGroup(15),
                        icmpjitter(16),
                        lspPing(17),
                        lspTrace(18),
                        ethernetPing(19),
                        ethernetJitter(20),
                        lspPingPseudowire(21),
                        video(22),
                        y1731Delay(23),
                        y1731Loss(24),
                        mcastJitter(25)
                    }

-- Operation type for Auto SAA L3 MPLS VPN textual convention

RttMplsVpnMonRttType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Specifies the type of RTT operation to be performed for
        Auto SAA L3 MPLS VPN.

        The value 'jitter' will cause the Auto SAA L3 MPLS VPN to
        automatically configure jitter operations.

        The value 'echo' will cause the Auto SAA L3 MPLS VPN to
        automatically configure jitter operations.

        The value 'pathEcho' will cause the Auto SAA L3 MPLS VPN to
        automatically configure jitter operations."
    SYNTAX          INTEGER  {
                        jitter(1),
                        echo(2),
                        pathEcho(3)
                    }

-- --
-- Auto SAA L3 MPLS VPN LSP Path Discovery
-- Failure Cause textual convention

RttMplsVpnMonLpdFailureSense ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "These are the defined values for the causes of failure in
        LSP Path Discovery.

        unknown(1)                      - The cause of failure for the
                                          LSP Path Discovery cannot be
                                          determined. The discovery for
                                          the target PE may not have 
                                          started.
        noPath(2)                       - No paths were found to the
                                          target FEC while doing the
                                          LSP Path Discovery.
        allPathsBroken(3)               - All paths to the target FEC
                                          are broken. This means an
                                          untagged interface on the LSP
                                          to the target.
        allPathsUnexplorable(4)         - All paths to the target FEC are
                                          unexplorable. This identifies
                                          a case where there is some
                                          problem in reaching the next
                                          hop while doing Discovery.
        allPathsBrokenOrUnexplorable(5) - All paths to the target FEC are
                                          are either broken or
                                          unexplorable.
        timeout(6)                      - The LSP Path Discovery could
                                          not be completed for the
                                          target FEC within the
                                          configured time.
        error(7)                        - Error occurred while
                                          performing LSP Path Discovery.
                                          It might be also due to some
                                          reasons unrelated to LSP Path
                                          Discovery."
    SYNTAX          INTEGER  {
                        unknown(1),
                        noPath(2),
                        allPathsBroken(3),
                        allPathsUnexplorable(4),
                        allPathsBrokenOrUnexplorable(5),
                        timeout(6),
                        error(7)
                    }

-- textual convention

RttMplsVpnMonLpdGrpStatus ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "These are the defined values for the status of the LPD Group.

        unknown(1) - This indicates that some/all of the probes which are
                     part of the LPD group have not completed even
                     a single operation, so the group status cannot be
                     identified.
             up(2) - This state indicates that all the probes which are
                     part of the LPD group are up with latest return
                     code as 'ok'.
        partial(3) - This state indicates that some probes are up and
                     running fine and some are not 'ok'.
           down(4) - This state indicates that all the probes to the
                     target are not running fine. This state indicates
                     that there is connectivity problem to the target
                     PE."
    SYNTAX          INTEGER  {
                        unknown(1),
                        up(2),
                        partial(3),
                        down(4)
                    }

RttMonProtocol ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Specifies the protocol to be used to perform the timed
        echo request/response.  The following protocols are
        defined:

        NOTE: All protocols that end in 'Appl' will support
              the asymetric request/response (ARR) protocol.  
              See the DESCRIPTION for ciscoRttMonMIB for a
              complete description of the asymetric 
              request/response protocol.

        notApplicable     - no protocol is defined
        ipIcmpEcho        - uses Echo Request/Reply as defined
                             in RFC792 for Internet Protocol
                             networks
        ipUdpEchoAppl     - uses the UDP based echo server
        snaRUEcho         - uses the REQECHO and ECHOTEST RU's
                             to an SSCP over an SNA LU-SSCP
                             session
        snaLU0EchoAppl    - uses test RU's sent to the Echo 
                             Server over an SNA LU0-LU0 session
        snaLU2EchoAppl    - uses test RU's sent to the Echo 
                             Server over an SNA LU2-LU2 session
        snaLU62Echo       - uses the native appn ping ie. aping 
        snaLU62EchoAppl   - uses test RU's sent to the ARR
                             Echo Server over an SNA LU6.2-LU6.2
                             session
        appleTalkEcho     - uses Echo Request/Reply as defined
                             for appleTalk networks
        appleTalkEchoAppl - uses the appleTalk based echo
                             server
        decNetEcho        - uses Echo Request/Reply as defined
                             for DECNet networks
        decNetEchoAppl    - uses the DECnet based echo server
        ipxEcho           - uses Echo Request/Reply as defined
                             for Novell IPX networks
        ipxEchoAppl       - uses the Novel IPX based echo
                             server
        isoClnsEcho       - uses Echo Request/Reply as defined
                             for ISO CLNS networks
        isoClnsEchoAppl   - uses the ISO CLNS based echo
                             server
        vinesEcho         - uses Echo Request/Reply as defined
                             for VINES networks
        vinesEchoAppl     - uses the VINES based echo server
        xnsEcho           - uses Echo Request/Reply as defined
                             for XNS networks
        xnsEchoAppl       - uses the XNS based echo server
        apolloEcho        - uses Echo Request/Reply as defined
                             for APOLLO networks
        apolloEchoAppl    - uses the APOLLO based echo
                             server
        netbiosEchoAppl   - uses the netbios based echo
                             server
        ipTcpConn         - uses the tcp's connect mechanism
        httpAppl          - uses udp for name resolution, 
                            tcp connect and tcp data transfer
                            mechanisms for HTTP data download
                            from a particular HTTP Server
        dnsAppl           - uses udp for name resolution
        jitterAppl        - uses udp for packet transfers
        dlswAppl          - uses tcp for sending keepalives
        dhcpAppl          - uses udp for sending dhcp requests
        ftpAppl           - uses tcp for connect & data transfer
        mplsLspPingAppl   - uses MPLS Echo Request/Response as per
                            draft-ietf-mpls-lsp-ping-04 ietf
                            standard
        voipAppl          - uses Symphony infrastructure to measure
                            H.323/SIP call set up time
        rtpAppl           - uses Symphony infrastructure to measure
                            rtp packets delay variance.
        icmpJitterAppl    - uses ICMP Timestamp for packet transfer 
                            to measure jitter.
        ethernetPingAppl    - uses regular 802.1ag loopback frame
        ethernetJitterAppl  - uses CFM frames .
        videoAppl           - uses synthetic traffic depending on video 
                                         profile
        y1731dmm            - used to measure Y1731 delay
        y17311dm            - used to measure Y1731 1DM
        y1731lmm            - used to measure Y1731 Loss measurement
        y1731slm            - used to measure Y1731 Synthetic Loss measurement
        mcastJitterAppl     - uses udp jitter to measure multicast network
                              performance"
    SYNTAX          INTEGER  {
                        notApplicable(1),
                        ipIcmpEcho(2),
                        ipUdpEchoAppl(3),
                        snaRUEcho(4),
                        snaLU0EchoAppl(5),
                        snaLU2EchoAppl(6),
                        snaLU62Echo(7),
                        snaLU62EchoAppl(8),
                        appleTalkEcho(9),
                        appleTalkEchoAppl(10),
                        decNetEcho(11),
                        decNetEchoAppl(12),
                        ipxEcho(13),
                        ipxEchoAppl(14),
                        isoClnsEcho(15),
                        isoClnsEchoAppl(16),
                        vinesEcho(17),
                        vinesEchoAppl(18),
                        xnsEcho(19),
                        xnsEchoAppl(20),
                        apolloEcho(21),
                        apolloEchoAppl(22),
                        netbiosEchoAppl(23),
                        ipTcpConn(24),
                        httpAppl(25),
                        dnsAppl(26),
                        jitterAppl(27),
                        dlswAppl(28),
                        dhcpAppl(29),
                        ftpAppl(30),
                        mplsLspPingAppl(31),
                        voipAppl(32),
                        rtpAppl(33),
                        icmpJitterAppl(34),
                        ethernetPingAppl(35),
                        ethernetJitterAppl(36),
                        videoAppl(37),
                        y1731dmm(38),
                        y17311dm(39),
                        y1731lmm(40),
                        mcastJitterAppl(41),
                        y1731slm(42)
                    }

RttMonCodecType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Specifies the codec type to be used with the jitter probe.
        The following codec types are defined:

        notApplicable     - no CodecType is defined
        g711ulaw          - uses G.711 U Law 64000 bps
        g711alaw          - uses G.711 A Law 64000 bps
        g729a             - uses G.729 8000 bps"
    SYNTAX          INTEGER  {
                        notApplicable(0),
                        g711ulaw(1),
                        g711alaw(2),
                        g729a(3)
                    }

RttMonLSPPingReplyMode ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Specifies the Reply mode for the MPLS LSP Echo request
        packets. The following reply modes are supported:

        replyIpv4Udp(1)         - an mpls echo request will normally
                                 have reply via IPv4 UDP packets.
        replyIpv4UdpRA(2)       - reply via IPv4 UDP Router Alert. Used
                                 when IPv4 return path is deemed 
                                 unreliable."
    SYNTAX          INTEGER  {
                        replyIpv4Udp(1),
                        replyIpv4UdpRA(2)
                    }

RttMonTargetAddress ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "A string which specifies the address of the target for
        the RTT operation; a value of RttMonTargetAddress
        which corresponds to a 'broadcast' address is disallowed.

        The interpretation of this string depends on the type of
        RTT operation selected, as specified by RttMonProtocol; 
        consequently, this object cannot be created until 
        RttMonProtocol has been created (or must be in the same 
        PDU).

        SNA addresses will be provided in ASCII, but will be
        converted to EBCDIC

        It is interpreted as follows, for the specified values of
        RttMonProtocol:

        ipIcmpEcho, ipUdpEchoAppl, ipTcpConn, jitterAppl, dlswAppl,
        dnsAppl, httpAppl, and dhcpAppl
             - 4 octets

        snaRUEcho
             - N octets, containing the value of the sna
                HOSTNAME of which the SSCP LU will be used
                for the operation.  For many systems this value
                can be empty, and the system will use the
                implied SSCP LU.  For example 'NSPECHO'.

        snaLU0EchoAppl and snaLU2EchoAppl 
             - N octets, the first x octets are the HOSTNAME
                (Alternatively, this could be a PU name defined
                to transport to the desired HOST), the second
                y octets are the APPLID, and the last z octets 
                are the MODENAME of the Echo Server (blank 
                for a MODENAME default). The address will be 
                encoded with a size byte preceding each of 
                the x y and z called s. For example sxsysz 
                as in '0x06CWBC060x07NSPECHO0x00' where 
                HOSTNAME = CWBC06, APPLID = NSPECHO, and 
                MODENAME is defaulted to 8 blanks.  
                NOTE: MODENAME is either size 0 or 8.

        snaLU62Echo and snaLU62EchoAppl
             - N octets, the first x octets are the LU-NAME,
                the second y octets are the TP-NAME, and the 
                last z octets are the MODENAME of the Echo 
                Server.  The address will be encoded with a size
                byte preceding each of the x y and z called s.
                For example sxsysz (zero size before z for a
                MODENAME default).  The LU-NAME is composed of
                8 bytes '.' 8 bytes.  The Transaction Program
                name (TP-NAME) is 1-64 bytes.  The MODENAME
                is 8 bytes.

        appleTalkEcho, appleTalkEchoAppl

        decNetEcho, decNetEchoAppl

        ipxEcho, ipxEchoAppl

        isoClnsEcho, isoClnsEchoAppl

        vinesEcho, vinesEchoAppl

        xnsEcho, xnsEchoAppl
        apolloEcho, apolloEchoAppl

        netbiosEchoAppl, voipAppl
                - unsupported protocols.

        mplsLspPingAppl
                - 8 octets, the first 4 octets are the FEC address
                and the next 4 octets are the FEC address mask."
    SYNTAX          OCTET STRING

RttMonReactVar ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The following are specific Reaction variables for a
        particular probe type:
         rtt(1)            - Round Trip Time
         jitterSDAvg(2)    - Jitter average from source to Destination
         jitterDSAvg(3)    - Jitter average from destination to source
         packetLossSD(4)   - Packet loss from source to destination
         packetLossDS(5)   - Packet loss from destination to source
         mos(6)            - Mean Opinion Score
         timeout(7)        - Timeout of the Operation
         connectionLoss(8) - Connection Failed to the destination
         verifyError(9)    - Data corruption occurs
         jitterAvg(10)     - Jitter Average in both the directions
         icpif(11)         - Calculated Planning Impairment Factor
         packetMIA(12)     - Missing In Action
         packetLateArrival(13)   - Packets arriving Late
         packetOutOfSequence(14) - Packets arriving out of sequence
         maxOfPositiveSD(15)     - Maximum positive jitter from
                                   Source to Destination
         maxOfNegativeSD(16)     - Maximum negative jitter from
                                   Source to Destination
         maxOfPositiveDS(17)     - Maximum positive jitter from
                                   Destination to Source
         maxOfNegativeDS(18)     - Maximum negative jitter from
                                   Destination to Source.
         iaJitterDS(19)          - Inter arrival jitter from
                                   Destination to Source
         frameLossDS(20)         - Number of frame loss recorded
                                   at source DSP
         mosLQDS(21)             - Listener quality MOS at Source
         mosCQDS(22)             - Conversational quality MOS at source
         rFactorDS(23)           - R-Factor value at Destination.
         successivePacketLoss(24)- Successive Dropped Packet
         maxOfLatencyDS(25)      - Maximum Latency from Destination 
                                   to Source
         maxOfLatencySD(26)      - Maximum Latency from Source 
                                   to Destination
         latencyDSAvg(27)        - Latency average from Destination 
                                   to Source
         latencySDAvg(28)        - Latency average from Source 
                                   to Destination
         packetLoss(29)          - Packets loss in both directions
         iaJitterSD(30)          - Inter arrival jitter from
                                   Source to Destination
         mosCQSD(31)             - Conversational quality MOS at 
                                   Destination
         rFactorSD(32)           - R-Factor value at Destination."
    SYNTAX          INTEGER  {
                        rtt(1),
                        jitterSDAvg(2),
                        jitterDSAvg(3),
                        packetLossSD(4),
                        packetLossDS(5),
                        mos(6),
                        timeout(7),
                        connectionLoss(8),
                        verifyError(9),
                        jitterAvg(10),
                        icpif(11),
                        packetMIA(12),
                        packetLateArrival(13),
                        packetOutOfSequence(14),
                        maxOfPositiveSD(15),
                        maxOfNegativeSD(16),
                        maxOfPositiveDS(17),
                        maxOfNegativeDS(18),
                        iaJitterDS(19),
                        frameLossDS(20),
                        mosLQDS(21),
                        mosCQDS(22),
                        rFactorDS(23),
                        successivePacketLoss(24),
                        maxOfLatencyDS(25),
                        maxOfLatencySD(26),
                        latencyDSAvg(27),
                        latencySDAvg(28),
                        packetLoss(29),
                        iaJitterSD(30),
                        mosCQSD(31),
                        rFactorSD(32)
                    }

RttMonIdLst ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "A string that specifies a list of the IP SLA probe
        identifiers or other numeric identifiers.
        The identifiers will be specified in the following form.
        (a) Individual identifiers with comma separated as 1,5,3.
        (b) Range form including hyphens with multiple ranges
        being 
           separated by comma as 1-10,12-34.
        (c) Mix of the above two forms as 1,2,4-10,12,15,19-25."
    SYNTAX          OCTET STRING (SIZE (0..255))

RttMonCtrlIndex ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The value of this object identifies the row in the
        ipslaEthernetGrpCtrlTable and ipslaEthernetGrpReactTable.
        It can be used for other IP SLA control tables."
    SYNTAX          Unsigned32 (1..2147483647)

END








































