-- *****************************************************************
-- CISCO-DYNAMIC-ARP-INSPECTION-CAPABILITY.my:
-- Cisco CISCO-DYNAMIC-ARP-INSPECTION-MIB AGENT-CAPABILITIES
--   
-- January 2004, Edward Pham
--   
-- Copyright (c) 2004, 2007, 2010-2011 by Cisco Systems Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-DYNAMIC-ARP-INSPECTION-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    Unsigned32
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    RowStatus
        FROM SNMPv2-TC
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoDynamicArpInspCapability MODULE-IDENTITY
    LAST-UPDATED    "201103240000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "The capabilities description of
        CISCO-DYNAMIC-ARP-INSPECTION-MIB."
    REVISION        "201103240000Z"
    DESCRIPTION
        "Added cdaiCapV15R0002SGPCat4K agent
        capability statement."
    REVISION        "201005070000Z"
    DESCRIPTION
        "Added cdaiCapV12R0254SGPCat4K agent
        capability statement."
    REVISION        "200707020000Z"
    DESCRIPTION
        "Added cdaiCapV12R0233SXHPCat6k agent
        capability statement."
    REVISION        "200401130000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 382 }



cdaiCapabilityCatOSV08R0301Cat6k AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.3(1) on Catalyst 6000/6500
                          and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-DYNAMIC-ARP-INSPECTION-MIB capabilities."

    SUPPORTS        CISCO-DYNAMIC-ARP-INSPECTION-MIB
    INCLUDES        {
                        cdaiVlanConfigGroup,
                        cdaiGlobalLoggingGroup,
                        cdaiIfConfigGroup
                    }
    VARIATION       cdaiVlanDynArpInspEnable
    DESCRIPTION
        "Only support false(2) on management VLAN 1."

    ::= { ciscoDynamicArpInspCapability 1 }

cdaiCapV12R0233SXHPCat6k AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXH on Catalyst 6000/6500
                         series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-DYNAMIC-ARP-INSPECTION-MIB capabilities."

    SUPPORTS        CISCO-DYNAMIC-ARP-INSPECTION-MIB
    INCLUDES        {
                        cdaiVlanConfigGroup,
                        cdaiIfConfigGroup,
                        cdaiIfRateLimitGroup
                    }
    VARIATION       cdaiIfRateLimit
    SYNTAX          Unsigned32 (0..2048 | 4294967295)
    DESCRIPTION
        "Only limited set of values are supported."

    ::= { ciscoDynamicArpInspCapability 2 }

cdaiCapV12R0254SGPCat4K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(54)SG on Cat4K family switches."
    STATUS          current
    DESCRIPTION
        "CISCO-DYNAMIC-ARP-INSPECTION-MIB capabilities."

    SUPPORTS        CISCO-DYNAMIC-ARP-INSPECTION-MIB
    INCLUDES        {
                        cdaiVlanConfigGroup,
                        cdaiIfConfigGroup,
                        cdaiIfRateLimitGroup
                    }
    VARIATION       cdaiIfRateLimit
    SYNTAX          Unsigned32 (0..2048 | 4294967295)
    DESCRIPTION
        "Only limited set of values are supported."

    ::= { ciscoDynamicArpInspCapability 3 }

cdaiCapV15R0002SGPCat4K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 15.0(2)SG on Cat4K family switches."
    STATUS          current
    DESCRIPTION
        "CISCO-DYNAMIC-ARP-INSPECTION-MIB capabilities."

    SUPPORTS        CISCO-DYNAMIC-ARP-INSPECTION-MIB
    INCLUDES        {
                        cdaiVlanConfigGroup,
                        cdaiIfConfigGroup,
                        cdaiIfRateLimitGroup,
                        cdaiLoggingConfigGroup,
                        cdaiAddressValidationGroup,
                        cdaiVlanCfgGroup,
                        cdaiVlanStatisticsGroup,
                        cdaiLogBufferGroup,
                        cdaiVlanExtStatisticsGroup,
                        cdaiVlanArpProbeGroup,
                        cdaiLogBufferActionGroup
                    }
    VARIATION       cdaiIfRateLimit
    SYNTAX          Unsigned32 (0..2048 | 4294967295)
    DESCRIPTION
        "Only limited set of values are supported."

    VARIATION       cdaiLogBufferSize
    SYNTAX          Unsigned32 (0..1024)
    DESCRIPTION
        "Only limited set of values are supported."

    VARIATION       cdaiLoggingRate
    SYNTAX          Unsigned32 (0..1024)
    DESCRIPTION
        "Only limited set of values are supported."

    VARIATION       cdaiLoggingInterval
    SYNTAX          Unsigned32 (0..86400)
    DESCRIPTION
        "Only limited set of values are supported."

    VARIATION       cdaiVlanCfgStorageType
    ACCESS          read-only
    DESCRIPTION
        "Write-access is not supported."

    VARIATION       cdaiVlanCfgRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only limited set of values are supported."

    ::= { ciscoDynamicArpInspCapability 4 }

END



