-- *****************************************************************
-- CISCO-SSG-MIB.my:  MIB file for SSG Multi-service Gateway
--
-- January 2002, Thamilarasu K,  October 2003, Sheetal Tilve
--
-- Copyright (c) 1996, 2002, 2003, 2005 by cisco Systems, Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-SSG-MIB DEFINITIONS ::= BEGIN

IMPORTS
        MODULE-IDENTITY,
        OBJECT-TYPE,
        Counter32,
        Gauge32,
        Unsigned32,
        NOTIFICATION-TYPE
            FROM SNMPv2-SMI
        MODULE-COMPLIANCE,
        NOTIFICATION-GROUP,
        OBJECT-GROUP
            FROM SNMPv2-CONF
        TimeInterval,
        DateAndTime,
        TruthValue,
        DisplayString,
        RowStatus
            FROM SNMPv2-TC
        InetAddressType,
        InetAddress
            FROM INET-ADDRESS-MIB
        InterfaceIndex
            FROM IF-MIB
        CiscoPort
            FROM CISCO-TC
        ciscoMgmt
            FROM CISCO-SMI;

ciscoSsgMIB MODULE-IDENTITY
        LAST-UPDATED        "200512220000Z"
        ORGANIZATION        "Cisco Systems, Inc."
        CONTACT-INFO
                "       Cisco Systems
                        Customer Service

                Postal: 170 W Tasman Drive
                        San Jose, CA  95134
                        USA

                   Tel: +1 800 553-NETS

                E-mail: cs-ssg@cisco.com"
        DESCRIPTION
                "The MIB Module manages Service Selection Gateway(SSG)
                devices.
                
                Service Selection Gateway(SSG) is a switching solution
                for service providers who offer intranet,extranet, and
                Internet connections to subscribers using broadband
                access technology such as digital subscriber lines,
                cable modems, or wireless to allow simultaneous access
                to network services.
                
                Acronyms and terms:
                
                SSD   Service Selection Dashboard
                SESM  Subscriber Edge Service Manager
                GGSN  Gateway GPRS Support Node
                APN   Access Point Name"
        REVISION        "200512220000Z"
        DESCRIPTION  
                "Imported Unsigned32 from SNMPv2-SMI instead 
                 of CISCO-TC."
        REVISION        "200310170000Z"
        DESCRIPTION
                "Added new objects for Transparent Auto-Logon
                 feature."
        REVISION        "200203250000Z"
        DESCRIPTION
                "Initial version of this MIB module."
        ::= { ciscoMgmt 260 }



ciscoSsgMIBObjects OBJECT IDENTIFIER ::=  { ciscoSsgMIB 1 }

cssgCfgObjects          OBJECT IDENTIFIER ::=  { ciscoSsgMIBObjects 1 }
cssgStatsObjects        OBJECT IDENTIFIER ::=  { ciscoSsgMIBObjects 2 }
cssgService             OBJECT IDENTIFIER ::=  { ciscoSsgMIBObjects 3 }
cssgExcludedAPN         OBJECT IDENTIFIER ::=  { ciscoSsgMIBObjects 4 }
cssgExcludedDomain      OBJECT IDENTIFIER ::=  { ciscoSsgMIBObjects 5 }
cssgTcpRedirect         OBJECT IDENTIFIER ::=  { ciscoSsgMIBObjects 6 }
cssgServiceIfBinds      OBJECT IDENTIFIER ::=  { ciscoSsgMIBObjects 7 }
cssgRadiusClients       OBJECT IDENTIFIER ::=  { ciscoSsgMIBObjects 8 }
cssgPortMap             OBJECT IDENTIFIER ::=  { ciscoSsgMIBObjects 9 }
cssgTal                 OBJECT IDENTIFIER ::=  { ciscoSsgMIBObjects 10 }

cssgCfgSsgEnabled OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "An indication of whether SSG Service is enabled."
    ::= { cssgCfgObjects 1 }

cssgCfgAutoDomainMode OBJECT-TYPE
    SYNTAX INTEGER {
               disabled(1),
               basic(2),
               extended(3)
           }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "An indication of whether Auto-Domain feature is enabled.
        This feature allows a user to be automatically connected
        to a service based on the APN or structured username."
    ::= { cssgCfgObjects 2 }


cssgCfgLocalForwardingEnabled OBJECT-TYPE
    SYNTAX         TruthValue
    MAX-ACCESS     read-write
    STATUS         current
    DESCRIPTION
        "An indication of whether Local Forwarding is enabled.
        This feature enables SSG to forward packets
        locally between connected subscribers."
    ::= { cssgCfgObjects 3 }

cssgCfgAutoLogOffMode OBJECT-TYPE
    SYNTAX       INTEGER {
                    disabled(1),
                    icmp(2),
                    arp(3)
                 }
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "An indication of whether Auto Logoff feature is enabled.
        This feature enables SSG to initiate logoff if connectivity
        to a host is lost.  Connectivity to a host is checked using
        ARP or ICMP ping mechanisms."
    ::= { cssgCfgObjects 4 }

cssgCfgRadiusProxyEnabled OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "An indication of whether Radius-Proxy feature is enabled.
        This feature allows SSG to act as a generic Radius Proxy
        for non-SSD clients such as GGSN."
    ::= { cssgCfgObjects 5 }

cssgCfgTcpRedirectEnabled OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "An indication of whether TCP redirect is enabled.  This
        feature redirects certain TCP packets to captive portals."
    ::= { cssgCfgObjects 6 }

cssgCfgAutoDomainNatEnabled OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "An indication of whether NAT(Network Address Translation)
        is enabled for autodomain users. This feature determines 
        whether the subscriber gets the autodomain service assigned
        IP Address."
    ::= { cssgCfgObjects 7 }

cssgCfgPortBundleHostKeyEnabled OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "An indication of whether PortBundle-Host Key feature is 
        enabled. This feature enables SESM to identify subscribers
        based on the PortBundle(combination of IP Address, and a
        range of ports) assigned by the SSG."
    ::= { cssgCfgObjects 8 }

cssgCfgTransPassThroughEnabled OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "An indication of whether Transparent pass through feature is
        enabled.  This feature allows an unauthenticated subscriber
        traffic to be routed through SSG in either direction."
    ::= { cssgCfgObjects 9 }

cssgCfgAutoLogOffInterval OBJECT-TYPE
    SYNTAX       TimeInterval
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "The time-interval at which connectivity to a host is checked. 
        If the host is not reachable, SSG logs off the host if 
        auto-logff feature is enabled."
    ::= { cssgCfgObjects 10 }

cssgCfgAutoLogOffIcmpRetries OBJECT-TYPE
    SYNTAX        Unsigned32 (1..65535)
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The number of ICMP ping retries SSG does to check
        connectivity to a host."
    DEFVAL        { 2 }
    ::= { cssgCfgObjects 11 }

cssgCfgMaxServicesPerUser OBJECT-TYPE
    SYNTAX        Unsigned32 (1..20)
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The maximum number of services allowed per user."
    ::= { cssgCfgObjects 12 }

cssgCfgAccountingEnabled OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "An indication of whether Acccounting is enabled in SSG.
        If enabled, SSG generates Accounting Records and sends to
        AAA Server."
    ::= { cssgCfgObjects 13 }

cssgCfgDefaultNetworkType OBJECT-TYPE
    SYNTAX        InetAddressType
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "A value that represents the type of the IP Address
        stored in the object cssgCfgDefaultNetwork."
    ::= { cssgCfgObjects 14 }

cssgCfgDefaultNetwork OBJECT-TYPE
    SYNTAX        InetAddress
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The IP Address or subnet that users will be able to access
        without authentication.  This is the address where the Cisco
        SSD/SESM resides."
    ::= { cssgCfgObjects 15 }
  
cssgCfgRadiusAuthenPort OBJECT-TYPE
    SYNTAX        CiscoPort
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The port on which SSG receives access request packets from
        Radius clients."
    ::= { cssgCfgObjects 16 }
    
cssgCfgRadiusAccountingPort OBJECT-TYPE
    SYNTAX        CiscoPort
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The port on which SSG receives accounting packets from Radius
        clients."
    ::= { cssgCfgObjects 17 }

cssgCfgRadiusFwdAcctPktsEnabled OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "An indication of whether SSG forwards Accounting Packets
        received from Radius Clients to AAA Server."
    ::= { cssgCfgObjects 18 }

cssgCfgAccountingInterval OBJECT-TYPE
    SYNTAX         Unsigned32 (60..2147483647)
    UNITS          "seconds"
    MAX-ACCESS     read-write
    STATUS         current
    DESCRIPTION
        "The interval at which Accounting records are sent to AAA
        Server."
    ::= { cssgCfgObjects 19 }

cssgCfgTCPRedirGrpForUnAuthUsers OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The TCP Redirect Group to which Unauthenticated users are
        directed."
    ::= { cssgCfgObjects 20 }

cssgCfgTCPRedirGrpForUnAuthServ OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The TCP Redirect Group to which unauthorized service access
        users are directed."
    ::= { cssgCfgObjects 21 }

cssgCfgTcpRedirGrpForSMTP OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "TCP Redirect Group to which SMTP traffic is redirected."
    ::= { cssgCfgObjects 22 }

cssgCfgTcpRedirGrpForInitialCapt OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The TCP Redirect Group for initial captivation."
    ::= { cssgCfgObjects 23 }

cssgCfgTcpRedirGrpForAdvCapt OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The TCP Redirect Group for advertising captivation."
    ::= { cssgCfgObjects 24 }

cssgCfgRadiusClntRbtNotifEnabled OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "An indication of whether SSG generates notification if a
        Radius Client reboots."
    DEFVAL        { false }
    ::= { cssgCfgObjects 25 }

cssgCfgAAAServerDownNotifEnabled OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "An indication of whether SSG generates notification if
        connectivity to AAA is lost or if it goes down."
    DEFVAL        { false }
    ::= { cssgCfgObjects 26 }

cssgCfgTalEnabled OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "An indication of whether Transparent Auto Logon feature
         is enabled on SSG." 
    DEFVAL        { false }
    ::= { cssgCfgObjects 27 }

cssgStatsLoginAttempts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The number of login attempts onto SSG."
    ::= { cssgStatsObjects 1 }

cssgStatsLoginsSuccessful OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The number of successful logins onto SSG."
    ::= { cssgStatsObjects 2 }

cssgStatsActiveSessions OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The current number of active connections on SSG."
    ::= { cssgStatsObjects 3 }

cssgStatsActiveHosts OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The current number of active Hosts on SSG."
    ::= { cssgStatsObjects 4 }
    
cssgStatsActiveServices OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The current number of active services on SSG."
    ::= { cssgStatsObjects 5 }
        
cssgStatsPODs OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The number of Packets of Death sent to Radius Client."
    ::= { cssgStatsObjects 6 }

cssgServiceTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF CssgServiceEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A list of SSG Services which subscribers have logged onto.
        A Service entry in this table is transient data and gets
        removed when the last subscriber using this Service logs off."
    ::= { cssgService 1 }

cssgServiceEntry OBJECT-TYPE
    SYNTAX         CssgServiceEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
            "Detailed information concerning a Service."
    INDEX { cssgServiceName }
    ::= { cssgServiceTable 1 }

CssgServiceEntry ::= SEQUENCE {
    cssgServiceName                 DisplayString,
    cssgServiceMode                 INTEGER,
    cssgServiceType                 INTEGER,
    cssgServiceIdleTimeout          Unsigned32,
    cssgServiceSessionTimeout       Unsigned32,
    cssgServiceActiveSessions       Gauge32,
    cssgServiceDNSPrimaryIpType     InetAddressType,
    cssgServiceDNSPrimary           InetAddress,
    cssgServiceDNSSecondaryIpType   InetAddressType,
    cssgServiceDNSSecondary         InetAddress,
    cssgServiceUpstreamQOSEnabled   TruthValue,
    cssgServiceDownStreamQOSEnabled TruthValue,
    cssgServiceOpenGarden           TruthValue,
    cssgServicePrepaid              TruthValue
}

cssgServiceName OBJECT-TYPE
    SYNTAX         DisplayString (SIZE(1..32))
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "The name of the service profile."
    ::= { cssgServiceEntry 1 }

cssgServiceMode OBJECT-TYPE
    SYNTAX         INTEGER {
                       unknown(1),
                       concurrent(2),
                       sequential(3)
                   }
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "An optional attribute which defines whether the user is able
        to log in to a service while simultaneously connected to
        other services (concurrent) or cannot access any other
        services while using this service (sequential).
        The default is concurrent."
    DEFVAL { concurrent }
    ::= { cssgServiceEntry 2 }

cssgServiceType OBJECT-TYPE
    SYNTAX         INTEGER {
                       unknown(1),
                       passthrough(2),
                       tunnel(3),
                       proxy(4)
                   }
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "This attribute indicates the type of service.

             pass-through - Indicates that the user authentication is
                            not done during logon to this service.
                            This is the default.
                            
             tunnel       - Indicates that this is a L2TP tunneled
                            service.

             proxy        - Indicates that the SSG performs user
                            authentication during logon to this 
                            service."

    ::= { cssgServiceEntry 3 }

cssgServiceIdleTimeout OBJECT-TYPE
    SYNTAX         Unsigned32
    UNITS          "seconds"
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "The idle timeout of a session in seconds. A value of 0
        indicates that there is no timeout."
    ::= { cssgServiceEntry 4 }

cssgServiceSessionTimeout OBJECT-TYPE
    SYNTAX         Unsigned32
    UNITS          "seconds"
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "The maximum length of a session in seconds. A value of 0
        indicates that there is no timeout."
    ::= { cssgServiceEntry 5 }

cssgServiceActiveSessions OBJECT-TYPE
    SYNTAX         Gauge32
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "The active number of connections to this service."
    ::= { cssgServiceEntry 6 }

cssgServiceDNSPrimaryIpType OBJECT-TYPE
    SYNTAX         InetAddressType
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "The IP address type of Primary DNS Server for this service."
    ::= { cssgServiceEntry 7 }

cssgServiceDNSPrimary OBJECT-TYPE
    SYNTAX         InetAddress
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "The primary DNS server for this service."
    ::= { cssgServiceEntry 8 }

cssgServiceDNSSecondaryIpType OBJECT-TYPE
    SYNTAX         InetAddressType
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "The IP Address type of Secondary DNS Server for this service."
    ::= { cssgServiceEntry 9 }

cssgServiceDNSSecondary OBJECT-TYPE
    SYNTAX         InetAddress
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "The Secondary DNS Server for this service."
    ::= { cssgServiceEntry 10 }

cssgServiceUpstreamQOSEnabled OBJECT-TYPE
    SYNTAX         TruthValue
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "An indication of whether upstream policing is enabled for 
        this service."
    REFERENCE
        "The rate-limit features of Committed Access Rate(CAR)."
    ::= { cssgServiceEntry 11 }

cssgServiceDownStreamQOSEnabled OBJECT-TYPE
    SYNTAX         TruthValue
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "An indication of whether downstream policing is enabled for
        this service."
    REFERENCE
        "The rate-limit features of Committed Access Rate(CAR)."
    ::= { cssgServiceEntry 12 }

cssgServiceOpenGarden OBJECT-TYPE
    SYNTAX         TruthValue
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "An indication of whether this is a Open Garden service.  An
        Open Garden Service is a service that can be accessed without
        authentication."
    ::= { cssgServiceEntry 13 }

cssgServicePrepaid OBJECT-TYPE
    SYNTAX         TruthValue
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "An indication of whether this service is a prepaid service."
    ::= { cssgServiceEntry 14 }
  
cssgServiceRouteTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF CssgServiceRouteEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A list of route entries that belong to a particular service."
    ::= { cssgService 2 }
    
cssgServiceRouteEntry OBJECT-TYPE
    SYNTAX         CssgServiceRouteEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "An entry in Services Route Table."
    INDEX { cssgServiceName,
            cssgServiceRouteType,
            cssgServiceRouteAddr,
            cssgServiceRouteMaskType,
            cssgServiceRouteMask
          }
    ::= { cssgServiceRouteTable 1 }
    
CssgServiceRouteEntry ::= SEQUENCE {
    cssgServiceRouteType             InetAddressType,
    cssgServiceRouteAddr             InetAddress,
    cssgServiceRouteMaskType         InetAddressType,
    cssgServiceRouteMask             InetAddress,
    cssgServiceRoutePermission       INTEGER
}

cssgServiceRouteType OBJECT-TYPE
    SYNTAX         InetAddressType
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A value that represents the type of the address stored in
        cssgServiceServRouteAddr."
    ::= { cssgServiceRouteEntry 1 }

cssgServiceRouteAddr OBJECT-TYPE
    SYNTAX         InetAddress
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "The IP Address of the networks available to the user of
        this service."
    ::= { cssgServiceRouteEntry 2 }

cssgServiceRouteMaskType OBJECT-TYPE
    SYNTAX         InetAddressType
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A value that represents the type of the address stored in
        cssgServiceServRouteMask."
    ::= { cssgServiceRouteEntry 3 }

cssgServiceRouteMask OBJECT-TYPE
    SYNTAX         InetAddress
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "Indicate the mask to be ANDed with the destination address
        before being compared to the value in cssgServiceRouteAddr."
    ::= { cssgServiceRouteEntry 4 }

cssgServiceRoutePermission OBJECT-TYPE
    SYNTAX         INTEGER {
                       permit(1),
                       deny(2)
                   }
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
        "Indicates the action on packets, when the destination 
        address matches with the cssgServiceRouteAddr."
    ::= { cssgServiceRouteEntry 5 }

    
cssgExcludedAPNTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF CssgExcludedAPNEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A list of APNs excluded from using auto-main feature of SSG."
    ::= { cssgExcludedAPN 1 }

cssgExcludedAPNEntry OBJECT-TYPE
    SYNTAX      CssgExcludedAPNEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information concerning an APN."
    INDEX { cssgExcludedAPNName }
    ::= { cssgExcludedAPNTable 1 }

CssgExcludedAPNEntry  ::= SEQUENCE {

    cssgExcludedAPNName      DisplayString,
    cssgExcludedAPNRowStatus RowStatus
}

cssgExcludedAPNName OBJECT-TYPE
    SYNTAX         DisplayString (SIZE(1..32))
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "The name of the excluded APN."
    ::= { cssgExcludedAPNEntry 1 }

cssgExcludedAPNRowStatus OBJECT-TYPE
    SYNTAX         RowStatus
    MAX-ACCESS     read-create
    STATUS         current
    DESCRIPTION
        "The status of this table entry.
        
        This object can also be used to create or delete conceptual
        row in this table.

        To create a row, set this object to 'createAndGo'.
        There are no mandatory objects in a create request.

        To delete a row, set this object to 'destroy'."
    ::= { cssgExcludedAPNEntry 2 }

cssgExcludedDomainTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF CssgExcludedDomainEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A list of Domain names excluded from using auto-domain
        feature of SSG."
    ::= { cssgExcludedDomain 1 }

cssgExcludedDomainEntry OBJECT-TYPE
    SYNTAX      CssgExcludedDomainEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Information concerning an excluded Domain."
    INDEX { cssgExcludedDomainName }
    ::= { cssgExcludedDomainTable 1 }

CssgExcludedDomainEntry  ::= SEQUENCE {

    cssgExcludedDomainName      DisplayString,
    cssgExcludedDomainRowStatus RowStatus
}

cssgExcludedDomainName OBJECT-TYPE
    SYNTAX         DisplayString (SIZE(1..32))
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "The name of the excluded Domain."
    ::= { cssgExcludedDomainEntry 1 }

cssgExcludedDomainRowStatus OBJECT-TYPE
    SYNTAX         RowStatus
    MAX-ACCESS     read-create
    STATUS         current
    DESCRIPTION
        "The status of this table entry.
        
        This object can also be used to create or delete conceptual
        row in this table.

        To create a row, set this object to 'createAndGo'.
        There are no mandatory objects in a create request.

        To delete a row, set this object to 'destroy'."
    ::= { cssgExcludedDomainEntry 2 }

cssgServiceIfBindTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF CssgServiceIfBindEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "In SSG, a Service can be configured to use a particular
        interface/ip address.  This table is a list of services and
        the interface to which they are bound."
    ::= { cssgServiceIfBinds 1 }
    
cssgServiceIfBindEntry OBJECT-TYPE
    SYNTAX         CssgServiceIfBindEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A Interface-Service Bind entry."
    INDEX { cssgServiceName }
    ::= { cssgServiceIfBindTable 1 }
    
CssgServiceIfBindEntry ::= SEQUENCE {
    cssgServiceIfIndex     InterfaceIndex,
    cssgServiceIfRowStatus RowStatus
}

cssgServiceIfIndex OBJECT-TYPE
    SYNTAX       InterfaceIndex
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The interface index to which the Service is bound."
    ::= { cssgServiceIfBindEntry 1 }

cssgServiceIfRowStatus OBJECT-TYPE
    SYNTAX       RowStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The status of this table entry.
        
        This object can also be used to create or delete conceptual
        row in this table.

        To create a row, set this object to 'createAndGo'.
        cssgServiceIfIndex is a mandatory object for a create request.

        To delete a row, set this object to 'destroy'."
    ::= { cssgServiceIfBindEntry 2 }

cssgTcpRedirectGrpTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CssgTcpRedirectGrpEntry
    MAX-ACCESS  not-accessible
    STATUS         current
    DESCRIPTION
        "A list of TCP Redirect group.  A TCP Redirect group is
        a list of one more servers that make up a captive portal
        group."
    ::= { cssgTcpRedirect 1 }

cssgTcpRedirectGrpEntry OBJECT-TYPE
    SYNTAX         CssgTcpRedirectGrpEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "Detailed information concerning a TCP Redirect group."
    INDEX { cssgTcpRedirectGrpName,
            cssgTcpRedirectGrpServerAddrType,
            cssgTcpRedirectGrpServerAddr,
            cssgTcpRedirectGrpServerPort
          }
    ::= { cssgTcpRedirectGrpTable 1 }

CssgTcpRedirectGrpEntry  ::= SEQUENCE {
    cssgTcpRedirectGrpName  DisplayString,
    cssgTcpRedirectGrpServerAddrType  InetAddressType,
    cssgTcpRedirectGrpServerAddr      InetAddress,
    cssgTcpRedirectGrpServerPort      CiscoPort,
    cssgTcpRedirectGrpRowStatus       RowStatus
}

cssgTcpRedirectGrpName OBJECT-TYPE
    SYNTAX         DisplayString (SIZE(1..32))
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "The name of the redirect-group."
    ::= { cssgTcpRedirectGrpEntry 1 }

cssgTcpRedirectGrpServerAddrType OBJECT-TYPE
    SYNTAX         InetAddressType
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A value that represents the typeof the address stored in
        cssgTcpRedirectGrpServerAddr object."
    ::= { cssgTcpRedirectGrpEntry 2 }

cssgTcpRedirectGrpServerAddr OBJECT-TYPE
    SYNTAX         InetAddress
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "The IP address of the server in the server-group."
    ::= { cssgTcpRedirectGrpEntry 3 }
    
cssgTcpRedirectGrpServerPort OBJECT-TYPE
    SYNTAX         CiscoPort
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "The port of the server to which TCP traffic to be redirected."
    ::= { cssgTcpRedirectGrpEntry 4 }

cssgTcpRedirectGrpRowStatus OBJECT-TYPE
    SYNTAX         RowStatus
    MAX-ACCESS     read-create
    STATUS         current
    DESCRIPTION
        "The status of this table entry.
        
        This object can also be used to create or delete conceptual
        row in this table.

        To create a row, set this object to 'createAndGo'.
        There are no mandatory objects in a create request.

        To delete a row, set this object to 'destroy'."
    ::= { cssgTcpRedirectGrpEntry 5 }
    
cssgNetworkGrpTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF CssgNetworkGrpEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A list of network groups.  When a network-group, a list of
        networks, associated with a TCP Redirect group, subscribers
        attempting to connect to these networks will be redirected to
        the TCP redirect group."
    ::= { cssgTcpRedirect 2 }
    
cssgNetworkGrpEntry OBJECT-TYPE
    SYNTAX         CssgNetworkGrpEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "Detailed information concerning a network group entry."
    INDEX { cssgNetworkGrpName,
            cssgNetworkGrpNetIpType,
            cssgNetworkGrpNetIpAddr,
            cssgNetworkGrpNetMaskType,
            cssgNetworkGrpNetMask
          }
    ::= { cssgNetworkGrpTable 1 }
    
CssgNetworkGrpEntry ::= SEQUENCE {
    cssgNetworkGrpName   DisplayString,
    cssgNetworkGrpNetIpType    InetAddressType,
    cssgNetworkGrpNetIpAddr    InetAddress,
    cssgNetworkGrpNetMaskType  InetAddressType,
    cssgNetworkGrpNetMask      InetAddress,
    cssgNetworkGrpNetRowStatus RowStatus
}   

cssgNetworkGrpName OBJECT-TYPE
    SYNTAX       DisplayString (SIZE(1..32))
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "The name of the network group.  A network group, which is a
        group of networks, is associated with a Server group for 
        traffic redirection i.e., packets to the networks in the network
        group will be directed to the servers in the server group."
    ::= { cssgNetworkGrpEntry 1 }

cssgNetworkGrpNetIpType OBJECT-TYPE
    SYNTAX    InetAddressType
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "A value that represents the type of the IP Address in the
        object cssgNetworkGrpNetIpAddr."
    ::= { cssgNetworkGrpEntry 2 }

cssgNetworkGrpNetIpAddr OBJECT-TYPE
    SYNTAX       InetAddress
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "The IP address of a network in this network group."
    ::= { cssgNetworkGrpEntry 3 }

cssgNetworkGrpNetMaskType OBJECT-TYPE
    SYNTAX       InetAddressType
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "A value that represents the type of the address stored in
        cssgNetworkGrpNetMask."
    ::= { cssgNetworkGrpEntry 4 }

cssgNetworkGrpNetMask OBJECT-TYPE
    SYNTAX       InetAddress
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Indicate the mask to be ANDed with the destination address
        before being compared to the value in cssgNetworkGrpNetIpAddr."
    ::= { cssgNetworkGrpEntry 5 }

cssgNetworkGrpNetRowStatus OBJECT-TYPE
    SYNTAX    RowStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The status of this table entry.
        
        This object can also be used to create or delete conceptual
        row in this table.

        To create a row, set this object to 'createAndGo'.
        There are no mandatory objects in a create request.

        To delete a row, set this object to 'destroy'."
    ::= { cssgNetworkGrpEntry 6 }

cssgPortGrpTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF CssgPortGrpEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A list of port groups."
    ::= { cssgTcpRedirect 3 }
    
cssgPortGrpEntry OBJECT-TYPE
    SYNTAX         CssgPortGrpEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A Port group entry."
    INDEX { cssgPortGrpName, cssgPortGrpPortNo }
    ::= { cssgPortGrpTable 1 }
    
CssgPortGrpEntry ::= SEQUENCE {
    cssgPortGrpName      DisplayString,
    cssgPortGrpPortNo    CiscoPort,
    cssgPortGrpPortRowStatus RowStatus
}   

cssgPortGrpName  OBJECT-TYPE
    SYNTAX    DisplayString (SIZE(1..32))
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "The name of the port group.  The port group defines a list
        of ports traffic to whom can be redirected to a TCP Redirect
        group."
    ::= { cssgPortGrpEntry 1 }

cssgPortGrpPortNo OBJECT-TYPE
    SYNTAX    CiscoPort
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A port in the port group."
    ::= { cssgPortGrpEntry 2 }

cssgPortGrpPortRowStatus OBJECT-TYPE
    SYNTAX    RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "The status of this table entry.
        
        This object can also be used to create or delete conceptual
        row in this table.

        To create a row, set this object to 'createAndGo'.

        To delete a row, set this object to 'destroy'."
    ::= { cssgPortGrpEntry 3 }

cssgTcpRedirNetworkGrpMapTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF CssgTcpRedirNetworkGrpMapEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A list of Network and Server Group associations."
    ::= { cssgTcpRedirect 4 }
    
cssgTcpRedirNetworkGrpMapEntry OBJECT-TYPE
    SYNTAX        CssgTcpRedirNetworkGrpMapEntry  
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Detailed information concerning a Server and Network
        group association."
    INDEX { cssgTcpRedirectGrpName }
    ::= { cssgTcpRedirNetworkGrpMapTable 1 }
    
CssgTcpRedirNetworkGrpMapEntry ::= SEQUENCE {
    cssgTcpRedirNetworkMapGrpName DisplayString,
    cssgTcpRedirNetworkGrpMapRowStat RowStatus
}

cssgTcpRedirNetworkMapGrpName OBJECT-TYPE
    SYNTAX     DisplayString (SIZE(1..32))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "A network group name.  A network group is a set of network
        groups that can be associated with TCP Redirect for traffic
        redirection."
    ::= { cssgTcpRedirNetworkGrpMapEntry 1 }

cssgTcpRedirNetworkGrpMapRowStat OBJECT-TYPE
    SYNTAX         RowStatus
    MAX-ACCESS     read-create
    STATUS         current
    DESCRIPTION
        "The status of this table entry.
        
        This object can also be used to create or delete conceptual
        row in this table.

        To create a row, set this object to 'createAndGo'.
        There are no mandatory objects in a create request.

        To delete a row, set this object to 'destroy'."
    ::= { cssgTcpRedirNetworkGrpMapEntry 2 }

cssgTcpRedirPortGrpMapTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF CssgTcpRedirPortGrpMapEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A list of Server and Port Group associations."
    ::= { cssgTcpRedirect 5 }
    
cssgTcpRedirPortGrpMapEntry OBJECT-TYPE
    SYNTAX        CssgTcpRedirPortGrpMapEntry  
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "An instance of Server and Port group association."
    INDEX { cssgTcpRedirectGrpName }
    ::= { cssgTcpRedirPortGrpMapTable 1 }
    
CssgTcpRedirPortGrpMapEntry ::= SEQUENCE {
    cssgTcpRedirPortMapGrpName DisplayString,
    cssgTcpRedirPortGrpMapRowStat RowStatus
}

cssgTcpRedirPortMapGrpName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The name of the Port Group.  A Port Group is a set of ports
        that can be associated with a TCP Redirect Group for traffic
        redirection."
    ::= { cssgTcpRedirPortGrpMapEntry 1 }

cssgTcpRedirPortGrpMapRowStat OBJECT-TYPE
    SYNTAX         RowStatus
    MAX-ACCESS     read-create
    STATUS         current
    DESCRIPTION
        "The status of this table entry.
        
        This object can also be used to create or delete conceptual
        row in this table.

        To create a row, set this object to 'createAndGo'.
        There are no mandatory objects in a create request.

        To delete a row, set this object to 'destroy'."
    ::= { cssgTcpRedirPortGrpMapEntry 2 }
    

cssgTcpRedirPortNoMapTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF CssgTcpRedirPortNoMapEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A list of Ports nos and the corresponding Server group
        which they are associated with."
    ::= { cssgTcpRedirect 6 }
    
cssgTcpRedirPortNoMapEntry OBJECT-TYPE
    SYNTAX        CssgTcpRedirPortNoMapEntry  
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "An instance of a Server group and Port association."
    INDEX { cssgTcpRedirectGrpName }
    ::= { cssgTcpRedirPortNoMapTable 1 }
    
CssgTcpRedirPortNoMapEntry ::= SEQUENCE {
    cssgTcpRedirPortNo           CiscoPort,
    cssgTcpRedirPortNoMapRowStat RowStatus
}

cssgTcpRedirPortNo OBJECT-TYPE
    SYNTAX      CiscoPort
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The Port No associated with the Service Group name."
    ::= { cssgTcpRedirPortNoMapEntry 1 }

cssgTcpRedirPortNoMapRowStat OBJECT-TYPE
    SYNTAX         RowStatus
    MAX-ACCESS     read-create
    STATUS         current
    DESCRIPTION
        "The status of this table entry.
        
        This object can also be used to create or delete conceptual
        row in this table.

        To create a row, set this object to 'createAndGo'.
        cssgTcpRedirPortNo is a  mandatory object for a create request.

        To delete a row, set this object to 'destroy'."
    ::= { cssgTcpRedirPortNoMapEntry 2 }

cssgRadiusClientTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF CssgRadiusClientEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A list of non-SSD clients to which SSG act as Radius
        proxy."
    ::= { cssgRadiusClients 1 }

cssgRadiusClientEntry OBJECT-TYPE
    SYNTAX         CssgRadiusClientEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "Detailed information concerning a Radius client entry."
    INDEX {
            cssgRadiusClientAddrType,
            cssgRadiusClientAddr
          }
    ::= { cssgRadiusClientTable 1 }

CssgRadiusClientEntry ::= SEQUENCE {

    cssgRadiusClientAddrType InetAddressType,
    cssgRadiusClientAddr     InetAddress,
    cssgRadiusClientRowStatus RowStatus
}

cssgRadiusClientAddrType OBJECT-TYPE
    SYNTAX         InetAddressType
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "The type of the address stored in cssgRadiusClientAddr."
    ::= { cssgRadiusClientEntry 1 }

cssgRadiusClientAddr OBJECT-TYPE
    SYNTAX         InetAddress
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "The network layer address of the Radius client to which 
        SSG acts as Radius Proxy."
    ::= { cssgRadiusClientEntry 2 }
    
cssgRadiusClientRowStatus OBJECT-TYPE    
    SYNTAX         RowStatus
    MAX-ACCESS     read-create
    STATUS         current
    DESCRIPTION
        "The status of this table entry.
        
        This object can also be used to create or delete conceptual
        row in this table.

        To create a row, set this object to 'createAndGo'.
        There are no mandatory objects in a create request.

        To delete a row, set this object to 'destroy'."
    ::= { cssgRadiusClientEntry 3 }
        
cssgPortMapLength OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The length of the port-bundle i.e, no of ports in a bundle."
    ::= { cssgPortMap 1 }
      
cssgPortMapTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CssgPortMapEntry
    MAX-ACCESS  not-accessible
    STATUS         current
    DESCRIPTION
        "The list of TCP Port-maps."
    ::= { cssgPortMap 2 }
     
cssgPortMapEntry OBJECT-TYPE
    SYNTAX         CssgPortMapEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "An entry in the cssgPortMapTable."
    INDEX {
            cssgPortMapSourceIpType,
            cssgPortMapSourceIp
          }
    ::= { cssgPortMapTable 1 }

CssgPortMapEntry ::= SEQUENCE {

    cssgPortMapSourceIpType InetAddressType,
    cssgPortMapSourceIp     InetAddress,
    cssgPortMapPortRangeFrom CiscoPort,
    cssgPortMapPortRangeTo   CiscoPort,
    cssgPortMapRowStatus  RowStatus
}

cssgPortMapSourceIpType OBJECT-TYPE
    SYNTAX         InetAddressType
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "A value that represents the type of the IP address stored
        in cssgPortMapSourceIP object."
    ::= { cssgPortMapEntry 1 }

cssgPortMapSourceIp OBJECT-TYPE
    SYNTAX         InetAddress
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "Specifies SSG source IP addresses to be used 
        while NATting packets from downstream traffic i.e.,
        traffic from Subscriber to SSG."
    ::= { cssgPortMapEntry 2 }
    
cssgPortMapPortRangeFrom OBJECT-TYPE
    SYNTAX         CiscoPort
    MAX-ACCESS     read-create
    STATUS         current
    DESCRIPTION
        "The lower limit of the range ports in the Port Map."
    ::= { cssgPortMapEntry 3 }

cssgPortMapPortRangeTo OBJECT-TYPE
    SYNTAX         CiscoPort
    MAX-ACCESS     read-create
    STATUS         current
    DESCRIPTION
        "The upper limit of the range ports in the Port Map."
    ::= { cssgPortMapEntry 4 }
    
    
cssgPortMapRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this table entry.
        
        This object can also be used to create or delete conceptual
        row in this table.

        To create a row, set this object to 'createAndGo'.
        cssgPortMapPortRangeFrom and cssgPortMapPortRangeTo are
        mandatory objects in a create request.

        To delete a row, set this object to 'destroy'."
    ::= { cssgPortMapEntry 5 }

cssgTalWaitingForAuthUsers OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of currently existing users waiting for
         authorization."
    ::= { cssgTal 1 }

cssgTalUnidentifiedUsers OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of currently existing unidentified users. These
         are users for which there was no response received from AAA
         and hence it is not clear if they are valid users."
    ::= { cssgTal 2 }

cssgTalSuspectUsers OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of currently existing Suspect Users."
    ::= { cssgTal 3 }

cssgTalPassthroughUsers OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of currently existing transparent pass-through
         users."
    ::= { cssgTal 4 }

cssgTalMaxAuthRate OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum rate of authorization requests per second.
         At a given time, the maximum rate of authorization requests
         will overwrite the previous value."
    ::= { cssgTal 5 }

cssgTalMaxAuthRateTimestamp OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the local time on the SSG when the Maximum rate
         of authorization requests per second, indicated by 
         cssgTalMaxAuthRate, was recorded."
    ::= { cssgTal 6 }

cssgTalMinAuthRate OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Minimum rate of authorization requests per second.
         At a given time, the minimum rate of authorization
         requests will overwrite the previous value."
    ::= { cssgTal 7 }

cssgTalMinAuthRateTimestamp OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the local time on the SSG when the Minimum rate
         of authorization requests per second, indicated by 
         cssgTalMinAuthRate, was recorded."
    ::= { cssgTal 8 }

cssgTalCurrentAuthRate OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The last recorded rate of authorization requests per second, 
         on SSG." 
    ::= { cssgTal 9 }

cssgTalCurrentAuthRateTimestamp OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the local time on the SSG when cssgTalCurrentAuthRate,
         was recorded."
    ::= { cssgTal 10 }

cssgTalResetAuthRates OBJECT-TYPE
    SYNTAX      INTEGER {
                   unknown(1),
                   reset(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Setting this variable to 'reset' indicates that the Minimum
         and Maximum rates of authorization would be reset to the 
         last recorded rate of authorization requests per second.
         Setting it to 'unknown' will not result in any changes.
         An snmp-get on this value will always return 'unknown'."
    ::= { cssgTal 11 }

cssgTalMaxPendingAuthReqs OBJECT-TYPE
    SYNTAX      Unsigned32 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The maximum number of outstanding TAL authorization 
         requests allowed on SSG. If the number of authorization 
         requests goes beyond this value, SSG does a SYS log 
         message and any packets received that would result in 
         SSG sending a new radius request will be dropped at the 
         CEF path itself. 
         When this value is set, it will be applicable from that 
         point onwards. If the number of existing requests exceeds 
         the new values, these requests will not be discarded."
    ::= { cssgTal 12 }

cssgTalMaxAuthReqsRate OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The maximum number of authorization requests per second 
         allowed on SSG. If this value is set, SSG throttles the 
         authorization requests sent per second as per this value."
    ::= { cssgTal 13 }

cssgTalDropPakDuringAuthorization OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value 'true' indicates that any packets that are 
         received from the user during user authorization would 
         be dropped. The value 'false' indicates that the packets 
         will not be dropped." 
    DEFVAL      { false }
    ::= { cssgTal 14 }

cssgTalUnidentifiedUserAllowTraff OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value 'true' indicates that traffic from/to 
         unidentified users would be allowed. A value of 'false' 
         indicates that traffic from/to unidentified users will 
         not be allowed."
    DEFVAL      { false }
    ::= { cssgTal 15 }

cssgTalMaxSuspectUsers OBJECT-TYPE
    SYNTAX      Unsigned32 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The maximum number of suspect users allowed."
    DEFVAL      { 5000 }
    ::= { cssgTal 16 }

cssgTalSuspectUserTimeout OBJECT-TYPE
    SYNTAX      Unsigned32 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The timeout value for a suspect user in minutes.
         If a packet is received for a suspect user, then packets
         from/to this user will be dropped/tcp-redirected, until 
         a value of cssgTalSuspectUserTimeout is reached. 
         After this timeout, any new traffic received by SSG from the 
         suspect user will trigger the TAL procedure all over again."
    DEFVAL      { 60 }
    ::= { cssgTal 17 }

cssgTalUnidentifiedUserTimeout OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The timeout value for an unidentified user in minutes.
         After this time expiry, authorization will be done again 
         when a packet is received from this user."
    DEFVAL      { 10 }
    ::= { cssgTal 18 }

cssgTalUserInfoTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF CssgTalUserInfoEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                 "A list of all the transparent users, along with 
                  their user-state."
         ::= { cssgTal 19 }

cssgTalUserInfoEntry OBJECT-TYPE
         SYNTAX      CssgTalUserInfoEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                 "A conceptual row in the TAL user info table."
         INDEX { cssgTalUserIPAddressType, cssgTalUserIPAddress }
         ::= { cssgTalUserInfoTable 1 }

CssgTalUserInfoEntry ::=
         SEQUENCE {
             cssgTalUserIPAddressType InetAddressType,
             cssgTalUserIPAddress     InetAddress,
             cssgTalUserState         INTEGER
         }

cssgTalUserIPAddressType OBJECT-TYPE
         SYNTAX      InetAddressType
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                 "This is the IP address type of a particular
                  transparent user and is used as index (together with
                  cssgTalUserIPAddress) to identify a unique entry in
                  the Tal User Info table."
         ::= { cssgTalUserInfoEntry 1 }

cssgTalUserIPAddress OBJECT-TYPE
    SYNTAX       InetAddress
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "IP Address of the transparent user."
    ::= { cssgTalUserInfoEntry 2 }

cssgTalUserState OBJECT-TYPE
         SYNTAX      INTEGER {
                        other(1),
                        authorizing(2),
                        unidentified(3),
                        suspect(4),
                        passthrough(5)
                     }
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                 "The state of the transparent user."
         ::= { cssgTalUserInfoEntry 3 }

-- Notifications

ciscoSsgMIBNotifications OBJECT IDENTIFIER ::= { ciscoSsgMIB 0 }

ciscoSsgRadiusClientReboot NOTIFICATION-TYPE
    STATUS    current
    DESCRIPTION
        "The notification is sent when the connectivity to GGSN is
        lost."
    ::= { ciscoSsgMIBNotifications 1 }

ciscoSsgRadiusAAAServerDown NOTIFICATION-TYPE
    STATUS    current
    DESCRIPTION
        "The notification is sent when the connectivity to AAA is
        lost or when AAA Server is down."
    ::= { ciscoSsgMIBNotifications 2 }

ciscoSsgMIBConformance OBJECT IDENTIFIER ::= { ciscoSsgMIB 3 }
ciscoSsgMIBCompliances OBJECT IDENTIFIER ::= { ciscoSsgMIBConformance 1}
ciscoSsgMIBGroups      OBJECT IDENTIFIER ::= { ciscoSsgMIBConformance 2}


-- Conformance

ciscoSsgMIBCompliance MODULE-COMPLIANCE
    STATUS  deprecated -- superceded by ciscoSsgMIBComplianceRev1
    DESCRIPTION
        "The compliance statement for entities which implement
        CISCO-SSG-MIB."
    MODULE
        MANDATORY-GROUPS {
            ciscoSsgCfgGroup,
            ciscoSsgStatsGroup,
            ciscoSsgServicesGroup,
            ciscoSsgExclusionsGroup,
            ciscoSsgTcpRedirectGroup,
            ciscoSsgServiceInterfaceGroup,
            ciscoSsgRadiusClientsGroup,
            ciscoSsgPortMapGroup,
            ciscoSsgNotificationGroup

        }
    ::= { ciscoSsgMIBCompliances 1 }

ciscoSsgMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS current
    DESCRIPTION
        "The compliance statement for entities which implement
        CISCO-SSG-MIB."
    MODULE
        MANDATORY-GROUPS {
            ciscoSsgCfgGroupRev1,
            ciscoSsgStatsGroup,
            ciscoSsgServicesGroup,
            ciscoSsgExclusionsGroup,
            ciscoSsgTcpRedirectGroup,
            ciscoSsgServiceInterfaceGroup,
            ciscoSsgRadiusClientsGroup,
            ciscoSsgPortMapGroup,
            ciscoSsgNotificationGroup,
            ciscoSsgTalUserInfoGroup

        }
    ::= { ciscoSsgMIBCompliances 2 }

-- Units of Conformance

ciscoSsgCfgGroup OBJECT-GROUP
    OBJECTS {
        cssgCfgSsgEnabled,
        cssgCfgAutoDomainMode,
        cssgCfgLocalForwardingEnabled,
        cssgCfgAutoLogOffMode,
        cssgCfgRadiusProxyEnabled,
        cssgCfgTcpRedirectEnabled,
        cssgCfgAutoDomainNatEnabled,
        cssgCfgPortBundleHostKeyEnabled,
        cssgCfgTransPassThroughEnabled,
        cssgCfgAutoLogOffInterval,
        cssgCfgAutoLogOffIcmpRetries,
        cssgCfgMaxServicesPerUser,
        cssgCfgAccountingEnabled,
        cssgCfgDefaultNetworkType,
        cssgCfgDefaultNetwork,
        cssgCfgRadiusAuthenPort,
        cssgCfgRadiusAccountingPort,
        cssgCfgRadiusFwdAcctPktsEnabled,
        cssgCfgAccountingInterval,
        cssgCfgTCPRedirGrpForUnAuthUsers,
        cssgCfgTCPRedirGrpForUnAuthServ,
        cssgCfgTcpRedirGrpForSMTP,
        cssgCfgTcpRedirGrpForInitialCapt,
        cssgCfgTcpRedirGrpForAdvCapt,
        cssgCfgRadiusClntRbtNotifEnabled,
        cssgCfgAAAServerDownNotifEnabled
    }
    STATUS deprecated -- superceded by ciscoSsgCfgGroupRev1
    DESCRIPTION
        "A collection of configurable parameters in SSG MIB."
    ::= { ciscoSsgMIBGroups 1 }

ciscoSsgStatsGroup OBJECT-GROUP
    OBJECTS {
        cssgStatsLoginAttempts,
        cssgStatsLoginsSuccessful,
        cssgStatsActiveSessions,
        cssgStatsActiveHosts,
        cssgStatsActiveServices,
        cssgStatsPODs 
    }
    STATUS current
    DESCRIPTION
        "A collection of statistics objects for SSG MIB."
    ::= { ciscoSsgMIBGroups 2 }

ciscoSsgServicesGroup OBJECT-GROUP
    OBJECTS {
        cssgServiceMode,
        cssgServiceType,
        cssgServiceIdleTimeout,
        cssgServiceSessionTimeout,
        cssgServiceActiveSessions,
        cssgServiceDNSPrimaryIpType,
        cssgServiceDNSPrimary,
        cssgServiceDNSSecondaryIpType,
        cssgServiceDNSSecondary,
        cssgServiceUpstreamQOSEnabled,
        cssgServiceDownStreamQOSEnabled,
        cssgServiceOpenGarden,
        cssgServicePrepaid,
        cssgServiceRoutePermission
    }
    STATUS current
    DESCRIPTION
        "A collection of objects pertaining to Services."
    ::= { ciscoSsgMIBGroups 3 }

ciscoSsgExclusionsGroup OBJECT-GROUP
    OBJECTS {
        cssgExcludedAPNRowStatus,
        cssgExcludedDomainRowStatus
    }
    STATUS current
    DESCRIPTION
        "A collection of objects pertaining to excluded APN/Domain."
    ::= { ciscoSsgMIBGroups 4 }

ciscoSsgTcpRedirectGroup OBJECT-GROUP
    OBJECTS {
        cssgTcpRedirectGrpRowStatus,
        cssgNetworkGrpNetRowStatus,
        cssgPortGrpPortRowStatus,
        cssgTcpRedirNetworkMapGrpName,
        cssgTcpRedirNetworkGrpMapRowStat,
        cssgTcpRedirPortMapGrpName,
        cssgTcpRedirPortGrpMapRowStat,
        cssgTcpRedirPortNo,
        cssgTcpRedirPortNoMapRowStat
    }
    STATUS current
    DESCRIPTION
        "A collection of objects pertaining to TCP Redirect."
    ::= { ciscoSsgMIBGroups 5 }

ciscoSsgServiceInterfaceGroup OBJECT-GROUP
    OBJECTS {
        cssgServiceIfIndex,
        cssgServiceIfRowStatus
    }
    STATUS current
    DESCRIPTION
        "A collection of objects pertaining to Service-Interface bind."
    ::= { ciscoSsgMIBGroups 6 }

ciscoSsgRadiusClientsGroup OBJECT-GROUP
    OBJECTS {
        cssgRadiusClientRowStatus
    }
    STATUS current
    DESCRIPTION
        "A collection of objects pertaining to Radius Client."
    ::= { ciscoSsgMIBGroups 7 }

ciscoSsgPortMapGroup OBJECT-GROUP
    OBJECTS {
        cssgPortMapLength,
        cssgPortMapPortRangeFrom,
        cssgPortMapPortRangeTo,
        cssgPortMapRowStatus
    }
    STATUS current
    DESCRIPTION
        "A collection of objects pertaining to Port Map Group."
    ::= { ciscoSsgMIBGroups 8 }

ciscoSsgNotificationGroup NOTIFICATION-GROUP
    NOTIFICATIONS {
        ciscoSsgRadiusClientReboot,
        ciscoSsgRadiusAAAServerDown
    }
    STATUS current
    DESCRIPTION
        "A collection of notifications generated by SSG."
    ::= { ciscoSsgMIBGroups 9 }

ciscoSsgCfgGroupRev1 OBJECT-GROUP
    OBJECTS {
        cssgCfgSsgEnabled,
        cssgCfgAutoDomainMode,
        cssgCfgLocalForwardingEnabled,
        cssgCfgAutoLogOffMode,
        cssgCfgRadiusProxyEnabled,
        cssgCfgTcpRedirectEnabled,
        cssgCfgAutoDomainNatEnabled,
        cssgCfgPortBundleHostKeyEnabled,
        cssgCfgTransPassThroughEnabled,
        cssgCfgAutoLogOffInterval,
        cssgCfgAutoLogOffIcmpRetries,
        cssgCfgMaxServicesPerUser,
        cssgCfgAccountingEnabled,
        cssgCfgDefaultNetworkType,
        cssgCfgDefaultNetwork,
        cssgCfgRadiusAuthenPort,
        cssgCfgRadiusAccountingPort,
        cssgCfgRadiusFwdAcctPktsEnabled,
        cssgCfgAccountingInterval,
        cssgCfgTCPRedirGrpForUnAuthUsers,
        cssgCfgTCPRedirGrpForUnAuthServ,
        cssgCfgTcpRedirGrpForSMTP,
        cssgCfgTcpRedirGrpForInitialCapt,
        cssgCfgTcpRedirGrpForAdvCapt,
        cssgCfgRadiusClntRbtNotifEnabled,
        cssgCfgAAAServerDownNotifEnabled,
        cssgCfgTalEnabled
    }
    STATUS current
    DESCRIPTION
        "A collection of configurable parameters in SSG MIB."
    ::= { ciscoSsgMIBGroups 10 }

ciscoSsgTalUserInfoGroup OBJECT-GROUP
    OBJECTS {
        cssgTalWaitingForAuthUsers,
        cssgTalUnidentifiedUsers,
        cssgTalSuspectUsers,
        cssgTalPassthroughUsers,
        cssgTalMaxAuthRate,
        cssgTalMaxAuthRateTimestamp,
        cssgTalMinAuthRate,
        cssgTalMinAuthRateTimestamp,
        cssgTalCurrentAuthRate,
        cssgTalCurrentAuthRateTimestamp,
        cssgTalResetAuthRates,
        cssgTalMaxPendingAuthReqs,
        cssgTalMaxAuthReqsRate,
        cssgTalDropPakDuringAuthorization,
        cssgTalUnidentifiedUserAllowTraff,
        cssgTalMaxSuspectUsers,
        cssgTalSuspectUserTimeout,
        cssgTalUnidentifiedUserTimeout,

        cssgTalUserState
    }
    STATUS current
    DESCRIPTION
        "A collection of objects pertaining to 
         Transparent Auto-Logon Group."
    ::= { ciscoSsgMIBGroups 11 }

END
    
