-- $ID$
-- ********************************************************************
-- CISCO-GGSN-MIB.my: MIB file for GGSN
--   
-- Dec 2001, Rajesh M. L.
-- Jan 2010, Raagavendran Sridharan
-- Copyright (c) 2000-2012 by Cisco Systems Inc.
-- All rights reserved.
-- ********************************************************************
-- $Endlog$

CISCO-GGSN-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    NOTIFICATION-TYPE,
    OBJECT-TYPE,
    Integer32,
    Counter32,
    Counter64,
    Unsigned32,
    Gauge32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    InterfaceIndexOrZero,
    ifIndex
        FROM IF-MIB
    DisplayString,
    TruthValue,
    TimeStamp,
    RowStatus
        FROM SNMPv2-TC
    InetAddressType,
    InetAddress,
    InetAddressDNS,
    InetAddressPrefixLength
        FROM INET-ADDRESS-MIB
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    CiscoAlarmSeverity,
    CiscoInetAddressMask
        FROM CISCO-TC
    cGtpPathAddressType,
    cGtpPathAddress,
    cGtpPathPort
        FROM CISCO-GTP-MIB
    ciscoMgmt
        FROM CISCO-SMI;


cGgsnMIB MODULE-IDENTITY
    LAST-UPDATED    "201205040000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-gprs@cisco.com"
    DESCRIPTION
        "This MIB module manages the Gateway GPRS Support
        Node (GGSN) devices. 

        A GGSN device provides interworking with external 
        packet-data network of a particular GPRS service
        provider. It provides a combination of IP routing
        and GPRS specific functionality to support mobile
        users.

        GTP version1 is introduced in  UMTS release 99 and
        Cisco GGSN will support both GTP version 1 (GTP v1)
        and version zero (GTP v0) simultaneously. 

        GTP v1 supports multiple PDP contexts sharing one 
        IP address.  TFTs are introduced to achieve this.
        Each TFT is associated with a PDP context and there
        may exist one PDP context without TFT amongst all 
        PDP contexts sharing the same IP address. Each TFT 
        has one to eight packet filters each assigned with
        a precedence index.  These packet filters are 
        evaluated one at a time against the packet header 
        information in sequence of their precedence index.
        A match is claimed if all the filters are matched
        and the PDP context that the TFT belongs to will be
        selected, else the checks are performed against the 
        filters of another PDP context.  If the packet 
        header doesn't contain any TFT packet filter
        information, then the PDP context without the TFT is 
        selected for further processing.

        Note on notifications:

        When an alarm occurs on the device, if the alarm's
        severity is higher than the severity filter threshold,
        a notification is generated by the device; and if
        cGgsnNotifEnabled is 'true', then the device's
        SNMP-engine configuration will be searched to
        determine where to send the notification. 

        Acronyms and terms:

         APN    Access Point Name
         CSG    Content Service Gateway
         CDR    Charging Data Record
         DCCA   Diameter Credit Control Application
         ETSI   European Telecommunications Standards Institute
         GGSN   Gateway GPRS Support Node
         GPRS   General Packet Radio Service
         GSM    Global System for Mobile communication
         GTP    GPRS Tunneling Protocol
         G-PDU  GTP PDU 
         IE     Information Element
         MS     Mobile Station
         MSISDN Mobile Station ISDN number
         PDP    Packet Data Protocol
         PDU    Protocol Data Unit
         PLMN   Public Land Mobile Network
         SGSN   Serving GPRS support Node
         SLB     Server Load Balancing
         TFT    Traffic Flow Template
         T-PDU  the payload of G-PDU 
         UMTS   Universal Mobile Telecommunications System
         IMS    IP Multimedia Subsystem
         COPS   Common Open Policy Service protocol
         PEP    Policy Enforcement Point
         PDF    Policy Decision Function
         P-CSCF Proxy Call Session Control Function
         PLMN   Public Land Mobile Network
         QS     Quota Server
         UE     User Equipment

        REFERENCE

        [1] GSM 03.60: Digital cellular telecommunications
            system (Phase 2+); General Packet Radio Service
            (GPRS); Service description; Stage 2. V7.1.0

        [2] GSM 09.60: Digital cellular telecommunication
            system (Phase 2+); General Packet Radio Service
            (GPRS); GPRS Tunnelling Protocol (GTP) across
            Gn and Gp Interface. V7.3.0

        [3] 3GPP; Technical Specification Group Services
            and System Aspects; QoS Concept and Architecture.
            3G TS 23.107 v3.2.0.

        [4] 3GPP; Technical Specification Group Core Network;
            General Packet Radio Service(GPRS); GPRS 
            Tunnelling Protocol (GTP) across Gn and Gp 
            Interface (Release 1999). 3G TS 29.060 v3.5.0.

        [5] 3GPP: Technical Specification Group Core Network;
            Policy control over Go interface (Release 5).
            3GPP TS 29.207 V5.2.0"
    REVISION        "201205040000Z"
    DESCRIPTION
        "Modified description for cGgsnSentSigMessages and
        cGgsnReceivedSigMessages."
    REVISION        "201201110000Z"
    DESCRIPTION
        "Modified description for cGgsnSlbVserAddrType."
    REVISION        "201103210000Z"
    DESCRIPTION
        "Added the following objects to cGgsnIpDupProtectTable

        cGgsnMsExcludeRangeStartIpv6Prefixlen,
        cGgsnMsExcludeRangeEndIpv6Prefixlen.

        Added the following objects to cGgsnPlmnIpAddrRangeTable

        cGgsnPlmnAddrRangeFirstIpv6Prefixlen,
        cGgsnPlmnAddrRangeLastIpv6Prefixlen.

        Modified the description of the following objects

        cGgsnMsExcludeRangeStartIpType,
        cGgsnMsExcludeRangeEndIpType,
        cGgsnPlmnAddrRangeIpAddrType,
        cGgsnIpDupProtectRowStatus and
        cGgsnPlmnAddrRangeRowStatus.


        Added a OBJECT-GROUP cGgsnConfigurationsGroupSup1.

        Deprecated the compliance group cGgsnMIBComplianceRev9 and 
        added a new compliance group cGgsnMIBComplianceRev10."
    REVISION        "201103010000Z"
    DESCRIPTION
        "Modified description for cGgsnSlbVserNextHopAddrType
        and cGgsnDefaultAggregIpAddrType."
    REVISION        "201003230000Z"
    DESCRIPTION
        "Added the 'release100' enumeration to cGgsnVersion."
    REVISION        "201002190000Z"
    DESCRIPTION
        "Added new table cGgsnGtpEncapsuTable.

        Added OBJECT-GROUP cGgsnStatusGroupR90.

        Added MODULE-COMPLIANCE cGgsnMIBComplianceRev9, which
        deprecates cGgsnMIBComplianceRev8."
    REVISION        "200811030000Z"
    DESCRIPTION
        "Added the 'release90' enumeration to cGgsnVersion."
    REVISION        "200802040000Z"
    DESCRIPTION
        "Deprecated cGgsnCompliance3GppGgsn.
        Added a Enumerated value to cGgsnVersion."
    REVISION        "200610050000Z"
    DESCRIPTION
        "+ Added cGgsnTotalCreatedIpv6Pdps,
        cGgsnTotalDeletedIpv6Pdps,
        cGgsnTotalRejectedIpv6Pdps, cGgsnSentIpv6SigMessages,
        cGgsnReceivedIpv6SigMessages,
        cGgsnSentIpv6PDUs, cGgsnReceivedIpv6PDUs,
        cGgsnSentIpv6PDUOctets, cGgsnReceivedIpv6PDUOctets,
        to cGgsnStatistics.
        + Added cGgsnActivatedIpv6Gtpv0Pdp,
        cGgsnActivatedIpv6Gtpv1Pdp,
        cGgsnActivatedIpv6Ms to cGgsnStatus.
        - Deprecated cGgsnCreateReqV1UpdExistPdp.
        - Deprecated all the objects of cGgsnPdpsRejStatistics.
        + Added cGgsnVersionNotSupportedMsgs,
        cGgsnUnkownGtpMsgs, cGgsnTooShortMsgs,
        cGgsnMandIeMissingMsgs, cGgsnMandIeIncorrectMsgs,
        cGgsnOptIeInvalidMsgs, cGgsnIeUnknownMsgs,
        cGgsnIeOutOfOrderMsgs, cGgsnIeUnexpectedMsgs,
        cGgsnIeDuplicatedMsgs, cGgsnOptIeIncorrectMsgs,
        cGgsnPdpWithoutTftExistsPdps to cGgsnStatistics.
        - Deprecated cGgsnPdfTable and all the table objects.
        - Deprecated cGgsnPdfNotifEnabled,
        cGgsnPdfServerAddrType,cGgsnPdfServerAddr,
        cGgsnPdfStateUpNotif, cGgsnPdfStateDownNotif."
    REVISION        "200603300900Z"
    DESCRIPTION
        "- Deprecated cGgsnSlbNotif.
        + Added cGgsnSlbNotifyCacFailure and
          cGgsnSlbNotifySessionDeletion to 
          cGgsnConfigurations."
    REVISION        "200508241800Z"
    DESCRIPTION
        "Added cGgsnSlbCacFailures,
        cGgsnSlbSessionFailures,
        cGgsnRedundancyStatistics to
        cGgsnStatistics.

        + Added cGgsnSlbVserverTable,
        cGgsnSlbVserverEntry,
        cGgsnSlbVserAddrType,
        cGgsnSlbVserAddress to 
        cGgsnConfigurations.

        + Added cGgsnPrepaidPDPs,
        cGgsnPostpaidPDPs to cGgsnStatus.

        + Added cGgsnNotifPdpMsisdn
        to cGgsnNotifInfo."
    REVISION        "200501041800Z"
    DESCRIPTION
        "Added cGgsnConfigVersion to
        cGgsnStatus."
    REVISION        "200411230100Z"
    DESCRIPTION
        "- Deprecated cGgsnNotification
        + Added cGgsnGlobalErrorNotif,
          cGgsnAccessPointNameNotif, 
          cGgsnPacketDataProtocolNotif.

        + Added cGgsnNotifAccessPointName,
          cGgsnNotifPdpImsi,
          cGgsnGlobalErrorTypes,
          cGgsnAccessPointErrorTypes,
          cGgsnPacketDataProtoErrorTypes to 
          cGgsnNotifInfo.

        - Deprecated cGgsnNotifEnabled
        + Added cGgsnServiceNotifEnabled,
          cGgsnMemoryNotifEnabled,
          cGgsnPdfNotifEnabled,
          cGgsnGlobalErrorNotifEnabled,
          cGgsnAccessPointNotifEnabled,
          cGgsnPdpNotifEnabled to 
          cGgsnNotifMgmt"
    REVISION        "200402230100Z"
    DESCRIPTION
        "+ Added cGgsnInServiceNotif,
        cGgsnMaintenanceNotif, 
        cGgsnMemThresholdReachedNotif, 
        cGgsnMemThresholdClearedNotif, 
        cGgsnPdfStateUpNotif, cGgsnPdfStateDownNotif to 
        cGgsnNotifications.

        + Added cGgsnPdfTable, cGgsnPcscfTable,
        cGgsnMemoryThreshold, cGgsnServiceMode,
        cGgsnPlmnTable, cGgsnSessionTimeout, 
        cGgsnThruputIntervalOne, cGgsnThruputIntervalTwo,
        cGgsnCompliance3GppGgsn, cGgsnCreateReqV1UpdExistPdp,
        cGgsnRadAttrSessTimeout, cGgsnDownlinkVerifyMsDisable
        to cGgsnConfigurations.

        + Added cGgsnVersionNotSupportedRejPdps,
        cGgsnUnkownMessageRejPdps, cGgsnMsgTooShortRejPdps,
        cGgsnMandIeMissingRejPdps, 
        cGgsnMandIeIncorrectRejPdps,
        cGgsnOptIeInvalidRejPdps, cGgsnIeUnknownRejPdps,
        cGgsnIeOutOfOrderRejPdps, cGgsnIeUnexpectedRejPdps,
        cGgsnIeDuplicatedRejPdps, cGgsnOptIeIncorrectRejPdps,
        cGgsnPdpWithoutTftExistsRejPdps
        to cGgsnPdpsRejStatistics.

        + Added cGgsnSgsnStatTable to cGgsnStatistics.

        + Added cGgsnHCSentGPDUOctets and deprecated
        cGgsnSentGPDUOctets.

        + Added cGgsnHCReceivedGPDUOctets and deprecated
        cGgsnReceivedGPDUOctets.

        + Added cGgsnServiceModeStatus to cGgsnStatus.

        + Added cGgsnPdfServerAddrType, cGgsnPdfServerAddr
        to cGgsnNotifInfo."
    REVISION        "200312310100Z"
    DESCRIPTION
        "+ Added cGgsnPlmnIpAddrRangeTable to
        cGgsnConfigurations.
        + Added cGgsnTftSemanticErrorPdps, 
        cGgsnTftSyntacticErrorPdps,
        cGgsnPktFilterSemanticErrorPdps,
        cGgsnPktFilterSyntacticErrorPdps to cGgsnStatistics.
        + Added cGgsnActiveGtpVersion0Pdps,
        cGgsnActiveGtpVersion1Pdps, cGgsnGtpEncapInterface
        to cGgsnStatus."
    REVISION        "200112081500Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 240 }


-- Object definitions

cGgsnMIBObjects  OBJECT IDENTIFIER
    ::= { cGgsnMIB 1 }

cGgsnStatistics  OBJECT IDENTIFIER
    ::= { cGgsnMIBObjects 1 }

cGgsnNotifMgmt  OBJECT IDENTIFIER
    ::= { cGgsnMIBObjects 2 }

cGgsnConfigurations  OBJECT IDENTIFIER
    ::= { cGgsnMIBObjects 3 }

cGgsnStatus  OBJECT IDENTIFIER
    ::= { cGgsnMIBObjects 4 }

cGgsnNotifInfo  OBJECT IDENTIFIER
    ::= { cGgsnMIBObjects 5 }


-- MIBObjects
--   

--   
-- Statistics

cGgsnSentSigMessages OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of GTPv0 and GTPv1 signalling messages sent.

        Trigger Condition: This counter is updated whenever a 
        GTPv0 and GTPv1 signalling messages is sent out, including retries." 
    ::= { cGgsnStatistics 1 }

cGgsnReceivedSigMessages OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of GTPv0 and GTPv1 signalling messages received.

        Trigger Condition: This counter is updated whenever a 
        GTPv0 and GTPv1 signalling message is received." 
    ::= { cGgsnStatistics 2 }

cGgsnUnexpectedSigMessages OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of unexpected GTP signalling messages received.

        Trigger Condition: This counter is updated whenever an 
        unexpected Signalling message is received. 
        Condition includes,
          a) A Response message for which there is no corresponding 
             outstanding Request.
          b) A GTP control plane message a GSN is not expected to 
             handle (such as a PDU Notification Request received by 
             a GGSN).
          c) Charging messages in GTP path and vice-versa.
          d) LFN bit not being set when CG path uses short-header 
             and vice-versa." 
    ::= { cGgsnStatistics 3 }

cGgsnSentGPDUs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of G-PDU messages sent.

        Trigger Condition: This counter is updated whenever a G-PDU 
        is sent out by the GGSN." 
    ::= { cGgsnStatistics 4 }

cGgsnReceivedGPDUs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of G-PDU messages received.

        Trigger Condition: This counter is incremented for each 
        G-PDU received." 
    ::= { cGgsnStatistics 5 }

cGgsnSentGPDUOctets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "bytes"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of total bytes sent in G-PDU messages.

        Trigger Condition: This counter is updated whenever a G-PDU 
        is sent out by the GGSN." 
    ::= { cGgsnStatistics 6 }

cGgsnReceivedGPDUOctets OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "bytes"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of total bytes received in G-PDU messages.

        Trigger Condition: This counter is incremented for each 
         G-PDU received." 
    ::= { cGgsnStatistics 7 }

cGgsnUnexpectedGPDUs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of unexpected G-PDU messages, for example,
        non existent PDP contexts and ACL denial.

        Trigger Condition: This counter is updated whenever an 
        unexpected G-PDU message is received.
        Conditions include,
          a) G-PDU for a non existent PDP.
          b) ACL denial." 
    ::= { cGgsnStatistics 8 }

cGgsnActivationRejectedPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of PDP contexts that the activation request
        was rejected.

        Trigger Condition: This counter is updated when a PDP 
        activation request is rejected. 
        The cause for rejection can be 
          a) Resource limitations like max PDP limit is reached,
             Out of memory.
          b) Config restrictions like trying to create NIPDP on an 
             APN on which the same is disabled, 
          c) Creating secondary contexts on PPP/PPP-Regen PDPs." 
    ::= { cGgsnStatistics 9 }

cGgsnOutOfResourcePdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of PDP contexts that the activation request
        rejected due to the GGSN running out of resources for
        transmitting GTP packets. Examples:
         - Out of memory;
         - The number of PDPs on GGSN reached limit;
         - all dynamic PDP address are occupied;

        Trigger Condition: 
          a) Out of memory.
          b) Number of PDPs on GGSN reached limit.
          c) Number of of PPP-regen PDPs reaches max limit.
          d) All dynamic PDP address are occupied.
          e) Incorrect configs for create pdp req.
          f) Qos negotiation fails.
          g) Create PDP req received for non-transparent APN but 
             no radius server is present for authorization.
          h) Attempt to create a PDP with IP address that is 
             already in use.
          i) Attempt to create a PPP-Regen PDP but the vtemplate 
             for PPP-regen is not properly configured or VPDN 
             configs are not proper.
          j) Number of pending signalling messages that needs to 
             be processed by the GGSN is beyond the max limit(100)." 
    ::= { cGgsnStatistics 10 }

cGgsnParserErrorMessages OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of GTP messages received with wrong value.
        It includes the following cases:

         - mandatory and optional information element in the GTP
           packet is duplicated, missing, unknown, incorrect or
           out of order.

         - the GTP message is too short to hold the GTP header for
           the supported version.

         - the GTP messages running an unsupported version of GTP.

         - Unknown GTP message type.

        Trigger Condition: This counter is triggered when a 
        signalling message is received with parsing related errors 
        such as missing/unknown/invalid/unexpected/duplicate 
        mandatory/optional IE's in the messages." 
    ::= { cGgsnStatistics 11 }

cGgsnTotalCreatedPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of PDP contexts
        created.

        Trigger Condition: This counter is updated whenever a PDP 
        context is created. This includes static, dynamic, IP, 
        PPP, network init PDPs." 
    ::= { cGgsnStatistics 12 }

cGgsnTotalDeletedPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of PDP contexts
        deleted.

        Trigger Condition: This counter is updated whenever a PDP 
        context is deleted. This includes static, dynamic, IP, PPP, 
        network init PDPs." 
    ::= { cGgsnStatistics 13 }

cGgsnTotalNetworkInitPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of PDP contexts
        activated by the GGSN that were initiated by the PDN.

        Trigger Condition: This counter will be updated on successful 
        creation of network initiated PDP." 
    ::= { cGgsnStatistics 14 }

cGgsnTotalPppPdpsCreated OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of PPP PDP
        contexts created.

        Trigger Condition: This counter is updated whenever a 
        PPP PDP context is created." 
    ::= { cGgsnStatistics 15 }

cGgsnTotalPppPdpsDeleted OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of PPP PDP
        contexts deleted.

        Trigger Condition: This counter is updated whenever a 
        PPP PDP context is deleted." 
    ::= { cGgsnStatistics 16 }

cGgsnOutOfResourcePppRegenPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of create PDP
        context and delete PDP context requests rejected due to 
        unavailable resource on the GGSN for PPP regeneration.

        Trigger Condition:
          a) Out of memory.
          b) Number of PPP-regen PDPs reaches max limit.
          c) All dynamic PDP address are occupied.
          d) Attempt to create a PPP-Regen PDP but the vtemplate 
             for PPP-regen is not properly configured or VPDN 
             configs are not proper." 
    ::= { cGgsnStatistics 17 }

cGgsnDroppedPppRegenPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of create PDP
        context and delete PDP context requests that were dropped 
        due to the threshold limit being reached for maximum number
        of PPP regeneration sessions allowed on the GGSN.

        Trigger Condition: This counter is updated when a new PPP 
        regen PDP activation request is received by GGSN and max 
        allowed PPP Regen session is reached." 
    ::= { cGgsnStatistics 18 }

cGgsnTftSemanticErrorPdps OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of received PDP
        context messages that had TFTs with semantic errors.

        Trigger Condition: This counter is triggered by the create,
        update PDP context request message."
    REFERENCE
        "3GPP; Technical Specification Group Core Network;
         General Packet Radio Service(GPRS); GPRS
         Tunnelling Protocol (GTP) across Gn and Gp
         Interface (Release 1999). 3G TS 29.060 v3.5.0." 
    ::= { cGgsnStatistics 19 }

cGgsnTftSyntacticErrorPdps OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of received PDP
        context messages that had TFTs with syntactic errors.

        Trigger Condition: This counter is triggered by the create,
        update PDP context request message."
    REFERENCE
        "3GPP; Technical Specification Group Core Network;
         General Packet Radio Service(GPRS); GPRS
         Tunnelling Protocol (GTP) across Gn and Gp
         Interface (Release 1999). 3G TS 29.060 v3.5.0." 
    ::= { cGgsnStatistics 20 }

cGgsnPktFilterSemanticErrorPdps OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of received PDP
        context messages that had packet filters with semantic errors.

        Trigger Condition: This counter is triggered by the create,
        update PDP context request message."
    REFERENCE
        "3GPP; Technical Specification Group Core Network;
         General Packet Radio Service(GPRS); GPRS
         Tunnelling Protocol (GTP) across Gn and Gp
         Interface (Release 1999). 3G TS 29.060 v3.5.0." 
    ::= { cGgsnStatistics 21 }

cGgsnPktFilterSyntacticErrorPdps OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of received PDP
        context messages that had packet filters with syntactic
        errors.

        Trigger Condition: This counter is triggered by the create,
        update PDP context request message."
    REFERENCE
        "3GPP; Technical Specification Group Core Network;
         General Packet Radio Service(GPRS); GPRS
         Tunnelling Protocol (GTP) across Gn and Gp
         Interface (Release 1999). 3G TS 29.060 v3.5.0." 
    ::= { cGgsnStatistics 22 }

cGgsnHCSentGPDUOctets OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of total bytes sent in G-PDU messages.

        Trigger Condition: This counter is updated whenever a G-PDU
        is sent out by the GGSN." 
    ::= { cGgsnStatistics 23 }

cGgsnHCReceivedGPDUOctets OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of total bytes received in G-PDU messages.

        Trigger Condition: This counter is incremented for each
        G-PDU received." 
    ::= { cGgsnStatistics 24 }
-- Rejected PDP Statistics per cause

cGgsnPdpsRejStatistics  OBJECT IDENTIFIER
    ::= { cGgsnStatistics 25 }


cGgsnVersionNotSupportedRejPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of PDP contexts that were rejected due to the
        cause of Version Not Supported.

        Trigger Condition: This counter is triggered by create/update
        PDP / PPP PDP context request message. This object is
        deprecated by cGgsnVersionNotSupportedMsgs." 
    ::= { cGgsnPdpsRejStatistics 1 }

cGgsnUnkownMessageRejPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of PDP contexts that were rejected due to the
        cause of Unknown Message.

        Trigger Condition: This counter is triggered by create/update
        PDP / PPP PDP context request message. This object is
        deprecated by cGgsnUnkownGtpMsgs." 
    ::= { cGgsnPdpsRejStatistics 2 }

cGgsnMsgTooShortRejPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of PDP contexts that were rejected due to the
        cause of Message Too Short.

        Trigger Condition: This counter is triggered by create/update
        PDP / PPP PDP context request message. This object is
        deprecated by cGgsnTooShortMsgs." 
    ::= { cGgsnPdpsRejStatistics 3 }

cGgsnMandIeMissingRejPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of PDP contexts that were rejected due to the
        cause of Mandatory IE Missing.

        Trigger Condition: This counter is triggered by create/update
        PDP / PPP PDP context request message. This object is
        deprecated by cGgsnMandIeMissingMsgs." 
    ::= { cGgsnPdpsRejStatistics 4 }

cGgsnMandIeIncorrectRejPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of PDP contexts that were rejected due to the
        cause of Mandatory IE Incorrect.

        Trigger Condition: This counter is triggered by create/update
        PDP / PPP PDP context request message. This object is
        deprecated by cGgsnMandIeIncorrectMsgs." 
    ::= { cGgsnPdpsRejStatistics 5 }

cGgsnOptIeInvalidRejPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of PDP contexts that rejected due to the
        cause of Optional IE Invalid.

        Trigger Condition: This counter is triggered by create/update
        PDP / PPP PDP context request message. This object is
        deprecated by cGgsnOptIeInvalidMsgs." 
    ::= { cGgsnPdpsRejStatistics 6 }

cGgsnIeUnknownRejPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of PDP contexts that rejected due to the
        cause of IE Unknown.

        Trigger Condition: This counter is triggered by create/update
        PDP / PPP PDP context request message. This object is
        deprecated by cGgsnIeUnknownMsgs." 
    ::= { cGgsnPdpsRejStatistics 7 }

cGgsnIeOutOfOrderRejPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of PDP contexts that rejected due to the
        cause of IE Out of Order.

        Trigger Condition: This counter is triggered by create/update
        PDP / PPP PDP context request message. This object is
        deprecated by cGgsnIeOutOfOrderMsgs." 
    ::= { cGgsnPdpsRejStatistics 8 }

cGgsnIeUnexpectedRejPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of PDP contexts that rejected due to the
        cause of IE Unexpected.

        Trigger Condition: This counter is triggered by create/update
        PDP / PPP PDP context request message. This object is
        deprecated by cGgsnIeUnexpectedMsgs." 
    ::= { cGgsnPdpsRejStatistics 9 }

cGgsnIeDuplicatedRejPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of PDP contexts that rejected due to the
        cause of IE Duplicated.

        Trigger Condition: This counter is triggered by create/update
        PDP / PPP PDP context request message. This object is
        deprecated by cGgsnIeDuplicatedMsgs." 
    ::= { cGgsnPdpsRejStatistics 10 }

cGgsnOptIeIncorrectRejPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of PDP contexts that rejected due to the
        cause of Optional IE Incorrect.

        Trigger Condition: This counter is triggered by create/update
        PDP / PPP PDP context request message. This object is
        deprecated by cGgsnOptIeIncorrectMsgs." 
    ::= { cGgsnPdpsRejStatistics 11 }

cGgsnPdpWithoutTftExistsRejPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of PDP contexts that are rejected due to
        the cause of PDP context without TFT already exists.

        Trigger Condition: This counter is triggered by create/update
        PDP / PPP PDP context request message. This object is
        deprecated by cGgsnPdpWithoutTftExistsPdps." 
    ::= { cGgsnPdpsRejStatistics 12 }

cGgsnSgsnStatTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CGgsnSgsnStatEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table has the statistics of the interface (Gi, Gn, Gp)
        upstream and downstream traffic per SGSN for a 
        configurable duration set in cGgsnThruputIntervalOne and
        cGgsnThruputIntervalTwo.

        Creation of row(s) will happen when there is a valid value set 
        to cGgsnThruputIntervalOne or cGgsnThruputIntervalTwo and
        when a PATH is established.

        Deletion of row(s) will happen when either the PATH gets
        removed or the throughput intervals(cGgsnThruputIntervalOne,
        cGgsnThruputIntervalTwo) is unset."
    ::= { cGgsnStatistics 26 }

cGgsnSgsnStatEntry OBJECT-TYPE
    SYNTAX          CGgsnSgsnStatEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in this table."
    INDEX           {
                        cGtpPathAddressType,
                        cGtpPathAddress,
                        cGtpPathPort,
                        cGgsnSgsnThruPutInterval
                    } 
    ::= { cGgsnSgsnStatTable 1 }

CGgsnSgsnStatEntry ::= SEQUENCE {
        cGgsnSgsnThruPutInterval      Integer32,
        cGgsnSgsnThruPutLastCollected Integer32,
        cGgsnSgsnUpStreamPktCnt       Gauge32,
        cGgsnSgsnUpStreamByteCnt      Gauge32,
        cGgsnSgsnDownStreamPktCnt     Gauge32,
        cGgsnSgsnDownStreamByteCnt    Gauge32
}

cGgsnSgsnThruPutInterval OBJECT-TYPE
    SYNTAX          Integer32 (1..65535)
    UNITS           "minutes"
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object should be one of the values set in the objects
        cGgsnThruputIntervalOne or cGgsnThruputIntervalTwo except
        for value '0', which means the throughput collection is
        disabled." 
    ::= { cGgsnSgsnStatEntry 1 }

cGgsnSgsnThruPutLastCollected OBJECT-TYPE
    SYNTAX          Integer32 (0..65535)
    UNITS           "minutes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the delta value between the time
        when this data is collected and the time it is been
        retrieved." 
    ::= { cGgsnSgsnStatEntry 2 }

cGgsnSgsnUpStreamPktCnt OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of upstream
        packets sent on this SGSN data path. Data flow from
        MS to PDN is considered to be upstream traffic.

        When the throughput intervals (cGgsnThruputIntervalOne or
        cGgsnThruputIntervalTwo) is set to some valid value this
        object is set to '0' (meaning, a fresh throughput collection
        is started). Until the first expiry of the throughput 
        interval , this object will be '0'. On further periodic expiry,
        the throughput upstream packet count per SGSN is collected and 
        updated to this object" 
    ::= { cGgsnSgsnStatEntry 3 }

cGgsnSgsnUpStreamByteCnt OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of upstream
        bytes sent on this SGSN data path. Data flow from
        MS to PDN is considered to be upstream traffic.

        When the throughput intervals (cGgsnThruputIntervalOne or
        cGgsnThruputIntervalTwo) is set to some valid value this
        object is set to '0' (meaning, a fresh throughput collection
        is started). Until the first expiry of the throughput 
        interval , this object will be '0'. On further periodic expiry,
        the throughput upstream byte count per SGSN is collected and 
        updated to this object" 
    ::= { cGgsnSgsnStatEntry 4 }

cGgsnSgsnDownStreamPktCnt OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of downstream
        packets sent on this SGSN data path. Data flow from
        PDN to MS is considered to be downstream traffic.

        When the throughput interval (cGgsnThruputIntervalOne or
        cGgsnThruputIntervalTwo) is set to some valid value, this
        object is set to '0' (meaning, a fresh throughput collection
        is started). Until the first expiry of the throughput 
        interval , this object will be '0'. On further periodic expiry,
        the throughput downstream packet count per SGSN is collected 
        and updated to this object." 
    ::= { cGgsnSgsnStatEntry 5 }

cGgsnSgsnDownStreamByteCnt OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of downstream
        bytes sent on this SGSN data path. Data flow from
        PDN to MS is considered to be downstream traffic.

        When the throughput interval (cGgsnThruputIntervalOne or
        cGgsnThruputIntervalTwo) is set to some valid value, this
        object is set to '0' (meaning, a fresh throughput collection
        is started). Until the first expiry of the throughput 
        interval , this object will be '0'. On further periodic expiry,
        the throughput downstream byte count per SGSN is collected and 
        updated to this object." 
    ::= { cGgsnSgsnStatEntry 6 }
 

-- Redundancy Statistics

cGgsnRedundancyStatistics  OBJECT IDENTIFIER
    ::= { cGgsnStatistics 27 }


cGgsnTotalMessages OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This counter will maintain the count of total number of
        messages of all kind.

        Trigger Condition: The counter is increamented whenever
        a redundancy message is sent." 
    ::= { cGgsnRedundancyStatistics 1 }

cGgsnContextSetupMessages OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The PDP context is check pointed to standby only after it
        goes to active.

        This object is a counter, which maintains the total count
        of PDP context setup messages.

        Trigger Condition: This counter is updated whenever
        a PDP context setup message is check pointed to standby." 
    ::= { cGgsnRedundancyStatistics 2 }

cGgsnContextModifyMessages OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "For modify or update PDP context, the categories get
        affected and new quota is assigned to them. This new info 
        must be check pointed to the standby.

        This object maintains the total number of context modify 
        messages which are check pointed to standby.

        Trigger Condition: This counter is incremented whenever a
        context modify message is check pointed to standby." 
    ::= { cGgsnRedundancyStatistics 3 }

cGgsnContextRemoveMessages OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "When the PDP context is deleted, deletion event is
        check pointed to the standby, so that the corresponding 
        backup context deleted as well.

        This object will maintain the total number of context 
        removed messages which are check pointed to standby.

        Trigger Condition: The counter is incremented for every 
        context remove message, which is check pointed." 
    ::= { cGgsnRedundancyStatistics 4 }

cGgsnPathSetupMessages OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Messages (of any kind PDP create/delete etc)indicate
        the presence of other GSN. Path is setup between the GSNs 
        when they transmit the messages.

        This object contains the number of path setup messages
        between SGSN and GGSN.

        Trigger Condition: This counter is updated for every path
        setup messages sent." 
    ::= { cGgsnRedundancyStatistics 5 }

cGgsnPathModifyMessages OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object will contain the total number of path Modify
        messages.

        The IE recovery count is used to indicate restart of other
        GSN. Any change related to path or GSN will be check pointed
        to standby.

        Trigger Condition: This counter is incremented for every change
        related to path." 
    ::= { cGgsnRedundancyStatistics 6 }

cGgsnPathRemoveMessages OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object will keep track of all the messages which are
        responsible for path removal between the GSNs.
        As long as context remain established, the path between the  
        GSNs is alive. In an instant where the last context is released
        and the echo timer is not enabled, the path timer is started 
        within which the PDP context is expected to keep the path
        live, when the timer expires, path is Removed.

        Trigger Condition: This timer is triggered when the path
        between the GSNs is removed." 
    ::= { cGgsnRedundancyStatistics 7 }

cGgsnCGFReadyMessages OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The charging information are sent from GGSN to charging
        gateway. GTP' protocol is used between them.

        This object will consists of total number of CGF ready 
        messages.

        Trigger Condition: The counter is incremented when CGF ready
        message is check pointed to standby." 
    ::= { cGgsnRedundancyStatistics 8 }

cGgsnCGFModifyMessages OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Significant information related to change in state of
        CGF must be check pointed to GGSN.

        This object indicates the total number of CGF modify 
        messages recieved.

        Trigger condition: This counter is triggered when there
        is a change in CGF state." 
    ::= { cGgsnRedundancyStatistics 9 }

cGgsnCGFRemoveMessages OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object maintains the count for all the messages
        responsible for CGF removal

        Trigger Condition: This counter is triggered when
        context is deleted." 
    ::= { cGgsnRedundancyStatistics 10 }

cGgsnInternalStateMsgs OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The GGSN certain information which are sent out to other
        GSN's  (SGSN) and CGF. On failover these information must be 
        consistent. Information like, IE recovery count sent to the 
        other GSN's for path management, local record sequence number
        and charging ID etc.

        Trigger Condition: The counter is incremented for each of
        these kind of messages." 
    ::= { cGgsnRedundancyStatistics 11 }

cGgsnSlbCacFailures OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object will keep track of number of CAC Failure
        notifications sent to SLB.

        Trigger Condition: The counter is incremented whenever
        GGSN sends CAC failure notification to SLB." 
    ::= { cGgsnStatistics 28 }

cGgsnSlbSessionFailures OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object will keep track of number of Session failure
        notifications sent to SLB.

        Trigger Condition: The counter is incremented whenever
        GGSN sends Session failure notification to SLB." 
    ::= { cGgsnStatistics 29 }

cGgsnTotalCreatedIpv6Pdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "PDPs"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of successfully
        created ipv6 PDP contexts.

        Trigger Condition: The counter is incremented whenever a ipv6 
        PDP context is created. This includes static, dynamic,
        IP PDPs." 
    ::= { cGgsnStatistics 30 }

cGgsnTotalDeletedIpv6Pdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "PDPs"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of ipv6 PDP contexts
        deleted.

        Trigger Condition: The counter is incremented whenever a ipv6 
        PDP context is deleted.  This includes static, dynamic, IP, PPP
        PDPs." 
    ::= { cGgsnStatistics 31 }

cGgsnTotalRejectedIpv6Pdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "PDPs"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of rejected ipv6 PDP
        context activation requests.

        Trigger Condition: The counter is incremented when a ipv6 PDP
        activation request is rejected." 
    ::= { cGgsnStatistics 32 }

cGgsnSentIpv6SigMessages OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "messages"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of GTP signalling messages related to
        the IPv6 PDP sent by GGSN.

        Trigger Condition: The counter is incremented whenever a
        GTP signalling message for IPv6 PDP is sent out, including
        retries." 
    ::= { cGgsnStatistics 33 }

cGgsnReceivedIpv6SigMessages OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "messages"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of GTP signalling messages related to
        the IPv6 PDP received by GGSN.

        Trigger Condition: The counter is incremented whenever a
        GTP signalling message for IPv6 PDP is received." 
    ::= { cGgsnStatistics 34 }

cGgsnSentIpv6PDUs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of ipv6 data packets sent by GGSN.

        Trigger Condition: The counter is incremented whenever a G-PDU
        is sent out by the GGSN." 
    ::= { cGgsnStatistics 35 }

cGgsnReceivedIpv6PDUs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of ipv6 data packets receivd by GGSN.

        Trigger Condition: This counter is incremented for each
        G-PDU received." 
    ::= { cGgsnStatistics 36 }

cGgsnSentIpv6PDUOctets OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of ipv6 data bytes sent, in PDU messages, by GGSN.

        Trigger Condition: The counter is incremented whenever a G-PDU
        is sent out by the GGSN." 
    ::= { cGgsnStatistics 37 }

cGgsnReceivedIpv6PDUOctets OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of ipv6 data bytes received, in PDU messages,
        by GGSN.

        Trigger Condition: The counter is incremented for each
         G-PDU received." 
    ::= { cGgsnStatistics 38 }

cGgsnVersionNotSupportedMsgs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "messages"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of GTP messages received from devices running an
        unsupported version of the GTP." 
    ::= { cGgsnStatistics 39 }

cGgsnUnkownGtpMsgs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "messages"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of unknown GTP messages received." 
    ::= { cGgsnStatistics 40 }

cGgsnTooShortMsgs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "messages"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of GTP messages received that are too short to
        hold the GTP header for the supported GTP version." 
    ::= { cGgsnStatistics 41 }

cGgsnMandIeMissingMsgs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "messages"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of GTP messages received with a missing mandatory
        information element." 
    ::= { cGgsnStatistics 42 }

cGgsnMandIeIncorrectMsgs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "messages"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of GTP messages received with an incorrect
        mandatory information element, for example, with an
        information element that has an incorrect length." 
    ::= { cGgsnStatistics 43 }

cGgsnOptIeInvalidMsgs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "messages"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of GTP messages received with an information
        element that contains a value that is not within the defined
        range for that IE.  GTP messages with invalid optional IEs
        are processed as if the IE was not present." 
    ::= { cGgsnStatistics 44 }

cGgsnIeUnknownMsgs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "messages"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of GTP messages received with an information
        element of an unknown type." 
    ::= { cGgsnStatistics 45 }

cGgsnIeOutOfOrderMsgs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "messages"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of GTP messages received with an information
        element out of order." 
    ::= { cGgsnStatistics 46 }

cGgsnIeUnexpectedMsgs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "messages"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of GTP messages received with an information
        element that is not expected in the GTP message, but is defined
        in GTP.  GTP messages with unexpected IEs are processed as if
        the IE was not present." 
    ::= { cGgsnStatistics 47 }

cGgsnIeDuplicatedMsgs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "messages"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of GTP messages received with a duplicated
        information element." 
    ::= { cGgsnStatistics 48 }

cGgsnOptIeIncorrectMsgs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "messages"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of GTP messages received with an optional IE
        that is incorrect, which prevents the GGSN from processing
        the GTP message correctly." 
    ::= { cGgsnStatistics 49 }

cGgsnPdpWithoutTftExistsPdps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of create PDP context requests received without
        traffic flow template information element." 
    ::= { cGgsnStatistics 50 }

-- Notification and alarm related objects

cGgsnNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "Indicates whether cGgsnNotification notification will
        be sent when a notification is generated by the device.
          - 'true',  it will enable the device to send a notification,
                     as well as logging the notification to the
                     cGgsnHistNotifTable.
          - 'false', it will prevent the device from sending out a
                     notification, but it will still log the
                     notification into cGgsnHistNotifTable."
    DEFVAL          { false } 
    ::= { cGgsnNotifMgmt 1 }

cGgsnNotifLeastSeverLevel OBJECT-TYPE
    SYNTAX          CiscoAlarmSeverity
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Indicates the least severity level of the cGgsnNotification
        notifications to be generated by the device. Thus, notifications
        are not generated for alarms with a severity level less urgent 
        than the value of this object. This object cannot be set to
        cleared(1) or indeterminate(2)."
    DEFVAL          { info } 
    ::= { cGgsnNotifMgmt 2 }

cGgsnGeneratedNotifs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "notifications"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of cGgsnNotification notifications that have
        been generated since sysUpTime." 
    ::= { cGgsnNotifMgmt 3 }

cGgsnIgnoredAlarms OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "notifications"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of alarms which are less severe than
        cGgsnNotifLeastSeverLevel since sysUpTime, and thus,
        for which no notification was generated." 
    ::= { cGgsnNotifMgmt 4 }

cGgsnHistNotifMaxLength OBJECT-TYPE
    SYNTAX          Integer32 (1..2147483647)
    UNITS           "entries"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The maximum number of entries to be retained in the
        cGgsnHistNotifTable. When the table is full, the oldest 
        entries are removed to make space for new entries."
    DEFVAL          { 100 } 
    ::= { cGgsnNotifMgmt 5 }

cGgsnHistNotifLatestIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4294967295)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The value of cGgsnHistNotifIndex for the most recently
        created entry in cGgsnHistNotifTable." 
    ::= { cGgsnNotifMgmt 6 }

cGgsnHistNotifTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CGgsnHistNotifEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A history table of the most recent cGgsnNotification
        notifications generated by this device.
        If a new cGgsnNotification notification is generated when
        the number of entries is equal to cGgsnHistNotifMaxLength,
        then the oldest entry is deleted and replaced with an entry
        for the latest notification."
    ::= { cGgsnNotifMgmt 7 }

cGgsnHistNotifEntry OBJECT-TYPE
    SYNTAX          CGgsnHistNotifEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Detailed information concerning a particular notification
        that previously generated from this device."
    INDEX           { cGgsnHistNotifIndex } 
    ::= { cGgsnHistNotifTable 1 }

CGgsnHistNotifEntry ::= SEQUENCE {
        cGgsnHistNotifIndex          Unsigned32,
        cGgsnHistNotifType           INTEGER,
        cGgsnHistNotifSeverity       CiscoAlarmSeverity,
        cGgsnHistNotifTimestamp      TimeStamp,
        cGgsnHistNotifGgsnIpAddrType InetAddressType,
        cGgsnHistNotifGgsnIpAddr     InetAddress,
        cGgsnHistNotifInfo           DisplayString
}

cGgsnHistNotifIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4294967295)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A monotonically increasing integer for the sole purpose of
        indexing notifications. When it reaches the maximum value,
        it wraps the value back to 1." 
    ::= { cGgsnHistNotifEntry 1 }

cGgsnHistNotifType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        ggsnServiceUp(1),
                        ggsnServiceDown(2),
                        mapSgsnUp(3),
                        mapSgsnDown(4),
                        noResource(5),
                        noRADIUS(6),
                        noDHCPServer(7),
                        ipAllocationFail(8),
                        authenticationFail(9),
                        apnUnreachable(10)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the type of notification." 
    ::= { cGgsnHistNotifEntry 2 }

cGgsnHistNotifSeverity OBJECT-TYPE
    SYNTAX          CiscoAlarmSeverity
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the severity level of the
        notification. This object cannot be set to cleared(1)
        or indeterminate(2)." 
    ::= { cGgsnHistNotifEntry 3 }

cGgsnHistNotifTimestamp OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the value of sysUpTime when
        this notification was generated." 
    ::= { cGgsnHistNotifEntry 4 }

cGgsnHistNotifGgsnIpAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the type of Internet address
        by which cGgsnHistNotifGgsnIpAddr is reachable." 
    ::= { cGgsnHistNotifEntry 5 }

cGgsnHistNotifGgsnIpAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The object indicates the IP address that uniquely
        identifies the device which generated the notification." 
    ::= { cGgsnHistNotifEntry 6 }

cGgsnHistNotifInfo OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (1..64))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "A textual description of cGgsnHistNotifType, which
        potentially contains additional information (more than
        just the type of alarm).
        If the text of the message exceeds 64 bytes, the message
        will be truncated to 63 bytes and a '*' character will
        be appended to indicate the message has been truncated." 
    ::= { cGgsnHistNotifEntry 7 }
 


cGgsnServiceNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Indicates whether cGgsnInServiceNotif notification and
        cGgsnMaintenanceNotif notification will be sent when a
        notification is generated by the device.
         - 'true',  it will enable the device to send a notification.
         - 'false', it will prevent the device from sending out a
                    notification."
    DEFVAL          { false } 
    ::= { cGgsnNotifMgmt 8 }

cGgsnMemoryNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Indicates whether cGgsnMemThresholdReachedNotif notification
        and cGgsnMemThresholdClearedNotif notification will be sent 
        when a notification is generated by the device.
         - 'true',  it will enable the device to send a notification.
         - 'false', it will prevent the device from sending out a
                    notification."
    DEFVAL          { false } 
    ::= { cGgsnNotifMgmt 9 }

cGgsnPdfNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "Indicates whether cGgsnPdfStateUpNotif notification and
        cGgsnPdfStateDownNotiff notification will be sent when a
        notification is generated by the device.
         - 'true',  it will enable the device to send a notification.
         - 'false', it will prevent the device from sending out a
                    notification."
    DEFVAL          { false } 
    ::= { cGgsnNotifMgmt 10 }

cGgsnGlobalErrorNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Indicates whether cGgsnGlobalErrorNotif notification will be
        sent when a notification is generated by the device.
         - 'true',  it will enable the device to send a notification.
         - 'false', it will prevent the device from sending out a
                    notification."
    DEFVAL          { false } 
    ::= { cGgsnNotifMgmt 11 }

cGgsnAccessPointNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Indicates whether cGgsnAccessPointNameNotif notification will
        be sent when a notification is generated by the device.
         - 'true',  it will enable the device to send a notification.
         - 'false', it will prevent the device from sending out a
                    notification."
    DEFVAL          { false } 
    ::= { cGgsnNotifMgmt 12 }

cGgsnPdpNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Indicates whether cGgsnPacketDataProtocolNotif notification
        will be sent when a notification is generated by the device.
         - 'true',  it will enable the device to send a notification.
         - 'false', it will prevent the device from sending out a
                    notification."
    DEFVAL          { false } 
    ::= { cGgsnNotifMgmt 13 }

-- Configurations

cGgsnDefaultIpAllocationMethod OBJECT-TYPE
    SYNTAX          INTEGER  {
                        disable(1),
                        dhcp(2),
                        radius(3)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Specifies the default method by which the GGSN obtains
        address leases for mobile user sessions.

           - 'disable', which indicates that dynamic address 
           allocation is disabled.

           - 'dhcp', which indicates that the DHCP server 
           will be used.

           - 'radius', which indicates that the radius server
           will be used."
    DEFVAL          { disable } 
    ::= { cGgsnConfigurations 1 }

cGgsnIdlePdpPurgeTimer OBJECT-TYPE
    SYNTAX          Unsigned32 (0..255)
    UNITS           "hours"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the time that the GGSN waits
        before purging idle PDP contexts. A value '0' will
        disable the purge timer."
    DEFVAL          { 72 } 
    ::= { cGgsnConfigurations 2 }

cGgsnIpDupProtectTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CGgsnIpDupProtectEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the range of IP address used in the
        GPRS PLMN. These IP addresses are used to avoid IP address 
        duplication in GPRS network. IP address duplication occurs 
        when a MS uses an IP address which is already used in the PLMN.
        The IP addresses configured inside GPRS network should be in 
        these ranges and MS IP address should not be in this range."
    ::= { cGgsnConfigurations 3 }

cGgsnIpDupProtectEntry OBJECT-TYPE
    SYNTAX          CGgsnIpDupProtectEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Entry containing the start and end IP address in the address
        range. An Entry with start IP > end IP is not allowed.
        No new entry will be accepted if that would cause any IP
        address(es) to be represented by more than one row in this 
        table."
    INDEX           {
                        cGgsnMsExcludeRangeStartIpType,
                        cGgsnMsExcludeRangeStartIp,
                        cGgsnMsExcludeRangeEndIpType,
                        cGgsnMsExcludeRangeEndIp
                    } 
    ::= { cGgsnIpDupProtectTable 1 }

CGgsnIpDupProtectEntry ::= SEQUENCE {
        cGgsnMsExcludeRangeStartIpType        InetAddressType,
        cGgsnMsExcludeRangeStartIp            InetAddress,
        cGgsnMsExcludeRangeEndIpType          InetAddressType,
        cGgsnMsExcludeRangeEndIp              InetAddress,
        cGgsnIpDupProtectRowStatus            RowStatus,
        cGgsnMsExcludeRangeStartIpv6Prefixlen InetAddressPrefixLength,
        cGgsnMsExcludeRangeEndIpv6Prefixlen   InetAddressPrefixLength
}

cGgsnMsExcludeRangeStartIpType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The type of Internet address by which
        cGgsnMsExcludeRangeStartIp is reachable. The value of this 
        object should be same as cGgsnMsExcludeRangeEndIpType." 
    ::= { cGgsnIpDupProtectEntry 1 }

cGgsnMsExcludeRangeStartIp OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (4..20))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Starting IP address in the address range." 
    ::= { cGgsnIpDupProtectEntry 2 }

cGgsnMsExcludeRangeEndIpType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The type of Internet address by which cGgsnMsExcludeRangeEndIp
        is reachable. The value of this object should be same as
        cGgsnMsExcludeRangeStartIpType." 
    ::= { cGgsnIpDupProtectEntry 3 }

cGgsnMsExcludeRangeEndIp OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (4..20))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Ending IP address in the address range." 
    ::= { cGgsnIpDupProtectEntry 4 }

cGgsnIpDupProtectRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to create a new row or delete an
        existing row in this table.

        To create a row, set this object to 'createAndGo' and the
        objects cGgsnMsExcludeRangeStartIpv6Prefixlen and
        cGgsnMsExcludeRangeEndIpv6Prefixlen should be set to valid
        values.
        To delete a row, set this object to 'destroy'." 
    ::= { cGgsnIpDupProtectEntry 5 }

cGgsnMsExcludeRangeStartIpv6Prefixlen OBJECT-TYPE
    SYNTAX          InetAddressPrefixLength
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the IPv6 prefix length supplied for
        the cGgsnMsExcludeRangeStartIp.The value of this object
        will be zero when cGgsnMsExcludeRangeStartIpType is IPv4." 
    ::= { cGgsnIpDupProtectEntry 6 }

cGgsnMsExcludeRangeEndIpv6Prefixlen OBJECT-TYPE
    SYNTAX          InetAddressPrefixLength
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the IPv6 prefix length supplied for
        the cGgsnMsExcludeRangeEndIp.The value of this object
        will be zero when cGgsnMsExcludeRangeEndIpType is IPv4." 
    ::= { cGgsnIpDupProtectEntry 7 }
 


cGgsnDefaultAggregTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CGgsnDefaultAggregEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the list of default aggregate routes
        configured on the GGSN. GGSN uses a static host route to 
        forward user data packets for each PDP context received 
        from Gi interface to Gn interface. Using the aggregate 
        route (address range), the total number of static routes 
        implemented in the GGSN for PDP requests can be greatly 
        reduced."
    ::= { cGgsnConfigurations 4 }

cGgsnDefaultAggregEntry OBJECT-TYPE
    SYNTAX          CGgsnDefaultAggregEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An Entry contains the IP network prefix which is used to
        combine the routes of PDP requests for the same network as 
        a single route on the GGSN."
    INDEX           {
                        cGgsnDefaultAggregIpAddrType,
                        cGgsnDefaultAggregIpAddr,
                        cGgsnDefaultAggregIpMask
                    } 
    ::= { cGgsnDefaultAggregTable 1 }

CGgsnDefaultAggregEntry ::= SEQUENCE {
        cGgsnDefaultAggregIpAddrType InetAddressType,
        cGgsnDefaultAggregIpAddr     InetAddress,
        cGgsnDefaultAggregIpMask     CiscoInetAddressMask,
        cGgsnDefaultAggregRowStatus  RowStatus
}

cGgsnDefaultAggregIpAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the type of Internet address denoted by
        cGgsnDefaultAggregIpAddr." 
    ::= { cGgsnDefaultAggregEntry 1 }

cGgsnDefaultAggregIpAddr OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (4..20))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the IP address whose network prefix
        is going to be defined by cGgsnDefaultAggregIpMask." 
    ::= { cGgsnDefaultAggregEntry 2 }

cGgsnDefaultAggregIpMask OBJECT-TYPE
    SYNTAX          CiscoInetAddressMask
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the net-mask pertaining to
        cGgsnDefaultAggregIpAddr." 
    ::= { cGgsnDefaultAggregEntry 3 }

cGgsnDefaultAggregRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to create a new row or delete an
        existing row in this table.

        To create a row, set this object to 'createAndGo'.
        To delete a row, set this object to 'destroy'.
        The values 'createAndWait' and 'notInService' are
        not supported." 
    ::= { cGgsnDefaultAggregEntry 4 }
 


cGgsnDefaultAaaAuthServerGroup OBJECT-TYPE
    SYNTAX          DisplayString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the AAA radius server group
        that is used for authentication by all APN's on this GGSN." 
    ::= { cGgsnConfigurations 5 }

cGgsnDefaultAaaAccServerGroup OBJECT-TYPE
    SYNTAX          DisplayString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the AAA radius server group
        that is used for accounting  by all APN's on this GGSN." 
    ::= { cGgsnConfigurations 6 }

cGgsnPppVirtualTemplate OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the virtual template interface used
        by PPP Type PDP's." 
    ::= { cGgsnConfigurations 7 }

cGgsnPppRegenVirtualTemplate OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the virtual template interface used
        for PPP Regeneration by the APN's on which PPP Regeneration 
        is configured.

        The value zero indicates that no interface is specified."
    DEFVAL          { 0 } 
    ::= { cGgsnConfigurations 8 }

cGgsnPlmnIpAddrRangeTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CGgsnPlmnIpAddrRangeEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the range of IP addresses that belong
        to the PLMN nodes in a GPRS network. This range does not 
        include address of various entities like RADIUS, DHCP, DNS 
        servers, etc., which are not part of PLMN."
    ::= { cGgsnConfigurations 9 }

cGgsnPlmnIpAddrRangeEntry OBJECT-TYPE
    SYNTAX          CGgsnPlmnIpAddrRangeEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Entry containing the first and last IP address in the address
        range. An Entry with first-IP > last-IP is not allowed. No 
        new entry will be accepted if that would cause any IP 
        address(es) to be represented by more than one row in this 
        table."
    INDEX           {
                        cGgsnPlmnAddrRangeIpAddrType,
                        cGgsnPlmnAddrRangeFirstIp,
                        cGgsnPlmnAddrRangeLastIp
                    } 
    ::= { cGgsnPlmnIpAddrRangeTable 1 }

CGgsnPlmnIpAddrRangeEntry ::= SEQUENCE {
        cGgsnPlmnAddrRangeIpAddrType         InetAddressType,
        cGgsnPlmnAddrRangeFirstIp            InetAddress,
        cGgsnPlmnAddrRangeLastIp             InetAddress,
        cGgsnPlmnAddrRangeRowStatus          RowStatus,
        cGgsnPlmnAddrRangeUsage              INTEGER,
        cGgsnPlmnAddrRangeFirstIpv6Prefixlen InetAddressPrefixLength,
        cGgsnPlmnAddrRangeLastIpv6Prefixlen  InetAddressPrefixLength
}

cGgsnPlmnAddrRangeIpAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The address type for cGgsnPlmnAddrRangeFirstIp and
        cGgsnPlmnAddrRangeLastIp addresses." 
    ::= { cGgsnPlmnIpAddrRangeEntry 1 }

cGgsnPlmnAddrRangeFirstIp OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (4..20))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "First IP address in the address range." 
    ::= { cGgsnPlmnIpAddrRangeEntry 2 }

cGgsnPlmnAddrRangeLastIp OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (4..20))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Last IP address in the address range." 
    ::= { cGgsnPlmnIpAddrRangeEntry 3 }

cGgsnPlmnAddrRangeRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to create a new row or delete an
        existing row in this table.

        To create a row, set this object to 'createAndGo' and the
        objects cGgsnPlmnAddrRangeFirstIpv6Prefixlen and
        cGgsnPlmnAddrRangeLastIpv6Prefixlen should be set to valid
        values.
        To delete a row, set this object to 'destroy'.
        To modify a row, the row needs to be deleted and created fresh
        with new values." 
    ::= { cGgsnPlmnIpAddrRangeEntry 4 }

cGgsnPlmnAddrRangeUsage OBJECT-TYPE
    SYNTAX          INTEGER  {
                        security(1),
                        sgsn(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies how the address range will be used by
        the GGSN.  

        When set to 'security', the address range is used for GGSN
        security feature i.e. any TPDU with destination address that
        falls in this address range will be discarded.

        When set to 'sgsn', the address range denotes the sgsn address
        range in the local PLMN which can be used to check roaming MS."
    DEFVAL          { security } 
    ::= { cGgsnPlmnIpAddrRangeEntry 5 }

cGgsnPlmnAddrRangeFirstIpv6Prefixlen OBJECT-TYPE
    SYNTAX          InetAddressPrefixLength
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the IPv6 prefix length supplied for
        the cGgsnPlmnAddrRangeFirstIp .The value of this object
        will be zero when cGgsnPlmnAddrRangeFirstIpType is IPv4." 
    ::= { cGgsnPlmnIpAddrRangeEntry 6 }

cGgsnPlmnAddrRangeLastIpv6Prefixlen OBJECT-TYPE
    SYNTAX          InetAddressPrefixLength
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the IPv6 prefix length supplied for
        the cGgsnPlmnAddrRangeLastIp .The value of this object
        will be zero when cGgsnPlmnAddrRangeLastIpType is IPv4." 
    ::= { cGgsnPlmnIpAddrRangeEntry 7 }
 

-- IMS Configurations

cGgsnImsConfigurations  OBJECT IDENTIFIER
    ::= { cGgsnConfigurations 10 }


cGgsnPdfTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CGgsnPdfEntry 
    MAX-ACCESS      not-accessible
    STATUS          deprecated
    DESCRIPTION
        "This table contains the details of PDF server that the GGSN
        supports. The table elements describes their properties.

        PDF's are the server's to which the client GGSN makes the
        TCP connection using the COPS protocol over the Go
        interface. GGSN can have connections with multiple
        PDF's."
    ::= { cGgsnImsConfigurations 1 }

cGgsnPdfEntry OBJECT-TYPE
    SYNTAX          CGgsnPdfEntry
    MAX-ACCESS      not-accessible
    STATUS          deprecated
    DESCRIPTION
        "Entry containing the PDF servers details (name and
        IP address) and also how the GGSN should communicate
        with PDF, like timeout when there is no response,
        number of retries."
    INDEX           {
                        cGgsnPdfGroupName,
                        cGgsnPdfDomainName,
                        cGgsnPdfIpAddressType,
                        cGgsnPdfIpAddress
                    } 
    ::= { cGgsnPdfTable 1 }

CGgsnPdfEntry ::= SEQUENCE {
        cGgsnPdfGroupName         SnmpAdminString,
        cGgsnPdfDomainName        InetAddressDNS,
        cGgsnPdfIpAddressType     InetAddressType,
        cGgsnPdfIpAddress         InetAddress,
        cGgsnPdfRowStatus         RowStatus,
        cGgsnPdfReconnectTimeOut  Unsigned32,
        cGgsnPdfReconnectRetries  Unsigned32,
        cGgsnPdfReconExpPdpDelete TruthValue,
        cGgsnPdfReqRetryTimeOut   Unsigned32,
        cGgsnPdfReqRetries        Unsigned32
}

cGgsnPdfGroupName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..100))
    MAX-ACCESS      not-accessible
    STATUS          deprecated
    DESCRIPTION
        "This object specifies the PDF group name. Currently
        this group name is just an identity to this group." 
    ::= { cGgsnPdfEntry 1 }

cGgsnPdfDomainName OBJECT-TYPE
    SYNTAX          InetAddressDNS (SIZE  (1..100))
    MAX-ACCESS      not-accessible
    STATUS          deprecated
    DESCRIPTION
        "This is a Fully Qualified Domain Name (FQDN), which has
        to be configured along with the IP address of the PDF.
        There will be no name resolving for the FQDN, it will 
        be used as it is." 
    ::= { cGgsnPdfEntry 2 }

cGgsnPdfIpAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          deprecated
    DESCRIPTION
        "This object specifies the type of IP address of
        the PDF server." 
    ::= { cGgsnPdfEntry 3 }

cGgsnPdfIpAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          deprecated
    DESCRIPTION
        "This object specifies the IP address of the PDF
        server. The type of the address is specified by
        the object cGgsnPdfIpAddressType." 
    ::= { cGgsnPdfEntry 4 }

cGgsnPdfRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "This object is used to create a new row or delete an
        existing row in this table.

        To create a row, set this object to 'createAndGo(4)'.
        To delete a row, set this object to 'destroy(6)'." 
    ::= { cGgsnPdfEntry 5 }

cGgsnPdfReconnectTimeOut OBJECT-TYPE
    SYNTAX          Unsigned32 (1..60)
    UNITS           "minutes"
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "Whenever a connection outage is detected (by keepalive
        mechanism etc.) by GGSN to the PDF server. The GGSN waits for
        the interval configured in this object. Once this timer is
        expired, another attempt is made for connection 
        establishment."
    DEFVAL          { 1 } 
    ::= { cGgsnPdfEntry 6 }

cGgsnPdfReconnectRetries OBJECT-TYPE
    SYNTAX          Unsigned32 (0..10 | 65535)
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "This is the number of attempts for connection establishment
        after the timeout value set in cGgsnPdfReconnectTimeOut.
        After the configured number of retries, all the COPS sessions
        (and associated PDP contexts) are cleared.

        The value '65535' which is default, will be infinite retries."
    DEFVAL          { 65535 } 
    ::= { cGgsnPdfEntry 7 }

cGgsnPdfReconExpPdpDelete OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "This objects defines the handling of the PDP context in
        the connection loss scenario. When this object is set to
        true, then on connection loss, the PDP delete will be
        initiated."
    DEFVAL          { false } 
    ::= { cGgsnPdfEntry 8 }

cGgsnPdfReqRetryTimeOut OBJECT-TYPE
    SYNTAX          Unsigned32 (1..60)
    UNITS           "seconds"
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "For each COPS REQ sent to PDF, GGSN will start a request retry
        timer with this value. If DEC is not received within the
        timeout, the REQ is resent for cGgsnPdfReqRetries times."
    DEFVAL          { 1 } 
    ::= { cGgsnPdfEntry 9 }

cGgsnPdfReqRetries OBJECT-TYPE
    SYNTAX          Unsigned32 (0..10)
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "This is the number of retries which has to be sent for the
        COPS REQ being sent. If DEC is not received even after sending
        the COPS REQ for configured number of retries, the PDP context
        activation/modification (which had triggered this REQ) is
        rejected."
    DEFVAL          { 3 } 
    ::= { cGgsnPdfEntry 10 }
 


cGgsnPcscfTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CGgsnPcscfEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the entries of P-CSCF groups with the
        addresses configured. One or more IP address can be
        configured per group name. This group in turn will be mapped
        to the APN.

        P-CSCF is a network element providing session management
        services. When the UE request the GGSN for P-CSCF 
        address through activate PDP Request, these addresses
        will be returned to the UE in the order which they are
        configured."
    ::= { cGgsnImsConfigurations 2 }

cGgsnPcscfEntry OBJECT-TYPE
    SYNTAX          CGgsnPcscfEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry is created when the user configures the
        group name and an IP address is set."
    INDEX           {
                        cGgsnPcscfGroupName,
                        cGgsnPcscfIpAddressType,
                        cGgsnPcscfIpAddress
                    } 
    ::= { cGgsnPcscfTable 1 }

CGgsnPcscfEntry ::= SEQUENCE {
        cGgsnPcscfGroupName     SnmpAdminString,
        cGgsnPcscfIpAddressType InetAddressType,
        cGgsnPcscfIpAddress     InetAddress,
        cGgsnPcscfRowStatus     RowStatus
}

cGgsnPcscfGroupName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..100))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This group name is the identifier for the P-CSCF
        addresses configured." 
    ::= { cGgsnPcscfEntry 1 }

cGgsnPcscfIpAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the type of the P-CSCF
        IP address." 
    ::= { cGgsnPcscfEntry 2 }

cGgsnPcscfIpAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the IP address of the P-CSCF.
        The type of this address is specified by the object
        cGgsnPcscfIpAddressType." 
    ::= { cGgsnPcscfEntry 3 }

cGgsnPcscfRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to create a new row or delete an
        existing row in this table.

        To create a row, set this object to 'createAndGo(4)'.
        To delete a row, set this object to 'destroy(6)'." 
    ::= { cGgsnPcscfEntry 4 }
 


cGgsnMemoryThreshold OBJECT-TYPE
    SYNTAX          Unsigned32 (0..1024)
    UNITS           "98304Bytes"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "GGSN memory overload protection is a mechanism to
        prevent GGSN from completely running out of memory
        when GGSN is running near its capacity or in some
        failure scenarios like CG down. A protection mechanism
        was put into place where charging triggers would be
        ignored, PDP create would be rejected, PDP update
        request will delete PDP, once the available memory on 
        the GGSN drops below a configured threshold. 

        Charging triggers occurs due to certain criteria's like
        volume limit, time limit. When one of the conditions is
        met , the CDR's are closed and will be updated to the
        charging gateway."
    DEFVAL          { 0 } 
    ::= { cGgsnConfigurations 11 }

cGgsnServiceMode OBJECT-TYPE
    SYNTAX          INTEGER  {
                        inService(1),
                        maintenance(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "GGSN supports this GPRS service mode for maintenance
        purposes. Two modes are supported in GGSN, operational and
        maintenance mode. 'inService' mode represents nominal 
        operation, and there will be no change in the way the GGSN 
        operates.  'maintenance' mode imposes restrictions, such as 
        some of the configurations allowed by the GGSN, and no new 
        PDPs will be accepted.  'maintenance' mode can be useful to 
        make some changes to the configuration of the GGSN without 
        affecting the existing PDPs.

        'maintenance' mode gloablly applies to the GGSN, which means 
        the whole box will be put in maintenance mode. There also 
        exists APN level maintenance mode, which is defined in 
        CISCO-GPRS_ACC-PT-MIB, and charging maintenance mode which
        is defined in CISCO-GPRS-CHARGING-MIB, which is out of 
        scope of this MIB.

        Internally GGSN maintains three states (inService, 
        maintenance and outOfService ), which can be viewed with
        cGgsnServiceModeStatus.

        The SNMP entity generates notification when switching modes. 
        It uses the cGgsnInServiceNotif and cGgsnMaintenanceNotif
        for this purpose."
    DEFVAL          { inService } 
    ::= { cGgsnConfigurations 12 }

cGgsnPlmnTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CGgsnPlmnEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Mobile Country Code (MCC) and Mobile Network Code (MNC)
        together identify a GPRS PLMN of an operator. PLMN Ids
        other than home PLMNs are considered as foreign. There
        will be some situations where some foreign PLMNs has to
        be treated as trusted PLMNs. 

        This table contains the list of PLMNs, there can be one
        home PLMN entry and multiple trusted PLMN entry."
    ::= { cGgsnConfigurations 13 }

cGgsnPlmnEntry OBJECT-TYPE
    SYNTAX          CGgsnPlmnEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Entry containing list of home PLMN Ids and the Trusted
        PLMN Ids."
    INDEX           {
                        cGgsnPlmnMcc,
                        cGgsnPlmnMnc
                    } 
    ::= { cGgsnPlmnTable 1 }

CGgsnPlmnEntry ::= SEQUENCE {
        cGgsnPlmnMcc       SnmpAdminString,
        cGgsnPlmnMnc       SnmpAdminString,
        cGgsnPlmnRowStatus RowStatus,
        cGgsnPlmnScope     INTEGER
}

cGgsnPlmnMcc OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (3))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The Mobile Country Code (MCC) is part of the PLMN Id."
    REFERENCE
        "Digital cellular telecommunications system (Phase 2+);
        Numbering, addressing and identification
        (GSM 03.03 version 7.3.0 Release 1998)
        Available SMG only" 
    ::= { cGgsnPlmnEntry 1 }

cGgsnPlmnMnc OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (2..3))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The Mobile Network Code (MNC) is part of the PLMN Id."
    REFERENCE
        "Digital cellular telecommunications system (Phase 2+);
        Numbering, addressing and identification
        (GSM 03.03 version 7.3.0 Release 1998)
        Available SMG only" 
    ::= { cGgsnPlmnEntry 2 }

cGgsnPlmnRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to create a new row or delete an
        existing row in this table.

        To create a row, set this object to 'createAndGo'.
        To delete a row, set this object to 'destroy'.
        To modify a row, the row needs to be deleted and created fresh
        with new values." 
    ::= { cGgsnPlmnEntry 3 }

cGgsnPlmnScope OBJECT-TYPE
    SYNTAX          INTEGER  {
                        home(1),
                        trusted(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies whether the PLMN is home or
        trusted. Only one PLMN entry can be home"
    DEFVAL          { home } 
    ::= { cGgsnPlmnEntry 4 }
 


cGgsnSessionTimeout OBJECT-TYPE
    SYNTAX          Unsigned32 (0 | 30..4294967)
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the PDP context timeout value. The
        PDP context will be terminated after this timer expiry.

        The value present in this will have meaning when the object
        cGgsnRadAttrSessTimeout is set to 'true' and if the
        attribute#27 not received from the AAA."
    DEFVAL          { 0 } 
    ::= { cGgsnConfigurations 14 }

cGgsnThruputIntervalOne OBJECT-TYPE
    SYNTAX          Unsigned32 (0..65535)
    UNITS           "minutes"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object and cGgsnThruputIntervalTwo specifies the
        interval at which the data throughput needs to be
        collected per APN/SGSN.

        Once this object is set to some valid value, the data
        throughput collections gets started for per configured
        APN and per PATH created. The data throughput collection
        is updated periodically (each expiry of configured throughput
        interval) to the corresponding objects (cGgsnSgsnStatTable 
        for per SGSN and cgprsAccPtThruputStatsTable for per APN).

        When this object is set to '0', the collection for this
        interval get stopped and the data related to this interval
        is deleted from the tables (cGgsnSgsnStatTable and
        cgprsAccPtThruputStatsTable).

        INCONSISTENT value SNMP error will happen when trying to set
        cGgsnThruputIntervalOne and cGgsnThruputIntervalTwo with same
        value expect '0'. Setting the same value to the same object
        will reset the value / collection status for that interval."
    DEFVAL          { 0 } 
    ::= { cGgsnConfigurations 15 }

cGgsnThruputIntervalTwo OBJECT-TYPE
    SYNTAX          Unsigned32 (0..65535)
    UNITS           "minutes"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the time interval TWO for
        collecting the throughput per APN/SGSN.

        This object is same as cGgsnThruputIntervalOne. It's just
        an option for a second throughput collection for a different
        throughput interval time.

        The value 0 means the timer TWO will be disabled.

        INCONSISTENT value SNMP error will happen when trying to set
        cGgsnThruputIntervalOne and cGgsnThruputIntervalTwo with same
        value expect '0'. Setting the same value to the same object
        will reset the value / collection status for that interval."
    DEFVAL          { 0 } 
    ::= { cGgsnConfigurations 16 }

cGgsnCompliance3GppGgsn OBJECT-TYPE
    SYNTAX          INTEGER  {
                        default(0),
                        release40(1)
                    }
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object specifies the compliance level for the
        particular GGSN version present in cGgsnVersion. This 
        object can be used to set back the compliance level to
        the previous GGSN version.

        When set to 'default', the compliance level for that
        GGSN version indicated by the object cGgsnVersion will 
        be considered.

        Currently, when the cGgsnVersion is holding a value of
        'release50', the compliance level can be set back to
        'release40'. This object is deprecated as the standard
        GGSN 8.0 release deprecated this configuration."
    REFERENCE       "3GPP TS 29.060 v3.15.0/v4.6.0/v5.4.0"
    DEFVAL          { default } 
    ::= { cGgsnConfigurations 17 }

cGgsnCreateReqV1UpdExistPdp OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object is used for backward compatibility due to
        to implementation of CR 311.

        CR 311: The SGSN shall not send a Create PDP Context Request 
        for an already active context. If a new Create PDP Context 
        Request is incoming on TEID 0 for an already active PDP 
        context, this Create PDP Context Request must be considered 
        related to a new session. The existing PDP context shall be 
        torn down locally, and the associated PDP contexts deleted 
        locally, before the new session is created. If a new Create 
        PDP Context Request is incoming on a TEID which is different 
        from 0 and this TEID is already allocated to one or more 
        activated PDP contexts, and the NSAPI IE value in this message
        matches the NSAPI value of an active PDP context, the GGSN 
        shall send back a Create PDP Context Response with a rejection 
        cause code. It is implementation dependent deciding whether 
        to teardown or keep the existing PDP context.

        'false' - The changes due to CR 311 will be applicable.
        'true'  - The changes due to CR 311 will not be taken
                  into account.

        This object has no meaning when the object 
        cGgsnCompliance3GppGgsn holds a value of 'release40'. This
        object is deprecated as the standerd GGSN release 5.2
        deprecated this configuration."
    REFERENCE       "3GPP TS 29.060 v3.15.0/v4.6.0/v5.4.0"
    DEFVAL          { false } 
    ::= { cGgsnConfigurations 18 }

cGgsnRadAttrSessTimeout OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object is used for enabling the session timeout feature
        on the global (router) level set using cGgsnSessionTimeout, APN 
        level (cgprsAccPtAbsoluteSessionTimer, which is defined in 
        CISCO-GPRS-ACC-PT-MIB and is outside the scope of this MIB) 
        and also parse the RADIUS attribute #27 present in the 
        access-accept request.

        'true'  - Session timeout is enabled.
        'false' - Session timeout is disabled."
    DEFVAL          { false } 
    ::= { cGgsnConfigurations 19 }

cGgsnDownlinkVerifyMsDisable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object enables the feature which will allow the GGSN
        to route IP packets beyond MS. This works only if a static
        route is added in GGSN to the node beyond the MS.

        On enabling this feature, GGSN will route the packets in
        both process switch path and cef switch path. This is 
        supported only for IP PDP type.

        This feature has some limitations:
        - This is not scalable, since the operator has to add static
          route to all the node beyond the MS.
        - Only works for MS having static address.
        - In case of GTPv1 the MS has to select TFT's so as to allow
          traffic flow in the downlink direction.
        - IP address assignment/Radius for the devices behind the MS 
          needs to be done within the scope of that network; the GGSN 
          will not provide this facility in anyway for the hosts 
          behind the MS. 
        - In case for MWAM and Cat6500/7600 environment, the static 
          route should be added only on that particular GGSN on the 
          MWAM from where the MS is reachable.

        'true' - Routing beyond MS is enabled.
        'false' - Routing beyond MS is disabled."
    DEFVAL          { false } 
    ::= { cGgsnConfigurations 20 }

cGgsnSlbMode OBJECT-TYPE
    SYNTAX          INTEGER  {
                        directed(1),
                        dispatched(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "GTP SLB can operate in two modes-dispatched and directed.

        - 'dispatched' mode: It forwards the create request without
        changing the destination IP address (vserver address) and the
        create response comes from the same (vserver) address.

        - 'directed' mode: It changes the destination IP address to
        that of GGSN's VT and the create response comes from the
        GGSN VT." 
    ::= { cGgsnConfigurations 21 }

cGgsnSlbNotif OBJECT-TYPE
    SYNTAX          INTEGER  {
                        cacFailure(1),
                        sessionDeletion(2)
                    }
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object is used to enable or disable the GGSN behavior
        of sending CAC failure notification to SLB, or session failure
        notification to SLB.

        If this object is set to cacFailure(1), then this object is
        required to enable the feature in the dispatched mode
        of operation of SLB.

        If this object is set to sessionDeletion(2), then GGSN will
        send delete notification message to SLB when the last PDP 
        associated with a IMSI is deleted. This object is deprecated
        by cGgsnSlbNotifyCacFailure and 
        cGgsnSlbNotifySessionDeletion." 
    ::= { cGgsnConfigurations 22 }

cGgsnSlbVserverTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CGgsnSlbVserverEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table includes the different virtual servers
        (IP address of virtual servers) and the
        elements gives the interface to reach these servers.

        The table is indexed on the vserver address.

        The table objects can be modified, when the RowStatus
         (cGgsnSlbVserRowStatus) is active."
    ::= { cGgsnConfigurations 23 }

cGgsnSlbVserverEntry OBJECT-TYPE
    SYNTAX          CGgsnSlbVserverEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Entry contains the Virtual server details(IP address type,
        IP address)and next hop address and VRF name."
    INDEX           {
                        cGgsnSlbVserAddrType,
                        cGgsnSlbVserAddress
                    } 
    ::= { cGgsnSlbVserverTable 1 }

CGgsnSlbVserverEntry ::= SEQUENCE {
        cGgsnSlbVserAddrType        InetAddressType,
        cGgsnSlbVserAddress         InetAddress,
        cGgsnSlbVserNextHopAddrType InetAddressType,
        cGgsnSlbVserNextHopAddress  InetAddress,
        cGgsnSlbVserVrfName         SnmpAdminString,
        cGgsnSlbVserRowStatus       RowStatus
}

cGgsnSlbVserAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the address type of the vserver." 
    ::= { cGgsnSlbVserverEntry 1 }

cGgsnSlbVserAddress OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (4..20))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the address of GTP vservers.
        It is required only in directed mode. If SLB is running
        in directed mode and this object is not configured, then
        the feature remains disabled.

        If SLB is running in the dispatched mode, the vserver that
        forwarded the create request is known to the GGSN and
        thus it is possible to send the notification directly to
        the vserver." 
    ::= { cGgsnSlbVserverEntry 2 }

cGgsnSlbVserNextHopAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the IP address type to reach the
        virtual server."
    DEFVAL          { ipv4 } 
    ::= { cGgsnSlbVserverEntry 3 }

cGgsnSlbVserNextHopAddress OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (4..20))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the IP address to reach the vserver." 
    ::= { cGgsnSlbVserverEntry 4 }

cGgsnSlbVserVrfName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the VRF name on an interface on GGSN
        connected to SLB, to reach the vserver." 
    ::= { cGgsnSlbVserverEntry 5 }

cGgsnSlbVserRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object will create new row into the table or deletes the
        existing one.

        To create a row, set this object to 'createAndGo(4)'.
        To delete a row, set this object to 'destroy(6)'." 
    ::= { cGgsnSlbVserverEntry 6 }
 


cGgsnSlbNotifyCacFailure OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object is used to enable or disable the GGSN behavior
        of sending CAC failure notification to SLB.

        CAC fails on GGSN if either the maximum number of PDPs
        reaches limit or there is not enough bandwidth for the
        traffic class for the APN.

        If this object is set to 'true', GGSN sends the notification
        to all the SLB vservers when UMTS CAC fails."
    DEFVAL          { false } 
    ::= { cGgsnConfigurations 24 }

cGgsnSlbNotifySessionDeletion OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object is used to enable or disable the GGSN behavior
        of sending session deletion notification to SLB.

        If this object is set to 'true', GGSN sends delete notification
        message to SLB when the last PDP associated with a IMSI is
        deleted."
    DEFVAL          { false } 
    ::= { cGgsnConfigurations 25 }

-- Status

cGgsnVersion OBJECT-TYPE
    SYNTAX          INTEGER  {
                        release14(1),
                        release30(2),
                        release40(3),
                        release31(4),
                        release50(5),
                        release60(6),
                        release70(7),
                        release80(8),
                        release90(9),
                        release100(10)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the which release of GPRS
        image is currently running on the GGSN." 
    ::= { cGgsnStatus 1 }

cGgsnActiveNetworkInitPdps OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the number of network initiated
        PDP contexts that are currently active.

        Trigger Condition: This counter is incremented /
        decremented by the create/delete PDP context request
        message respectively." 
    ::= { cGgsnStatus 2 }

cGgsnActivePppPdps OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the number of PPP PDP contexts
        that are currently active.

        Trigger Condition: This counter is incremented /
        decremented by the create/delete PPP PDP context request
        message respectively." 
    ::= { cGgsnStatus 3 }

cGgsnActivePppRegenPdps OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the number of PPP-Regen PDP contexts
        that are currently active.

        Trigger Condition: This counter is incremented /
        decremented by the create/delete PPP Regeneration PDP
        context request message respectively." 
    ::= { cGgsnStatus 4 }

cGgsnPendingPppRegenPdps OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the current number of pending
        PPP regeneration sessions.

        Trigger Condition: This counter is triggered 
        by the create PPP Regeneration PDP context request 
        message." 
    ::= { cGgsnStatus 5 }

cGgsnActiveGtpVersion0Pdps OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the current number of active GTP v0 PDP
        contexts.

        Trigger Condition: This counter is incremented /
        decremented by the create/delete PDP context request
        message respectively." 
    ::= { cGgsnStatus 6 }

cGgsnActiveGtpVersion1Pdps OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the current number of active GTP v1 PDP
        contexts.

        Trigger Condition: This counter is incremented /
        decremented by the create/delete PDP context request
        message respectively." 
    ::= { cGgsnStatus 7 }

cGgsnGtpEncapInterface OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the ifIndex of the interface on which
        gtp encapsulation is configured. Only one interface can
        be configured with gtp encapsulation on the GGSN. A zero value
        indicates that no interface is configured with gtp 
        encapsulation." 
    ::= { cGgsnStatus 8 }

cGgsnServiceModeStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        inService(1),
                        maintenance(2),
                        outOfServiceInProgress(3),
                        outOfService(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the internal service mode which
        GGSN maintains. The service switching is done with object
        cGgsnServiceMode." 
    ::= { cGgsnStatus 9 }

cGgsnConfigVersion OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the config version of GPRS
        image. The value of this object will be of the form
        Version.Release.Maintenence.

        This object provides information on the ability 
        of the devices to support configuration operations." 
    ::= { cGgsnStatus 10 }

cGgsnPrepaidPDPs OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the number of prepaid PDPs created
        since the last clearance of statistics 
        (GPRS service aware statistics)." 
    ::= { cGgsnStatus 11 }

cGgsnPostpaidPDPs OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the current number of postpaid PDPs,
        created since the last clearance of statistics
        (GPRS service aware statistics)." 
    ::= { cGgsnStatus 12 }

cGgsnActivatedIpv6Gtpv0Pdp OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "PDPs"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the current number of active GTP v0
        ipv6 PDP contexts.

        Trigger Condition: This counter is incremented by the create
        PDP context request and decremented by the delete PDP context
        request message." 
    ::= { cGgsnStatus 13 }

cGgsnActivatedIpv6Gtpv1Pdp OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "PDPs"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the current number of active GTP v1
        ipv6 PDP contexts.

        Trigger Condition: This counter is incremented by the create
        PDP context request and decremented by the delete PDP context
        request message." 
    ::= { cGgsnStatus 14 }

cGgsnActivatedIpv6Ms OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "PDPs"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the current number of MS with active
        IPv6 PDPs." 
    ::= { cGgsnStatus 15 }

cGgsnGtpEncapsuTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CGgsnGtpEncapsuEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains information about ifIndex of the
        interfaces on which gtp encapsulation is configured."
    ::= { cGgsnStatus 16 }

cGgsnGtpEncapsuEntry OBJECT-TYPE
    SYNTAX          CGgsnGtpEncapsuEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The cGgsnGtpEncapsuEntry represents the ifIndex of the
        interface on which gtp encapsulation is configured.
        Only one interface can be configured with gtp
        encapsulation on the GGSN. Entry in the table created whenever
        interface is configured with gtp encapsulation, 
        Entry is deleted whenever unconfiguring the gtp
        encapsulation  from the interface."
    INDEX           { ifIndex } 
    ::= { cGgsnGtpEncapsuTable 1 }

CGgsnGtpEncapsuEntry ::= SEQUENCE {
        cGgsnGtpEncapsuInterface InterfaceIndexOrZero
}

cGgsnGtpEncapsuInterface OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the ifIndex of the interface on
        which gtp encapsulation is configured. Only one interface can
        be configured with gtp encapsulation on the GGSN. A zero value
        indicates that no interface is configured with gtp 
        encapsulation." 
    ::= { cGgsnGtpEncapsuEntry 1 }
 


-- Notif Info

cGgsnPdfServerAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      accessible-for-notify
    STATUS          deprecated
    DESCRIPTION
        "This object specifies the type of IP address of
        the PDF server." 
    ::= { cGgsnNotifInfo 1 }

cGgsnPdfServerAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      accessible-for-notify
    STATUS          deprecated
    DESCRIPTION
        "This object specifies the IP address of the PDF
        server. The type of this address is specified by
        the object cGgsnPdfServerAddrType." 
    ::= { cGgsnNotifInfo 2 }

cGgsnNotifAccessPointName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..100))
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object specifies the Access Point Name and is used
        specify the name in the cGgsnAccessPointNameNotif 
        notification." 
    ::= { cGgsnNotifInfo 3 }

cGgsnNotifPdpImsi OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..8))
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object specifies the International Mobile Subscriber
        Identity (IMSI) of the user for whom the notification
        is generated.  This object is used to specify IMSI of the
        user in the cGgsnPacketDataProtocolNotif notification." 
    ::= { cGgsnNotifInfo 4 }

cGgsnGlobalErrorTypes OBJECT-TYPE
    SYNTAX          INTEGER  {
                        ggsnServiceUp(1),
                        ggsnServiceDown(2),
                        mapSgsnUp(3),
                        mapSgsnDown(4),
                        noDHCPServer(5)
                    }
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object indicates the types of global errors
        as follows.

        'ggsnServiceUp'   -  GGSN service has started
        'ggsnServiceDown' -  GGSN service is shutdown
        'mapSgsnUp'       -  MAP-SGSN service has started
        'mapSgsnDown'     -  MAP-SGSN service is shutdown
        'noDHCPServer'    -- DHCP server is not configured" 
    ::= { cGgsnNotifInfo 5 }

cGgsnAccessPointErrorTypes OBJECT-TYPE
    SYNTAX          INTEGER  {
                        noRadius(1),
                        ipAllocationFail(2),
                        apnUnreachable(3)
                    }
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object indicates the types access point errors as
        follows.

         'noRadius'    - RADIUS Server is not configured. 
         'ipAllocationFail' - Unable to allocate IP address.
         'apnUnreachable' -  Unable to reach access point." 
    ::= { cGgsnNotifInfo 6 }

cGgsnPacketDataProtoErrorTypes OBJECT-TYPE
    SYNTAX          INTEGER  {
                        noResource(1),
                        authenticationFail(2),
                        ccrInitFail(3),
                        quotaPushFail(4)
                    }
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object indicates the types of Packet Data Protocol
        errors as follows.

         'noResource' - Mobile Station initiated PDP count reaches
                        the specified limit or
                        Network initiated PDP count reaches the 
                        specified limit.

         'authenticationFail' - Authentication failed.

         'ccrInitFail' - CCR(initial)is sent to diameter server, and 
                         Tx timer expires before getting CCA (initial)
                         response. The action on the PDP context 
                         creation is determined by the configured
                         failure handling, as specified in 
                         cGgsnSADccaCcfh object in 
                         CISCO-GGSN-SERVICE-AWARE-MIB.

         'quotaPushFail' - Quota Push failed, when the path between
                           CSG-QS is down or when CSG sends a negative
                           Response for quota push request." 
    ::= { cGgsnNotifInfo 7 }

cGgsnNotifPdpMsisdn OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object specifies the Mobile Subscriber ISDN (MSISDN)
        value of the user for whom the notification is generated.
        This object is used to specify MSISDN of the
        user in the cGgsnPacketDataProtocolNotif notification." 
    ::= { cGgsnNotifInfo 8 }
-- Notification Definitions

cGgsnNotifPrefix  OBJECT IDENTIFIER
    ::= { cGgsnMIB 2 }

cGgsnNotifications  OBJECT IDENTIFIER
    ::= { cGgsnNotifPrefix 0 }


-- notifications

cGgsnNotification NOTIFICATION-TYPE
    OBJECTS         {
                        cGgsnHistNotifType,
                        cGgsnHistNotifSeverity,
                        cGgsnHistNotifTimestamp,
                        cGgsnHistNotifGgsnIpAddrType,
                        cGgsnHistNotifGgsnIpAddr,
                        cGgsnHistNotifInfo
                    }
    STATUS          deprecated
    DESCRIPTION
        "This notification indicates the occurrence of a GGSN
        related alarm. If and when additional useful information
        is available for specific types of alarms, then that  
        information may be appended to the end of the
        notification in additional varbinds."
   ::= { cGgsnNotifications 1 }

cGgsnInServiceNotif NOTIFICATION-TYPE
    STATUS          current
    DESCRIPTION
        "A notification of this type is generated when GGSN is
        placed in inService mode which is specified by
        cGgsnServiceModeStatus."
   ::= { cGgsnNotifications 2 }

cGgsnMaintenanceNotif NOTIFICATION-TYPE
    STATUS          current
    DESCRIPTION
        "A notification of this type is generated when GGSN is
        placed in maintenance mode which is specified by
        cGgsnServiceModeStatus."
   ::= { cGgsnNotifications 3 }

cGgsnMemThresholdReachedNotif NOTIFICATION-TYPE
    STATUS          current
    DESCRIPTION
        "A notification of this type is generated when GGSN
        reaches the memory threshold value specified by
        cGgsnMemoryThreshold."
   ::= { cGgsnNotifications 4 }

cGgsnMemThresholdClearedNotif NOTIFICATION-TYPE
    STATUS          current
    DESCRIPTION
        "A notification of this type is generated when GGSN
        retains the memory and falls below threshold value 
        speficied by cGgsnMemoryThreshold."
   ::= { cGgsnNotifications 5 }

cGgsnPdfStateUpNotif NOTIFICATION-TYPE
    OBJECTS         {
                        cGgsnPdfServerAddrType,
                        cGgsnPdfServerAddr
                    }
    STATUS          deprecated
    DESCRIPTION
        "A notification of this type is generated when PDF
        connection comes UP."
   ::= { cGgsnNotifications 6 }

cGgsnPdfStateDownNotif NOTIFICATION-TYPE
    OBJECTS         {
                        cGgsnPdfServerAddrType,
                        cGgsnPdfServerAddr
                    }
    STATUS          deprecated
    DESCRIPTION
        "A notification of this type is generated when PDF
        connection goes DOWN."
   ::= { cGgsnNotifications 7 }

cGgsnGlobalErrorNotif NOTIFICATION-TYPE
    OBJECTS         {
                        cGgsnGlobalErrorTypes,
                        cGgsnHistNotifSeverity,
                        cGgsnHistNotifTimestamp,
                        cGgsnHistNotifGgsnIpAddrType,
                        cGgsnHistNotifGgsnIpAddr,
                        cGgsnHistNotifInfo
                    }
    STATUS          current
    DESCRIPTION
        "This notification indicates the occurrence of a GGSN
        related alarm."
   ::= { cGgsnNotifications 8 }

cGgsnAccessPointNameNotif NOTIFICATION-TYPE
    OBJECTS         {
                        cGgsnAccessPointErrorTypes,
                        cGgsnHistNotifSeverity,
                        cGgsnHistNotifTimestamp,
                        cGgsnHistNotifGgsnIpAddrType,
                        cGgsnHistNotifGgsnIpAddr,
                        cGgsnHistNotifInfo,
                        cGgsnNotifAccessPointName
                    }
    STATUS          current
    DESCRIPTION
        "This notification indicates the occurrence of a APN
        related alarm."
   ::= { cGgsnNotifications 9 }

cGgsnPacketDataProtocolNotif NOTIFICATION-TYPE
    OBJECTS         {
                        cGgsnPacketDataProtoErrorTypes,
                        cGgsnHistNotifSeverity,
                        cGgsnHistNotifTimestamp,
                        cGgsnHistNotifGgsnIpAddrType,
                        cGgsnHistNotifGgsnIpAddr,
                        cGgsnHistNotifInfo,
                        cGgsnNotifPdpImsi,
                        cGgsnNotifPdpMsisdn,
                        cGgsnNotifAccessPointName
                    }
    STATUS          current
    DESCRIPTION
        "This notification indicates the occurrence of a User
        related alarm."
   ::= { cGgsnNotifications 10 }
cGgsnMIBConformances  OBJECT IDENTIFIER
    ::= { cGgsnMIB 3 }

cGgsnMIBCompliances  OBJECT IDENTIFIER
    ::= { cGgsnMIBConformances 1 }

cGgsnMIBGroups  OBJECT IDENTIFIER
    ::= { cGgsnMIBConformances 2 }


-- Compliances statements

cGgsnMIBCompliance MODULE-COMPLIANCE
    STATUS          obsolete
    DESCRIPTION
        "The compliance statements for entities which
        implement the CISCO GGSN MIB.

        This is deprecated by cGgsnMIBComplianceRev1."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cGgsnStatisticsGroup,
                        cGgsnNotifMgmtGroup,
                        cGgsnConfigurationsGroup,
                        cGgsnNotifGroup,
                        cGgsnStatusGroup
                    }
    ::= { cGgsnMIBCompliances 1 }

cGgsnMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statements for entities which
        implement the CISCO GGSN MIB.

        This is deprecated by cGgsnMIBComplianceRev2"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cGgsnStatisticsGroup,
                        cGgsnNotifMgmtGroup,
                        cGgsnConfigurationsGroupRev1,
                        cGgsnNotifGroup,
                        cGgsnStatusGroup
                    }

    GROUP           cGgsnUmtsGroup
    DESCRIPTION
        "This group is mandatory for a GGSN that supports GTP v1."

    OBJECT          cGgsnHistNotifGgsnIpAddrType
    SYNTAX          INTEGER  {
                        unknown(0),
                        ipv4(1)
                    }
    DESCRIPTION
        "Support for ipv6(2) and dns(16) is not mandatory."

    OBJECT          cGgsnIpDupProtectRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnDefaultAggregRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnAddrRangeRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."
    ::= { cGgsnMIBCompliances 2 }

cGgsnMIBComplianceRev2 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statements for entities which
        implement the CISCO GGSN MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cGgsnStatisticsGroupRev1,
                        cGgsnNotifMgmtGroup,
                        cGgsnConfigurationsGroupRev2,
                        cGgsnNotifGroupRev1,
                        cGgsnStatusGroupRev1,
                        cGgsnNotifInfoGroup
                    }

    GROUP           cGgsnUmtsGroup
    DESCRIPTION
        "This group is mandatory for a GGSN that supports GTP v1."

    OBJECT          cGgsnHistNotifGgsnIpAddrType
    SYNTAX          INTEGER  {
                        unknown(0),
                        ipv4(1)
                    }
    DESCRIPTION
        "Support for ipv6(2) and dns(16) is not mandatory."

    OBJECT          cGgsnIpDupProtectRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnDefaultAggregRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnAddrRangeRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPdfRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPcscfRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."
    ::= { cGgsnMIBCompliances 3 }

cGgsnMIBComplianceRev3 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statements for entities which
        implement the CISCO GGSN MIB.

        This is deprecated by cGgsnMIBComplianceRev4."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cGgsnStatisticsGroupRev1,
                        cGgsnNotifMgmtGroupRev1,
                        cGgsnConfigurationsGroupRev2,
                        cGgsnNotifGroupRev2,
                        cGgsnStatusGroupRev1,
                        cGgsnNotifInfoGroupRev1
                    }

    GROUP           cGgsnUmtsGroup
    DESCRIPTION
        "This group is mandatory for a GGSN that supports GTP v1."

    OBJECT          cGgsnHistNotifGgsnIpAddrType
    SYNTAX          INTEGER  {
                        unknown(0),
                        ipv4(1)
                    }
    DESCRIPTION
        "Support for ipv6(2) and dns(16) is not mandatory."

    OBJECT          cGgsnIpDupProtectRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnDefaultAggregRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnAddrRangeRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPdfRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPcscfRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."
    ::= { cGgsnMIBCompliances 4 }

cGgsnMIBComplianceRev4 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statements for entities which
        implement the CISCO GGSN MIB.

        This is deprecated by cGgsnMIBComplianceRev5."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cGgsnStatisticsGroupRev1,
                        cGgsnNotifMgmtGroupRev1,
                        cGgsnConfigurationsGroupRev2,
                        cGgsnNotifGroupRev2,
                        cGgsnStatusGroupRev1,
                        cGgsnNotifInfoGroupRev1,
                        cGgsnStatusGroupConfigVer
                    }

    GROUP           cGgsnUmtsGroup
    DESCRIPTION
        "This group is mandatory for a GGSN that supports GTP v1."

    OBJECT          cGgsnHistNotifGgsnIpAddrType
    SYNTAX          INTEGER  {
                        unknown(0),
                        ipv4(1)
                    }
    DESCRIPTION
        "Support for ipv6(2) and dns(16) is not mandatory."

    OBJECT          cGgsnIpDupProtectRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnDefaultAggregRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnAddrRangeRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPdfRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPcscfRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."
    ::= { cGgsnMIBCompliances 5 }

cGgsnMIBComplianceRev5 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statements for entities which
        implement the CISCO GGSN MIB.

        This is deprecated by cGgsnMIBComplianceRev6."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cGgsnStatisticsGroupRev1,
                        cGgsnNotifMgmtGroupRev1,
                        cGgsnConfigurationsGroupRev2,
                        cGgsnNotifGroupRev2,
                        cGgsnStatusGroupRev1,
                        cGgsnNotifInfoGroupRev1,
                        cGgsnStatusGroupConfigVer,
                        cGgsnConfigurationsGroupR60,
                        cGgsnStatisticsGroupR60,
                        cGgsnStatusGroupR60,
                        cGgsnNotifInfoGroupR60
                    }

    GROUP           cGgsnUmtsGroup
    DESCRIPTION
        "This group is mandatory for a GGSN that supports GTP v1."

    OBJECT          cGgsnHistNotifGgsnIpAddrType
    SYNTAX          INTEGER  {
                        unknown(0),
                        ipv4(1)
                    }
    DESCRIPTION
        "Support for ipv6(2) and dns(16) is not mandatory."

    OBJECT          cGgsnIpDupProtectRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnDefaultAggregRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnAddrRangeRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPdfRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPcscfRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnSlbVserRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."
    ::= { cGgsnMIBCompliances 6 }

cGgsnMIBComplianceRev6 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statements for entities which
        implement the CISCO GGSN MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cGgsnStatisticsGroupRev1,
                        cGgsnNotifMgmtGroupRev1,
                        cGgsnConfigurationsGroupRev2,
                        cGgsnNotifGroupRev2,
                        cGgsnStatusGroupRev1,
                        cGgsnNotifInfoGroupRev1,
                        cGgsnStatusGroupConfigVer,
                        cGgsnStatisticsGroupR60,
                        cGgsnStatusGroupR60,
                        cGgsnConfigurationsGroupR60Rev1
                    }

    GROUP           cGgsnUmtsGroup
    DESCRIPTION
        "This group is mandatory for a GGSN that supports GTP v1."

    OBJECT          cGgsnHistNotifGgsnIpAddrType
    SYNTAX          INTEGER  {
                        unknown(0),
                        ipv4(1)
                    }
    DESCRIPTION
        "Support for ipv6(2) and dns(16) is not mandatory."

    OBJECT          cGgsnIpDupProtectRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnDefaultAggregRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnAddrRangeRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPdfRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPcscfRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnSlbVserRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."
    ::= { cGgsnMIBCompliances 7 }

cGgsnMIBComplianceRev7 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statements for entities which
        implement the CISCO GGSN MIB. This is deprecated by
        cGgsnMIBComplianceRev8."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cGgsnStatisticsGroupRev2,
                        cGgsnNotifMgmtGroupRev2,
                        cGgsnConfigurationsGroupRev3,
                        cGgsnNotifGroupRev3,
                        cGgsnStatusGroupRev1,
                        cGgsnNotifInfoGroupRev2,
                        cGgsnStatusGroupConfigVer,
                        cGgsnStatisticsGroupR60,
                        cGgsnStatusGroupR60,
                        cGgsnNotifInfoGroupR60,
                        cGgsnConfigurationsGroupR60Rev1,
                        cGgsnStatusGroupR70
                    }

    GROUP           cGgsnUmtsGroup
    DESCRIPTION
        "This group is mandatory for a GGSN that supports GTP v1."

    OBJECT          cGgsnHistNotifGgsnIpAddrType
    SYNTAX          INTEGER  {
                        unknown(0),
                        ipv4(1)
                    }
    DESCRIPTION
        "Support for ipv6(2) and dns(16) is not mandatory."

    OBJECT          cGgsnIpDupProtectRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnDefaultAggregRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnAddrRangeRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPcscfRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnSlbVserRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."
    ::= { cGgsnMIBCompliances 8 }

cGgsnMIBComplianceRev8 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statements for entities which
        implement the CISCO GGSN MIB.This is deprecated by
        cGgsnMIBComplianceRev9."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cGgsnStatisticsGroupRev2,
                        cGgsnNotifMgmtGroupRev2,
                        cGgsnConfigurationsGroupRev4,
                        cGgsnNotifGroupRev3,
                        cGgsnStatusGroupRev1,
                        cGgsnNotifInfoGroupRev2,
                        cGgsnStatusGroupConfigVer,
                        cGgsnStatisticsGroupR60,
                        cGgsnStatusGroupR60,
                        cGgsnNotifInfoGroupR60,
                        cGgsnConfigurationsGroupR60Rev1,
                        cGgsnStatusGroupR70
                    }
    ::= { cGgsnMIBCompliances 9 }

cGgsnMIBComplianceRev9 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statements for entities which
        implement the CISCO GGSN MIB.This is deprecated by
        cGgsnMIBComplianceRev10."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cGgsnStatisticsGroupRev2,
                        cGgsnNotifMgmtGroupRev2,
                        cGgsnConfigurationsGroupRev4,
                        cGgsnNotifGroupRev3,
                        cGgsnStatusGroupRev1,
                        cGgsnNotifInfoGroupRev2,
                        cGgsnStatusGroupConfigVer,
                        cGgsnStatisticsGroupR60,
                        cGgsnStatusGroupR60,
                        cGgsnNotifInfoGroupR60,
                        cGgsnConfigurationsGroupR60Rev1,
                        cGgsnStatusGroupR70,
                        cGgsnStatusGroupR90
                    }

    GROUP           cGgsnUmtsGroup
    DESCRIPTION
        "This group is mandatory for a GGSN that supports GTP v1."

    OBJECT          cGgsnHistNotifGgsnIpAddrType
    SYNTAX          INTEGER  {
                        unknown(0),
                        ipv4(1)
                    }
    DESCRIPTION
        "Support for ipv6(2) and dns(16) is not mandatory."

    OBJECT          cGgsnIpDupProtectRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnDefaultAggregRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnAddrRangeRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPcscfRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnSlbVserRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."
    ::= { cGgsnMIBCompliances 10 }

cGgsnMIBComplianceRev10 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statements for entities which
        implement the CISCO GGSN MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cGgsnStatisticsGroupRev2,
                        cGgsnNotifMgmtGroupRev2,
                        cGgsnConfigurationsGroupRev4,
                        cGgsnNotifGroupRev3,
                        cGgsnStatusGroupRev1,
                        cGgsnNotifInfoGroupRev2,
                        cGgsnStatusGroupConfigVer,
                        cGgsnStatisticsGroupR60,
                        cGgsnStatusGroupR60,
                        cGgsnNotifInfoGroupR60,
                        cGgsnConfigurationsGroupR60Rev1,
                        cGgsnStatusGroupR70,
                        cGgsnStatusGroupR90,
                        cGgsnConfigurationsGroupSup1
                    }

    GROUP           cGgsnUmtsGroup
    DESCRIPTION
        "This group is mandatory for a GGSN that supports GTP v1."

    OBJECT          cGgsnHistNotifGgsnIpAddrType
    SYNTAX          INTEGER  {
                        unknown(0),
                        ipv4(1)
                    }
    DESCRIPTION
        "Support for ipv6(2) and dns(16) is not mandatory."

    OBJECT          cGgsnIpDupProtectRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnDefaultAggregRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnAddrRangeRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPcscfRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnPlmnRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."

    OBJECT          cGgsnSlbVserRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "The states notInService(2), notReady(3) and
        createAndWait(5) need not be supported."
    ::= { cGgsnMIBCompliances 11 }

-- units of conformance

cGgsnStatisticsGroup OBJECT-GROUP
    OBJECTS         {
                        cGgsnSentSigMessages,
                        cGgsnReceivedSigMessages,
                        cGgsnUnexpectedSigMessages,
                        cGgsnSentGPDUs,
                        cGgsnReceivedGPDUs,
                        cGgsnSentGPDUOctets,
                        cGgsnReceivedGPDUOctets,
                        cGgsnUnexpectedGPDUs,
                        cGgsnActivationRejectedPdps,
                        cGgsnOutOfResourcePdps,
                        cGgsnParserErrorMessages,
                        cGgsnTotalCreatedPdps,
                        cGgsnTotalDeletedPdps,
                        cGgsnTotalNetworkInitPdps,
                        cGgsnTotalPppPdpsCreated,
                        cGgsnTotalPppPdpsDeleted,
                        cGgsnOutOfResourcePppRegenPdps,
                        cGgsnDroppedPppRegenPdps
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of statistics on GGSN."
    ::= { cGgsnMIBGroups 1 }

cGgsnNotifMgmtGroup OBJECT-GROUP
    OBJECTS         {
                        cGgsnNotifEnabled,
                        cGgsnNotifLeastSeverLevel,
                        cGgsnGeneratedNotifs,
                        cGgsnIgnoredAlarms,
                        cGgsnHistNotifMaxLength,
                        cGgsnHistNotifLatestIndex,
                        cGgsnHistNotifType,
                        cGgsnHistNotifSeverity,
                        cGgsnHistNotifTimestamp,
                        cGgsnHistNotifGgsnIpAddrType,
                        cGgsnHistNotifGgsnIpAddr,
                        cGgsnHistNotifInfo
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects related with notification
        management on GGSN."
    ::= { cGgsnMIBGroups 2 }

cGgsnConfigurationsGroup OBJECT-GROUP
    OBJECTS         {
                        cGgsnDefaultIpAllocationMethod,
                        cGgsnIdlePdpPurgeTimer,
                        cGgsnIpDupProtectRowStatus,
                        cGgsnDefaultAggregRowStatus,
                        cGgsnDefaultAaaAuthServerGroup,
                        cGgsnDefaultAaaAccServerGroup,
                        cGgsnPppVirtualTemplate,
                        cGgsnPppRegenVirtualTemplate
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects related with configurations on
        GGSN. This is deprecated by cGgsnConfigurationsGroupRev1."
    ::= { cGgsnMIBGroups 3 }

cGgsnNotifGroup NOTIFICATION-GROUP
   NOTIFICATIONS    { cGgsnNotification }
    STATUS          deprecated
    DESCRIPTION
        "A collection of notifications."
    ::= { cGgsnMIBGroups 4 }

cGgsnStatusGroup OBJECT-GROUP
    OBJECTS         {
                        cGgsnVersion,
                        cGgsnActiveNetworkInitPdps,
                        cGgsnActivePppPdps,
                        cGgsnActivePppRegenPdps,
                        cGgsnPendingPppRegenPdps
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects representing status on GGSN."
    ::= { cGgsnMIBGroups 5 }

cGgsnConfigurationsGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        cGgsnDefaultIpAllocationMethod,
                        cGgsnIdlePdpPurgeTimer,
                        cGgsnIpDupProtectRowStatus,
                        cGgsnDefaultAggregRowStatus,
                        cGgsnDefaultAaaAuthServerGroup,
                        cGgsnDefaultAaaAccServerGroup,
                        cGgsnPppVirtualTemplate,
                        cGgsnPppRegenVirtualTemplate,
                        cGgsnPlmnAddrRangeRowStatus
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects related with configurations on GGSN."
    ::= { cGgsnMIBGroups 6 }

cGgsnUmtsGroup OBJECT-GROUP
    OBJECTS         {
                        cGgsnTftSemanticErrorPdps,
                        cGgsnTftSyntacticErrorPdps,
                        cGgsnPktFilterSemanticErrorPdps,
                        cGgsnPktFilterSyntacticErrorPdps,
                        cGgsnPlmnAddrRangeUsage,
                        cGgsnActiveGtpVersion0Pdps,
                        cGgsnActiveGtpVersion1Pdps,
                        cGgsnGtpEncapInterface
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects pertaining to GTP v1."
    ::= { cGgsnMIBGroups 7 }

cGgsnStatisticsGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        cGgsnSentSigMessages,
                        cGgsnReceivedSigMessages,
                        cGgsnUnexpectedSigMessages,
                        cGgsnSentGPDUs,
                        cGgsnReceivedGPDUs,
                        cGgsnUnexpectedGPDUs,
                        cGgsnActivationRejectedPdps,
                        cGgsnOutOfResourcePdps,
                        cGgsnParserErrorMessages,
                        cGgsnTotalCreatedPdps,
                        cGgsnTotalDeletedPdps,
                        cGgsnTotalNetworkInitPdps,
                        cGgsnTotalPppPdpsCreated,
                        cGgsnTotalPppPdpsDeleted,
                        cGgsnOutOfResourcePppRegenPdps,
                        cGgsnDroppedPppRegenPdps,
                        cGgsnHCSentGPDUOctets,
                        cGgsnHCReceivedGPDUOctets,
                        cGgsnVersionNotSupportedRejPdps,
                        cGgsnUnkownMessageRejPdps,
                        cGgsnMsgTooShortRejPdps,
                        cGgsnMandIeMissingRejPdps,
                        cGgsnMandIeIncorrectRejPdps,
                        cGgsnOptIeInvalidRejPdps,
                        cGgsnIeUnknownRejPdps,
                        cGgsnIeOutOfOrderRejPdps,
                        cGgsnIeUnexpectedRejPdps,
                        cGgsnIeDuplicatedRejPdps,
                        cGgsnOptIeIncorrectRejPdps,
                        cGgsnPdpWithoutTftExistsRejPdps,
                        cGgsnSgsnThruPutLastCollected,
                        cGgsnSgsnUpStreamPktCnt,
                        cGgsnSgsnUpStreamByteCnt,
                        cGgsnSgsnDownStreamPktCnt,
                        cGgsnSgsnDownStreamByteCnt
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of statistics on GGSN. This group is
        deprecated by cGgsnStatisticsGroupRev2."
    ::= { cGgsnMIBGroups 8 }

cGgsnNotifGroupRev1 NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        cGgsnNotification,
                        cGgsnInServiceNotif,
                        cGgsnMaintenanceNotif,
                        cGgsnMemThresholdReachedNotif,
                        cGgsnMemThresholdClearedNotif,
                        cGgsnPdfStateUpNotif,
                        cGgsnPdfStateDownNotif
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of notifications."
    ::= { cGgsnMIBGroups 9 }

cGgsnConfigurationsGroupRev2 OBJECT-GROUP
    OBJECTS         {
                        cGgsnDefaultIpAllocationMethod,
                        cGgsnIdlePdpPurgeTimer,
                        cGgsnIpDupProtectRowStatus,
                        cGgsnDefaultAggregRowStatus,
                        cGgsnDefaultAaaAuthServerGroup,
                        cGgsnDefaultAaaAccServerGroup,
                        cGgsnPppVirtualTemplate,
                        cGgsnPppRegenVirtualTemplate,
                        cGgsnPlmnAddrRangeRowStatus,
                        cGgsnPdfRowStatus,
                        cGgsnPdfReconnectTimeOut,
                        cGgsnPdfReconnectRetries,
                        cGgsnPdfReconExpPdpDelete,
                        cGgsnPdfReqRetryTimeOut,
                        cGgsnPdfReqRetries,
                        cGgsnPcscfRowStatus,
                        cGgsnMemoryThreshold,
                        cGgsnServiceMode,
                        cGgsnPlmnRowStatus,
                        cGgsnPlmnScope,
                        cGgsnSessionTimeout,
                        cGgsnThruputIntervalOne,
                        cGgsnThruputIntervalTwo,
                        cGgsnCompliance3GppGgsn,
                        cGgsnCreateReqV1UpdExistPdp,
                        cGgsnRadAttrSessTimeout,
                        cGgsnDownlinkVerifyMsDisable
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects related with configurations on GGSN.
        This object group is superceded by 
        cGgsnConfigurationsGroupRev3."
    ::= { cGgsnMIBGroups 10 }

cGgsnStatusGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        cGgsnVersion,
                        cGgsnActiveNetworkInitPdps,
                        cGgsnActivePppPdps,
                        cGgsnActivePppRegenPdps,
                        cGgsnPendingPppRegenPdps,
                        cGgsnServiceModeStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects representing status on GGSN."
    ::= { cGgsnMIBGroups 11 }

cGgsnNotifInfoGroup OBJECT-GROUP
    OBJECTS         {
                        cGgsnPdfServerAddrType,
                        cGgsnPdfServerAddr
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects representing Notif Info on GGSN."
    ::= { cGgsnMIBGroups 12 }

cGgsnNotifGroupRev2 NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        cGgsnInServiceNotif,
                        cGgsnMaintenanceNotif,
                        cGgsnMemThresholdReachedNotif,
                        cGgsnMemThresholdClearedNotif,
                        cGgsnPdfStateUpNotif,
                        cGgsnPdfStateDownNotif,
                        cGgsnGlobalErrorNotif,
                        cGgsnAccessPointNameNotif,
                        cGgsnPacketDataProtocolNotif
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of notifications. This object group
        is superceded by cGgsnNotifGroupRev3."
    ::= { cGgsnMIBGroups 13 }

cGgsnNotifInfoGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        cGgsnPdfServerAddrType,
                        cGgsnPdfServerAddr,
                        cGgsnNotifAccessPointName,
                        cGgsnNotifPdpImsi,
                        cGgsnGlobalErrorTypes,
                        cGgsnAccessPointErrorTypes,
                        cGgsnPacketDataProtoErrorTypes
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects representing Notif Info on GGSN.
        This object group is superceded by cGgsnNotifInfoGroupRev2."
    ::= { cGgsnMIBGroups 14 }

cGgsnNotifMgmtGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        cGgsnNotifLeastSeverLevel,
                        cGgsnGeneratedNotifs,
                        cGgsnIgnoredAlarms,
                        cGgsnHistNotifMaxLength,
                        cGgsnHistNotifLatestIndex,
                        cGgsnHistNotifType,
                        cGgsnHistNotifSeverity,
                        cGgsnHistNotifTimestamp,
                        cGgsnHistNotifGgsnIpAddrType,
                        cGgsnHistNotifGgsnIpAddr,
                        cGgsnHistNotifInfo,
                        cGgsnServiceNotifEnabled,
                        cGgsnMemoryNotifEnabled,
                        cGgsnPdfNotifEnabled,
                        cGgsnGlobalErrorNotifEnabled,
                        cGgsnAccessPointNotifEnabled,
                        cGgsnPdpNotifEnabled
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects related with notification
        management on GGSN. This object group is superceded by
        cGgsnNotifMgmtGroupRev2."
    ::= { cGgsnMIBGroups 15 }

cGgsnStatusGroupConfigVer OBJECT-GROUP
    OBJECTS         { cGgsnConfigVersion }
    STATUS          current
    DESCRIPTION
        "A collection of objects representing config version of GGSN."
    ::= { cGgsnMIBGroups 16 }

cGgsnConfigurationsGroupR60 OBJECT-GROUP
    OBJECTS         {
                        cGgsnSlbMode,
                        cGgsnSlbNotif,
                        cGgsnSlbVserRowStatus,
                        cGgsnSlbVserNextHopAddrType,
                        cGgsnSlbVserNextHopAddress,
                        cGgsnSlbVserVrfName
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects representing configurations on GGSN.
        This group is deprecated by cGgsnConfigurationsGroupR60Rev1."
    ::= { cGgsnMIBGroups 17 }

cGgsnStatisticsGroupR60 OBJECT-GROUP
    OBJECTS         {
                        cGgsnTotalMessages,
                        cGgsnContextSetupMessages,
                        cGgsnContextModifyMessages,
                        cGgsnContextRemoveMessages,
                        cGgsnPathSetupMessages,
                        cGgsnPathModifyMessages,
                        cGgsnPathRemoveMessages,
                        cGgsnCGFReadyMessages,
                        cGgsnCGFModifyMessages,
                        cGgsnCGFRemoveMessages,
                        cGgsnInternalStateMsgs,
                        cGgsnSlbCacFailures,
                        cGgsnSlbSessionFailures
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects related with statistics."
    ::= { cGgsnMIBGroups 18 }

cGgsnStatusGroupR60 OBJECT-GROUP
    OBJECTS         {
                        cGgsnPrepaidPDPs,
                        cGgsnPostpaidPDPs
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects related to gtp status."
    ::= { cGgsnMIBGroups 19 }

cGgsnNotifInfoGroupR60 OBJECT-GROUP
    OBJECTS         { cGgsnNotifPdpMsisdn }
    STATUS          current
    DESCRIPTION
        "A collection of objects representing the Notif info on
        GGSN."
    ::= { cGgsnMIBGroups 20 }

cGgsnConfigurationsGroupR60Rev1 OBJECT-GROUP
    OBJECTS         {
                        cGgsnSlbMode,
                        cGgsnSlbVserRowStatus,
                        cGgsnSlbVserNextHopAddrType,
                        cGgsnSlbVserNextHopAddress,
                        cGgsnSlbVserVrfName,
                        cGgsnSlbNotifyCacFailure,
                        cGgsnSlbNotifySessionDeletion
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects representing configurations on GGSN."
    ::= { cGgsnMIBGroups 21 }

cGgsnStatisticsGroupRev2 OBJECT-GROUP
    OBJECTS         {
                        cGgsnSentSigMessages,
                        cGgsnReceivedSigMessages,
                        cGgsnUnexpectedSigMessages,
                        cGgsnSentGPDUs,
                        cGgsnReceivedGPDUs,
                        cGgsnUnexpectedGPDUs,
                        cGgsnActivationRejectedPdps,
                        cGgsnOutOfResourcePdps,
                        cGgsnParserErrorMessages,
                        cGgsnTotalCreatedPdps,
                        cGgsnTotalDeletedPdps,
                        cGgsnTotalNetworkInitPdps,
                        cGgsnTotalPppPdpsCreated,
                        cGgsnTotalPppPdpsDeleted,
                        cGgsnOutOfResourcePppRegenPdps,
                        cGgsnDroppedPppRegenPdps,
                        cGgsnHCSentGPDUOctets,
                        cGgsnHCReceivedGPDUOctets,
                        cGgsnSgsnThruPutLastCollected,
                        cGgsnSgsnUpStreamPktCnt,
                        cGgsnSgsnUpStreamByteCnt,
                        cGgsnSgsnDownStreamPktCnt,
                        cGgsnSgsnDownStreamByteCnt,
                        cGgsnTotalCreatedIpv6Pdps,
                        cGgsnTotalDeletedIpv6Pdps,
                        cGgsnTotalRejectedIpv6Pdps,
                        cGgsnSentIpv6SigMessages,
                        cGgsnReceivedIpv6SigMessages,
                        cGgsnSentIpv6PDUs,
                        cGgsnReceivedIpv6PDUs,
                        cGgsnSentIpv6PDUOctets,
                        cGgsnReceivedIpv6PDUOctets,
                        cGgsnVersionNotSupportedMsgs,
                        cGgsnUnkownGtpMsgs,
                        cGgsnTooShortMsgs,
                        cGgsnMandIeMissingMsgs,
                        cGgsnMandIeIncorrectMsgs,
                        cGgsnOptIeInvalidMsgs,
                        cGgsnIeUnknownMsgs,
                        cGgsnIeOutOfOrderMsgs,
                        cGgsnIeUnexpectedMsgs,
                        cGgsnIeDuplicatedMsgs,
                        cGgsnOptIeIncorrectMsgs,
                        cGgsnPdpWithoutTftExistsPdps
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects related with statistics."
    ::= { cGgsnMIBGroups 22 }

cGgsnStatusGroupR70 OBJECT-GROUP
    OBJECTS         {
                        cGgsnActivatedIpv6Gtpv0Pdp,
                        cGgsnActivatedIpv6Gtpv1Pdp,
                        cGgsnActivatedIpv6Ms
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects related with status."
    ::= { cGgsnMIBGroups 23 }

cGgsnConfigurationsGroupRev3 OBJECT-GROUP
    OBJECTS         {
                        cGgsnDefaultIpAllocationMethod,
                        cGgsnIdlePdpPurgeTimer,
                        cGgsnIpDupProtectRowStatus,
                        cGgsnDefaultAggregRowStatus,
                        cGgsnDefaultAaaAuthServerGroup,
                        cGgsnDefaultAaaAccServerGroup,
                        cGgsnPppVirtualTemplate,
                        cGgsnPppRegenVirtualTemplate,
                        cGgsnPlmnAddrRangeRowStatus,
                        cGgsnPcscfRowStatus,
                        cGgsnMemoryThreshold,
                        cGgsnServiceMode,
                        cGgsnPlmnRowStatus,
                        cGgsnPlmnScope,
                        cGgsnSessionTimeout,
                        cGgsnThruputIntervalOne,
                        cGgsnThruputIntervalTwo,
                        cGgsnCompliance3GppGgsn,
                        cGgsnRadAttrSessTimeout,
                        cGgsnDownlinkVerifyMsDisable
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects related with configurations on GGSN.
        This is deprecated by cGgsnConfigurationsGroupRev4."
    ::= { cGgsnMIBGroups 24 }

cGgsnNotifMgmtGroupRev2 OBJECT-GROUP
    OBJECTS         {
                        cGgsnNotifLeastSeverLevel,
                        cGgsnGeneratedNotifs,
                        cGgsnIgnoredAlarms,
                        cGgsnHistNotifMaxLength,
                        cGgsnHistNotifLatestIndex,
                        cGgsnHistNotifType,
                        cGgsnHistNotifSeverity,
                        cGgsnHistNotifTimestamp,
                        cGgsnHistNotifGgsnIpAddrType,
                        cGgsnHistNotifGgsnIpAddr,
                        cGgsnHistNotifInfo,
                        cGgsnServiceNotifEnabled,
                        cGgsnMemoryNotifEnabled,
                        cGgsnGlobalErrorNotifEnabled,
                        cGgsnAccessPointNotifEnabled,
                        cGgsnPdpNotifEnabled
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects related with notification
        management on GGSN."
    ::= { cGgsnMIBGroups 25 }

cGgsnNotifGroupRev3 NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        cGgsnInServiceNotif,
                        cGgsnMaintenanceNotif,
                        cGgsnMemThresholdReachedNotif,
                        cGgsnMemThresholdClearedNotif,
                        cGgsnGlobalErrorNotif,
                        cGgsnAccessPointNameNotif,
                        cGgsnPacketDataProtocolNotif
                    }
    STATUS          current
    DESCRIPTION
        "A collection of notifications."
    ::= { cGgsnMIBGroups 26 }

cGgsnNotifInfoGroupRev2 OBJECT-GROUP
    OBJECTS         {
                        cGgsnNotifAccessPointName,
                        cGgsnNotifPdpImsi,
                        cGgsnGlobalErrorTypes,
                        cGgsnAccessPointErrorTypes,
                        cGgsnPacketDataProtoErrorTypes
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects representing Notif Info on GGSN."
    ::= { cGgsnMIBGroups 27 }

cGgsnConfigurationsGroupRev4 OBJECT-GROUP
    OBJECTS         {
                        cGgsnDefaultIpAllocationMethod,
                        cGgsnIdlePdpPurgeTimer,
                        cGgsnIpDupProtectRowStatus,
                        cGgsnDefaultAggregRowStatus,
                        cGgsnDefaultAaaAuthServerGroup,
                        cGgsnDefaultAaaAccServerGroup,
                        cGgsnPppVirtualTemplate,
                        cGgsnPppRegenVirtualTemplate,
                        cGgsnPlmnAddrRangeRowStatus,
                        cGgsnPcscfRowStatus,
                        cGgsnMemoryThreshold,
                        cGgsnServiceMode,
                        cGgsnPlmnRowStatus,
                        cGgsnPlmnScope,
                        cGgsnSessionTimeout,
                        cGgsnThruputIntervalOne,
                        cGgsnThruputIntervalTwo,
                        cGgsnRadAttrSessTimeout,
                        cGgsnDownlinkVerifyMsDisable
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects related with configurations on GGSN."
    ::= { cGgsnMIBGroups 28 }

cGgsnStatusGroupR90 OBJECT-GROUP
    OBJECTS         { cGgsnGtpEncapsuInterface }
    STATUS          current
    DESCRIPTION
        "A collection of objects which maintains the mapping
        between CGSN interfaces and gtp encapsulated interfaces."
    ::= { cGgsnMIBGroups 29 }

cGgsnConfigurationsGroupSup1 OBJECT-GROUP
    OBJECTS         {
                        cGgsnMsExcludeRangeStartIpv6Prefixlen,
                        cGgsnMsExcludeRangeEndIpv6Prefixlen,
                        cGgsnPlmnAddrRangeFirstIpv6Prefixlen,
                        cGgsnPlmnAddrRangeLastIpv6Prefixlen
                    }
    STATUS          current
    DESCRIPTION
        "This group is supplementary to cGgsnConfigurationsGroupRev4."
    ::= { cGgsnMIBGroups 30 }

END






















































