-- *****************************************************************
-- IBM DLC Switch MIB definition.
--
-- September 1996, Dennis Ignacio.
--
-- Copyright (c) 1996-1997, 1998 by cisco Systems, Inc.
-- All rights reserved.
-- *****************************************************************
--

CISCO-DLC-SWITCH-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    Integer32
        FROM SNMPv2-SMI
    MacAddress, TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP   
	FROM SNMPv2-CONF
    ifIndex
        FROM RFC1213-MIB
    InterfaceIndexOrZero
	FROM IF-MIB
    ciscoMgmt
        FROM CISCO-SMI
;

ciscoDlcSwitchMIB MODULE-IDENTITY
          LAST-UPDATED "9702190000Z"
          ORGANIZATION "Cisco Systems, Inc."
          CONTACT-INFO
                "       Cisco Systems
                        Customer Service

                Postal: 170 W. Tasman Drive
                        San Jose, CA  95134
                        USA

                   Tel: +1 800 553-NETS

                E-mail: cs-fras@cisco.com"
           DESCRIPTION       
	       "This is the MIB module for objects used to
                manage FRAS sessions to the endstation. 
		These objects are specific to downstream or 
		enduster sessions only. It does not contain 
		objects supported by the FRAS-HOST MIB which 
		are specific to upstream or host-end sessions."

::= { ciscoMgmt 76 }

--
--  The following functionality will be modelled in this MIB module:
--
--     1. Frame-Relay Access Support
--

ciscoDlcSwitchMIBObjects      	OBJECT IDENTIFIER ::= { ciscoDlcSwitchMIB 1}
 

--  THE BNN FORMAT (RFC 1490 Routed Format)
--  ==============
--
--  The following FRAS types of connections are modeled in the BNN 
--  group of this MIB:
--
--     1. SDLC
--     2. LLC (Token-Ring or Ethernet)
--
--
--
--  THE BAN FORMAT (RFC 1490 Bridged Format)
--  ==============
--
--  The following FRAS types of connections are modeled in the BAN
--  group of this MIBi:
--
--     1. SDLC
--     2. LLC (Token-Ring or Ethernet)
--
--  -------------------------------------------------------------

frasBnnSdlc        OBJECT IDENTIFIER ::= { ciscoDlcSwitchMIBObjects 1 }
frasBnnLlc         OBJECT IDENTIFIER ::= { ciscoDlcSwitchMIBObjects 2 }
frasBanSdlc        OBJECT IDENTIFIER ::= { ciscoDlcSwitchMIBObjects 3 }
frasBanLlc         OBJECT IDENTIFIER ::= { ciscoDlcSwitchMIBObjects 4 }

-- **************************************************************
-- *  Textual convention definitions				*
-- **************************************************************

SAP ::= TEXTUAL-CONVENTION
	STATUS	current
	DESCRIPTION
	  "Service Access Point - is a term that denotes the means
	   by which a user entity in layer n+1 accesses a service
	   of a provider entity in layer n."
	SYNTAX	OCTET STRING (SIZE(1))

SdlcAddress ::= TEXTUAL-CONVENTION
        STATUS  current
        DESCRIPTION
          "A hexadecimal address assigned to a secondary
	   poll station of an SDLC device."
        SYNTAX  OCTET STRING (SIZE(1))

--  *************************************************************
--  *                                                           *
--  *   D L C   S W I T C H      F R A S  -  B N N              *
--  *                                                           *
--  *   Boundary Network Node / Routed Format                   *
--  *                                                           *
--  *************************************************************

--  *************************************************************
--  *                                                           *
--  * 	THE FRAS BNN SDLC CONNECTION TABLE			*
--  *                                                           *
--  *************************************************************

frasBnnSdlcConTable         OBJECT-TYPE
                SYNTAX          SEQUENCE OF FrasBnnSdlcConEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION
                       "This table contains mapping information 
			for each SDLC Link Station in a FRAS-BNN
                        to SDLC connection. All entries are derived
			entirely from the router configuration." 
                ::= { frasBnnSdlc  1 }

frasBnnSdlcConEntry         OBJECT-TYPE
                SYNTAX          FrasBnnSdlcConEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION
                       "This table contains the entries defined
                        for a specific SDLC Link Station in a
			BNN-SDLC configuration."
                INDEX   { ifIndex, bnnSdlcConAddress }
                ::= { frasBnnSdlcConTable 1 }
 
FrasBnnSdlcConEntry  ::= SEQUENCE {
                bnnSdlcConAddress          SdlcAddress,
                bnnSdlcConState            INTEGER,
                bnnSdlcConDlci             Integer32,
                bnnSdlcConFRInterface      InterfaceIndexOrZero,
                bnnSdlcConLocalSap         SAP,
                bnnSdlcConRemoteSap        SAP
}
 
bnnSdlcConAddress           OBJECT-TYPE
                SYNTAX          SdlcAddress
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION
                       "This value is the poll address of the
                        secondary link station for this SDLC link.
                        It uniquely identifies the SDLC link station
                        within a single SDLC port."
                ::= { frasBnnSdlcConEntry 1 }
 
bnnSdlcConState             OBJECT-TYPE
                SYNTAX          INTEGER {
                        reset           (1),
                        testSent        (2),
                        xidexchg        (3),
			connrqsent	(4),
			sigstnwait	(5),
			connrspwait	(6),
			connrspsent	(7),
                        contacted       (8),
			discwait	(9)
                }
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Contains the FRAS state of the Link Station.
                         reset - no activity
                         testSent - TEST Frames sent
                         xidexchg - XID exchange in progress
			 connrqsent - Connect request sent
			 sigstnwait - Signal station wait state
			 connrspwait - Connect response wait state
			 connrspsent - Connect response sent
                         contacted - Session established 
			 discwait - Disconnect wait state"
                ::= { frasBnnSdlcConEntry 2 }
 
bnnSdlcConDlci             	OBJECT-TYPE
                SYNTAX          Integer32 (16..1022)
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "The Data Link Connection Identifier used for
                        this particular connection."
                ::= { frasBnnSdlcConEntry 3 }
 
bnnSdlcConFRInterface      	OBJECT-TYPE
                SYNTAX          InterfaceIndexOrZero 
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "This is the Frame-Relay interface which the
                        SDLC Link Station is using to connect to the
                        Host."
                ::= { frasBnnSdlcConEntry 4 }
 
bnnSdlcConLocalSap 		OBJECT-TYPE
                SYNTAX          SAP
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "The Local SAP for this SDLC station's
                       	corresponding LLC session to the host."
                ::= { frasBnnSdlcConEntry 5 }
 
bnnSdlcConRemoteSap         OBJECT-TYPE
                SYNTAX          SAP
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "The Remote SAP for this SDLC station's
                        corresponding LLC session to the host."
                ::= { frasBnnSdlcConEntry 6 }
 


--  *************************************************************
--  *                                                           *
--  *	THE FRAS BNN LLC2 CONNECTION  TABLE       		*
--  *                                                           *
--  *************************************************************

frasBnnLlcConTable      	OBJECT-TYPE
                SYNTAX          SEQUENCE OF FrasBnnLlcConEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION
                       "This table contains information for
                        each End Station in a FRAS-BNN to 
			LLC connection. The entries are derived
			entirely from the router configuration."
                ::= { frasBnnLlc 1 }

frasBnnLlcConEntry		OBJECT-TYPE
                SYNTAX          FrasBnnLlcConEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION
                        "This table contains information for
			a specific End Station's connection
			state in a BNN-LLC connection."
                INDEX   { ifIndex, 
				bnnLlcConDeviceMacAddress,
				bnnLlcConLanLocalSap,
				bnnLlcConLanRemoteSap }
                ::= { frasBnnLlcConTable 1 }

FrasBnnLlcConEntry  ::= SEQUENCE {
		bnnLlcConDeviceMacAddress	MacAddress,
		bnnLlcConLanLocalSap    	SAP,
		bnnLlcConLanRemoteSap		SAP,
		bnnLlcConLanInterface		InterfaceIndexOrZero,
		bnnLlcConDlci			Integer32,
                bnnLlcConState          	INTEGER,
		bnnLlcConLocalMacAddress	MacAddress,
		bnnLlcConFrLocalSap		SAP,
		bnnLlcConFrRemoteSap		SAP
}

bnnLlcConDeviceMacAddress   	OBJECT-TYPE
                SYNTAX          MacAddress
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION
                       "This value is the End Station's Local
                       	Mac-Address."
                ::= { frasBnnLlcConEntry 1 }

bnnLlcConLanLocalSap        	OBJECT-TYPE
                SYNTAX          SAP
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION
                        "The End Station's Local SAP."
                ::= { frasBnnLlcConEntry 2 }

bnnLlcConLanRemoteSap       	OBJECT-TYPE
                SYNTAX          SAP
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION
                        "The End Station's Remote SAP."
                ::= { frasBnnLlcConEntry 3 }

bnnLlcConLanInterface       	OBJECT-TYPE
                SYNTAX          InterfaceIndexOrZero
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "This is the physical interace which the
                        End Station is attached to."
                ::= { frasBnnLlcConEntry 4 }

bnnLlcConDlci               	OBJECT-TYPE
                SYNTAX          Integer32 (16..1022)
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "The Data Link Connection Identifier
                        associated with the corresponding
                        LLC2 session over Frame-Relay to the host."
                ::= { frasBnnLlcConEntry 5 }

bnnLlcConState              	OBJECT-TYPE
                SYNTAX          INTEGER {
                        reset           (1),
                        testSent        (2),
                        xidexchg        (3),
                        connrqsent      (4),
                        sigstnwait      (5),
                        connrspwait     (6),
                        connrspsent     (7),
                        contacted       (8),
                        discwait        (9)              
                }
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "Contains the FRAS state of the Link Station.
            		reset - no activity
                        testSent - TEST Frames sent
                        xidexchg - XID exchange in progress
                        connrqsent - Connect request sent
                        sigstnwait - Signal station wait state
                        connrspwait - Connect response wait state
                        connrspsent - Connect response sent
                        contacted - Session established
                        discwait - Disconnect wait state"
                ::= { frasBnnLlcConEntry 6 }

bnnLlcConLocalMacAddress    	OBJECT-TYPE
                SYNTAX          MacAddress
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "The Mac-Address configured as the End Station's
               		target or Remote address."
                ::= { frasBnnLlcConEntry 7 }

bnnLlcConFrLocalSap         	OBJECT-TYPE
                SYNTAX          SAP
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "The FRAS router's Local SAP."
                ::= { frasBnnLlcConEntry 8 }

bnnLlcConFrRemoteSap        	OBJECT-TYPE
                SYNTAX          SAP
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "The FRAS router's Remote SAP."
                ::= { frasBnnLlcConEntry 9 }


--  *************************************************************
--  *                                                           *
--  *   D L C   S W I T C H      F R A S  -  B A N              *
--  *								*
--  *   Boundary Access Node / 802.5 Bridged Format		*
--  *                                                           *
--  *************************************************************

--  *************************************************************
--  *                                                           *
--  *	THE FRAS BAN SDLC CONNECTION TABLE			*
--  *                                                           *
--  *************************************************************

frasBanSdlcConTable      	OBJECT-TYPE
                SYNTAX          SEQUENCE OF FrasBanSdlcConEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION
                       "This table contains information for
                        each SDLC Link Station in a FRAS-BAN
                        to SDLC connection. The entries are
			derived entirely from the router 
			configuration."
                ::= { frasBanSdlc 1 }

frasBanSdlcConEntry		OBJECT-TYPE
		SYNTAX		FrasBanSdlcConEntry
		MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION
                       "This table contains information for
                     	a specific SDLC Link Station in a
			configured for a BAN connection."
		INDEX	{ ifIndex, 
			  banSdlcConAddress,
			  banSdlcConBanDlciMac }
                ::= { frasBanSdlcConTable 1 }

FrasBanSdlcConEntry  ::= SEQUENCE {
		banSdlcConLocalInterface	InterfaceIndexOrZero,
                banSdlcConAddress 		SdlcAddress,
		banSdlcConBanDlciMac		MacAddress,
		banSdlcConDlci			Integer32,
		banSdlcConState			INTEGER,
		banSdlcConVmac			MacAddress,
		banSdlcConBniAddress		MacAddress,
		banSdlcConFrLocalSap		SAP,
		banSdlcConFrRemoteSap		SAP
}

banSdlcConLocalInterface	OBJECT-TYPE
                SYNTAX          InterfaceIndexOrZero
		MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
		       "This is the physical interface the
			SDLC Link Stations are connected to."
		::= { frasBanSdlcConEntry 1 }

banSdlcConAddress		OBJECT-TYPE
		SYNTAX          SdlcAddress
                MAX-ACCESS      read-only
                STATUS          current
		DESCRIPTION
                       "This value is the poll address of the
                        secondary link station for this SDLC link.
                        It uniquely identifies the SDLC link station
                        within a single SDLC port."
		::= { frasBanSdlcConEntry 2 }


banSdlcConBanDlciMac		OBJECT-TYPE
		SYNTAX		MacAddress
		MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "The End Station's target or Remote
			mac-address."
		::= { frasBanSdlcConEntry 3 }

banSdlcConDlci		OBJECT-TYPE
		SYNTAX      	Integer32 (16..1022)
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
		       "The Data Link Connection Identifier
			for the corresponding LLC2 session	
			over Frame-Relay to the host."
		::= { frasBanSdlcConEntry 4 }

banSdlcConState  		OBJECT-TYPE
                SYNTAX          INTEGER {
                        reset           (1),
                        testSent        (2),
                        xidexchg        (3),
                        connrqsent      (4),
                        sigstnwait      (5),
                        connrspwait     (6),
                        connrspsent     (7),
                        contacted       (8),
                        discwait        (9)
                }
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Contains the FRAS state of the Link Station.
                         reset - no activity
                         testSent- TEST Frames sent
                         xidexchg - XID exchange in progress
			 connrqsent - Connect request sent
                         sigstnwait - Signal station wait state
                         connrspwait - Connect response wait state
                         connrspsent - Connect response sent
                         contacted - Session established
                         discwait - Disconnect wait state"
                ::= { frasBanSdlcConEntry 5 }

banSdlcConVmac			OBJECT-TYPE
                SYNTAX          MacAddress
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "The End Station's virtual Mac-Address
                        which is comprised of a TR formatted
			template and the SDLC Link Station
			address appended on the last nibble."
                ::= { frasBanSdlcConEntry 6 }

banSdlcConBniAddress		OBJECT-TYPE
		SYNTAX          MacAddress
		MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "BNI is Boundary Node Identifier which is
			the FRAS-BAN connection's Remote address
			in TR-format. It is by default 4fff.0000.0000"
                ::= { frasBanSdlcConEntry 7 }

banSdlcConFrLocalSap    	OBJECT-TYPE
                SYNTAX          SAP
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "The FRAS router's Local SAP."
                ::= { frasBanSdlcConEntry 8 }

banSdlcConFrRemoteSap          	OBJECT-TYPE
                SYNTAX          SAP
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "The FRAS router's Remote SAP."
                ::= { frasBanSdlcConEntry 9 }


--  *************************************************************
--  *                                                           *
--  *   THE FRAS BAN LLC2 CONNECTION  TABLE          		*
--  *                                                           *
--  *************************************************************

frasBanLlcConTable          	OBJECT-TYPE
                SYNTAX          SEQUENCE OF FrasBanLlcConEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION
                       "This table contains information for each
                        LAN attached End Station in a FRAS-BAN
                        to LAN connection. The entries are from
			endstations which have their destination
			mac-addresses as the BAN-DLCI-MAC address."
                ::= { frasBanLlc 1 }
 
frasBanLlcConEntry  	OBJECT-TYPE
                SYNTAX          FrasBanLlcConEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION
                       "This table contains information for a
                       	specific LAN attached End Station."
                INDEX   { banLlcEndstnLocalMac,
			  banLlcConLocalSap,
			  banLlcConRemoteSap,
			  banLlcBanDlciMac }
                ::= { frasBanLlcConTable 1 }
 
FrasBanLlcConEntry  ::= SEQUENCE {
                banLlcEndstnLocalMac        	MacAddress,
                banLlcBanDlciMac            	MacAddress,
		banLlcConLocalSap		SAP,
		banLlcConRemoteSap		SAP,
                banLlcConDlci               	Integer32,
                banLlcConState              	INTEGER,
                banLlcConFrInterface        	InterfaceIndexOrZero,
                banLlcBniAddress            	MacAddress,
		banLlcConFrLocalSap		SAP,
		banLlcConFrRemoteSap		SAP
}

 
banLlcEndstnLocalMac        OBJECT-TYPE
                SYNTAX          MacAddress
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "This value is the End Station's Local
                        Mac-Address."
                ::= { frasBanLlcConEntry 1 }

banLlcBanDlciMac            OBJECT-TYPE
                SYNTAX          MacAddress
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "This value is the End Station's Remote
                        Mac-Address. It is also the FRAS-BAN connection's
                        Local Mac-Address."
                ::= { frasBanLlcConEntry 2 }

banLlcConLocalSap		OBJECT-TYPE
                SYNTAX          SAP
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "The endstation's Local SAP."
                ::= { frasBanLlcConEntry 3 }

banLlcConRemoteSap		OBJECT-TYPE
                SYNTAX          SAP
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "The endstation's Remote SAP."
                ::= { frasBanLlcConEntry 4 }

banLlcConDlci               	OBJECT-TYPE
                SYNTAX          Integer32 (16..1022)
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "The Data Link Connection Identifier
                        associated with the corresponding LLC2
                        session over Frame-Relay to the host."
                ::= { frasBanLlcConEntry 5 }

banLlcConState              OBJECT-TYPE
                SYNTAX          INTEGER {
                        reset           (1),
                        testSent        (2),
                        xidexchg        (3),
			connrqsent      (4),
                        sigstnwait      (5),
                        connrspwait     (6),
                        connrspsent     (7),
                        contacted       (8),
                        discwait        (9)
                }
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "Contains the FRAS state of the Link Station.
                        reset - no activity
                        testSent- TEST Frames sent
                        xidexchg - XID exchange in progress
			connrqsent - Connect request sent
                        sigstnwait - Signal station wait state
                        connrspwait - Connect response wait state
                        connrspsent - Connect response sent
                        contacted - Session established
                        discwait - Disconnect wait state"
                ::= { frasBanLlcConEntry 6 }

banLlcConFrInterface        OBJECT-TYPE
                SYNTAX          InterfaceIndexOrZero
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "This is the Frame-Relay interface
                        for this particular session."
                ::= { frasBanLlcConEntry 7 }
 
banLlcBniAddress            OBJECT-TYPE
                SYNTAX          MacAddress
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "This value is the FRAS-BAN connection's Target
                        Mac-Address. It is by default 4fff.0000.0000"
                ::= { frasBanLlcConEntry 8 }

banLlcConFrLocalSap             OBJECT-TYPE
                SYNTAX          SAP
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                      "The Local SAP of the corresponding LLC2
                        session over Frame-Relay to the host."
                ::= { frasBanLlcConEntry 9 }

banLlcConFrRemoteSap            OBJECT-TYPE
                SYNTAX          SAP
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                       "The Remote SAP of the corresponding LLC2
                        session over Frame-Relay to the host."
                ::= { frasBanLlcConEntry 10 }



-- **********************************************************************
-- * CONFORMANCE INFORMATION						*
-- **********************************************************************
ciscoDlcSwitchConformance	OBJECT IDENTIFIER ::= { ciscoDlcSwitchMIB 2 }
ciscoDlcSwitchCompliances	OBJECT IDENTIFIER ::= { ciscoDlcSwitchConformance 1 }
ciscoDlcSwitchGroups		OBJECT IDENTIFIER ::= { ciscoDlcSwitchConformance 2 }



-- 
--  COMPLIANCE STATEMENTS						
-- 


ciscoDlcSwitchCoreCompliance	MODULE-COMPLIANCE
	STATUS 	current
	DESCRIPTION
	  "The core compliance statement for all FRAS connections."
	MODULE
	   MANDATORY-GROUPS	{
		frasBnnSdlcGroup,
		frasBnnLlcGroup,   
		frasBanSdlcGroup, 
		frasBanLlcGroup
	    }

	::= { ciscoDlcSwitchCompliances 1 }


--
-- Core Conformance Groups for All Connection Components
--

frasBnnSdlcGroup OBJECT-GROUP
    OBJECTS  {
	bnnSdlcConState,
	bnnSdlcConDlci,
	bnnSdlcConFRInterface,
	bnnSdlcConLocalSap,
	bnnSdlcConRemoteSap
    }
    STATUS current
    DESCRIPTION	
       "The frasBnnSdlcGroup defines objects
        which are common to the BNN SDLC of all
        compliant connections."
    ::= { ciscoDlcSwitchGroups 1 }


frasBnnLlcGroup OBJECT-GROUP
    OBJECTS  {	
	bnnLlcConLanInterface,
	bnnLlcConDlci,	
	bnnLlcConState,
	bnnLlcConLocalMacAddress,
	bnnLlcConFrLocalSap,
	bnnLlcConFrRemoteSap
    }
    STATUS current
    DESCRIPTION
       "The frasBnnLlcGroup defines objects
        which are common to the BNN LLC of all
        compliant connections."
    ::= { ciscoDlcSwitchGroups 2 }


frasBanSdlcGroup OBJECT-GROUP
    OBJECTS  {
	banSdlcConLocalInterface,
	banSdlcConAddress,
	banSdlcConBanDlciMac,
	banSdlcConDlci,
	banSdlcConState,
	banSdlcConVmac,
	banSdlcConBniAddress,
	banSdlcConFrLocalSap,
	banSdlcConFrRemoteSap
    }
    STATUS current
    DESCRIPTION
       "The frasBanSdlcGroup defines objects
        which are common to the BAN SDLC of all
        compliant connections."
    ::= { ciscoDlcSwitchGroups 3 }


frasBanLlcGroup OBJECT-GROUP
    OBJECTS  {
	banLlcEndstnLocalMac,
	banLlcBanDlciMac,
	banLlcConDlci,
	banLlcConLocalSap,
	banLlcConRemoteSap,
	banLlcConState,
	banLlcConFrInterface,
	banLlcBniAddress,
	banLlcConFrLocalSap,
	banLlcConFrRemoteSap
    }
    STATUS current
    DESCRIPTION
       "The frasBanLlcGroup defines objects
        which are common to the BAN LLC of all
        compliant connections."
    ::= { ciscoDlcSwitchGroups 4 }


END





