-- ********************************************************************
-- CISCO-XGCP-MIB
--
-- Media Gateway Control Protocol Management Information Base
--
-- August 2002, Margaret Hsieh
--
-- Copyright (c) 2002-2006 by Cisco Systems, Inc.
-- All rights reserved.
-- *********************************************************************

CISCO-XGCP-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, Counter32,
    Unsigned32
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, TruthValue         
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP   
        FROM SNMPv2-CONF
    InetAddress, InetAddressType
        FROM INET-ADDRESS-MIB
    cmgwIndex, CCallControlProfileIndexOrZero 
        FROM CISCO-MEDIA-GATEWAY-MIB
    CMgcGroupIndexOrZero
       FROM CISCO-MGC-MIB
    CiscoPort
        FROM CISCO-TC
    ciscoMgmt
        FROM CISCO-SMI
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB;


ciscoXgcpMIB MODULE-IDENTITY
    LAST-UPDATED "200602210000Z"
    ORGANIZATION "Cisco Systems, Inc."
    CONTACT-INFO
        "        Cisco Systems
                 Customer Service
         Postal: 170 W Tasman Drive
                 San Jose, CA 95134
                 USA
            Tel: +1 800 553-NETS
         E-mail: cs-voice-gateway@cisco.com"
 
    DESCRIPTION
        "This MIB is an enhancement for existing XGCP-MIB.

         xGCP is a set of protocols, for example SGCP (Simple
         Gateway Control Protocol) and MGCP (Media Gateway
         Control Protocol), which are designed as a control 
         protocol within a distributed system that appears  
         to the outside as a single VoIP/VoATM gateway. 
         This system is composed of a call agent (or MGC,
         Media Gateway Controller) and of a set of  
         'media gateways' that perform the conversion of media   
         signals between circuits and packets.  
         In the xGCP model, the gateways focus on the audio signal 
         translation function, while the call agent handles the  
         signaling and call processing functions.

         Examples of Gateway Control Protocols are:
           * Simple Gateway Control Protocol (SGCP)
           * Media Gateway Control Protocol (MGCP)

         xGCP assumes a connection model where the basic constructs are:

           Endpoints   : sources or sinks of data that could be physical
                         or virtual.

           Connections : an association between two or more endpoints 
                         with the purpose of transmitting data between 
                         these endpoints. 
                         Once this association is established for both
                         endpoints, data transfer between these 
                         endpoints can take place. 

         Connections are grouped in calls. One or more connections 
         can belong to one call. Connections and calls are set up at 
         the initiative of one or several call agents.

         Terminologies used:
        
         AAL    : ATM Adaptation Layer
         AUCX   : Audit Connection Command used by the MGC to find out  
                  the status of a given gateway connection.
         AUEP   : Audit Endpoint Command used by the MGC to find out the 
                  status of a given endpoint.
         CCAPI  : Call Control Application Program Interface.
         CID    : Channel Identifier
         CRCX   : Connection Command from a MGC to request the 
                  gateway
         MG     : Media Gateway
         MGC    : Media Gateway Controller
         DLCX   : Delete Command. This command can be initiated by 
                  either the MGC or gateway.
         GSM    : Global System for Mobile Communications
         GW     : Gateway.
         HP     : Hairpin
         MDCX   : Modify Connection Command from a MGC to request the 
                  gateway
         NSE    : Negative Stuffing Event 
         NTFY   : A Notify Command sent from a gateway to a MGC in  
                  response to a RQNT command.
         PSTN   : Public Switched Telephone Network
         RQNT   : Request To Nofity Command from a MGC to request the 
                  gateway to provide a notification for configuration 
                  changes.
         RSIP   : Restart in Progress Command.  This command can be 
                  initiated by either the MGC or gateway.
         SPRT   : Simple Packet Relay Transport
         SSE    : Silicon Switching Engine
         TDM    : Time Division Multiplexing
         TGW    : Target Gateway
         TWC    : Three Way Calling
         VCCI   : Virtual Circuit Connection Identifier
         VMG    : Virtual Media Gateway. It is a logical representation of
                  a module (or a set of modules) that has MG functionality.
                  There could be multiple VMGs in a device.
         VoAAL2 : Voice over AAL2"
 
    REVISION    "200602210000Z"
    DESCRIPTION
        "Added 7 new MGCP Packages to cXgcpMediaGwTable."

    REVISION    "200512210000Z"
    DESCRIPTION
        "Sanitized the whole MIB."

    REVISION    "200508240000Z"
    DESCRIPTION
        "[1] Added table for Media Gateway statistics regarding
             Received and transmitted network messages.
         [2] Added table for active connections that are controlled
             by the Media Gateway."

    REVISION    "200508090000Z"
    DESCRIPTION
        "Added cXgcpMediaGwAnnexabSdpEnabled to cXgcpMediaGwTable."

    REVISION    "200503070000Z"
    DESCRIPTION
        "Added the following objects to cXgcpMediaGwTable
             cXgcpMediaGwLongDurTimer,
             cXgcpMediaGwProfile
        "

    REVISION    "200411150000Z"
    DESCRIPTION
        "Added the following objects to cXgcpMediaGwTable
             cXgcpMediaGwConfiguredPackages,
             cXgcpMediaGwConnOosRsipBehavior
        "
        
    REVISION    "200408300000Z"
    DESCRIPTION
        "[1] Added the value resetTimerForEndpoint to
             CXgcpRetryMethod textual convention. 
         [2] Widened the range of cXgcpMediaGwMaxExpTimeout.
         [3] Added cXgcpMediaGwCaleaEnabled to cXgcpMediaGwTable.
        "
        
    REVISION      "200405140000Z"
    DESCRIPTION
        "Added the following objects:
             cXgcpMediaGwLastFailMgcAddrType,
             cXgcpMediaGwLastFailMgcAddr,
             cXgcpMediaGwDtmfRelay
        "

    REVISION      "200302030000Z"
    DESCRIPTION
        "Initial version of this MIB module."

    ::= { ciscoMgmt 318 }


cXgcpNotifications          OBJECT IDENTIFIER ::= { ciscoXgcpMIB 0 }
cXgcpObjects                OBJECT IDENTIFIER ::= { ciscoXgcpMIB 1 }

cXgcpMgcCfg                 OBJECT IDENTIFIER ::= { cXgcpObjects 1 }
cXgcpMediaGw                OBJECT IDENTIFIER ::= { cXgcpObjects 2 }
cXgcpStats                  OBJECT IDENTIFIER ::= { cXgcpObjects 3 }
cXgcpConnection             OBJECT IDENTIFIER ::= { cXgcpObjects 4 }

--*********************************************************************
--
-- Textual Conventions
--
--*********************************************************************

CXgcpRetryMethod ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Method of resetting retry timer in XGCP.

         When media gateway re-try to communication to a call agent,
         the timeout for each re-try is doubled.
     
         Example: 
               re-try time is 3
               initial timeout is 2 (any unit)
               maximum possible retry time is 256
               MGC group has 2 MGC and each MGC has two IP address

           timeout for neverResetTimer will be as:
               MGC 1 IP11: 2 4 8
               MGC 1 IP12: 16 32 64
               MGC 2 IP21: 128 256 512
               MGC 1 IP22: 1024 2048 4096

           timeout for resetTimerForNewMgc will be as:
               MGC 1 IP11: 2 4 8
               MGC 1 IP12: 16 32 64
               MGC 2 IP21: 2 4 8
               MGC 1 IP22: 16 32 64

           timeout for resetTimerForNewAddr will be as:
               MGC 1 IP11: 2 4 8
               MGC 1 IP12: 2 4 8
               MGC 2 IP21: 2 4 8
               MGC 1 IP22: 2 4 8              

           timeout for resetTimerForEndpoint will be as:
               MGC 1 IP11: 2 4 8
               MGC 1 IP12: 16 32 64 
               MGC 2 IP21: 128 256 256 
               MGC 1 IP22: 256 256 256    
        "
    SYNTAX     INTEGER {
                  neverResetTimer (1),
                  resetTimerForNewMgc (2),
                  resetTimerForNewAddr (3),
                  resetTimerForEndpoint (4)
               }

--
--  MGC Call Events Textual Convention
--
CXgcpCallEvent ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Represents possible Gateway Control Protocol Call Events.
         ack               - Acknowledgement msg
         createConn        - Create connection msg
         deleteConn        - Delete connection msg
         modifyConn        - Modify connection msg
         notifyReq         - Notify request msg
         alert             - CCAPI alert event
         callConnect       - CCAPI call connect event
         confReady         - CCAPI conference ready 
         confDestroy       - CCAPI conference destroyed
         callDisconnect    - CCAPI call disconnect
         callProceed       - CCAPI call proceeding
         offHook           - CCAPI off-hook/call setup ind
         onHook            - CCAPI on-hook/call disconnected
         mediaEvent        - Media Events
         intEven           - Internal Events
         dissocConf        - Dissociate Conf
         assocConf         - Associate Conf
         modifyDone        - CCAPI Call modify done event
         voiceModeDone     - Voice Cut-thru has happened
         nse               - CCAPI NSE events
         callHandoff       - Handoff Call to some other app
         babblerAuditResp  - CCAPI babbler audit response
         "
    SYNTAX      INTEGER {
         ack               (0),
         createConn        (1),
         deleteConn        (2),
         modifyConn        (3),
         notifyReq         (4),
         alert             (5),
         callConnect       (6),
         confReady         (7),
         confDestroy       (8),
         callDisconnect    (9),
         callProceed       (10),
         offHook           (11),
         onHook            (12),
         mediaEvent        (13),
         intEven           (14),
         dissocConf        (15),
         assocConf         (16),
         modifyDone        (17),
         voiceModeDone     (18),
         nse               (19),
         callHandoff       (20),
         babblerAuditResp  (21)
    }

-- *****************************************************************
-- The XGCP MGC Table 
-- *****************************************************************
cXgcpMgcConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CXgcpMgcConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This is a table which is used to provision a MGC or MGC
         group for a MG. Each entry corresponds to a MGC or a 
         MGC group for a single MG.
        "
    ::= { cXgcpMgcCfg 1 }

cXgcpMgcConfigEntry OBJECT-TYPE
    SYNTAX          CXgcpMgcConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each row corresponds to a MGC or a group of MGCs for a media 
         gateway."
    INDEX   { cmgwIndex }
    ::= { cXgcpMgcConfigTable 1 }

CXgcpMgcConfigEntry ::= SEQUENCE {
    cXgcpMgcConfigMgcGrpNum       CMgcGroupIndexOrZero,
    cXgcpMgcConfigAddrType        InetAddressType,
    cXgcpMgcConfigAddress         InetAddress,
    cXgcpMgcConfigProtocolIndex   Integer32,
    cXgcpMgcConfigGatewayUdpPort  CiscoPort
}

cXgcpMgcConfigMgcGrpNum OBJECT-TYPE
    SYNTAX              CMgcGroupIndexOrZero 
    MAX-ACCESS          read-write
    STATUS              current
    DESCRIPTION
        "This object specifies which MGC Redundant Group 
         will be used in XGCP. 
         The value of this object refers to the object cMgcGrpIndex
         from MGC Redundant Group Table, cMgcGrpParamTable.

         There are two conditions to associate a MGC group:
         1. At least one MGC is associated with the MGC group
         2. At least one protocol is associated with the MGC 
            group

         If the value of the object is non-zero, it means
         the media gateway has a MGC Redundant Group.
         In the call setup, the parameters of call agents
         within the MGC Redundant Group will be sequentially
         tried according to its preference.

         This object cXgcpMgcConfigMgcGrpNum and object
         cXgcpMgcConfigAddress are mutually exclusive.
         The object cXgcpMgcConfigAddress can be set only when
         the object cXgcpMgcConfigMgcGrpNum is equal to 0.

         If the value of the object is 0, which means there is
         no MGC Redundant Group associated with the media gateway. 
         It has only one call agent (in media gateway level) to 
         communicate with. This call agent is indicated by 
         cXgcpMgcConfigAddress and will be used in call setup 
         (if call set-up on media gateway level).  "
    DEFVAL { 0 }
    ::= { cXgcpMgcConfigEntry 1 }

cXgcpMgcConfigAddrType  OBJECT-TYPE
    SYNTAX              InetAddressType
    MAX-ACCESS          read-write
    STATUS              current
    DESCRIPTION
        "This object specifies the address type of the MGC
         (object cXgcpMgcConfigAddress), either ipv4 or ipv6."
    DEFVAL { ipv4 }
    ::= { cXgcpMgcConfigEntry 2 }

cXgcpMgcConfigAddress  OBJECT-TYPE
    SYNTAX             InetAddress
    MAX-ACCESS         read-write
    STATUS             current
    DESCRIPTION
        "This object specifies the address of the MGC
         the gateway used to communicate with in call setup.

         This object cXgcpMgcConfigAddress and object 
         cXgcpMgcConfigMgcGrpNum are mutually exclusive.
         The object cXgcpMgcConfigAddress can be set only when
         the object cXgcpMgcConfigMgcGrpNum is equal to 0.
         Otherwise, the SET will be rejected with error. "
    DEFVAL { '00000000'h }
    ::= { cXgcpMgcConfigEntry 3 }

cXgcpMgcConfigProtocolIndex OBJECT-TYPE
    SYNTAX              Integer32 (1..32)
    MAX-ACCESS          read-write
    STATUS              current
    DESCRIPTION
        "This object specifies which protocol that the MG
         should use to communicate with the MGC when it
         try to set up the call.

         The value of this object is the same as the value of object
         cMediaGwProtocolIndex from protocol table 
         (cMediaGwProtocolTable).

         If the value of cXgcpMgcConfigMgcGrpNum is non-zero, this 
         object will be ignored because the protocol will be 
         determined by the MGC group.

         The initial value is 1, means the system should have at
         least one default protocol between the gateway and the MGC
         created in the cMeidaGwProtocolTable when the system is
         initialized. "
    DEFVAL { 1 }
    ::= { cXgcpMgcConfigEntry 4 }

cXgcpMgcConfigGatewayUdpPort  OBJECT-TYPE
    SYNTAX                    CiscoPort 
    MAX-ACCESS                read-only
    STATUS                    current
    DESCRIPTION
        "The UDP port of the MG which is used to communicate with
         call agent in MGCP."
    REFERENCE
        "RFC2705 - Media Gateway Control Protocol (MGCP)
         version 1.0 : Section 3.6 Transmission over UDP
        "
    DEFVAL { 2427 }
    ::= { cXgcpMgcConfigEntry 5 }

-- *********************************************************************
-- The XGCP Media Gateway 
-- *********************************************************************
cXgcpMediaGwTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CXgcpMediaGwEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table is used to provision xGCP configuration in
         a MG."
    ::= { cXgcpMediaGw 1 }

cXgcpMediaGwEntry OBJECT-TYPE
    SYNTAX          CXgcpMediaGwEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents the xGCP attributes for a media 
         gateway.

         An entry is created when the system detects the XGCP stack 
         at system start-up.
         Accordingly, the existing entry shall be deleted when 
         the system can't locate the XGCP stack at system start-up."
    INDEX   { cmgwIndex }

    ::= { cXgcpMediaGwTable 1 }

CXgcpMediaGwEntry ::= SEQUENCE {
    cXgcpMediaGwRequestTimeOut       Integer32,
    cXgcpMediaGwRequestRetries       Integer32,
    cXgcpMediaGwRequestRetryMethod   CXgcpRetryMethod,
    cXgcpMediaGwMaxExpTimeout        Integer32,
    cXgcpMediaGwRestartMwd           Integer32,
    cXgcpMediaGwRestartDelay         Integer32,
    cXgcpMediaGwDefaultPackage       INTEGER,
    cXgcpMediaGwSupportedPackages    BITS,
    cXgcpMediaGwSimpleSdpEnabled     TruthValue,
    cXgcpMediaGwAckSdpEnabled        TruthValue,
    cXgcpMediaGwUndottedNotation     TruthValue,
    cXgcpMediaGwQuarantineProcess    TruthValue,
    cXgcpMediaGwQuarantineLoop       TruthValue,
    cXgcpMediaGwQuarantinePersist    TruthValue,
    cXgcpMediaGwPiggybackMsg         TruthValue,
    cXgcpMediaGwMaxMsgSize           Integer32,
    cXgcpMediaGwLastFailMgcAddrType  InetAddressType,
    cXgcpMediaGwLastFailMgcAddr      InetAddress,
    cXgcpMediaGwDtmfRelay            TruthValue,
    cXgcpMediaGwCaleaEnabled         TruthValue,
    cXgcpMediaGwConfiguredPackages   BITS,
    cXgcpMediaGwConnOosRsipBehavior  INTEGER,
    cXgcpMediaGwLongDurTimer         Integer32,
    cXgcpMediaGwProfile              CCallControlProfileIndexOrZero,
    cXgcpMediaGwAnnexabSdpEnabled    TruthValue
}

cXgcpMediaGwRequestTimeOut OBJECT-TYPE
    SYNTAX                 Integer32 (1..10000)  
    UNITS                  "milliseconds"
    MAX-ACCESS             read-write
    STATUS                 current
    DESCRIPTION
        "The request timeout is the period that the XGCP protocol 
         waits before retransmitting an unacknowledged message.
         It is the responsibility of the requesting entity to 
         provide suitable timeouts for all outstanding commands, 
         and to retry commands when timeouts exceeded. "
    REFERENCE
        "RFC2705 - Media Gateway Control Protocol (MGCP)
         version 1.0 : 
         Section 3.6.3 Computing retransmission timers"
    DEFVAL { 500 }
    ::= { cXgcpMediaGwEntry 1 }

cXgcpMediaGwRequestRetries  OBJECT-TYPE
    SYNTAX                  Integer32 (0..10)
    UNITS                   "times"
    MAX-ACCESS              read-write
    STATUS                  current
    DESCRIPTION
        "This object specifies the number of retries for a request 
         that exceeds timeout without acknowledge before it tries 
         to connect to another MGC."
    REFERENCE
        "RFC2705 - Media Gateway Control Protocol (MGCP)
         version 1.0 : 
         Section 2.1.4 Names of Call Agents and other entities"
    DEFVAL { 3 }
    ::= { cXgcpMediaGwEntry 2 }

cXgcpMediaGwRequestRetryMethod OBJECT-TYPE
    SYNTAX                     CXgcpRetryMethod 
    MAX-ACCESS                 read-write
    STATUS                     current
    DESCRIPTION
        "This object specifies command retry method."
    ::= { cXgcpMediaGwEntry 3 }

cXgcpMediaGwMaxExpTimeout OBJECT-TYPE
    SYNTAX                Integer32 (1..60000)
    UNITS                 "milliseconds"
    MAX-ACCESS            read-write
    STATUS                current
    DESCRIPTION
        "This object specifies the maximum timeout for 
         exponential command retry by the media gateway."
    DEFVAL { 4000 }
    ::= { cXgcpMediaGwEntry 4 }

cXgcpMediaGwRestartMwd OBJECT-TYPE
    SYNTAX             Integer32 (0..600000)
    UNITS              "milliseconds"
    MAX-ACCESS         read-write
    STATUS             current
    DESCRIPTION
        "The maximum waiting delay (MWD) timeout value is used 
         for the media gateway to send the first Restart In 
         Progress to the MGC.

         When a gateway is powered on, it should initiate a restart 
         timer to a random value, uniformly distributed between 0 and 
         a maximum waiting delay (MWD). The gateway should send the 
         first RSIP message when the timer expires.

         The initial value of this object is chosen in an
         implementation-dependent manner by the MGCP functionality
         based on the call volume of the system. "
    REFERENCE
        "RFC2705 - Media Gateway Control Protocol (MGCP)
         version 1.0 : Section 4.3.4 Fighting the restart avalanche"
    DEFVAL { 3000 }
    ::= { cXgcpMediaGwEntry 5 }

cXgcpMediaGwRestartDelay OBJECT-TYPE
    SYNTAX               Integer32 (0..600)
    UNITS                "seconds"
    MAX-ACCESS           read-write
    STATUS               current
    DESCRIPTION
        "This object specifies the Restart Delay Timeout for
         the restart process for a gateway to send out 
         RestartInProgress when it is powered on or
         been reset.

         The purpose of setting the Restart Delay timer before 
         sending the RestartInProgress notification to the 
         media gateway controller is to avoid the network 
         congestion during the critical period of service 
         restoration. "
    REFERENCE
        "RFC2705 - Media Gateway Control Protocol (MGCP)
         version 1.0 : Section 4.3.4 Fighting the restart avalanche"
    DEFVAL { 0 }
    ::= { cXgcpMediaGwEntry 6 }

cXgcpMediaGwDefaultPackage OBJECT-TYPE
    SYNTAX                 INTEGER {
                              packageDC    (1),
                              packageG     (2),
                              packageD     (3),
                              packageM     (4),
                              packageT     (5),
                              packageL     (6),
                              packageH     (7),
                              packageR     (8),
                              packageN     (9),
                              packageA     (10),
                              packageS     (11),
                              packageATM   (12),
                              packageMS    (13),
                              packageDT    (14),
                              packageMO    (15),
                              packageRES   (16),
                              packageSASDI (17),
                              packageIT    (18),
                              packageMT    (19),
                              packageB     (20),
                              packageSST   (21),
                              packageMDR   (22),
                              packageFXR   (23),
                              packageBA    (24),
                              packageMD    (25),
                              packageNAS   (26),
                              packageMDSTE (27),
                              packagePRE   (28),
                              packageLCS   (29),
                              packageSRTP  (30),
                              packageFM    (31)
                           }
    MAX-ACCESS             read-write 
    STATUS                 current
    DESCRIPTION
        "This object represents the default capability package
         supported in the gateway. 

         packageDC   ( 1) - Don't Care package
         packageG    ( 2) - Generic package
         packageD    ( 3) - DTMF package
         packageM    ( 4) - MF package
         packageT    ( 5) - Trunk package
         packageL    ( 6) - Line package
         packageH    ( 7) - Handset package
         packageR    ( 8) - RTP package
         packageN    ( 9) - NAS package
         packageA    (l0) - Announcement Server package
         packageS    (11) - Script package
         packageATM  (12) - ATM package
         packageMS   (13) - MF CAS package
         packageDT   (14) - DTMF CAS package
         packageMO   (15) - MO package
         packageRES  (16) - RES package
         packageSASDI(17) - ASDI package (S) NCS
         packageIT   (18) - IT package (S) TGCP
         packageMT   (19) - MT package
         packageB    (20) - B package
         packageSST  (21) - SST package
         packageMDR  (22) - MDR package
         packageFXR  (23) - FAX package
         packageBA   (24) - Bulk Audit package
         packageMD   (25) - MD package
         packageNAS  (26) - Network Access Server package
         packageMDSTE(27) - Modem relay Secure Telephone 
                            Equipment package
         packagePRE  (28) - PRE package
         packageLCS  (29) - MGCP Line Control Signaling package
         packageSRTP (30) - Secure RTP package
         packageFM   (31) - Media Format Package
        "
    REFERENCE
        "RFC2705 - Media Gateway Control Protocol (MGCP)
         version 1.0 : 6.1.  Basic packages"
    DEFVAL { packageG }
    ::= { cXgcpMediaGwEntry 7 }

cXgcpMediaGwSupportedPackages OBJECT-TYPE
    SYNTAX                    BITS {
                              notFound     (0),
                              packageDC    (1),
                              packageG     (2),
                              packageD     (3),
                              packageM     (4),
                              packageT     (5),
                              packageL     (6),
                              packageH     (7),
                              packageR     (8),
                              packageN     (9),
                              packageA     (10),
                              packageS     (11),
                              packageATM   (12),
                              packageMS    (13),
                              packageDT    (14),
                              packageMO    (15),
                              packageRES   (16),
                              packageSASDI (17),
                              packageIT    (18),
                              packageMT    (19),
                              packageB     (20),
                              packageSST   (21),
                              packageMDR   (22),
                              packageFXR   (23),
                              packageBA    (24),
                              packageMD    (25),
                              packageNAS   (26),
                              packageMDSTE (27),
                              packagePRE   (28),
                              packageLCS   (29),
                              packageSRTP  (30),
                              packageFM    (31)
                              } 
    MAX-ACCESS                read-only
    STATUS                    current
    DESCRIPTION
        "This object represents the bit map of MGCP supported 
         packages. 

         Bit 0  - Not Found
         Bit 1  - Package DC     (Don't care package)
         Bit 2  - Package G      (Generic package)
         Bit 3  - Package D      (DTMF package)
         Bit 4  - Package M      (MF package)
         Bit 5  - Package T      (Trunk package)
         Bit 6  - Package L      (Line package)
         Bit 7  - Package H      (Handset package)
         Bit 8  - Package R      (RTP package)
         Bit 9  - Package N      (NAS package)
         Bit 10 - Package A      (Announcement Server package)
         Bit 11 - Package S      (Script package) 
         Bit 12 - Package ATM    (ATM package)
         Bit 13 - Package MS     (MF CAS package)
         Bit 14 - Package DT     (DTMF CAS package)
         Bit 15 - Package MO     (MO package)
         Bit 16 - Package RES    (RES package)
         Bit 17 - Package S_ASDI (ASDI package (S) NCS)
         Bit 18 - Package IT     (IT package (S) TGCP)
         Bit 19 - Package MT     (MT package)
         Bit 20 - Package B      (B package)
         Bit 21 - Package SST    (SST package)
         Bit 22 - Package MDR    (MDR package)
         Bit 23 - Package FXR    (FAX package)
         Bit 24 - Package BA     (Bulk Audit package)
         Bit 25 - Package MD     (MD package)
         Bit 26 - Package NAS    (Network Access Server package)
         Bit 27 - Package MDSTE  (Modem relay Secure Telephone 
                                  Equipment package)
         Bit 28 - Package PRE    (PRE package)
         Bit 29 - Package LCS    (MGCP Line Control Signaling package)
         Bit 33 - Package SRTP   (Secure RTP package)
         Bit 31 - Package FM     (Media Format Package)

         The value 0 means there is no supported packages. 
        "
    REFERENCE
        "RFC2705 - Media Gateway Control Protocol (MGCP)
         version 1.0 : 6.1.  Basic packages "
    ::= { cXgcpMediaGwEntry 8 }

cXgcpMediaGwSimpleSdpEnabled OBJECT-TYPE
    SYNTAX                   TruthValue
    MAX-ACCESS               read-write
    STATUS                   current
    DESCRIPTION
        "This object is used to enable/disable building of 
         s, t, o lines in SDP message.

         where  o  field indicates the owner/creator and session 
                   identifier
                s  field indicates the session name
                t  field indicates the duration while a session 
                   is valid.

         If this object is set to 'true'(enabled), SDP will NOT
         include the fields s, t, and o.
     
         If this object is set to 'false', then it indicates that
         the o, s, t lines be built before sending SDP 
         (Session Description Protocol). "
    DEFVAL { false }
    ::= { cXgcpMediaGwEntry 9 }

cXgcpMediaGwAckSdpEnabled OBJECT-TYPE
    SYNTAX                TruthValue
    MAX-ACCESS            read-write
    STATUS                current
    DESCRIPTION
        "This object specifies the ACK SDP is enabled or not.

         If this object is set to 'true', then it sends ADP with ACK
         when CODEC or reportable NTE delta changed, or an attempt
         is made to change CODEC, VAD, Packet-period, echo 
         cancellation during FAX/modem mode. "
    DEFVAL { false }
    ::= { cXgcpMediaGwEntry 10 }

cXgcpMediaGwUndottedNotation OBJECT-TYPE
    SYNTAX                   TruthValue
    MAX-ACCESS               read-write
    STATUS                   current
    DESCRIPTION
        "This object enables/disables the undotted notation 
         for CODEC.

         This object is used to set CODEC notation to 
         'dotted' or 'undotted' in SDP between the gateway
         and the call agent.
         For example, 'G.726' is 'dotted', while 'G726'
         is 'undotted'.

         If it is set to 'true', then the 'undotted'
         notation for CODEC is enabled. "
    DEFVAL { false }
    ::= { cXgcpMediaGwEntry 11 }

cXgcpMediaGwQuarantineProcess OBJECT-TYPE
    SYNTAX                    TruthValue
    MAX-ACCESS                read-write
    STATUS                    current
    DESCRIPTION
        "This object is used to determine how to handle persistent 
         events.

         If this object is set to 'true', the quarantined events
         should be processed, otherwise the quarantined events is 
         discarded. "
    REFERENCE
        "RFC2705 - Media Gateway Control Protocol (MGCP)
         version 1.0 : Section 3.2.2.12.  QuarantineHandling"
    DEFVAL { false }
    ::= { cXgcpMediaGwEntry 12 }

cXgcpMediaGwQuarantineLoop OBJECT-TYPE
    SYNTAX                 TruthValue
    MAX-ACCESS             read-write
    STATUS                 current
    DESCRIPTION
        "This object controls the default quarantine mode.
         If this object is set to 'true', the default quarantine
         mode is 'loop', not 'step'.

         When this object is set to 'true', the gateway is expected
         to generate multiple notifications (loop), not at most one
         notification (step by step), in response to quarantined 
         events.

         This object will be ignored if the object
         cXgcpMediaGwQuarantineProcess is set to 'false'. "
    REFERENCE
        "RFC2705 - Media Gateway Control Protocol (MGCP)
         version 1.0 : Section 2.3.2.  NotificationRequest "
    DEFVAL { true }
    ::= { cXgcpMediaGwEntry 13 }

cXgcpMediaGwQuarantinePersist OBJECT-TYPE
    SYNTAX                    TruthValue
    MAX-ACCESS                read-write
    STATUS                    current
    DESCRIPTION
        "This object specifies how the persist events will
         be handled in quarantine processing.
         If this object is set to 'true', the persistent events
         bypass quarantine buffer.

         This object will be ignored if the object
         cXgcpMediaGwQuarantineProcess is set to 'false'. "
    REFERENCE
        "RFC2705 - Media Gateway Control Protocol (MGCP)
         version 1.0 : Section 2.3.2.  NotificationRequest"
    DEFVAL { false }
    ::= { cXgcpMediaGwEntry 14 }

cXgcpMediaGwPiggybackMsg OBJECT-TYPE
    SYNTAX               TruthValue
    MAX-ACCESS           read-write
    STATUS               current
    DESCRIPTION
        "This object enables/disables the piggyback message 
         generating.
         If the piggyback message generating is enabled, 
         a call agent can send several MGCP messages in the 
         same UDP packets to the gateway.  "
    REFERENCE
        "RFC2705 - Media Gateway Control Protocol (MGCP)
         version 1.0 : Section 3.6.4.  Piggy backing"
    DEFVAL { true }
    ::= { cXgcpMediaGwEntry 15 }

cXgcpMediaGwMaxMsgSize OBJECT-TYPE
    SYNTAX             Integer32 (0..65535)
    UNITS              "bytes"
    MAX-ACCESS         read-write
    STATUS             current
    DESCRIPTION
        "This object specifies the maximum allowed xGCP message 
         size which is used for checking if the size will be 
         supported by the call agent via (AuditEndPoint) response.
         A value of 0 means that there is no limit to the size of 
         the XGCP message."
    REFERENCE
        "RFC2705 - Media Gateway Control Protocol (MGCP)
         version 1.0 : Section 2.3.8 Audit Endpoint "
    DEFVAL { 0 }
    ::= { cXgcpMediaGwEntry 16 }

cXgcpMediaGwLastFailMgcAddrType  OBJECT-TYPE 
    SYNTAX                InetAddressType
    MAX-ACCESS            read-only
    STATUS                current
    DESCRIPTION
        "This object indicates the address type, either IPv4 or
         IPv6, of cxeCallCtrlLastFailMgcAddr."
    ::= { cXgcpMediaGwEntry 17 }

cXgcpMediaGwLastFailMgcAddr  OBJECT-TYPE
    SYNTAX            InetAddress
    MAX-ACCESS        read-only
    STATUS            current
    DESCRIPTION
        "This object indicates the address of last MGC which the
         media gateway had tried to communicate with but failed."
    ::= { cXgcpMediaGwEntry 18 }

cXgcpMediaGwDtmfRelay  OBJECT-TYPE
    SYNTAX            TruthValue
    MAX-ACCESS        read-write
    STATUS             current
    DESCRIPTION
        "When this object is set to 'true', the digits will be
         sent as peer-to-peer packet in the bearer.
         When this object is set to 'false', the digits will be
         sent as regular voice packets in the bearer.

         For low complexity CODECS (such as G.711), the preferred
         value for this object could be 'false'.
         For high complexity CODECS (such as G.729A), the preferred
         value for this object should be 'true', otherwise
         the digits may not get recognized properly at the remote
         end."
    ::= { cXgcpMediaGwEntry 19 }

cXgcpMediaGwCaleaEnabled OBJECT-TYPE
    SYNTAX            TruthValue
    MAX-ACCESS        read-write
    STATUS            current
    DESCRIPTION
        "CALEA, Communication Assistance for Law Enforcement Act, 
         is a feature that allows for a lawful intercept of a 
         call details and call contents originating or terminating
         on specific terminals. 
         CALEA feature can be turned on or off.  A value 'true' 
         specifies CALEA enabled and a value 'false' specifies 
         CALEA disabled."
    DEFVAL { false }
    ::= { cXgcpMediaGwEntry 20 }

cXgcpMediaGwConfiguredPackages OBJECT-TYPE
    SYNTAX                    BITS {
                              notFound     (0),
                              packageDC    (1),
                              packageG     (2),
                              packageD     (3),
                              packageM     (4),
                              packageT     (5),
                              packageL     (6),
                              packageH     (7),
                              packageR     (8),
                              packageN     (9),
                              packageA     (10),
                              packageS     (11),
                              packageATM   (12),
                              packageMS    (13),
                              packageDT    (14),
                              packageMO    (15),
                              packageRES   (16),
                              packageSASDI (17),
                              packageIT    (18),
                              packageMT    (19),
                              packageB     (20),
                              packageSST   (21),
                              packageMDR   (22),
                              packageFXR   (23),
                              packageBA    (24),
                              packageMD    (25),
                              packageNAS   (26),
                              packageMDSTE (27),
                              packagePRE   (28),
                              packageLCS   (29),
                              packageSRTP  (30),
                              packageFM    (31)
                              } 
    MAX-ACCESS                read-write
    STATUS                    current
    DESCRIPTION
        "This object represents the bit map of MGCP packages
         configured and supported in the gateway. 

         Bit 0  - Not Found
         Bit 1  - Package DC     (Don't care package)
         Bit 2  - Package G      (Generic package)
         Bit 3  - Package D      (DTMF package)
         Bit 4  - Package M      (MF package)
         Bit 5  - Package T      (Trunk package)
         Bit 6  - Package L      (Line package)
         Bit 7  - Package H      (Handset package)
         Bit 8  - Package R      (RTP package)
         Bit 9  - Package N      (NAS package)
         Bit 10 - Package A      (Announcement Server package)
         Bit 11 - Package S      (Script package) 
         Bit 12 - Package ATM    (ATM package)
         Bit 13 - Package MS     (MF CAS package)
         Bit 14 - Package DT     (DTMF CAS package)
         Bit 15 - Package MO     (MO package)
         Bit 16 - Package RES    (RES package)
         Bit 17 - Package S_ASDI (ASDI package (S) NCS)
         Bit 18 - Package IT     (IT package (S) TGCP)
         Bit 19 - Package MT     (MT package)
         Bit 20 - Package B      (B package)
         Bit 21 - Package SST    (SST package)
         Bit 22 - Package MDR    (MDR package)
         Bit 23 - Package FXR    (FAX package)
         Bit 24 - Package BA     (Bulk Audit package)
         Bit 25 - Package MD     (MD package)
         Bit 26 - Package NAS    (Network Access Server package)
         Bit 27 - Package MDSTE  (Modem relay Secure Telephone
                                  Equipment package)
         Bit 28 - Package PRE    (PRE package)
         Bit 29 - Package LCS    (MGCP Line Control Signaling package)
         Bit 33 - Package SRTP   (Secure RTP package)
         Bit 31 - Package FM     (Media Format Package)

         The value 0 means there is no supported packages. 
        "
    REFERENCE
        "RFC2705 - Media Gateway Control Protocol (MGCP)
         version 1.0 : 6.1.  Basic packages "
    ::= { cXgcpMediaGwEntry 21 }

cXgcpMediaGwConnOosRsipBehavior OBJECT-TYPE
    SYNTAX            INTEGER {
                          sendDlcx (1),
                          rsipOnly (2)
                      }
     
    MAX-ACCESS        read-write
    STATUS            current
    DESCRIPTION
         "This object specifies the RSIP behavior of the endpoints with
         active calls (in connections) when they are forced to
         out-of-service.

         The following values can be set for this object:

         sendDlcx - The media gateway sends RSIP-graceful and then
                    individual DLCX command to delete the endpoints of
                    each connection and its children before it sends 
                    out RSIP-forced command when an endpoint goes into
                    alarm or placed out-of-service forcefully through
                    the user command if the endpoint or its children
                    has any calls (in connections).

         rsipOnly - The media gateway sends out RSIP-forced command, 
                    and delete the connections without any DLCX or 
                    RSIP-graceful command.

         This object is applicable only if the endpoint or its children
         have any calls. If there are no calls on the endpoint, the
         media gateway sends RSIP-forced command when the endpoint is
         forced to out-of-service."
    DEFVAL { sendDlcx }         
    ::= { cXgcpMediaGwEntry 22 }

cXgcpMediaGwLongDurTimer OBJECT-TYPE
    SYNTAX      Integer32(1..65536)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This object specifies the long duration timer. It is used
         to define the long duration of a connection. Once the timer 
         expires, a notification will be sent to the MGC to indicate
         that a connection has established for the defined long
         duration." 
    DEFVAL { 3600 }
    ::= { cXgcpMediaGwEntry 23 }

cXgcpMediaGwProfile OBJECT-TYPE
    SYNTAX      CCallControlProfileIndexOrZero
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This object specifies the XGCP profile in the media
         gateway level.

         The value of 0 means the XGCP default profile is
         used in the media gateway level.

         If the value of ccasIfExtVoiceCfgCcntrlProfile is 0,
         then the endpoint uses the profile specified in this 
         object."
    DEFVAL { 0 }
    ::= { cXgcpMediaGwEntry 24 }

cXgcpMediaGwAnnexabSdpEnabled OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This object specifies the format for parsing or generating
         G.723 or G.729 codec in SDP message for the media gateway.

         The value 'true' means using Annex A and B in fmtp line 
         complying with RFC 3555.

         The value 'false' means using Annex A and B in SDP 
         attribute codec string."
    DEFVAL { false }
    ::= { cXgcpMediaGwEntry 25 }


-- *****************************************************************
-- The XGCP Statistics table
-- *****************************************************************
cXgcpMsgStatsTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF CXgcpMsgStatsEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "This table contains statistical information on the transmitted
         and received network messages between MG and MGC, since the MG reset.

         The entries in this table are uniquly identified by the VMG index and
         the MGC address.

         This table contains statistics of the most recently received 64 MGC
         addressess for every VMG present in the device. When a new address is
         received and the number of entries for this MGC exceeds 64, then a
         least recently received entry is deleted."
    ::= { cXgcpStats 1 }

cXgcpMsgStatsEntry OBJECT-TYPE
    SYNTAX         CXgcpMsgStatsEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "This entry contains the statistical information on the
         received and transmitted network messages with the associated MGC
         address."
    INDEX   { cmgwIndex, cXgcpMsgStatsIndex }
    ::= { cXgcpMsgStatsTable 1 }

CXgcpMsgStatsEntry ::= SEQUENCE {
    cXgcpMsgStatsIndex              Integer32,
    cXgcpMsgStatsMgcIPAddressType   InetAddressType,
    cXgcpMsgStatsMgcIPAddress       InetAddress,
    cXgcpMsgStatsSuccessMessages    Counter32,
    cXgcpMsgStatsFailMessages       Counter32,
    cXgcpMsgStatsIncompleteMessages Counter32
}

cXgcpMsgStatsIndex  OBJECT-TYPE
    SYNTAX          Integer32 (1..64)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A unique index to identify a specific MGC address
         for tracking xGCP statistics between MGC and MG."
    ::= { cXgcpMsgStatsEntry 1 }

cXgcpMsgStatsMgcIPAddressType OBJECT-TYPE
    SYNTAX                InetAddressType
    MAX-ACCESS            read-only
    STATUS                current
    DESCRIPTION
        "This object indicates the address type of 
         cXgcpMsgStatsMgcIPAddress. "
    ::= { cXgcpMsgStatsEntry 2 }

cXgcpMsgStatsMgcIPAddress OBJECT-TYPE
    SYNTAX                InetAddress
    MAX-ACCESS            read-only
    STATUS                current
    DESCRIPTION
        "This object indicates IP address of the MGC. 
         The IP address should be unique on the table."
    ::= { cXgcpMsgStatsEntry 3 }

cXgcpMsgStatsSuccessMessages  OBJECT-TYPE
    SYNTAX                    Counter32
    MAX-ACCESS                read-only
    STATUS                    current
    DESCRIPTION
        "This object indicates the number of successful messages
         that communicate with the MGC on that IP address.

         Successful messages apply to both transmit and
         receive messages.

           Transmit: Positive ACK received from the MGC.

           Receive : Positive ACK sent to the MGC. This implies that the
                     format of the message is correct and the request
                     can be fulfilled."
    ::= { cXgcpMsgStatsEntry 4 }

cXgcpMsgStatsFailMessages  OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "This object indicates the number of failed messages
         that communicate with the MGC on that IP address.

         Failed messages apply to both transmit and receive
         messages. 

           Transmit: Either NAK has been received from the MGC or message
                     times out waiting for ACK.   
           Receive:  Format of the received message is bad or
                     the request was NAK'ed."
    ::= { cXgcpMsgStatsEntry 5 }
 
cXgcpMsgStatsIncompleteMessages  OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "This object indicates the number of transmit messages for which
         time out occurred while waiting for an ACK."
    ::= { cXgcpMsgStatsEntry 6 }

--
--  Table for received and transmitted network messages at the MG level.
--

cXgcpStatsTable      OBJECT-TYPE
    SYNTAX         SEQUENCE OF CXgcpStatsEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "This table contains information on the received and transmitted
         network messages, based on each message type, for all the VMGs
         present in the device.
        
         The table will have one entry for every VMG present in the device.
         When a new MG is instantiated, the device creates an entry. The entry
         is destroyed if the associated VMG is terminated."
    ::= { cXgcpStats 2 }

cXgcpStatsEntry OBJECT-TYPE
    SYNTAX         CXgcpStatsEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "This entry contains the information on the associated VMG's received
         and transmitted network messages.

         The value of each statistical object is incremented when the MG
         receives or transmits an XGCP message corresponding to that object
         type. All these values are set to '0' upon restarting of the VMG."
    INDEX   { cmgwIndex }
    ::= { cXgcpStatsTable 1 }

CXgcpStatsEntry ::= SEQUENCE {
    cXgcpStatsUdpRxPkts        Counter32,
    cXgcpStatsUdpTxPkts        Counter32,
    cXgcpStatsUnRecRxPkts      Counter32,
    cXgcpStatsMsgParsingErrors Counter32,
    cXgcpStatsDupAckTxMsgs     Counter32,
    cXgcpStatsInvalidVerCount  Counter32,
    cXgcpStatsUnknownMgcRxPkts Counter32,
    cXgcpStatsAckTxMsgs        Counter32,
    cXgcpStatsNackTxMsgs       Counter32,
    cXgcpStatsAckRxMsgs        Counter32,
    cXgcpStatsNackRxMsgs       Counter32,
    cXgcpStatsRxCrcxs          Counter32,
    cXgcpStatsRxSuccCrcxs      Counter32,
    cXgcpStatsRxFailCrcxs      Counter32,
    cXgcpStatsRxDlcxs          Counter32,
    cXgcpStatsRxSuccDlcxs      Counter32,
    cXgcpStatsRxFailDlcxs      Counter32,
    cXgcpStatsTxDlcxs          Counter32,
    cXgcpStatsTxSuccDlcxs      Counter32,
    cXgcpStatsTxFailDlcxs      Counter32,
    cXgcpStatsRxMdcxs          Counter32,
    cXgcpStatsRxSuccMdcxs      Counter32,
    cXgcpStatsRxFailMdcxs      Counter32,
    cXgcpStatsRxRqnts          Counter32,
    cXgcpStatsRxSuccRqnts      Counter32,
    cXgcpStatsRxFailRqnts      Counter32,
    cXgcpStatsRxAucxs          Counter32,
    cXgcpStatsRxSuccAucxs      Counter32,
    cXgcpStatsRxFailAucxs      Counter32,
    cXgcpStatsRxAueps          Counter32,
    cXgcpStatsRxSuccAueps      Counter32,
    cXgcpStatsRxFailAueps      Counter32,
    cXgcpStatsTxRsips          Counter32,
    cXgcpStatsTxSuccRsips      Counter32,
    cXgcpStatsTxFailRsips      Counter32,
    cXgcpStatsTxNotifies       Counter32,
    cXgcpStatsTxSuccNotifies   Counter32,
    cXgcpStatsTxFailNotifies   Counter32
}

cXgcpStatsUdpRxPkts  OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of UDP packets received from all the MGCs."
    ::= { cXgcpStatsEntry 1 }

cXgcpStatsUdpTxPkts  OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of UDP packets sent to all the MGCs."
    ::= { cXgcpStatsEntry 2 }

cXgcpStatsUnRecRxPkts OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of unrecognized UDP packets received from all the MGCs."
    ::= { cXgcpStatsEntry 3 }

cXgcpStatsMsgParsingErrors  OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of messages with parsing errors received from all the MGCs."
    ::= { cXgcpStatsEntry 4 }

cXgcpStatsDupAckTxMsgs  OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of duplicate response messages sent to the MGCs."
    ::= { cXgcpStatsEntry 5 }

cXgcpStatsInvalidVerCount  OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of invalid protocol version messages received from all the
         MGCs."
    ::= { cXgcpStatsEntry 6 }

cXgcpStatsUnknownMgcRxPkts  OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of unknown message packets received from all the MGCs."
    ::= { cXgcpStatsEntry 7 }

cXgcpStatsAckTxMsgs   OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of acknowledgment messages sent by the MG."
    ::= { cXgcpStatsEntry 8 }

cXgcpStatsNackTxMsgs  OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of negative acknowledgment messages sent by the MG."
    ::= { cXgcpStatsEntry 9 }

cXgcpStatsAckRxMsgs   OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of acknowledgment messages received by the MG."
    ::= { cXgcpStatsEntry 10 }

cXgcpStatsNackRxMsgs  OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of negative acknowledgment messages received by the MG."
    ::= { cXgcpStatsEntry 11}

cXgcpStatsRxCrcxs     OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of CRCX messages received by the MG."
    ::= { cXgcpStatsEntry 12}

cXgcpStatsRxSuccCrcxs OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of CRCX messages received, that were successful."
    ::= { cXgcpStatsEntry 13}

cXgcpStatsRxFailCrcxs OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of CRCX messages received, that failed."
    ::= { cXgcpStatsEntry 14}

cXgcpStatsRxDlcxs     OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of DLCX messages received."
    ::= { cXgcpStatsEntry 15}

cXgcpStatsRxSuccDlcxs OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of DLCX messages received, that were successful."
    ::= { cXgcpStatsEntry 16}

cXgcpStatsRxFailDlcxs OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of DLCX messages received, that failed."
    ::= { cXgcpStatsEntry 17}

cXgcpStatsTxDlcxs     OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of DLCX messages sent."
    ::= { cXgcpStatsEntry 18}

cXgcpStatsTxSuccDlcxs OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of DLCX messages sent, that were successful."
    ::= { cXgcpStatsEntry 19}

cXgcpStatsTxFailDlcxs OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of DLCX messages sent, that failed."
    ::= { cXgcpStatsEntry 20}

cXgcpStatsRxMdcxs     OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of MDCX messages received."
    ::= { cXgcpStatsEntry 21}

cXgcpStatsRxSuccMdcxs OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of MDCX messages received, that were successful."
    ::= { cXgcpStatsEntry 22}

cXgcpStatsRxFailMdcxs OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of MDCX messages received, that failed."
    ::= { cXgcpStatsEntry 23}

cXgcpStatsRxRqnts     OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of RQNT messages received."
    ::= { cXgcpStatsEntry 24}

cXgcpStatsRxSuccRqnts OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of RQNT messages received, that were successful."
    ::= { cXgcpStatsEntry 25}

cXgcpStatsRxFailRqnts OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of RQNT messages received, that failed."
    ::= { cXgcpStatsEntry 26}

cXgcpStatsRxAucxs     OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of AUCX messages received."
    ::= { cXgcpStatsEntry 27}

cXgcpStatsRxSuccAucxs OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of AUCX messages received, that were successful."
    ::= { cXgcpStatsEntry 28}

cXgcpStatsRxFailAucxs OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of AUCX messages received, that failed."
    ::= { cXgcpStatsEntry 29}

cXgcpStatsRxAueps     OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of AUEP messages received."
    ::= { cXgcpStatsEntry 30}

cXgcpStatsRxSuccAueps OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of AUEP messages received, that were successful."
    ::= { cXgcpStatsEntry 31}

cXgcpStatsRxFailAueps OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of AUEP messages received, that failed."
    ::= { cXgcpStatsEntry 32}

cXgcpStatsTxRsips     OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of RSIP messages sent."
    ::= { cXgcpStatsEntry 33}

cXgcpStatsTxSuccRsips OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of RSIP messages sent, that were successful."
    ::= { cXgcpStatsEntry 34}

cXgcpStatsTxFailRsips OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of RSIP messages sent, that failed."
    ::= { cXgcpStatsEntry 35}

cXgcpStatsTxNotifies  OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of NTFY messages sent."
    ::= { cXgcpStatsEntry 36}

cXgcpStatsTxSuccNotifies   OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of NTFY messages sent, that were successful."
    ::= { cXgcpStatsEntry 37}

cXgcpStatsTxFailNotifies   OBJECT-TYPE
    SYNTAX                 Counter32
    MAX-ACCESS             read-only
    STATUS                 current
    DESCRIPTION
        "Number of NTFY messages sent, that failed."
    ::= { cXgcpStatsEntry 38}

--
--  Table for active connections that are controlled by the MG.
--

cXgcpConnectionTable OBJECT-TYPE
    SYNTAX         SEQUENCE OF CXgcpConnectionEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "This table contains information on the active connections of all the
         VMGs present in the device.
        
         A MG may have zero or more number of calls at any given
         time. Each call consists of one or more connection.

         The table will have one entry per VMG per connection present in the
         device. When a new connection is established, the device creates an
         entry. The entry is destroyed if the associated connection is torn
         down."
    ::= { cXgcpConnection 1 }

cXgcpConnectionEntry OBJECT-TYPE
    SYNTAX         CXgcpConnectionEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
        "This entry contains the information about an active connection."
    INDEX   { cmgwIndex, cXgcpConnId }
    ::= { cXgcpConnectionTable 1 }

CXgcpConnectionEntry ::= SEQUENCE {
    cXgcpConnId                 Unsigned32,
    cXgcpConnEndPoint           SnmpAdminString,
    cXgcpConnCallId             SnmpAdminString,
    cXgcpConnLocalUdpPort       CiscoPort,
    cXgcpConnRemoteUdpPort      CiscoPort,
    cXgcpConnMode               INTEGER,
    cXgcpConnVccId              Unsigned32,
    cXgcpConnChannelId          Unsigned32,
    cXgcpConnCallState          INTEGER,
    cXgcpConnCodec              INTEGER,
    cXgcpConnLastSuccEvent      CXgcpCallEvent,
    cXgcpConnLastSuccIntEvent   CXgcpCallEvent,
    cXgcpConnLastFailedEvent    CXgcpCallEvent,
    cXgcpConnLastReqEvent       CXgcpCallEvent,
    cXgcpConnEventResult        INTEGER,
    cXgcpConnEncrSuite          INTEGER
}

cXgcpConnId   OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4294967295)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Connection ID generated by the gateway and sent in the
         ACK message."
    ::= { cXgcpConnectionEntry 1 }

cXgcpConnEndPoint  OBJECT-TYPE
    SYNTAX          SnmpAdminString 
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The physical or virtual entity that acts as a source or sink of data
         in the MG is called an endpoint. Every end point in the MG is
         assigned a textual name by the MG."
    ::= { cXgcpConnectionEntry 2 }

cXgcpConnCallId  OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Call ID associated with this connection. Call ID is a parameter that
         identifies the call to which this connection belongs to. A call ID is
         unique within a VMG instance."
    ::= { cXgcpConnectionEntry 3 }

cXgcpConnLocalUdpPort  OBJECT-TYPE
    SYNTAX          CiscoPort
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The local UDP port used for the connection."
    ::= { cXgcpConnectionEntry 4 }

cXgcpConnRemoteUdpPort  OBJECT-TYPE
    SYNTAX          CiscoPort
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The remote UDP port used for the connection."
    ::= { cXgcpConnectionEntry 5 }

cXgcpConnMode  OBJECT-TYPE
    SYNTAX      INTEGER {
         invalid     (0),
         sendOnly    (1),
         recvOnly    (2),
         sendRecv    (3),
         inActive    (4),
         loopBack    (5),
         contTest    (6),
         data        (7),
         netwLoop    (8),
         netwTest    (9),
         conference  (10)
    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Represents possible MG connection modes.
         invalid     - Invalid value for mode
         sendOnly    - The GW should only send packets
         recvOnly    - The GW should only receive packets
         sendRecv    - The GW can send and receive packets
         inActive    - The GW should neither send nor receive
                       packets
         loopBack    - The GW should place the circuit in loopback
                       mode
         contTest    - The GW should place the circuit in test mode
         data        - The GW should use the circuit for network
                       access for data
         netwLoop    - The GW should place the connection in
                       network loopback mode
         netwTest    - The GW should place the connection in
                       network continuity test mode
         conference  - The GW should place the connection in
                       conference mode."
    ::= { cXgcpConnectionEntry 6 }

cXgcpConnVccId  OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4294967295)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "VCCI used for the VoAAL2 call. The object should have a non-zero
         value only if the associated call is of VoAAL2 type. For all other
         calls the value should be '0'."
    ::= { cXgcpConnectionEntry 7 }

cXgcpConnChannelId  OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4294967295)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "CID used for the VoAAL2 call. The object should have a non-zero
         value only if the associated call is of VoAAL2 type. For all other
         calls the value should be '0'."
    ::= { cXgcpConnectionEntry 8 }

cXgcpConnCallState  OBJECT-TYPE
    SYNTAX      INTEGER {
         idle                   (0),
         setting                (1),
         connecting             (2),
         conferencing           (3),
         active                 (4),
         confDestroying         (5),
         disconnecting          (6),
         inactive               (7),
         voiceConnecting        (8),
         voiceActive            (9),
         confDissociating       (10),
         callLegsDissociated    (11),
         hpConnecting           (12),
         hpConnected            (13),
         hpConferencing         (14),
         hpActive               (15),
         voipConfDestroy        (16),
         erroState              (17),
         connectingInactive     (18),
         confDestroyingInactive (19),
         confTest               (20),
         setupWait              (21),
         waitNseSent            (22),
         twcActive              (23),
         waitState              (24),
         handOver               (25)
    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Represents possible MG call states.
         idle                   - Idle
         setting                - Incoming call from PSTN
         connecting             - CRCX message received
         conferencing           - Call connected, await
                                  conf
         active                 - Conference created
         confDestroying         - Destroying conference
         disconnecting          - Conf destroyed, disconnect call
         inactive               - call in inactive mode
         voiceConnecting        - Creating telephony call leg only
         voiceActive            - Telephony call leg created
         confDissociating       - Destroying conf
         callLegsDissociated    - Conf destroyed
         hpConnecting           - connecting TDM hair-pin call leg
         hpConnected            - one HP call leg connected
         hpConferencing         - Conferencing TDM Hairpin call leg
         hpActive               - TDM hair-pinning active state
         voipConfDestroy        - Conf destroyed, make HP call
         erroState              - call in error state
         connectingInactive     - creating inactive connection
         confDestroyingInactive - conf destroy inactive conn
         confTest               - AAL2/IP continuity test
         setupWait              - Waiting for setup information
         waitNseSent            - Wait for NSE event to be sent
         twcActive              - TWC call active
         waitState              - App is waiting for call control
         handOver               - App is grabbing back the control"
    ::= { cXgcpConnectionEntry 9 }

cXgcpConnCodec  OBJECT-TYPE
    SYNTAX       INTEGER
    {
         notApplicable        (0),
         g711ulaw             (1),
         g711alaw             (2),
         g726k32             (3),
         g726k24             (4),
         g726k16             (5),
         g729                 (6),
         g729a                (7),
         g729b                (8),
         g729bLowComp         (9),
         g728                 (10),
         g723                 (11),
         g7231HighRate        (12),
         g7231aHighRate       (13),
         g7231LowRate         (14),
         g7231aLowRate        (15),
         gsmFullRate          (16),
         gsmHalfRate          (17),
         gsmEnhancedFullRate  (18),
         gsmEnhancedHalfRate  (19),
         g729ab               (20),
         clearChannel         (128),
         nse                  (129),
         xnse                 (130),
         nte                  (131),
         t38                  (132),
         modemRelay           (133),
         mdsteModemRelay      (134),
         sse                  (135),
         codecUnknown         (200)
    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Specifies the codec type to be used with the Call.
         The following codec types are defined:

         notApplicable        - no Codec Type is defined
         g711ulaw             - G.711 mu-law
         g711alaw             - G.711 A-law
         g726k32             - G.726 32K
         g726k24             - G.726 24K
         g726k16             - G.726 16K
         g729                 - G.729
         g729a                - G.729-A
         g729b                - G.729-B
         g729bLowComp         - G.729-B Low Complexity
         g728                 - G.728
         g723                 - G.723
         g7231HighRate        - G.723.1 High Rate
         g7231aHighRate       - G.723.1 Annex A High Rate
         g7231LowRate         - G.723.1 Low Rate
         g7231aLowRate        - G.723.1 Annex A Low Rate
         gsmFullRate          - GSM full rate
         gsmHalfRate          - GSM half rate
         gsmEnhancedFullRate  - GSM enhanced full rate
         gsmEnhancedHalfRate  - GSM enhanced half rate
         g729ab               - G.729-A-B.
         clearChannel         - Nx64 clear channel
         nse                  - For NSE
         xnse                 - For X-NSE
         nte                  - For telephone-event
         t38                  - T-38
         modemRelay           - Modem Relay
         mdsteModemRelay      - For X+mdste
         sse                  - For SSE
         codecUnknown         - Unknown Codec"
    REFERENCE
         "RFC-3551"
    ::= { cXgcpConnectionEntry 10 }

cXgcpConnLastSuccEvent  OBJECT-TYPE
    SYNTAX          CXgcpCallEvent
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "A call event is defined as something that happens to a call at a
         given time. This object contains the latest MG call event
         that was successful."
    ::= { cXgcpConnectionEntry 11 }

cXgcpConnLastSuccIntEvent  OBJECT-TYPE
    SYNTAX          CXgcpCallEvent
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object contains the latest MG internal call event
         that was successful."
    ::= { cXgcpConnectionEntry 12 }

cXgcpConnLastFailedEvent  OBJECT-TYPE
    SYNTAX          CXgcpCallEvent
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object contains the latest MG call event that was
         failed."
    ::= { cXgcpConnectionEntry 13 }

cXgcpConnLastReqEvent  OBJECT-TYPE
    SYNTAX          CXgcpCallEvent
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object contains the latest requested MG call event."
    ::= { cXgcpConnectionEntry 14 }

cXgcpConnEventResult  OBJECT-TYPE
    SYNTAX      INTEGER {
         normalOk                (0),
         invalidOk               (1),
         callRecordReleased      (2),
         invalidCallId           (10),
         invalidConnId           (11),
         duplicatedMsg           (12),
         ackFailure              (13),
         deleteFailure           (14),
         createAckFailure        (15),
         createAckMissing        (16),
         deleteAckFailure        (17),
         notifyFailure           (18),
         invalidState            (19),
         invalidProtocolVer      (20),
         tgwDown                 (30),
         tgwNotReady             (31),
         callVdbFailure          (32),
         prevRtpPortLocked       (33),
         connRecordMissing       (34),
         endPointNotRdy          (35),
         memResourceError        (36),
         callCacFailure          (37),
         confRsrcError           (38),
         gwRsrcNotAvailable      (39),
         reqEventFailure         (40),
         invalidCcapiEvent       (41),
         ignoreCcapiEvent        (42),
         signalFailure           (50),
         abnormalOnhook          (51),
         invalidOffhook          (52),
         invalidCot              (53),
         cotFailure              (54),
         cotDisableFailure       (55),
         callSetupReqFailure     (60),
         callSetupIndFailure     (61),
         callContextFailure      (62),
         callPeerFailure         (63),
         callVoxCallFailure      (64),
         callVoipCallFailure     (65),
         callDiscFailure         (66),
         callModifyFailure       (67),
         callAlertFailure        (68),
         callDeleteFailure       (69),
         callUnknownFeature      (70),
         upSupportedCodec        (71),
         noDigitMap              (72),
         ignoreDigit             (73),
         digitsOverflow          (74),
         digitsNotifyFailure     (75),
         codecNotMatched         (76),
         invalidConnMode         (77),
         glare                   (78),
         peerMissing             (90),
         peerNotReady            (91),
         peerInWrongState        (92),
         peerDisconnectFailure   (93),
         noConferenceId          (94),
         confCreateFailure       (95),
         confDestroyFailure      (96),
         unknownConnType         (97),
         invalidEndpoint         (98),
         invalidNseEvent         (100),
         nseRcvdOnWrongLeg       (101),
         sendNseFailure          (102),
         playToneFailure         (103),
         codecSpecInError        (104),
         mediaSpecUpsupported    (105),
         mediaChangeFail         (106),
         invalidNsePayload       (107),
         nsePayloadNotAvail      (108),
         embMdcxError            (109),
         mdcxLeg1Error           (110),
         mdcxLeg2Error           (111),
         deferMsg                (112),
         transError              (115),
         discOnWrongLeg          (120),
         invalidNteEvent         (130),
         notEnabledNteEvent      (131),
         nteEventExecuteFail     (132),
         sendNteFailure          (133),
         invalidSsePayload       (140),
         ssePayloadNotAvailable  (141),
         invalidModemRelayParam  (142),
         modemRelayNotSupported  (143),
         invalidXcapXcpar        (144),
         invalidSprtPayload      (145),
         sprtPayloadNotAvailable (146)
    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Represents possible MG call event results.

         normalOk                -  Normal event processed OK
         invalidOk               -  Invalid event processed OK
         callRecordReleased      -  The call record is released
         invalidCallId           -  TGW find invalid call id
         invalidConnId           -  TGW find invalid connection id
         duplicatedMsg           -  TGW find duplicated sgcp msg
         ackFailure              -  TGW can't send sgcp ack msg
         deleteFailure           -  TGW can't send sgcp delete msg
         createAckFailure        -  TGW can't send create ack msg
         createAckMissing        -  TGW did't send sgcp ack msg
         deleteAckFailure        -  TGW can't send delete ack msg
         notifyFailure           -  TGW can't send sgcp notify msg
         invalidState            -  TGW find event in wrong state 
         invalidProtocolVer      -  GW finds protocl ver. not
                                    supported
         tgwDown                 -  TGW in graceful shutdown mode
         tgwNotReady             -  TGW not ready for the event
         callVdbFailure          -  TGW can't obtain the vdbptr
         prevRtpPortLocked       -  TGW find previous rtp port
                                    locked
         connRecordMissing       -  TGW can't find conn record
         endPointNotRdy          -  TGW not ready for the event
         memResourceError        -  TGW has transient mem alloc err
         callCacFailure          -  GW does not have the bandwidth
         confRsrcError           -  GW cannot get conf resource
         gwRsrcNotAvailable      -  GW does not have available
                                    resource
         reqEventFailure         -  TGW can't handle requested
                                    event
         invalidCcapiEvent       -  TGW can't handle the ccapi
                                    event
         ignoreCcapiEvent        -  TGW will ignore the ccapi event
         signalFailure           -  TGW can't handle the signal
         abnormalOnhook          -  TGW find abnormal onhook
         invalidOffhook          -  TGW find invalid offhook
         invalidCot              -  TGW find invalid cot
         cotFailure              -  TGW failed to do COT
         cotDisableFailure       -  TGW failed to disable COT
         callSetupReqFailure     -  TGW can't setup call request
         callSetupIndFailure     -  TGW can't handle call
                                    indication
         callContextFailure      -  TGW can't setup the context
         callPeerFailure         -  TGW can't setup the peer
         callVoxCallFailure      -  TGW can't setup the voip/voaal2
                                    call
         callVoipCallFailure     -  TGW can't setup the voip call 
         callDiscFailure         -  TGW can't disconnect the call 
         callModifyFailure       -  TGW can't modify the call parm
         callAlertFailure        -  TGW can't alert the call
         callDeleteFailure       -  TGW can't delete the call
         callUnknownFeature      -  TGW can't handle unknow feature
         upSupportedCodec        -  TGW find unsupported codec
         noDigitMap              -  TGW can't find the digit map
         ignoreDigit             -  TGW can't process the digits
         digitsOverflow          -  TGW can't handle too many digits
         digitsNotifyFailure     -  TGW can't send the digits out
         codecNotMatched         -  TGW codec doesn't match rmt TGW
         invalidConnMode         -  TGW can't understand con mode
         glare                   -  GW encountered a glare condition
         peerMissing             -  TGW find not find the peer
         peerNotReady            -  TGW find peer not ready
         peerInWrongState        -  TGW find the peer in wrong state
         peerDisconnectFailure   -  TGW can't disconnect the peer
         noConferenceId          -  TGW can't find the conference
                                    ID
         confCreateFailure       -  TGW can't create conference
         confDestroyFailure      -  TGW can't destroy conference
         unknownConnType         -  TGW can't handle the con type
         invalidEndpoint         -  TGW can't connect to endpoint
         invalidNseEvent         -  Invalid NSE event
         nseRcvdOnWrongLeg       -  The NSE events come to a wrong
                                    leg
         sendNseFailure          -  Cannot send an NSE event
         playToneFailure         -  Cannot play NSE-requested tone
         codecSpecInError        -  Codec list provided in error
         mediaSpecUpsupported    -  Media specified not supported
         mediaChangeFail         -  Media change failed
         invalidNsePayload       -  Invalid payload type in SDP
         nsePayloadNotAvail      -  Specified NSE payload not free
         embMdcxError            -  Emb modify connection error
         mdcxLeg1Error           -  Modify connection leg1 error
         mdcxLeg2Error           -  Modify connection leg2 error
         deferMsg                -  For deferring events
         transError              -  TGW endpoint in transition
                                    state
         discOnWrongLeg          -  Disconnection on wrong call leg
         invalidNteEvent         -  Invalid NTE event
         notEnabledNteEvent      -  The NTE event has not been
                                    enabled for use
         nteEventExecuteFail     -  NTE execution failed
         sendNteFailure          -  Cannot send an NTE event
         invalidSsePayload       -  Invalid SSE payload
         ssePayloadNotAvailable  -  SSE payload is not available
         invalidModemRelayParam  -  Invalid Modem Relay Param
         modemRelayNotSupported  -  Modem Relay not supported in
                                    endpt
         invalidXcapXcpar        -  Invalid X-Cap or X-Cpar in SDP
         invalidSprtPayload      -  Invalid SPRT payload
         sprtPayloadNotAvailable -  SPRT payload is not available"
    ::= { cXgcpConnectionEntry 15 }

cXgcpConnEncrSuite  OBJECT-TYPE
    SYNTAX          INTEGER {
        none    (0),
        aes128Cm (1)
    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Specifies what type of encryption suite is used to encode the
         information sent through this connection.

         none     - No Encryption suite is used
         aes128Cm - AES-128 countermode encryption suite is used."
    ::= { cXgcpConnectionEntry 16 }

--**********************************************************************
-- Conformance 
--**********************************************************************

-- 
-- conformance information
--

cXgcpMIBConformance OBJECT IDENTIFIER ::= { ciscoXgcpMIB 2 }

cXgcpMIBCompliances OBJECT IDENTIFIER ::= { cXgcpMIBConformance 1 }

cXgcpMIBGroups      OBJECT IDENTIFIER ::= { cXgcpMIBConformance 2 }


-- 
-- Conformance and compliance statements statements
--

ciscoXgcpMIBCompliance MODULE-COMPLIANCE
    STATUS  deprecated
    DESCRIPTION
        "The compliance statement for the SNMPv2 entities which 
         implement XGCP.
         This has been replaced by ciscoXgcpMIBComplianceRev1.
        "
    MODULE  -- this module
        MANDATORY-GROUPS {
            cXgcpMgcConfigGroup,
            cXgcpMediaGwGroup,
            cXgcpMsgStatsGroup
        }

    OBJECT  cXgcpMgcConfigAddrType
    SYNTAX  InetAddressType
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address type"

    OBJECT  cXgcpMgcConfigAddress
    SYNTAX  InetAddress (SIZE(4))
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address"

    OBJECT  cXgcpMsgStatsMgcIPAddressType
    SYNTAX  InetAddressType 
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address type"

    OBJECT  cXgcpMsgStatsMgcIPAddress
    SYNTAX  InetAddress (SIZE(4))
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address"

    ::= { cXgcpMIBCompliances 1 }

ciscoXgcpMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS  deprecated -- replaced by ciscoXgcpMIBComplianceRev2
    DESCRIPTION
        "The compliance statement for the SNMPv2 entities which 
         implement CISCO-XGCP-MIB.
        "
    MODULE  -- this module
        MANDATORY-GROUPS {
            cXgcpMgcConfigGroup,
            cXgcpMediaGwGroup,
            cXgcpMsgStatsGroup
        }

    OBJECT  cXgcpMgcConfigAddrType
    SYNTAX  InetAddressType
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address type"

    OBJECT  cXgcpMgcConfigAddress
    SYNTAX  InetAddress (SIZE(4))
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address"

    OBJECT  cXgcpMsgStatsMgcIPAddressType
    SYNTAX  InetAddressType 
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address type"

    OBJECT  cXgcpMsgStatsMgcIPAddress
    SYNTAX  InetAddress (SIZE(4))
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address"

    GROUP  cXgcpMediaGwGroupSup1
    DESCRIPTION
       "The implementation of this group is optional except for
        the media gateway supports the XGCP packages provisioning
        and other extended configuration."

    ::= { cXgcpMIBCompliances 2 }

ciscoXgcpMIBComplianceRev2 MODULE-COMPLIANCE
    STATUS  deprecated -- superceded by ciscoXgcpMIBComplianceRev3
    DESCRIPTION
        "The compliance statement for the SNMPv2 entities which 
         implement CISCO-XGCP-MIB.
        "
    MODULE  -- this module
        MANDATORY-GROUPS {
            cXgcpMgcConfigGroup,
            cXgcpMediaGwGroup,
            cXgcpMsgStatsGroup
        }

    OBJECT  cXgcpMgcConfigAddrType
    SYNTAX  InetAddressType
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address type"

    OBJECT  cXgcpMgcConfigAddress
    SYNTAX  InetAddress (SIZE(4))
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address"

    OBJECT  cXgcpMsgStatsMgcIPAddressType
    SYNTAX  InetAddressType 
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address type"

    OBJECT  cXgcpMsgStatsMgcIPAddress
    SYNTAX  InetAddress (SIZE(4))
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address"

    GROUP  cXgcpMediaGwGroupSup2
    DESCRIPTION
       "The implementation of this group is optional except for
        the media gateway supports the XGCP packages provisioning
        and other extended configuration."

    ::= { cXgcpMIBCompliances 3 }

ciscoXgcpMIBComplianceRev3 MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
        "The compliance statement for the SNMPv2 entities which 
         implement CISCO-XGCP-MIB.
        "
    MODULE  -- this module
        MANDATORY-GROUPS {
            cXgcpMgcConfigGroup,
            cXgcpMediaGwGroup,
            cXgcpMsgStatsGroup,
            cXgcpStatsGroup,
            cXgcpConnectionGroup
        }

    OBJECT  cXgcpMgcConfigAddrType
    SYNTAX  InetAddressType
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address type"

    OBJECT  cXgcpMgcConfigAddress
    SYNTAX  InetAddress (SIZE(4))
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address"

    OBJECT  cXgcpMsgStatsMgcIPAddressType
    SYNTAX  InetAddressType 
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address type"

    OBJECT  cXgcpMsgStatsMgcIPAddress
    SYNTAX  InetAddress (SIZE(4))
    DESCRIPTION
       "The minimal requirement for supporting this object is 'ipv4' 
        address"

    GROUP  cXgcpMediaGwGroupSup2
    DESCRIPTION
       "The implementation of this group is optional except for
        the media gateway supports the XGCP packages provisioning
        and other extended configuration."
    ::= { cXgcpMIBCompliances 4 }

--
-- units of conformance
--
-- MIB Groups
--
cXgcpMgcConfigGroup OBJECT-GROUP
    OBJECTS {
        cXgcpMgcConfigMgcGrpNum,
        cXgcpMgcConfigAddress,
        cXgcpMgcConfigAddrType,
        cXgcpMgcConfigProtocolIndex,
        cXgcpMgcConfigGatewayUdpPort
    }
    STATUS    current
    DESCRIPTION
        "This group contains the MGC objects for SGCP/MGCP that 
         the MG connects to."
    ::= { cXgcpMIBGroups 1 }

cXgcpMediaGwGroup OBJECT-GROUP
    OBJECTS {
        cXgcpMediaGwRequestTimeOut,
        cXgcpMediaGwRequestRetries,
        cXgcpMediaGwRequestRetryMethod,
        cXgcpMediaGwMaxExpTimeout,
        cXgcpMediaGwRestartMwd,
        cXgcpMediaGwRestartDelay,
        cXgcpMediaGwDefaultPackage,
        cXgcpMediaGwSupportedPackages,
        cXgcpMediaGwSimpleSdpEnabled,
        cXgcpMediaGwAckSdpEnabled,
        cXgcpMediaGwUndottedNotation,
        cXgcpMediaGwQuarantineProcess,
        cXgcpMediaGwQuarantineLoop,
        cXgcpMediaGwQuarantinePersist,
        cXgcpMediaGwPiggybackMsg,
        cXgcpMediaGwMaxMsgSize,
        cXgcpMediaGwLastFailMgcAddrType,
        cXgcpMediaGwLastFailMgcAddr,
        cXgcpMediaGwDtmfRelay,
        cXgcpMediaGwCaleaEnabled
    }
    STATUS    current
    DESCRIPTION
        "This group contains core objects for SGCP/MGCP on the 
         MG."
    ::= { cXgcpMIBGroups 2 }

cXgcpMsgStatsGroup OBJECT-GROUP
    OBJECTS {
        cXgcpMsgStatsMgcIPAddressType,
        cXgcpMsgStatsMgcIPAddress,
        cXgcpMsgStatsSuccessMessages,
        cXgcpMsgStatsFailMessages,
        cXgcpMsgStatsIncompleteMessages
    }
    STATUS    current
    DESCRIPTION
        "This group contains statistics objects for SGCP/MGCP 
         on the MGC and the MG."
    ::= { cXgcpMIBGroups 3 }

cXgcpMediaGwGroupSup1 OBJECT-GROUP
    OBJECTS {
        cXgcpMediaGwConfiguredPackages,
        cXgcpMediaGwConnOosRsipBehavior,
        cXgcpMediaGwLongDurTimer,
        cXgcpMediaGwProfile
    }
    STATUS    deprecated -- replaced by cXgcpMediaGwGroupSup2
    DESCRIPTION
        "This group contains supplimentary objects for XGCP
         extended provisioning in the MG." 
    ::= { cXgcpMIBGroups 4 }

cXgcpMediaGwGroupSup2 OBJECT-GROUP
    OBJECTS {
        cXgcpMediaGwConfiguredPackages,
        cXgcpMediaGwConnOosRsipBehavior,
        cXgcpMediaGwLongDurTimer,
        cXgcpMediaGwProfile,
        cXgcpMediaGwAnnexabSdpEnabled
    }
    STATUS    current
    DESCRIPTION
        "This group contains supplimentary objects for XGCP
         extended provisioning in the MG." 
    ::= { cXgcpMIBGroups 5 }

cXgcpStatsGroup OBJECT-GROUP
    OBJECTS {
        cXgcpStatsUdpRxPkts,
        cXgcpStatsUdpTxPkts,
        cXgcpStatsUnRecRxPkts,
        cXgcpStatsMsgParsingErrors,
        cXgcpStatsDupAckTxMsgs,
        cXgcpStatsInvalidVerCount,
        cXgcpStatsUnknownMgcRxPkts,
        cXgcpStatsAckTxMsgs,
        cXgcpStatsNackTxMsgs,
        cXgcpStatsAckRxMsgs,
        cXgcpStatsNackRxMsgs,
        cXgcpStatsRxCrcxs,
        cXgcpStatsRxSuccCrcxs,
        cXgcpStatsRxFailCrcxs,
        cXgcpStatsRxDlcxs,
        cXgcpStatsRxSuccDlcxs,
        cXgcpStatsRxFailDlcxs,
        cXgcpStatsTxDlcxs,
        cXgcpStatsTxSuccDlcxs,
        cXgcpStatsTxFailDlcxs,
        cXgcpStatsRxMdcxs,
        cXgcpStatsRxSuccMdcxs,
        cXgcpStatsRxFailMdcxs,
        cXgcpStatsRxRqnts,
        cXgcpStatsRxSuccRqnts,
        cXgcpStatsRxFailRqnts,
        cXgcpStatsRxAucxs,
        cXgcpStatsRxSuccAucxs,
        cXgcpStatsRxFailAucxs,
        cXgcpStatsRxAueps,
        cXgcpStatsRxSuccAueps,
        cXgcpStatsRxFailAueps,
        cXgcpStatsTxRsips,
        cXgcpStatsTxSuccRsips,
        cXgcpStatsTxFailRsips,
        cXgcpStatsTxNotifies,
        cXgcpStatsTxSuccNotifies,
        cXgcpStatsTxFailNotifies
    }
    STATUS    current
    DESCRIPTION
        "This group contains the received and transmitted
         network messages for every virtual MG present in
         the managed system.
        "
    ::= { cXgcpMIBGroups 6 }

cXgcpConnectionGroup OBJECT-GROUP
    OBJECTS {
        cXgcpConnEndPoint,
        cXgcpConnCallId,
        cXgcpConnLocalUdpPort,
        cXgcpConnRemoteUdpPort,
        cXgcpConnMode,
        cXgcpConnVccId,
        cXgcpConnChannelId,
        cXgcpConnCallState,
        cXgcpConnCodec,
        cXgcpConnLastSuccEvent,
        cXgcpConnLastSuccIntEvent,
        cXgcpConnLastFailedEvent,
        cXgcpConnLastReqEvent,
        cXgcpConnEventResult,
        cXgcpConnEncrSuite
    }
    STATUS    current
    DESCRIPTION
        "This group contains active connections information that 
         are controlled by the Gateway Control Protocol.
        "
    ::= { cXgcpMIBGroups 7 }

END


