-- *****************************************************************
-- CISCO-IPSLA-ETHERNET-MIB.my:  IP SLA Ethernet MIB file
--   
-- February 2006, Minghui Zhu
--   
-- Copyright (c) 2006-2012 by cisco Systems Inc.
-- All rights reserved.
--   
-- *****************************************************************

CISCO-IPSLA-ETHERNET-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Counter32,
    Gauge32,
    Unsigned32,
    TimeTicks,
    Counter64
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    TimeStamp,
    StorageType,
    RowStatus
        FROM SNMPv2-TC
    VlanId
        FROM Q-BRIDGE-MIB
    Dot1agCfmMaintDomainNameType,
    Dot1agCfmMaintDomainName
        FROM IEEE8021-CFM-MIB
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    Layer2Cos
        FROM CISCO-TC
    rttMonCtrlAdminIndex
        FROM CISCO-RTTMON-MIB
    RttResponseSense,
    RttMonRttType,
    RttMonReactVar,
    RttMonCtrlIndex,
    RttMonIdLst
        FROM CISCO-RTTMON-TC-MIB
    ciscoMgmt
        FROM CISCO-SMI;


ciscoIpSlaEthernetMIB MODULE-IDENTITY
    LAST-UPDATED    "201205150000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems, Inc.
            Customer Service 

            Postal: 170 W Tasman Drive
            San Jose, CA 95134

            Tel:    +1 800 553 NETS
            Email:  cs-ipsla@cisco.com"
    DESCRIPTION
        "This MIB module consists of two parts.

        1) Auto-Ethernet-CFM Control:
          |-- ipslaEthernetGrpCtrlTable
          |-- ipslaEthernetGrpReactTable

        2) ethernetJitter Stats:
          |-- ipslaEtherJitterLatestStatsTable
          |-- ipslaEtherJitterAggStatsTable

        The first part defines a mechanism to manage IP SLA 
        Auto-Ethernet-CFM operation.  

        IP SLA is a capability which utilizes active monitoring for 
        network perfomance.  It can be used for network 
        troubleshooting, network assessment and health monitoring.

        IEEE 802.1ag defines Connection Fault Management (CFM) for 
        Ethernet layer.  CFM can be used to detect, isolate and report
        the connectivity faults, and allows discovery and verification 
        of the path through briges and LANs.  

        Auto-Ethernet-CFM operation integrates the capabilities of 
        IP SLA and IEEE 802.1ag.  It's capable of discovering all the
        existing MEPs in a specified VLAN or Ethernet Virtual Connection
        within a specified maintenance domain.  After which, it creates, 
        configures, and schedules an IP SLA operation for each MEP 
        automatically.

        IP SLA currently supports two types of operations for 
        end-to-end Ethernet connectivity - 'ethernetPing' and 
        'ethernetJitter'.

        'ethernetPing' can be used to monitor the connectivity and
        measure RTT by sending the regular 802.1ag loopback frame
        to a particular MEP.

        'ethernetJitter' can be used to measure metrics such as 
        RTT, Jitter, frame loss, one-way latency by sending multiple 
        enhanced CFM frames at specified interval to a particular MEP.

        Without Auto-Ethernet-CFM operation, the two types of operations
        can also be created, configured, and scheduled manually through 
        CISCO-RTTMON-MIB by specifing the target MEP's identifier 
        in addition to the VLAN or Ethernet Virtual Connection and 
        Maintenance Domain.

        With Auto-Ethernet-CFM operation, the two types of operations
        will be created automatically.  The Auto-Ethernet-CFM will pass
        all the values specified in this module to the corresponding 
        objects in CISCO-RTTMON-MIB for each MEP discovered.

           CISCO-IPSLA-ETHERNET-MIB         CISCO-RTTMON-MIB

          ipslaEthernetGrpCtrlTable     -> rttMonCtrlAdminTable
                                       |
                                        -> rttMonEchoAdminTable 

          ipslaEthernetGrpReactTable    -> rttMonReactTable

        The second part defines a collection of statistics resulting 
        from 'ethernetJitter' operation created either manually or 
        automatically.


        Glossary:
          CFM - Connection Fault Management 
          DSAP - Domain Service Access Point: A member of a set of 
              SAPs at which a Maintenance Domain is capable of 
              offering connectivity to systems outside the Maintenance 
              Domain.
          IP SLA - Cisco IOS IP Service Level Agreements
          IP SLA operation - Refers to the 'ethernetPing' or 
              'ethernetJitter' operation supported by IP SLA.  
          MEP - Maintenance association End Point: An actively managed 
              CFM entity, associated with a specific DSAP of a 
              service instance, which can generate and receive CFM 
              PDUs and track any responses.  
          maintenance domain - The network or the part of the network 
              for which faults in connectivity are to be managed.  
              The boundary of a Maintenance Domain is defined by a set 
              of DSAPs, each of which can become a point of connectivity
              to a service instance.
          Maintenance Domain Name - The identifier, unique over the 
              domain for which CFM is to protect against accidental 
              concatenation of service instances, of a particular 
              Maintenance Domain.
          RTT - Round Trip Time
          SAP - Service Access Point at which a service is offered.
          service instance - A service instance is a set of SAPs, 
              selected from among the DSAPs defining a Maintenance 
              Domain, such that a Data.Request primitive presented 
              to one SAP can result in a Data.Indication primitive 
              occurring at one or more of the other SAPs in the set.  
              It corresponds to a VLAN or an Ethernet Virtual Connection.
          TLV - Stands for Type, Length, Value, and denotes a method of
              encoding variable-length and/or optional information in a
              PDU.  TLVs are not aligned to any particular word or octet
              boundary.  TLVs follow each other with no padding between 
              TLVs.
          VLAN - Virtual Local Area Network: A subset of the active 
              topology of a Bridged Local Area Network.  Associated 
              with each VLAN is a VLAN Identifier.

        REFERENCE:
            IEEE 802.1ag Draft 6.0 'Virtual Briged Local Area Networks 
             - Amendments 5: Connectivity Fault Management' July 2006"
    REVISION        "201205150000Z"
    DESCRIPTION
        "Added new object group ciscoIpSlaEthernetY1731Group.

        Added new compliance ciscoIpSlaEthernetComplianceRev3, which
        deprecates ciscoIpSlaEthenetComplianceRev2"
    REVISION        "200801020000Z"
    DESCRIPTION
        "Added object ipslaEthernetGrpCtrlEVC and
        ipslaEthernetGrpCtrlServiceInsType."
    REVISION        "200602080000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 585 }


ciscoIpSlaEthernetMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoIpSlaEthernetMIB 0 }

ciscoIpSlaEthernetMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoIpSlaEthernetMIB 1 }

ipslaEthernetGrpCtrl  OBJECT IDENTIFIER
    ::= { ciscoIpSlaEthernetMIBObjects 1 }

ipslaEthernetStats  OBJECT IDENTIFIER
    ::= { ciscoIpSlaEthernetMIBObjects 2 }

ipslaEthernetLatestOper  OBJECT IDENTIFIER
    ::= { ciscoIpSlaEthernetMIBObjects 3 }


ipslaEthernetGrpCtrlTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IpslaEthernetGrpCtrlEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains Auto-Ethernet-CFM control data.  When a
        row transition to the 'active' state, the IP SLA agent will
        discover all the MEPs inside the specified VLAN and maintenance
        domain and create IP SLA ethernet operations based on the
        value of ipslaEthernetGrpCtrlRttType for each MEP.

        All the values in this table will be passed to the corresponding
        objects in the rttMonCtrlAdminTable and rttMonEchoAdminTable of 
        CISCO-RTTMON-MIB so that each IP SLA Ethernet operation will 
        have the same configuration as specified for Auto-Ethernet-CFM.

        - Objects in this table       - Corresponding objects in 
                                            rttMonCtrlAdminTable
        ipslaEthernetGrpCtrlStatus     rttMonCtrlAdminStatus 
        ipslaEthernetGrpCtrlRttType    rttMonCtrlAdminRttType 
        ipslaEthernetGrpCtrlOwner      rttMonCtrlAdminOwner 
        ipslaEthernetGrpCtrlTag        rttMonCtrlAdminTag 
        ipslaEthernetGrpCtrlThreshold  rttMonCtrlAdminThreshold
        ipslaEthernetGrpCtrlTimeout    rttMonCtrlAdminTimeout 

        - Objects in this table       - Corresponding objects in 
                                            rttMonEchoAdminTable
        ipslaEthernetGrpCtrlVLAN        rttMonEchoAdminTargetVLAN 
        ipslaEthernetGrpCtrlDomainName  rttMonEchoAdminTargetDomainName
        ipslaEthernetGrpCtrlReqDataSize rttMonEchoAdminPktDataRequestSize
        ipslaEthernetGrpCtrlCOS         rttMonEchoAdminEthernetCOS
        ipslaEthernetGrpCtrlInterval   rttMonEchoAdminInterval
        ipslaEthernetGrpCtrlNumFrames  rttMonEchoAdminNumPackets
        ipslaEthernetGrpCtrlEVC        rttMonEchoAdminTargetEVC"
    ::= { ipslaEthernetGrpCtrl 1 }

ipslaEthernetGrpCtrlEntry OBJECT-TYPE
    SYNTAX          IpslaEthernetGrpCtrlEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A collection of objects that define a conceptual
        Auto-Ethernet-CFM control row.

        The following objects must be specified in order to create this 
        conceptual row.
         - ipslaEthernetGrpCtrlStatus
         - ipslaEthernetGrpCtrlRttType

        The following objects must be specified in order to activate this
        conceptual row.
         - ipslaEthernetGrpCtrlVLAN
                    OR
         - ipslaEthernetGrpCtrlEVC

         - ipslaEthernetGrpCtrlDomainName
         - ipslaEthernetGrpSchedulePeriod
         - ipslaEthernetGrpScheduleRttStartTime

        This conceptual row can be delete at any time by set the
        ipslaEthernetGrpCtrlStatus to 'destroy'.  When this row is
        deleted, All the IP SLA operations created by this row will
        be destroyed."
    INDEX           { ipslaEthernetGrpCtrlIndex } 
    ::= { ipslaEthernetGrpCtrlTable 1 }

IpslaEthernetGrpCtrlEntry ::= SEQUENCE {
        ipslaEthernetGrpCtrlIndex            RttMonCtrlIndex,
        ipslaEthernetGrpCtrlStatus           RowStatus,
        ipslaEthernetGrpCtrlStorageType      StorageType,
        ipslaEthernetGrpCtrlRttType          RttMonRttType,
        ipslaEthernetGrpCtrlOwner            SnmpAdminString,
        ipslaEthernetGrpCtrlTag              SnmpAdminString,
        ipslaEthernetGrpCtrlThreshold        Unsigned32,
        ipslaEthernetGrpCtrlTimeout          Unsigned32,
        ipslaEthernetGrpCtrlProbeList        RttMonIdLst,
        ipslaEthernetGrpCtrlVLAN             VlanId,
        ipslaEthernetGrpCtrlDomainNameType   Dot1agCfmMaintDomainNameType,
        ipslaEthernetGrpCtrlDomainName       Dot1agCfmMaintDomainName,
        ipslaEthernetGrpCtrlReqDataSize      Unsigned32,
        ipslaEthernetGrpCtrlMPIDExLst        RttMonIdLst,
        ipslaEthernetGrpCtrlCOS              Layer2Cos,
        ipslaEthernetGrpCtrlInterval         Unsigned32,
        ipslaEthernetGrpCtrlNumFrames        Unsigned32,
        ipslaEthernetGrpScheduleRttStartTime TimeTicks,
        ipslaEthernetGrpSchedulePeriod       Unsigned32,
        ipslaEthernetGrpScheduleFrequency    Unsigned32,
        ipslaEthernetGrpCtrlEVC              SnmpAdminString,
        ipslaEthernetGrpCtrlServiceInsType   INTEGER
}

ipslaEthernetGrpCtrlIndex OBJECT-TYPE
    SYNTAX          RttMonCtrlIndex
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates a row in the ipslaEthernetGrpCtrlTable.

        This value is a pseudo-random number selected by the management
        station when creating a row via the
        ipslaEthernetGrpCtrlStatus object.
        For easy management, user can select range of numbers for
        different maintenance domain.  
        For instance, the ipslaEthernetGrpCtrlIndex 1-100 will be
        used for Domain_A, 101-200 will be used for Domain_B.      

        If the pseudo-random number is already in use an
        'inconsistentValue' return code will be returned when set
        operation is attempted." 
    ::= { ipslaEthernetGrpCtrlEntry 1 }

ipslaEthernetGrpCtrlStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the status of Auto-Ethernet-CFM
        control row.

        Following objects must be specified in order for this object to
        become active.
          - ipslaEthernetGrpCtrlRttType

          - ipslaEthernetGrpCtrlVLAN
                      OR
          - ipslaEthernetGrpCtrlEVC

          - ipslaEthernetGrpCtrlServiceInsType
          - ipslaEthernetGrpCtrlDomainName
          - ipslaEthernetGrpSchedulePeriod
          - ipslaEthernetGrpScheduleRttStartTime
        All other objects can assume default values.

        The following objects cannot be modified after creating the
        Auto-Ethernet-CFM conceptual row.
         - ipslaEthernetGrpCtrlRttType

         - ipslaEthernetGrpCtrlVLAN
                     OR
         - ipslaEthernetGrpCtrlEVC

         - ipslaEthernetGrpCtrlDomainName
         - ipslaEthernetGrpCtrlServiceInsType 

        The following objects can be modified even after creating the
        Auto-Ethernet-CFM conceptual row by setting this object to
        'notInService'
         - All other writable objects in ipslaEthernetGrpCtrlTable except
           ipslaEthernetGrpCtrlRttType, ipslaEthernetGrpCtrlVLAN,
           ipslaEthernetGrpCtrlDomainName, ipslaEthernetGrpCtrlEVC and
           ipslaEthernetGrpCtrlServiceInsType
         - Objects in the ipslaEthernetGrpScheduleTable.

        The following objects can be modified as needed without setting
        this object to 'notInService' even after creating the
        Auto-Ethernet-CFM conceptual row.
         - Objects in ipslaEthernetGrpReactTable.

        This object can be set to 'destroy' from any value at any
        time.  When this object is set to 'destroy' it will stop and
        destroy all the IP SLA operations created by this 
        Auto-Ethernet-CFM before destroying Auto-Ethernet-CFM
        control row." 
    ::= { ipslaEthernetGrpCtrlEntry 2 }

ipslaEthernetGrpCtrlStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies how the SNMP entity stores the data
        contained by the corresponding conceptual row.  

        This object can be set to either 'volatile' or 'nonVolatile'.
        Other values are not applicable for this conceptual row and
        are not supported."
    DEFVAL          { volatile } 
    ::= { ipslaEthernetGrpCtrlEntry 3 }

ipslaEthernetGrpCtrlRttType OBJECT-TYPE
    SYNTAX          RttMonRttType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The type of IP SLA operation to be created by this
        Auto-Ethernet-CFM.

        This value can only be set to type 'ethernetPing' and 
        'ethernetJitter'.

        'ethernetPing' operation sends the regular 802.1ag loopback 
        frame to the target MEP to monitor the connectivity and perform 
        delay analysis.  

        'ethernetJitter'sends multiple enhanced CFM frames at a 
        specified interval to the target MEP to measure metrics such as 
        RTT, jitter, frame loss, one-way latency and so on. 

        This value must be set before setting any other
        parameter configuration of an Auto-Ethernet-CFM." 
    ::= { ipslaEthernetGrpCtrlEntry 4 }

ipslaEthernetGrpCtrlOwner OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..255))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "A string which used by a managing application to identify
        the entity that created this Auto-Ethernet-CFM."
    DEFVAL          { "" } 
    ::= { ipslaEthernetGrpCtrlEntry 5 }

ipslaEthernetGrpCtrlTag OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..255))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "A string which used by a managing application to identify
        the target VLAN and maintenance domain of this 
        Auto-Ethernet-CFM."
    DEFVAL          { "" } 
    ::= { ipslaEthernetGrpCtrlEntry 6 }

ipslaEthernetGrpCtrlThreshold OBJECT-TYPE
    SYNTAX          Unsigned32 (0..2147483647)
    UNITS           "milliseconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the threshold value of a particular
        object.

        This value will be examined for each IP SLA operations
        created by the Auto-Ethernet-CFM.

        For 'ethernetPing', if the value of 
        rttMonLatestRttOperCompletionTime is greater than this
        value, the 'overThreshold' will be reported through
        rttMonLatestRttOperSense defined in CISCO-RTTMON-MIB.

        For 'ethernetJitter', if the value of 
        ipslaEtherJitterLatestAvgJitter value is greater than this
        value, the 'overThreshold' will be reported through
        ipslaEtherJitterLatestSense defined this module."
    DEFVAL          { 5000 } 
    ::= { ipslaEthernetGrpCtrlEntry 7 }

ipslaEthernetGrpCtrlTimeout OBJECT-TYPE
    SYNTAX          Unsigned32 (0..604800000)
    UNITS           "milliseconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Specifies the duration to wait for an IP SLA operation
        created by this Auto-Ethernet-CFM to complete.

        For 'ethernetPing', if the value of 
        rttMonLatestRttOperCompletionTime is greater than this
        value, the 'timeout' will be reported through
        rttMonLatestRttOperSense defined in CISCO-RTTMON-MIB.

        For 'ethernetJitter', if all the frames sent to target MEP
        have not been recievied within this duration, the 'timeout'
        will be reported through ipslaEtherJitterLatestSense 
        defined this module.

        The value of this object cannot be set to a value which would
        specify a duration exceeding ipslaEthernetGrpScheduleFrequency."
    DEFVAL          { 5000 } 
    ::= { ipslaEthernetGrpCtrlEntry 8 }

ipslaEthernetGrpCtrlProbeList OBJECT-TYPE
    SYNTAX          RttMonIdLst
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the identifiers of the IP SLA
        operations that are created by the Auto-Ethernet-CFM.

        The identifier will be stored in rttMonCtrlAdminIndex defined
        in CISCO-RTTMON-MIB for each IP SLA operation." 
    ::= { ipslaEthernetGrpCtrlEntry 9 }

ipslaEthernetGrpCtrlVLAN OBJECT-TYPE
    SYNTAX          VlanId
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the identifier of VLAN for which
        the Auto-Ethernet-CFM operation will be used.

        It is an unique identifier for a service instance within 
        a Maintenance Domain specified by ipslaEthernetGrpCtrlDomainName.

        The Auto-Ethernet-CFM will find all the MEPs participating 
        in this VLAN and create IP SLA operations for each MEP 
        corresponding to value specified in ipslaEthernetGrpCtrlRttType.

        The value of this object is in effect only when the value of
        ipslaEthernetGrpCtrlServiceInsType is set to 'vlan'." 
    ::= { ipslaEthernetGrpCtrlEntry 10 }

ipslaEthernetGrpCtrlDomainNameType OBJECT-TYPE
    SYNTAX          Dot1agCfmMaintDomainNameType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the type of maintenance domain name
        to be used by the Auto-Ethernet-CFM operation.

        This object can only be set to the following values:
          'none'(1) 
          'charString'(4)
        Other values are not supported.
        Value 'none' means that the ipslaEthernetGrpCtrlDomainName
        has not been specified."
    DEFVAL          { none } 
    ::= { ipslaEthernetGrpCtrlEntry 11 }

ipslaEthernetGrpCtrlDomainName OBJECT-TYPE
    SYNTAX          Dot1agCfmMaintDomainName
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the maintenance domain name
        to be used by the Auto-Ethernet-CFM operation.

        The Auto-Ethernet-CFM operation discovers all the MEPs 
        participating in the VLAN specified by ipslaEthernetGrpCtrlVLAN 
        within this maintenance domain and create IP SLA operations 
        for each MEP corresponding to value specified in 
        ipslaEthernetGrpCtrlRttType.

        As long as the value of this object is specified, the value of 
        ipslaEthernetGrpCtrlDomainNameType must be set to 'charString'." 
    ::= { ipslaEthernetGrpCtrlEntry 12 }

ipslaEthernetGrpCtrlReqDataSize OBJECT-TYPE
    SYNTAX          Unsigned32 (0..1400)
    UNITS           "octets"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the padding that needs to be inserted
        into each ethernet frame of the IP SLA operation.

        The total ethernet frame size of the IP SLA operation is:

        CFM_header + TLVs + si_length + dm_length + padding size 

        where dm_length = number of octets of the maintenance domain name
              si_length = number of octets of the service instance name
              CFM_header = 8 octets
              TLVs = 60 octets for 'ethernetPing' 
                     45 octets for 'ethernetJitter' 

        If the total frame size exceeds 1500, only 1500 will be 
        sent to the target MEP."
    DEFVAL          { 0 } 
    ::= { ipslaEthernetGrpCtrlEntry 13 }

ipslaEthernetGrpCtrlMPIDExLst OBJECT-TYPE
    SYNTAX          RttMonIdLst
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the identifiers of the MEPs that will
        be excluded when create IP SLA operations by Auto-Ethernet-CFM
        operation." 
    ::= { ipslaEthernetGrpCtrlEntry 14 }

ipslaEthernetGrpCtrlCOS OBJECT-TYPE
    SYNTAX          Layer2Cos
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the Class Of Service field in an
        Ethernet frame header."
    DEFVAL          { 0 } 
    ::= { ipslaEthernetGrpCtrlEntry 15 }

ipslaEthernetGrpCtrlInterval OBJECT-TYPE
    SYNTAX          Unsigned32 (1..60000)
    UNITS           "milliseconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This value specifies the inter-frame delay between Ethernet
        frames that need to be transmitted to the target MEPs.

        This object is applicable to 'ethernetJitter' operation only."
    DEFVAL          { 20 } 
    ::= { ipslaEthernetGrpCtrlEntry 16 }

ipslaEthernetGrpCtrlNumFrames OBJECT-TYPE
    SYNTAX          Unsigned32 (1..60000)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This value specifies the number of Ethernet frames that need
        to be transmitted to the target MEPs.  

        This object is applicable to 'ethernetJitter' operation only."
    DEFVAL          { 10 } 
    ::= { ipslaEthernetGrpCtrlEntry 17 }

ipslaEthernetGrpScheduleRttStartTime OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the time when this conceptual row
        will become 'active'.  ipslaEthernetGrpSchedulePeriod object 
        must be specified before setting this object.

        When sysUpTime equals this value, this object will
        cause the conceptual Auto-Ethernet-CFM row transmit
        to 'active'and start to discover the existing MEPs.  
        Meanwhile the IP SLA operations will be created for 
        each discovered MEP, and rttMonCtrlAdminStatus of each 
        IP SLA operation will transmit to 'active'.

        If this object has value as 1, the conceptual Auto-Ethernet-CFM 
        row will transmit to 'active' right now.
        Value of 0 puts this conceptual row in pending state."
    DEFVAL          { 0 } 
    ::= { ipslaEthernetGrpCtrlEntry 18 }

ipslaEthernetGrpSchedulePeriod OBJECT-TYPE
    SYNTAX          Unsigned32 (1..604800)
    UNITS           "seconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Specifies the time duration over which all the IP SLA
        operations created by the current Auto-Ethernet-CFM 
        have to be scheduled.

        For instance, if there are three MEPs discovered, there
        will be three IP SLA operations created.  If this object 
        is set to 30, ipslaEthernetGrpScheduleRttStartTime is set 
        to T, the start time of three operations will be
        spreaded evenly within 30 seconds, i.e.  

        start time:    T+0 -------- T+9 ----------T+19
                     operation1  operation2    operation3

        This object must be set first before setting
        ipslaEthernetGrpScheduleRttStartTime." 
    ::= { ipslaEthernetGrpCtrlEntry 19 }

ipslaEthernetGrpScheduleFrequency OBJECT-TYPE
    SYNTAX          Unsigned32 (1..604800)
    UNITS           "seconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Specifies the duration between initiating each IP SLA
        operation created by the Auto-Ethernet-CFM.

        Take above example, if the ipslaEthernetGrpScheduleFrequency
        is set to 60, then the start time of each IP SLA operation
        like:

        start time:      T+0 -------- T+9 ----------T+19-----
                       operation1  operation2    operation3   
        start again:   --T+60-------- T+69 ----------T+79--
                       operation1  operation2    operation3   
        start 3rd time:--T+120-------- T+129 ----------T+139--
                        operation1  operation2    operation3   

        This object cannot be set to a value which would be a
        shorter duration than ipslaEthernetGrpCtrlTimeout.
        The default value of this object is the value set to
        ipslaEthernetGrpSchedulePeriod.  

        This value will be passed to rttMonCtrlAdminFrequency for 
        all the IP SLA operations created by the Auto-Ethernet-CFM." 
    ::= { ipslaEthernetGrpCtrlEntry 20 }

ipslaEthernetGrpCtrlEVC OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..100))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the Ethernet Virtual Connection for which
        the Auto-Ethernet-CFM operation will be used.

        It is an unique identifier for a service instance within 
        a Maintenance Domain specified by ipslaEthernetGrpCtrlDomainName.

        The Auto-Ethernet-CFM will find all the MEPs participating 
        in this Ethernet Virtual Connection and create IP SLA operations for 
        each MEP corresponding to value specified in 
        ipslaEthernetGrpCtrlRttType.

        The value of this object is in effect only when the value of
        ipslaEthernetGrpCtrlServiceInsType is set to 'evc'." 
    ::= { ipslaEthernetGrpCtrlEntry 21 }

ipslaEthernetGrpCtrlServiceInsType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        vlan(1),
                        evc(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the type of service instance to be used
        by the Auto-Ethernet-CFM operation.

        When this object is set to value 'vlan', ipslaEthernetGrpCtrlVLAN
        must be set, and the value of ipslaEthernetGrpCtrlVLAN will be
        used by the Auto-Ethernet-CFM to discover the participating MEPs.

        When this object is set to value 'evc', ipslaEthernetGrpCtrlEVC
        must be set, and the value of ipslaEthernetGrpCtrlEVC will be
        used by the Auto-Ethernet-CFM to discover the participating MEPs." 
    ::= { ipslaEthernetGrpCtrlEntry 22 }
 

-- Auto-Ethernet-CFM Reaction Table

ipslaEthernetGrpReactTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IpslaEthernetGrpReactEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table that contains the reaction configurations for
        Auto-Ethernet-CFM operation.

        The reaction configuration specifies the network perfomance
        parameter needs to be monitored, the threshold for the parameter,
        the type of threshold violation that will trigger a reaction, 
        and how to react upon a threshold being violated.

        This allows for proactive monitoring in an environment where 
        user can be alerted to potential network problems, rather than 
        having to manually examine data.   

        Each conceptual row in ipslaEthernetGrpReactTable corresponds 
        to a reaction configured for a corresponding Auto-Ethernet-CFM
        operation.

        Each Auto-Ethernet-CFM operation can have multiple parameters
        monitored and hence there can be multiple reaction configuration
        rows for a particular Auto-Ethernet-CFM operation.

        The reaction configurations in this table for a particular
        Auto-Ethernet-CFM operation will be passed to the 
        corresponding objects in rttMonReactTable of CISCO-RTTMON-MIB 
        for all the IP SLA operations created by this Auto-Ethernet-CFM.
        This makes the IP SLA operation capable of reacting to certain 
        measured network condition such as long round trip delay, 
        big jitter, etc., by generating a notification to a network 
        management application based on defined thresholds.

        - Objects in this table             - Corresponding objects in
                                              rttMonReactTable
        ipslaEthernetGrpReactConfigIndex      rttMonReactConfigIndex
        ipslaEthernetGrpReactVar              rttMonReactVar
        ipslaEthernetGrpReactThresholdType    rttMonReactThresholdType
        ipslaEthernetGrpReactThresholdRising  rttMonReactThresholdRising
        ipslaEthernetGrpReactThresholdFalling rttMonReactThresholdFalling
        ipslaEthernetGrpReactThresholdCountX  rttMonReactThresholdCountX
        ipslaEthernetGrpReactThresholdCountY  rttMonReactThresholdCountY
        ipslaEthernetGrpReactActionType       rttMonReactActionType
        ipslaEthernetGrpReactStatus           rttMonReactStatus

        This table is coupled with ipslaEthernetGrpCtrlTable.  When an
        entry in the ipslaEthernetGrpCtrlTable is destroyed, the 
        corresponding entries in this table will be destroyed too."
    ::= { ipslaEthernetGrpCtrl 2 }

ipslaEthernetGrpReactEntry OBJECT-TYPE
    SYNTAX          IpslaEthernetGrpReactEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A collection of objects that define a conceptual
        Auto-Ethernet-CFM reaction configuration row.

        In order to create this conceptual row,
        ipslaEthernetGrpReactStatus must be set to 'createAndGo' and 
        ipslaEthernetGrpReactVar must be specified.

        This conceptual row can be deleted at any time by set 
        ipslaEthernetGrpReactStatus to 'destroy'.  When this row is
        deleted, the corresponding reaction configuration of all the 
        IP SLA operations are deleted."
    INDEX           {
                        ipslaEthernetGrpCtrlIndex,
                        ipslaEthernetGrpReactConfigIndex
                    } 
    ::= { ipslaEthernetGrpReactTable 1 }

IpslaEthernetGrpReactEntry ::= SEQUENCE {
        ipslaEthernetGrpReactConfigIndex      RttMonCtrlIndex,
        ipslaEthernetGrpReactStatus           RowStatus,
        ipslaEthernetGrpReactStorageType      StorageType,
        ipslaEthernetGrpReactVar              RttMonReactVar,
        ipslaEthernetGrpReactThresholdType    INTEGER,
        ipslaEthernetGrpReactThresholdRising  Unsigned32,
        ipslaEthernetGrpReactThresholdFalling Unsigned32,
        ipslaEthernetGrpReactThresholdCountX  Unsigned32,
        ipslaEthernetGrpReactThresholdCountY  Unsigned32,
        ipslaEthernetGrpReactActionType       INTEGER
}

ipslaEthernetGrpReactConfigIndex OBJECT-TYPE
    SYNTAX          RttMonCtrlIndex
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object along with ipslaEthernetGrpCtrlEntry identifies
        a particular reaction-configuration for a particular 
        Auto-Ethernet-CFM operation.

        This is a pseudo-random number selected by the management
        station when creating a row via the ipslaEthernetGrpReactStatus.
        If the pseudo-random number is already in use an
        'inconsistentValue' return code will be returned when
        set operation is attempted." 
    ::= { ipslaEthernetGrpReactEntry 1 }

ipslaEthernetGrpReactStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This objects specifies the status of the conceptual
        Auto-Ethernet-CFM reaction control row.  Only 'createAndGo' 
        and 'destroy' operations are permitted on the row.

        In order for this object to become 'active',
        ipslaEthernetGrpReactVar must be defined.
        All other objects assume the default value.

        When this object is in 'active' state, all the writable objects
        except ipslaEthernetGrpReactVar can be modified.

        When this object moves to 'active' state, the rttMonReactStatus
        of the individual IP SLA operations moves to 'active' state, thus
        the performance parameter specified in the reaction configuration
        is monitored for each IP SLA operation and the notifications are 
        generated when the threshold violation takes place.

        This object can be set to 'destroy' from any value at any time.
        When this object is set to 'destroy', the reaction configuration
        of both Auto-Ethernet-CFM operation and IP SLA operations
        are removed." 
    ::= { ipslaEthernetGrpReactEntry 2 }

ipslaEthernetGrpReactStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies how the SNMP entity stores the data
        contained by the corresponding conceptual row.

        This object can be set to either 'volatile' or 'nonVolatile'.
        Other values are not applicable for this conceptual row and
        are not supported."
    DEFVAL          { volatile } 
    ::= { ipslaEthernetGrpReactEntry 3 }

ipslaEthernetGrpReactVar OBJECT-TYPE
    SYNTAX          RttMonReactVar
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the performance parameter that will
        be monitored by the IP SLA operations which are created 
        via Auto-Ethernet-CFM operation.   

        The performance parameters that are valid to both 
        'ethernetJitter' and 'ethernetPing' include:
            - 'connectionLoss'
            - 'rtt'
            - 'timeout'

        The performance parameters that are only valid to 
        'ethernetJitter' include:
            - 'jitterSDAvg'
            - 'jitterDSAvg'
            - 'jitterAvg'
            - 'maxOfPositiveSD'
            - 'maxOfNegativeSD'
            - 'maxOfPositiveDS'
            - 'maxOfNegativeDS'
            - 'packetLateArrival'
            - 'packetLossDS'
            - 'packetLossSD'
            - 'packetOutOfSequence'
            - 'packetMIA'" 
    ::= { ipslaEthernetGrpReactEntry 4 }

ipslaEthernetGrpReactThresholdType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        never(1),
                        immediate(2),
                        consecutive(3),
                        xOfy(4),
                        average(5)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the type of threshold violation that
        will trigger an notification.

        The notification will be sent accordingly only when the object 
        rttMonReactOccurred which is defined in CISCO-RTTMON-MIB for IP 
        SLA operation is set to 'true' or 'false'.


        'never'     - rttMonReactOccurred is never set

        'immediate' - rttMonReactOccurred is set to 'true' when the
                     value of parameter for which reaction is
                     configured ( e.g.  rtt, jitterAvg) violates the 
                     threshold.

                     Conversely, rttMonReactOccurred is set to 'false'
                     when the parameter ( e.g.  rtt, jitterAvg) is below 
                     the threshold limits.

        'consecutive'- rttMonReactOccurred is set to true when the value
                     of parameter for which reaction is configured
                     ( e.g.  rtt, jitterAvg) violates the threshold for 
                     configured consecutive times.

                     Conversely, rttMonReactOccurred is set to false
                     when the value of parameter ( e.g.  rtt, jitterAvg)
                     is below the threshold limits for the same number 
                     of consecutive operations.

        'xOfy'     - rttMonReactOccurred is set to true when x
                     ( as specified by 
                     ipslaEthernetGrpReactThresholdCountX )
                     out of the last y ( as specified by
                     ipslaEthernetGrpReactThresholdCountY ) times the 
                     value of parameter for which the reaction is 
                     configured ( e.g.  rtt, jitterAvg) violates the 
                     threshold.

                     Conversely, it is set to false when x, out of the
                     last y times the value of parameter ( e.g.  rtt, 
                     jitterAvg) is below the threshold limits.

        'average'  - rttMonReactOccurred is set to true when the
                     average (ipslaEthernetGrpReactThresholdCountX 
                     times ) value of parameter for which reaction is
                     configured ( e.g.  rtt, jitterAvg) violates the 
                     threshold condition.

                     Conversely, it is set to false when the average 
                     value of parameter ( e.g.  rtt, jitterAvg)."
    DEFVAL          { never } 
    ::= { ipslaEthernetGrpReactEntry 5 }

ipslaEthernetGrpReactThresholdRising OBJECT-TYPE
    SYNTAX          Unsigned32 (0..2147483647)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the higher threshold limit.
        If the value of monitored parameter ( e.g rtt, jitterAvg, 
        packetLossSD etc ) rises above this limit and if the condition 
        specified in ipslaEthernetGrpReactThresholdType are satisfied, 
        a notification is generated.

        Default value of ipslaEthernetGrpReactThresholdRising for
        'rtt' is 5000.
        'jitterAvg' is 100.
        'jitterSDAvg' is 100.
        'jitterDSAvg' is 100.
        'maxOfPositiveSD' is 10000.
        'maxOfNegativeSD' is 10000.
        'maxOfPositiveDS' is 10000.
        'maxOfNegativeDS' is 10000.
        'packetLossSD' is 10000.
        'packetLossDS' is 10000.
        'packetMIA' is 10000.
        'packetLateArrival' is 10000.
        'packetOutOfSequence' is 10000.

        This object is not applicable if the ipslaEthernetGrpReactVar 
        is 'timeout' or 'connectionLoss'.  For 'timeout' and 
        'connectionLoss', the default value will be 0." 
    ::= { ipslaEthernetGrpReactEntry 6 }

ipslaEthernetGrpReactThresholdFalling OBJECT-TYPE
    SYNTAX          Unsigned32 (0..2147483647)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the lower threshold limit.
        If the value of monitored parameter ( e.g rtt, jitterAvg, 
        packetLossSD etc ) falls below this limit and if the condition 
        specified in ipslaEthernetGrpReactThresholdType are satisfied, 
        a notification is generated.

        Default value of ipslaEthernetGrpReactThresholdFalling for
        'rtt' is 3000.
        'jitterAvg' is 100.
        'jitterSDAvg' is 100.
        'jitterDSAvg' is 100.
        'maxOfPositiveSD' is 10000.
        'maxOfNegativeSD' is 10000.
        'maxOfPositiveDS' is 10000.
        'maxOfNegativeDS' is 10000.
        'packetLossSD' is 10000.
        'packetLossDS' is 10000.
        'packetMIA' is 10000.
        'packetLateArrival' is 10000.
        'packetOutOfSequence' is 10000.

        This object is not applicable if the ipslaEthernetGrpReactVar 
        is 'timeout' or 'connectionLoss'.  For 'timeout' and 
        'connectionLoss', the default value will be 0." 
    ::= { ipslaEthernetGrpReactEntry 7 }

ipslaEthernetGrpReactThresholdCountX OBJECT-TYPE
    SYNTAX          Unsigned32 (1..16)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "If ipslaEthernetGrpReactThresholdType value is 'xOfy', this
        object specifies the 'x' value.

        If ipslaEthernetGrpReactThresholdType value is 'consecutive',
        this object specifies the number of consecutive occurrences
        that needs threshold violation before setting 
        rttMonReactOccurred as 'true'.

        If ipslaEthernetGrpReactThresholdType value is 'average', 
        this object specifies the number of samples that needs be 
        considered for calculating average.  

        This object has no meaning if ipslaEthernetGrpReactThresholdType
        has value of 'never' and 'immediate'."
    DEFVAL          { 5 } 
    ::= { ipslaEthernetGrpReactEntry 8 }

ipslaEthernetGrpReactThresholdCountY OBJECT-TYPE
    SYNTAX          Unsigned32 (1..16)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the 'y' value of the xOfy condition
        if ipslaEthernetGrpReactThresholdType is 'xOfy'.

        For other values of ipslaEthernetGrpReactThresholdType, this 
        object is not applicable."
    DEFVAL          { 5 } 
    ::= { ipslaEthernetGrpReactEntry 9 }

ipslaEthernetGrpReactActionType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        none(1),
                        notification(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies what type of reaction to generate
        if an IP SLA operation violates one of the watched
        conditions (specified in ipslaEthernetGrpReactVar):
            'none'         - no reaction is generated.
            'notification' - a notification is generated."
    DEFVAL          { none } 
    ::= { ipslaEthernetGrpReactEntry 10 }
 

-- LatestEthernetJitterOper Table

ipslaEtherJitterLatestStatsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IpslaEtherJitterLatestStatsEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The 'ethernetJitter' operation sends out frames at the
        frequency specified by rttMonCtrlAdminFrequency.  
        This table contains the statistics calculated for the 
        latest sent frames.

        Each conceptual row in this table corresponds to an 
        'ethernetJitter' operation defined in rttMonCtrlAdminTable 
        and has same index as rttMonCtrlAdminTable."
    ::= { ipslaEthernetLatestOper 1 }

ipslaEtherJitterLatestStatsEntry OBJECT-TYPE
    SYNTAX          IpslaEtherJitterLatestStatsEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A collection of objects that record the latest Ethernet jitter
        operation.

        An entry is created only when the following 
        objects are valid.  
        - rttMonCtrlAdminRttType
        - rttMonEchoAdminProtocol

        The entry will start to collect data when rttMonCtrlAdminStatus 
        is in 'active' state.  The entry will be removed when the 
        rttMonCtrlAdminStatus is changed to 'destroy' state."
    INDEX           { rttMonCtrlAdminIndex } 
    ::= { ipslaEtherJitterLatestStatsTable 1 }

IpslaEtherJitterLatestStatsEntry ::= SEQUENCE {
        ipslaEtherJitterLatestNumRTT     Gauge32,
        ipslaEtherJitterLatestRTTSum     Gauge32,
        ipslaEtherJitterLatestRTTSum2    Gauge32,
        ipslaEtherJitterLatestRTTMin     Gauge32,
        ipslaEtherJitterLatestRTTMax     Gauge32,
        ipslaEtherJitterLatestMinPosSD   Gauge32,
        ipslaEtherJitterLatestMaxPosSD   Gauge32,
        ipslaEtherJitterLatestNumPosSD   Gauge32,
        ipslaEtherJitterLatestSumPosSD   Gauge32,
        ipslaEtherJitterLatestSum2PosSD  Gauge32,
        ipslaEtherJitterLatestMinNegSD   Gauge32,
        ipslaEtherJitterLatestMaxNegSD   Gauge32,
        ipslaEtherJitterLatestNumNegSD   Gauge32,
        ipslaEtherJitterLatestSumNegSD   Gauge32,
        ipslaEtherJitterLatestSum2NegSD  Gauge32,
        ipslaEtherJitterLatestMinPosDS   Gauge32,
        ipslaEtherJitterLatestMaxPosDS   Gauge32,
        ipslaEtherJitterLatestNumPosDS   Gauge32,
        ipslaEtherJitterLatestSumPosDS   Gauge32,
        ipslaEtherJitterLatestSum2PosDS  Gauge32,
        ipslaEtherJitterLatestMinNegDS   Gauge32,
        ipslaEtherJitterLatestMaxNegDS   Gauge32,
        ipslaEtherJitterLatestNumNegDS   Gauge32,
        ipslaEtherJitterLatestSumNegDS   Gauge32,
        ipslaEtherJitterLatestSum2NegDS  Gauge32,
        ipslaEtherJitterLatestFrmLossSD  Gauge32,
        ipslaEtherJitterLatestFrmLossDS  Gauge32,
        ipslaEtherJitterLatestFrmOutSeq  Gauge32,
        ipslaEtherJitterLatestFrmMIA     Gauge32,
        ipslaEtherJitterLatestFrmSkipped Gauge32,
        ipslaEtherJitterLatestSense      RttResponseSense,
        ipslaEtherJitterLatestFrmLateA   Gauge32,
        ipslaEtherJitterLatestMinSucFrmL Gauge32,
        ipslaEtherJitterLatestMaxSucFrmL Gauge32,
        ipslaEtherJitterLatestOWSumSD    Gauge32,
        ipslaEtherJitterLatestOWSum2SD   Gauge32,
        ipslaEtherJitterLatestOWMinSD    Gauge32,
        ipslaEtherJitterLatestOWMaxSD    Gauge32,
        ipslaEtherJitterLatestOWSumDS    Gauge32,
        ipslaEtherJitterLatestOWSum2DS   Gauge32,
        ipslaEtherJitterLatestOWMinDS    Gauge32,
        ipslaEtherJitterLatestOWMaxDS    Gauge32,
        ipslaEtherJitterLatestNumOW      Gauge32,
        ipslaEtherJitterLatestAvgJitter  Gauge32,
        ipslaEtherJitterLatestAvgSDJ     Gauge32,
        ipslaEtherJitterLatestAvgDSJ     Gauge32,
        ipslaEtherJitterLatestOWAvgSD    Gauge32,
        ipslaEtherJitterLatestOWAvgDS    Gauge32,
        ipslaEtherJitterLatestIAJOut     Gauge32,
        ipslaEtherJitterLatestIAJIn      Gauge32,
        ipslaEtherJLatestFrmUnProcessed  Gauge32
}

ipslaEtherJitterLatestNumRTT OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of RTT's that were successfully measured." 
    ::= { ipslaEtherJitterLatestStatsEntry 1 }

ipslaEtherJitterLatestRTTSum OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of RTT's that are successfully measured.
        The number of successfully measured RTT is 
        stored in ipslaEtherJitterLatestNumRTT." 
    ::= { ipslaEtherJitterLatestStatsEntry 2 }

ipslaEtherJitterLatestRTTSum2 OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of RTT's that are successfully measured." 
    ::= { ipslaEtherJitterLatestStatsEntry 3 }

ipslaEtherJitterLatestRTTMin OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of RTT's that were successfully measured." 
    ::= { ipslaEtherJitterLatestStatsEntry 4 }

ipslaEtherJitterLatestRTTMax OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of RTT's that were successfully measured." 
    ::= { ipslaEtherJitterLatestStatsEntry 5 }

ipslaEtherJitterLatestMinPosSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of all positive jitter values for frames sent
        from source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 6 }

ipslaEtherJitterLatestMaxPosSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of all positive jitter values for frames sent
        from source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 7 }

ipslaEtherJitterLatestNumPosSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "occurrences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of all positive jitter values for frames
        sent from source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 8 }

ipslaEtherJitterLatestSumPosSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of all positive jitter values for frames sent
        source to destination.  The number of such values
        is stored in ipslaEtherJitterLatestNumPosSD." 
    ::= { ipslaEtherJitterLatestStatsEntry 9 }

ipslaEtherJitterLatestSum2PosSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of square of all positive jitter values for
        frames sent from source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 10 }

ipslaEtherJitterLatestMinNegSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of absolute values of all negative jitter values
        for frames sent from source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 11 }

ipslaEtherJitterLatestMaxNegSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of absolute values of all negative jitter values
        for frames sent from source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 12 }

ipslaEtherJitterLatestNumNegSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "occurrences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of all negative jitter values for frames
        sent from source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 13 }

ipslaEtherJitterLatestSumNegSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of all negative jitter values for frames sent
        from source to destination.  The number of such values
        is stored in ipslaEtherJitterLatestNumNegSD." 
    ::= { ipslaEtherJitterLatestStatsEntry 14 }

ipslaEtherJitterLatestSum2NegSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of square of all negative jitter values for
        frames sent from source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 15 }

ipslaEtherJitterLatestMinPosDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of all positive jitter values for frames sent
        from destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 16 }

ipslaEtherJitterLatestMaxPosDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of all positive jitter values for frames sent
        from destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 17 }

ipslaEtherJitterLatestNumPosDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "occurrences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of all positive jitter values for frames
        sent from destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 18 }

ipslaEtherJitterLatestSumPosDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of all positive jitter values for frames sent
        from destination to source.  The number of such values
        is stored in ipslaEtherJitterLatestNumPosDS." 
    ::= { ipslaEtherJitterLatestStatsEntry 19 }

ipslaEtherJitterLatestSum2PosDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of all positive jitter values for
        frames sent from destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 20 }

ipslaEtherJitterLatestMinNegDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of all negative jitter values for frames sent
        from destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 21 }

ipslaEtherJitterLatestMaxNegDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of all negative jitter values for frames sent
        from destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 22 }

ipslaEtherJitterLatestNumNegDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "occurrences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of all negative jitter values for frames
        sent from destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 23 }

ipslaEtherJitterLatestSumNegDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of all negative jitter values for frames sent
        from destination to source.  The number of such values
        is stored in ipslaEtherJitterLatestNumNegDS." 
    ::= { ipslaEtherJitterLatestStatsEntry 24 }

ipslaEtherJitterLatestSum2NegDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of all negative jitter values for
        frames sent from destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 25 }

ipslaEtherJitterLatestFrmLossSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of frames lost when sent from source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 26 }

ipslaEtherJitterLatestFrmLossDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of frames lost when sent from destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 27 }

ipslaEtherJitterLatestFrmOutSeq OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of frames arrived out of sequence." 
    ::= { ipslaEtherJitterLatestStatsEntry 28 }

ipslaEtherJitterLatestFrmMIA OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of frames that are lost for which we cannot determine
        the direction." 
    ::= { ipslaEtherJitterLatestStatsEntry 29 }

ipslaEtherJitterLatestFrmSkipped OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of frames in the operation that could not be
        initiated due to an internal error." 
    ::= { ipslaEtherJitterLatestStatsEntry 30 }

ipslaEtherJitterLatestSense OBJECT-TYPE
    SYNTAX          RttResponseSense
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "An application specific sense code for the completion status." 
    ::= { ipslaEtherJitterLatestStatsEntry 31 }

ipslaEtherJitterLatestFrmLateA OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of frames that arrived after the timeout." 
    ::= { ipslaEtherJitterLatestStatsEntry 32 }

ipslaEtherJitterLatestMinSucFrmL OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum number of frames that are dropped
        successively." 
    ::= { ipslaEtherJitterLatestStatsEntry 33 }

ipslaEtherJitterLatestMaxSucFrmL OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum number of frames that are dropped
        successively." 
    ::= { ipslaEtherJitterLatestStatsEntry 34 }

ipslaEtherJitterLatestOWSumSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of one way trip time from source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 35 }

ipslaEtherJitterLatestOWSum2SD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of one way trip time from source to
        destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 36 }

ipslaEtherJitterLatestOWMinSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of all one way trip time from
        source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 37 }

ipslaEtherJitterLatestOWMaxSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of all one way trip time from
        source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 38 }

ipslaEtherJitterLatestOWSumDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of one way trip time from destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 39 }

ipslaEtherJitterLatestOWSum2DS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of one way trip time from
        destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 40 }

ipslaEtherJitterLatestOWMinDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of all one way trip time from
        destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 41 }

ipslaEtherJitterLatestOWMaxDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of all one way trip time from
        destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 42 }

ipslaEtherJitterLatestNumOW OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of successful one way trip time measurements." 
    ::= { ipslaEtherJitterLatestStatsEntry 43 }

ipslaEtherJitterLatestAvgJitter OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The average of positive and negative jitter values
        in Source-to-Destination and Destination-to-Source
        direction." 
    ::= { ipslaEtherJitterLatestStatsEntry 44 }

ipslaEtherJitterLatestAvgSDJ OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The average of positive and negative jitter values
        from source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 45 }

ipslaEtherJitterLatestAvgDSJ OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The average of positive and negative jitter values
        from destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 46 }

ipslaEtherJitterLatestOWAvgSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The average one way trip time from source to destination." 
    ::= { ipslaEtherJitterLatestStatsEntry 47 }

ipslaEtherJitterLatestOWAvgDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The average one way trip time from destination to source." 
    ::= { ipslaEtherJitterLatestStatsEntry 48 }

ipslaEtherJitterLatestIAJOut OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Inter-arrival jitter (RFC 1889) at responder."
    REFERENCE
        "Refer to the following documents for the definition: 
               RFC 1889, Section 6.3.1" 
    ::= { ipslaEtherJitterLatestStatsEntry 49 }

ipslaEtherJitterLatestIAJIn OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Inter-arrival jitter (RFC 1889) at source."
    REFERENCE
        "Refer to the following documents for the definition: 
               RFC 1889, Section 6.3.1" 
    ::= { ipslaEtherJitterLatestStatsEntry 50 }

ipslaEtherJLatestFrmUnProcessed OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of frames in the operation that could not be
        processed due to high CPU load." 
    ::= { ipslaEtherJitterLatestStatsEntry 51 }
 

-- Ethernet Jitter Statistics Table

ipslaEtherJitterAggStatsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IpslaEtherJitterAggStatsEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The 'ethernetJitter' statistics table contains summarized
        information of the results for a conceptual control
        row.  A rolling accumulated history of this information
        is maintained in a series of hourly 'group(s)'.

        When ipslaEtherJAggStatsStartTimeId groups exceeds 
        the rttMonStatisticsAdminNumHourGroups value, the 
        oldest corresponding hourly group will be deleted and will 
        be replaced with the new ipslaEtherJAggStatsStartTimeId 
        hourly group."
    ::= { ipslaEthernetStats 1 }

ipslaEtherJitterAggStatsEntry OBJECT-TYPE
    SYNTAX          IpslaEtherJitterAggStatsEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry contains the objects which accumulate the
        results of a series of 'ethernetJitter' operations
        over a 60 minute time period or a time period stored
        in rttMonScheduleAdminRttLife, whichever is smaller.

        An entry is created only if when the following
        objects are valid.
        - rttMonCtrlAdminRttType
        - rttMonEchoAdminProtocol

        The entry will start to collect data when rttMonCtrlAdminStatus
        is in 'active' state.  The entry will be removed when the
        rttMonCtrlAdminStatus is changed to 'destroy' state."
    INDEX           {
                        rttMonCtrlAdminIndex,
                        ipslaEtherJAggStatsStartTimeId
                    } 
    ::= { ipslaEtherJitterAggStatsTable 1 }

IpslaEtherJitterAggStatsEntry ::= SEQUENCE {
        ipslaEtherJAggStatsStartTimeId                       TimeStamp,
        ipslaEtherJAggMeasuredCmpletions                     Counter32,
        ipslaEtherJAggMeasuredOvThrshlds                     Counter32,
        ipslaEtherJAggMeasuredNumRTTs                        Counter32,
        ipslaEtherJAggMeasuredRTTSums                        Counter32,
        ipslaEtherJAggMeasuredRTTSum2Ls                      Counter32,
        ipslaEtherJAggMeasuredRTTSum2Hs                      Counter32,
        ipslaEtherJAggMeasuredRTTMin                         Gauge32,
        ipslaEtherJAggMeasuredRTTMax                         Gauge32,
        ipslaEtherJAggMeasuredMinPosSD                       Gauge32,
        ipslaEtherJAggMeasuredMaxPosSD                       Gauge32,
        ipslaEtherJAggMeasuredNumPosSDs                      Counter32,
        ipslaEtherJAggMeasuredSumPosSDs                      Counter32,
        ipslaEtherJAggMeasuredSum2PSDLs                      Counter32,
        ipslaEtherJAggMeasuredSum2PSDHs                      Counter32,
        ipslaEtherJAggMeasuredMinNegSD                       Gauge32,
        ipslaEtherJAggMeasuredMaxNegSD                       Gauge32,
        ipslaEtherJAggMeasuredNumNegSDs                      Counter32,
        ipslaEtherJAggMeasuredSumNegSDs                      Counter32,
        ipslaEtherJAggMeasuredSum2NSDLs                      Counter32,
        ipslaEtherJAggMeasuredSum2NSDHs                      Counter32,
        ipslaEtherJAggMeasuredMinPosDS                       Gauge32,
        ipslaEtherJAggMeasuredMaxPosDS                       Gauge32,
        ipslaEtherJAggMeasuredNumPosDSes                     Counter32,
        ipslaEtherJAggMeasuredSumPosDSes                     Counter32,
        ipslaEtherJAggMeasuredSum2PDSLs                      Counter32,
        ipslaEtherJAggMeasuredSum2PDSHs                      Counter32,
        ipslaEtherJAggMeasuredMinNegDS                       Gauge32,
        ipslaEtherJAggMeasuredMaxNegDS                       Gauge32,
        ipslaEtherJAggMeasuredNumNegDSes                     Counter32,
        ipslaEtherJAggMeasuredSumNegDSes                     Counter32,
        ipslaEtherJAggMeasuredSum2NDSLs                      Counter32,
        ipslaEtherJAggMeasuredSum2NDSHs                      Counter32,
        ipslaEtherJAggMeasuredFrmLossSDs                     Counter32,
        ipslaEtherJAggMeasuredFrmLssDSes                     Counter32,
        ipslaEtherJAggMeasuredFrmOutSeqs                     Counter32,
        ipslaEtherJAggMeasuredFrmMIAes                       Counter32,
        ipslaEtherJAggMeasuredFrmSkippds                     Counter32,
        ipslaEtherJAggMeasuredErrors                         Counter32,
        ipslaEtherJAggMeasuredBusies                         Counter32,
        ipslaEtherJAggMeasuredOWSumSDs                       Counter32,
        ipslaEtherJAggMeasuredOWSum2SDLs                     Counter32,
        ipslaEtherJAggMeasuredOWSum2SDHs                     Counter32,
        ipslaEtherJAggMeasuredOWMinSD                        Gauge32,
        ipslaEtherJAggMeasuredOWMaxSD                        Gauge32,
        ipslaEtherJAggMeasuredOWSumDSes                      Counter32,
        ipslaEtherJAggMeasuredOWSum2DSLs                     Counter32,
        ipslaEtherJAggMeasuredOWSum2DSHs                     Counter32,
        ipslaEtherJAggMeasuredOWMinDS                        Gauge32,
        ipslaEtherJAggMeasuredOWMaxDS                        Gauge32,
        ipslaEtherJAggMeasuredNumOWs                         Counter32,
        ipslaEtherJAggMeasuredAvgJ                           Gauge32,
        ipslaEtherJAggMeasuredAvgJSD                         Gauge32,
        ipslaEtherJAggMeasuredAvgJDS                         Gauge32,
        ipslaEtherJAggMinSucFrmLoss                          Gauge32,
        ipslaEtherJAggMaxSucFrmLoss                          Gauge32,
        ipslaEtherJAggMeasuredIAJOut                         Gauge32,
        ipslaEtherJAggMeasuredIAJIn                          Gauge32,
        ipslaEtherJAggMeasuredFrmLateAs                      Counter32,
        ipslaEtherJAggMeasuredFrmUnPrcds                     Counter32,
        ipslaEtherJAggMeasuredMaxPosTW                       Gauge32,
        ipslaEtherJAggMeasuredMaxNegTW                       Gauge32,
        ipslaEtherJAggMeasuredMinPosTW                       Gauge32,
        ipslaEtherJAggMeasuredMinNegTW                       Gauge32,
        ipslaEtherJAggMeasuredTxFrmsSD                       Counter64,
        ipslaEtherJAggMeasuredTxFrmsDS                       Counter64,
        ipslaEtherJAggMeasuredRxFrmsSD                       Counter64,
        ipslaEtherJAggMeasuredRxFrmsDS                       Counter64,
        ipslaEtherJAggMeasuredMinLossNumeratorSD             Gauge32,
        ipslaEtherJAggMeasuredMinLossDenominatorSD           Gauge32,
        ipslaEtherJAggMeasuredMaxLossNumeratorSD             Gauge32,
        ipslaEtherJAggMeasuredMaxLossDenominatorSD           Gauge32,
        ipslaEtherJAggMeasuredAvgLossNumeratorSD             Gauge32,
        ipslaEtherJAggMeasuredAvgLossDenominatorSD           Gauge32,
        ipslaEtherJAggMeasuredMinLossNumeratorDS             Gauge32,
        ipslaEtherJAggMeasuredMinLossDenominatorDS           Gauge32,
        ipslaEtherJAggMeasuredMaxLossNumeratorDS             Gauge32,
        ipslaEtherJAggMeasuredMaxLossDenominatorDS           Gauge32,
        ipslaEtherJAggMeasuredAvgLossNumeratorDS             Gauge32,
        ipslaEtherJAggMeasuredAvgLossDenominatorDS           Gauge32,
        ipslaEtherJAggMeasuredCumulativeLossNumeratorSD      Gauge32,
        ipslaEtherJAggMeasuredCumulativeLossDenominatorSD    Gauge32,
        ipslaEtherJAggMeasuredCumulativeAvgLossNumeratorSD   Gauge32,
        ipslaEtherJAggMeasuredCumulativeAvgLossDenominatorSD Gauge32,
        ipslaEtherJAggMeasuredCumulativeLossNumeratorDS      Gauge32,
        ipslaEtherJAggMeasuredCumulativeLossDenominatorDS    Gauge32,
        ipslaEtherJAggMeasuredCumulativeAvgLossNumeratorDS   Gauge32,
        ipslaEtherJAggMeasuredCumulativeAvgLossDenominatorDS Gauge32
}

ipslaEtherJAggStatsStartTimeId OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The value of sysUpTime at the time when this
        row was created." 
    ::= { ipslaEtherJitterAggStatsEntry 1 }

ipslaEtherJAggMeasuredCmpletions OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "completions"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of Ethernet jitter operations that have completed
        successfully." 
    ::= { ipslaEtherJitterAggStatsEntry 2 }

ipslaEtherJAggMeasuredOvThrshlds OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "operations"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of Ethernet jitter operations that violate
        jitterAvg threshold which is defined in RttMonReactVar." 
    ::= { ipslaEtherJitterAggStatsEntry 3 }

ipslaEtherJAggMeasuredNumRTTs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of RTTs that are successfully measured." 
    ::= { ipslaEtherJitterAggStatsEntry 4 }

ipslaEtherJAggMeasuredRTTSums OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of RTTs that are successfully measured for this
        ipslaEtherJAggMeasuredStartTimeId hourly group.  The number
        of the successfully measured RTT is stored in the
        ipslaEtherJAggMeasuredNumRTTs." 
    ::= { ipslaEtherJitterAggStatsEntry 5 }

ipslaEtherJAggMeasuredRTTSum2Ls OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of RTTs that are successfully measured
        (low order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 6 }

ipslaEtherJAggMeasuredRTTSum2Hs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of RTTs that are successfully measured
        (high order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 7 }

ipslaEtherJAggMeasuredRTTMin OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of RTTs that were successfully measured." 
    ::= { ipslaEtherJitterAggStatsEntry 8 }

ipslaEtherJAggMeasuredRTTMax OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of RTTs that were successfully measured." 
    ::= { ipslaEtherJitterAggStatsEntry 9 }

ipslaEtherJAggMeasuredMinPosSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of absolute values of all positive jitter values
        for frames sent from source to destination." 
    ::= { ipslaEtherJitterAggStatsEntry 10 }

ipslaEtherJAggMeasuredMaxPosSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of absolute values of all positive jitter values
        for frames sent from source to destination." 
    ::= { ipslaEtherJitterAggStatsEntry 11 }

ipslaEtherJAggMeasuredNumPosSDs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "occurrences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of all positive jitter values for frames
        sent from source to destination." 
    ::= { ipslaEtherJitterAggStatsEntry 12 }

ipslaEtherJAggMeasuredSumPosSDs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of all positive jitter values for frames sent
        from source to destination.  The number of such values
        is stored in ipslaEtherJAggMeasuredNumPosSDs." 
    ::= { ipslaEtherJitterAggStatsEntry 13 }

ipslaEtherJAggMeasuredSum2PSDLs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of square of all positive jitter values for frames
        sent from source to destination (low order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 14 }

ipslaEtherJAggMeasuredSum2PSDHs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of square of all positive jitter values for frames
        sent from source to destination (high order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 15 }

ipslaEtherJAggMeasuredMinNegSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of all negative jitter values for frames sent
        from source to destination." 
    ::= { ipslaEtherJitterAggStatsEntry 16 }

ipslaEtherJAggMeasuredMaxNegSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of all negative jitter values for frames sent
        from source to destination." 
    ::= { ipslaEtherJitterAggStatsEntry 17 }

ipslaEtherJAggMeasuredNumNegSDs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "occurrences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of all negative jitter values for frames
        sent from source to destination." 
    ::= { ipslaEtherJitterAggStatsEntry 18 }

ipslaEtherJAggMeasuredSumNegSDs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of all negative jitter values for frames sent
        from source to destination.  The number of such values
        is stored in ipslaEtherJAggMeasuredNumNegSDs." 
    ::= { ipslaEtherJitterAggStatsEntry 19 }

ipslaEtherJAggMeasuredSum2NSDLs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of square of all negative jitter values for
        frames sent from source to destination (low order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 20 }

ipslaEtherJAggMeasuredSum2NSDHs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of square of all negative jitter values for
        frames sent from source to destination (high order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 21 }

ipslaEtherJAggMeasuredMinPosDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of all positive jitter values for frames sent
        from destination to source." 
    ::= { ipslaEtherJitterAggStatsEntry 22 }

ipslaEtherJAggMeasuredMaxPosDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of all positive jitter values for frames sent
        from destination to source." 
    ::= { ipslaEtherJitterAggStatsEntry 23 }

ipslaEtherJAggMeasuredNumPosDSes OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "occurrences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of all positive jitter values for frames
        sent from destination to source." 
    ::= { ipslaEtherJitterAggStatsEntry 24 }

ipslaEtherJAggMeasuredSumPosDSes OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of all positive jitter values for frames sent
        from destination to source.  The number of such values
        is stored in ipslaEtherJAggMeasuredNumPosDSes." 
    ::= { ipslaEtherJitterAggStatsEntry 25 }

ipslaEtherJAggMeasuredSum2PDSLs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of all positive jitter values for
        frames sent from destination to source (low order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 26 }

ipslaEtherJAggMeasuredSum2PDSHs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of all positive jitter values for
        frames sent from destination to source (high order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 27 }

ipslaEtherJAggMeasuredMinNegDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of all negative jitter values for frames sent
        from destination to source." 
    ::= { ipslaEtherJitterAggStatsEntry 28 }

ipslaEtherJAggMeasuredMaxNegDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of all negative jitter values for frames sent
        from destination to source." 
    ::= { ipslaEtherJitterAggStatsEntry 29 }

ipslaEtherJAggMeasuredNumNegDSes OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "occurrences"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of all negative jitter values for frames
        sent from destination to source." 
    ::= { ipslaEtherJitterAggStatsEntry 30 }

ipslaEtherJAggMeasuredSumNegDSes OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of all negative jitter values for frames sent
        from destination to source.  The number of such values
        is stored in ipslaEtherJAggMeasuredNumNegDSes." 
    ::= { ipslaEtherJitterAggStatsEntry 31 }

ipslaEtherJAggMeasuredSum2NDSLs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of all negative jitter values for
        frames sent from destination to source (low order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 32 }

ipslaEtherJAggMeasuredSum2NDSHs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of all negative jitter values for
        frames sent from destination to source (high order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 33 }

ipslaEtherJAggMeasuredFrmLossSDs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of lost frames when sent from source to destination." 
    ::= { ipslaEtherJitterAggStatsEntry 34 }

ipslaEtherJAggMeasuredFrmLssDSes OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of lost frames when sent from destination to source." 
    ::= { ipslaEtherJitterAggStatsEntry 35 }

ipslaEtherJAggMeasuredFrmOutSeqs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of frames arrived out of sequence." 
    ::= { ipslaEtherJitterAggStatsEntry 36 }

ipslaEtherJAggMeasuredFrmMIAes OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of frames that are lost for which we cannot determine
        the direction." 
    ::= { ipslaEtherJitterAggStatsEntry 37 }

ipslaEtherJAggMeasuredFrmSkippds OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of frames that are skipped per operation because
        the router could not send the packet out." 
    ::= { ipslaEtherJitterAggStatsEntry 38 }

ipslaEtherJAggMeasuredErrors OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "errors"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of occasions when an Ethernet jitter operation could
        not be initiated because of an internal error." 
    ::= { ipslaEtherJitterAggStatsEntry 39 }

ipslaEtherJAggMeasuredBusies OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "busies"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of occasions when an Ethernet jitter operation could
        not be initiated because a previous Ethernet jitter operation 
        has not been completed." 
    ::= { ipslaEtherJitterAggStatsEntry 40 }

ipslaEtherJAggMeasuredOWSumSDs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of one way trip time from source to destination." 
    ::= { ipslaEtherJitterAggStatsEntry 41 }

ipslaEtherJAggMeasuredOWSum2SDLs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of one way trip time from source to
        destination (low order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 42 }

ipslaEtherJAggMeasuredOWSum2SDHs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of one way trip time from source to
        destination (high order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 43 }

ipslaEtherJAggMeasuredOWMinSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of all one way trip time from source to
        destination." 
    ::= { ipslaEtherJitterAggStatsEntry 44 }

ipslaEtherJAggMeasuredOWMaxSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of all one way trip time from source to
        destination." 
    ::= { ipslaEtherJitterAggStatsEntry 45 }

ipslaEtherJAggMeasuredOWSumDSes OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of one way trip time from destination to source." 
    ::= { ipslaEtherJitterAggStatsEntry 46 }

ipslaEtherJAggMeasuredOWSum2DSLs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of one way trip time from destination
        to source (low order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 47 }

ipslaEtherJAggMeasuredOWSum2DSHs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The sum of squares of one way trip time from destination
        to source (high order 32 bits)." 
    ::= { ipslaEtherJitterAggStatsEntry 48 }

ipslaEtherJAggMeasuredOWMinDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum of all one way trip time from destination
        to source." 
    ::= { ipslaEtherJitterAggStatsEntry 49 }

ipslaEtherJAggMeasuredOWMaxDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum of all one way trip time from destination
        to source." 
    ::= { ipslaEtherJitterAggStatsEntry 50 }

ipslaEtherJAggMeasuredNumOWs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of one way trip time that are successfully
        measured." 
    ::= { ipslaEtherJitterAggStatsEntry 51 }

ipslaEtherJAggMeasuredAvgJ OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The average of positive and negative jitter
        values for source-to-destination and 
        destination-to-source direction." 
    ::= { ipslaEtherJitterAggStatsEntry 52 }

ipslaEtherJAggMeasuredAvgJSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The average of positive and negative jitter
        values in source-to-destination direction." 
    ::= { ipslaEtherJitterAggStatsEntry 53 }

ipslaEtherJAggMeasuredAvgJDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The average of positive and negative jitter
        values in destination-to-source direction." 
    ::= { ipslaEtherJitterAggStatsEntry 54 }

ipslaEtherJAggMinSucFrmLoss OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The minimum number of frames that are dropped
        successively." 
    ::= { ipslaEtherJitterAggStatsEntry 55 }

ipslaEtherJAggMaxSucFrmLoss OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum number of frames that are dropped
        successively." 
    ::= { ipslaEtherJitterAggStatsEntry 56 }

ipslaEtherJAggMeasuredIAJOut OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Inter-arrival jitter (RFC 1889) at responder"
    REFERENCE
        "Refer to the following documents for the definition: 
               RFC 1889, Section 6.3.1" 
    ::= { ipslaEtherJitterAggStatsEntry 57 }

ipslaEtherJAggMeasuredIAJIn OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Inter-arrival jitter (RFC 1889) at sender"
    REFERENCE
        "Refer to the following documents for the definition: 
               RFC 1889, Section 6.3.1" 
    ::= { ipslaEtherJitterAggStatsEntry 58 }

ipslaEtherJAggMeasuredFrmLateAs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of frames that arrived after the timeout." 
    ::= { ipslaEtherJitterAggStatsEntry 59 }

ipslaEtherJAggMeasuredFrmUnPrcds OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of frames that arrived but could not be
        processed due to the internal error." 
    ::= { ipslaEtherJitterAggStatsEntry 60 }

ipslaEtherJAggMeasuredMaxPosTW OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "microseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The two-way maximum of all positive jitter values for
        frames." 
    ::= { ipslaEtherJitterAggStatsEntry 61 }

ipslaEtherJAggMeasuredMaxNegTW OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "microseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The two-way maximum of all negative jitter values for
        frames." 
    ::= { ipslaEtherJitterAggStatsEntry 62 }

ipslaEtherJAggMeasuredMinPosTW OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "microseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The two-way minimum of all positive jitter values for
        frames." 
    ::= { ipslaEtherJitterAggStatsEntry 63 }

ipslaEtherJAggMeasuredMinNegTW OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "microseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The two-way minimum of all negative jitter values for
        frames." 
    ::= { ipslaEtherJitterAggStatsEntry 64 }

ipslaEtherJAggMeasuredTxFrmsSD OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of data frames sent from source to
        destination." 
    ::= { ipslaEtherJitterAggStatsEntry 65 }

ipslaEtherJAggMeasuredTxFrmsDS OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of data frames sent from destination to
        source." 
    ::= { ipslaEtherJitterAggStatsEntry 66 }

ipslaEtherJAggMeasuredRxFrmsSD OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of data frames received from source to
        destination." 
    ::= { ipslaEtherJitterAggStatsEntry 67 }

ipslaEtherJAggMeasuredRxFrmsDS OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of data frames received from destination to
        source." 
    ::= { ipslaEtherJitterAggStatsEntry 68 }

ipslaEtherJAggMeasuredMinLossNumeratorSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The numerator for the minimum loss ratio recorded in
        the source to destination direction." 
    ::= { ipslaEtherJitterAggStatsEntry 69 }

ipslaEtherJAggMeasuredMinLossDenominatorSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The denominator for the minimum loss ratio recorded in
        the source to destination direction." 
    ::= { ipslaEtherJitterAggStatsEntry 70 }

ipslaEtherJAggMeasuredMaxLossNumeratorSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The numerator for the maximum loss ratio recorded in
        the source to destination direction." 
    ::= { ipslaEtherJitterAggStatsEntry 71 }

ipslaEtherJAggMeasuredMaxLossDenominatorSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The denominator for the maximum loss ratio recorded in
        the source to destination direction." 
    ::= { ipslaEtherJitterAggStatsEntry 72 }

ipslaEtherJAggMeasuredAvgLossNumeratorSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The numerator for the average loss ratio recorded in
        the source to destination direction." 
    ::= { ipslaEtherJitterAggStatsEntry 73 }

ipslaEtherJAggMeasuredAvgLossDenominatorSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The denominator for the average loss ratio recorded in
        the source to destination direction." 
    ::= { ipslaEtherJitterAggStatsEntry 74 }

ipslaEtherJAggMeasuredMinLossNumeratorDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The numerator for the minimum loss ratio recorded in
        the destination to source direction." 
    ::= { ipslaEtherJitterAggStatsEntry 75 }

ipslaEtherJAggMeasuredMinLossDenominatorDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The denominator for the minimum loss ratio recorded in
        the destination to source direction." 
    ::= { ipslaEtherJitterAggStatsEntry 76 }

ipslaEtherJAggMeasuredMaxLossNumeratorDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The numerator for the maximum loss ratio recorded in
        the destination to source direction." 
    ::= { ipslaEtherJitterAggStatsEntry 77 }

ipslaEtherJAggMeasuredMaxLossDenominatorDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The denominator for the maximum loss ratio recorded in
        the destination to source direction." 
    ::= { ipslaEtherJitterAggStatsEntry 78 }

ipslaEtherJAggMeasuredAvgLossNumeratorDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The numerator for the average loss ratio recorded in
        the destination to source direction." 
    ::= { ipslaEtherJitterAggStatsEntry 79 }

ipslaEtherJAggMeasuredAvgLossDenominatorDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The denominator for the average loss ratio recorded in
        the destination to source direction." 
    ::= { ipslaEtherJitterAggStatsEntry 80 }

ipslaEtherJAggMeasuredCumulativeLossNumeratorSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The numerator for the loss ratio recorded in
        the source to destination direction.  This value is  
        cumulative over the period of this interval." 
    ::= { ipslaEtherJitterAggStatsEntry 81 }

ipslaEtherJAggMeasuredCumulativeLossDenominatorSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The denominator for the loss ratio recorded in
        the source to destination direction.  This value is 
        cumulative over the period of this interval." 
    ::= { ipslaEtherJitterAggStatsEntry 82 }

ipslaEtherJAggMeasuredCumulativeAvgLossNumeratorSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The numerator for the average loss ratio recorded in
        the source to destination direction.  This value is 
        cumulative over the perios of this interval." 
    ::= { ipslaEtherJitterAggStatsEntry 83 }

ipslaEtherJAggMeasuredCumulativeAvgLossDenominatorSD OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The denominator for the average loss ratio recorded in
        the source to destination direction.  This value is 
        cumulative over the period of this interval." 
    ::= { ipslaEtherJitterAggStatsEntry 84 }

ipslaEtherJAggMeasuredCumulativeLossNumeratorDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The numerator for the loss ratio recorded in
        the destination to source direction.  This value is 
        cumulative over the period of this interval." 
    ::= { ipslaEtherJitterAggStatsEntry 85 }

ipslaEtherJAggMeasuredCumulativeLossDenominatorDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The denominator for the loss ratio recorded in
        the destination to source direction.  This valued is 
        cumulative over the period of this interval." 
    ::= { ipslaEtherJitterAggStatsEntry 86 }

ipslaEtherJAggMeasuredCumulativeAvgLossNumeratorDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The numerator for the average loss ratio recorded in
        the destination to source direction.  This value is 
        cumulative over the period of this interval." 
    ::= { ipslaEtherJitterAggStatsEntry 87 }

ipslaEtherJAggMeasuredCumulativeAvgLossDenominatorDS OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "frames"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The denominator for the average loss ratio recorded in
        the destination to source direction.  This value is 
        cumulative over the period of this interval." 
    ::= { ipslaEtherJitterAggStatsEntry 88 }
 

-- Conformance Information

ciscoIpSlaEthernetMIBConform  OBJECT IDENTIFIER
    ::= { ciscoIpSlaEthernetMIB 2 }

ciscoIpSlaEthernetCompliances  OBJECT IDENTIFIER
    ::= { ciscoIpSlaEthernetMIBConform 1 }

ciscoIpSlaEthernetMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoIpSlaEthernetMIBConform 2 }


-- ciscoIpSlaEthernetCompliance is superceded by
-- ciscoIpSlaEthernetComplianceRev2

ciscoIpSlaEthernetCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for
        (1) Ethernet Jitter operation and statistics"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoIpSlaEthernetAutoGroup,
                        ciscoIpSlaEthernetStatsGroup
                    }
    ::= { ciscoIpSlaEthernetCompliances 1 }

ciscoIpSlaEthernetComplianceRev2 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for
        (1) Ethernet Jitter operation and statistics
        (2) supporting IP SLA Auto-Ethernet-CFM"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoIpSlaEthernetAutoGroup,
                        ciscoIpSlaEthernetStatsGroup
                    }

    GROUP           ciscoIpSlaEthernetAutoEVCGroup
    DESCRIPTION
        "ciscoIpSlaEthernetAutoEVCGroup is only mandatory
        for the devices that support Ethernet CFM  with
        Virtual Connection."
    ::= { ciscoIpSlaEthernetCompliances 2 }

ciscoIpSlaEthernetComplianceRev3 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for
        (1) Ethernet Jitter operation and statistics
        (2) supporting IP SLA Y1731"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoIpSlaEthernetAutoGroup,
                        ciscoIpSlaEthernetStatsGroup
                    }

    GROUP           ciscoIpSlaEthernetY1731Group
    DESCRIPTION
        "ciscoIpSlaEthernetY1731Group is only mandatory
        for the devices that support Ethernet CFM  with
        Virtual Connection."

    GROUP           ciscoIpSlaEthernetAutoEVCGroup
    DESCRIPTION
        "ciscoIpSlaEthernetAutoEVCGroup is only mandatory for devices
        that support Ethernet CFM with Virtual Connection."
    ::= { ciscoIpSlaEthernetCompliances 3 }

ciscoIpSlaEthernetAutoGroup OBJECT-GROUP
    OBJECTS         {
                        ipslaEthernetGrpCtrlStatus,
                        ipslaEthernetGrpCtrlStorageType,
                        ipslaEthernetGrpCtrlRttType,
                        ipslaEthernetGrpCtrlOwner,
                        ipslaEthernetGrpCtrlTag,
                        ipslaEthernetGrpCtrlThreshold,
                        ipslaEthernetGrpCtrlTimeout,
                        ipslaEthernetGrpCtrlProbeList,
                        ipslaEthernetGrpCtrlVLAN,
                        ipslaEthernetGrpCtrlDomainNameType,
                        ipslaEthernetGrpCtrlDomainName,
                        ipslaEthernetGrpCtrlReqDataSize,
                        ipslaEthernetGrpCtrlMPIDExLst,
                        ipslaEthernetGrpCtrlCOS,
                        ipslaEthernetGrpCtrlInterval,
                        ipslaEthernetGrpCtrlNumFrames,
                        ipslaEthernetGrpReactStatus,
                        ipslaEthernetGrpReactStorageType,
                        ipslaEthernetGrpReactVar,
                        ipslaEthernetGrpReactThresholdType,
                        ipslaEthernetGrpReactThresholdRising,
                        ipslaEthernetGrpReactThresholdFalling,
                        ipslaEthernetGrpReactThresholdCountX,
                        ipslaEthernetGrpReactThresholdCountY,
                        ipslaEthernetGrpReactActionType,
                        ipslaEthernetGrpScheduleRttStartTime,
                        ipslaEthernetGrpSchedulePeriod,
                        ipslaEthernetGrpScheduleFrequency
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects that were added to support
        Auto-Ethernet-CFM."
    ::= { ciscoIpSlaEthernetMIBGroups 1 }

ciscoIpSlaEthernetStatsGroup OBJECT-GROUP
    OBJECTS         {
                        ipslaEtherJitterLatestNumRTT,
                        ipslaEtherJitterLatestRTTSum,
                        ipslaEtherJitterLatestRTTSum2,
                        ipslaEtherJitterLatestRTTMin,
                        ipslaEtherJitterLatestRTTMax,
                        ipslaEtherJitterLatestMinPosSD,
                        ipslaEtherJitterLatestMaxPosSD,
                        ipslaEtherJitterLatestNumPosSD,
                        ipslaEtherJitterLatestSumPosSD,
                        ipslaEtherJitterLatestSum2PosSD,
                        ipslaEtherJitterLatestMinNegSD,
                        ipslaEtherJitterLatestMaxNegSD,
                        ipslaEtherJitterLatestNumNegSD,
                        ipslaEtherJitterLatestSumNegSD,
                        ipslaEtherJitterLatestSum2NegSD,
                        ipslaEtherJitterLatestMinPosDS,
                        ipslaEtherJitterLatestMaxPosDS,
                        ipslaEtherJitterLatestNumPosDS,
                        ipslaEtherJitterLatestSumPosDS,
                        ipslaEtherJitterLatestSum2PosDS,
                        ipslaEtherJitterLatestMinNegDS,
                        ipslaEtherJitterLatestMaxNegDS,
                        ipslaEtherJitterLatestNumNegDS,
                        ipslaEtherJitterLatestSumNegDS,
                        ipslaEtherJitterLatestSum2NegDS,
                        ipslaEtherJitterLatestFrmLossSD,
                        ipslaEtherJitterLatestFrmLossDS,
                        ipslaEtherJitterLatestFrmOutSeq,
                        ipslaEtherJitterLatestFrmMIA,
                        ipslaEtherJitterLatestFrmSkipped,
                        ipslaEtherJitterLatestSense,
                        ipslaEtherJitterLatestFrmLateA,
                        ipslaEtherJitterLatestMinSucFrmL,
                        ipslaEtherJitterLatestMaxSucFrmL,
                        ipslaEtherJitterLatestOWSumSD,
                        ipslaEtherJitterLatestOWSum2SD,
                        ipslaEtherJitterLatestOWMinSD,
                        ipslaEtherJitterLatestOWMaxSD,
                        ipslaEtherJitterLatestOWSumDS,
                        ipslaEtherJitterLatestOWSum2DS,
                        ipslaEtherJitterLatestOWMinDS,
                        ipslaEtherJitterLatestOWMaxDS,
                        ipslaEtherJitterLatestNumOW,
                        ipslaEtherJitterLatestAvgJitter,
                        ipslaEtherJitterLatestAvgSDJ,
                        ipslaEtherJitterLatestAvgDSJ,
                        ipslaEtherJitterLatestOWAvgSD,
                        ipslaEtherJitterLatestOWAvgDS,
                        ipslaEtherJitterLatestIAJOut,
                        ipslaEtherJitterLatestIAJIn,
                        ipslaEtherJLatestFrmUnProcessed,
                        ipslaEtherJAggMeasuredCmpletions,
                        ipslaEtherJAggMeasuredOvThrshlds,
                        ipslaEtherJAggMeasuredNumRTTs,
                        ipslaEtherJAggMeasuredRTTSums,
                        ipslaEtherJAggMeasuredRTTSum2Ls,
                        ipslaEtherJAggMeasuredRTTSum2Hs,
                        ipslaEtherJAggMeasuredRTTMin,
                        ipslaEtherJAggMeasuredRTTMax,
                        ipslaEtherJAggMeasuredMinPosSD,
                        ipslaEtherJAggMeasuredMaxPosSD,
                        ipslaEtherJAggMeasuredNumPosSDs,
                        ipslaEtherJAggMeasuredSumPosSDs,
                        ipslaEtherJAggMeasuredSum2PSDLs,
                        ipslaEtherJAggMeasuredSum2PSDHs,
                        ipslaEtherJAggMeasuredMinNegSD,
                        ipslaEtherJAggMeasuredMaxNegSD,
                        ipslaEtherJAggMeasuredNumNegSDs,
                        ipslaEtherJAggMeasuredSumNegSDs,
                        ipslaEtherJAggMeasuredSum2NSDLs,
                        ipslaEtherJAggMeasuredSum2NSDHs,
                        ipslaEtherJAggMeasuredMinPosDS,
                        ipslaEtherJAggMeasuredMaxPosDS,
                        ipslaEtherJAggMeasuredNumPosDSes,
                        ipslaEtherJAggMeasuredSumPosDSes,
                        ipslaEtherJAggMeasuredSum2PDSLs,
                        ipslaEtherJAggMeasuredSum2PDSHs,
                        ipslaEtherJAggMeasuredMinNegDS,
                        ipslaEtherJAggMeasuredMaxNegDS,
                        ipslaEtherJAggMeasuredNumNegDSes,
                        ipslaEtherJAggMeasuredSumNegDSes,
                        ipslaEtherJAggMeasuredSum2NDSLs,
                        ipslaEtherJAggMeasuredSum2NDSHs,
                        ipslaEtherJAggMeasuredFrmLossSDs,
                        ipslaEtherJAggMeasuredFrmLssDSes,
                        ipslaEtherJAggMeasuredFrmOutSeqs,
                        ipslaEtherJAggMeasuredFrmMIAes,
                        ipslaEtherJAggMeasuredFrmSkippds,
                        ipslaEtherJAggMeasuredErrors,
                        ipslaEtherJAggMeasuredBusies,
                        ipslaEtherJAggMeasuredOWSumSDs,
                        ipslaEtherJAggMeasuredOWSum2SDLs,
                        ipslaEtherJAggMeasuredOWSum2SDHs,
                        ipslaEtherJAggMeasuredOWMinSD,
                        ipslaEtherJAggMeasuredOWMaxSD,
                        ipslaEtherJAggMeasuredOWSumDSes,
                        ipslaEtherJAggMeasuredOWSum2DSLs,
                        ipslaEtherJAggMeasuredOWSum2DSHs,
                        ipslaEtherJAggMeasuredOWMinDS,
                        ipslaEtherJAggMeasuredOWMaxDS,
                        ipslaEtherJAggMeasuredNumOWs,
                        ipslaEtherJAggMeasuredAvgJ,
                        ipslaEtherJAggMeasuredAvgJSD,
                        ipslaEtherJAggMeasuredAvgJDS,
                        ipslaEtherJAggMinSucFrmLoss,
                        ipslaEtherJAggMaxSucFrmLoss,
                        ipslaEtherJAggMeasuredIAJOut,
                        ipslaEtherJAggMeasuredIAJIn,
                        ipslaEtherJAggMeasuredFrmLateAs,
                        ipslaEtherJAggMeasuredFrmUnPrcds
                    }
    STATUS          current
    DESCRIPTION
        "A collection of statistics objects related to
        Ethernet Jitter Probe."
    ::= { ciscoIpSlaEthernetMIBGroups 2 }

ciscoIpSlaEthernetAutoEVCGroup OBJECT-GROUP
    OBJECTS         {
                        ipslaEthernetGrpCtrlEVC,
                        ipslaEthernetGrpCtrlServiceInsType
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects which provides the support for
        Auto-Ethernet-CFM ping/jitter operation with Ethernet 
        Virtual Connection."
    ::= { ciscoIpSlaEthernetMIBGroups 3 }

ciscoIpSlaEthernetY1731Group OBJECT-GROUP
    OBJECTS         {
                        ipslaEtherJAggMeasuredMaxPosTW,
                        ipslaEtherJAggMeasuredMaxNegTW,
                        ipslaEtherJAggMeasuredMinPosTW,
                        ipslaEtherJAggMeasuredMinNegTW,
                        ipslaEtherJAggMeasuredTxFrmsSD,
                        ipslaEtherJAggMeasuredTxFrmsDS,
                        ipslaEtherJAggMeasuredRxFrmsSD,
                        ipslaEtherJAggMeasuredRxFrmsDS,
                        ipslaEtherJAggMeasuredMinLossNumeratorSD,
                        ipslaEtherJAggMeasuredMinLossDenominatorSD,
                        ipslaEtherJAggMeasuredMaxLossNumeratorSD,
                        ipslaEtherJAggMeasuredMaxLossDenominatorSD,
                        ipslaEtherJAggMeasuredAvgLossNumeratorSD,
                        ipslaEtherJAggMeasuredAvgLossDenominatorSD,
                        ipslaEtherJAggMeasuredMinLossNumeratorDS,
                        ipslaEtherJAggMeasuredMinLossDenominatorDS,
                        ipslaEtherJAggMeasuredMaxLossNumeratorDS,
                        ipslaEtherJAggMeasuredMaxLossDenominatorDS,
                        ipslaEtherJAggMeasuredAvgLossNumeratorDS,
                        ipslaEtherJAggMeasuredAvgLossDenominatorDS,
                        ipslaEtherJAggMeasuredCumulativeLossNumeratorSD,
                        ipslaEtherJAggMeasuredCumulativeLossDenominatorSD,
                        ipslaEtherJAggMeasuredCumulativeAvgLossNumeratorSD,
                        ipslaEtherJAggMeasuredCumulativeAvgLossDenominatorSD,
                        ipslaEtherJAggMeasuredCumulativeLossNumeratorDS,
                        ipslaEtherJAggMeasuredCumulativeLossDenominatorDS,
                        ipslaEtherJAggMeasuredCumulativeAvgLossNumeratorDS,
                        ipslaEtherJAggMeasuredCumulativeAvgLossDenominatorDS
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects which provides the support for
        Y1731 operation with Ethernet 
        Virtual Connection."
    ::= { ciscoIpSlaEthernetMIBGroups 4 }

END

















































































































































































































































































































































































































