-- *****************************************************************
-- CISCO-ENTITY-QFP-MIB.my
--   
-- This MIB module is used to monitor Quantum Flow Processors (QFP).
--   
-- November 2009, Muthukrishnan Venkatraman
--   
-- Copyright (c) 2009, 2012, 2014 by cisco Systems Inc.
-- All rights reserved.
--   
-- *****************************************************************

CISCO-ENTITY-QFP-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Gauge32,
    NOTIFICATION-TYPE,
    Counter32,
    Counter64,
    Unsigned32,
    Integer32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    TEXTUAL-CONVENTION,
    DateAndTime,
    TruthValue
        FROM SNMPv2-TC
    entPhysicalIndex
        FROM ENTITY-MIB
    CounterBasedGauge64
        FROM HCNUM-TC
    ciscoMgmt
        FROM CISCO-SMI;


ciscoEntityQfpMIB MODULE-IDENTITY
    LAST-UPDATED    "201406180000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service


            Postal: 170 W Tasman Drive

            San Jose, CA  95134

            USA


            Tel: +1 800 553-NETS


            E-mail: cs-snmp@cisco.com"
    DESCRIPTION
        "This MIB module defines managed objects that facilitate the
        management of Quantum Flow Processors (QFP), which are listed
        in the ENTITY-MIB (RFC 4133) entPhysicalTable as an
        entPhysicalClass of 'cpu'.

        The Quantum Flow Processors (QFP) technology is an architecture
        family developed by Cisco, which has fully integrated and
        programmable networking chip set that controls different
        functions of a system such as packet forwarding.

        This module contains objects to monitor various QFP
        statistics such as system, utilization, memory, etc.

        The utilization statistics can be used for future capacity
        planning. The calculation of this statistics may vary by
        devices which host QFPs, hence the user must refer to the
        specific device document of interest for the exact method
        of calculation. The utilization statistics have the following
        terminology.

        o Input - Communication channel where packets arrive on the
                  QFP.

        o Output - Communication channel where packets leave the QFP.

        o Priority - A classification applied to packets indicating
                     they should be treated with greater urgency.

        o Non-Priority - A classification applied to packets indicating
                         they should be treated with lesser urgency.

        o Processing Load - The percentage of time over some interval
                            that the QFP has spent forwarding packets,
                            relative to the total time spent both 
                            forwarding packets and being idle."
    REVISION        "201406180000Z"
    DESCRIPTION
        "Added the following objects to the MIB.

        ceqfpThroughputLicensedBW, ceqfpThroughputLevel,
        ceqfpThroughputInterval, ceqfpThroughputThreshold,
        ceqfpThroughputAvgRate to ceqfpThroughputTable.

        Added ceqfpThroughputNotifEnabled to ciscoEntityQfpNotif group.

        Added ceqfpThroughputNotif as a new notification to the MIB.

        Added a new MIB conform group, ceqfpThroughputGroup for the new
        objects.

        Also modified the ciscoEntityQfpMIBComplianceRev2 to add the new
        group ceqfpThroughputGroup."
    REVISION        "201206060000Z"
    DESCRIPTION
        "Added the following new objects to the
        ceqfpMemoryResourceTable.
        ceqfpMemoryResTotalOvrflw, ceqfpMemoryHCResTotal,
        ceqfpMemoryResInUseOvrflw, ceqfpMemoryHCResInUse,
        ceqfpMemoryResFreeOvrflw,ceqfpMemoryHCResFree,
        ceqfpMemoryResLowFreeWatermarkOvrflw,
        ceqfpMemoryHCResLowFreeWatermark.

        Added following new compliance groups.
        ciscoEntityQfpMemoryResourceOvrflwGroup,
        ciscoEntityQfpMemoryHCResourceGroup.

        Added new compliance ciscoEntityQfpMIBComplianceRev2 which
        deprecates ciscoEntityQfpMIBComplianceRev1."
    REVISION        "200912020000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 715 }



CiscoQfpPacketRate ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d"
    STATUS          current
    DESCRIPTION
        "An estimate of throughput in units of packets per second.

        The CiscoQfpPacketRate type represents a non-negative integer,
        which may increase or decrease, but shall never exceed a 
        maximum value, nor fall below a minimum value of Counter64.
        The Counter64 syntax is used for encoding rules."
    SYNTAX          Counter64

CiscoQfpBitRate ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d"
    STATUS          current
    DESCRIPTION
        "An estimate of throughput in units of bits per second.

        The CiscoQfpBitRate type represents a non-negative integer,
        which may increase or decrease, but shall never exceed a 
        maximum value, nor fall below a minimum value of Counter64.
        The Counter64 syntax is used for encoding rules."
    SYNTAX          Counter64

CiscoQfpTimeInterval ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "An enumerated integer-value describing the available interval
        values for which the periodic statistics are to be collected.

        fiveSeconds (1)   - Interval to collect last 5 seconds       
                            statistics
        oneMinute(2)      - Interval to collect last 1 minute
                            statistics
        fiveMinutes(3)    - Interval to collect last 5 minutes       
                            statistics
        sixtyMinutes(4)   - Interval to collect last 60 minutes       
                            statistics"
    SYNTAX          INTEGER  {
                        fiveSeconds(1),
                        oneMinute(2),
                        fiveMinutes(3),
                        sixtyMinutes(4)
                    }

CiscoQfpMemoryResource ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "An enumerated integer-value describing various memory resources
        used by the QFP.

        dram (1) - Dynamic Random Access Memory (DRAM) memory resource"
    SYNTAX          INTEGER  {
                        dram(1)
                    }
ciscoEntityQfpMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoEntityQfpMIB 0 }

ciscoEntityQfpMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoEntityQfpMIB 1 }

ciscoEntityQfpMIBConform  OBJECT IDENTIFIER
    ::= { ciscoEntityQfpMIB 2 }

ciscoEntityQfp  OBJECT IDENTIFIER
    ::= { ciscoEntityQfpMIBObjects 1 }

ciscoEntityQfpNotif  OBJECT IDENTIFIER
    ::= { ciscoEntityQfpMIBObjects 2 }


ceqfpSystemTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeqfpSystemEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table maintains the QFP system information for each QFP
        physical entity.

        An agent creates a conceptual row to this table corresponding
        to a QFP physical entity upon detection of a physical entity
        supporting the QFP system information.

        An agent destroys a conceptual row from this table       
        corresponding to a QFP physical entity upon removal
        of the QFP host physical entity."
    ::= { ciscoEntityQfp 1 }

ceqfpSystemEntry OBJECT-TYPE
    SYNTAX          CeqfpSystemEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A conceptual row in the ceqfpSystemTable. There is an entry
        in this table for each QFP entity, as defined by a value of
        entPhysicalIndex."
    INDEX           { entPhysicalIndex } 
    ::= { ceqfpSystemTable 1 }

CeqfpSystemEntry ::= SEQUENCE {
        ceqfpSystemTrafficDirection INTEGER,
        ceqfpSystemState            INTEGER,
        ceqfpNumberSystemLoads      Counter32,
        ceqfpSystemLastLoadTime     DateAndTime
}

ceqfpSystemTrafficDirection OBJECT-TYPE
    SYNTAX          INTEGER  {
                        none(1),
                        ingress(2),
                        egress(3),
                        both(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the traffic direction that this QFP is
        assigned to process. The enumerated values are described below.

        none (1)    - The QFP is not assigned to processes any traffic
                      yet
        ingress (2) - The QFP processes inbound traffic
        egress (3)  - The QFP processes outbound traffic
        both (4)    - The QFP processes both inbound and outbound
                      traffic" 
    ::= { ceqfpSystemEntry 1 }

ceqfpSystemState OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        reset(2),
                        init(3),
                        active(4),
                        activeSolo(5),
                        standby(6),
                        hotStandby(7)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the current QFP state. The enumerated
        values are described below.

        unknown (1)    - The state of the QFP is unknown
        reset (2)      - The QFP is reset
        init (3)       - The QFP is being initialized
        active (4)     - The QFP is active in a system with redundant
                         QFP
        activeSolo (5) - The QFP is active and there is no redundant
                         QFP in the system
        standby (6)    - The QFP is standby in a redundant system.
        hotStandby (7) - The QFP is standby and synchronized with
                         active, so that a switchover in this state
                         will preserve state of the active. Stateful 
                         datapath features are synchronized between the
                         active QFP and standby QFP" 
    ::= { ceqfpSystemEntry 2 }

ceqfpNumberSystemLoads OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the number of times the QFP is loaded,
        since the QFP host is up." 
    ::= { ceqfpSystemEntry 3 }

ceqfpSystemLastLoadTime OBJECT-TYPE
    SYNTAX          DateAndTime
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP last load time." 
    ::= { ceqfpSystemEntry 4 }
 


ceqfpFiveSecondUtilAlgo OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        fiveSecSample(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This objects represents the method used to calculate 5 Second
        interval utilization data. The enumerated values are described
        below.

        unknown       (1) - The calculation method is unknown
        fiveSecSample (2) - The value is calculated based on the last
                            5 second sampling period of utilization
                            data." 
    ::= { ciscoEntityQfp 2 }

ceqfpOneMinuteUtilAlgo OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        fiveSecSMA(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This objects represents the method used to calculate 1 Minute
        interval utilization data. The enumerated values are described
        below.

        unknown    (1) - The calculation method is unknown
        fiveSecSMA (2) - The value is calculated using Simple Moving  
                         Average of last 12 five seconds utilization
                         data." 
    ::= { ciscoEntityQfp 3 }

ceqfpFiveMinutesUtilAlgo OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        fiveSecSMA(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This objects represents the method used to calculate 5 Minutes
        interval utilization data. The enumerated values are described
        below.

        unknown    (1) - The calculation method is unknown
        fiveSecSMA (2) - The value is calculated using Simple Moving  
                         Average of last 60 five seconds utilization
                         data." 
    ::= { ciscoEntityQfp 4 }

ceqfpSixtyMinutesUtilAlgo OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        fiveSecSMA(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This objects represents the method used to calculate 60 Minutes
        interval utilization data. The enumerated values are described
        below.

        unknown    (1) - The calculation method is unknown
        fiveSecSMA (1) - The value is calculated using Simple Moving  
                         Average of last 720 five seconds utilization
                         data." 
    ::= { ciscoEntityQfp 5 }

ceqfpUtilizationTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeqfpUtilizationEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table maintains the utilization statistics collected
        by each QFP physical entity at various time interval such as
        last 5 seconds, 1 minute, etc.

        An agent creates a conceptual row to this table corresponding
        to a QFP physical entity for a time interval upon detection of
        a physical entity supporting the utilization statistics for a
        time interval.

        The agent destroys a conceptual row from this table       
        corresponding to a QFP physical entity for a time interval
        upon removal of the QFP host physical entity or it does not
        receive the utilization statistics update for a certain time
        period. The time period to wait before deleting an entry from
        this table would be the discretion of the supporting device."
    ::= { ciscoEntityQfp 6 }

ceqfpUtilizationEntry OBJECT-TYPE
    SYNTAX          CeqfpUtilizationEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A conceptual row in the ceqfpUtilizationTable. There is
        an entry in this table for each QFP entity by a value of
        entPhysicalIndex and the supported time interval by a value 
        of ceqfpUtilTimeInterval.

        The method of utilization data calculation for each interval
        period can be identified through the respective interval
        scalar objects. For example the utilizaiton data calculation
        method for 'fiveSecond' interval can be identified by
        ceqfpFiveSecondUtilAlgo."
    INDEX           {
                        entPhysicalIndex,
                        ceqfpUtilTimeInterval
                    } 
    ::= { ceqfpUtilizationTable 1 }

CeqfpUtilizationEntry ::= SEQUENCE {
        ceqfpUtilTimeInterval             CiscoQfpTimeInterval,
        ceqfpUtilInputPriorityPktRate     CiscoQfpPacketRate,
        ceqfpUtilInputPriorityBitRate     CiscoQfpBitRate,
        ceqfpUtilInputNonPriorityPktRate  CiscoQfpPacketRate,
        ceqfpUtilInputNonPriorityBitRate  CiscoQfpBitRate,
        ceqfpUtilInputTotalPktRate        CiscoQfpPacketRate,
        ceqfpUtilInputTotalBitRate        CiscoQfpBitRate,
        ceqfpUtilOutputPriorityPktRate    CiscoQfpPacketRate,
        ceqfpUtilOutputPriorityBitRate    CiscoQfpBitRate,
        ceqfpUtilOutputNonPriorityPktRate CiscoQfpPacketRate,
        ceqfpUtilOutputNonPriorityBitRate CiscoQfpBitRate,
        ceqfpUtilOutputTotalPktRate       CiscoQfpPacketRate,
        ceqfpUtilOutputTotalBitRate       CiscoQfpBitRate,
        ceqfpUtilProcessingLoad           Gauge32
}

ceqfpUtilTimeInterval OBJECT-TYPE
    SYNTAX          CiscoQfpTimeInterval
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object identifies the time interval for which the
        utilization statistics being collected. The interval 
        values can be 5 second, 1 minute, etc. as specified in 
        the CiscoQfpTimeInterval." 
    ::= { ceqfpUtilizationEntry 1 }

ceqfpUtilInputPriorityPktRate OBJECT-TYPE
    SYNTAX          CiscoQfpPacketRate
    UNITS           "packets per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP input channel priority packet
        rate during this interval." 
    ::= { ceqfpUtilizationEntry 2 }

ceqfpUtilInputPriorityBitRate OBJECT-TYPE
    SYNTAX          CiscoQfpBitRate
    UNITS           "bits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP input channel priority bit rate
        during this interval." 
    ::= { ceqfpUtilizationEntry 3 }

ceqfpUtilInputNonPriorityPktRate OBJECT-TYPE
    SYNTAX          CiscoQfpPacketRate
    UNITS           "packets per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP input channel non-priority
        packet rate during this interval." 
    ::= { ceqfpUtilizationEntry 4 }

ceqfpUtilInputNonPriorityBitRate OBJECT-TYPE
    SYNTAX          CiscoQfpBitRate
    UNITS           "bits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP input channel non-priority
        bit rate during this interval." 
    ::= { ceqfpUtilizationEntry 5 }

ceqfpUtilInputTotalPktRate OBJECT-TYPE
    SYNTAX          CiscoQfpPacketRate
    UNITS           "packets per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP input channel total packet rate
        during this interval, which includes both priority and
        non-priority input packet rate." 
    ::= { ceqfpUtilizationEntry 6 }

ceqfpUtilInputTotalBitRate OBJECT-TYPE
    SYNTAX          CiscoQfpBitRate
    UNITS           "bits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP input channel total bit rate
        during this interval, which includes both priority and
        non-priority input bit rate." 
    ::= { ceqfpUtilizationEntry 7 }

ceqfpUtilOutputPriorityPktRate OBJECT-TYPE
    SYNTAX          CiscoQfpPacketRate
    UNITS           "packets per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP output channel priority packet
        rate during this interval." 
    ::= { ceqfpUtilizationEntry 8 }

ceqfpUtilOutputPriorityBitRate OBJECT-TYPE
    SYNTAX          CiscoQfpBitRate
    UNITS           "bits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP output channel priority bit
        rate during this interval." 
    ::= { ceqfpUtilizationEntry 9 }

ceqfpUtilOutputNonPriorityPktRate OBJECT-TYPE
    SYNTAX          CiscoQfpPacketRate
    UNITS           "packets per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP output channel non-priority
        packet rate during this interval." 
    ::= { ceqfpUtilizationEntry 10 }

ceqfpUtilOutputNonPriorityBitRate OBJECT-TYPE
    SYNTAX          CiscoQfpBitRate
    UNITS           "bits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP output channel non-priority
        bit rate during this interval." 
    ::= { ceqfpUtilizationEntry 11 }

ceqfpUtilOutputTotalPktRate OBJECT-TYPE
    SYNTAX          CiscoQfpPacketRate
    UNITS           "packets per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP output channel total packet rate
        during this interval, which includes both priority and
        non-priority output packet rate." 
    ::= { ceqfpUtilizationEntry 12 }

ceqfpUtilOutputTotalBitRate OBJECT-TYPE
    SYNTAX          CiscoQfpBitRate
    UNITS           "bits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP output channel total bit rate
        during this interval, which includes both priority and
        non-priority bit rate." 
    ::= { ceqfpUtilizationEntry 13 }

ceqfpUtilProcessingLoad OBJECT-TYPE
    SYNTAX          Gauge32 (0..100)
    UNITS           "percent"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the QFP processing load during this
        interval." 
    ::= { ceqfpUtilizationEntry 14 }
 


ceqfpMemoryResourceTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeqfpMemoryResourceEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table maintains the memory resources statistics for
        each QFP physical entity.

        An agent creates a conceptual row to this table corresponding
        to a QFP physical entity and its supported memory resource type
        upon detection of a physical entity supporting the memory 
        resource statistics for a memory resource type.

        An agent destroys a conceptual row from this table       
        corresponding to a QFP physical entity and its supported
        memory resource type upon removal of the QFP host physical
        entity or it does not receive memory resource statistics
        update for a certain time period. The time period to wait
        before deleting an entry from this table would be the
        discretion of the supporting device."
    ::= { ciscoEntityQfp 7 }

ceqfpMemoryResourceEntry OBJECT-TYPE
    SYNTAX          CeqfpMemoryResourceEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A conceptual row in the ceqfpMemoryResourceTable. There
        is an entry in this table for each QFP entity by a value 
        of entPhysicalIndex and the supported memory resource type 
        by a value of ceqfpMemoryResType."
    INDEX           {
                        entPhysicalIndex,
                        ceqfpMemoryResType
                    } 
    ::= { ceqfpMemoryResourceTable 1 }

CeqfpMemoryResourceEntry ::= SEQUENCE {
        ceqfpMemoryResType                   CiscoQfpMemoryResource,
        ceqfpMemoryResTotal                  Gauge32,
        ceqfpMemoryResInUse                  Gauge32,
        ceqfpMemoryResFree                   Gauge32,
        ceqfpMemoryResLowFreeWatermark       Gauge32,
        ceqfpMemoryResRisingThreshold        Unsigned32,
        ceqfpMemoryResFallingThreshold       Unsigned32,
        ceqfpMemoryResTotalOvrflw            Gauge32,
        ceqfpMemoryHCResTotal                CounterBasedGauge64,
        ceqfpMemoryResInUseOvrflw            Gauge32,
        ceqfpMemoryHCResInUse                CounterBasedGauge64,
        ceqfpMemoryResFreeOvrflw             Gauge32,
        ceqfpMemoryHCResFree                 CounterBasedGauge64,
        ceqfpMemoryResLowFreeWatermarkOvrflw Gauge32,
        ceqfpMemoryHCResLowFreeWatermark     CounterBasedGauge64
}

ceqfpMemoryResType OBJECT-TYPE
    SYNTAX          CiscoQfpMemoryResource
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the type of the memory resource used by
        the QFP. This object is one of the indices to uniquely identify
        the QFP memory resource type." 
    ::= { ceqfpMemoryResourceEntry 1 }

ceqfpMemoryResTotal OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "kilo bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents total memory available on this memory
        resource." 
    ::= { ceqfpMemoryResourceEntry 2 }

ceqfpMemoryResInUse OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "kilo bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the memory which is currently under use
        on this memory resource." 
    ::= { ceqfpMemoryResourceEntry 3 }

ceqfpMemoryResFree OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "kilo bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the memory which is currently free on
        this memory resource." 
    ::= { ceqfpMemoryResourceEntry 4 }

ceqfpMemoryResLowFreeWatermark OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "kilo bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents lowest free water mark on this memory
        resource." 
    ::= { ceqfpMemoryResourceEntry 5 }

ceqfpMemoryResRisingThreshold OBJECT-TYPE
    SYNTAX          Unsigned32 (0..100)
    UNITS           "percent"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the rising threshold value for this
        memory resource. A value of zero means that the rising
        threshold is not supported for this memory resource.

        The value of this object can not be set to lower than or
        equal to ceqfpMemoryResFallingThreshold.

        A rising (ceqfpMemoryResRisingThreshNotif) notification
        will be generated, whenever the memory resource usage
        (ceqfpMemoryHCResInUse) is equal to or greater than this
        value.

        After a rising notification is generated, another such 
        notification will not be generated until the 
        ceqfpMemoryResInUse falls below this value and reaches 
        the ceqfpMemoryResFallingThreshold."
    DEFVAL          { 90 } 
    ::= { ceqfpMemoryResourceEntry 6 }

ceqfpMemoryResFallingThreshold OBJECT-TYPE
    SYNTAX          Unsigned32 (0..100)
    UNITS           "percent"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the falling threshold value for this
        memory resource. A value of zero means that the falling
        threshold is not supported for this memory resource.

        The value of this object can not be set to higher than or
        equal to ceqfpMemoryResRisingThreshold.

        A falling (ceqfpMemoryResRisingThreshNotif) notification 
        will be generated, whenever the memory resource usage
        (ceqfpMemoryHCResInUse) is equal to or lesser than this value.

        After a falling notification is generated, another 
        such notification will not be generated until the 
        ceqfpMemoryResInUse rises above this value and reaches 
        the ceqfpMemoryResRisingThreshold."
    DEFVAL          { 85 } 
    ::= { ceqfpMemoryResourceEntry 7 }

ceqfpMemoryResTotalOvrflw OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "kilo bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the upper 32-bit of
        ceqfpMemoryResTotal.
        This object needs to be supported only when the value of
        ceqfpMemoryResTotal exceeds 32-bit, otherwise this object value
        would be set to 0." 
    ::= { ceqfpMemoryResourceEntry 8 }

ceqfpMemoryHCResTotal OBJECT-TYPE
    SYNTAX          CounterBasedGauge64
    UNITS           "kilo bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object is a 64-bit version of ceqfpMemoryResTotal." 
    ::= { ceqfpMemoryResourceEntry 9 }

ceqfpMemoryResInUseOvrflw OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "kilo bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the upper 32-bit of
        ceqfpMemoryResInUse.
        This object needs to be supported only when the value of
        ceqfpMemoryResInUse exceeds 32-bit, otherwise this object value
        would be set to 0." 
    ::= { ceqfpMemoryResourceEntry 10 }

ceqfpMemoryHCResInUse OBJECT-TYPE
    SYNTAX          CounterBasedGauge64
    UNITS           "kilo bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object is a 64-bit version of ceqfpMemoryInRes." 
    ::= { ceqfpMemoryResourceEntry 11 }

ceqfpMemoryResFreeOvrflw OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "kilo bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the upper 32-bit of ceqfpMemoryResFree.
        This object needs to be supported only when the value of
        ceqfpMemoryResFree exceeds 32-bit, otherwise this object value
        would be set to 0." 
    ::= { ceqfpMemoryResourceEntry 12 }

ceqfpMemoryHCResFree OBJECT-TYPE
    SYNTAX          CounterBasedGauge64
    UNITS           "kilo bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object is a 64-bit version of ceqfpMemoryResFree." 
    ::= { ceqfpMemoryResourceEntry 13 }

ceqfpMemoryResLowFreeWatermarkOvrflw OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "kilo bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the upper 32-bit of
        ceqfpMemoryResLowFreeWatermark. This object needs to be
        supported only when the value of ceqfpMemoryResLowFreeWatermark
        exceeds 32-bit, otherwise this object value would be set to 0." 
    ::= { ceqfpMemoryResourceEntry 14 }

ceqfpMemoryHCResLowFreeWatermark OBJECT-TYPE
    SYNTAX          CounterBasedGauge64
    UNITS           "kilo bytes"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object is a 64-bit version of
        ceqfpMemoryResLowFreeWatermark." 
    ::= { ceqfpMemoryResourceEntry 15 }
 


ceqfpThroughputTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeqfpThroughputEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table maintains the throughput information for each
        QFP physical entity.

                An agent creates a conceptual row to this table
        corresponding to a QFP physical entity upon detection of a
        physical entity supporting the QFP throughput information.

                An agent destroys a conceptual row from this table     

        corresponding to a QFP physical entity upon removal of the QFP
        host physical entity."
    ::= { ciscoEntityQfp 8 }

ceqfpThroughputEntry OBJECT-TYPE
    SYNTAX          CeqfpThroughputEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A conceptual row in the ceqfpThroughputTable. There is an entry
        in this table for each QFP entity, as defined by a value of
        entPhysicalIndex."
    INDEX           { entPhysicalIndex } 
    ::= { ceqfpThroughputTable 1 }

CeqfpThroughputEntry ::= SEQUENCE {
        ceqfpThroughputLicensedBW Counter64,
        ceqfpThroughputLevel      INTEGER,
        ceqfpThroughputInterval   Integer32,
        ceqfpThroughputThreshold  Integer32,
        ceqfpThroughputAvgRate    Counter64
}

ceqfpThroughputLicensedBW OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "bits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the bandwidth for installed
        throughput license." 
    ::= { ceqfpThroughputEntry 1 }

ceqfpThroughputLevel OBJECT-TYPE
    SYNTAX          INTEGER  {
                        normal(1),
                        warning(2),
                        exceed(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the current throughput level for
        installed throughput license.

                        normal  (1) - Throughput usage is normal
                        warning (2) - Throughput usage has crossed the
                                      configured threshold limit
                        exceed  (3) - Throughput usage has exceeded the
                                      total licensed bandwidth" 
    ::= { ceqfpThroughputEntry 2 }

ceqfpThroughputInterval OBJECT-TYPE
    SYNTAX          Integer32 (10..86400)
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object represents the configured time interval at which the
        ceqfpThroughputLevel is checked."
    ::= { ceqfpThroughputEntry 3 }

ceqfpThroughputThreshold OBJECT-TYPE
    SYNTAX          Integer32 (75..95)
    UNITS           "percent"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object represents the configured throughput threshold."
    ::= { ceqfpThroughputEntry 4 }

ceqfpThroughputAvgRate OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "bits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The object represents the average throughput rate in the
        interval ceqfpThroughputInterval." 
    ::= { ceqfpThroughputEntry 5 }
 


ceqfpMemoryResThreshNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object controls memory resource rising and falling
        threshold notification.

        When this object contains a value 'true', then generation of
        memory resource threshold notification is enabled. If this
        object contains a value 'false', then generation of memory
        resource threshold notification is disabled."
    DEFVAL          { false } 
    ::= { ciscoEntityQfpNotif 1 }

ceqfpMemoryResCurrentRisingThresh OBJECT-TYPE
    SYNTAX          Unsigned32 (1..100)
    UNITS           "percent"
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object represents the current rising threshold
        value, which triggers the rising threshold notification
        (ceqfpMemoryResRisingThreshNotif)." 
    ::= { ciscoEntityQfpNotif 2 }

ceqfpMemoryResCurrentFallingThresh OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "percent"
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object represents the current falling threshold
        value, which triggers the falling threshold notification
        (ceqfpMemoryResFallingThreshNotif)." 
    ::= { ciscoEntityQfpNotif 3 }

ceqfpThroughputNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object controls throughput rate notification.

        When this object contains a value 'true', then generation of
        ceqfpThroughputNotif is enabled. If this object contains a value
        'false', then generation of ceqfpThroughputNotif is disabled."
    DEFVAL          { false } 
    ::= { ciscoEntityQfpNotif 4 }
ciscoEntityQfpMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoEntityQfpMIBConform 1 }


ceqfpMemoryResRisingThreshNotif NOTIFICATION-TYPE
    OBJECTS         {
                        ceqfpMemoryResInUse,
                        ceqfpMemoryResCurrentRisingThresh
                    }
    STATUS          current
    DESCRIPTION
        "A notification indicating that the QFP memory usage is rising
        the threshold on this memory resource.

        This notification will be sent, whenever the QFP memory
        usage (ceqfpMemoryResInUse) is equal to or above the 
        rising threshold (ceqfpMemoryResRisingThreshold).

        An agent may throttle the generation of consecutive
        ceqfpMemoryResRisingThreshNotif notification so that
        there is at least a five second (suggested default)
        gap between notification of this type."
   ::= { ciscoEntityQfpMIBNotifs 1 }

ceqfpMemoryResFallingThreshNotif NOTIFICATION-TYPE
    OBJECTS         {
                        ceqfpMemoryResInUse,
                        ceqfpMemoryResCurrentFallingThresh
                    }
    STATUS          current
    DESCRIPTION
        "A notification indicating that the QFP memory usage is equal
        to or below the falling threshold on this memory resource.

        This notification will be sent, whenever the QFP memory
        usage (ceqfpMemoryResInUse) is equal to or below the 
        falling threshold (ceqfpMemoryResFallingThreshold).

        An agent may throttle the generation of consecutive
        ceqfpMemoryResFallingThreshNotif notification so that
        there is at least a five second (suggested default)
        gap between notification of this type."
   ::= { ciscoEntityQfpMIBNotifs 2 }

ceqfpThroughputNotif NOTIFICATION-TYPE
    OBJECTS         {
                        ceqfpThroughputLicensedBW,
                        ceqfpThroughputLevel,
                        ceqfpThroughputAvgRate
                    }
    STATUS          current
    DESCRIPTION
        "A notification indicating that the average throughput rate for
        the configured interval has exceeded the threshold or reached
        maximum bandwidth allowed.

        This notification will be sent, whenever the ceqfpThroughputLevel
        object has the value warning(2) or exceed(3). The condition for
        trap generation will be checked in every
        ceqfpThroughputInterval.

        ceqfpThroughputNotif with ceqfpThrougputLevel as warning(2)
        indicates that average throughput rate has crossed the
        configured threshold.

        ceqfpThroughputNotif with ceqfpThrougputLevel as exceed(3)
        indicates that average throughput rate has reached maximum
        licensed bandwidth."
   ::= { ciscoEntityQfpMIBNotifs 3 }
ciscoEntityQfpMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoEntityQfpMIBConform 2 }


ciscoEntityQfpMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for CISCO-ENTITY-QFP-MIB"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoEntityQfpSystemGroup,
                        ciscoEntityQfpUtilizationGroup,
                        ciscoEntityQfpUtilizationAlgoGroup
                    }

    GROUP           ciscoEntityQfpMemoryResourceGroup
    DESCRIPTION
        "This group is optional for the QFP entity, which does not use
        the listed memory resources."

    GROUP           ciscoEntityQfpMemoryResNotifGroup
    DESCRIPTION
        "This group is optional for the QFP, which does not support the
        memory resource."

    GROUP           ciscoEntityQfpNotifGroup
    DESCRIPTION
        "This group is optional."

    OBJECT          ceqfpMemoryResRisingThreshold
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not mandatory."

    OBJECT          ceqfpMemoryResFallingThreshold
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not mandatory."
    ::= { ciscoEntityQfpMIBCompliances 1 }

ciscoEntityQfpMIBComplianceRev2 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for CISCO-ENTITY-QFP-MIB.
        This compliance module deprecates
        ciscoEntityQfpMIBComplianceRev1."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoEntityQfpSystemGroup,
                        ciscoEntityQfpUtilizationGroup,
                        ciscoEntityQfpUtilizationAlgoGroup
                    }

    GROUP           ciscoEntityQfpMemoryResourceGroup
    DESCRIPTION
        "This group is optional for the QFP entity, which does not use
        the listed memory resources."

    GROUP           ciscoEntityQfpMemoryResourceOvrflwGroup
    DESCRIPTION
        "This group is optional."

    GROUP           ciscoEntityQfpMemoryHCResourceGroup
    DESCRIPTION
        "This group is optional."

    GROUP           ciscoEntityQfpMemoryResNotifGroup
    DESCRIPTION
        "This group is optional for the QFP, which does not support the
        memory resource."

    GROUP           ciscoEntityQfpNotifGroup
    DESCRIPTION
        "This group is optional."

    GROUP           ceqfpThroughputGroup
    DESCRIPTION
        "This group is optional."

    OBJECT          ceqfpMemoryResRisingThreshold
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not mandatory."

    OBJECT          ceqfpMemoryResFallingThreshold
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not mandatory."
    ::= { ciscoEntityQfpMIBCompliances 2 }

ciscoEntityQfpSystemGroup OBJECT-GROUP
    OBJECTS         {
                        ceqfpSystemTrafficDirection,
                        ceqfpSystemState,
                        ceqfpNumberSystemLoads,
                        ceqfpSystemLastLoadTime
                    }
    STATUS          current
    DESCRIPTION
        "This group contains collection of QFP system information."
    ::= { ciscoEntityQfpMIBGroups 1 }

ciscoEntityQfpUtilizationAlgoGroup OBJECT-GROUP
    OBJECTS         {
                        ceqfpFiveSecondUtilAlgo,
                        ceqfpOneMinuteUtilAlgo,
                        ceqfpFiveMinutesUtilAlgo,
                        ceqfpSixtyMinutesUtilAlgo
                    }
    STATUS          current
    DESCRIPTION
        "This group contains collection of QFP utilization algorithm
        objects."
    ::= { ciscoEntityQfpMIBGroups 2 }

-- Units of Conformance

ciscoEntityQfpUtilizationGroup OBJECT-GROUP
    OBJECTS         {
                        ceqfpUtilInputPriorityPktRate,
                        ceqfpUtilInputPriorityBitRate,
                        ceqfpUtilInputNonPriorityPktRate,
                        ceqfpUtilInputNonPriorityBitRate,
                        ceqfpUtilInputTotalPktRate,
                        ceqfpUtilInputTotalBitRate,
                        ceqfpUtilOutputPriorityPktRate,
                        ceqfpUtilOutputPriorityBitRate,
                        ceqfpUtilOutputNonPriorityPktRate,
                        ceqfpUtilOutputNonPriorityBitRate,
                        ceqfpUtilOutputTotalPktRate,
                        ceqfpUtilOutputTotalBitRate,
                        ceqfpUtilProcessingLoad
                    }
    STATUS          current
    DESCRIPTION
        "This group contains collection of QFP utilization information."
    ::= { ciscoEntityQfpMIBGroups 3 }

ciscoEntityQfpMemoryResourceGroup OBJECT-GROUP
    OBJECTS         {
                        ceqfpMemoryResTotal,
                        ceqfpMemoryResInUse,
                        ceqfpMemoryResFree,
                        ceqfpMemoryResLowFreeWatermark,
                        ceqfpMemoryResRisingThreshold,
                        ceqfpMemoryResFallingThreshold
                    }
    STATUS          current
    DESCRIPTION
        "This group contains collection of QFP memory resource
        information."
    ::= { ciscoEntityQfpMIBGroups 4 }

ciscoEntityQfpNotifGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        ceqfpMemoryResRisingThreshNotif,
                        ceqfpMemoryResFallingThreshNotif,
                        ceqfpThroughputNotif
                    }
    STATUS          current
    DESCRIPTION
        "This group contains collection of QFP notifications."
    ::= { ciscoEntityQfpMIBGroups 5 }

ciscoEntityQfpMemoryResNotifGroup OBJECT-GROUP
    OBJECTS         {
                        ceqfpMemoryResThreshNotifEnabled,
                        ceqfpMemoryResCurrentRisingThresh,
                        ceqfpMemoryResCurrentFallingThresh
                    }
    STATUS          current
    DESCRIPTION
        "This group contains memory resource notification control
        objects."
    ::= { ciscoEntityQfpMIBGroups 6 }

ciscoEntityQfpMemoryResourceOvrflwGroup OBJECT-GROUP
    OBJECTS         {
                        ceqfpMemoryResTotalOvrflw,
                        ceqfpMemoryResInUseOvrflw,
                        ceqfpMemoryResFreeOvrflw,
                        ceqfpMemoryResLowFreeWatermarkOvrflw
                    }
    STATUS          current
    DESCRIPTION
        "This group contains collection of upper 32-bit QFP memory
        resource
        information."
    ::= { ciscoEntityQfpMIBGroups 7 }

ciscoEntityQfpMemoryHCResourceGroup OBJECT-GROUP
    OBJECTS         {
                        ceqfpMemoryHCResTotal,
                        ceqfpMemoryHCResInUse,
                        ceqfpMemoryHCResFree,
                        ceqfpMemoryHCResLowFreeWatermark
                    }
    STATUS          current
    DESCRIPTION
        "This group contains collection of high capacity(HC) objects of
        QFP memory resource information."
    ::= { ciscoEntityQfpMIBGroups 8 }

ceqfpThroughputGroup OBJECT-GROUP
    OBJECTS         {
                        ceqfpThroughputLicensedBW,
                        ceqfpThroughputLevel,
                        ceqfpThroughputInterval,
                        ceqfpThroughputThreshold,
                        ceqfpThroughputAvgRate,
                        ceqfpThroughputNotifEnabled
                    }
    STATUS          current
    DESCRIPTION
        "This group contains collection of throughput rate information."
    ::= { ciscoEntityQfpMIBGroups 9 }

END



























