-- ****************************************************
-- CISCO-ERR-DISABLE-MIB.my
-- MIB support for the Error Disable feature
--   
-- Copyright (c) 2006, 2008-2013, 2016 by Cisco Systems Inc.
-- All rights reserved.
--   
-- ****************************************************

CISCO-ERR-DISABLE-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    NOTIFICATION-TYPE,
    Unsigned32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    ifIndex
        FROM IF-MIB
    TEXTUAL-CONVENTION,
    TruthValue
        FROM SNMPv2-TC
    TimeIntervalSec
        FROM CISCO-TC
    VlanIndexOrZero
        FROM CISCO-PRIVATE-VLAN-MIB
    ciscoMgmt
        FROM CISCO-SMI;


ciscoErrDisableMIB MODULE-IDENTITY
    LAST-UPDATED    "201606020000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "This MIB module provides the ability for a Network
        Management Station (NMS) to configure and monitor the
        error-disable feature via SNMP.

        The error-disable feature allows other software
        features running in a system to operationally disable a
        system entity upon detecting abnormal conditions. 

        Examples of such a system entity include interfaces, a
        vlan configured in the system, or a VLAN allowed on
        specific layer 2 multi-vlan interface.

        More specific examples:

            a) When BPDU guard is enabled on an interface
            it is expected that no BPDU packets are received by
            the interface. If a BPDU packet is received, then the
            BPDU guard will operationally disable the
            interface. 

            b) Users can configure a particular threshold of
            broadcast packets received on an interface. If the
            number of packets received exceeds the threshold, then
            storm-control will disable the interface. 

            c) When unidirectional Link Detection (UDLD) detects a
            unidirectional link on an interface, it can disable
            the interface.

            d) On a trunk or a multi-vlan layer 2 port, if
            port-security detects violation on a particular vlan,
            then it can operationally disable that vlan on that
            port.

        The definition of 'abnormal condition' is under the
        control of features that make use of the error-disable
        feature to disable system entities.

        The error-disable feature supports the following
        configuration:

            1) Whether software features can in fact use the
            error-disable feature upon detecting abnormal
            conditions.
               NOTE: Some software features will ALWAYS use the
               error-disable feature to disable entities upon
               detection of error.

            2) Whether the system can attempt to automatically
            recover after a system entity has been disabled (e.g., 
            A system can attempt to bring up a physical interface
            which had been disabled earlier)

            3) If error recovery is possible, then the time
            interval to wait before the system starts the recovery
            attempt."
    REVISION        "201606020000Z"
    DESCRIPTION
        "Added the following new enumerations in
        CErrDisableFeatureID:
        other(36), portReinitLimitReached(37),
        adminRxBBCreditPerfBufIncomp(38), ficonNotEnabled(39),
        adminModeIncomp(40), adminSpeedIncomp(41), ncompAdminRxBBCredit(42),
        adminRxBufSizeIncomp(43), eppFailure(44), osmEPortUp(45),
        osmNonEPortUp(46), udldUniDir(47), udldTxRxLoop(48),
        udldNeighbourMismatch(49), udldEmptyEcho(50),
        udldAggrasiveModeLinkFailed(51), excessivePortInterrupts(52),
        channelErrDisabled(53), hwProgFailed(54),
        internalHandshakeFailed(55), stpInconsistencyOnVpcPeerLink(56),
        stpPortStateFailure(57), ipConflict(58),
        multipleMSapIdsRcvd(59), oneHundredPdusWithoutAck(60),
        and ipQosCompatCheckFailure(61)."
    REVISION        "201304230000Z"
    DESCRIPTION
        "Added ciscoErrDisableFeatureFlapGroup and
        a new enumeration flapControl(4) in 
        cErrDisableFeatureConfigurable."
    REVISION        "201010190000Z"
    DESCRIPTION
        "Added a new enumeration in CErrDisableFeatureID:
        tranceiverIncomp(35)."
    REVISION        "200903230000Z"
    DESCRIPTION
        "Added the following new enumerations in
        CErrDisableFeatureID:
        sfpConfigMismatch(24), communityLimit(25), invalidPolicy(26),
        lsGroup(27), ekey(28), portModeFailure(29), 
        pppoeIaRateLimit(30), oamRemoteCriticalEvent(31),
        oamRemoteDyingGasp(32), oamRemoteLinkFault(33),
        and mvrp(34). 

        Added the new enumeration detectShutdownVlan(3) 
        to cErrDisableFeatureConfigurable.

        Added ciscoErrDisableShutdownVlanGroup."
    REVISION        "200804070000Z"
    DESCRIPTION
        "Added the following new enumerations in
        CErrDisableFeatureID:
        packetBuffer(18), macLimit(19), linkMonitorFailure(20),
        oamRemoteFailure(21), dot1adIncompEtype(22), and
        dot1adIncompTunnel(23).

        cErrDisableInterfaceEvent notification is deprecated 
        and replaced by a new notification 
        cErrDisableInterfaceEventRev1.

        Modified the description of cErrDisableNotifEnable
        to add control for cErrDisableInterfaceEventRev1
        notification."
    REVISION        "200605310000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 548 }


ciscoErrDisableMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoErrDisableMIB 0 }

ciscoErrDisableMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoErrDisableMIB 1 }

ciscoErrDisableMIBConform  OBJECT IDENTIFIER
    ::= { ciscoErrDisableMIB 2 }

cErrDisableGlobalObjects  OBJECT IDENTIFIER
    ::= { ciscoErrDisableMIBObjects 1 }

cErrDisableFeatureObjects  OBJECT IDENTIFIER
    ::= { ciscoErrDisableMIBObjects 2 }

cErrDisableIfObjects  OBJECT IDENTIFIER
    ::= { ciscoErrDisableMIBObjects 3 }


-- Textual Conventions

CErrDisableFeatureID ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "An integer-value assigned to various features/events
        that can error disable a system entity

        udld: Unidirectional Link Detection

        bpduGuard: Spanning Tree BPDU Guard feature that prevents
        processing BPDU packets on an access interface

        channelMisconfig: General Link Aggregation mis-configuration

        pagpFlap: Cisco's PAGP Link Aggregation protocol errors

        dtpFlap: Dynamic Trunking Protocol errors

        linkFlap: Link State flapping

        l2ptGuard: L2 Protocol Tunnel errors

        dot1xSecurityViolation: 802.1x authentication violations

        portSecurity: Port Security violations

        gbicInvalid: Invalid GBIC errors (examples include
        unsupported GBIC being inserted)

        dhcpRateLimit: DHCP snooping rate limit violation

        unicastFlood: Unicast Flooding threshold violations

        vmps: VLAN Membership Policy Server feature related errors

        stormControl: storm control (broadcast/multicast/unicast)
        threshold violations

        inlinePower: Errors in inline power

        arpInspection: Errors detected by Dynamic Arp Inspection
        (DAI) feature

        portLoopback: Interface Loopback Error

        packetBuffer: Packet Buffer Error

        macLimit: Errors detected by Mac Address Limit feature

        linkMonitorFailure: Link Monitoring failure

        oamRemoteFailure: Remote Failure detected by Ethernet OAM
        (Operations, Administration, and Maintenance) feature   

        dot1adIncompEtype: 802.1ad Ether-type Incompatible errors

        dot1adIncompTunnel: 802.1ad Pdu Tunnel Incompatible errors

        sfpConfigMismatch: Mismatch on SFP configuration

        communityLimit: Vlan Community Limit violations

        invalidPolicy: QoS Policy violation

        lsGroup: Errors detected by Link State Group Tracking feature

        ekey: Errors detected by Error Key Mechanism

        portModeFailure: Port mode change failure

        pppoeIaRateLimit: Errors detected by PPPoE Intermediate Agent 
        Rate Limit feature

        oamRemoteCriticalEvent: Ethernet OAM Remote Critical Event 
        Failure  

        oamRemoteDyingGasp: Ethernet OAM Remote Dying Gasp Failure

        oamRemoteLinkFault: Ethernet OAM Remote Link Fault Failure

        mvrp: Errors detected by Multiple VLAN Registration Protocol

        tranceiverIncomp: Tranceiver incompatible errors

        other: Any other feature not covered by enumerations listed here

        portReinitLimitReached: Port reinitialization limit reached

        adminRxBBCreditPerfBufIncomp: Incompatible admin port rxbbcredit performance buffers

        ficonNotEnabled: Ficon not enabled

        adminModeIncomp: Incompatible port admin mode

        adminSpeedIncomp: Incompatible port admin speed

        adminRxBBCreditIncomp: Incompatible admin port rxbbcredit

        adminRxBufSizeIncomp: Incompatible admin port rxbufsize

        eppFailure: EPP Failure

        osmEPortUp: First interface in this group is E

        osmNonEPortUp: Other interfaces in this group are not shut

        udldUniDir: Unidirectional UDLD detected

        udldTxRxLoop: UDLD Tx-Rx loop

        udldNeighbourMismatch: UDLD neighbor mismatch

        udldEmptyEcho: UDLD empty echo

        udldAggrasiveModeLinkFailed: UDLD detected link failure in aggressive mode

        excessivePortInterrupts: Error disabled due to excessive port interrupts

        channelErrDisabled: Channel error-disabled

        hwProgFailed: hardware programming failed

        internalHandshakeFailed: Internal handshake failure

        stpInconsistencyOnVpcPeerLink: STP inconsistency on VPC peer-link

        stpPortStateFailure: STP has set port state to failure

        ipConflict: Error disabled due to IP address conflict

        multipleMSapIdsRcvd: DCX Multiple MSAP IDs recieved for the port

        oneHundredPdusWithoutAck: DCX Recieved 100 PDUs without ACK

        ipQosCompatCheckFailure: IP Qos DCBXP compat check failed"
    SYNTAX          INTEGER  {
                        udld(1),
                        bpduGuard(2),
                        channelMisconfig(3),
                        pagpFlap(4),
                        dtpFlap(5),
                        linkFlap(6),
                        l2ptGuard(7),
                        dot1xSecurityViolation(8),
                        portSecurityViolation(9),
                        gbicInvalid(10),
                        dhcpRateLimit(11),
                        unicastFlood(12),
                        vmps(13),
                        stormControl(14),
                        inlinePower(15),
                        arpInspection(16),
                        portLoopback(17),
                        packetBuffer(18),
                        macLimit(19),
                        linkMonitorFailure(20),
                        oamRemoteFailure(21),
                        dot1adIncompEtype(22),
                        dot1adIncompTunnel(23),
                        sfpConfigMismatch(24),
                        communityLimit(25),
                        invalidPolicy(26),
                        lsGroup(27),
                        ekey(28),
                        portModeFailure(29),
                        pppoeIaRateLimit(30),
                        oamRemoteCriticalEvent(31),
                        oamRemoteDyingGasp(32),
                        oamRemoteLinkFault(33),
                        mvrp(34),
                        tranceiverIncomp(35),
                        other(36),
                        portReinitLimitReached(37),
                        adminRxBBCreditPerfBufIncomp(38),
                        ficonNotEnabled(39),
                        adminModeIncomp(40),
                        adminSpeedIncomp(41),
                        adminRxBBCreditIncomp(42),
                        adminRxBufSizeIncomp(43),
                        eppFailure(44),
                        osmEPortUp(45),
                        osmNonEPortUp(46),
                        udldUniDir(47),
                        udldTxRxLoop(48),
                        udldNeighbourMismatch(49),
                        udldEmptyEcho(50),
                        udldAggrasiveModeLinkFailed(51),
                        excessivePortInterrupts(52),
                        channelErrDisabled(53),
                        hwProgFailed(54),
                        internalHandshakeFailed(55),
                        stpInconsistencyOnVpcPeerLink(56),
                        stpPortStateFailure(57),
                        ipConflict(58),
                        multipleMSapIdsRcvd(59),
                        oneHundredPdusWithoutAck(60),
                        ipQosCompatCheckFailure(61)
                    }

-- Global configuration objects

cErrDisableRecoveryInterval OBJECT-TYPE
    SYNTAX          TimeIntervalSec
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the error-disable recovery time
        interval.
        When a system entity is operationally disabled upon
        detecting abnormal condition by a particular feature,
        the system waits for a period equal to this time interval,
        and then re-enable the entity if automatic recovery is
        enabled for the feature." 
    ::= { cErrDisableGlobalObjects 1 }

cErrDisableNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether cErrDisableInterfaceEvent
        and cErrDisableInterfaceEventRev1
        notifications should be generated when a system entity is
        error-disabled." 
    ::= { cErrDisableGlobalObjects 2 }

cErrDisableNotifRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "Notification/Minute"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The value of this object specifies the maximum number of
        error-disable notifications the device will generate per
        minute. 

        A value of '0' specifies no limit and the device
        will generate a notification for each error-disable
        event." 
    ::= { cErrDisableGlobalObjects 3 }

cErrDisableFeatureTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CErrDisableFeatureEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the error-disable related info
        for each feature employing the error-disable
        feature."
    ::= { cErrDisableFeatureObjects 1 }

cErrDisableFeatureEntry OBJECT-TYPE
    SYNTAX          CErrDisableFeatureEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry is created for each feature that employs the
        error-disable feature."
    INDEX           { cErrDisableFeatureIndex } 
    ::= { cErrDisableFeatureTable 1 }

CErrDisableFeatureEntry ::= SEQUENCE {
        cErrDisableFeatureIndex              CErrDisableFeatureID,
        cErrDisableFeatureConfigurable       BITS,
        cErrDisableFeatureDetectEnable       TruthValue,
        cErrDisableFeatureRecoveryEnable     TruthValue,
        cErrDisableFeatureRecoveryInterval   TimeIntervalSec,
        cErrDisableFeatureDetectShutdownVlan TruthValue,
        cErrDisableFeatureMaxFlapCount       Unsigned32,
        cErrDisableFeatureFlapTimePeriod     Unsigned32
}

cErrDisableFeatureIndex OBJECT-TYPE
    SYNTAX          CErrDisableFeatureID
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies a feature that makes
        use of the error-disable feature." 
    ::= { cErrDisableFeatureEntry 1 }

cErrDisableFeatureConfigurable OBJECT-TYPE
    SYNTAX          BITS {
                        detectionEnable(0),
                        recoveryEnable(1),
                        recoveryInterval(2),
                        detectShutdownVlan(3),
                        flapControl(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates whether the error-disable related
        configuration is configurable for this feature. If a bit
        is set to 1, then the corresponding error-disable
        configuration can be configured.

        'detectionEnable'    - indicates the error-disable detection
                               can be enabled/disabled for this feature
                               via cErrDisableFeatureDetectEnable.
        'recoveryEnable'     - indicates the error-disable recovery
                               can be enabled/disabled for this feature
                               via cErrDisableFeatureRecoveryEnable.
        'recoveryInterval'   - indicates the error-disable recovery
                               Interval can be configured via
                               cErrDisableFeatureRecoveryInterval.
        'detectShutdownVlan' - indicates the error-disable detection
                               shutdown vlan mode can be configured for
                               this feature via 
                               cErrDisableFeatureDetectShutdownVlan. 
        'flapControl'        - indicates the error-disable flap control
                               can be configured via 
                               cErrDisableFeatureMaxFlapCount and
                               cErrDisableFeatureFlapTimePeriod." 
    ::= { cErrDisableFeatureEntry 2 }

cErrDisableFeatureDetectEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the error-disable detection
        is enabled for the feature.

        Note:
           This object is read-write only for those features
           that are configurable, meaning:
           cErrDisableFeatureConfigurable.<featureIndex> has the
           first bit set to 1." 
    ::= { cErrDisableFeatureEntry 3 }

cErrDisableFeatureRecoveryEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the system can
        automatically recover a system entity that has been
        disabled by the feature." 
    ::= { cErrDisableFeatureEntry 4 }

cErrDisableFeatureRecoveryInterval OBJECT-TYPE
    SYNTAX          TimeIntervalSec
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the error-recovery time interval
        that will be used by the system for any system entity that
        is error-disabled by this particular feature.

        If the value of this object is '0', then the device will
        use the value specified by the global configuration object
        cErrDisableRecoveryInterval." 
    ::= { cErrDisableFeatureEntry 5 }

cErrDisableFeatureDetectShutdownVlan OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether shutting down the violating
        VLAN on an interface is enabled or not. The value of 'true'
        indicates that shutting down the violating VLAN on an 
        interface is enabled. The value of 'false' indicates that 
        shutting down the violating VLAN on an interface is 
        disabled." 
    ::= { cErrDisableFeatureEntry 6 }

cErrDisableFeatureMaxFlapCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the maximum number of flaps that
        are allowed to occur before setting to error disable state.
        A read-only value of zero indicates that no flap control
        is present." 
    ::= { cErrDisableFeatureEntry 7 }

cErrDisableFeatureFlapTimePeriod OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the period of time counting the number of
        flaps that are allowed before setting to error disable state.
        A read-only value of zero indicates that no flap control
        is present." 
    ::= { cErrDisableFeatureEntry 8 }
 


cErrDisableIfStatusTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CErrDisableIfStatusEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides interface (port) specific
        error-disable status information. Each conceptual row
        provides status information about a {interface, vlan}
        disabled by a feature.

        On a trunk or multi-vlan access interface, a given vlan on
        the interface can be error-disabled. In this case, the row is
        indexed by the ifIndex for the interface and the vlan
        index corresponding to the vlan in question.

        If the interface is carrying only 1 vlan or the entire
        trunk interface is error-disabled (due to link flaps, for
        example) then the vlan index portion of the row index is
        0."
    ::= { cErrDisableIfObjects 1 }

cErrDisableIfStatusEntry OBJECT-TYPE
    SYNTAX          CErrDisableIfStatusEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A collection of objects that specify the status of an
        error-disabled Interface or {interface, vlan}."
    INDEX           {
                        ifIndex,
                        cErrDisableIfStatusVlanIndex
                    } 
    ::= { cErrDisableIfStatusTable 1 }

CErrDisableIfStatusEntry ::= SEQUENCE {
        cErrDisableIfStatusVlanIndex     VlanIndexOrZero,
        cErrDisableIfStatusCause         CErrDisableFeatureID,
        cErrDisableIfStatusTimeToRecover TimeIntervalSec
}

cErrDisableIfStatusVlanIndex OBJECT-TYPE
    SYNTAX          VlanIndexOrZero
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the vlan of the given interface
        that has been error-disabled. If the physical interface is
        error-disabled then the value of this object is 0." 
    ::= { cErrDisableIfStatusEntry 1 }

cErrDisableIfStatusCause OBJECT-TYPE
    SYNTAX          CErrDisableFeatureID
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the feature/event that caused the
        {interface, vlan} (or the entire interface) to be
        error-disabled." 
    ::= { cErrDisableIfStatusEntry 2 }

cErrDisableIfStatusTimeToRecover OBJECT-TYPE
    SYNTAX          TimeIntervalSec
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Time left before the system attempts an automatic
        recovery of the interface or the vlan of the given 
        interface. If no recovery is scheduled, then the value 
        of this object is '0'." 
    ::= { cErrDisableIfStatusEntry 3 }
 

-- Notifications

cErrDisableNotificationsPrefix  OBJECT IDENTIFIER
    ::= { ciscoErrDisableMIBNotifs 1 }


cErrDisableInterfaceEvent NOTIFICATION-TYPE
    OBJECTS         { cErrDisableIfStatusCause }
    STATUS          deprecated
    DESCRIPTION
        "The cErrDisableInterfaceEvent is generated when an interface
        or {interface, vlan} is error-disabled by the feature
        specified in cErrDisableIfStatusCause.

        cErrDisableInterfaceEvent is deprecated and replaced by 
        cErrDisableInterfaceEventRev1."
   ::= { cErrDisableNotificationsPrefix 1 }

cErrDisableInterfaceEventRev1 NOTIFICATION-TYPE
    OBJECTS         { cErrDisableIfStatusCause }
    STATUS          current
    DESCRIPTION
        "The cErrDisableInterfaceEventRev1 is generated when an
        interface or {interface, vlan} is error-disabled by the 
        feature specified in cErrDisableIfStatusCause.

        cErrDisableInterfaceEventRev1 deprecates 
        cErrDisableInterfaceEvent to make it RFC 2578 compliant. 
        According to section 8.5 of RFC 2578, the next
        to last sub-identifier in the name of any newly-defined
        notification must have the value zero."
   ::= { ciscoErrDisableMIBNotifs 2 }
-- MIB Conformance statements

ciscoErrDisableMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoErrDisableMIBConform 1 }

ciscoErrDisableMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoErrDisableMIBConform 2 }


ciscoErrDisableMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the cisco errdisable MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoErrDisableGlobalCfgGroup,
                        ciscoErrDisableFeatureCfgGroup,
                        ciscoErrDisableIfStatusGroup
                    }

    GROUP           ciscoErrDisableNotifCfgGroup
    DESCRIPTION
        "This group is mandatory if the managed system
        supports notifications for error-disable events."

    GROUP           ciscoErrDisableNotifGroup
    DESCRIPTION
        "This group is mandatory if the managed system
        supports notifications for error-disable events."
    ::= { ciscoErrDisableMIBCompliances 1 }

ciscoErrDisableMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the cisco errdisable MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoErrDisableGlobalCfgGroup,
                        ciscoErrDisableFeatureCfgGroup,
                        ciscoErrDisableIfStatusGroup
                    }

    GROUP           ciscoErrDisableNotifCfgGroup
    DESCRIPTION
        "This group is mandatory if the managed system
        supports notifications for error-disable events."

    GROUP           ciscoErrDisableNotifGroupRev1
    DESCRIPTION
        "This group is mandatory if the managed system
        supports notifications for error-disable events."

    GROUP           ciscoErrDisableShutdownVlanGroup
    DESCRIPTION
        "This group is mandatory if the managed system
        supports the configuration on error-disable 
        detection shutdown vlan mode."

    OBJECT          cErrDisableRecoveryInterval
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableNotifEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableNotifRate
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableFeatureDetectEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableFeatureRecoveryEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableFeatureRecoveryInterval
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableFeatureDetectShutdownVlan
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."
    ::= { ciscoErrDisableMIBCompliances 2 }

ciscoErrDisableMIBComplianceRev2 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for the cisco errdisable MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoErrDisableGlobalCfgGroup,
                        ciscoErrDisableFeatureCfgGroup,
                        ciscoErrDisableIfStatusGroup
                    }

    GROUP           ciscoErrDisableNotifCfgGroup
    DESCRIPTION
        "This group is mandatory if the managed system
        supports notifications for error-disable events."

    GROUP           ciscoErrDisableNotifGroupRev1
    DESCRIPTION
        "This group is mandatory if the managed system
        supports notifications for error-disable events."

    GROUP           ciscoErrDisableShutdownVlanGroup
    DESCRIPTION
        "This group is mandatory if the managed system
        supports the configuration on error-disable 
        detection shutdown vlan mode."

    GROUP           ciscoErrDisableFeatureFlapGroup
    DESCRIPTION
        "This group is mandatory if the managed system
        supports the configuration on error-disable 
        flap control."

    OBJECT          cErrDisableRecoveryInterval
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableNotifEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableNotifRate
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableFeatureDetectEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableFeatureRecoveryEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableFeatureRecoveryInterval
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableFeatureDetectShutdownVlan
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableFeatureMaxFlapCount
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cErrDisableFeatureFlapTimePeriod
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."
    ::= { ciscoErrDisableMIBCompliances 3 }

-- Object groups

ciscoErrDisableGlobalCfgGroup OBJECT-GROUP
    OBJECTS         { cErrDisableRecoveryInterval }
    STATUS          current
    DESCRIPTION
        "A collection of objects to configure error-disable
        functionality."
    ::= { ciscoErrDisableMIBGroups 1 }

ciscoErrDisableFeatureCfgGroup OBJECT-GROUP
    OBJECTS         {
                        cErrDisableFeatureConfigurable,
                        cErrDisableFeatureDetectEnable,
                        cErrDisableFeatureRecoveryEnable,
                        cErrDisableFeatureRecoveryInterval
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects to manage the configuration of
        the error-disable feature."
    ::= { ciscoErrDisableMIBGroups 2 }

ciscoErrDisableIfStatusGroup OBJECT-GROUP
    OBJECTS         {
                        cErrDisableIfStatusCause,
                        cErrDisableIfStatusTimeToRecover
                    }
    STATUS          current
    DESCRIPTION
        "A collection of error-disable interface status objects."
    ::= { ciscoErrDisableMIBGroups 3 }

ciscoErrDisableNotifCfgGroup OBJECT-GROUP
    OBJECTS         {
                        cErrDisableNotifEnable,
                        cErrDisableNotifRate
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects to configure error-disable
        notifications."
    ::= { ciscoErrDisableMIBGroups 4 }

ciscoErrDisableNotifGroup NOTIFICATION-GROUP
   NOTIFICATIONS    { cErrDisableInterfaceEvent }
    STATUS          deprecated
    DESCRIPTION
        "A collection of error-disable notification objects."
    ::= { ciscoErrDisableMIBGroups 5 }

ciscoErrDisableNotifGroupRev1 NOTIFICATION-GROUP
   NOTIFICATIONS    { cErrDisableInterfaceEventRev1 }
    STATUS          current
    DESCRIPTION
        "A collection of error-disable notification objects."
    ::= { ciscoErrDisableMIBGroups 6 }

ciscoErrDisableShutdownVlanGroup OBJECT-GROUP
    OBJECTS         { cErrDisableFeatureDetectShutdownVlan }
    STATUS          current
    DESCRIPTION
        "A collection of objects to manage the configuration of
        error-disable detection shutdown vlan mode."
    ::= { ciscoErrDisableMIBGroups 7 }

ciscoErrDisableFeatureFlapGroup OBJECT-GROUP
    OBJECTS         {
                        cErrDisableFeatureMaxFlapCount,
                        cErrDisableFeatureFlapTimePeriod
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects to manage the configuration of
        the error-disable flap control."
    ::= { ciscoErrDisableMIBGroups 8 }

END




