-- *****************************************************************
-- CISCO-TRUSTSEC-INTERFACE-CAPABILITY.my:
-- Cisco CISCO-TRUSTSEC-INTERFACE-MIB AGENT-CAPABILITIES
--   
-- Jun 2009, Liwei Lue
--   
-- Copyright (c) 2009-2012 by Cisco Systems, Inc.
-- All rights reserved.
-- ****************************************************************

CISCO-TRUSTSEC-INTERFACE-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    Unsigned32,
    Integer32
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    RowStatus
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoTrustSecInterfaceCapability MODULE-IDENTITY
    LAST-UPDATED    "201209040000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems, Inc
            Customer Service

            Postal: 170 West Tasman Drive
                    San Jose, CA  95134
                    USA

               Tel: +1 800 553-NETS

            E-mail: cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "The capabilities description of CISCO-TRUSTSEC-INTERFACE-MIB."
    REVISION        "201209040000Z"
    DESCRIPTION
        "Added capability statement
        ciscoTrustSecInterfaceCapV15R0101SYPCat6k."
    REVISION        "201010300000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 597 }



ciscoTrustSecInterfaceCapV12R0250SYPCat6k AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(50)SY on Catalyst 6000/6500
                     series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-TRUSTSEC-INTERFACE-MIB capabilities."

    SUPPORTS        CISCO-TRUSTSEC-INTERFACE-MIB
    INCLUDES        {
                        ciscoTrustSecIfMIBIfConfigGroup,
                        ciscoTrustSecIfMIBDot1xGroup,
                        ciscoTrustSecIfMIBManualGroup,
                        ciscoTrustSecIfMIBL3ForwardGroup,
                        ciscoTrustSecIfMIBStatusGroup,
                        ciscoTrustSecIfMIBStatisticGroup,
                        ciscoTrustSecIfMIBAuthorizationGroup,
                        ciscoTrustSecIfMIBIfcStatisticGroup,
                        ciscoTrustSecIfMIBEventStatisticGroup,
                        ciscoTrustSecIfMIBIfModeStatisticGroup
                    }
    VARIATION       ctsiIfDot1xReauthInterval
    SYNTAX          Integer32 (0..2147482)
    DESCRIPTION
        "Only a limited set of values is supported."

    VARIATION       ctsiIfDot1xSapModeList
    SYNTAX          OCTET STRING (SIZE (1..4))
    DESCRIPTION
        "Only a limited set of values is supported."

    VARIATION       ctsiIfDot1xStorageType
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       ctsiIfDot1xRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only a limited set of enumerated values is supported."

    VARIATION       ctsiIfManualDynamicPeerId
    SYNTAX          SnmpAdminString (SIZE (0..128))
    DESCRIPTION
        "Only a limited set of values are supported."

    VARIATION       ctsiIfManualSapModeList
    SYNTAX          OCTET STRING (SIZE (1..4))
    DESCRIPTION
        "Only a limited set of values are supported."

    VARIATION       ctsiIfManualStorageType
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       ctsiIfManualRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only a limited set of enumerated values is supported."

    VARIATION       ctsiIfL3ForwardStorageType
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       ctsiIfL3ForwardRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only a limited set of enumerated values is supported."

    ::= { ciscoTrustSecInterfaceCapability 1 }

ciscoTrustSecInterfaceCapV15R0101SYPCat6k AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 15.1(1)SY on Catalyst 6000/6500
                     series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-TRUSTSEC-INTERFACE-MIB capabilities."

    SUPPORTS        CISCO-TRUSTSEC-INTERFACE-MIB
    INCLUDES        {
                        ciscoTrustSecIfMIBIfConfigGroup,
                        ciscoTrustSecIfMIBDot1xGroup,
                        ciscoTrustSecIfMIBManualGroup,
                        ciscoTrustSecIfMIBL3ForwardGroup,
                        ciscoTrustSecIfMIBStatusGroup,
                        ciscoTrustSecIfMIBStatisticGroup,
                        ciscoTrustSecIfMIBAuthorizationGroup,
                        ciscoTrustSecIfMIBIfcStatisticGroup,
                        ciscoTrustSecIfMIBEventStatisticGroup,
                        ciscoTrustSecIfMIBIfModeStatisticGroup,
                        ciscoTrustSecIfMIBNotifsCtrlGrp,
                        ciscoTrustSecIfMIBNotifsOnlyInfoGrp,
                        ciscoTrustSecIfMIBNotifsGrp
                    }
    VARIATION       ctsiIfDot1xReauthInterval
    SYNTAX          Integer32 (0..2147482)
    DESCRIPTION
        "Only a limited set of values is supported."

    VARIATION       ctsiIfDot1xSapModeList
    SYNTAX          OCTET STRING (SIZE (1..4))
    DESCRIPTION
        "Only a limited set of values is supported."

    VARIATION       ctsiIfDot1xStorageType
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       ctsiIfDot1xRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only a limited set of enumerated values is supported."

    VARIATION       ctsiIfManualDynamicPeerId
    SYNTAX          SnmpAdminString (SIZE (0..128))
    DESCRIPTION
        "Only a limited set of values are supported."

    VARIATION       ctsiIfManualSapModeList
    SYNTAX          OCTET STRING (SIZE (1..4))
    DESCRIPTION
        "Only a limited set of values are supported."

    VARIATION       ctsiIfManualStorageType
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       ctsiIfManualRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only a limited set of enumerated values is supported."

    VARIATION       ctsiIfL3ForwardStorageType
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       ctsiIfL3ForwardRowStatus
    SYNTAX          RowStatus {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only a limited set of enumerated values is supported."

    ::= { ciscoTrustSecInterfaceCapability 2 }

END





