-- *********************************************************************
-- CISCO-ST-TC.my: Storage TC Mib
--   
-- September 2002, Vinay Gaonkar
--   
-- Copyright (c) 2002-2008-2012 by cisco Systems Inc.
-- All rights reserved.
--   
-- *******************************************************************

CISCO-ST-TC DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    Integer32
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    ciscoModules
        FROM CISCO-SMI;


storageTextualConventions MODULE-IDENTITY
    LAST-UPDATED    "201208080000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service
            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA
            Tel: +1 800 553 -NETS
            E-mail: cs-san@cisco.com"
    DESCRIPTION
        "This module defines textual conventions used in
        Storage Area Network technology specific mibs."
    REVISION        "201208080000Z"
    DESCRIPTION
        "Added sixteenG and automaxSixteenG in fcIfSpeed"
    REVISION        "201107260000Z"
    DESCRIPTION
        "-Added following enum to FcIfSpeed:
        autoMaxEightG."
    REVISION        "201012240000Z"
    DESCRIPTION
        "-Added following enums to FcIfSpeed:
        autoMax4G, eightG and tenG."
    REVISION        "200805160000Z"
    DESCRIPTION
        "-Added following enums to FcPortTypes
        TEXTUAL CONVENTION
        npPort, tfPort, tnpPort
        -Added following enums to InterfaceOperMode 
        TEXTUAL CONVENTION.
        npPort, tfPort, tnpPort
        -Added following enums to FcPortModuleTypes
        TEXTUAL CONVENTION
        sfpDwdm, qsfp, x2Dwdm
        - Updated the description of the following objects:
        FcPortTxTypes,
        FcNameId."
    REVISION        "200512170000Z"
    DESCRIPTION
        "- Added following TCs
        FcIfSfpDiagLevelType 
        FcIfServiceStateType
        - Added following enums in FcPortModuleTypes
        xfp, x2Short, x2Medium, x2Tall, xpakShort, 
        xpakMedium, xpakTall and xenpak. 
        - Added following enums in FcPortTxTypes. 
        tenGigBaseSr, tenGigBaseLr, tenGigBaseEr, 
        tenGigBaseLx4, tenGigBaseSw, tenGigBaseLw, 
        tenGigBaseEw. 
        - Added following enums in FcIfSpeed 
        fourG and autoMaxTwoG."
    REVISION        "200405180000Z"
    DESCRIPTION
        "Added new textual convention 'InterfaceOperMode'."
    REVISION        "200309260000Z"
    DESCRIPTION
        "Obtained the OID for this MIB."
    REVISION        "200308070000Z"
    DESCRIPTION
        "Added stPort(15) to FcPortTypes."
    REVISION        "200210040000Z"
    DESCRIPTION
        "Added fvPort and portOperDown to FcPortTypes.
        Added FcAddress and FcAddressType."
    REVISION        "200209240000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoModules 4 }



VsanIndex ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The VSAN id of a VSAN which uniquely identifies
        a VSAN within a fabric. VSAN id is 12-bit 
        wide; so theoretically, 4096 VSANs can be defined in 
        a fabric and this device can be part of. However, VSAN 
        numbers 0 , 4094 and 4095 are reserved."
    SYNTAX          Integer32 (1..4094)

DomainId ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The Domain Id of the switch. This is assigned
        dynamically if the Domain Manager is enabled on 
        the switch or could be configured statically by 
        the user."
    SYNTAX          Integer32 (1..239)

DomainIdOrZero ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The Textual convention is an extension to
        textual convetion 'DomainId'. It includes 
        the value '0'in addition the range 1-239.
        Value '0' indicates that Domain Id has  
        been neither configured nor assigned."
    SYNTAX          Integer32 (0..239)

FcAddressId ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents Fibre Channel Address ID, a 24-bit
        value unique within the address space of a Fabric."
    SYNTAX          OCTET STRING (SIZE (3))

FcNameId ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents the World Wide Name (WWN) associated with
        a Fibre Channel (FC) entity. A WWN is a 64 bit address
        to uniquely identify each entity within a Fibre Channel
        fabric."

    REFERENCE
        "Fibre Channel Framing and Signaling (FC-FS) Rev 1.70
               - Section 14 Name_Indentifier Formats."
    SYNTAX          OCTET STRING (SIZE (8))

FcNameIdOrZero ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The World Wide Name (WWN) associated with a Fibre Channel
        (FC) entity.  WWNs were initially defined as 64-bits in
        length.  The latest definition (for future use) is 128-bits
        long.  The zero-length string value is used in circumstances
        where the WWN is unassigned/unknown."
    SYNTAX          OCTET STRING (SIZE (0 | 8 | 16))

FcClassOfServices ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents the class of service capability of an
        NxPort or FxPort."
    SYNTAX          BITS {
                        classF(0),
                        class1(1),
                        class2(2),
                        class3(3),
                        class4(4),
                        class5(5),
                        class6(6)
                    }

FcPortTypes ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents fibre channel port types:
        auto (1)   - Mode is determined by port initialization 
                    scheme.
        fPort (2)  - Fibre channel fabric port. 
        flPort (3) - Fibre channel arbitrated loop port.
        ePort (4)  - Fabric Expansion port.
        bPort (5)  - Bridging port.
        fxPort (6) - This port can only be f_port or fl_port.
        sdPort (7) - SPAN destination port. SD_ports transmit 
                    traffic copied from one or more source ports
                    for monitoring purposes.        
        tlPort (8) - Translation loop port.
        nPort (9)   - Fibre channel N port.
        nlPort (10) - Fibre channel NL port.
        nxPort (11) - This port can only be n_port or nl_port.

          -- read only port types.
        tePort (12) - Trunking e_port.
                     Note: A port which is administratively set
                     to 'ePort', will operationally have type
                     'tePort' if fcIfOperTrunkMode has the value
                     'trunk'.
        fvPort (13) - Virtual Port.
        portOperDown (14) - port operationally down
                            If a port is operationally down, the
                            port mode is unknown. In such cases
                            the operational port mode is shown 
                            as 'portOperDown'. 
        stPort (15) - SPAN Tunnel destination port.
        npPort (16) - N Proxy port mode applicable only to N-port
                      Virtualizer (NPV)
        tfPort (17) - Trunking fibre channel fabric port.
        tnpPort (18) - Trunking N Proxy port mode applicable only
                      to N-port Virtualizer (NPV)."
    SYNTAX          INTEGER  {
                        auto(1),
                        fPort(2),
                        flPort(3),
                        ePort(4),
                        bPort(5),
                        fxPort(6),
                        sdPort(7),
                        tlPort(8),
                        nPort(9),
                        nlPort(10),
                        nxPort(11),
                        tePort(12),
                        fvPort(13),
                        portOperDown(14),
                        stPort(15),
                        npPort(16),
                        tfPort(17),
                        tnpPort(18)
                    }

FcPortTxTypes ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents port transciever technology types.
        unknown (1) - unknown
        longWaveLaser (2) - 1550nm laser
        shortWaveLaser (3) - 850nm laser
        longWaveLaserCostReduced (4) - 1310nm laser
        electrical (5) - electrical 
        tenGigBaseSr (6)  - 10GBASE-SR 850nm laser
        tenGigBaseLr (7)  - 10GBASE-LR 1310nm laser
        tenGigBaseEr (8)  - 10GBASE-ER 1550nm laser
        tenGigBaseLx4 (9) - 10GBASE-LX4 WWDM 1300nm laser
        tenGigBaseSw (10)  - 850nm laser
        tenGigBaseLw (11) - 1310nm laser
        tenGigBaseEw (12) - 1550nm laser
        ."

    REFERENCE
        "IEEE Std 802.3-2005 carrier sense multiple access 
        with collision detection (CSMA/CD) access method 
        and physical layer specification."
    SYNTAX          INTEGER  {
                        unknown(1),
                        longWaveLaser(2),
                        shortWaveLaser(3),
                        longWaveLaserCostReduced(4),
                        electrical(5),
                        tenGigBaseSr(6),
                        tenGigBaseLr(7),
                        tenGigBaseEr(8),
                        tenGigBaseLx4(9),
                        tenGigBaseSw(10),
                        tenGigBaseLw(11),
                        tenGigBaseEw(12)
                    }

FcPortModuleTypes ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents module type of the port connector. This
        object refers to the hardware implementation of the port.
        The enums are defined as per FC-GS-4 standard.
        unknown             (1) - unknown
        other               (2) - other
        gbic                (3) - gbic (gigabit interface card)
        embedded            (4) - gbic is part of the line card 
                                  and is unremovable
        glm                 (5) - if its a gigabit link module 
                                  (GLM). A GLM has a different 
                                  form factor than GBIC. GLM is 
                                  not supported by our switch.
        gbicWithSerialID    (6) - If GBIC serial id can be read
        gbicWithoutSerialID (7) - If GBIC serial id cannot be read
        sfpWithSerialID     (8) - If small form factor (SFP) 
                                  pluggable GBICs serial id can 
                                  be read
        sfpWithoutSerialID  (9) - If small form factor (SFP) 
                                  pluggable GBICs serial id 
                                  cannot be read
        The following enums are module types for 10 gigabit small 
        form factor pluggable sfp port connectors.
        xfp                (10) - xfp 
        x2Short            (11) - x2 short 
        x2Medium           (12) - x2 medium
        x2Tall             (13) - x2 tall
        xpakShort          (14) - xpak short
        xpakMedium         (15) - xpak medium
        xpakTall           (16) - xpak tall
        xenpak             (17) - xenpak
        sfpDwdm            (18) - DWDM SFP type
        qsfp               (19) - Quad small form-factor (QSFP) 
                                                          pluggable type
        x2Dwdm             (20) - x2 DWDM
        ."
    SYNTAX          INTEGER  {
                        unknown(1),
                        other(2),
                        gbic(3),
                        embedded(4),
                        glm(5),
                        gbicWithSerialID(6),
                        gbicWithoutSerialID(7),
                        sfpWithSerialID(8),
                        sfpWithoutSerialID(9),
                        xfp(10),
                        x2Short(11),
                        x2Medium(12),
                        x2Tall(13),
                        xpakShort(14),
                        xpakMedium(15),
                        xpakTall(16),
                        xenpak(17),
                        sfpDwdm(18),
                        qsfp(19),
                        x2Dwdm(20)
                    }

FcIfSpeed ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents the speed of a fibre channel port.
        Following are the meanings of the enumerated values:
          auto      (1) - Negotiate to determine the speed 
                          automatically.
          oneG      (2) - 1Gbit 
          twoG      (3) - 2Gbit
          fourG     (4) - 4Gbit 
          autoMaxTwoG (5)  - Negotiate to determine the 
                             speed automatically upto a 
                             maximum of 2Gbit.
          eightG    (6) - 8Gbit
          autoMaxFourG (7) - Negotiate to determine the
                             speed automatically upto a
                             maximum of 4Gbit.          
          tenG      (8) - 10GBit.
          autoMaxEightG (9) - Negotiate to determine the
                             speed automatically upto a
                             maximum of 8Gbit.
          sixteenG  (10) - 16GBit.
          autoMaxSixteenG (11) - Negotiate to determine the
                             speed automatically upto a
                             maximum of 16Gbit."
    SYNTAX          INTEGER  {
                        auto(1),
                        oneG(2),
                        twoG(3),
                        fourG(4),
                        autoMaxTwoG(5),
                        eightG(6),
                        autoMaxFourG(7),
                        tenG(8),
                        autoMaxEightG(9),
                        sixteenG(10),
                        autoMaxSixteenG(11)
                    }

PortMemberList ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "A list of ifIndex's of the ports that are members of
        this list.

        The value of this object is a concatenation of zero or
        more 4-octet strings, where each 4-octet string contains
        a 32-bit ifIndex value in network byte order.

        A zero length string value means this list has no
        members."
    SYNTAX          OCTET STRING (SIZE (0..64))

FcAddress ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents either the Fibre Channel Address ID or
        the World Wide Name associated with a Fibre
        Channel (FC) Entity."
    SYNTAX          OCTET STRING (SIZE (3 | 8))

FcAddressType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Denotes if a Fibre Channel Address is
        a World Wide Name (WWN) or a Fibre
        Channel Address ID (FCID).
        wwn(1) - address is WWN.
        fcid(2) - address is FCID."
    SYNTAX          INTEGER  {
                        wwn(1),
                        fcid(2)
                    }

InterfaceOperMode ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents the operational mode of an interface
        auto (1) - Mode is determined by port initialization
                   scheme.
        fPort (2) - Fibre channel fabric port.
        flPort (3) - Fibre channel arbitrated loop port.
        ePort (4)  - Fabric Expansion port.
        bPort (5)  - Bridging port.
        fxPort (6) - This port can only be f_port or fl_port.
        sdPort (7) - SPAN destination port. SD_ports transmit
                     traffic copied from one or more source
                     ports for monitoring purposes.
        tlPort (8) - Translation loop port.
        nPort (9)   - Fibre channel N port.
        nlPort (10) - Fibre channel NL port.
        nxPort (11) - This port can only be n_port or nl_port.

        -- read only port types.
        tePort (12) - Trunking e_port.
                  Note: A port which is administratively set
                  to 'ePort', will operationally have type
                  'tePort' if fcIfOperTrunkMode has the value
                  'trunk'.
        fvPort (13) - Virtual Port.
        portOperDown (14) - port operationally down
                          If a port is operationally down, the
                          port mode is unknown. In such cases
                          the operational port mode is shown
                          as 'portOperDown'.
        stPort (15) - SPAN Tunnel destination port.
        mgmtPort(16) - Mgmt Port.
        ipsPort(17) - Ethernet Port.
        evPort(18) - FCIP tunnels on Ethernet ports.
        npPort (19) - N Proxy port mode applicable only 
                      to N-port Virtualizer (NPV).
        tfPort (20) - Trunking fibre channel fabric port.
        tnpPort (21) - Trunking N Proxy port mode applicable only
                              to N-port Virtualizer (NPV)."
    SYNTAX          INTEGER  {
                        auto(1),
                        fPort(2),
                        flPort(3),
                        ePort(4),
                        bPort(5),
                        fxPort(6),
                        sdPort(7),
                        tlPort(8),
                        nPort(9),
                        nlPort(10),
                        nxPort(11),
                        tePort(12),
                        fvPort(13),
                        portOperDown(14),
                        stPort(15),
                        mgmtPort(16),
                        ipsPort(17),
                        evPort(18),
                        npPort(19),
                        tfPort(20),
                        tnpPort(21)
                    }

FcIfServiceStateType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents the service state of a Fibre Channel
        interface. Following are the meanings of the 
        enumerated values:

        inService    (1) - interface is in service and is
                      allowed to become operational.
        outOfService (2) - interface is removed from service 
                      and is not allowed to become 
                      operational."
    SYNTAX          INTEGER  {
                        inService(1),
                        outOfService(2)
                    }

FcIfSfpDiagLevelType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents the severity level of the SFP
        diagnostic information of an interface for 
        temperature, voltage, current, optical 
        transmit and receive power."
    SYNTAX          INTEGER  {
                        unknown(1),
                        normal(2),
                        lowWarning(3),
                        lowAlarm(4),
                        highWarning(5),
                        highAlarm(6)
                    }

END


