-- *****************************************************************
-- CISCO-VPC-CAPABILITY.my:
-- Cisco CISCO-VPC-MIB AGENT-CAPABILITIES
--   
-- July 2013, Alex Zhang
--   
-- Copyright (c) 2013 by cisco Systems Inc.
-- All rights reserved.
--   
-- *****************************************************************

CISCO-VPC-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoVpcCapability MODULE-IDENTITY
    LAST-UPDATED    "201307100000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "The capabilities description of CISCO-VPC-MIB."
    REVISION        "201307100000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 619 }



ciscoVpcCapNxOSV06R0202PN7K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco NX-OS 6.2(2) on Nexus 7000 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-VPC-MIB capabilities."

    SUPPORTS        CISCO-VPC-MIB
    INCLUDES        {
                        cVpcPeerKeepAliveConfigInfoGroup,
                        cVpcPeerKeepAliveStatusInfoGroup,
                        cVpcMIBRoleGroup,
                        cVpcMIBStatisticsGroup,
                        cVpcMIBPeerLinkStatusGroup,
                        cVpcMIBHostLinkStatusGroup
                    }
    VARIATION       cVpcPeerKeepAliveDestAddrType
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcPeerKeepAliveDestAddr
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcPeerKeepAliveSourceAddrType
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcPeerKeepAliveSourceAddr
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcPeerKeepAliveUdpPort
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcPeerKeepAliveInterval
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcPeerKeepAliveTimeout
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcPeerKeepAliveHoldTimeout
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcPeerKeepAliveTos
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcPeerKeepAlivePrecedence
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcPeerKeepAliveTosByte
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcPeerKeepAliveVrfName
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcSystemAdminMacAddress
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcSystemAdminPriority
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cVpcLocalRoleAdminPriority
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    ::= { ciscoVpcCapability 1 }

END








