-- *****************************************************************
-- CISCO-MAU-CAPABILITY.my:
-- Cisco MAU-MIB AGENT-CAPABILITIES
--   
-- Oct 2004, Liwei Lue
--   
-- Copyright (c) 2004-2014 by Cisco Systems Inc.
-- All rights reserved.
-- ****************************************************************

CISCO-MAU-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoMauCapability MODULE-IDENTITY
    LAST-UPDATED    "201407300000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "The capabilities description of MAU-MIB."
    REVISION        "201407300000Z"
    DESCRIPTION
        "Added capability statement ciscoMauCapV05R0003U0401PN3K."
    REVISION        "201109280000Z"
    DESCRIPTION
        "Added capability statement ciscoMauCapV12R0233SXJPCat6K
        and ciscoMauCapV15R0001SYPCat6K."
    REVISION        "200810280000Z"
    DESCRIPTION
        "Added capability statement
        ciscoMauCapV12R0233SXIPCat6K."
    REVISION        "200707130000Z"
    DESCRIPTION
        "Added capability statement
        ciscoMauCapV12R0233SXHPCat6K."
    REVISION        "200410220000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 411 }



ciscoMauCapCatOSV08R0401 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.4(1)."
    STATUS          current
    DESCRIPTION
        "MAU-MIB capabilities."

    SUPPORTS        MAU-MIB
    INCLUDES        {
                        mauIfGrpBasic,
                        mauIfGrpHighCapacity,
                        mauIfGrpJack,
                        mauIfGrpAutoNeg2
                    }
    VARIATION       ifMauType
    DESCRIPTION
        "Only limited set of object identifiers are
        supported in CatOS. They are
        dot3MauType10BaseTHD    (1.3.6.1.2.1.26.4.10)
        dot3MauType10BaseTFD    (1.3.6.1.2.1.26.4.11)
        dot3MauType10BaseFLHD   (1.3.6.1.2.1.26.4.12)
        dot3MauType10BaseFLFD   (1.3.6.1.2.1.26.4.13)
        dot3MauType100BaseT4    (1.3.6.1.2.1.26.4.14)
        dot3MauType100BaseTXHD  (1.3.6.1.2.1.26.4.15)
        dot3MauType100BaseTXFD  (1.3.6.1.2.1.26.4.16)
        dot3MauType100BaseFXHD  (1.3.6.1.2.1.26.4.17)
        dot3MauType100BaseFXFD  (1.3.6.1.2.1.26.4.18)
        dot3MauType1000BaseXHD  (1.3.6.1.2.1.26.4.21)
        dot3MauType1000BaseXFD  (1.3.6.1.2.1.26.4.22)
        dot3MauType1000BaseLXHD (1.3.6.1.2.1.26.4.23)
        dot3MauType1000BaseLXFD (1.3.6.1.2.1.26.4.24)
        dot3MauType1000BaseSXHD (1.3.6.1.2.1.26.4.25)
        dot3MauType1000BaseSXFD (1.3.6.1.2.1.26.4.26)
        dot3MauType1000BaseCXHD (1.3.6.1.2.1.26.4.27)
        dot3MauType1000BaseCXFD (1.3.6.1.2.1.26.4.28)
        dot3MauType1000BaseTHD  (1.3.6.1.2.1.26.4.29)
        dot3MauType1000BaseTFD  (1.3.6.1.2.1.26.4.30)
        dot3MauType10GigBaseLX4 (1.3.6.1.2.1.26.4.32)
        dot3MauType10GigBaseER  (1.3.6.1.2.1.26.4.34)
        dot3MauType10GigBaseLR  (1.3.6.1.2.1.26.4.35)
        dot3MauType10GigBaseSR  (1.3.6.1.2.1.26.4.36)
        dot3MauType10GigBaseEW  (1.3.6.1.2.1.26.4.38)
        dot3MauType10GigBaseLW  (1.3.6.1.2.1.26.4.39)
        dot3MauType10GigBaseSW  (1.3.6.1.2.1.26.4.40)"

    VARIATION       ifMauStatus
    SYNTAX          INTEGER  {
                        other(1),
                        unknown(2),
                        operational(3),
                        standby(4),
                        shutdown(5)
                    }
    DESCRIPTION
        "The 'reset' value cannot be supported with
        any current hardware.  Can not write values
        'other', 'unknown', and 'shutdown' in CatOS."

    VARIATION       ifMauMediaAvailable
    SYNTAX          INTEGER  {
                        other(1),
                        unknown(2),
                        available(3),
                        notAvailable(4)
                    }
    DESCRIPTION
        "Only limited set of enumerated values are
        supported."

    VARIATION       ifMauJabberState
    SYNTAX          INTEGER  {
                        other(1)
                    }
    DESCRIPTION
        "Only limited set of enumerated values are
        supported."

    VARIATION       ifMauJabberingStateEnters
    DESCRIPTION
        "Always return 0."

    VARIATION       ifMauFalseCarriers
    DESCRIPTION
        "Always return 0."

    VARIATION       ifMauDefaultType
    DESCRIPTION
        "Only limited set of object identifiers are
        supported in CatOS. They are
        dot3MauType10BaseTHD   (1.3.6.1.2.1.26.4.10)
        dot3MauType10BaseTFD   (1.3.6.1.2.1.26.4.11)
        dot3MauType10BaseFLHD  (1.3.6.1.2.1.26.4.12)
        dot3MauType10BaseFLFD  (1.3.6.1.2.1.26.4.13)
        dot3MauType100BaseT4   (1.3.6.1.2.1.26.4.14)
        dot3MauType100BaseTXHD (1.3.6.1.2.1.26.4.15)
        dot3MauType100BaseTXFD (1.3.6.1.2.1.26.4.16)
        dot3MauType100BaseFXHD (1.3.6.1.2.1.26.4.17)
        dot3MauType100BaseFXFD (1.3.6.1.2.1.26.4.18)
        dot3MauType1000BaseXHD (1.3.6.1.2.1.26.4.21)
        dot3MauType1000BaseXFD (1.3.6.1.2.1.26.4.22)
        dot3MauType1000BaseLXHD(1.3.6.1.2.1.26.4.23)
        dot3MauType1000BaseLXFD(1.3.6.1.2.1.26.4.24)
        dot3MauType1000BaseSXHD(1.3.6.1.2.1.26.4.25)
        dot3MauType1000BaseSXFD(1.3.6.1.2.1.26.4.26)
        dot3MauType1000BaseCXHD(1.3.6.1.2.1.26.4.27)
        dot3MauType1000BaseCXFD(1.3.6.1.2.1.26.4.28)
        dot3MauType1000BaseTHD (1.3.6.1.2.1.26.4.29)
        dot3MauType1000BaseTFD (1.3.6.1.2.1.26.4.30)
        dot3MauType10GigBaseLX4(1.3.6.1.2.1.26.4.32)
        dot3MauType10GigBaseER (1.3.6.1.2.1.26.4.34)
        dot3MauType10GigBaseLR (1.3.6.1.2.1.26.4.35)
        dot3MauType10GigBaseSR (1.3.6.1.2.1.26.4.36)
        dot3MauType10GigBaseEW (1.3.6.1.2.1.26.4.38)
        dot3MauType10GigBaseLW (1.3.6.1.2.1.26.4.39)
        dot3MauType10GigBaseSW (1.3.6.1.2.1.26.4.40)"

    VARIATION       ifJackType
    SYNTAX          INTEGER  {
                        other(1),
                        rj45S(3),
                        fiberSC(8),
                        telco(11),
                        mtrj(12)
                    }
    DESCRIPTION
        "Only limited set of enumerated values are
        supported."

    VARIATION       ifMauAutoNegConfig
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available on CatOS."

    VARIATION       ifMauAutoNegRestart
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available on CatOS."

    VARIATION       ifMauAutoNegCapAdvertisedBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseT(1), -- 10BASE-T half duplex
                        baseTFD(2), -- 10BASE-T full duplex
                        b100baseT4(3), -- 100BASE-T4
                        b100baseTX(4), -- 100BASE-TX half duplex
                        b100baseTXFD(5), -- 100BASE-TX full duplex
                        b100baseT2(6), -- 100BASE-T2 half duplex
                        b100baseT2FD(7), -- 100BASE-T2 full duplex
                        bFdxPause(8), -- PAUSE for full-duplex
                                       -- links
                        bFdxAPause(9), -- Asymmetric PAUSE for
                                       -- full-duplex links
                        bFdxSPause(10), -- Symmetric PAUSE for
                                        -- full-duplex links
                        bFdxBPause(11), -- Asymmetric and Symmetric
                                        -- PAUSE for full-duplex
                                        -- links
                        b1000baseX(12), -- 1000BASE-X, -LX, -SX,
                                        -- -CX half duplex
                        b1000baseXFD(13), -- 1000BASE-X, -LX, -SX,
                                          -- -CX full duplex
                        b1000baseT(14), -- 1000BASE-T half duplex
                        b1000baseTFD(15) -- 1000BASE-T full duplex                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values are
        supported."

    VARIATION       ifMauTypeListBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseTHD(10), -- 10BASE-T half duplex
                        b10baseTFD(11), -- 10BASE-T full duplex
                        b10baseFLHD(12), -- 10BASE-FL half duplex
                        b10baseFLFD(13), -- 10BASE-FL full duplex
                        b100baseT4(14), -- 100BASE-T4
                        b100baseTXHD(15), -- 100BASE-TX half duplex
                        b100baseTXFD(16), -- 100BASE-TX full duplex
                        b100baseFXHD(17), -- 100BASE-FX half duplex
                        b100baseFXFD(18), -- 100BASE-FX full duplex
                        b1000baseXHD(21), -- 1000BASE-X half duplex
                        b1000baseXFD(22), -- 1000BASE-X full duplex
                        b1000baseLXHD(23), -- 1000BASE-LX half duplex
                        b1000baseLXFD(24), -- 1000BASE-LX full duplex
                        b1000baseSXHD(25), -- 1000BASE-SX half duplex
                        b1000baseSXFD(26), -- 1000BASE-SX full duplex
                        b1000baseCXHD(27), -- 1000BASE-CX half duplex
                        b1000baseCXFD(28), -- 1000BASE-CX full duplex
                        b1000baseTHD(29), -- 1000BASE-T half duplex
                        b1000baseTFD(30), -- 1000BASE-T full duplex
                        b10GbaseLX4(32), -- 10GBASE-LX4
                        b10GbaseER(34), -- 10GBASE-ER
                        b10GbaseLR(35), -- 10GBASE-LR
                        b10GbaseSR(36), -- 10GBASE-SR
                        b10GbaseEW(38), -- 10GBASE-EW
                        b10GbaseLW(39), -- 10GBASE-LW
                        b10GbaseSW(40) -- 10GBASE-SW                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       ifMauAutoNegRemoteFaultAdvertised
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available on CatOS."

    VARIATION       ifMauAutoNegRemoteFaultReceived
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available on CatOS."

    VARIATION       ifMauAutoNegCapReceivedBits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available on CatOS."

    ::= { ciscoMauCapability 1 }

ciscoMauCapV12R0233SXHPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXH on Catalyst 6000/6500
                     series devices."
    STATUS          current
    DESCRIPTION
        "MAU-MIB capabilities."

    SUPPORTS        MAU-MIB
    INCLUDES        {
                        mauIfGrpBasic,
                        mauIfGrpHighCapacity,
                        mauIfGrpAutoNeg2
                    }
    VARIATION       ifMauStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauMediaAvailable
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauMediaAvailableStateExits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauJabberState
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauJabberingStateEnters
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauFalseCarriers
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauType
    DESCRIPTION
        "Only limited set of object identifiers are
        supported.
        unknownMauType         (0.0)
        dot3MauType10BaseTHD   (1.3.6.1.2.1.26.4.10)
        dot3MauType10BaseTFD   (1.3.6.1.2.1.26.4.11)
        dot3MauType100BaseTXHD (1.3.6.1.2.1.26.4.15)
        dot3MauType100BaseTXFD (1.3.6.1.2.1.26.4.16)
        dot3MauType100BaseFXHD (1.3.6.1.2.1.26.4.17)
        dot3MauType100BaseFXFD (1.3.6.1.2.1.26.4.18)
        dot3MauType1000BaseXHD (1.3.6.1.2.1.26.4.21)
        dot3MauType1000BaseXFD (1.3.6.1.2.1.26.4.22)
        dot3MauType1000BaseLXHD(1.3.6.1.2.1.26.4.23)
        dot3MauType1000BaseLXFD(1.3.6.1.2.1.26.4.24)
        dot3MauType1000BaseSXHD(1.3.6.1.2.1.26.4.25)
        dot3MauType1000BaseSXFD(1.3.6.1.2.1.26.4.26)
        dot3MauType1000BaseCXHD(1.3.6.1.2.1.26.4.27)
        dot3MauType1000BaseCXFD(1.3.6.1.2.1.26.4.28)
        dot3MauType1000BaseTHD (1.3.6.1.2.1.26.4.29)
        dot3MauType1000BaseTFD (1.3.6.1.2.1.26.4.30)
        dot3MauType10GigBaseX  (1.3.6.1.2.1.26.4.31)
        dot3MauType10GigBaseLX4(1.3.6.1.2.1.26.4.32)
        dot3MauType10GigBaseR  (1.3.6.1.2.1.26.4.33)
        dot3MauType10GigBaseER (1.3.6.1.2.1.26.4.34)
        dot3MauType10GigBaseLR (1.3.6.1.2.1.26.4.35)
        dot3MauType10GigBaseSR (1.3.6.1.2.1.26.4.36)
        dot3MauType10GigBaseW  (1.3.6.1.2.1.26.4.37)
        dot3MauType10GigBaseEW (1.3.6.1.2.1.26.4.38)
        dot3MauType10GigBaseLW (1.3.6.1.2.1.26.4.39)
        dot3MauType10GigBaseSW (1.3.6.1.2.1.26.4.40)"

    VARIATION       ifMauDefaultType
    DESCRIPTION
        "Only limited set of object identifiers are
        supported.
        unknownMauType         (0.0)
        dot3MauType10BaseTHD   (1.3.6.1.2.1.26.4.10)
        dot3MauType10BaseTFD   (1.3.6.1.2.1.26.4.11)
        dot3MauType100BaseTXHD (1.3.6.1.2.1.26.4.15)
        dot3MauType100BaseTXFD (1.3.6.1.2.1.26.4.16)
        dot3MauType100BaseFXHD (1.3.6.1.2.1.26.4.17)
        dot3MauType100BaseFXFD (1.3.6.1.2.1.26.4.18)
        dot3MauType1000BaseXHD (1.3.6.1.2.1.26.4.21)
        dot3MauType1000BaseXFD (1.3.6.1.2.1.26.4.22)
        dot3MauType1000BaseLXHD(1.3.6.1.2.1.26.4.23)
        dot3MauType1000BaseLXFD(1.3.6.1.2.1.26.4.24)
        dot3MauType1000BaseSXHD(1.3.6.1.2.1.26.4.25)
        dot3MauType1000BaseSXFD(1.3.6.1.2.1.26.4.26)
        dot3MauType1000BaseCXHD(1.3.6.1.2.1.26.4.27)
        dot3MauType1000BaseCXFD(1.3.6.1.2.1.26.4.28)
        dot3MauType1000BaseTHD (1.3.6.1.2.1.26.4.29)
        dot3MauType1000BaseTFD (1.3.6.1.2.1.26.4.30)
        dot3MauType10GigBaseX  (1.3.6.1.2.1.26.4.31)
        dot3MauType10GigBaseLX4(1.3.6.1.2.1.26.4.32)
        dot3MauType10GigBaseR  (1.3.6.1.2.1.26.4.33)
        dot3MauType10GigBaseER (1.3.6.1.2.1.26.4.34)
        dot3MauType10GigBaseLR (1.3.6.1.2.1.26.4.35)
        dot3MauType10GigBaseSR (1.3.6.1.2.1.26.4.36)
        dot3MauType10GigBaseW  (1.3.6.1.2.1.26.4.37)
        dot3MauType10GigBaseEW (1.3.6.1.2.1.26.4.38)
        dot3MauType10GigBaseLW (1.3.6.1.2.1.26.4.39)
        dot3MauType10GigBaseSW (1.3.6.1.2.1.26.4.40)"

    VARIATION       ifMauTypeListBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseTHD(10), -- 10BASE-T half duplex
                        b10baseTFD(11), -- 10BASE-T full duplex
                        b100baseTXHD(15), -- 100BASE-TX half duplex
                        b100baseTXFD(16), -- 100BASE-TX full duplex
                        b100baseFXHD(17), -- 100BASE-FX half duplex
                        b100baseFXFD(18), -- 100BASE-FX full duplex
                        b1000baseXHD(21), -- 1000BASE-X half duplex
                        b1000baseXFD(22), -- 1000BASE-X full duplex
                        b1000baseLXHD(23), -- 1000BASE-LX half duplex
                        b1000baseLXFD(24), -- 1000BASE-LX full duplex
                        b1000baseSXHD(25), -- 1000BASE-SX half duplex
                        b1000baseSXFD(26), -- 1000BASE-SX full duplex
                        b1000baseCXHD(27), -- 1000BASE-CX half duplex
                        b1000baseCXFD(28), -- 1000BASE-CX full duplex
                        b1000baseTHD(29), -- 1000BASE-T half duplex
                        b1000baseTFD(30), -- 1000BASE-T full duplex
                        b10GbaseX(31), -- 10GBASE-X
                        b10GbaseLX4(32), -- 10GBASE-LX4
                        b10GbaseR(33), -- 10GBASE-R
                        b10GbaseER(34), -- 10GBASE-ER
                        b10GbaseLR(35), -- 10GBASE-LR
                        b10GbaseSR(36), -- 10GBASE-SR
                        b10GbaseW(37), -- 10GBASE-W
                        b10GbaseEW(38), -- 10GBASE-EW
                        b10GbaseLW(39), -- 10GBASE-LW
                        b10GbaseSW(40) -- 10GBASE-SW                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       ifMauAutoNegRemoteSignaling
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegConfig
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegCapabilityBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseT(1), -- 10BASE-T half duplex
                        baseTFD(2), -- 10BASE-T full duplex
                        b100baseTX(4), -- 100BASE-TX half duplex
                        b100baseTXFD(5), -- 100BASE-TX full duplex
                        bFdxPause(8), -- PAUSE for full-duplex
                                       -- links
                        bfdxAPause(9), -- Asymmetric PAUSE for full-duplex
                                       -- links
                        bfdxSPause(10), -- Symmetric PAUSE for full-duplex
                                        -- links
                        bfdxBPause(11), -- Asymmetric and Symmetric PAUSE
                                        -- for full-duplex links
                        b1000baseX(12), -- 1000BASE-X, -LX, -SX,
                                        -- -CX half duplex
                        b1000baseXFD(13), -- 1000BASE-X, -LX, -SX,
                                          -- -CX full duplex
                        b1000baseT(14), -- 1000BASE-T half duplex
                        b1000baseTFD(15) -- 1000BASE-T full duplex                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values are
        supported."

    VARIATION       ifMauAutoNegCapAdvertisedBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseT(1), -- 10BASE-T half duplex
                        baseTFD(2), -- 10BASE-T full duplex
                        b100baseTX(4), -- 100BASE-TX half duplex
                        b100baseTXFD(5), -- 100BASE-TX full duplex
                        bFdxPause(8), -- PAUSE for full-duplex
                                       -- links
                        bfdxAPause(9), -- Asymmetric PAUSE for full-duplex
                                       -- links
                        bfdxSPause(10), -- Symmetric PAUSE for full-duplex
                                        -- links
                        bfdxBPause(11), -- Asymmetric and Symmetric PAUSE
                                        -- for full-duplex links
                        b1000baseX(12), -- 1000BASE-X, -LX, -SX,
                                        -- -CX half duplex
                        b1000baseXFD(13), -- 1000BASE-X, -LX, -SX,
                                          -- -CX full duplex
                        b1000baseT(14), -- 1000BASE-T half duplex
                        b1000baseTFD(15) -- 1000BASE-T full duplex                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values are
        supported.  When ifMauAutoNegCapabilityBits has the
        value '6C F3', the write access is supported and the
        supported write access values are: 0x6C 0xF0 and 0x6C 0xF3.
        6C F3(0110 1100 1111 0011) - speed auto
        6C F0(0110 1100 1111 0000) - speed auto 10 100"

    VARIATION       ifMauAutoNegCapReceivedBits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegRestart
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    ::= { ciscoMauCapability 2 }

ciscoMauCapV12R0233SXIPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXI on Catalyst 6000/6500
                     series devices."
    STATUS          current
    DESCRIPTION
        "MAU-MIB capabilities."

    SUPPORTS        MAU-MIB
    INCLUDES        {
                        mauIfGrpBasic,
                        mauIfGrpHighCapacity,
                        mauIfGrpAutoNeg2,
                        mauIfGrpJack
                    }
    VARIATION       ifMauStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauMediaAvailable
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauMediaAvailableStateExits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauJabberState
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauJabberingStateEnters
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauFalseCarriers
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauType
    DESCRIPTION
        "Only limited set of object identifiers are
        supported.
        unknownMauType         (0.0)
        dot3MauType10BaseTHD   (1.3.6.1.2.1.26.4.10)
        dot3MauType10BaseTFD   (1.3.6.1.2.1.26.4.11)
        dot3MauType100BaseTXHD (1.3.6.1.2.1.26.4.15)
        dot3MauType100BaseTXFD (1.3.6.1.2.1.26.4.16)
        dot3MauType100BaseFXHD (1.3.6.1.2.1.26.4.17)
        dot3MauType100BaseFXFD (1.3.6.1.2.1.26.4.18)
        dot3MauType1000BaseXHD (1.3.6.1.2.1.26.4.21)
        dot3MauType1000BaseXFD (1.3.6.1.2.1.26.4.22)
        dot3MauType1000BaseLXHD(1.3.6.1.2.1.26.4.23)
        dot3MauType1000BaseLXFD(1.3.6.1.2.1.26.4.24)
        dot3MauType1000BaseSXHD(1.3.6.1.2.1.26.4.25)
        dot3MauType1000BaseSXFD(1.3.6.1.2.1.26.4.26)
        dot3MauType1000BaseCXHD(1.3.6.1.2.1.26.4.27)
        dot3MauType1000BaseCXFD(1.3.6.1.2.1.26.4.28)
        dot3MauType1000BaseTHD (1.3.6.1.2.1.26.4.29)
        dot3MauType1000BaseTFD (1.3.6.1.2.1.26.4.30)
        dot3MauType10GigBaseX  (1.3.6.1.2.1.26.4.31)
        dot3MauType10GigBaseLX4(1.3.6.1.2.1.26.4.32)
        dot3MauType10GigBaseR  (1.3.6.1.2.1.26.4.33)
        dot3MauType10GigBaseER (1.3.6.1.2.1.26.4.34)
        dot3MauType10GigBaseLR (1.3.6.1.2.1.26.4.35)
        dot3MauType10GigBaseSR (1.3.6.1.2.1.26.4.36)
        dot3MauType10GigBaseW  (1.3.6.1.2.1.26.4.37)
        dot3MauType10GigBaseEW (1.3.6.1.2.1.26.4.38)
        dot3MauType10GigBaseLW (1.3.6.1.2.1.26.4.39)
        dot3MauType10GigBaseSW (1.3.6.1.2.1.26.4.40)"

    VARIATION       ifMauDefaultType
    DESCRIPTION
        "Only limited set of object identifiers are
        supported.
        unknownMauType         (0.0)
        dot3MauType10BaseTHD   (1.3.6.1.2.1.26.4.10)
        dot3MauType10BaseTFD   (1.3.6.1.2.1.26.4.11)
        dot3MauType100BaseTXHD (1.3.6.1.2.1.26.4.15)
        dot3MauType100BaseTXFD (1.3.6.1.2.1.26.4.16)
        dot3MauType100BaseFXHD (1.3.6.1.2.1.26.4.17)
        dot3MauType100BaseFXFD (1.3.6.1.2.1.26.4.18)
        dot3MauType1000BaseXHD (1.3.6.1.2.1.26.4.21)
        dot3MauType1000BaseXFD (1.3.6.1.2.1.26.4.22)
        dot3MauType1000BaseLXHD(1.3.6.1.2.1.26.4.23)
        dot3MauType1000BaseLXFD(1.3.6.1.2.1.26.4.24)
        dot3MauType1000BaseSXHD(1.3.6.1.2.1.26.4.25)
        dot3MauType1000BaseSXFD(1.3.6.1.2.1.26.4.26)
        dot3MauType1000BaseCXHD(1.3.6.1.2.1.26.4.27)
        dot3MauType1000BaseCXFD(1.3.6.1.2.1.26.4.28)
        dot3MauType1000BaseTHD (1.3.6.1.2.1.26.4.29)
        dot3MauType1000BaseTFD (1.3.6.1.2.1.26.4.30)
        dot3MauType10GigBaseX  (1.3.6.1.2.1.26.4.31)
        dot3MauType10GigBaseLX4(1.3.6.1.2.1.26.4.32)
        dot3MauType10GigBaseR  (1.3.6.1.2.1.26.4.33)
        dot3MauType10GigBaseER (1.3.6.1.2.1.26.4.34)
        dot3MauType10GigBaseLR (1.3.6.1.2.1.26.4.35)
        dot3MauType10GigBaseSR (1.3.6.1.2.1.26.4.36)
        dot3MauType10GigBaseW  (1.3.6.1.2.1.26.4.37)
        dot3MauType10GigBaseEW (1.3.6.1.2.1.26.4.38)
        dot3MauType10GigBaseLW (1.3.6.1.2.1.26.4.39)
        dot3MauType10GigBaseSW (1.3.6.1.2.1.26.4.40)"

    VARIATION       ifMauTypeListBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseTHD(10), -- 10BASE-T half duplex
                        b10baseTFD(11), -- 10BASE-T full duplex
                        b100baseTXHD(15), -- 100BASE-TX half duplex
                        b100baseTXFD(16), -- 100BASE-TX full duplex
                        b100baseFXHD(17), -- 100BASE-FX half duplex
                        b100baseFXFD(18), -- 100BASE-FX full duplex
                        b1000baseXHD(21), -- 1000BASE-X half duplex
                        b1000baseXFD(22), -- 1000BASE-X full duplex
                        b1000baseLXHD(23), -- 1000BASE-LX half duplex
                        b1000baseLXFD(24), -- 1000BASE-LX full duplex
                        b1000baseSXHD(25), -- 1000BASE-SX half duplex
                        b1000baseSXFD(26), -- 1000BASE-SX full duplex
                        b1000baseCXHD(27), -- 1000BASE-CX half duplex
                        b1000baseCXFD(28), -- 1000BASE-CX full duplex
                        b1000baseTHD(29), -- 1000BASE-T half duplex
                        b1000baseTFD(30), -- 1000BASE-T full duplex
                        b10GbaseX(31), -- 10GBASE-X
                        b10GbaseLX4(32), -- 10GBASE-LX4
                        b10GbaseR(33), -- 10GBASE-R
                        b10GbaseER(34), -- 10GBASE-ER
                        b10GbaseLR(35), -- 10GBASE-LR
                        b10GbaseSR(36), -- 10GBASE-SR
                        b10GbaseW(37), -- 10GBASE-W
                        b10GbaseEW(38), -- 10GBASE-EW
                        b10GbaseLW(39), -- 10GBASE-LW
                        b10GbaseSW(40) -- 10GBASE-SW                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       ifMauAutoNegRemoteSignaling
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegConfig
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegCapabilityBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseT(1), -- 10BASE-T half duplex
                        baseTFD(2), -- 10BASE-T full duplex
                        b100baseTX(4), -- 100BASE-TX half duplex
                        b100baseTXFD(5), -- 100BASE-TX full duplex
                        bFdxPause(8), -- PAUSE for full-duplex
                                       -- links
                        bfdxAPause(9), -- Asymmetric PAUSE for
                                       -- full-duplex links
                        bfdxSPause(10), -- Symmetric PAUSE for
                                        -- full-duplex links
                        bfdxBPause(11), -- Asymmetric and Symmetric
                                        -- PAUSE for full-duplex links
                        b1000baseX(12), -- 1000BASE-X, -LX, -SX,
                                        -- -CX half duplex
                        b1000baseXFD(13), -- 1000BASE-X, -LX, -SX,
                                          -- -CX full duplex
                        b1000baseT(14), -- 1000BASE-T half duplex
                        b1000baseTFD(15) -- 1000BASE-T full duplex                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values are
        supported."

    VARIATION       ifMauAutoNegCapAdvertisedBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseT(1), -- 10BASE-T half duplex
                        baseTFD(2), -- 10BASE-T full duplex
                        b100baseTX(4), -- 100BASE-TX half duplex
                        b100baseTXFD(5), -- 100BASE-TX full duplex
                        bFdxPause(8), -- PAUSE for full-duplex
                                       -- links
                        bfdxAPause(9), -- Asymmetric PAUSE for
                                       -- full-duplex links
                        bfdxSPause(10), -- Symmetric PAUSE for
                                        -- full-duplex links
                        bfdxBPause(11), -- Asymmetric and Symmetric
                                        -- PAUSE for full-duplex links
                        b1000baseX(12), -- 1000BASE-X, -LX, -SX, -CX
                                        -- half duplex
                        b1000baseXFD(13), -- 1000BASE-X, -LX, -SX, -CX
                                          -- full duplex
                        b1000baseT(14), -- 1000BASE-T half duplex
                        b1000baseTFD(15) -- 1000BASE-T full duplex                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values are
        supported.  When ifMauAutoNegCapabilityBits has the
        value '6C F3', the write access is supported and the
        supported write access values are: 0x6C 0xF0 and 0x6C 0xF3.
        6C F3(0110 1100 1111 0011) - speed auto
        6C F0(0110 1100 1111 0000) - speed auto 10 100"

    VARIATION       ifMauAutoNegCapReceivedBits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegRestart
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifJackType
    SYNTAX          INTEGER  {
                        other(1),
                        rj45S(3),
                        fiberSC(8),
                        fiberMIC(9),
                        fiberST(10),
                        telco(11),
                        mtrj(12),
                        fiberLC(14)
                    }
    DESCRIPTION
        "Only limited set of enumerated values is supported."

    ::= { ciscoMauCapability 3 }

ciscoMauCapV12R0233SXJPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXJ on Catalyst 6000/6500
                     series devices."
    STATUS          current
    DESCRIPTION
        "MAU-MIB capabilities."

    SUPPORTS        MAU-MIB
    INCLUDES        {
                        mauIfGrpBasic,
                        mauIfGrpHighCapacity,
                        mauIfGrpAutoNeg2,
                        mauIfGrpJack
                    }
    VARIATION       ifMauStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauMediaAvailable
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauMediaAvailableStateExits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauJabberState
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauJabberingStateEnters
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauFalseCarriers
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauType
    DESCRIPTION
        "Only limited set of object identifiers are
        supported.
        unknownMauType         (0.0)
        dot3MauType10BaseTHD   (1.3.6.1.2.1.26.4.10)
        dot3MauType10BaseTFD   (1.3.6.1.2.1.26.4.11)
        dot3MauType100BaseTXHD (1.3.6.1.2.1.26.4.15)
        dot3MauType100BaseTXFD (1.3.6.1.2.1.26.4.16)
        dot3MauType100BaseFXHD (1.3.6.1.2.1.26.4.17)
        dot3MauType100BaseFXFD (1.3.6.1.2.1.26.4.18)
        dot3MauType1000BaseXHD (1.3.6.1.2.1.26.4.21)
        dot3MauType1000BaseXFD (1.3.6.1.2.1.26.4.22)
        dot3MauType1000BaseLXHD(1.3.6.1.2.1.26.4.23)
        dot3MauType1000BaseLXFD(1.3.6.1.2.1.26.4.24)
        dot3MauType1000BaseSXHD(1.3.6.1.2.1.26.4.25)
        dot3MauType1000BaseSXFD(1.3.6.1.2.1.26.4.26)
        dot3MauType1000BaseCXHD(1.3.6.1.2.1.26.4.27)
        dot3MauType1000BaseCXFD(1.3.6.1.2.1.26.4.28)
        dot3MauType1000BaseTHD (1.3.6.1.2.1.26.4.29)
        dot3MauType1000BaseTFD (1.3.6.1.2.1.26.4.30)
        dot3MauType10GigBaseX  (1.3.6.1.2.1.26.4.31)
        dot3MauType10GigBaseLX4(1.3.6.1.2.1.26.4.32)
        dot3MauType10GigBaseR  (1.3.6.1.2.1.26.4.33)
        dot3MauType10GigBaseER (1.3.6.1.2.1.26.4.34)
        dot3MauType10GigBaseLR (1.3.6.1.2.1.26.4.35)
        dot3MauType10GigBaseSR (1.3.6.1.2.1.26.4.36)
        dot3MauType10GigBaseW  (1.3.6.1.2.1.26.4.37)
        dot3MauType10GigBaseEW (1.3.6.1.2.1.26.4.38)
        dot3MauType10GigBaseLW (1.3.6.1.2.1.26.4.39)
        dot3MauType10GigBaseSW (1.3.6.1.2.1.26.4.40)
        -- new since RFC 3636:
        dot3MauType10GigBaseCX4(1.3.6.1.2.1.26.4.41)
        dot3MauType100BaseBX10D(1.3.6.1.2.1.26.4.44)
        dot3MauType100BaseBX10U(1.3.6.1.2.1.26.4.45)
        dot3MauType1000BaseBX10D(1.3.6.1.2.1.26.4.47)
        dot3MauType1000BaseBX10U(1.3.6.1.2.1.26.4.48)
        dot3MauType10GbaseT    (1.3.6.1.2.1.26.4.54)
        dot3MauType10GbaseLRM  (1.3.6.1.2.1.26.4.55)"

    VARIATION       ifMauDefaultType
    DESCRIPTION
        "Only limited set of object identifiers are
        supported.
        unknownMauType         (0.0)
        dot3MauType10BaseTHD   (1.3.6.1.2.1.26.4.10)
        dot3MauType10BaseTFD   (1.3.6.1.2.1.26.4.11)
        dot3MauType100BaseTXHD (1.3.6.1.2.1.26.4.15)
        dot3MauType100BaseTXFD (1.3.6.1.2.1.26.4.16)
        dot3MauType100BaseFXHD (1.3.6.1.2.1.26.4.17)
        dot3MauType100BaseFXFD (1.3.6.1.2.1.26.4.18)
        dot3MauType1000BaseXHD (1.3.6.1.2.1.26.4.21)
        dot3MauType1000BaseXFD (1.3.6.1.2.1.26.4.22)
        dot3MauType1000BaseLXHD(1.3.6.1.2.1.26.4.23)
        dot3MauType1000BaseLXFD(1.3.6.1.2.1.26.4.24)
        dot3MauType1000BaseSXHD(1.3.6.1.2.1.26.4.25)
        dot3MauType1000BaseSXFD(1.3.6.1.2.1.26.4.26)
        dot3MauType1000BaseCXHD(1.3.6.1.2.1.26.4.27)
        dot3MauType1000BaseCXFD(1.3.6.1.2.1.26.4.28)
        dot3MauType1000BaseTHD (1.3.6.1.2.1.26.4.29)
        dot3MauType1000BaseTFD (1.3.6.1.2.1.26.4.30)
        dot3MauType10GigBaseX  (1.3.6.1.2.1.26.4.31)
        dot3MauType10GigBaseLX4(1.3.6.1.2.1.26.4.32)
        dot3MauType10GigBaseR  (1.3.6.1.2.1.26.4.33)
        dot3MauType10GigBaseER (1.3.6.1.2.1.26.4.34)
        dot3MauType10GigBaseLR (1.3.6.1.2.1.26.4.35)
        dot3MauType10GigBaseSR (1.3.6.1.2.1.26.4.36)
        dot3MauType10GigBaseW  (1.3.6.1.2.1.26.4.37)
        dot3MauType10GigBaseEW (1.3.6.1.2.1.26.4.38)
        dot3MauType10GigBaseLW (1.3.6.1.2.1.26.4.39)
        dot3MauType10GigBaseSW (1.3.6.1.2.1.26.4.40)
        -- new since RFC 3636:
        dot3MauType10GigBaseCX4(1.3.6.1.2.1.26.4.41)
        dot3MauType100BaseBX10D(1.3.6.1.2.1.26.4.44)
        dot3MauType100BaseBX10U(1.3.6.1.2.1.26.4.45)
        dot3MauType1000BaseBX10D(1.3.6.1.2.1.26.4.47)
        dot3MauType1000BaseBX10U(1.3.6.1.2.1.26.4.48)
        dot3MauType10GbaseT    (1.3.6.1.2.1.26.4.54)
        dot3MauType10GbaseLRM  (1.3.6.1.2.1.26.4.55)"

    VARIATION       ifMauTypeListBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseTHD(10), -- 10BASE-T half duplex
                        b10baseTFD(11), -- 10BASE-T full duplex
                        b100baseTXHD(15), -- 100BASE-TX half duplex
                        b100baseTXFD(16), -- 100BASE-TX full duplex
                        b100baseFXHD(17), -- 100BASE-FX half duplex
                        b100baseFXFD(18), -- 100BASE-FX full duplex
                        b1000baseXHD(21), -- 1000BASE-X half duplex
                        b1000baseXFD(22), -- 1000BASE-X full duplex
                        b1000baseLXHD(23), -- 1000BASE-LX half duplex
                        b1000baseLXFD(24), -- 1000BASE-LX full duplex
                        b1000baseSXHD(25), -- 1000BASE-SX half duplex
                        b1000baseSXFD(26), -- 1000BASE-SX full duplex
                        b1000baseCXHD(27), -- 1000BASE-CX half duplex
                        b1000baseCXFD(28), -- 1000BASE-CX full duplex
                        b1000baseTHD(29), -- 1000BASE-T half duplex
                        b1000baseTFD(30), -- 1000BASE-T full duplex
                        b10GbaseX(31), -- 10GBASE-X
                        b10GbaseLX4(32), -- 10GBASE-LX4
                        b10GbaseR(33), -- 10GBASE-R
                        b10GbaseER(34), -- 10GBASE-ER
                        b10GbaseLR(35), -- 10GBASE-LR
                        b10GbaseSR(36), -- 10GBASE-SR
                        b10GbaseW(37), -- 10GBASE-W
                        b10GbaseEW(38), -- 10GBASE-EW
                        b10GbaseLW(39), -- 10GBASE-LW
                        b10GbaseSW(40), -- 10GBASE-SW
                                         -- new since RFC 3636
                        b10GbaseCX4(41), -- 10GBASE-CX4
                        b100BaseBX10D(44), -- 100BASE-BX10D
                        b100BaseBX10U(45), -- 100BASE-BX10U
                        b1000BaseBX10D(47), -- 1000BASE-BX10D
                        b1000BaseBX10U(48), -- 1000BASE-BX10U
                        b10GbaseT(54), -- 10GBASE-T
                        b10GbaseLRM(55) -- 10GBASE-LRM                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       ifMauAutoNegRemoteSignaling
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegConfig
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegCapabilityBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseT(1), -- 10BASE-T half duplex
                        baseTFD(2), -- 10BASE-T full duplex
                        b100baseTX(4), -- 100BASE-TX half duplex
                        b100baseTXFD(5), -- 100BASE-TX full duplex
                        bFdxPause(8), -- PAUSE for full-duplex
                                       -- links
                        bfdxAPause(9), -- Asymmetric PAUSE for
                                       -- full-duplex links
                        bfdxSPause(10), -- Symmetric PAUSE for
                                        -- full-duplex links
                        bfdxBPause(11), -- Asymmetric and Symmetric
                                        -- PAUSE for full-duplex links
                        b1000baseX(12), -- 1000BASE-X, -LX, -SX,
                                        -- -CX half duplex
                        b1000baseXFD(13), -- 1000BASE-X, -LX, -SX,
                                          -- -CX full duplex
                        b1000baseT(14), -- 1000BASE-T half duplex
                        b1000baseTFD(15), -- 1000BASE-T full duplex
                                          -- new since RFC 3636
                        b10GbaseT(16) -- 10GBASE-T                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values are
        supported."

    VARIATION       ifMauAutoNegCapAdvertisedBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseT(1), -- 10BASE-T half duplex
                        baseTFD(2), -- 10BASE-T full duplex
                        b100baseTX(4), -- 100BASE-TX half duplex
                        b100baseTXFD(5), -- 100BASE-TX full duplex
                        bFdxPause(8), -- PAUSE for full-duplex
                                       -- links
                        bfdxAPause(9), -- Asymmetric PAUSE for
                                       -- full-duplex links
                        bfdxSPause(10), -- Symmetric PAUSE for
                                        -- full-duplex links
                        bfdxBPause(11), -- Asymmetric and Symmetric
                                        -- PAUSE for full-duplex links
                        b1000baseX(12), -- 1000BASE-X, -LX, -SX, -CX
                                        -- half duplex
                        b1000baseXFD(13), -- 1000BASE-X, -LX, -SX, -CX
                                          -- full duplex
                        b1000baseT(14), -- 1000BASE-T half duplex
                        b1000baseTFD(15), -- 1000BASE-T full duplex
                                          -- new since RFC 3636
                        b10GbaseT(16) -- 10GBASE-T                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values are
        supported.  When ifMauAutoNegCapabilityBits has the
        value '6C F3', the write access is supported and the
        supported write access values are: 0x6C 0xF0 and 0x6C 0xF3.
        6C F3(0110 1100 1111 0011) - speed auto
        6C F0(0110 1100 1111 0000) - speed auto 10 100"

    VARIATION       ifMauAutoNegCapReceivedBits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegRestart
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifJackType
    SYNTAX          INTEGER  {
                        other(1), -- undefined or unknown
                        rj45S(3), -- RJ45 shielded
                        fiberSC(8), -- SC fiber
                        fiberMIC(9), -- MIC fiber
                        fiberST(10), -- ST fiber
                        telco(11), -- Telco
                        mtrj(12), -- MT-RJ fiber
                        fiberLC(14), -- LC fiber
                                      -- new since RFC 3636
                        cx4(15) -- IB4X for 10GBASE-CX4                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values is supported."

    ::= { ciscoMauCapability 4 }

ciscoMauCapV15R0001SYPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 15.0(1)SY on Catalyst 6000/6500
                     series devices."
    STATUS          current
    DESCRIPTION
        "MAU-MIB capabilities."

    SUPPORTS        MAU-MIB
    INCLUDES        {
                        mauIfGrpBasic,
                        mauIfGrpHighCapacity,
                        mauIfGrpAutoNeg2,
                        mauIfGrpJack
                    }
    VARIATION       ifMauStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauMediaAvailable
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauMediaAvailableStateExits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauJabberState
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauJabberingStateEnters
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauFalseCarriers
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauType
    DESCRIPTION
        "Only limited set of object identifiers are
        supported.
        unknownMauType         (0.0)
        dot3MauType10BaseTHD   (1.3.6.1.2.1.26.4.10)
        dot3MauType10BaseTFD   (1.3.6.1.2.1.26.4.11)
        dot3MauType100BaseTXHD (1.3.6.1.2.1.26.4.15)
        dot3MauType100BaseTXFD (1.3.6.1.2.1.26.4.16)
        dot3MauType100BaseFXHD (1.3.6.1.2.1.26.4.17)
        dot3MauType100BaseFXFD (1.3.6.1.2.1.26.4.18)
        dot3MauType1000BaseXHD (1.3.6.1.2.1.26.4.21)
        dot3MauType1000BaseXFD (1.3.6.1.2.1.26.4.22)
        dot3MauType1000BaseLXHD(1.3.6.1.2.1.26.4.23)
        dot3MauType1000BaseLXFD(1.3.6.1.2.1.26.4.24)
        dot3MauType1000BaseSXHD(1.3.6.1.2.1.26.4.25)
        dot3MauType1000BaseSXFD(1.3.6.1.2.1.26.4.26)
        dot3MauType1000BaseCXHD(1.3.6.1.2.1.26.4.27)
        dot3MauType1000BaseCXFD(1.3.6.1.2.1.26.4.28)
        dot3MauType1000BaseTHD (1.3.6.1.2.1.26.4.29)
        dot3MauType1000BaseTFD (1.3.6.1.2.1.26.4.30)
        dot3MauType10GigBaseX  (1.3.6.1.2.1.26.4.31)
        dot3MauType10GigBaseLX4(1.3.6.1.2.1.26.4.32)
        dot3MauType10GigBaseR  (1.3.6.1.2.1.26.4.33)
        dot3MauType10GigBaseER (1.3.6.1.2.1.26.4.34)
        dot3MauType10GigBaseLR (1.3.6.1.2.1.26.4.35)
        dot3MauType10GigBaseSR (1.3.6.1.2.1.26.4.36)
        dot3MauType10GigBaseW  (1.3.6.1.2.1.26.4.37)
        dot3MauType10GigBaseEW (1.3.6.1.2.1.26.4.38)
        dot3MauType10GigBaseLW (1.3.6.1.2.1.26.4.39)
        dot3MauType10GigBaseSW (1.3.6.1.2.1.26.4.40)
        -- new since RFC 3636:
        dot3MauType10GigBaseCX4(1.3.6.1.2.1.26.4.41)
        dot3MauType100BaseBX10D(1.3.6.1.2.1.26.4.44)
        dot3MauType100BaseBX10U(1.3.6.1.2.1.26.4.45)
        dot3MauType1000BaseBX10D(1.3.6.1.2.1.26.4.47)
        dot3MauType1000BaseBX10U(1.3.6.1.2.1.26.4.48)
        dot3MauType10GbaseT    (1.3.6.1.2.1.26.4.54)
        dot3MauType10GbaseLRM  (1.3.6.1.2.1.26.4.55)"

    VARIATION       ifMauDefaultType
    DESCRIPTION
        "Only limited set of object identifiers are
        supported.
        unknownMauType         (0.0)
        dot3MauType10BaseTHD   (1.3.6.1.2.1.26.4.10)
        dot3MauType10BaseTFD   (1.3.6.1.2.1.26.4.11)
        dot3MauType100BaseTXHD (1.3.6.1.2.1.26.4.15)
        dot3MauType100BaseTXFD (1.3.6.1.2.1.26.4.16)
        dot3MauType100BaseFXHD (1.3.6.1.2.1.26.4.17)
        dot3MauType100BaseFXFD (1.3.6.1.2.1.26.4.18)
        dot3MauType1000BaseXHD (1.3.6.1.2.1.26.4.21)
        dot3MauType1000BaseXFD (1.3.6.1.2.1.26.4.22)
        dot3MauType1000BaseLXHD(1.3.6.1.2.1.26.4.23)
        dot3MauType1000BaseLXFD(1.3.6.1.2.1.26.4.24)
        dot3MauType1000BaseSXHD(1.3.6.1.2.1.26.4.25)
        dot3MauType1000BaseSXFD(1.3.6.1.2.1.26.4.26)
        dot3MauType1000BaseCXHD(1.3.6.1.2.1.26.4.27)
        dot3MauType1000BaseCXFD(1.3.6.1.2.1.26.4.28)
        dot3MauType1000BaseTHD (1.3.6.1.2.1.26.4.29)
        dot3MauType1000BaseTFD (1.3.6.1.2.1.26.4.30)
        dot3MauType10GigBaseX  (1.3.6.1.2.1.26.4.31)
        dot3MauType10GigBaseLX4(1.3.6.1.2.1.26.4.32)
        dot3MauType10GigBaseR  (1.3.6.1.2.1.26.4.33)
        dot3MauType10GigBaseER (1.3.6.1.2.1.26.4.34)
        dot3MauType10GigBaseLR (1.3.6.1.2.1.26.4.35)
        dot3MauType10GigBaseSR (1.3.6.1.2.1.26.4.36)
        dot3MauType10GigBaseW  (1.3.6.1.2.1.26.4.37)
        dot3MauType10GigBaseEW (1.3.6.1.2.1.26.4.38)
        dot3MauType10GigBaseLW (1.3.6.1.2.1.26.4.39)
        dot3MauType10GigBaseSW (1.3.6.1.2.1.26.4.40)
        -- new since RFC 3636:
        dot3MauType10GigBaseCX4(1.3.6.1.2.1.26.4.41)
        dot3MauType100BaseBX10D(1.3.6.1.2.1.26.4.44)
        dot3MauType100BaseBX10U(1.3.6.1.2.1.26.4.45)
        dot3MauType1000BaseBX10D(1.3.6.1.2.1.26.4.47)
        dot3MauType1000BaseBX10U(1.3.6.1.2.1.26.4.48)
        dot3MauType10GbaseT    (1.3.6.1.2.1.26.4.54)
        dot3MauType10GbaseLRM  (1.3.6.1.2.1.26.4.55)"

    VARIATION       ifMauTypeListBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseTHD(10), -- 10BASE-T half duplex
                        b10baseTFD(11), -- 10BASE-T full duplex
                        b100baseTXHD(15), -- 100BASE-TX half duplex
                        b100baseTXFD(16), -- 100BASE-TX full duplex
                        b100baseFXHD(17), -- 100BASE-FX half duplex
                        b100baseFXFD(18), -- 100BASE-FX full duplex
                        b1000baseXHD(21), -- 1000BASE-X half duplex
                        b1000baseXFD(22), -- 1000BASE-X full duplex
                        b1000baseLXHD(23), -- 1000BASE-LX half duplex
                        b1000baseLXFD(24), -- 1000BASE-LX full duplex
                        b1000baseSXHD(25), -- 1000BASE-SX half duplex
                        b1000baseSXFD(26), -- 1000BASE-SX full duplex
                        b1000baseCXHD(27), -- 1000BASE-CX half duplex
                        b1000baseCXFD(28), -- 1000BASE-CX full duplex
                        b1000baseTHD(29), -- 1000BASE-T half duplex
                        b1000baseTFD(30), -- 1000BASE-T full duplex
                        b10GbaseX(31), -- 10GBASE-X
                        b10GbaseLX4(32), -- 10GBASE-LX4
                        b10GbaseR(33), -- 10GBASE-R
                        b10GbaseER(34), -- 10GBASE-ER
                        b10GbaseLR(35), -- 10GBASE-LR
                        b10GbaseSR(36), -- 10GBASE-SR
                        b10GbaseW(37), -- 10GBASE-W
                        b10GbaseEW(38), -- 10GBASE-EW
                        b10GbaseLW(39), -- 10GBASE-LW
                        b10GbaseSW(40), -- 10GBASE-SW
                                         -- new since RFC 3636
                        b10GbaseCX4(41), -- 10GBASE-CX4
                        b100BaseBX10D(44), -- 100BASE-BX10D
                        b100BaseBX10U(45), -- 100BASE-BX10U
                        b1000BaseBX10D(47), -- 1000BASE-BX10D
                        b1000BaseBX10U(48), -- 1000BASE-BX10U
                        b10GbaseT(54), -- 10GBASE-T
                        b10GbaseLRM(55) -- 10GBASE-LRM                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values
        is supported."

    VARIATION       ifMauAutoNegRemoteSignaling
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegConfig
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegCapabilityBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseT(1), -- 10BASE-T half duplex
                        baseTFD(2), -- 10BASE-T full duplex
                        b100baseTX(4), -- 100BASE-TX half duplex
                        b100baseTXFD(5), -- 100BASE-TX full duplex
                        bFdxPause(8), -- PAUSE for full-duplex
                                       -- links
                        bfdxAPause(9), -- Asymmetric PAUSE for
                                       -- full-duplex links
                        bfdxSPause(10), -- Symmetric PAUSE for
                                        -- full-duplex links
                        bfdxBPause(11), -- Asymmetric and Symmetric
                                        -- PAUSE for full-duplex links
                        b1000baseX(12), -- 1000BASE-X, -LX, -SX,
                                        -- -CX half duplex
                        b1000baseXFD(13), -- 1000BASE-X, -LX, -SX,
                                          -- -CX full duplex
                        b1000baseT(14), -- 1000BASE-T half duplex
                        b1000baseTFD(15), -- 1000BASE-T full duplex
                                          -- new since RFC 3636
                        b10GbaseT(16) -- 10GBASE-T                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values are
        supported."

    VARIATION       ifMauAutoNegCapAdvertisedBits
    SYNTAX          BITS {
                        bOther(0), -- other or unknown
                        b10baseT(1), -- 10BASE-T half duplex
                        baseTFD(2), -- 10BASE-T full duplex
                        b100baseTX(4), -- 100BASE-TX half duplex
                        b100baseTXFD(5), -- 100BASE-TX full duplex
                        bFdxPause(8), -- PAUSE for full-duplex
                                       -- links
                        bfdxAPause(9), -- Asymmetric PAUSE for
                                       -- full-duplex links
                        bfdxSPause(10), -- Symmetric PAUSE for
                                        -- full-duplex links
                        bfdxBPause(11), -- Asymmetric and Symmetric
                                        -- PAUSE for full-duplex links
                        b1000baseX(12), -- 1000BASE-X, -LX, -SX, -CX
                                        -- half duplex
                        b1000baseXFD(13), -- 1000BASE-X, -LX, -SX, -CX
                                          -- full duplex
                        b1000baseT(14), -- 1000BASE-T half duplex
                        b1000baseTFD(15), -- 1000BASE-T full duplex
                                          -- new since RFC 3636
                        b10GbaseT(16) -- 10GBASE-T                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values are
        supported.  When ifMauAutoNegCapabilityBits has the
        value '6C F3', the write access is supported and the
        supported write access values are: 0x6C 0xF0 and 0x6C 0xF3.
        6C F3(0110 1100 1111 0011) - speed auto
        6C F0(0110 1100 1111 0000) - speed auto 10 100"

    VARIATION       ifMauAutoNegCapReceivedBits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegRestart
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifJackType
    SYNTAX          INTEGER  {
                        other(1), -- undefined or unknown
                        rj45S(3), -- RJ45 shielded
                        fiberSC(8), -- SC fiber
                        fiberMIC(9), -- MIC fiber
                        fiberST(10), -- ST fiber
                        telco(11), -- Telco
                        mtrj(12), -- MT-RJ fiber
                        fiberLC(14), -- LC fiber
                                      -- new since RFC 3636
                        cx4(15) -- IB4X for 10GBASE-CX4                        
                    }
    DESCRIPTION
        "Only limited set of enumerated values is supported."

    ::= { ciscoMauCapability 5 }

ciscoMauCapV05R0003U0401PN3K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco NX-OS 5.0(3)U4(1) on Nexus 3000 series
                     devices."
    STATUS          current
    DESCRIPTION
        "MAU-MIB capabilities."

    SUPPORTS        MAU-MIB
    INCLUDES        {
                        mauIfGrpBasic,
                        mauIfGrpHighCapacity,
                        mauIfGrpAutoNeg2
                    }
    VARIATION       ifMauStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauMediaAvailable
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauMediaAvailableStateExits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauJabberState
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauJabberingStateEnters
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauFalseCarriers
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauDefaultType
    DESCRIPTION
        "Only limited set of object identifiers are supported and are
        depended on the interface type or the transceiver being used.
        Unable to set if the object value of ifMauAutoNegAdminStatus
        is 'enabled'."

    VARIATION       ifMauAutoNegRemoteSignaling
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegConfig
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegCapAdvertisedBits
    DESCRIPTION
        "Only limited set of enumerated values are supported and
        are depended on the interface type or the transceiver being
        used."

    VARIATION       ifMauAutoNegCapReceivedBits
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    VARIATION       ifMauAutoNegRestart
    ACCESS          not-implemented
    DESCRIPTION
        "Information not available."

    ::= { ciscoMauCapability 6 }

END




