-- *****************************************************************
-- CISCO-FLASH-CAPABILITY.my: CISCO-FLASH-MIB AGENT-CAPABILITIES
--   
-- September 2001, A S Kiran Koushik
-- April 2004, Wen Xu
--   
-- Copyright (c) 2001, 2003, 2004, 2008 by Cisco Systems Inc.
-- All rights reserved.
--   
-- *****************************************************************

CISCO-FLASH-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    DisplayString
        FROM SNMPv2-TC
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoFlashCapability MODULE-IDENTITY
    LAST-UPDATED    "200801180000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-snmp@cisco.com"
    DESCRIPTION
        "Agent capabilities for CISCO-FLASH-MIB"
    REVISION        "200801180000Z"
    DESCRIPTION
        "Added ciscoFlashMibCapXRV03R06PCRS1
        agent capability statement."
    REVISION        "200404010000Z"
    DESCRIPTION
        "Added ciscoFlashMibCapCatOSV08R0301."
    REVISION        "200310210000Z"
    DESCRIPTION
        "Added ciscoFlashMibCapCatOSV7R0501Cat6k,
        and ciscoFlashMibCapV12R0113ECat6K."
    REVISION        "200109251234Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 222 }



ciscoFlashCapabilityV12R00S AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.0S"
    STATUS          current
    DESCRIPTION
        "CISCO-FLASH-MIB capabilities"

    SUPPORTS        CISCO-FLASH-MIB
    INCLUDES        { ciscoFlashDeviceInfoGroup }
    VARIATION       ciscoFlashDeviceChangeTrap
    DESCRIPTION
        "A ciscoFlashDeviceChangeTrap is sent whenever a
        removable Flash device is inserted or removed.
        If the value of ciscoFlashDeviceSize is 0, it means
        that the flash device was removed.
        If the value of ciscoFlashDeviceSize is greater than
        zero, it means that the flash device was inserted."

    ::= { ciscoFlashCapability 1 }

ciscoFlashCapabilityV12R01 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.1"
    STATUS          current
    DESCRIPTION
        "CISCO-FLASH-MIB capabilities"

    SUPPORTS        CISCO-FLASH-MIB
    INCLUDES        { ciscoFlashDeviceInfoGroup }
    VARIATION       ciscoFlashDeviceChangeTrap
    DESCRIPTION
        "A ciscoFlashDeviceChangeTrap is sent whenever a
        removable Flash device is inserted or removed.
        If the value of ciscoFlashDeviceSize is 0, it means
        that the flash device was removed.
        If the value of ciscoFlashDeviceSize is greater than
        zero, it means that the flash device was inserted."

    ::= { ciscoFlashCapability 2 }

ciscoFlashCapabilityV12R02 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2"
    STATUS          current
    DESCRIPTION
        "CISCO-FLASH-MIB capabilities"

    SUPPORTS        CISCO-FLASH-MIB
    INCLUDES        { ciscoFlashDeviceInfoGroup }
    VARIATION       ciscoFlashDeviceChangeTrap
    DESCRIPTION
        "A ciscoFlashDeviceChangeTrap is sent whenever a
        removable Flash device is inserted or removed.
        If the value of ciscoFlashDeviceSize is 0, it means
        that the flash device was removed.
        If the value of ciscoFlashDeviceSize is greater than
        zero, it means that the flash device was inserted."

    ::= { ciscoFlashCapability 3 }

ciscoFlashMibCapCatOSV7R0501Cat4k AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 7.5(1) on  Catalyst 4000."
    STATUS          current
    DESCRIPTION
        "CISCO-FLASH-MIB capabilities."

    SUPPORTS        CISCO-FLASH-MIB
    INCLUDES        {
                        ciscoFlashDeviceInfoGroup,
                        ciscoFlashPartitionInfoGroup,
                        ciscoFlashFileInfoGroupRev1,
                        ciscoFlashCopyOpGroup,
                        ciscoFlashMiscOpGroup,
                        ciscoFlashNotifGroup
                    }
    VARIATION       ciscoFlashCopyCommand
    SYNTAX          INTEGER  {
                        copyToFlashWithoutErase(2),
                        copyFromFlash(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values are supported."

    VARIATION       ciscoFlashCopyProtocol
    SYNTAX          INTEGER  {
                        tftp(1),
                        rcp(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values are supported."

    VARIATION       ciscoFlashCopySourceName
    SYNTAX          DisplayString (SIZE (1..63))
    DESCRIPTION
        "Only support up to 63 characters long."

    VARIATION       ciscoFlashCopyRemoteUserName
    SYNTAX          DisplayString (SIZE (1..40))
    DESCRIPTION
        "Only support up to 40 characters long."

    VARIATION       ciscoFlashMiscOpCommand
    SYNTAX          INTEGER  {
                        verify(2),
                        delete(3),
                        undelete(4),
                        squeeze(5),
                        format(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values are supported."

    VARIATION       ciscoFlashMiscOpDestinationName
    SYNTAX          DisplayString (SIZE (1..63))
    DESCRIPTION
        "Only support up to 63 characters long."

    VARIATION       ciscoFlashPartitioningCompletionTrap
    ACCESS          not-implemented
    DESCRIPTION
        "The current implentation does not support flash partitioning.
        Hense, this object is not supported."

    ::= { ciscoFlashCapability 4 }

ciscoFlashMibCapCatOSV7R0501Cat6k AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 7.5(1) on Catalyst 6000."
    STATUS          current
    DESCRIPTION
        "CISCO-FLASH-MIB capabilities."

    SUPPORTS        CISCO-FLASH-MIB
    INCLUDES        {
                        ciscoFlashDeviceInfoGroupRev1,
                        ciscoFlashPartitionInfoGroup,
                        ciscoFlashFileInfoGroupRev1,
                        ciscoFlashCopyOpGroup,
                        ciscoFlashMiscOpGroup,
                        ciscoFlashNotifGroupRev1
                    }
    VARIATION       ciscoFlashCopyCommand
    SYNTAX          INTEGER  {
                        copyToFlashWithoutErase(2),
                        copyFromFlash(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values are supported."

    VARIATION       ciscoFlashCopyProtocol
    SYNTAX          INTEGER  {
                        tftp(1),
                        rcp(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values are supported."

    VARIATION       ciscoFlashCopySourceName
    SYNTAX          DisplayString (SIZE (1..63))
    DESCRIPTION
        "Only support up to 63 characters long."

    VARIATION       ciscoFlashCopyRemoteUserName
    SYNTAX          DisplayString (SIZE (1..40))
    DESCRIPTION
        "Only support up to 40 characters long."

    VARIATION       ciscoFlashMiscOpCommand
    SYNTAX          INTEGER  {
                        verify(2),
                        delete(3),
                        undelete(4),
                        squeeze(5),
                        format(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values are supported."

    VARIATION       ciscoFlashMiscOpDestinationName
    SYNTAX          DisplayString (SIZE (1..63))
    DESCRIPTION
        "Only support up to 63 characters long."

    VARIATION       ciscoFlashPartitioningCompletionTrap
    ACCESS          not-implemented
    DESCRIPTION
        "The current implentation does not support flash partitioning.
        Hense, this object is not supported."

    ::= { ciscoFlashCapability 5 }

ciscoFlashMibCapV12R0113ECat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.1(13E) on Catalyst 6000/6500 and Cisco
                7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-FLASH-MIB capabilities."

    SUPPORTS        CISCO-FLASH-MIB
    INCLUDES        {
                        ciscoFlashDeviceInfoGroupRev1,
                        ciscoFlashPartitionInfoGroup,
                        ciscoFlashFileInfoGroupRev1,
                        ciscoFlashCopyOpGroup,
                        ciscoFlashMiscOpGroup,
                        ciscoFlashNotifGroupRev1
                    }
    VARIATION       ciscoFlashCopyProtocol
    SYNTAX          INTEGER  {
                        tftp(1),
                        rcp(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values are supported."

    VARIATION       ciscoFlashPartitioningCompletionTrap
    ACCESS          not-implemented
    DESCRIPTION
        "The current implentation does not support flash partitioning.
        Hense, this object is not supported."

    ::= { ciscoFlashCapability 6 }

ciscoFlashMibCapCatOSV08R0301 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.3(1)on Catalyst 6000/6500
                and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-FLASH-MIB capabilities."

    SUPPORTS        CISCO-FLASH-MIB
    INCLUDES        {
                        ciscoFlashDeviceInfoGroupRev1,
                        ciscoFlashPartitionInfoGroup,
                        ciscoFlashFileInfoGroupRev1,
                        ciscoFlashCopyOpGroupRev1,
                        ciscoFlashMiscOpGroup,
                        ciscoFlashNotifGroupRev1
                    }
    VARIATION       ciscoFlashCopyCommand
    SYNTAX          INTEGER  {
                        copyToFlashWithoutErase(2),
                        copyFromFlash(3)
                    }
    DESCRIPTION
        "Only limited set of enumerated values are supported."

    VARIATION       ciscoFlashCopyProtocol
    SYNTAX          INTEGER  {
                        tftp(1),
                        rcp(2)
                    }
    DESCRIPTION
        "Only limited set of enumerated values are supported."

    VARIATION       ciscoFlashCopySourceName
    SYNTAX          DisplayString (SIZE (1..63))
    DESCRIPTION
        "Only support up to 63 characters long."

    VARIATION       ciscoFlashCopyRemoteUserName
    SYNTAX          DisplayString (SIZE (1..40))
    DESCRIPTION
        "Only support up to 40 characters long."

    VARIATION       ciscoFlashMiscOpCommand
    SYNTAX          INTEGER  {
                        verify(2),
                        delete(3),
                        undelete(4),
                        squeeze(5),
                        format(6)
                    }
    DESCRIPTION
        "Only limited set of enumerated values are supported."

    VARIATION       ciscoFlashMiscOpDestinationName
    SYNTAX          DisplayString (SIZE (1..63))
    DESCRIPTION
        "Only support up to 63 characters long."

    VARIATION       ciscoFlashPartitioningCompletionTrap
    ACCESS          not-implemented
    DESCRIPTION
        "The current implentation does not support flash
        partitioning.  Hense, this object is not
        supported."

    ::= { ciscoFlashCapability 7 }

ciscoFlashMibCapXRV03R06PCRS1 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS XR 3.6 on CRS-1"
    STATUS          current
    DESCRIPTION
        "CISCO-FLASH-MIB capabilities."

    SUPPORTS        CISCO-FLASH-MIB
    INCLUDES        {
                        ciscoFlashDeviceInfoGroupRev1,
                        ciscoFlashPartitionInfoGroup,
                        ciscoFlashFileInfoGroupRev1,
                        ciscoFlashNotifGroupRev1,
                        ciscoFlashCopyOpGroup,
                        ciscoFlashMiscOpGroup
                    }
    VARIATION       ciscoFlashCfgDevInsNotifEnable
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       ciscoFlashCfgDevRemNotifEnable
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       ciscoFlashPartitioningCommand
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       ciscoFlashPartitioningDestinationName
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       ciscoFlashPartitioningPartitionCount
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       ciscoFlashPartitioningPartitionSizes
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       ciscoFlashPartitioningStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       ciscoFlashPartitioningNotifyOnCompletion
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported"

    VARIATION       ciscoFlashPartitioningTime
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       ciscoFlashPartitioningEntryStatus
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    VARIATION       ciscoFlashPartitioningCompletionTrap
    ACCESS          not-implemented
    DESCRIPTION
        "Not supported."

    ::= { ciscoFlashCapability 8 }

END




