DISMAN-TRACEROUTE-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32,
    Gauge32, Unsigned32, mib-2,
    NOTIFICATION-TYPE,
    OBJECT-IDENTITY
        FROM SNMPv2-SMI                  -- RFC2578
    RowStatus, StorageType,
    TruthValue, DateAndTime
        FROM SNMPv2-TC                   -- RFC2579
    MODULE-COMPLIANCE, OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF                 -- RFC2580
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB          -- RFC3411
    InterfaceIndexOrZero                 -- RFC2863
        FROM IF-MIB
    InetAddressType, InetAddress
        FROM INET-ADDRESS-MIB            -- RFC4001
    OperationResponseStatus
        FROM DISMAN-PING-MIB;            -- RFC4560

 traceRouteMIB MODULE-IDENTITY
    LAST-UPDATED "200606130000Z"         -- 13 June 2006
    ORGANIZATION "IETF Distributed Management Working Group"
    CONTACT-INFO
        "Juergen Quittek

        NEC Europe Ltd.
        Network Laboratories
        Kurfuersten-Anlage 36
        69115 Heidelberg
        Germany

        Phone: +49 6221 4342-115
        Email: quittek@netlab.nec.de"
    DESCRIPTION
        "The Traceroute MIB (DISMAN-TRACEROUTE-MIB) provides
        access to the traceroute capability at a remote host.

        Copyright (C) The Internet Society (2006). This version of
        this MIB module is part of RFC 4560; see the RFC itself for
        full legal notices."

     --  Revision history


     REVISION     "200606130000Z"         -- 13 June 2006
     DESCRIPTION
         "Updated version, published as RFC 4560.
             - Correctly considered IPv6 in DESCRIPTION clause of
               object traceRouteCtlDataSize
             - Replaced references to RFC 2575 by RFC 3415
             - Replaced references to RFC 2571 by RFC 3411
             - Replaced references to RFC 2851 by RFC 4001
             - Clarified DESCRIPTION clause of object
               traceRouteResultsLastGoodPath
             - Changed range of object traceRouteCtlInitialTtl
               from (0..255) to (1..255)
             - Extended DESCRIPTION clause of traceRouteResultsTable
               describing re-initialization of entries
             - Changed SYNTAX of traceRouteResultsTestAttempts and
               traceRouteResultsTestSuccesses from Unsigned32 to
               Gauge32
             - Changed status of traceRouteCompliance to deprecated
             - Added traceRouteFullCompliance and
               traceRouteMinimumCompliance
             - Changed status of traceRouteGroup and
               traceRouteTimeStampGroup to deprecated
             - Added traceRouteMinimumGroup,
               traceRouteCtlRowStatusGroup, and
               traceRouteHistoryGroup
             - Changed DEFVAL of object
               traceRouteCtlTargetAddressType from { ipv4 }
               to { unknown }
             - Changed DEFVAL of object traceRouteCtlDescr
               from { '00'H } to { ''H }
             - Added DEFVAL for object traceRouteCtlTrapGeneration
               of DEFVAL { { } }"
     REVISION     "200009210000Z"         -- 21 September 2000
     DESCRIPTION
         "Initial version, published as RFC 2925."

    ::= { mib-2 81 }

 -- Top level structure of the MIB

 traceRouteNotifications  OBJECT IDENTIFIER ::= { traceRouteMIB 0 }
 traceRouteObjects        OBJECT IDENTIFIER ::= { traceRouteMIB 1 }
 traceRouteConformance    OBJECT IDENTIFIER ::= { traceRouteMIB 2 }

 -- The registration node (point) for traceroute implementation types

 traceRouteImplementationTypeDomains OBJECT IDENTIFIER
 ::= { traceRouteMIB 3 }


 traceRouteUsingUdpProbes OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
        "Indicates that an implementation is using UDP probes to
        perform the traceroute operation."
    ::= { traceRouteImplementationTypeDomains 1 }


 -- Simple Object Definitions

 traceRouteMaxConcurrentRequests OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "requests"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
       "The maximum number of concurrent active traceroute requests
       that are allowed within an agent implementation.  A value
       of 0 for this object implies that there is no limit for
       the number of concurrent active requests in effect.

       The limit applies only to new requests being activated.
       When a new value is set, the agent will continue processing
       all the requests already active, even if their number
       exceeds the limit just imposed."
    DEFVAL { 10 }
    ::= { traceRouteObjects 1 }


  -- Traceroute Control Table

 traceRouteCtlTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF TraceRouteCtlEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines the Remote Operations Traceroute Control Table for
        providing the capability of invoking traceroute from a remote
        host.  The results of traceroute operations can be stored in
        the traceRouteResultsTable, traceRouteProbeHistoryTable, and
        the traceRouteHopsTable."
   ::= { traceRouteObjects 2 }

 traceRouteCtlEntry OBJECT-TYPE
    SYNTAX      TraceRouteCtlEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION


        "Defines an entry in the traceRouteCtlTable.  The first
        index element, traceRouteCtlOwnerIndex, is of type
        SnmpAdminString, a textual convention that allows for
        use of the SNMPv3 View-Based Access Control Model
        (RFC 3415, VACM) and that allows a management
        application to identify its entries.  The second index,
        traceRouteCtlTestName (also an SnmpAdminString),
        enables the same management application to have
        multiple requests outstanding."
    INDEX {
            traceRouteCtlOwnerIndex,
            traceRouteCtlTestName
          }
    ::= { traceRouteCtlTable 1 }

 TraceRouteCtlEntry ::=
    SEQUENCE {
      traceRouteCtlOwnerIndex         SnmpAdminString,
      traceRouteCtlTestName           SnmpAdminString,
      traceRouteCtlTargetAddressType  InetAddressType,
      traceRouteCtlTargetAddress      InetAddress,
      traceRouteCtlByPassRouteTable   TruthValue,
      traceRouteCtlDataSize           Unsigned32,
      traceRouteCtlTimeOut            Unsigned32,
      traceRouteCtlProbesPerHop       Unsigned32,
      traceRouteCtlPort               Unsigned32,
      traceRouteCtlMaxTtl             Unsigned32,
      traceRouteCtlDSField            Unsigned32,
      traceRouteCtlSourceAddressType  InetAddressType,
      traceRouteCtlSourceAddress      InetAddress,
      traceRouteCtlIfIndex            InterfaceIndexOrZero,
      traceRouteCtlMiscOptions        SnmpAdminString,
      traceRouteCtlMaxFailures        Unsigned32,
      traceRouteCtlDontFragment       TruthValue,
      traceRouteCtlInitialTtl         Unsigned32,
      traceRouteCtlFrequency          Unsigned32,
      traceRouteCtlStorageType        StorageType,
      traceRouteCtlAdminStatus        INTEGER,
      traceRouteCtlDescr              SnmpAdminString,
      traceRouteCtlMaxRows            Unsigned32,
      traceRouteCtlTrapGeneration     BITS,
      traceRouteCtlCreateHopsEntries  TruthValue,
      traceRouteCtlType               OBJECT IDENTIFIER,
      traceRouteCtlRowStatus          RowStatus
    }

 traceRouteCtlOwnerIndex OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(0..32))


    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "To facilitate the provisioning of access control by a
       security administrator using the View-Based Access
       Control Model (RFC 3415, VACM) for tables in which
       multiple users may need to create or
       modify entries independently, the initial index is used as
       an 'owner index'.  Such an initial index has a syntax of
       SnmpAdminString and can thus be trivially mapped to a
       securityName or groupName defined in VACM, in
       accordance with a security policy.

       When used in conjunction with such a security policy,
       all entries in the table belonging to a particular user
       (or group) will have the same value for this initial
       index.  For a given user's entries in a particular
       table, the object identifiers for the information in
       these entries will have the same subidentifiers (except
       for the 'column' subidentifier) up to the end of the
       encoded owner index. To configure VACM to permit access
       to this portion of the table, one would create
       vacmViewTreeFamilyTable entries with the value of
       vacmViewTreeFamilySubtree including the owner index
       portion, and vacmViewTreeFamilyMask 'wildcarding' the
       column subidentifier.  More elaborate configurations
       are possible."
    ::= { traceRouteCtlEntry 1 }

  traceRouteCtlTestName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(0..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of a traceroute test.  This is locally unique,
        within the scope of a traceRouteCtlOwnerIndex."
    ::= { traceRouteCtlEntry 2 }

 traceRouteCtlTargetAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the type of host address to be used on the
        traceroute request at the remote host."
    DEFVAL { unknown }
    ::= { traceRouteCtlEntry 3 }



 traceRouteCtlTargetAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the host address used on the
        traceroute request at the remote host.  The
        host address type can be determined by
        examining the value of the corresponding
        traceRouteCtlTargetAddressType.

        A value for this object MUST be set prior to
        transitioning its corresponding traceRouteCtlEntry to
        active(1) via traceRouteCtlRowStatus."
    ::= { traceRouteCtlEntry 4 }

 traceRouteCtlByPassRouteTable OBJECT-TYPE
    SYNTAX TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
       "The purpose of this object is to enable optional
       bypassing the route table.  If enabled, the remote
       host will bypass the normal routing tables and send
       directly to a host on an attached network.  If the
       host is not on a directly attached network, an
       error is returned.  This option can be used to perform
       the traceroute operation to a local host through an
       interface that has no route defined (e.g., after the
       interface was dropped by the routing daemon at the host)."
    DEFVAL { false }
    ::= { traceRouteCtlEntry 5 }

 traceRouteCtlDataSize OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65507)
    UNITS       "octets"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the size of the data portion of a traceroute
        request, in octets.  If the RECOMMENDED traceroute method
        (UDP datagrams as probes) is used, then the value
        contained in this object MUST be applied.  If another
        traceroute method is used for which the specified size
        is not appropriate, then the implementation SHOULD use
        whatever size (appropriate to the method) is closest to
        the specified size.




        The maximum value for this object was computed by
        subtracting the smallest possible IP header size of
        20 octets (IPv4 header with no options) and the UDP
        header size of 8 octets from the maximum IP packet size.
        An IP packet has a maximum size of 65535 octets
        (excluding IPv6 Jumbograms)."
    DEFVAL { 0 }
    ::= { traceRouteCtlEntry 6 }

 traceRouteCtlTimeOut OBJECT-TYPE
    SYNTAX      Unsigned32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the time-out value, in seconds, for
        a traceroute request."
    DEFVAL { 3 }
    ::= { traceRouteCtlEntry 7 }

 traceRouteCtlProbesPerHop OBJECT-TYPE
    SYNTAX      Unsigned32 (1..10)
    UNITS       "probes"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the number of times to reissue a traceroute
        request with the same time-to-live (TTL) value."
    DEFVAL { 3 }
    ::= { traceRouteCtlEntry 8 }

 traceRouteCtlPort OBJECT-TYPE
    SYNTAX      Unsigned32 (1..65535)
    UNITS       "UDP Port"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the (initial) UDP port to send the traceroute
        request to.  A port needs to be specified that is not in
        use at the destination (target) host.  The default
        value for this object is the IANA assigned port,
        33434, for the traceroute function."
    DEFVAL { 33434 }
    ::= { traceRouteCtlEntry 9 }

 traceRouteCtlMaxTtl OBJECT-TYPE
    SYNTAX      Unsigned32 (1..255)
    UNITS       "time-to-live value"


    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the maximum time-to-live value."
    DEFVAL { 30 }
    ::= { traceRouteCtlEntry 10 }

 traceRouteCtlDSField OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    MAX-ACCESS  read-create
    STATUS      current

    DESCRIPTION
        "Specifies the value to store in the Type of Service
        (TOS) octet in the IPv4 header or in the Traffic
        Class octet in the IPv6 header, respectively, of the
        IP packet used to encapsulate the traceroute probe.

        The octet to be set in the IP header contains the
        Differentiated Services (DS) Field in the six most
        significant bits.

        This option can be used to determine what effect an
        explicit DS Field setting has on a traceroute response.
        Not all values are legal or meaningful.  A value of 0
        means that the function represented by this option is
        not supported.  DS Field usage is often not supported
        by IP implementations, and not all values are supported.
        Refer to RFC 2474 and RFC 3260 for guidance on usage of
        this field."
    REFERENCE
        "Refer to RFC 1812 for the definition of the IPv4 TOS
        octet and to RFC 2460 for the definition of the IPv6
        Traffic Class octet.  Refer to RFC 2474 and RFC 3260
        for the definition of the Differentiated Services Field."
    DEFVAL { 0 }
    ::= { traceRouteCtlEntry 11 }

 traceRouteCtlSourceAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the type of the source address,
        traceRouteCtlSourceAddress, to be used at a remote host
        when a traceroute operation is performed."
    DEFVAL { unknown }
    ::= { traceRouteCtlEntry 12 }


 traceRouteCtlSourceAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Use the specified IP address (which must be given as an
        IP number, not a hostname) as the source address in
        outgoing probe packets.  On hosts with more than one IP
        address, this option can be used to select the address
        to be used.  If the IP address is not one of this
        machine's interface addresses, an error is returned, and
        nothing is sent.  A zero-length octet string value for
        this object disables source address specification.
        The address type (InetAddressType) that relates to
        this object is specified by the corresponding value
        of traceRouteCtlSourceAddressType."
    DEFVAL { ''H }
    ::= { traceRouteCtlEntry 13 }

 traceRouteCtlIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Setting this object to an interface's ifIndex prior
        to starting a remote traceroute operation directs
        the traceroute probes to be transmitted over the
        specified interface.  A value of zero for this object
        implies that this option is not enabled."
    DEFVAL { 0 }
    ::= { traceRouteCtlEntry 14 }

 traceRouteCtlMiscOptions OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enables an application to specify implementation-dependent
        options."
    DEFVAL { ''H }
    ::= { traceRouteCtlEntry 15 }

 traceRouteCtlMaxFailures OBJECT-TYPE
    SYNTAX      Unsigned32 (0..255)
    UNITS       "timeouts"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION


        "The value of this object indicates the maximum number
        of consecutive timeouts allowed before a remote traceroute
        request is terminated.  A value of either 255 (maximum
        hop count/possible TTL value) or 0 indicates that the
        function of terminating a remote traceroute request when a
        specific number of consecutive timeouts are detected is
        disabled."
    DEFVAL { 5 }
    ::= { traceRouteCtlEntry 16 }

 traceRouteCtlDontFragment OBJECT-TYPE
    SYNTAX         TruthValue
    MAX-ACCESS     read-create
    STATUS         current
    DESCRIPTION
        "This object enables setting of the don't fragment flag (DF)
        in the IP header for a probe.  Use of this object enables
        a manual PATH MTU test is performed."
    DEFVAL  { false }
    ::= { traceRouteCtlEntry 17 }

 traceRouteCtlInitialTtl OBJECT-TYPE
    SYNTAX         Unsigned32 (1..255)
    MAX-ACCESS     read-create
    STATUS         current
    DESCRIPTION
        "The value of this object specifies the initial TTL value to
        use.  This enables bypassing the initial (often well known)
        portion of a path."
    DEFVAL { 1 }
    ::= { traceRouteCtlEntry 18 }

 traceRouteCtlFrequency  OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The number of seconds to wait before repeating a
        traceroute test, as defined by the value of the
        various objects in the corresponding row.

        After a single test is completed the number of seconds
        as defined by the value of traceRouteCtlFrequency MUST
        elapse before the next traceroute test is started.

        A value of 0 for this object implies that the test
        as defined by the corresponding entry will not be


        repeated."
    DEFVAL { 0 }
    ::= { traceRouteCtlEntry 19 }

 traceRouteCtlStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this conceptual row.
        Conceptual rows having the value 'permanent' need not
        allow write-access to any columnar objects in the row."
    DEFVAL { nonVolatile }
    ::= { traceRouteCtlEntry 20 }

 traceRouteCtlAdminStatus OBJECT-TYPE
    SYNTAX      INTEGER {

                          enabled(1), -- operation should be started
                          disabled(2) -- operation should be stopped
                        }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Reflects the desired state that an traceRouteCtlEntry
        should be in:

           enabled(1)  - Attempt to activate the test as defined by
                         this traceRouteCtlEntry.
           disabled(2) - Deactivate the test as defined by this
                         traceRouteCtlEntry.

        Refer to the corresponding traceRouteResultsOperStatus to
        determine the operational state of the test defined by
        this entry."
     DEFVAL { disabled }
    ::= { traceRouteCtlEntry 21 }

 traceRouteCtlDescr OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The purpose of this object is to provide a
        descriptive name of the remote traceroute
        test."
    DEFVAL { ''H }
    ::= { traceRouteCtlEntry 22 }


 traceRouteCtlMaxRows OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "rows"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The maximum number of corresponding entries allowed
        in the traceRouteProbeHistoryTable.  An implementation
        of this MIB will remove the oldest corresponding entry
        in the traceRouteProbeHistoryTable to allow the
        addition of an new entry once the number of
        corresponding rows in the traceRouteProbeHistoryTable
        reaches this value.

        Old entries are not removed when a new test is
        started.  Entries are added to the
        traceRouteProbeHistoryTable until traceRouteCtlMaxRows
        is reached before entries begin to be removed.
        A value of 0 for this object disables creation of
        traceRouteProbeHistoryTable entries."
    DEFVAL      { 50 }
    ::= { traceRouteCtlEntry 23 }

 traceRouteCtlTrapGeneration OBJECT-TYPE
    SYNTAX      BITS {
                  pathChange(0),
                  testFailure(1),
                  testCompletion(2)
                }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object determines when and whether to
        generate a notification for this entry:

        pathChange(0)     - Generate a traceRoutePathChange
            notification when the current path varies from a
            previously determined path.
        testFailure(1)    - Generate a traceRouteTestFailed
            notification when the full path to a target
            can't be determined.
        testCompletion(2) - Generate a traceRouteTestCompleted
            notification when the path to a target has been
            determined.

        The value of this object defaults to an empty set,
        indicating that none of the above options has been
        selected."


    DEFVAL { { } }
    ::= { traceRouteCtlEntry 24 }

 traceRouteCtlCreateHopsEntries OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The current path for a traceroute test is kept in the
        traceRouteHopsTable on a per-hop basis when the value of
        this object is true(1)."
    DEFVAL { false }
    ::= { traceRouteCtlEntry 25 }

 traceRouteCtlType OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The value of this object is used either to report or to
        select the implementation method to be used for
        performing a traceroute operation.  The value of this
        object may be selected from
        traceRouteImplementationTypeDomains.

        Additional implementation types should be allocated as
        required by implementers of the DISMAN-TRACEROUTE-MIB
        under their enterprise specific registration point,
        not beneath traceRouteImplementationTypeDomains."
    DEFVAL { traceRouteUsingUdpProbes }
    ::= { traceRouteCtlEntry 26 }

 traceRouteCtlRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object allows entries to be created and deleted
        in the traceRouteCtlTable.  Deletion of an entry in
        this table results in a deletion of all corresponding (same
        traceRouteCtlOwnerIndex and traceRouteCtlTestName
        index values) traceRouteResultsTable,
        traceRouteProbeHistoryTable, and traceRouteHopsTable
        entries.

        A value MUST be specified for traceRouteCtlTargetAddress
        prior to acceptance of a transition to active(1) state.




        When a value for pingCtlTargetAddress is set,
        the value of object pingCtlRowStatus changes
        from notReady(3) to notInService(2).

        Activation of a remote traceroute operation is
        controlled via traceRouteCtlAdminStatus, and not
        by transitioning of this object's value to active(1).

        Transitions in and out of active(1) state are not
        allowed while an entry's traceRouteResultsOperStatus
        is active(1), with the exception that deletion of
        an entry in this table by setting its RowStatus
        object to destroy(6) will stop an active
        traceroute operation.

        The operational state of an traceroute operation
        can be determined by examination of the corresponding
        traceRouteResultsOperStatus object."
    REFERENCE
        "See definition of RowStatus in RFC 2579, 'Textual
        Conventions for SMIv2.'"
    ::= { traceRouteCtlEntry 27 }


 -- Traceroute Results Table

 traceRouteResultsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF TraceRouteResultsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines the Remote Operations Traceroute Results Table for
        keeping track of the status of a traceRouteCtlEntry.

        An entry is added to the traceRouteResultsTable when an
        traceRouteCtlEntry is started by successful transition
        of its traceRouteCtlAdminStatus object to enabled(1).

        If the object traceRouteCtlAdminStatus already has the value
        enabled(1), and if the corresponding
        traceRouteResultsOperStatus object has the value
        completed(3), then successfully writing enabled(1) to the
        object traceRouteCtlAdminStatus re-initializes the already
        existing entry in the traceRouteResultsTable.  The values of
        objects in the re-initialized entry are the same as
        the values of objects in a new entry would be.

        An entry is removed from the traceRouteResultsTable when



        its corresponding traceRouteCtlEntry is deleted."
   ::= { traceRouteObjects 3 }

 traceRouteResultsEntry OBJECT-TYPE
    SYNTAX      TraceRouteResultsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines an entry in the traceRouteResultsTable.  The
        traceRouteResultsTable has the same indexing as the
        traceRouteCtlTable so that a traceRouteResultsEntry
        corresponds to the traceRouteCtlEntry that caused it to
        be created."
    INDEX {
            traceRouteCtlOwnerIndex,
            traceRouteCtlTestName
          }
    ::= { traceRouteResultsTable 1 }

 TraceRouteResultsEntry ::=
    SEQUENCE {
      traceRouteResultsOperStatus       INTEGER,
      traceRouteResultsCurHopCount      Gauge32,
      traceRouteResultsCurProbeCount    Gauge32,
      traceRouteResultsIpTgtAddrType    InetAddressType,
      traceRouteResultsIpTgtAddr        InetAddress,
      traceRouteResultsTestAttempts     Gauge32,
      traceRouteResultsTestSuccesses    Gauge32,
      traceRouteResultsLastGoodPath     DateAndTime
    }

 traceRouteResultsOperStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                          enabled(1),  -- test is in progress
                          disabled(2), -- test has stopped
                          completed(3) -- test is completed
                        }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reflects the operational state of an traceRouteCtlEntry:

           enabled(1)   - Test is active.
           disabled(2)  - Test has stopped.
           completed(3) - Test is completed."
    ::= { traceRouteResultsEntry 1 }

 traceRouteResultsCurHopCount OBJECT-TYPE


    SYNTAX      Gauge32
    UNITS       "hops"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reflects the current TTL value (from 1 to
        255) for a remote traceroute operation.
        Maximum TTL value is determined by
        traceRouteCtlMaxTtl."
    ::= { traceRouteResultsEntry 2 }

 traceRouteResultsCurProbeCount OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "probes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reflects the current probe count (1..10) for
        a remote traceroute operation.  The maximum
        probe count is determined by
        traceRouteCtlProbesPerHop."
    ::= { traceRouteResultsEntry 3 }

 traceRouteResultsIpTgtAddrType OBJECT-TYPE
    SYNTAX      InetAddressType

    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the type of address stored
        in the corresponding traceRouteResultsIpTgtAddr
        object."
    ::= { traceRouteResultsEntry 4 }

 traceRouteResultsIpTgtAddr OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reports the IP address associated
        with a traceRouteCtlTargetAddress value when the
        destination address is specified as a DNS name.
        The value of this object should be a zero-length
        octet string when a DNS name is not specified or
        when a specified DNS name fails to resolve."
    ::= { traceRouteResultsEntry 5 }

 traceRouteResultsTestAttempts OBJECT-TYPE


    SYNTAX      Gauge32
    UNITS       "tests"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current number of attempts to determine a path
        to a target.  The value of this object MUST be started
        at 0."
    ::= { traceRouteResultsEntry 6 }

 traceRouteResultsTestSuccesses OBJECT-TYPE
    SYNTAX      Gauge32
    UNITS       "tests"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current number of attempts to determine a path
        to a target that have succeeded.  The value of this
        object MUST be reported as 0 when no attempts have
        succeeded."
    ::= { traceRouteResultsEntry 7 }

 traceRouteResultsLastGoodPath OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The date and time when the last complete path
        was determined.  A path is complete if responses
        were received or timeout occurred for each hop on
        the path; i.e., for each TTL value from the value
        of the corresponding traceRouteCtlInitialTtl object
        up to the end of the path or (if no reply from the
        target IP address was received) up to the value of
        the corresponding traceRouteCtlMaxTtl object."
    ::= { traceRouteResultsEntry 8 }

 -- Trace Route Probe History Table

 traceRouteProbeHistoryTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF TraceRouteProbeHistoryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines the Remote Operations Traceroute Results Table
        for storing the results of a traceroute operation.

        An implementation of this MIB will remove the oldest


        entry in the traceRouteProbeHistoryTable of the
        corresponding entry in the traceRouteCtlTable to allow
        the addition of a new entry once the number of rows in
        the traceRouteProbeHistoryTable reaches the value specified
        by traceRouteCtlMaxRows for the corresponding entry in the
        traceRouteCtlTable."
   ::= { traceRouteObjects 4 }

 traceRouteProbeHistoryEntry OBJECT-TYPE
    SYNTAX      TraceRouteProbeHistoryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines a table for storing the results of a traceroute
        operation.  Entries in this table are limited by
        the value of the corresponding traceRouteCtlMaxRows
        object.

        The first two index elements identify the
        traceRouteCtlEntry that a traceRouteProbeHistoryEntry
        belongs to.  The third index element selects a single
        traceroute operation result.  The fourth and fifth indexes
        select the hop and the probe for a particular
        traceroute operation."
    INDEX {
             traceRouteCtlOwnerIndex,
             traceRouteCtlTestName,
             traceRouteProbeHistoryIndex,
             traceRouteProbeHistoryHopIndex,
             traceRouteProbeHistoryProbeIndex

          }
    ::= { traceRouteProbeHistoryTable 1 }

 TraceRouteProbeHistoryEntry ::=
    SEQUENCE {
      traceRouteProbeHistoryIndex         Unsigned32,
      traceRouteProbeHistoryHopIndex      Unsigned32,
      traceRouteProbeHistoryProbeIndex    Unsigned32,
      traceRouteProbeHistoryHAddrType     InetAddressType,
      traceRouteProbeHistoryHAddr         InetAddress,
      traceRouteProbeHistoryResponse      Unsigned32,
      traceRouteProbeHistoryStatus        OperationResponseStatus,
      traceRouteProbeHistoryLastRC        Integer32,
      traceRouteProbeHistoryTime          DateAndTime
    }

 traceRouteProbeHistoryIndex OBJECT-TYPE



    SYNTAX      Unsigned32 (1..'ffffffff'h)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in this table is created when the result of
        a traceroute probe is determined.  The initial 2 instance
        identifier index values identify the traceRouteCtlEntry
        that a probe result (traceRouteProbeHistoryEntry) belongs
        to.  An entry is removed from this table when
        its corresponding traceRouteCtlEntry is deleted.

        An implementation MUST start assigning
        traceRouteProbeHistoryIndex values at 1 and wrap after
        exceeding the maximum possible value, as defined by the
        limit of this object ('ffffffff'h)."
    ::= { traceRouteProbeHistoryEntry 1 }

 traceRouteProbeHistoryHopIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (1..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "Indicates which hop in a traceroute path the probe's
       results are for.  The value of this object is initially
       determined by the value of traceRouteCtlInitialTtl."
    ::= { traceRouteProbeHistoryEntry 2 }

 traceRouteProbeHistoryProbeIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (1..10)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "Indicates the index of a probe for a particular
       hop in a traceroute path.  The number of probes per
       hop is determined by the value of the corresponding
       traceRouteCtlProbesPerHop object."
    ::= { traceRouteProbeHistoryEntry 3 }

 traceRouteProbeHistoryHAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This objects indicates the type of address stored
        in the corresponding traceRouteProbeHistoryHAddr
        object."
    ::= { traceRouteProbeHistoryEntry 4 }




 traceRouteProbeHistoryHAddr OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "The address of a hop in a traceroute path.  This object
       is not allowed to be a DNS name.  The value of the
       corresponding object, traceRouteProbeHistoryHAddrType,
       indicates this object's IP address type."
    ::= { traceRouteProbeHistoryEntry 5 }

 traceRouteProbeHistoryResponse OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The amount of time measured in milliseconds from when
        a probe was sent to when its response was received or
        when it timed out.  The value of this object is reported
        as 0 when it is not possible to transmit a probe."
    ::= { traceRouteProbeHistoryEntry 6 }

 traceRouteProbeHistoryStatus OBJECT-TYPE
    SYNTAX      OperationResponseStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The result of a traceroute operation made by a remote
        host for a particular probe."
    ::= { traceRouteProbeHistoryEntry 7 }

 traceRouteProbeHistoryLastRC OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only

    STATUS      current
    DESCRIPTION
        "The last implementation-method-specific reply code received.

        Traceroute is usually implemented by transmitting a series of
        probe packets with increasing time-to-live values.  A probe
        packet is a UDP datagram encapsulated into an IP packet.
        Each hop in a path to the target (destination) host rejects
        the probe packets (probe's TTL too small, ICMP reply) until
        either the maximum TTL is exceeded or the target host is
        received."
    ::= { traceRouteProbeHistoryEntry 8 }



 traceRouteProbeHistoryTime OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Timestamp for when this probe's results were determined."
    ::= { traceRouteProbeHistoryEntry 9 }

 -- Traceroute Hop Results Table

 traceRouteHopsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF TraceRouteHopsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines the Remote Operations Traceroute Hop Table for
        keeping track of the results of traceroute tests on a
        per-hop basis."
    ::= { traceRouteObjects 5 }

 traceRouteHopsEntry OBJECT-TYPE
    SYNTAX      TraceRouteHopsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines an entry in the traceRouteHopsTable.
        The first two index elements identify the
        traceRouteCtlEntry that a traceRouteHopsEntry
        belongs to.  The third index element,
        traceRouteHopsHopIndex, selects a
        hop in a traceroute path."
    INDEX {
            traceRouteCtlOwnerIndex,
            traceRouteCtlTestName,
            traceRouteHopsHopIndex
          }

    ::= { traceRouteHopsTable 1 }

 TraceRouteHopsEntry ::=
    SEQUENCE {
        traceRouteHopsHopIndex         Unsigned32,
        traceRouteHopsIpTgtAddressType InetAddressType,
        traceRouteHopsIpTgtAddress     InetAddress,
        traceRouteHopsMinRtt           Unsigned32,
        traceRouteHopsMaxRtt           Unsigned32,
        traceRouteHopsAverageRtt       Unsigned32,
        traceRouteHopsRttSumOfSquares  Unsigned32,



        traceRouteHopsSentProbes       Unsigned32,
        traceRouteHopsProbeResponses   Unsigned32,
        traceRouteHopsLastGoodProbe    DateAndTime
      }

 traceRouteHopsHopIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (1..'ffffffff'h)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Specifies the hop index for a traceroute hop.  Values
        for this object with respect to the same
        traceRouteCtlOwnerIndex and traceRouteCtlTestName
        MUST start at 1 and be given increasing values for
        subsequent hops.  The value of traceRouteHopsHopIndex is not
        necessarily the number of the hop on the traced path.

        The traceRouteHopsTable keeps the current traceroute
        path per traceRouteCtlEntry if enabled by
        setting the corresponding traceRouteCtlCreateHopsEntries
        to true(1).

        All hops (traceRouteHopsTable entries) in a traceroute
        path MUST be updated at the same time when a traceroute
        operation is completed.  Care needs to be applied when a path
        either changes or can't be determined.  The initial portion
        of the path, up to the first hop change, MUST retain the
        same traceRouteHopsHopIndex values.  The remaining portion
        of the path SHOULD be assigned new traceRouteHopsHopIndex
        values."
    ::= { traceRouteHopsEntry 1 }

 traceRouteHopsIpTgtAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the type of address stored
        in the corresponding traceRouteHopsIpTgtAddress
        object."
    ::= { traceRouteHopsEntry 2 }

 traceRouteHopsIpTgtAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object reports the IP address associated with



        the hop.  A value for this object should be reported
        as a numeric IP address, not as a DNS name.

        The address type (InetAddressType) that relates to
        this object is specified by the corresponding value
        of pingCtlSourceAddressType."
    ::= { traceRouteHopsEntry 3 }

 traceRouteHopsMinRtt OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The minimum traceroute round-trip-time (RTT) received for
        this hop.  A value of 0 for this object implies that no
        RTT has been received."
    ::= { traceRouteHopsEntry 4 }

 traceRouteHopsMaxRtt OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The maximum traceroute round-trip-time (RTT) received for
        this hop.  A value of 0 for this object implies that no
        RTT has been received."
    ::= { traceRouteHopsEntry 5 }

 traceRouteHopsAverageRtt OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current average traceroute round-trip-time (RTT) for
        this hop."
    ::= { traceRouteHopsEntry 6 }

 traceRouteHopsRttSumOfSquares OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object contains the sum of the squares of all
        round-trip-times received for this hop.  Its purpose is
        to enable standard deviation calculation."
    ::= { traceRouteHopsEntry 7 }

 traceRouteHopsSentProbes OBJECT-TYPE



    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of this object reflects the number of probes sent
        for this hop during this traceroute test.  The value of this
        object should start at 0."
    ::= { traceRouteHopsEntry 8 }

 traceRouteHopsProbeResponses OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of responses received for this hop during this
        traceroute test.  This value of this object should start
        at 0."
    ::= { traceRouteHopsEntry 9 }

 traceRouteHopsLastGoodProbe OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Date and time at which the last response was received for a
         probe for this hop during this traceroute test."
    ::= { traceRouteHopsEntry 10 }

 -- Notification Definition section

 traceRoutePathChange NOTIFICATION-TYPE
      OBJECTS {
        traceRouteCtlTargetAddressType,
        traceRouteCtlTargetAddress,
        traceRouteResultsIpTgtAddrType,
        traceRouteResultsIpTgtAddr
      }
      STATUS  current
      DESCRIPTION
          "The path to a target has changed."
      ::= { traceRouteNotifications 1 }

 traceRouteTestFailed NOTIFICATION-TYPE
      OBJECTS {
        traceRouteCtlTargetAddressType,
        traceRouteCtlTargetAddress,
        traceRouteResultsIpTgtAddrType,
        traceRouteResultsIpTgtAddr



      }
      STATUS  current
      DESCRIPTION
          "Could not determine the path to a target."
      ::= { traceRouteNotifications 2 }

 traceRouteTestCompleted NOTIFICATION-TYPE
      OBJECTS {
        traceRouteCtlTargetAddressType,
        traceRouteCtlTargetAddress,
        traceRouteResultsIpTgtAddrType,
        traceRouteResultsIpTgtAddr
      }
      STATUS  current
      DESCRIPTION
          "The path to a target has just been determined."
      ::= { traceRouteNotifications 3 }

 -- Conformance information
 -- Compliance statements

 traceRouteCompliances OBJECT IDENTIFIER
      ::= { traceRouteConformance 1 }
 traceRouteGroups      OBJECT IDENTIFIER
      ::= { traceRouteConformance 2 }

 -- Compliance statements

 traceRouteFullCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for SNMP entities that
            fully implement the DISMAN-TRACEROUTE-MIB."
    MODULE  -- this module
        MANDATORY-GROUPS {
                            traceRouteMinimumGroup,
                            traceRouteCtlRowStatusGroup,
                            traceRouteHistoryGroup
                         }

        GROUP traceRouteHopsTableGroup
        DESCRIPTION
            "This group lists the objects that make up a
            traceRouteHopsEntry.  Support of the traceRouteHopsTable
            is optional."

        GROUP traceRouteNotificationsGroup
        DESCRIPTION



            "This group defines a collection of optional
            notifications."

        OBJECT traceRouteMaxConcurrentRequests
        MIN-ACCESS  read-only
        DESCRIPTION
            "The agent is not required to support SET
            operations to this object."

        OBJECT traceRouteCtlByPassRouteTable
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access to this object is not required by
            implementations that are not capable of its
            implementation.  The function represented by this
            object is implementable if the setsockopt
            SOL_SOCKET SO_DONTROUTE option is supported."

        OBJECT traceRouteCtlDSField
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  If write access is
            not supported, return a 0 as the value of this object.
            A value of 0 implies that the function represented by
            this option is not supported."

        OBJECT traceRouteCtlSourceAddressType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access to this object is not required by
            implementations that are not capable of binding the
            send socket with a source address.  An implementation
            is only required to support IPv4 and IPv6 addresses."

        OBJECT traceRouteCtlSourceAddress
        SYNTAX  InetAddress (SIZE(0|4|16))
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access to this object is not required by
            implementations that are not capable of binding the
            send socket with a source address.  An implementation
            is only required to support IPv4 and IPv6 addresses."

        OBJECT traceRouteCtlIfIndex
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  If write access is



            not supported, return a 0 as the value of this object.
            A value of 0 implies that the function represented by
            this option is not supported."

        OBJECT traceRouteCtlMiscOptions
        MIN-ACCESS  read-only
        DESCRIPTION
            "Support of this object is optional.  If not
            supporting, do not allow write access and return a
            zero-length octet string as the value of the object."

        OBJECT traceRouteCtlStorageType
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  It is also allowed
            that implementations support only the volatile(2)
            StorageType enumeration."

        OBJECT traceRouteCtlType
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  In addition, the only
            value that is RECOMMENDED to be supported by an
            implementation is traceRouteUsingUdpProbes."

        OBJECT traceRouteResultsIpTgtAddrType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteResultsIpTgtAddr
        SYNTAX  InetAddress (SIZE(0|4|16))
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteResultsLastGoodPath
        DESCRIPTION
            "If the traceRouteHopsTableGroup is implemented, then
            this object is mandatory for implementations that have
            access to a system clock and that are capable of setting
            the values for DateAndTime objects.  It is RECOMMENDED
            that when this object is not supported its values
            be reported as '0000000000000000'H."

        OBJECT traceRouteProbeHistoryHAddrType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }



        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteProbeHistoryHAddr
        SYNTAX  InetAddress (SIZE(0|4|16))
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteProbeHistoryTime
        DESCRIPTION
            "This object is mandatory for implementations that have
            access to a system clock and that are capable of setting
            the values for DateAndTime objects.  It is RECOMMENDED
            that when this object is not supported its values
            be reported as '0000000000000000'H."

        OBJECT traceRouteHopsIpTgtAddressType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteHopsIpTgtAddress
        SYNTAX  InetAddress (SIZE(0|4|16))
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteHopsLastGoodProbe
        DESCRIPTION
            "This object is mandatory for implementations that have
            access to a system clock and that are capable of setting
            the values for DateAndTime objects.  It is RECOMMENDED
            that when this object is not supported its values
            be reported as '0000000000000000'H."

    ::= { traceRouteCompliances 2 }

 traceRouteMinimumCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The minimum compliance statement for SNMP entities
            which implement the minimal subset of the
            DISMAN-TRACEROUTE-MIB.  Implementors might choose this
            subset for small devices with limited resources."
    MODULE  -- this module



        MANDATORY-GROUPS { traceRouteMinimumGroup }

        GROUP traceRouteCtlRowStatusGroup
        DESCRIPTION
            "A compliant implementation does not have to implement
            the traceRouteCtlRowStatusGroup."

        GROUP traceRouteHistoryGroup
        DESCRIPTION
            "A compliant implementation does not have to implement
            the traceRouteHistoryGroup."

        GROUP traceRouteHopsTableGroup
        DESCRIPTION
            "This group lists the objects that make up a
            traceRouteHopsEntry.  Support of the traceRouteHopsTable
            is optional."

        GROUP traceRouteNotificationsGroup
        DESCRIPTION
            "This group defines a collection of optional
            notifications."

        OBJECT traceRouteMaxConcurrentRequests
        MIN-ACCESS  read-only
        DESCRIPTION
            "The agent is not required to support SET
            operations to this object."

        OBJECT traceRouteCtlByPassRouteTable
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  If write access is
            not supported, return a false(2) as the value of this
            object.  A value of false(2) means that the function
            represented by this option is not supported."

        OBJECT traceRouteCtlDSField
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  If write access is
            not supported, return a 0 as the value of this object.
            A value of 0 implies that the function represented by
            this option is not supported."

        OBJECT traceRouteCtlSourceAddressType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        MIN-ACCESS  read-only



        DESCRIPTION
            "Write access to this object is not required by
            implementations that are not capable of binding the
            send socket with a source address.  An implementation
            is only required to support IPv4 and IPv6 addresses."

        OBJECT traceRouteCtlSourceAddress
        SYNTAX  InetAddress (SIZE(0|4|16))
        MIN-ACCESS  read-only

        DESCRIPTION
            "Write access to this object is not required by
            implementations that are not capable of binding the
            send socket with a source address.  An implementation
            is only required to support IPv4 and IPv6 addresses."

        OBJECT traceRouteCtlIfIndex
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  If write access is
            not supported, return a 0 as the value of this object.
            A value of 0 implies that the function represented by
            this option is not supported."

        OBJECT traceRouteCtlMiscOptions
        MIN-ACCESS  read-only
        DESCRIPTION
            "Support of this object is optional.  If not
            supporting, do not allow write access, and return a
            zero-length octet string as the value of the object."

        OBJECT traceRouteCtlDontFragment
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  If write access is
            not supported, return a false(2) as the value of this
            object.  A value of false(2) means that the function
            represented by this option is not supported."

        OBJECT traceRouteCtlInitialTtl
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  If write access is
            not supported, return a 1 as the value of this object."

        OBJECT traceRouteCtlFrequency
        MIN-ACCESS  read-only
        DESCRIPTION



            "Write access is not required.  If write access is
            not supported, return a 0 as the value of this object.
            A value of 0 implies that the function represented by
            this option is not supported."

        OBJECT traceRouteCtlStorageType
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  It is also allowed
            that implementations support only the volatile(2)
            StorageType enumeration."

        OBJECT traceRouteCtlDescr
        MIN-ACCESS  read-only
        DESCRIPTION
            "The agent is not required to support set
            operations to this object."

        OBJECT traceRouteCtlMaxRows
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  If the
            traceRouteHistoryGroup is not implemented, then write
            access to this object MUST be disabled, and the object
            MUST return a value of 0 when retrieved."

        OBJECT traceRouteCtlTrapGeneration
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  If the
            traceRouteNotificationsGroup is not implemented, then
            write access to this object MUST be disabled, and the
            object MUST return a value with no bit set when
            retrieved.  No bit set indicates that no notification
            is generated."

        OBJECT traceRouteCtlCreateHopsEntries
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  If the
            traceRouteHopsTableGroup is not implemented, then
            write access to this object MUST be disabled, and the
            object MUST return a value of false(2) when retrieved."

        OBJECT traceRouteCtlType
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  In addition, the only



            value that is RECOMMENDED to be supported by an
            implementation is traceRouteUsingUdpProbes."

        OBJECT traceRouteResultsIpTgtAddrType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteResultsIpTgtAddr
        SYNTAX  InetAddress (SIZE(0|4|16))
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteResultsLastGoodPath
        DESCRIPTION
            "This object is mandatory for implementations that have
            access to a system clock and that are capable of setting
            the values for DateAndTime objects.  It is RECOMMENDED
            that when this object is not supported its values
            be reported as '0000000000000000'H."

        OBJECT traceRouteProbeHistoryHAddrType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteProbeHistoryHAddr
        SYNTAX  InetAddress (SIZE(0|4|16))
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteProbeHistoryTime
        DESCRIPTION
            "If the traceRouteHistoryGroup is implemented, then
            this object is mandatory for implementations that have
            access to a system clock and that are capable of setting
            the values for DateAndTime objects.  It is RECOMMENDED
            that when this object is not supported its values
            be reported as '0000000000000000'H."

        OBJECT traceRouteHopsIpTgtAddressType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        DESCRIPTION
            "An implementation should only support IPv4 and



            globally unique IPv6 address values for this object."

        OBJECT traceRouteHopsIpTgtAddress
        SYNTAX  InetAddress (SIZE(0|4|16))
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteHopsLastGoodProbe
        DESCRIPTION
            "If the traceRouteHopsTableGroup is implemented, then
            this object is mandatory for implementations that have
            access to a system clock and that are capable of setting
            the values for DateAndTime objects.  It is RECOMMENDED
            that when this object is not supported its values
            be reported as '0000000000000000'H."

    ::= { traceRouteCompliances 3 }

 traceRouteCompliance MODULE-COMPLIANCE
    STATUS  deprecated
    DESCRIPTION
            "The compliance statement for the DISMAN-TRACEROUTE-MIB.
            This compliance statement has been deprecated because
            the traceRouteGroup and the traceRouteTimeStampGroup
            have been split and deprecated. The
            traceRouteFullCompliance is semantically identical to the
            deprecated traceRouteCompliance statement."
    MODULE  -- this module
        MANDATORY-GROUPS {
                            traceRouteGroup
                          }
        GROUP traceRouteTimeStampGroup
        DESCRIPTION
            "This group is mandatory for implementations that have
            access to a system clock and that are capable of setting
            the values for DateAndTime objects."

        GROUP traceRouteNotificationsGroup
        DESCRIPTION
            "This group defines a collection of optional
            notifications."

        GROUP traceRouteHopsTableGroup
        DESCRIPTION
            "This group lists the objects that make up a
            traceRouteHopsEntry.  Support of the traceRouteHopsTable
            is optional."



        OBJECT traceRouteMaxConcurrentRequests
        MIN-ACCESS  read-only
        DESCRIPTION
            "The agent is not required to support SET
            operations to this object."

        OBJECT traceRouteCtlByPassRouteTable
        MIN-ACCESS  read-only
        DESCRIPTION
            "This object is not required by implementations that
            are not capable of its implementation.  The function
            represented by this object is implementable if the
            setsockopt SOL_SOCKET SO_DONTROUTE option is
            supported."

        OBJECT traceRouteCtlSourceAddressType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        MIN-ACCESS  read-only

        DESCRIPTION
            "This object is not required by implementations that
            are not capable of binding the send socket with a
            source address.  An implementation is only required to
            support IPv4 and IPv6 addresses."

        OBJECT traceRouteCtlSourceAddress
        SYNTAX  InetAddress (SIZE(0|4|16))
        MIN-ACCESS  read-only
        DESCRIPTION
            "This object is not required by implementations that
            are not capable of binding the send socket with a
            source address.  An implementation is only required to
            support IPv4 and globally unique IPv6 addresses."

        OBJECT traceRouteCtlIfIndex
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  When write access is
            not supported, return a 0 as the value of this object.
            A value of 0 implies that the function represented by
            this option is not supported."

        OBJECT traceRouteCtlMiscOptions
        MIN-ACCESS  read-only
        DESCRIPTION
            "Support of this object is optional.  When not
            supporting, do not allow write access, and return a
            zero-length octet string as the value of the object."



        OBJECT traceRouteCtlStorageType
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  It is also allowed
           that implementations support only the volatile
            StorageType enumeration."

        OBJECT traceRouteCtlDSField
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  When write access is
            not supported, return a 0 as the value of this object.
            A value of 0 implies that the function represented by
            this option is not supported."

        OBJECT traceRouteCtlType
        MIN-ACCESS  read-only
        DESCRIPTION
            "Write access is not required.  In addition, the only
            value that is RECOMMENDED to be supported by an
            implementation is traceRouteUsingUdpProbes."

        OBJECT traceRouteResultsIpTgtAddrType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteResultsIpTgtAddr
        SYNTAX  InetAddress (SIZE(0|4|16))
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteProbeHistoryHAddrType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteProbeHistoryHAddr
        SYNTAX  InetAddress (SIZE(0|4|16))
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteHopsIpTgtAddressType
        SYNTAX  InetAddressType { unknown(0), ipv4(1), ipv6(2) }



        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."

        OBJECT traceRouteHopsIpTgtAddress
        SYNTAX  InetAddress (SIZE(0|4|16))
        DESCRIPTION
            "An implementation should only support IPv4 and
            globally unique IPv6 address values for this object."
    ::= { traceRouteCompliances 1 }

 -- MIB groupings

 traceRouteMinimumGroup OBJECT-GROUP
   OBJECTS {
             traceRouteMaxConcurrentRequests,
             traceRouteCtlTargetAddressType,
             traceRouteCtlTargetAddress,
             traceRouteCtlByPassRouteTable,
             traceRouteCtlDataSize,
             traceRouteCtlTimeOut,
             traceRouteCtlProbesPerHop,
             traceRouteCtlPort,
             traceRouteCtlMaxTtl,
             traceRouteCtlDSField,
             traceRouteCtlSourceAddressType,
             traceRouteCtlSourceAddress,
             traceRouteCtlIfIndex,
             traceRouteCtlMiscOptions,
             traceRouteCtlMaxFailures,
             traceRouteCtlDontFragment,
             traceRouteCtlInitialTtl,
             traceRouteCtlFrequency,
             traceRouteCtlStorageType,
             traceRouteCtlAdminStatus,
             traceRouteCtlMaxRows,
             traceRouteCtlTrapGeneration,
             traceRouteCtlDescr,
             traceRouteCtlCreateHopsEntries,
             traceRouteCtlType,
             traceRouteResultsOperStatus,
             traceRouteResultsCurHopCount,
             traceRouteResultsCurProbeCount,
             traceRouteResultsIpTgtAddrType,
             traceRouteResultsIpTgtAddr,
             traceRouteResultsTestAttempts,
             traceRouteResultsTestSuccesses,
             traceRouteResultsLastGoodPath



          }
   STATUS  current
   DESCRIPTION
       "The group of objects that constitute the remote traceroute
       operation."
   ::= { traceRouteGroups 5 }

 traceRouteCtlRowStatusGroup OBJECT-GROUP
   OBJECTS {
             traceRouteCtlRowStatus
          }
   STATUS  current
   DESCRIPTION
       "The RowStatus object of the traceRouteCtlTable."
   ::= { traceRouteGroups 6 }

 traceRouteHistoryGroup OBJECT-GROUP
   OBJECTS {
             traceRouteProbeHistoryHAddrType,
             traceRouteProbeHistoryHAddr,
             traceRouteProbeHistoryResponse,
             traceRouteProbeHistoryStatus,
             traceRouteProbeHistoryLastRC,
             traceRouteProbeHistoryTime
           }

   STATUS  current
   DESCRIPTION
       "The group of objects that constitute the history
       capability."
    ::= { traceRouteGroups 7 }

 traceRouteNotificationsGroup NOTIFICATION-GROUP
   NOTIFICATIONS {
             traceRoutePathChange,
             traceRouteTestFailed,
             traceRouteTestCompleted
          }
   STATUS   current
   DESCRIPTION
       "The notifications that are required to be supported by
       implementations of this MIB."
   ::= { traceRouteGroups 3 }

 traceRouteHopsTableGroup OBJECT-GROUP
   OBJECTS {
             traceRouteHopsIpTgtAddressType,
             traceRouteHopsIpTgtAddress,



             traceRouteHopsMinRtt,
             traceRouteHopsMaxRtt,
             traceRouteHopsAverageRtt,
             traceRouteHopsRttSumOfSquares,
             traceRouteHopsSentProbes,
             traceRouteHopsProbeResponses,
             traceRouteHopsLastGoodProbe
           }
    STATUS   current
    DESCRIPTION
        "The group of objects that constitute the
        traceRouteHopsTable."
  ::= { traceRouteGroups 4 }

 traceRouteGroup OBJECT-GROUP
   OBJECTS {
             traceRouteMaxConcurrentRequests,
             traceRouteCtlTargetAddressType,
             traceRouteCtlTargetAddress,
             traceRouteCtlByPassRouteTable,
             traceRouteCtlDataSize,
             traceRouteCtlTimeOut,
             traceRouteCtlProbesPerHop,
             traceRouteCtlPort,
             traceRouteCtlMaxTtl,
             traceRouteCtlDSField,
             traceRouteCtlSourceAddressType,
             traceRouteCtlSourceAddress,
             traceRouteCtlIfIndex,
             traceRouteCtlMiscOptions,
             traceRouteCtlMaxFailures,
             traceRouteCtlDontFragment,
             traceRouteCtlInitialTtl,
             traceRouteCtlFrequency,
             traceRouteCtlStorageType,
             traceRouteCtlAdminStatus,
             traceRouteCtlMaxRows,
             traceRouteCtlTrapGeneration,
             traceRouteCtlDescr,
             traceRouteCtlCreateHopsEntries,
             traceRouteCtlType,
             traceRouteCtlRowStatus,
             traceRouteResultsOperStatus,
             traceRouteResultsCurHopCount,
             traceRouteResultsCurProbeCount,
             traceRouteResultsIpTgtAddrType,
             traceRouteResultsIpTgtAddr,
             traceRouteResultsTestAttempts,



             traceRouteResultsTestSuccesses,
             traceRouteProbeHistoryHAddrType,
             traceRouteProbeHistoryHAddr,
             traceRouteProbeHistoryResponse,
             traceRouteProbeHistoryStatus,
             traceRouteProbeHistoryLastRC
          }
   STATUS  deprecated
   DESCRIPTION
       "The group of objects that constitute the remote traceroute
       operation."
   ::= { traceRouteGroups 1 }

 traceRouteTimeStampGroup OBJECT-GROUP
   OBJECTS {
             traceRouteResultsLastGoodPath,
             traceRouteProbeHistoryTime
           }
   STATUS  deprecated
   DESCRIPTION
       "The group of DateAndTime objects."
    ::= { traceRouteGroups 2 }

END





