 OSPFV3-MIB DEFINITIONS ::= BEGIN

 IMPORTS
         MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE, mib-2,
         Counter32, Gauge32, Integer32, Unsigned32
                 FROM SNMPv2-SMI
         TEXTUAL-CONVENTION, TruthValue, RowStatus, TimeStamp
                 FROM SNMPv2-TC
         MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
                 FROM SNMPv2-CONF
         InterfaceIndex
                 FROM IF-MIB
         InetAddressType, InetAddress, InetAddressPrefixLength,
         InetAddressIPv6
                 FROM INET-ADDRESS-MIB
         Metric, BigMetric, Status,
         HelloRange, DesignatedRouterPriority
                 FROM OSPF-MIB;

 ospfv3MIB MODULE-IDENTITY
         LAST-UPDATED "200908130000Z"
         ORGANIZATION "IETF OSPF Working Group"
         CONTACT-INFO
             "WG E-Mail: ospf@ietf.org
              WG Chairs: Acee Lindem
                         acee@redback.com

                         Abhay Roy
                         akr@cisco.com

              Editors:   Dan Joyal
                         Nortel
                         600 Technology Park Drive
                         Billerica, MA  01821, USA
                         djoyal@nortel.com

                         Vishwas Manral
                         IP Infusion
                         Almora, Uttarakhand
                         India
                         vishwas@ipinfusion.com"

          DESCRIPTION
             "The MIB module for OSPF version 3.

              Copyright (c) 2009 IETF Trust and the persons
              identified as authors of the code.  All rights
              reserved.

              Redistribution and use in source and binary forms, with
              or without modification, are permitted provided that
              the following conditions are met:

              - Redistributions of source code must retain the above
                copyright notice, this list of conditions and the
                following disclaimer.

             - Redistributions in binary form must reproduce the
               above copyright notice, this list of conditions and
               the following disclaimer in the documentation and/or
               other materials provided with the distribution.

             - Neither the name of Internet Society, IETF or IETF
               Trust, nor the names of specific contributors, may be
               used to endorse or promote products derived from this
               software without specific prior written permission.

               THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND
               CONTRIBUTORS 'AS IS' AND ANY EXPRESS OR IMPLIED
               WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
               WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A
               PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL
               THE COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY
               DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
               CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
               PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF
               USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)
               HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER
               IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING
               NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE
               USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
               POSSIBILITY OF SUCH DAMAGE.

               This version of this MIB module is part of RFC 5643;
               see the RFC itself for full legal notices."

          REVISION "200908130000Z"
          DESCRIPTION
              "Initial version, published as RFC 5643"
          ::= { mib-2 191 }

 -- Textual conventions

 Ospfv3UpToRefreshIntervalTC ::= TEXTUAL-CONVENTION
          DISPLAY-HINT "d"
          STATUS        current
          DESCRIPTION
               "The values one might be able to configure for
               variables bounded by the Refresh Interval."
          REFERENCE
               "OSPF Version 2, Appendix B, Architectural Constants"
          SYNTAX      Unsigned32 (1..1800)

 Ospfv3DeadIntervalRangeTC ::= TEXTUAL-CONVENTION
          DISPLAY-HINT "d"
          STATUS        current
          DESCRIPTION
               "The range, in seconds, of dead interval value."
          REFERENCE
               "OSPF for IPv6, Appendix C.3, Router Interface
               Parameters"
          SYNTAX      Unsigned32 (1..'FFFF'h)

 Ospfv3RouterIdTC ::= TEXTUAL-CONVENTION
          DISPLAY-HINT "d"
          STATUS      current
          DESCRIPTION
               "A 32-bit, unsigned integer uniquely identifying the
               router in the Autonomous System.  To ensure
               uniqueness, this may default to the value of one of
               the router's IPv4 host addresses if IPv4 is
               configured on the router."
          REFERENCE
               "OSPF for IPv6, Appendix C.1, Global Parameters"
          SYNTAX      Unsigned32 (1..'FFFFFFFF'h)

 Ospfv3LsIdTC ::= TEXTUAL-CONVENTION
          DISPLAY-HINT "d"
          STATUS      current
          DESCRIPTION
               "A unique 32-bit identifier of the piece of the
               routing domain that is being described by a link
               state advertisement.  In contrast to OSPFv2, the
               Link State ID (LSID) has no addressing semantics."
          REFERENCE
               "OSPF Version 2, Section 12.1.4, Link State ID"
          SYNTAX      Unsigned32 (1..'FFFFFFFF'h)

 Ospfv3AreaIdTC ::= TEXTUAL-CONVENTION

          DISPLAY-HINT "d"
          STATUS      current
          DESCRIPTION
               "An OSPFv3 Area Identifier.  A value of zero
               identifies the backbone area."
          REFERENCE
               "OSPF for IPv6, Appendix C.3 Router Interface
               Parameters"
          SYNTAX      Unsigned32 (0..'FFFFFFFF'h)

 Ospfv3IfInstIdTC ::= TEXTUAL-CONVENTION
          DISPLAY-HINT "d"
          STATUS      current
          DESCRIPTION
               "An OSPFv3 Interface Instance ID."
          REFERENCE
               "OSPF for IPv6, Appendix C.3, Router Interface
               Parameters"
          SYNTAX      Unsigned32 (0..255)

 Ospfv3LsaSequenceTC ::= TEXTUAL-CONVENTION
          DISPLAY-HINT "d"
          STATUS      current
          DESCRIPTION
             "The sequence number field is a signed 32-bit
             integer.  It is used to detect old and duplicate
             link state advertisements.  The space of
             sequence numbers is linearly ordered.  The
             larger the sequence number, the more recent the
             advertisement."
          REFERENCE
             "OSPF Version 2, Section 12.1.6, LS sequence
             number"
          SYNTAX      Integer32

 Ospfv3LsaAgeTC ::= TEXTUAL-CONVENTION
          DISPLAY-HINT "d"
          STATUS      current
          DESCRIPTION
             "The age of the link state advertisement in
             seconds.  The high-order bit of the LS age
             field is considered the DoNotAge bit for
             support of on-demand circuits."
          REFERENCE
             "OSPF Version 2, Section 12.1.1, LS age;
              Extending OSPF to Support Demand Circuits,
              Section 2.2, The LS age field"
          SYNTAX      Unsigned32 (0..3600 | 32768..36368)

 -- Top-level structure of MIB
 ospfv3Notifications  OBJECT IDENTIFIER ::= { ospfv3MIB 0 }
 ospfv3Objects        OBJECT IDENTIFIER ::= { ospfv3MIB 1 }
 ospfv3Conformance    OBJECT IDENTIFIER ::= { ospfv3MIB 2 }

 -- OSPFv3 General Variables

 -- These parameters apply globally to the Router's
 -- OSPFv3 Process.

 ospfv3GeneralGroup OBJECT IDENTIFIER ::= { ospfv3Objects 1 }

 ospfv3RouterId OBJECT-TYPE
         SYNTAX         Ospfv3RouterIdTC
         MAX-ACCESS     read-write
         STATUS         current
         DESCRIPTION
             "A 32-bit unsigned integer uniquely identifying
             the router in the Autonomous System.  To ensure
             uniqueness, this may default to the 32-bit
             unsigned integer representation of one of
             the router's IPv4 interface addresses (if IPv4
             is configured on the router).

             This object is persistent, and when written, the
             entity SHOULD save the change to non-volatile
             storage."
         REFERENCE
               "OSPF for IPv6, Appendix C.1, Global Parameters"
         ::= { ospfv3GeneralGroup 1 }

 ospfv3AdminStatus OBJECT-TYPE
         SYNTAX          Status
         MAX-ACCESS      read-write
         STATUS          current
         DESCRIPTION
             "The administrative status of OSPFv3 in the
             router.  The value 'enabled' denotes that the
             OSPFv3 Process is active on at least one
             interface; 'disabled' disables it on all
             interfaces.

             This object is persistent, and when written, the
             entity SHOULD save the change to non-volatile
             storage."
         ::= { ospfv3GeneralGroup 2 }

 ospfv3VersionNumber OBJECT-TYPE
         SYNTAX          INTEGER { version3 (3) }
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The version number of OSPF for IPv6 is 3."
         ::= { ospfv3GeneralGroup 3 }

 ospfv3AreaBdrRtrStatus OBJECT-TYPE
         SYNTAX          TruthValue
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "A flag to denote whether this router is an area
             border router.  The value of this object is true (1)
             when the router is an area border router."
         REFERENCE
             "OSPF Version 2, Section 3, Splitting the AS into
             Areas"
         ::= { ospfv3GeneralGroup 4 }

 ospfv3ASBdrRtrStatus OBJECT-TYPE
         SYNTAX          TruthValue
         MAX-ACCESS      read-write
         STATUS          current
         DESCRIPTION
             "A flag to note whether this router is
             configured as an Autonomous System border router.

             This object is persistent, and when written, the
             entity SHOULD save the change to non-volatile
             storage."
         REFERENCE
             "OSPF Version 2, Section 3.3, Classification of
             routers"
         ::= { ospfv3GeneralGroup 5 }

 ospfv3AsScopeLsaCount OBJECT-TYPE
         SYNTAX          Gauge32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The number of AS-scope (e.g., AS-External) link state
             advertisements in the link state database."
         ::= { ospfv3GeneralGroup 6 }

 ospfv3AsScopeLsaCksumSum OBJECT-TYPE
         SYNTAX          Unsigned32

         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The 32-bit unsigned sum of the LS checksums of
             the AS-scoped link state advertisements
             contained in the link state database.  This sum
             can be used to determine if there has been a
             change in a router's link state database or
             to compare the link state database of two
             routers."
         ::= { ospfv3GeneralGroup 7 }

 ospfv3OriginateNewLsas OBJECT-TYPE
         SYNTAX          Counter32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The number of new link state advertisements
             that have been originated.  This number is
             incremented each time the router originates a new
             LSA.

             Discontinuities in the value of this counter
             can occur at re-initialization of the management
             system and at other times as indicated by the
             value of ospfv3DiscontinuityTime."
         ::= { ospfv3GeneralGroup 8 }

 ospfv3RxNewLsas OBJECT-TYPE
         SYNTAX          Counter32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The number of link state advertisements
             received that are determined to be new
             instantiations.  This number does not include
             newer instantiations of self-originated link state
             advertisements.

             Discontinuities in the value of this counter
             can occur at re-initialization of the management
             system and at other times as indicated by the
             value of ospfv3DiscontinuityTime."
         ::= { ospfv3GeneralGroup 9 }

 ospfv3ExtLsaCount OBJECT-TYPE
         SYNTAX          Gauge32
         MAX-ACCESS      read-only

         STATUS          current
         DESCRIPTION
              "The number of External (LS type 0x4005) in the
              link state database."
         ::= { ospfv3GeneralGroup 10 }

 ospfv3ExtAreaLsdbLimit OBJECT-TYPE
         SYNTAX          Integer32 (-1..'7FFFFFFF'h)
         MAX-ACCESS      read-write
         STATUS          current
         DESCRIPTION
             "The maximum number of non-default
             AS-external-LSA entries that can be stored in the
             link state database.  If the value is -1, then
             there is no limit.

             When the number of non-default AS-external-LSAs
             in a router's link state database reaches
             ospfv3ExtAreaLsdbLimit, the router enters Overflow
             state.  The router never holds more than
             ospfv3ExtAreaLsdbLimit non-default AS-external-LSAs
             in its database.  ospfv3ExtAreaLsdbLimit MUST be set
             identically in all routers attached to the OSPFv3
             backbone and/or any regular OSPFv3 area (i.e.,
             OSPFv3 stub areas and not-so-stubby-areas (NSSAs)
             are excluded).

             This object is persistent, and when written, the
             entity SHOULD save the change to non-volatile
             storage."
         ::= { ospfv3GeneralGroup 11 }

 ospfv3ExitOverflowInterval OBJECT-TYPE
         SYNTAX          Unsigned32
         UNITS           "seconds"
         MAX-ACCESS      read-write
         STATUS          current
         DESCRIPTION
             "The number of seconds that, after entering
             Overflow state, a router will attempt to leave
             Overflow state.  This allows the router to again
             originate non-default, AS-External-LSAs.  When
             set to 0, the router will not leave Overflow
             state until restarted.

             This object is persistent, and when written, the
             entity SHOULD save the change to non-volatile
             storage."

         ::= { ospfv3GeneralGroup 12 }

 ospfv3DemandExtensions OBJECT-TYPE
         SYNTAX         TruthValue
         MAX-ACCESS     read-write
         STATUS         current
         DESCRIPTION
             "The router's support for demand circuits.
             The value of this object is true (1) when
             demand circuits are supported.

             This object is persistent, and when written, the
             entity SHOULD save the change to non-volatile
             storage."
         REFERENCE
             "OSPF Version 2; Extending OSPF to Support Demand
             Circuits"
         ::= { ospfv3GeneralGroup 13 }

 ospfv3ReferenceBandwidth OBJECT-TYPE
        SYNTAX       Unsigned32
        UNITS        "kilobits per second"
        MAX-ACCESS   read-write
        STATUS       current
        DESCRIPTION
            "Reference bandwidth in kilobits per second for
            calculating default interface metrics.  The
            default value is 100,000 KBPS (100 MBPS).

            This object is persistent, and when written, the
            entity SHOULD save the change to non-volatile
            storage."
        REFERENCE
            "OSPF Version 2, Appendix C.3, Router interface
            parameters"
        DEFVAL { 100000 }
     ::= { ospfv3GeneralGroup 14 }

 ospfv3RestartSupport OBJECT-TYPE
        SYNTAX       INTEGER { none(1),
                               plannedOnly(2),
                               plannedAndUnplanned(3)
                          }
        MAX-ACCESS   read-write
        STATUS       current
        DESCRIPTION
            "The router's support for OSPF graceful restart.
            Options include no restart support, only planned

            restarts, or both planned and unplanned restarts.

            This object is persistent, and when written, the
            entity SHOULD save the change to non-volatile
            storage."
        REFERENCE "Graceful OSPF Restart, Appendix B.1, Global
                     Parameters (Minimum subset)"
        ::= { ospfv3GeneralGroup 15 }

 ospfv3RestartInterval OBJECT-TYPE
        SYNTAX       Ospfv3UpToRefreshIntervalTC
        UNITS        "seconds"
        MAX-ACCESS   read-write
        STATUS       current
        DESCRIPTION
            "Configured OSPF graceful restart timeout interval.

            This object is persistent, and when written, the
            entity SHOULD save the change to non-volatile
            storage."
        REFERENCE "Graceful OSPF Restart, Appendix B.1, Global
                  Parameters (Minimum subset)"
        DEFVAL { 120 }
        ::= { ospfv3GeneralGroup 16 }

 ospfv3RestartStrictLsaChecking OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
          "Indicates if strict LSA checking is enabled for
          graceful restart.  A value of true (1) indicates that
          strict LSA checking is enabled.

          This object is persistent, and when written,
          the entity SHOULD save the change to non-volatile
          storage."
       REFERENCE "Graceful OSPF Restart, Appendix B.2, Global
                 Parameters (Optional)"
       DEFVAL { true }
       ::= { ospfv3GeneralGroup 17 }

 ospfv3RestartStatus OBJECT-TYPE
        SYNTAX       INTEGER { notRestarting(1),
                               plannedRestart(2),
                               unplannedRestart(3)
                             }
        MAX-ACCESS   read-only

        STATUS       current
        DESCRIPTION
           "The current status of OSPF graceful restart capability."
        ::= { ospfv3GeneralGroup 18 }

 ospfv3RestartAge OBJECT-TYPE
        SYNTAX       Ospfv3UpToRefreshIntervalTC
        UNITS        "seconds"
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
           "Remaining time in the current OSPF graceful restart
           interval."
        ::= { ospfv3GeneralGroup 19 }

 ospfv3RestartExitReason OBJECT-TYPE
        SYNTAX       INTEGER { none(1),
                               inProgress(2),
                               completed(3),
                               timedOut(4),
                               topologyChanged(5)
                             }
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
           "Describes the outcome of the last attempt at a
           graceful restart.

           none:            no restart has yet been attempted.
           inProgress:      a restart attempt is currently underway.
           completed:       the last restart completed successfully.
           timedOut:        the last restart timed out.
           topologyChanged: the last restart was aborted due to
                            a topology change."
     ::= { ospfv3GeneralGroup 20 }

 ospfv3NotificationEnable OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This object provides a coarse level of control
             over the generation of OSPFv3 notifications.

             If this object is set to true (1), then it enables
             the generation of OSPFv3 notifications.  If it is
             set to false (2), these notifications are not
             generated.

             This object is persistent, and when written, the
             entity SHOULD save the change to non-volatile
             storage."
    ::= { ospfv3GeneralGroup 21 }

ospfv3StubRouterSupport OBJECT-TYPE
     SYNTAX       TruthValue
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION
         "The router's support for stub router functionality.  An
         object value of true (1) indicates that stub router
         functionality is supported."
     REFERENCE
         "OSPF Stub Router Advertisement"
     ::= { ospfv3GeneralGroup 22 }

 ospfv3StubRouterAdvertisement OBJECT-TYPE
     SYNTAX       INTEGER {
                        doNotAdvertise(1),
                        advertise(2)
                        }
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
         "This object controls the advertisement of
         stub LSAs by the router.  The value
         doNotAdvertise (1) will result in the advertisement
         of standard LSAs and is the default value.

         This object is persistent, and when written,
         the entity SHOULD save the change to non-volatile
         storage."
     REFERENCE
         "OSPF Stub Router Advertisement, Section 2, Proposed
         Solution"
     DEFVAL { doNotAdvertise }
     ::= { ospfv3GeneralGroup 23 }

ospfv3DiscontinuityTime OBJECT-TYPE
    SYNTAX     TimeStamp
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The value of sysUpTime on the most recent occasion
        at which any one of this MIB's counters suffered
        a discontinuity.

        If no such discontinuities have occurred since the last
        re-initialization of the local management subsystem,
        then this object contains a zero value."
    ::= { ospfv3GeneralGroup 24 }

  ospfv3RestartTime OBJECT-TYPE
      SYNTAX     TimeStamp
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
         "The value of sysUpTime on the most recent occasion
          at which the ospfv3RestartExitReason was updated."
      ::= { ospfv3GeneralGroup 25 }

 -- The OSPFv3 Area Data Structure contains information
 -- regarding the various areas.  The interfaces and
 -- virtual links are configured as part of these areas.
 -- Area 0, by definition, is the backbone area.

 ospfv3AreaTable OBJECT-TYPE
         SYNTAX          SEQUENCE OF Ospfv3AreaEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "Information describing the configured
             parameters and cumulative statistics of the router's
             attached areas.  The interfaces and
             virtual links are configured as part of these areas.
             Area 0, by definition, is the backbone area."
         REFERENCE
             "OSPF Version 2, Section 6, The Area Data
             Structure"
         ::= { ospfv3Objects 2 }

 ospfv3AreaEntry OBJECT-TYPE
         SYNTAX          Ospfv3AreaEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "Information describing the configured
             parameters and cumulative statistics of one of the
             router's attached areas.

             The information in this table is persistent,
             and when written, the entity SHOULD save the a
             change to non-volatile storage."
         INDEX           { ospfv3AreaId }
         ::= { ospfv3AreaTable 1 }

 Ospfv3AreaEntry ::= SEQUENCE {
         ospfv3AreaId
                 Ospfv3AreaIdTC,
         ospfv3AreaImportAsExtern
                 INTEGER,
         ospfv3AreaSpfRuns
                 Counter32,
         ospfv3AreaBdrRtrCount
                 Gauge32,
         ospfv3AreaAsBdrRtrCount
                 Gauge32,
         ospfv3AreaScopeLsaCount
                 Gauge32,
         ospfv3AreaScopeLsaCksumSum
                 Unsigned32,
         ospfv3AreaSummary
                 INTEGER,
         ospfv3AreaRowStatus
                 RowStatus,
         ospfv3AreaStubMetric
                 BigMetric,
         ospfv3AreaNssaTranslatorRole
                 INTEGER,
         ospfv3AreaNssaTranslatorState
                 INTEGER,
         ospfv3AreaNssaTranslatorStabInterval
                 Unsigned32,
         ospfv3AreaNssaTranslatorEvents
                 Counter32,
         ospfv3AreaStubMetricType
                 INTEGER,
         ospfv3AreaTEEnabled
                 TruthValue
         }

 ospfv3AreaId OBJECT-TYPE
         SYNTAX          Ospfv3AreaIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "A 32-bit unsigned integer uniquely identifying an area.
             Area ID 0 is used for the OSPFv3 backbone."
         REFERENCE
             "OSPF Version 2, Appendix C.2, Area parameters"
         ::= { ospfv3AreaEntry 1 }

 ospfv3AreaImportAsExtern OBJECT-TYPE
         SYNTAX          INTEGER {
                         importExternal(1),   -- normal area
                         importNoExternal(2), -- stub area
                         importNssa(3)        -- not-so-stubby-area
                         }
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "Indicates whether an area is a stub area, NSSA, or
             standard area.  AS-scope LSAs are not imported into stub
             areas or NSSAs.  NSSAs import AS-External data as NSSA
             LSAs that have Area-scope."
         REFERENCE
             "OSPF Version 2, Appendix C.2, Area parameters"
         DEFVAL { importExternal }
         ::= { ospfv3AreaEntry 2 }

 ospfv3AreaSpfRuns OBJECT-TYPE
         SYNTAX          Counter32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The number of times that the intra-area route
             table has been calculated using this area's
             link state database.  This is typically done
             using Dijkstra's algorithm.

             Discontinuities in the value of this counter
             can occur at re-initialization of the management
             system and at other times as indicated by the
             value of ospfv3DiscontinuityTime."
         ::= { ospfv3AreaEntry 3 }

 ospfv3AreaBdrRtrCount OBJECT-TYPE
         SYNTAX          Gauge32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The total number of area border routers
             reachable within this area.  This is initially zero,
             and is calculated in each Shortest Path First (SPF)
             pass."
         DEFVAL { 0 }
         ::= { ospfv3AreaEntry 4 }

 ospfv3AreaAsBdrRtrCount OBJECT-TYPE
         SYNTAX          Gauge32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The total number of Autonomous System border
             routers reachable within this area.  This is
             initially zero, and is calculated in each SPF
             pass."
         DEFVAL { 0 }
         ::= { ospfv3AreaEntry 5 }

 ospfv3AreaScopeLsaCount OBJECT-TYPE
         SYNTAX          Gauge32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The total number of Area-scope link state
             advertisements in this area's link state
             database."
          DEFVAL { 0 }
         ::= { ospfv3AreaEntry 6 }

 ospfv3AreaScopeLsaCksumSum OBJECT-TYPE
         SYNTAX          Unsigned32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The 32-bit unsigned sum of the Area-scope link state
             advertisements' LS checksums contained in this
             area's link state database.  The sum can be used
             to determine if there has been a change in a
             router's link state database or to compare the
             link state database of two routers."
         ::= { ospfv3AreaEntry 7 }

 ospfv3AreaSummary OBJECT-TYPE
         SYNTAX          INTEGER {
                         noAreaSummary(1),
                         sendAreaSummary(2)
                         }
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The variable ospfv3AreaSummary controls the
             import of Inter-Area LSAs into stub and
             NSSA areas.  It has no effect on other areas.

             If it is noAreaSummary, the router will neither
             originate nor propagate Inter-Area LSAs into the
             stub or NSSA area.  It will only advertise a
             default route.

             If it is sendAreaSummary, the router will both
             summarize and propagate Inter-Area LSAs."
         DEFVAL   { sendAreaSummary }
         ::= { ospfv3AreaEntry 8 }

 ospfv3AreaRowStatus OBJECT-TYPE
         SYNTAX          RowStatus
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "This object permits management of the table by
             facilitating actions such as row creation,
             construction, and destruction.

             The value of this object has no effect on
             whether other objects in this conceptual row can be
             modified."
         ::= { ospfv3AreaEntry 9 }

 ospfv3AreaStubMetric OBJECT-TYPE
         SYNTAX          BigMetric
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The metric value advertised for the default route
             into stub and NSSA areas.  By default, this equals the
             least metric among the interfaces to other areas."
         ::= { ospfv3AreaEntry 10 }

 ospfv3AreaNssaTranslatorRole OBJECT-TYPE
         SYNTAX          INTEGER { always(1), candidate(2) }
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "Indicates an NSSA border router's policy to
             perform NSSA translation of NSSA-LSAs into
             AS-External-LSAs."
         DEFVAL { candidate }
         ::= { ospfv3AreaEntry 11 }

 ospfv3AreaNssaTranslatorState OBJECT-TYPE
         SYNTAX          INTEGER {
                         enabled(1),

                         elected(2),
                         disabled(3)
                         }
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
              "Indicates if and how an NSSA border router is
              performing NSSA translation of NSSA-LSAs into
              AS-External-LSAs.  When this object is set to
              'enabled', the NSSA border router's
              ospfv3AreaNssaTranslatorRole has been set to 'always'.
              When this object is set to 'elected', a candidate
              NSSA border router is translating NSSA-LSAs into
              AS-External-LSAs.  When this object is set to
              'disabled', a candidate NSSA Border router is NOT
              translating NSSA-LSAs into AS-External-LSAs."
         ::= { ospfv3AreaEntry 12 }

 ospfv3AreaNssaTranslatorStabInterval OBJECT-TYPE
         SYNTAX          Unsigned32
         UNITS           "seconds"
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The stability interval defined as the number of
             seconds after an elected translator determines its
             services are no longer required that it should
             continue to perform its translation duties."
         DEFVAL { 40 }
         ::= { ospfv3AreaEntry 13 }

 ospfv3AreaNssaTranslatorEvents OBJECT-TYPE
         SYNTAX          Counter32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "Indicates the number of Translator state changes
             that have occurred since the last start-up of the
             OSPFv3 routing process.

             Discontinuities in the value of this counter
             can occur at re-initialization of the management
             system and at other times as indicated by the
             value of ospfv3DiscontinuityTime."
         ::= { ospfv3AreaEntry 14 }

 ospfv3AreaStubMetricType OBJECT-TYPE
         SYNTAX       INTEGER {
                         ospfv3Metric(1),   -- OSPF Metric
                         comparableCost(2), -- external type 1
                         nonComparable(3)   -- external type 2
                         }
         MAX-ACCESS   read-create
         STATUS       current
         DESCRIPTION
             "This variable assigns the type of metric
             advertised as a default route."
         DEFVAL { ospfv3Metric }
         ::= { ospfv3AreaEntry 15 }

 ospfv3AreaTEEnabled OBJECT-TYPE
         SYNTAX          TruthValue
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
                "Indicates whether or not traffic engineering
                is enabled in the area.  The object is set
                to the value true (1) to enable traffic engineering.
                Traffic engineering is disabled by default."
         DEFVAL { false }
         ::= { ospfv3AreaEntry 16 }

 -- OSPFv3 AS-Scope Link State Database

 ospfv3AsLsdbTable OBJECT-TYPE
         SYNTAX          SEQUENCE OF Ospfv3AsLsdbEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The OSPFv3 Process's AS-scope link state database
             (LSDB).  The LSDB contains the AS-scope link state
             advertisements from throughout the areas that the
             device is attached to."
         ::= { ospfv3Objects 3 }

 ospfv3AsLsdbEntry OBJECT-TYPE
         SYNTAX          Ospfv3AsLsdbEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "A single AS-scope link state advertisement."
         INDEX           { ospfv3AsLsdbType,
                           ospfv3AsLsdbRouterId,
                           ospfv3AsLsdbLsid }

         ::= { ospfv3AsLsdbTable 1 }

 Ospfv3AsLsdbEntry ::= SEQUENCE {
         ospfv3AsLsdbType
                 Unsigned32,
         ospfv3AsLsdbRouterId
                 Ospfv3RouterIdTC,
         ospfv3AsLsdbLsid
                 Ospfv3LsIdTC,
         ospfv3AsLsdbSequence
                 Ospfv3LsaSequenceTC,
         ospfv3AsLsdbAge
                 Ospfv3LsaAgeTC,
         ospfv3AsLsdbChecksum
                 Integer32,
         ospfv3AsLsdbAdvertisement
                 OCTET STRING,
         ospfv3AsLsdbTypeKnown
                 TruthValue
         }

 ospfv3AsLsdbType OBJECT-TYPE
         SYNTAX          Unsigned32(0..'FFFFFFFF'h)
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The type of the link state advertisement.
             Each link state type has a separate
             advertisement format.  AS-scope LSAs not recognized
             by the router may be stored in the database."
         ::= { ospfv3AsLsdbEntry 1 }

 ospfv3AsLsdbRouterId OBJECT-TYPE
         SYNTAX          Ospfv3RouterIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The 32-bit number that uniquely identifies the
             originating router in the Autonomous System."
         REFERENCE
             "OSPF Version 2, Appendix C.1, Global parameters"
         ::= { ospfv3AsLsdbEntry 2 }

 ospfv3AsLsdbLsid OBJECT-TYPE
         SYNTAX          Ospfv3LsIdTC
         MAX-ACCESS      not-accessible
         STATUS          current

         DESCRIPTION
             "The Link State ID is an LS type-specific field
             containing a unique identifier;
             it identifies the piece of the routing domain
             that is being described by the advertisement.
             In contrast to OSPFv2, the LSID has no
             addressing semantics."
         ::= { ospfv3AsLsdbEntry 3 }

 -- Note that the OSPF sequence number is a 32-bit signed
 -- integer.  It starts with the value '80000001'h
 -- or -'7FFFFFFF'h, and increments until '7FFFFFFF'h.
 -- Thus, a typical sequence number will be very negative.

 ospfv3AsLsdbSequence OBJECT-TYPE
         SYNTAX          Ospfv3LsaSequenceTC
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The sequence number field is a signed 32-bit
             integer.  It is used to detect old and duplicate
             link state advertisements.  The space of
             sequence numbers is linearly ordered.  The
             larger the sequence number, the more recent the
             advertisement."
         REFERENCE
             "OSPF Version 2, Section 12.1.6, LS sequence
             number"
         ::= { ospfv3AsLsdbEntry 4 }

 ospfv3AsLsdbAge OBJECT-TYPE
         SYNTAX          Ospfv3LsaAgeTC
         UNITS           "seconds"
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "This field is the age of the link state
             advertisement in seconds.  The high-order bit
             of the LS age field is considered the DoNotAge
             bit for support of on-demand circuits."
         REFERENCE
             "OSPF Version 2, Section 12.1.1, LS age;
              Extending OSPF to Support Demand Circuits,
              Section 2.2, The LS age field."
         ::= { ospfv3AsLsdbEntry 5 }

 ospfv3AsLsdbChecksum OBJECT-TYPE
         SYNTAX          Integer32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "This field is the checksum of the complete
             contents of the advertisement, excepting the
             age field.  The age field is excepted so that
             an advertisement's age can be incremented
             without updating the checksum.  The checksum
             used is the same that is used for ISO
             connectionless datagrams; it is commonly
             referred to as the Fletcher checksum."
         REFERENCE
             "OSPF Version 2, Section 12.1.7, LS checksum"
         ::= { ospfv3AsLsdbEntry 6 }

 ospfv3AsLsdbAdvertisement OBJECT-TYPE
         SYNTAX          OCTET STRING (SIZE (1..65535))
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The entire link state advertisement, including
             its header."
         ::= { ospfv3AsLsdbEntry 7 }

 ospfv3AsLsdbTypeKnown OBJECT-TYPE
         SYNTAX          TruthValue
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The value true (1) indicates that the LSA type
             is recognized by this router."
         ::= { ospfv3AsLsdbEntry 8 }

  --  OSPFv3 Area-Scope Link State Database

 ospfv3AreaLsdbTable OBJECT-TYPE
         SYNTAX          SEQUENCE OF Ospfv3AreaLsdbEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The OSPFv3 Process's Area-scope LSDB.
             The LSDB contains the Area-scope link state
             advertisements from throughout the area that the
             device is attached to."
         ::= { ospfv3Objects 4 }

 ospfv3AreaLsdbEntry OBJECT-TYPE
         SYNTAX          Ospfv3AreaLsdbEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "A single Area-scope link state advertisement."
         INDEX           { ospfv3AreaLsdbAreaId,
                           ospfv3AreaLsdbType,
                           ospfv3AreaLsdbRouterId,
                           ospfv3AreaLsdbLsid }
         ::= { ospfv3AreaLsdbTable 1 }

 Ospfv3AreaLsdbEntry ::= SEQUENCE {
         ospfv3AreaLsdbAreaId
                 Ospfv3AreaIdTC,
         ospfv3AreaLsdbType
                 Unsigned32,
         ospfv3AreaLsdbRouterId
                 Ospfv3RouterIdTC,
         ospfv3AreaLsdbLsid
                 Ospfv3LsIdTC,
         ospfv3AreaLsdbSequence
                 Ospfv3LsaSequenceTC,
         ospfv3AreaLsdbAge
                 Ospfv3LsaAgeTC,
         ospfv3AreaLsdbChecksum
                 Integer32,
         ospfv3AreaLsdbAdvertisement
                 OCTET STRING,
         ospfv3AreaLsdbTypeKnown
                 TruthValue
         }

 ospfv3AreaLsdbAreaId OBJECT-TYPE
         SYNTAX          Ospfv3AreaIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The 32-bit identifier of the Area from which the
             LSA was received."
         REFERENCE
             "OSPF Version 2, Appendix C.2, Area parameters"
         ::= { ospfv3AreaLsdbEntry 1 }

 ospfv3AreaLsdbType OBJECT-TYPE
         SYNTAX          Unsigned32(0..'FFFFFFFF'h)
         MAX-ACCESS      not-accessible
         STATUS          current

         DESCRIPTION
             "The type of the link state advertisement.
             Each link state type has a separate
             advertisement format.  Area-scope LSAs unrecognized
             by the router are also stored in this database."
         ::= { ospfv3AreaLsdbEntry 2 }

 ospfv3AreaLsdbRouterId OBJECT-TYPE
         SYNTAX          Ospfv3RouterIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The 32-bit number that uniquely identifies the
             originating router in the Autonomous System."
         REFERENCE
             "OSPF Version 2, Appendix C.1, Global parameters"
         ::= { ospfv3AreaLsdbEntry 3 }

 ospfv3AreaLsdbLsid OBJECT-TYPE
         SYNTAX          Ospfv3LsIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The Link State ID is an LS type-specific field
             containing a unique identifier;
             it identifies the piece of the routing domain
             that is being described by the advertisement.
             In contrast to OSPFv2, the LSID has no
             addressing semantics."
         ::= { ospfv3AreaLsdbEntry 4 }

 -- Note that the OSPF sequence number is a 32-bit signed
 -- integer.  It starts with the value '80000001'h
 -- or -'7FFFFFFF'h, and increments until '7FFFFFFF'h.
 -- Thus, a typical sequence number will be very negative.

 ospfv3AreaLsdbSequence OBJECT-TYPE
         SYNTAX          Ospfv3LsaSequenceTC
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The sequence number field is a signed 32-bit
             integer.  It is used to detect old and
             duplicate link state advertisements.  The space
             of sequence numbers is linearly ordered.  The
             larger the sequence number, the more recent the
             advertisement."

         REFERENCE
             "OSPF Version 2, Section 12.1.6, LS sequence
             number"
         ::= { ospfv3AreaLsdbEntry 5 }

 ospfv3AreaLsdbAge OBJECT-TYPE
         SYNTAX          Ospfv3LsaAgeTC
         UNITS           "seconds"
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "This field is the age of the link state
             advertisement in seconds.  The high-order bit
             of the LS age field is considered the DoNotAge
             bit for support of on-demand circuits."
         REFERENCE
             "OSPF Version 2, Section 12.1.1, LS age;
              Extending OSPF to Support Demand Circuits,
              Section 2.2, The LS age field."
         ::= { ospfv3AreaLsdbEntry 6 }

 ospfv3AreaLsdbChecksum OBJECT-TYPE
         SYNTAX          Integer32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "This field is the checksum of the complete
             contents of the advertisement, excepting the
             age field.  The age field is excepted so that
             an advertisement's age can be incremented
             without updating the checksum.  The checksum
             used is the same that is used for ISO
             connectionless datagrams; it is commonly
             referred to as the Fletcher checksum."
         REFERENCE
             "OSPF Version 2, Section 12.1.7, LS checksum"
         ::= { ospfv3AreaLsdbEntry 7 }

 ospfv3AreaLsdbAdvertisement OBJECT-TYPE
         SYNTAX          OCTET STRING (SIZE (1..65535))
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The entire link state advertisement, including
             its header."
         ::= { ospfv3AreaLsdbEntry 8 }

 ospfv3AreaLsdbTypeKnown OBJECT-TYPE
         SYNTAX          TruthValue
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The value true (1) indicates that the LSA type is
             recognized by this router."
         ::= { ospfv3AreaLsdbEntry 9 }

 -- OSPFv3 Link-Scope Link State Database, for non-virtual interfaces

 ospfv3LinkLsdbTable OBJECT-TYPE
         SYNTAX          SEQUENCE OF Ospfv3LinkLsdbEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The OSPFv3 Process's Link-scope LSDB for non-virtual
             interfaces.  The LSDB contains the Link-scope link
             state advertisements from the interfaces that the
             device is attached to."
         ::= { ospfv3Objects 5 }

 ospfv3LinkLsdbEntry OBJECT-TYPE
         SYNTAX          Ospfv3LinkLsdbEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "A single Link-scope link state advertisement."
         INDEX           { ospfv3LinkLsdbIfIndex,
                           ospfv3LinkLsdbIfInstId,
                           ospfv3LinkLsdbType,
                           ospfv3LinkLsdbRouterId,
                           ospfv3LinkLsdbLsid }
         ::= { ospfv3LinkLsdbTable 1 }

 Ospfv3LinkLsdbEntry ::= SEQUENCE {
         ospfv3LinkLsdbIfIndex
                 InterfaceIndex,
         ospfv3LinkLsdbIfInstId
                 Ospfv3IfInstIdTC,
         ospfv3LinkLsdbType
                 Unsigned32,
         ospfv3LinkLsdbRouterId
                 Ospfv3RouterIdTC,
         ospfv3LinkLsdbLsid
                 Ospfv3LsIdTC,
         ospfv3LinkLsdbSequence
                 Ospfv3LsaSequenceTC,

         ospfv3LinkLsdbAge
                 Ospfv3LsaAgeTC,
         ospfv3LinkLsdbChecksum
                 Integer32,
         ospfv3LinkLsdbAdvertisement
                 OCTET STRING,
         ospfv3LinkLsdbTypeKnown
                 TruthValue
         }

 ospfv3LinkLsdbIfIndex OBJECT-TYPE
         SYNTAX         InterfaceIndex
         MAX-ACCESS     not-accessible
         STATUS         current
         DESCRIPTION
             "The identifier of the link from which the LSA
             was received."
         ::= { ospfv3LinkLsdbEntry 1 }

 ospfv3LinkLsdbIfInstId OBJECT-TYPE
         SYNTAX         Ospfv3IfInstIdTC
         MAX-ACCESS     not-accessible
         STATUS         current
         DESCRIPTION
             "The identifier of the interface instance from
             which the LSA was received."
         ::= { ospfv3LinkLsdbEntry 2 }

 ospfv3LinkLsdbType OBJECT-TYPE
         SYNTAX          Unsigned32(0..'FFFFFFFF'h)
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The type of the link state advertisement.
             Each link state type has a separate
             advertisement format.  Link-scope LSAs unrecognized
             by the router are also stored in this database."
         ::= { ospfv3LinkLsdbEntry 3 }

 ospfv3LinkLsdbRouterId OBJECT-TYPE
         SYNTAX          Ospfv3RouterIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The 32-bit number that uniquely identifies the
             originating router in the Autonomous System."
         REFERENCE
             "OSPF Version 2, Appendix C.1, Global parameters"

         ::= { ospfv3LinkLsdbEntry 4 }

 ospfv3LinkLsdbLsid OBJECT-TYPE
         SYNTAX        Ospfv3LsIdTC
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "The Link State ID is an LS type-specific field
             containing a unique identifier;
             it identifies the piece of the routing domain
             that is being described by the advertisement.
             In contrast to OSPFv2, the LSID has no
             addressing semantics.  However, in OSPFv3
             the Link State ID always contains the flooding
             scope of the LSA."
         ::= { ospfv3LinkLsdbEntry 5 }

 -- Note that the OSPF sequence number is a 32-bit signed
 -- integer.  It starts with the value '80000001'h
 -- or -'7FFFFFFF'h, and increments until '7FFFFFFF'h.
 -- Thus, a typical sequence number will be very negative.

 ospfv3LinkLsdbSequence OBJECT-TYPE
         SYNTAX          Ospfv3LsaSequenceTC
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The sequence number field is a signed 32-bit
             integer.  It is used to detect old and duplicate
             link state advertisements.  The space of
             sequence numbers is linearly ordered.  The
             larger the sequence number, the more recent the
             advertisement."
         REFERENCE
             "OSPF Version 2, Section 12.1.6, LS sequence
             number"
         ::= { ospfv3LinkLsdbEntry 6 }

 ospfv3LinkLsdbAge OBJECT-TYPE
         SYNTAX          Ospfv3LsaAgeTC
         UNITS           "seconds"
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "This field is the age of the link state
             advertisement in seconds.  The high-order bit
             of the LS age field is considered the DoNotAge
             bit for support of on-demand circuits."

         REFERENCE
             "OSPF Version 2, Section 12.1.1, LS age;
              Extending OSPF to Support Demand Circuits,
              Section 2.2, The LS age field."
         ::= { ospfv3LinkLsdbEntry 7 }

 ospfv3LinkLsdbChecksum OBJECT-TYPE
         SYNTAX          Integer32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "This field is the checksum of the complete
             contents of the advertisement, excepting the
             age field.  The age field is excepted so that
             an advertisement's age can be incremented
             without updating the checksum.  The checksum
             used is the same that is used for ISO
             connectionless datagrams; it is commonly
             referred to as the Fletcher checksum."
         REFERENCE
             "OSPF Version 2, Section 12.1.7, LS checksum"
         ::= { ospfv3LinkLsdbEntry 8 }

 ospfv3LinkLsdbAdvertisement OBJECT-TYPE
         SYNTAX          OCTET STRING (SIZE (1..65535))
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The entire link state advertisement, including
             its header."
         ::= { ospfv3LinkLsdbEntry 9 }

 ospfv3LinkLsdbTypeKnown OBJECT-TYPE
         SYNTAX          TruthValue
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The value true (1) indicates that the LSA type is
             recognized by this router."
         ::= { ospfv3LinkLsdbEntry 10 }

 -- OSPF Host Table

 ospfv3HostTable OBJECT-TYPE
         SYNTAX          SEQUENCE OF Ospfv3HostEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION

             "The Host/Metric Table indicates what hosts are
             directly attached to the router and their
             corresponding metrics."
         REFERENCE
             "OSPF Version 2, Appendix C.7, Host route
             parameters"
         ::= { ospfv3Objects 6 }

 ospfv3HostEntry OBJECT-TYPE
         SYNTAX          Ospfv3HostEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "A metric to be advertised when a given host is
             reachable.

             The information in this table is persistent, and
             when written, the entity SHOULD save the change
             to non-volatile storage."
         INDEX           { ospfv3HostAddressType,
                           ospfv3HostAddress }
         ::= { ospfv3HostTable 1 }

 Ospfv3HostEntry ::= SEQUENCE {
         ospfv3HostAddressType
                 InetAddressType,
         ospfv3HostAddress
                 InetAddress,
         ospfv3HostMetric
                 Metric,
         ospfv3HostRowStatus
                 RowStatus,
         ospfv3HostAreaID
                 Ospfv3AreaIdTC
         }

 ospfv3HostAddressType OBJECT-TYPE
         SYNTAX          InetAddressType
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The address type of ospfv3HostAddress.  Only IPv6
             global address type is expected."
         REFERENCE
             "OSPF Version 2, Appendix C.7, Host route
             parameters"
         ::= { ospfv3HostEntry 1 }

 ospfv3HostAddress OBJECT-TYPE
         SYNTAX          InetAddress
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The IPv6 address of the host.  Must be an
             IPv6 global address."
         REFERENCE
             "OSPF Version 2, Appendix C.7, Host route
             parameters"
         ::= { ospfv3HostEntry 2 }

 ospfv3HostMetric OBJECT-TYPE
         SYNTAX          Metric
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The metric to be advertised."
         REFERENCE
             "OSPF Version 2, Appendix C.7, Host route
             parameters"
         ::= { ospfv3HostEntry 3 }

 ospfv3HostRowStatus OBJECT-TYPE
         SYNTAX          RowStatus
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "This object permits management of the table by
             facilitating actions such as row creation,
             construction, and destruction.

             The value of this object has no effect on
             whether other objects in this conceptual row can be
             modified."
         ::= { ospfv3HostEntry 4 }

 ospfv3HostAreaID OBJECT-TYPE
         SYNTAX          Ospfv3AreaIdTC
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The Area the host entry is to be found within.
             By default, the area for the subsuming OSPFv3
             interface, or Area 0 if there is no subsuming
             interface."
         REFERENCE
             "OSPF Version 2, Appendix C.2, Area parameters"

         ::= { ospfv3HostEntry 5 }

 -- OSPFv3 Interface Table

 ospfv3IfTable OBJECT-TYPE
         SYNTAX          SEQUENCE OF Ospfv3IfEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The OSPFv3 Interface Table describes the
             interfaces from the viewpoint of OSPFv3."
         REFERENCE
             "OSPF for IPv6, Appendix C.3, Router Interface
             Parameters"
         ::= { ospfv3Objects 7 }

 ospfv3IfEntry OBJECT-TYPE
         SYNTAX          Ospfv3IfEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The OSPFv3 Interface Entry describes one
             interface from the viewpoint of OSPFv3.

             The information in this table is persistent,
             and when written, the entity SHOULD save the
             change to non-volatile storage."
         INDEX           { ospfv3IfIndex,
                           ospfv3IfInstId }
         ::= { ospfv3IfTable 1 }

 Ospfv3IfEntry ::= SEQUENCE {
         ospfv3IfIndex
                 InterfaceIndex,
         ospfv3IfInstId
                 Ospfv3IfInstIdTC,
         ospfv3IfAreaId
                 Ospfv3AreaIdTC,
         ospfv3IfType
                 INTEGER,
         ospfv3IfAdminStatus
                 Status,
         ospfv3IfRtrPriority
                 DesignatedRouterPriority,
         ospfv3IfTransitDelay
                 Ospfv3UpToRefreshIntervalTC,
         ospfv3IfRetransInterval
                 Ospfv3UpToRefreshIntervalTC,

         ospfv3IfHelloInterval
                 HelloRange,
         ospfv3IfRtrDeadInterval
                  Ospfv3DeadIntervalRangeTC,
         ospfv3IfPollInterval
                 Unsigned32,
         ospfv3IfState
                 INTEGER,
         ospfv3IfDesignatedRouter
                 Ospfv3RouterIdTC,
         ospfv3IfBackupDesignatedRouter
                 Ospfv3RouterIdTC,
         ospfv3IfEvents
                 Counter32,
         ospfv3IfRowStatus
                 RowStatus,
         ospfv3IfDemand
                 TruthValue,
         ospfv3IfMetricValue
                 Metric,
         ospfv3IfLinkScopeLsaCount
                 Gauge32,
         ospfv3IfLinkLsaCksumSum
                 Unsigned32,
         ospfv3IfDemandNbrProbe
                 TruthValue,
         ospfv3IfDemandNbrProbeRetransLimit
                 Unsigned32,
         ospfv3IfDemandNbrProbeInterval
                 Unsigned32,
         ospfv3IfTEDisabled
                 TruthValue,
         ospfv3IfLinkLSASuppression
                 TruthValue
         }

 ospfv3IfIndex OBJECT-TYPE
         SYNTAX          InterfaceIndex
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The interface index of this OSPFv3 interface.
             It corresponds to the interface index of the
             IPv6 interface on which OSPFv3 is configured."
         ::= { ospfv3IfEntry 1 }

 ospfv3IfInstId OBJECT-TYPE
         SYNTAX          Ospfv3IfInstIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "Enables multiple interface instances of OSPFv3
             to be run over a single link.  Each interface
             instance would be assigned a separate ID.  This ID
             has local link significance only."
         ::= { ospfv3IfEntry 2 }

 ospfv3IfAreaId OBJECT-TYPE
         SYNTAX          Ospfv3AreaIdTC
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "A 32-bit integer uniquely identifying the area
             to which the interface connects.  Area ID
             0 is used for the OSPFv3 backbone."
         DEFVAL          { 0 }
         ::= { ospfv3IfEntry 3 }

 ospfv3IfType OBJECT-TYPE
         SYNTAX          INTEGER {
                         broadcast(1),
                         nbma(2),
                         pointToPoint(3),
                         pointToMultipoint(5)
                         }
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The OSPFv3 interface type."
         ::= { ospfv3IfEntry 4 }

 ospfv3IfAdminStatus OBJECT-TYPE
         SYNTAX          Status
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The OSPFv3 interface's administrative status.
             The value formed on the interface; the interface
             will be advertised as an internal route to some
             area.  The value 'disabled' denotes that the
             interface is external to OSPFv3.

             Note that a value of 'disabled' for the object
             ospfv3AdminStatus will override a value of
             'enabled' for the interface."
         DEFVAL          { enabled }
         ::= { ospfv3IfEntry 5 }

 ospfv3IfRtrPriority OBJECT-TYPE
         SYNTAX          DesignatedRouterPriority
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The priority of this interface.  Used in
             multi-access networks, this field is used in
             the designated-router election algorithm.  The
             value 0 signifies that the router is not
             eligible to become the Designated Router on this
             particular network.  In the event of a tie in
             this value, routers will use their Router ID as
             a tie breaker."
         DEFVAL          { 1 }
         ::= { ospfv3IfEntry 6 }

 ospfv3IfTransitDelay OBJECT-TYPE
         SYNTAX          Ospfv3UpToRefreshIntervalTC
         UNITS           "seconds"
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The estimated number of seconds it takes to transmit
             a Link State Update packet over this interface.  LSAs
             contained in the update packet must have their age
             incremented by this amount before transmission.  This
             value should take into account the transmission and
             propagation delays of the interface."
         REFERENCE
             "OSPF for IPv6, Appendix C.3, Router Interface
             Parameters."
         DEFVAL          { 1 }
         ::= { ospfv3IfEntry 7 }

 ospfv3IfRetransInterval OBJECT-TYPE
         SYNTAX          Ospfv3UpToRefreshIntervalTC
         UNITS           "seconds"
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The number of seconds between link state
             advertisement retransmissions for adjacencies

             belonging to this interface.  This value is
             also used when retransmitting database
             description and Link State Request packets."
         DEFVAL          { 5 }
         ::= { ospfv3IfEntry 8 }

 ospfv3IfHelloInterval OBJECT-TYPE
         SYNTAX          HelloRange
         UNITS           "seconds"
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The length of time, in seconds, between the
             Hello packets that the router sends on the
             interface.  This value must be the same for all
             routers attached to a common network."
         DEFVAL          { 10 }
         ::= { ospfv3IfEntry 9 }

 ospfv3IfRtrDeadInterval OBJECT-TYPE
         SYNTAX          Ospfv3DeadIntervalRangeTC
         UNITS           "seconds"
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The number of seconds that a router's Hello
             packets have not been seen before its
             neighbors declare the router down on the interface.
             This should be some multiple of the Hello interval.
             This value must be the same for all routers attached
             to a common network."
         DEFVAL          { 40 }
         ::= { ospfv3IfEntry 10 }

 ospfv3IfPollInterval OBJECT-TYPE
         SYNTAX          Unsigned32
         UNITS           "seconds"
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The larger time interval, in seconds, between
             the Hello packets sent to an inactive,
             non-broadcast multi-access neighbor."
         DEFVAL          { 120 }
         ::= { ospfv3IfEntry 11 }

 ospfv3IfState OBJECT-TYPE
         SYNTAX          INTEGER {
                         down(1),
                         loopback(2),
                         waiting(3),
                         pointToPoint(4),
                         designatedRouter(5),
                         backupDesignatedRouter(6),
                         otherDesignatedRouter(7),
                         standby(8)
                         }
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The OSPFv3 interface state.  An interface may be
             in standby state if there are multiple interfaces
             on the link and another interface is active.  The
             interface may be in Down state if the underlying
             IPv6 interface is down or if the admin status is
             'disabled' either globally or for the interface."
         ::= { ospfv3IfEntry 12 }

 ospfv3IfDesignatedRouter OBJECT-TYPE
         SYNTAX          Ospfv3RouterIdTC
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The Router ID of the Designated Router."
         ::= { ospfv3IfEntry 13 }

 ospfv3IfBackupDesignatedRouter OBJECT-TYPE
         SYNTAX          Ospfv3RouterIdTC
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The Router ID of the Backup Designated
             Router."
         ::= { ospfv3IfEntry 14 }

 ospfv3IfEvents OBJECT-TYPE
         SYNTAX          Counter32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The number of times this OSPFv3 interface has
             changed its state or an error has occurred.

             Discontinuities in the value of this counter
             can occur at re-initialization of the management
             system and at other times as indicated by the
             value of ospfv3DiscontinuityTime."
         ::= { ospfv3IfEntry 15 }

  ospfv3IfRowStatus OBJECT-TYPE
         SYNTAX          RowStatus
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "This object permits management of the table by
             facilitating actions such as row creation,
             construction, and destruction.

             The value of this object has no effect on
             whether other objects in this conceptual row can be
             modified."
         ::= { ospfv3IfEntry 16 }

 ospfv3IfDemand OBJECT-TYPE
         SYNTAX          TruthValue
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "Indicates whether Demand OSPFv3 procedures
             (Hello suppression to FULL neighbors and
             setting the DoNotAge flag on propagated LSAs)
             should be performed on this interface."
         DEFVAL { false }
         ::= { ospfv3IfEntry 17 }

 ospfv3IfMetricValue OBJECT-TYPE
         SYNTAX          Metric
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The metric assigned to this interface.
              The default value of the metric is
              'Reference Bandwidth / ifSpeed'.  The value
              of the reference bandwidth can be set
              in the ospfv3ReferenceBandwidth object."
         ::= { ospfv3IfEntry 18 }

  ospfv3IfLinkScopeLsaCount OBJECT-TYPE
         SYNTAX          Gauge32
         MAX-ACCESS      read-only
         STATUS          current

         DESCRIPTION
             "The total number of Link-scope link state
             advertisements in this link's link state
             database."
         ::= { ospfv3IfEntry 19 }

  ospfv3IfLinkLsaCksumSum OBJECT-TYPE
         SYNTAX          Unsigned32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The 32-bit unsigned sum of the Link-scope link state
             advertisements' LS checksums contained in this
             link's link state database.  The sum can be used
             to determine if there has been a change in a
             router's link state database or to compare the
             link state database of two routers."
         ::= { ospfv3IfEntry 20 }

 ospfv3IfDemandNbrProbe OBJECT-TYPE
         SYNTAX          TruthValue
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
                "Indicates whether or not neighbor probing is
                enabled to determine whether or not the neighbor
                is inactive.  Neighbor probing is disabled by
                default."
         DEFVAL { false }
         ::= { ospfv3IfEntry 21 }

ospfv3IfDemandNbrProbeRetransLimit OBJECT-TYPE
        SYNTAX       Unsigned32
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION
           "The number of consecutive LSA retransmissions before
           the neighbor is deemed inactive and the neighbor
           adjacency is brought down."
        DEFVAL          { 10 }
        ::= { ospfv3IfEntry 22}

ospfv3IfDemandNbrProbeInterval OBJECT-TYPE
        SYNTAX       Unsigned32
        UNITS        "seconds"
        MAX-ACCESS   read-create
        STATUS       current

        DESCRIPTION
           "Defines how often the neighbor will be probed."
        DEFVAL          { 120 }
        ::= { ospfv3IfEntry 23 }

 ospfv3IfTEDisabled OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
           "Indicates whether or not traffic engineering
           is disabled on the interface when traffic
           engineering is enabled in the area where the
           interface is attached.  The object is set
           to the value true (1) to disable traffic engineering
           on the interface.  Traffic engineering is enabled
           by default on the interface when traffic engineering
           is enabled in the area where the interface is
           attached."
        DEFVAL { false }
        ::= { ospfv3IfEntry 24 }

 ospfv3IfLinkLSASuppression OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
           "Specifies whether or not link LSA origination is
           suppressed for broadcast or NBMA interface types.
           The object is set to value true (1) to suppress
           the origination."
        REFERENCE
             "OSPF for IPv6, Appendix C.3, Router Interface
                 Parameters"
        DEFVAL { false }
        ::= { ospfv3IfEntry 25 }

 -- OSPFv3 Virtual Interface Table

 ospfv3VirtIfTable OBJECT-TYPE
         SYNTAX          SEQUENCE OF Ospfv3VirtIfEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "Information about this router's virtual
             interfaces that the OSPFv3 Process is configured
             to carry on."

         REFERENCE
             "OSPF for IPv6, Appendix C.4, Virtual Link
             Parameters"
         ::= { ospfv3Objects 8 }

 ospfv3VirtIfEntry OBJECT-TYPE
         SYNTAX          Ospfv3VirtIfEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "Information about a single virtual interface.

             The information in this table is persistent,
             and when written, the entity SHOULD save the
             change to non-volatile storage."
         INDEX           { ospfv3VirtIfAreaId,
                           ospfv3VirtIfNeighbor }
         ::= { ospfv3VirtIfTable 1 }

 Ospfv3VirtIfEntry ::= SEQUENCE {
         ospfv3VirtIfAreaId
                 Ospfv3AreaIdTC,
         ospfv3VirtIfNeighbor
                 Ospfv3RouterIdTC,
         ospfv3VirtIfIndex
                 InterfaceIndex,
         ospfv3VirtIfInstId
                 Ospfv3IfInstIdTC,
         ospfv3VirtIfTransitDelay
                 Ospfv3UpToRefreshIntervalTC,
         ospfv3VirtIfRetransInterval
                 Ospfv3UpToRefreshIntervalTC,
         ospfv3VirtIfHelloInterval
                 HelloRange,
         ospfv3VirtIfRtrDeadInterval
                 Ospfv3DeadIntervalRangeTC,
         ospfv3VirtIfState
                 INTEGER,
         ospfv3VirtIfEvents
                 Counter32,
         ospfv3VirtIfRowStatus
                 RowStatus,
         ospfv3VirtIfLinkScopeLsaCount
                 Gauge32,
         ospfv3VirtIfLinkLsaCksumSum
                 Unsigned32
         }

 ospfv3VirtIfAreaId OBJECT-TYPE
         SYNTAX          Ospfv3AreaIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The transit area that the virtual link
             traverses.  By definition, this is not
             Area 0."
         ::= { ospfv3VirtIfEntry 1 }

 ospfv3VirtIfNeighbor OBJECT-TYPE
         SYNTAX          Ospfv3RouterIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The Router ID of the virtual neighbor."
         ::= { ospfv3VirtIfEntry 2 }

 ospfv3VirtIfIndex OBJECT-TYPE
         SYNTAX          InterfaceIndex
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The local interface index assigned by the
             OSPFv3 Process to this OSPFv3 virtual interface.
             It is advertised in Hellos sent over the virtual
             link and in the router's router-LSAs."
         ::= { ospfv3VirtIfEntry 3 }

 ospfv3VirtIfInstId OBJECT-TYPE
         SYNTAX          Ospfv3IfInstIdTC
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The local Interface Instance ID assigned by the
             OSPFv3 Process to this OSPFv3 virtual interface."
         ::= { ospfv3VirtIfEntry 4 }

 ospfv3VirtIfTransitDelay OBJECT-TYPE
         SYNTAX          Ospfv3UpToRefreshIntervalTC
         UNITS           "seconds"
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The estimated number of seconds it takes to
             transmit a Link State Update packet over this
             interface."
         DEFVAL          { 1 }

         ::= { ospfv3VirtIfEntry 5 }

 ospfv3VirtIfRetransInterval OBJECT-TYPE
         SYNTAX          Ospfv3UpToRefreshIntervalTC
         UNITS           "seconds"
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The number of seconds between link state
             advertisement retransmissions for adjacencies
             belonging to this interface.  This value is
             also used when retransmitting database
             description and Link State Request packets.  This
             value should be well over the expected
             round-trip time."
         DEFVAL          { 5 }
         ::= { ospfv3VirtIfEntry 6 }

 ospfv3VirtIfHelloInterval OBJECT-TYPE
         SYNTAX          HelloRange
         UNITS           "seconds"
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The length of time, in seconds, between the
             Hello packets that the router sends on the
             interface.  This value must be the same for the
             virtual neighbor."
         DEFVAL          { 10 }
         ::= { ospfv3VirtIfEntry 7 }

 ospfv3VirtIfRtrDeadInterval OBJECT-TYPE
         SYNTAX          Ospfv3DeadIntervalRangeTC
         UNITS           "seconds"
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The number of seconds that a router's Hello
             packets have not been seen before its
             neighbors declare the router down.  This should
             be some multiple of the Hello interval.  This
             value must be the same for the virtual
             neighbor."
         DEFVAL          { 60 }
         ::= { ospfv3VirtIfEntry 8 }

 ospfv3VirtIfState OBJECT-TYPE
         SYNTAX          INTEGER {
                         down(1),
                         pointToPoint(4)
                         }
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "OSPF virtual interface states.  The same encoding
             as the ospfV3IfTable is used."
         ::= { ospfv3VirtIfEntry 9 }

 ospfv3VirtIfEvents OBJECT-TYPE
         SYNTAX          Counter32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The number of state changes or error events on
             this virtual link.

             Discontinuities in the value of this counter
             can occur at re-initialization of the management
             system and at other times as indicated by the
             value of ospfv3DiscontinuityTime."
         ::= { ospfv3VirtIfEntry 10 }

 ospfv3VirtIfRowStatus OBJECT-TYPE
         SYNTAX          RowStatus
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "This object permits management of the table by
             facilitating actions such as row creation,
             construction, and destruction.

             The value of this object has no effect on
             whether other objects in this conceptual row can be
             modified."
         ::= { ospfv3VirtIfEntry 11 }

 ospfv3VirtIfLinkScopeLsaCount OBJECT-TYPE
         SYNTAX          Gauge32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The total number of Link-scope link state
             advertisements in this virtual link's link state
             database."

         ::= { ospfv3VirtIfEntry 12 }

 ospfv3VirtIfLinkLsaCksumSum OBJECT-TYPE
         SYNTAX          Unsigned32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The 32-bit unsigned sum of the Link-scope link state
             advertisements' LS checksums contained in this
             virtual link's link state database.  The sum can be used
             to determine if there has been a change in a
             router's link state database or to compare the
             link state database of two routers."
         ::= { ospfv3VirtIfEntry 13 }

 -- OSPFv3 Neighbor Table

 ospfv3NbrTable OBJECT-TYPE
         SYNTAX          SEQUENCE OF Ospfv3NbrEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "A table describing all neighbors in the
             locality of the OSPFv3 router."
         REFERENCE
             "OSPF Version 2, Section 10, The Neighbor Data
             Structure"
         ::= { ospfv3Objects 9 }

 ospfv3NbrEntry OBJECT-TYPE
         SYNTAX          Ospfv3NbrEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The information regarding a single neighbor."
         REFERENCE
             "OSPF Version 2, Section 10, The Neighbor Data
             Structure"
         INDEX           { ospfv3NbrIfIndex,
                           ospfv3NbrIfInstId,
                           ospfv3NbrRtrId }
         ::= { ospfv3NbrTable 1 }

 Ospfv3NbrEntry ::= SEQUENCE {
         ospfv3NbrIfIndex
                 InterfaceIndex,
         ospfv3NbrIfInstId
                 Ospfv3IfInstIdTC,

         ospfv3NbrRtrId
                 Ospfv3RouterIdTC,
         ospfv3NbrAddressType
                 InetAddressType,
         ospfv3NbrAddress
                 InetAddress,
         ospfv3NbrOptions
                 Integer32,
         ospfv3NbrPriority
                 DesignatedRouterPriority,
         ospfv3NbrState
                 INTEGER,
         ospfv3NbrEvents
                 Counter32,
         ospfv3NbrLsRetransQLen
                 Gauge32,
         ospfv3NbrHelloSuppressed
                 TruthValue,
         ospfv3NbrIfId
                 InterfaceIndex,
         ospfv3NbrRestartHelperStatus
                 INTEGER,
         ospfv3NbrRestartHelperAge
                 Ospfv3UpToRefreshIntervalTC,
         ospfv3NbrRestartHelperExitReason
                 INTEGER
         }

 ospfv3NbrIfIndex OBJECT-TYPE
         SYNTAX          InterfaceIndex
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The Local Link ID of the link over which the
              neighbor can be reached."
         ::= { ospfv3NbrEntry 1 }

 ospfv3NbrIfInstId OBJECT-TYPE
         SYNTAX          Ospfv3IfInstIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "Interface instance over which the neighbor
             can be reached.  This ID has local link
             significance only."
         ::= { ospfv3NbrEntry 2 }

 ospfv3NbrRtrId OBJECT-TYPE
         SYNTAX          Ospfv3RouterIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "A 32-bit unsigned integer uniquely identifying the
             neighboring router in the Autonomous System."
         ::= { ospfv3NbrEntry 3 }

 ospfv3NbrAddressType OBJECT-TYPE
         SYNTAX          InetAddressType
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The address type of ospfv3NbrAddress.  Only IPv6
             addresses without zone index are expected."
         ::= { ospfv3NbrEntry 4 }

 ospfv3NbrAddress OBJECT-TYPE
         SYNTAX          InetAddress
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The IPv6 address of the neighbor associated with
             the local link."
         ::= { ospfv3NbrEntry 5 }

 ospfv3NbrOptions OBJECT-TYPE
         SYNTAX          Integer32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "A bit mask corresponding to the neighbor's
             options field."
         REFERENCE
             "OSPF for IPv6, Appendix A.2, The Options Field"
         ::= { ospfv3NbrEntry 6 }

 ospfv3NbrPriority OBJECT-TYPE
         SYNTAX          DesignatedRouterPriority
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The priority of this neighbor in the designated-
             router election algorithm.  The value 0 signifies
             that the neighbor is not eligible to become the
             Designated Router on this particular network."
         ::= { ospfv3NbrEntry 7 }

 ospfv3NbrState OBJECT-TYPE
         SYNTAX          INTEGER {
                         down(1),
                         attempt(2),
                         init(3),
                         twoWay(4),
                         exchangeStart(5),
                         exchange(6),
                         loading(7),
                         full(8)
                         }
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The state of the relationship with this
             neighbor."
         REFERENCE
             "OSPF Version 2, Section 10.1, Neighbor states"
         ::= { ospfv3NbrEntry 8 }

 ospfv3NbrEvents OBJECT-TYPE
         SYNTAX          Counter32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The number of times this neighbor relationship
             has changed state or an error has occurred.

             Discontinuities in the value of this counter
             can occur at re-initialization of the management
             system and at other times as indicated by the
             value of ospfv3DiscontinuityTime."
         ::= { ospfv3NbrEntry 9 }

 ospfv3NbrLsRetransQLen OBJECT-TYPE
         SYNTAX          Gauge32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The current length of the retransmission
             queue."
         ::= { ospfv3NbrEntry 10 }

 ospfv3NbrHelloSuppressed OBJECT-TYPE
         SYNTAX          TruthValue
         MAX-ACCESS      read-only
         STATUS          current

         DESCRIPTION
             "Indicates whether Hellos are being suppressed
             to the neighbor."
         ::= { ospfv3NbrEntry 11 }

 ospfv3NbrIfId OBJECT-TYPE
         SYNTAX          InterfaceIndex
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The Interface ID that the neighbor advertises
             in its Hello packets on this link, that is, the
             neighbor's local interface index."
         ::= { ospfv3NbrEntry 12 }

 ospfv3NbrRestartHelperStatus OBJECT-TYPE
        SYNTAX       INTEGER { notHelping(1),
                               helping(2)
                             }
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
           "Indicates whether the router is acting
           as a graceful restart helper for the neighbor."
           ::= { ospfv3NbrEntry 13 }

 ospfv3NbrRestartHelperAge OBJECT-TYPE
        SYNTAX       Ospfv3UpToRefreshIntervalTC
        UNITS        "seconds"
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
           "Remaining time in current OSPF graceful restart
           interval, if the router is acting as a restart
           helper for the neighbor."
        ::= { ospfv3NbrEntry 14 }

 ospfv3NbrRestartHelperExitReason OBJECT-TYPE
        SYNTAX       INTEGER { none(1),
                               inProgress(2),
                               completed(3),
                               timedOut(4),
                               topologyChanged(5)
                             }
        MAX-ACCESS   read-only
        STATUS       current

        DESCRIPTION
           "Describes the outcome of the last attempt at acting
           as a graceful restart helper for the neighbor.

           none:            no restart has yet been attempted.
           inProgress:      a restart attempt is currently underway.
           completed:       the last restart completed successfully.
           timedOut:        the last restart timed out.
           topologyChanged: the last restart was aborted due to
                            a topology change."
     ::= { ospfv3NbrEntry 15 }

 -- OSPFv3 Configured Neighbor Table

 ospfv3CfgNbrTable OBJECT-TYPE
         SYNTAX          SEQUENCE OF Ospfv3CfgNbrEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "A table describing all configured neighbors.

             The Configured Neighbors table just gives
             OSPFv3 information for sending OSPFv3 packets
             to potential neighbors and is typically used
             on NBMA and Point-to-Multipoint networks.
             Once a Hello is received from a neighbor in
             the Configured Neighbor table, an entry for
             that neighbor is created in the Neighbor table
             and adjacency state is maintained there.
             Neighbors on multi-access or Point-to-Point
             networks can use multicast addressing, so only
             Neighbor table entries are created for them."
         REFERENCE
             "OSPF Version 2, Section 10, The Neighbor Data
             Structure"
         ::= { ospfv3Objects 10 }

 ospfv3CfgNbrEntry OBJECT-TYPE
         SYNTAX          Ospfv3CfgNbrEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The information regarding a single configured
             neighbor.

             The information in this table is persistent,
             and when written, the entity SHOULD save the
             change to non-volatile storage."

         REFERENCE
             "OSPF Version 2, Section 10, The Neighbor Data
             Structure"
         INDEX           { ospfv3CfgNbrIfIndex,
                           ospfv3CfgNbrIfInstId,
                           ospfv3CfgNbrAddressType,
                           ospfv3CfgNbrAddress }
         ::= { ospfv3CfgNbrTable 1 }

 Ospfv3CfgNbrEntry ::= SEQUENCE {
         ospfv3CfgNbrIfIndex
                 InterfaceIndex,
         ospfv3CfgNbrIfInstId
                 Ospfv3IfInstIdTC,
         ospfv3CfgNbrAddressType
                 InetAddressType,
         ospfv3CfgNbrAddress
                 InetAddress,
         ospfv3CfgNbrPriority
                 DesignatedRouterPriority,
         ospfv3CfgNbrRowStatus
                 RowStatus
         }

 ospfv3CfgNbrIfIndex OBJECT-TYPE
         SYNTAX          InterfaceIndex
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The Local Link ID of the link over which the
              neighbor can be reached."
         ::= { ospfv3CfgNbrEntry 1 }

 ospfv3CfgNbrIfInstId OBJECT-TYPE
         SYNTAX          Ospfv3IfInstIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "Interface instance over which the neighbor
             can be reached.  This ID has local link
             significance only."
         ::= { ospfv3CfgNbrEntry 2 }

 ospfv3CfgNbrAddressType OBJECT-TYPE
         SYNTAX          InetAddressType
         MAX-ACCESS      not-accessible
         STATUS          current

         DESCRIPTION
             "The address type of ospfv3NbrAddress.  Only IPv6
             addresses without zone index are expected."
         ::= { ospfv3CfgNbrEntry 3 }

 ospfv3CfgNbrAddress OBJECT-TYPE
         SYNTAX          InetAddress
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The IPv6 address of the neighbor associated with
             the local link."
         ::= { ospfv3CfgNbrEntry 4 }

 ospfv3CfgNbrPriority OBJECT-TYPE
         SYNTAX          DesignatedRouterPriority
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "The priority of this neighbor in the designated-
             router election algorithm.  The value 0 signifies
             that the neighbor is not eligible to become the
             Designated Router on this particular network."
         DEFVAL          { 1 }
         ::= { ospfv3CfgNbrEntry 5 }

 ospfv3CfgNbrRowStatus OBJECT-TYPE
         SYNTAX          RowStatus
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "This object permits management of the table by
             facilitating actions such as row creation,
             construction, and destruction.

             The value of this object has no effect on
             whether other objects in this conceptual row can be
             modified."
         ::= { ospfv3CfgNbrEntry 6 }

 -- OSPFv3 Virtual Neighbor Table

 ospfv3VirtNbrTable OBJECT-TYPE
         SYNTAX          SEQUENCE OF Ospfv3VirtNbrEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "A table describing all virtual neighbors."

         REFERENCE
             "OSPF Version 2, Section 15, Virtual Links"
         ::= { ospfv3Objects 11 }

 ospfv3VirtNbrEntry OBJECT-TYPE
         SYNTAX          Ospfv3VirtNbrEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "Virtual neighbor information."
         INDEX           { ospfv3VirtNbrArea,
                           ospfv3VirtNbrRtrId }
         ::= { ospfv3VirtNbrTable 1 }

 Ospfv3VirtNbrEntry ::= SEQUENCE {
         ospfv3VirtNbrArea
                 Ospfv3AreaIdTC,
         ospfv3VirtNbrRtrId
                 Ospfv3RouterIdTC,
         ospfv3VirtNbrIfIndex
                 InterfaceIndex,
         ospfv3VirtNbrIfInstId
                 Ospfv3IfInstIdTC,
         ospfv3VirtNbrAddressType
                 InetAddressType,
         ospfv3VirtNbrAddress
                 InetAddress,
         ospfv3VirtNbrOptions
                 Integer32,
         ospfv3VirtNbrState
                 INTEGER,
         ospfv3VirtNbrEvents
                 Counter32,
         ospfv3VirtNbrLsRetransQLen
                 Gauge32,
         ospfv3VirtNbrHelloSuppressed
                 TruthValue,
         ospfv3VirtNbrIfId
                 InterfaceIndex,
         ospfv3VirtNbrRestartHelperStatus
                 INTEGER,
         ospfv3VirtNbrRestartHelperAge
                 Ospfv3UpToRefreshIntervalTC,
         ospfv3VirtNbrRestartHelperExitReason
                 INTEGER
         }

 ospfv3VirtNbrArea OBJECT-TYPE
         SYNTAX          Ospfv3AreaIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The transit area Identifier."
         ::= { ospfv3VirtNbrEntry 1 }

 ospfv3VirtNbrRtrId OBJECT-TYPE
         SYNTAX          Ospfv3RouterIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "A 32-bit integer uniquely identifying the
             neighboring router in the Autonomous System."
         ::= { ospfv3VirtNbrEntry 2 }

 ospfv3VirtNbrIfIndex OBJECT-TYPE
         SYNTAX          InterfaceIndex
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The local Interface ID for the virtual link over
             which the neighbor can be reached."
         ::= { ospfv3VirtNbrEntry 3 }

 ospfv3VirtNbrIfInstId OBJECT-TYPE
         SYNTAX          Ospfv3IfInstIdTC
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The interface instance for the virtual link over
             which the neighbor can be reached."
         ::= { ospfv3VirtNbrEntry 4 }

 ospfv3VirtNbrAddressType OBJECT-TYPE
         SYNTAX          InetAddressType
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The address type of ospfv3VirtNbrAddress.  Only IPv6
             addresses without zone index are expected."
         ::= { ospfv3VirtNbrEntry 5 }

 ospfv3VirtNbrAddress OBJECT-TYPE
         SYNTAX          InetAddress
         MAX-ACCESS      read-only
         STATUS          current

         DESCRIPTION
             "The IPv6 address advertised by this virtual neighbor.
             It must be a global scope address."
         ::= { ospfv3VirtNbrEntry 6 }

 ospfv3VirtNbrOptions OBJECT-TYPE
         SYNTAX          Integer32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "A bit mask corresponding to the neighbor's options
             field."
         REFERENCE
             "OSPF for IPv6, Appendix A.2, The Options Field"
         ::= { ospfv3VirtNbrEntry 7 }

 ospfv3VirtNbrState OBJECT-TYPE
         SYNTAX          INTEGER {
                         down(1),
                         attempt(2),
                         init(3),
                         twoWay(4),
                         exchangeStart(5),
                         exchange(6),
                         loading(7),
                         full(8)
                         }
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The state of the virtual neighbor relationship."
         ::= { ospfv3VirtNbrEntry 8 }

 ospfv3VirtNbrEvents OBJECT-TYPE
         SYNTAX          Counter32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The number of times this virtual link has
             changed its state or an error has occurred.

             Discontinuities in the value of this counter
             can occur at re-initialization of the management
             system and at other times as indicated by the
             value of ospfv3DiscontinuityTime."
         ::= { ospfv3VirtNbrEntry 9 }

 ospfv3VirtNbrLsRetransQLen OBJECT-TYPE
         SYNTAX          Gauge32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The current length of the retransmission
             queue."
         ::= { ospfv3VirtNbrEntry 10 }

 ospfv3VirtNbrHelloSuppressed OBJECT-TYPE
         SYNTAX          TruthValue
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "Indicates whether Hellos are being suppressed
             to the neighbor."
         ::= { ospfv3VirtNbrEntry 11 }

 ospfv3VirtNbrIfId OBJECT-TYPE
         SYNTAX          InterfaceIndex
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The Interface ID that the neighbor advertises
             in its Hello packets on this virtual link, that is,
             the neighbor's local Interface ID."
         ::= { ospfv3VirtNbrEntry 12 }

ospfv3VirtNbrRestartHelperStatus OBJECT-TYPE
        SYNTAX       INTEGER { notHelping(1),
                               helping(2)
                             }
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "Indicates whether the router is acting
            as a graceful restart helper for the neighbor."
           ::= { ospfv3VirtNbrEntry 13 }

 ospfv3VirtNbrRestartHelperAge OBJECT-TYPE
        SYNTAX       Ospfv3UpToRefreshIntervalTC
        UNITS        "seconds"
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "Remaining time in the current OSPF graceful restart
            interval, if the router is acting as a restart
            helper for the neighbor."

        ::= { ospfv3VirtNbrEntry 14 }

 ospfv3VirtNbrRestartHelperExitReason OBJECT-TYPE
        SYNTAX       INTEGER { none(1),
                               inProgress(2),
                               completed(3),
                               timedOut(4),
                               topologyChanged(5)
                             }
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "Describes the outcome of the last attempt at acting
            as a graceful restart helper for the neighbor.

            none:            no restart has yet been attempted.
            inProgress:      a restart attempt is currently underway.
            completed:       the last restart completed successfully.
            timedOut:        the last restart timed out.
            topologyChanged: the last restart was aborted due to
                             a topology change."
     ::= { ospfv3VirtNbrEntry 15 }

 --
 -- The OSPFv3 Area Aggregate Table
 --

 ospfv3AreaAggregateTable OBJECT-TYPE
         SYNTAX          SEQUENCE OF Ospfv3AreaAggregateEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The Area Aggregate Table acts as an adjunct
             to the Area Table.  It describes those address
             aggregates that are configured to be propagated
             from an area.  Its purpose is to reduce the amount
             of information that is known beyond an area's
             borders.

             A range of IPv6 prefixes specified by a
             prefix / prefix length pair.  Note that if
             ranges are configured such that one range
             subsumes another range, the most specific
             match is the preferred one."
         ::= { ospfv3Objects 12 }

 ospfv3AreaAggregateEntry OBJECT-TYPE
         SYNTAX          Ospfv3AreaAggregateEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "A single area aggregate entry.

             Information in this table is persistent, and
             when this object is written, the entity SHOULD
             save the change to non-volatile storage."
         REFERENCE
             "OSPF Version 2, Appendix C.2, Area parameters"
         INDEX           { ospfv3AreaAggregateAreaID,
                           ospfv3AreaAggregateAreaLsdbType,
                           ospfv3AreaAggregatePrefixType,
                           ospfv3AreaAggregatePrefix,
                           ospfv3AreaAggregatePrefixLength }
         ::= { ospfv3AreaAggregateTable 1 }

 Ospfv3AreaAggregateEntry ::= SEQUENCE {
         ospfv3AreaAggregateAreaID
                 Ospfv3AreaIdTC,
         ospfv3AreaAggregateAreaLsdbType
                 INTEGER,
         ospfv3AreaAggregatePrefixType
                 InetAddressType,
         ospfv3AreaAggregatePrefix
                 InetAddress,
         ospfv3AreaAggregatePrefixLength
                 InetAddressPrefixLength,
         ospfv3AreaAggregateRowStatus
                 RowStatus,
         ospfv3AreaAggregateEffect
                 INTEGER,
         ospfv3AreaAggregateRouteTag
                 Unsigned32
         }

 ospfv3AreaAggregateAreaID OBJECT-TYPE
         SYNTAX          Ospfv3AreaIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The area the Address Aggregate is to be found
             within."
         REFERENCE
             "OSPF Version 2, Appendix C.2, Area parameters"
         ::= { ospfv3AreaAggregateEntry 1 }

 ospfv3AreaAggregateAreaLsdbType OBJECT-TYPE
         SYNTAX          INTEGER {
                         interAreaPrefixLsa(8195), -- 0x2003
                         nssaExternalLsa(8199)     -- 0x2007
                         }
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The type of the Address Aggregate.  This field
             specifies the Area LSDB type that this Address
             Aggregate applies to."
         REFERENCE
             "OSPF Version 2, Appendix A.4.1, The LSA header"
         ::= { ospfv3AreaAggregateEntry 2 }

 ospfv3AreaAggregatePrefixType OBJECT-TYPE
         SYNTAX          InetAddressType
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The prefix type of ospfv3AreaAggregatePrefix.  Only
             IPv6 addresses are expected."
         ::= { ospfv3AreaAggregateEntry 3 }

 ospfv3AreaAggregatePrefix OBJECT-TYPE
         SYNTAX          InetAddress (SIZE (0..16))
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The IPv6 prefix."
         REFERENCE
             "OSPF Version 2, Appendix C.2, Area parameters"
         ::= { ospfv3AreaAggregateEntry 4 }

 ospfv3AreaAggregatePrefixLength OBJECT-TYPE
         SYNTAX          InetAddressPrefixLength (3..128)
         UNITS           "bits"
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The length of the prefix (in bits).  A prefix can
             not be shorter than 3 bits."
         REFERENCE
             "OSPF Version 2, Appendix C.2, Area parameters"
         ::= { ospfv3AreaAggregateEntry 5 }

 ospfv3AreaAggregateRowStatus OBJECT-TYPE
         SYNTAX          RowStatus

         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "This object permits management of the table by
             facilitating actions such as row creation,
             construction, and destruction.

             The value of this object has no effect on
             whether other objects in this conceptual row can be
             modified."
         ::= { ospfv3AreaAggregateEntry 6 }

 ospfv3AreaAggregateEffect OBJECT-TYPE
         SYNTAX          INTEGER {
                         advertiseMatching(1),
                         doNotAdvertiseMatching(2)
                         }
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "Prefixes subsumed by ranges will either trigger the
             advertisement of the indicated aggregate
             (advertiseMatching) or result in the prefix not
             being advertised at all outside the area."
         DEFVAL          { advertiseMatching }
         ::= { ospfv3AreaAggregateEntry 7 }

 ospfv3AreaAggregateRouteTag OBJECT-TYPE
         SYNTAX          Unsigned32
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION
             "This tag is advertised only in the summarized
             As-External LSA when summarizing from NSSA-LSAs to
             AS-External-LSAs."
         DEFVAL         { 0 }
         ::= { ospfv3AreaAggregateEntry 8 }

 -- OSPFv3 Link-Scope Link State Database, for virtual interfaces

 ospfv3VirtLinkLsdbTable OBJECT-TYPE
         SYNTAX          SEQUENCE OF Ospfv3VirtLinkLsdbEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The OSPFv3 Process's Link-scope LSDB for virtual
             interfaces.  The LSDB contains the Link-scope link
             state advertisements from virtual interfaces."

         ::= { ospfv3Objects 13 }

 ospfv3VirtLinkLsdbEntry OBJECT-TYPE
         SYNTAX          Ospfv3VirtLinkLsdbEntry
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "A single Link-scope link state advertisement
             for a virtual interface."
         INDEX           { ospfv3VirtLinkLsdbIfAreaId,
                           ospfv3VirtLinkLsdbIfNeighbor,
                           ospfv3VirtLinkLsdbType,
                           ospfv3VirtLinkLsdbRouterId,
                           ospfv3VirtLinkLsdbLsid }
         ::= { ospfv3VirtLinkLsdbTable 1 }

 Ospfv3VirtLinkLsdbEntry ::= SEQUENCE {
         ospfv3VirtLinkLsdbIfAreaId
                 Ospfv3AreaIdTC,
         ospfv3VirtLinkLsdbIfNeighbor
                 Ospfv3RouterIdTC,
         ospfv3VirtLinkLsdbType
                 Unsigned32,
         ospfv3VirtLinkLsdbRouterId
                 Ospfv3RouterIdTC,
         ospfv3VirtLinkLsdbLsid
                 Ospfv3LsIdTC,
         ospfv3VirtLinkLsdbSequence
                 Ospfv3LsaSequenceTC,
         ospfv3VirtLinkLsdbAge
                 Ospfv3LsaAgeTC,
         ospfv3VirtLinkLsdbChecksum
                 Integer32,
         ospfv3VirtLinkLsdbAdvertisement
                 OCTET STRING,
         ospfv3VirtLinkLsdbTypeKnown
                 TruthValue
         }

 ospfv3VirtLinkLsdbIfAreaId OBJECT-TYPE
         SYNTAX          Ospfv3AreaIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The transit area that the virtual link
             traverses.  By definition, this is not
             Area 0."
         ::= { ospfv3VirtLinkLsdbEntry 1 }

 ospfv3VirtLinkLsdbIfNeighbor OBJECT-TYPE
         SYNTAX          Ospfv3RouterIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The Router ID of the virtual neighbor."
         ::= { ospfv3VirtLinkLsdbEntry 2 }

 ospfv3VirtLinkLsdbType OBJECT-TYPE
         SYNTAX          Unsigned32(0..'FFFFFFFF'h)
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The type of the link state advertisement.
             Each link state type has a separate
             advertisement format.  Link-scope LSAs unrecognized
             by the router are also stored in this database."
         ::= { ospfv3VirtLinkLsdbEntry 3 }

 ospfv3VirtLinkLsdbRouterId OBJECT-TYPE
         SYNTAX          Ospfv3RouterIdTC
         MAX-ACCESS      not-accessible
         STATUS          current
         DESCRIPTION
             "The 32-bit number that uniquely identifies the
             originating router in the Autonomous System."
         REFERENCE
             "OSPF Version 2, Appendix C.1, Global parameters"
         ::= { ospfv3VirtLinkLsdbEntry 4 }

 ospfv3VirtLinkLsdbLsid OBJECT-TYPE
         SYNTAX        Ospfv3LsIdTC
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "The Link State ID is an LS type-specific field
             containing a unique identifier;
             it identifies the piece of the routing domain
             that is being described by the advertisement.
             In contrast to OSPFv2, the LSID has no
             addressing semantics."
         ::= { ospfv3VirtLinkLsdbEntry 5 }

 -- Note that the OSPF sequence number is a 32-bit signed
 -- integer.  It starts with the value '80000001'h
 -- or -'7FFFFFFF'h, and increments until '7FFFFFFF'h.
 -- Thus, a typical sequence number will be very negative.

 ospfv3VirtLinkLsdbSequence OBJECT-TYPE
         SYNTAX          Ospfv3LsaSequenceTC
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The sequence number field is a signed 32-bit
             integer.  It is used to detect old and duplicate
             link state advertisements.  The space of
             sequence numbers is linearly ordered.  The
             larger the sequence number, the more recent the
             advertisement."
         REFERENCE
             "OSPF Version 2, Section 12.1.6, LS sequence
             number"
         ::= { ospfv3VirtLinkLsdbEntry 6 }

 ospfv3VirtLinkLsdbAge OBJECT-TYPE
         SYNTAX          Ospfv3LsaAgeTC
         UNITS           "seconds"
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "This field is the age of the link state
             advertisement in seconds.  The high-order bit
             of the LS age field is considered the DoNotAge
             bit for support of on-demand circuits."
         REFERENCE
             "OSPF Version 2, Section 12.1.1, LS age;
              Extending OSPF to Support Demand Circuits,
              Section 2.2, The LS age field."
         ::= { ospfv3VirtLinkLsdbEntry 7 }

 ospfv3VirtLinkLsdbChecksum OBJECT-TYPE
         SYNTAX          Integer32
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "This field is the checksum of the complete
             contents of the advertisement, excepting the
             age field.  The age field is excepted so that
             an advertisement's age can be incremented
             without updating the checksum.  The checksum
             used is the same that is used for ISO
             connectionless datagrams; it is commonly
             referred to as the Fletcher checksum."
         REFERENCE
             "OSPF Version 2, Section 12.1.7, LS checksum"
         ::= { ospfv3VirtLinkLsdbEntry 8 }

 ospfv3VirtLinkLsdbAdvertisement OBJECT-TYPE
         SYNTAX          OCTET STRING (SIZE (1..65535))
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The entire link state advertisement, including
             its header."
         ::= { ospfv3VirtLinkLsdbEntry 9 }

 ospfv3VirtLinkLsdbTypeKnown OBJECT-TYPE
         SYNTAX          TruthValue
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION
             "The value true (1) indicates that the LSA type is
             recognized by this router."
         ::= { ospfv3VirtLinkLsdbEntry 10 }

 -- The Ospfv3 Notification Table

 -- The Ospfv3 Notification Table records fields that are
 -- required for notifications.

 ospfv3NotificationEntry OBJECT IDENTIFIER
         ::= { ospfv3Objects 14 }

 ospfv3ConfigErrorType OBJECT-TYPE
     SYNTAX       INTEGER {
                     badVersion(1),
                     areaMismatch(2),
                     unknownNbmaNbr(3), -- Router is DR eligible
                     unknownVirtualNbr(4),
                     helloIntervalMismatch(5),
                     deadIntervalMismatch(6),
                     optionMismatch(7),
                     mtuMismatch(8),
                     duplicateRouterId(9),
                     noError(10) }
     MAX-ACCESS   accessible-for-notify
     STATUS   current
     DESCRIPTION
         "Potential types of configuration conflicts.
         Used by the ospfv3ConfigError and
         ospfv3ConfigVirtError notifications."
     ::= { ospfv3NotificationEntry 1 }

 ospfv3PacketType OBJECT-TYPE
     SYNTAX       INTEGER {
                     hello(1),
                     dbDescript(2),
                     lsReq(3),
                     lsUpdate(4),
                     lsAck(5),
                     nullPacket(6) }
     MAX-ACCESS   accessible-for-notify
     STATUS       current
     DESCRIPTION
         "OSPFv3 packet types."
     ::= { ospfv3NotificationEntry 2 }

 ospfv3PacketSrc  OBJECT-TYPE
     SYNTAX       InetAddressIPv6
     MAX-ACCESS   accessible-for-notify
     STATUS       current
     DESCRIPTION
         "The IPv6 address of an inbound packet that cannot
         be identified by a neighbor instance.

         Only IPv6 addresses without zone index are expected."
     ::= { ospfv3NotificationEntry 3 }

 -- Notification Definitions

 -- The notifications need to be throttled so as to not overwhelm the
 -- management agent in case of rapid changes to the OSPFv3 module.

ospfv3VirtIfStateChange NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId,  -- The originator of the notification
               ospfv3VirtIfState  -- The new state
        }
     STATUS       current
     DESCRIPTION
         "An ospfv3VirtIfStateChange notification signifies that
         there has been a change in the state of an OSPFv3 virtual
         interface.

         This notification should be generated when the interface
         state regresses (e.g., goes from Point-to-Point to Down)
         or progresses to a terminal state (i.e., Point-to-Point)."
     ::= { ospfv3Notifications 1 }

ospfv3NbrStateChange NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId, -- The originator of the notification
               ospfv3NbrState  -- The new state

        }
     STATUS       current
     DESCRIPTION
         "An ospfv3NbrStateChange notification signifies that
         there has been a change in the state of a
         non-virtual OSPFv3 neighbor.  This notification should be
         generated when the neighbor state regresses
         (e.g., goes from Attempt or Full to 1-Way or
         Down) or progresses to a terminal state (e.g.,
         2-Way or Full).  When a neighbor transitions
         from or to Full on non-broadcast multi-access
         and broadcast networks, the notification should be
         generated by the Designated Router.  A Designated
         Router transitioning to Down will be noted by
         ospfIfStateChange."
     ::= { ospfv3Notifications 2 }

ospfv3VirtNbrStateChange NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId, -- The originator of the notification
               ospfv3VirtNbrState  -- The new state
        }
     STATUS       current
     DESCRIPTION
         "An ospfv3VirtNbrStateChange notification signifies
         that there has been a change in the state of an OSPFv3
         virtual neighbor.  This notification should be generated
         when the neighbor state regresses (e.g., goes
         from Attempt or Full to 1-Way or Down) or
         progresses to a terminal state (e.g., Full)."
     ::= { ospfv3Notifications 3 }

ospfv3IfConfigError NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId, -- The originator of the notification
        ospfv3IfState,         -- State of the interface
        ospfv3PacketSrc,       -- IPv6 address of source
        ospfv3ConfigErrorType, -- Type of error
        ospfv3PacketType       -- Type of packet
        }
     STATUS       current
     DESCRIPTION
         "An ospfv3IfConfigError notification signifies that a
         packet has been received on a non-virtual
         interface from a router whose configuration
         parameters conflict with this router's
         configuration parameters.  Note that the event
         optionMismatch should cause a notification only if it
         prevents an adjacency from forming."
     ::= { ospfv3Notifications 4 }

ospfv3VirtIfConfigError NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId, -- The originator of the notification
        ospfv3VirtIfState,     -- State of the interface
        ospfv3ConfigErrorType, -- Type of error
        ospfv3PacketType
        }
     STATUS       current
     DESCRIPTION
         "An ospfv3VirtIfConfigError notification signifies that a
         packet has been received on a virtual interface
         from a router whose configuration parameters
         conflict with this router's configuration
         parameters.  Note that the event optionMismatch
         should cause a notification only if it prevents an
         adjacency from forming."
     ::= { ospfv3Notifications 5 }

ospfv3IfRxBadPacket NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId, -- The originator of the notification
        ospfv3IfState,         -- State of the interface
        ospfv3PacketSrc,       -- The source IPv6 address
        ospfv3PacketType       -- Type of packet
        }
     STATUS       current
     DESCRIPTION
         "An ospfv3IfRxBadPacket notification signifies that an
         OSPFv3 packet that cannot be parsed has been received on a
         non-virtual interface."
     ::= { ospfv3Notifications 6 }

ospfv3VirtIfRxBadPacket NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId, -- The originator of the notification
       ospfv3VirtIfState,      -- State of the interface
       ospfv3PacketType        -- Type of packet
       }
     STATUS       current
     DESCRIPTION
         "An ospfv3VirtIfRxBadPacket notification signifies
         that an OSPFv3 packet that cannot be parsed has been
         received on a virtual interface."
     ::= { ospfv3Notifications 7 }

ospfv3LsdbOverflow NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId, -- The originator of the notification
        ospfv3ExtAreaLsdbLimit -- Limit on External LSAs
        }
     STATUS       current

     DESCRIPTION
         "An ospfv3LsdbOverflow notification signifies that the
         number of LSAs in the router's link state
         database has exceeded ospfv3ExtAreaLsdbLimit."
     ::= { ospfv3Notifications 8 }

ospfv3LsdbApproachingOverflow NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId, -- The originator of the notification
        ospfv3ExtAreaLsdbLimit
        }
     STATUS       current
     DESCRIPTION
         "An ospfv3LsdbApproachingOverflow notification signifies
         that the number of LSAs in the router's
         link state database has exceeded ninety percent of
         ospfv3ExtAreaLsdbLimit."
     ::= { ospfv3Notifications 9 }

ospfv3IfStateChange NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId, -- The originator of the notification
        ospfv3IfState   -- The new state
        }
     STATUS       current
     DESCRIPTION
         "An ospfv3IfStateChange notification signifies that there
         has been a change in the state of a non-virtual
         OSPFv3 interface.  This notification should be generated
         when the interface state regresses (e.g., goes
         from DR to Down) or progresses to a terminal
         state (i.e., Point-to-Point, DR Other, DR, or
         Backup)."
     ::= { ospfv3Notifications 10 }

ospfv3NssaTranslatorStatusChange NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId, -- The originator of the notification
        ospfv3AreaNssaTranslatorState  -- new state
        }
     STATUS       current
     DESCRIPTION
         "An ospfv3NssaTranslatorStatusChange notification
         indicates that there has been a change in the router's
         ability to translate OSPFv3 NSSA LSAs into OSPFv3 External
         LSAs.  This notification should be generated when the
         Translator Status transitions from or to any defined
         status on a per-area basis."
     ::= { ospfv3Notifications 11 }

ospfv3RestartStatusChange NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId, -- The originator of the notification
               ospfv3RestartStatus,  -- new status
               ospfv3RestartInterval,
               ospfv3RestartExitReason
             }
     STATUS       current
     DESCRIPTION
         "An ospfv3RestartStatusChange notification signifies that
         there has been a change in the graceful restart
         state for the router.  This notification should be
         generated when the router restart status
         changes."
     ::= { ospfv3Notifications 12 }

ospfv3NbrRestartHelperStatusChange NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId, -- The originator of the notification
               ospfv3NbrRestartHelperStatus,  -- new status
               ospfv3NbrRestartHelperAge,
               ospfv3NbrRestartHelperExitReason
             }
     STATUS       current
     DESCRIPTION
         "An ospfv3NbrRestartHelperStatusChange notification
         signifies that there has been a change in the
         graceful restart helper state for the neighbor.
         This notification should be generated when the
         neighbor restart helper status transitions for a neighbor."
     ::= { ospfv3Notifications 13 }

ospfv3VirtNbrRestartHelperStatusChange NOTIFICATION-TYPE
     OBJECTS { ospfv3RouterId, -- The originator of the notification
               ospfv3VirtNbrRestartHelperStatus,  -- new status
               ospfv3VirtNbrRestartHelperAge,
               ospfv3VirtNbrRestartHelperExitReason
             }
     STATUS       current
     DESCRIPTION
         "An ospfv3VirtNbrRestartHelperStatusChange
         notification signifies that there has been a
         change in the graceful restart helper state for
         the virtual neighbor.  This notification should be
         generated when the virtual neighbor restart helper status
         transitions for a virtual neighbor."
     ::= { ospfv3Notifications 14 }

 -- Conformance Information

 ospfv3Groups      OBJECT IDENTIFIER ::= { ospfv3Conformance 1 }
 ospfv3Compliances OBJECT IDENTIFIER ::= { ospfv3Conformance 2 }

 -- Compliance Statements

 ospfv3FullCompliance MODULE-COMPLIANCE
         STATUS          current
         DESCRIPTION     "The compliance statement"
         MODULE          -- this module
         MANDATORY-GROUPS {
                         ospfv3BasicGroup,
                         ospfv3AreaGroup,
                         ospfv3IfGroup,
                         ospfv3VirtIfGroup,
                         ospfv3NbrGroup,
                         ospfv3CfgNbrGroup,
                         ospfv3VirtNbrGroup,
                         ospfv3AreaAggregateGroup
                         }

         GROUP           ospfv3AsLsdbGroup
         DESCRIPTION
             "This group is required for OSPFv3 systems that
             display their AS-scope link state database."

         GROUP           ospfv3AreaLsdbGroup
         DESCRIPTION
             "This group is required for OSPFv3 systems that
             display their Area-scope link state database."

         GROUP           ospfv3LinkLsdbGroup
         DESCRIPTION
             "This group is required for OSPFv3 systems that
             display their Link-scope link state database
             for non-virtual interfaces."

         GROUP           ospfv3VirtLinkLsdbGroup
         DESCRIPTION
             "This group is required for OSPFv3 systems that
             display their Link-scope link state database
             for virtual interfaces."

         GROUP           ospfv3HostGroup
         DESCRIPTION
             "This group is required for OSPFv3 systems that
             support attached hosts."

         GROUP           ospfv3NotificationObjectGroup
         DESCRIPTION
             "This group is required for OSPFv3 systems that
             support OSPFv3 notifications."

         GROUP           ospfv3NotificationGroup
         DESCRIPTION
             "This group is required for OSPFv3 systems that
             support OSPFv3 notifications."

         OBJECT          ospfv3NbrAddressType
         SYNTAX          InetAddressType { ipv6(2) }
         DESCRIPTION
             "An implementation is only required to support IPv6
             address without zone index."

         OBJECT          ospfv3NbrAddress
         SYNTAX          InetAddress (SIZE (16))
         DESCRIPTION
             "An implementation is only required to support IPv6
             address without zone index."

         OBJECT          ospfv3VirtNbrAddressType
         SYNTAX          InetAddressType { ipv6(2) }
         DESCRIPTION
             "An implementation is only required to support IPv6
             address without zone index."

         OBJECT          ospfv3VirtNbrAddress
         SYNTAX          InetAddress (SIZE (16))
         DESCRIPTION
             "An implementation is only required to support IPv6
             address without zone index."

         ::= { ospfv3Compliances 1 }

    ospfv3ReadOnlyCompliance MODULE-COMPLIANCE
       STATUS     current
       DESCRIPTION
               "When this MIB module is implemented without
               support for read-create (i.e., in read-only
               mode), the implementation can claim read-only
               compliance.  Such a device can then be monitored,
               but cannot be configured with this MIB."

       MODULE -- this module
            MANDATORY-GROUPS {
                    ospfv3BasicGroup,

                    ospfv3AreaGroup,
                    ospfv3IfGroup,
                    ospfv3VirtIfGroup,
                    ospfv3NbrGroup,
                    ospfv3CfgNbrGroup,
                    ospfv3VirtNbrGroup,
                    ospfv3AreaAggregateGroup
                    }

       GROUP           ospfv3AsLsdbGroup
       DESCRIPTION
           "This group is required for OSPFv3 systems that
           display their AS-scope link state database."

       GROUP           ospfv3AreaLsdbGroup
       DESCRIPTION
           "This group is required for OSPFv3 systems that
           display their Area-scope link state database."

       GROUP           ospfv3LinkLsdbGroup
       DESCRIPTION
           "This group is required for OSPFv3 systems that
           display their Link-scope link state database
           for non-virtual interfaces."

       GROUP           ospfv3VirtLinkLsdbGroup
       DESCRIPTION
           "This group is required for OSPFv3 systems that
           display their Link-scope link state database
           for virtual interfaces."

       GROUP           ospfv3HostGroup
       DESCRIPTION
           "This group is required for OSPFv3 systems that
           support attached hosts."

       GROUP           ospfv3NotificationObjectGroup
       DESCRIPTION
           "This group is required for OSPFv3 systems that
           support OSPFv3 notifications."

       GROUP           ospfv3NotificationGroup
       DESCRIPTION
           "This group is required for OSPFv3 systems that
           support OSPFv3 notifications."

       OBJECT ospfv3RouterId
       MIN-ACCESS read-only

       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3AdminStatus
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3ExtAreaLsdbLimit
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3ExitOverflowInterval
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3DemandExtensions
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3ReferenceBandwidth
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3RestartSupport
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3RestartInterval
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3RestartStrictLsaChecking
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3NotificationEnable
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3StubRouterAdvertisement
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3AreaImportAsExtern
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3AreaSummary
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3AreaRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3AreaStubMetric
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3AreaNssaTranslatorRole
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3AreaNssaTranslatorStabInterval
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3AreaStubMetricType
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3AreaTEEnabled
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3HostMetric
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3HostRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3HostAreaID
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfAreaId
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfType
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfAdminStatus
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfRtrPriority
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfTransitDelay
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfRetransInterval
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfHelloInterval
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfRtrDeadInterval
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfPollInterval
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfDemand
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfMetricValue
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfDemandNbrProbe
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfDemandNbrProbeRetransLimit
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfDemandNbrProbeInterval
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfTEDisabled
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3IfLinkLSASuppression
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3VirtIfTransitDelay
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3VirtIfRetransInterval
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3VirtIfHelloInterval
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3VirtIfRtrDeadInterval
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3VirtIfRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3CfgNbrPriority
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3CfgNbrRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3AreaAggregateRowStatus
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3AreaAggregateEffect
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."

       OBJECT ospfv3AreaAggregateRouteTag
       MIN-ACCESS read-only
       DESCRIPTION
            "Write access is not required."
    ::= { ospfv3Compliances 2 }

 -- units of conformance

 ospfv3BasicGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3RouterId,
                         ospfv3AdminStatus,
                         ospfv3VersionNumber,
                         ospfv3AreaBdrRtrStatus,
                         ospfv3ASBdrRtrStatus,
                         ospfv3AsScopeLsaCount,
                         ospfv3AsScopeLsaCksumSum,
                         ospfv3OriginateNewLsas,
                         ospfv3RxNewLsas,
                         ospfv3ExtLsaCount,
                         ospfv3ExtAreaLsdbLimit,
                         ospfv3ExitOverflowInterval,
                         ospfv3DemandExtensions,
                         ospfv3ReferenceBandwidth,
                         ospfv3RestartSupport,
                         ospfv3RestartInterval,
                         ospfv3RestartStrictLsaChecking,
                         ospfv3RestartStatus,
                         ospfv3RestartAge,
                         ospfv3RestartExitReason,
                         ospfv3NotificationEnable,
                         ospfv3StubRouterSupport,
                         ospfv3StubRouterAdvertisement,
                         ospfv3DiscontinuityTime,
                         ospfv3RestartTime
                         }
         STATUS          current

         DESCRIPTION
             "These objects are used for managing/monitoring
             OSPFv3 global parameters."
         ::= { ospfv3Groups 1 }

 ospfv3AreaGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3AreaImportAsExtern,
                         ospfv3AreaSpfRuns,
                         ospfv3AreaBdrRtrCount,
                         ospfv3AreaAsBdrRtrCount,
                         ospfv3AreaScopeLsaCount,
                         ospfv3AreaScopeLsaCksumSum,
                         ospfv3AreaSummary,
                         ospfv3AreaRowStatus,
                         ospfv3AreaStubMetric,
                         ospfv3AreaNssaTranslatorRole,
                         ospfv3AreaNssaTranslatorState,
                         ospfv3AreaNssaTranslatorStabInterval,
                         ospfv3AreaNssaTranslatorEvents,
                         ospfv3AreaStubMetricType,
                         ospfv3AreaTEEnabled
                         }
         STATUS          current
         DESCRIPTION
             "These objects are used for OSPFv3 systems
             supporting areas."
         ::= { ospfv3Groups 2 }

 ospfv3AsLsdbGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3AsLsdbSequence,
                         ospfv3AsLsdbAge,
                         ospfv3AsLsdbChecksum,
                         ospfv3AsLsdbAdvertisement,
                         ospfv3AsLsdbTypeKnown
                         }
         STATUS          current
         DESCRIPTION
             "These objects are used for OSPFv3 systems
             that display their AS-scope link state database."
         ::= { ospfv3Groups 3 }

 ospfv3AreaLsdbGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3AreaLsdbSequence,
                         ospfv3AreaLsdbAge,
                         ospfv3AreaLsdbChecksum,

                         ospfv3AreaLsdbAdvertisement,
                         ospfv3AreaLsdbTypeKnown
                         }
         STATUS          current
         DESCRIPTION
             "These objects are used for OSPFv3 systems
             that display their Area-scope link state database."
         ::= { ospfv3Groups 4 }

 ospfv3LinkLsdbGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3LinkLsdbSequence,
                         ospfv3LinkLsdbAge,
                         ospfv3LinkLsdbChecksum,
                         ospfv3LinkLsdbAdvertisement,
                         ospfv3LinkLsdbTypeKnown
                         }
         STATUS          current
         DESCRIPTION
             "These objects are used for OSPFv3 systems
             that display their Link-scope link state database
             for non-virtual interfaces."
         ::= { ospfv3Groups 5 }

 ospfv3HostGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3HostMetric,
                         ospfv3HostRowStatus,
                         ospfv3HostAreaID
                         }
         STATUS          current
         DESCRIPTION
             "These objects are used for OSPFv3 systems
             that support attached hosts."
         ::= { ospfv3Groups 6 }

 ospfv3IfGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3IfAreaId,
                         ospfv3IfType,
                         ospfv3IfAdminStatus,
                         ospfv3IfRtrPriority,
                         ospfv3IfTransitDelay,
                         ospfv3IfRetransInterval,
                         ospfv3IfHelloInterval,
                         ospfv3IfRtrDeadInterval,
                         ospfv3IfPollInterval,
                         ospfv3IfState,

                         ospfv3IfDesignatedRouter,
                         ospfv3IfBackupDesignatedRouter,
                         ospfv3IfEvents,
                         ospfv3IfRowStatus,
                         ospfv3IfDemand,
                         ospfv3IfMetricValue,
                         ospfv3IfLinkScopeLsaCount,
                         ospfv3IfLinkLsaCksumSum,
                         ospfv3IfDemandNbrProbe,
                         ospfv3IfDemandNbrProbeRetransLimit,
                         ospfv3IfDemandNbrProbeInterval,
                         ospfv3IfTEDisabled,
                         ospfv3IfLinkLSASuppression
                         }
         STATUS          current
         DESCRIPTION
             "These interface objects are used for
             managing/monitoring OSPFv3 interfaces."
         ::= { ospfv3Groups 7 }

 ospfv3VirtIfGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3VirtIfIndex,
                         ospfv3VirtIfInstId,
                         ospfv3VirtIfTransitDelay,
                         ospfv3VirtIfRetransInterval,
                         ospfv3VirtIfHelloInterval,
                         ospfv3VirtIfRtrDeadInterval,
                         ospfv3VirtIfState,
                         ospfv3VirtIfEvents,
                         ospfv3VirtIfRowStatus,
                         ospfv3VirtIfLinkScopeLsaCount,
                         ospfv3VirtIfLinkLsaCksumSum
                         }
         STATUS          current
         DESCRIPTION
             "These virtual interface objects are used for
             managing/monitoring OSPFv3 virtual interfaces."
         ::= { ospfv3Groups 8 }

 ospfv3NbrGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3NbrAddressType,
                         ospfv3NbrAddress,
                         ospfv3NbrOptions,
                         ospfv3NbrPriority,
                         ospfv3NbrState,
                         ospfv3NbrEvents,

                         ospfv3NbrLsRetransQLen,
                         ospfv3NbrHelloSuppressed,
                         ospfv3NbrIfId,
                         ospfv3NbrRestartHelperStatus,
                         ospfv3NbrRestartHelperAge,
                         ospfv3NbrRestartHelperExitReason
                         }
         STATUS          current
         DESCRIPTION
             "These neighbor objects are used for
             managing/monitoring OSPFv3 neighbors."
         ::= { ospfv3Groups 9 }

 ospfv3CfgNbrGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3CfgNbrPriority,
                         ospfv3CfgNbrRowStatus
                         }
         STATUS          current
         DESCRIPTION
             "These configured neighbor objects are used for
             managing/monitoring OSPFv3-configured neighbors."
         ::= { ospfv3Groups 10 }

 ospfv3VirtNbrGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3VirtNbrIfIndex,
                         ospfv3VirtNbrIfInstId,
                         ospfv3VirtNbrAddressType,
                         ospfv3VirtNbrAddress,
                         ospfv3VirtNbrOptions,
                         ospfv3VirtNbrState,
                         ospfv3VirtNbrEvents,
                         ospfv3VirtNbrLsRetransQLen,
                         ospfv3VirtNbrHelloSuppressed,
                         ospfv3VirtNbrIfId,
                         ospfv3VirtNbrRestartHelperStatus,
                         ospfv3VirtNbrRestartHelperAge,
                         ospfv3VirtNbrRestartHelperExitReason
                         }
         STATUS          current
         DESCRIPTION
             "These virtual neighbor objects are used for
             managing/monitoring OSPFv3 virtual neighbors."
         ::= { ospfv3Groups 11 }

 ospfv3AreaAggregateGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3AreaAggregateRowStatus,
                         ospfv3AreaAggregateEffect,
                         ospfv3AreaAggregateRouteTag
                         }
         STATUS          current
         DESCRIPTION
             "These area aggregate objects are required for
             aggregating OSPFv3 prefixes for summarization
             across areas."
         ::= { ospfv3Groups 12 }

 ospfv3VirtLinkLsdbGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3VirtLinkLsdbSequence,
                         ospfv3VirtLinkLsdbAge,
                         ospfv3VirtLinkLsdbChecksum,
                         ospfv3VirtLinkLsdbAdvertisement,
                         ospfv3VirtLinkLsdbTypeKnown
                         }
         STATUS          current
         DESCRIPTION
             "These objects are used for OSPFv3 systems
             that display their Link-scope link state database
             for virtual interfaces."
         ::= { ospfv3Groups 13 }

 ospfv3NotificationObjectGroup OBJECT-GROUP
         OBJECTS         {
                         ospfv3ConfigErrorType,
                         ospfv3PacketType,
                         ospfv3PacketSrc
                         }
         STATUS          current
         DESCRIPTION
             "These objects are used to record notification
             parameters."
         ::= { ospfv3Groups 14 }

 ospfv3NotificationGroup NOTIFICATION-GROUP
         NOTIFICATIONS   {
                         ospfv3VirtIfStateChange,
                         ospfv3NbrStateChange,
                         ospfv3VirtNbrStateChange,
                         ospfv3IfConfigError,
                         ospfv3VirtIfConfigError,
                         ospfv3IfRxBadPacket,

                         ospfv3VirtIfRxBadPacket,
                         ospfv3LsdbOverflow,
                         ospfv3LsdbApproachingOverflow,
                         ospfv3IfStateChange,
                         ospfv3NssaTranslatorStatusChange,
                         ospfv3RestartStatusChange,
                         ospfv3NbrRestartHelperStatusChange,
                         ospfv3VirtNbrRestartHelperStatusChange
                         }
         STATUS          current
         DESCRIPTION
             "This group is used for OSPFv3 notifications."
         ::= { ospfv3Groups 15 }

 END


