-- *****************************************************************
-- RSVP-MIB.my 
--
-- Nov 2008, Smruti Biswal
--
-- Copyright (c) 2008-2009 by cisco Systems, Inc.
-- All rights reserved.
--
-- *****************************************************************
RSVP-MIB DEFINITIONS ::= BEGIN

	IMPORTS
		MODULE-IDENTITY, OBJECT-TYPE, Gauge32,
		NOTIFICATION-TYPE, Integer32, mib-2
						    FROM SNMPv2-SMI
		TEXTUAL-CONVENTION, TruthValue,	RowStatus,
		TimeStamp, TestAndIncr,	TimeInterval
						    FROM SNMPv2-TC
		MODULE-COMPLIANCE, OBJECT-GROUP,
		NOTIFICATION-GROUP		    FROM SNMPv2-CONF
		Port, SessionNumber, SessionType,
		Protocol, QosService, intSrvFlowStatus,
		MessageSize, BitRate, BurstSize	    FROM INTEGRATED-SERVICES-MIB
		ifIndex, InterfaceIndex		    FROM IF-MIB;




    rsvp MODULE-IDENTITY
	    LAST-UPDATED "9808251820Z" -- Tue Aug 25 13:13:14 PDT 1998
	    ORGANIZATION "IETF RSVP Working Group"
	    CONTACT-INFO
	   "	   Fred	Baker
	   Postal: Cisco Systems
		   519 Lado Drive
		   Santa Barbara, California 93111
	   Tel:	   +1 805 681 0115
	   E-Mail: fred@cisco.com

		   John	Krawczyk
	   Postal: ArrowPoint Communications
		   235 Littleton Road
		   Westford, Massachusetts 01886
	   Tel:	   +1 508 692 5875
	   E-Mail: jjk@tiac.net

		   Arun	Sastry
	   Postal: Cisco Systems
		   3 The Square
		   Stockley Park, Uxbridge
		   Middlesex, UB11 1BN
		   UK
	   Tel:	   +44 181 756 8693
	   E-Mail: arun@cisco.com"
       DESCRIPTION
	  "The MIB module to describe the RSVP Protocol"
      ::= { mib-2 51 }

  rsvpObjects		    OBJECT IDENTIFIER ::= { rsvp 1 } --	tables
  rsvpGenObjects	    OBJECT IDENTIFIER ::= { rsvp 2 } --	global objects
  rsvpNotificationsPrefix   OBJECT IDENTIFIER ::= { rsvp 3 } --	traps
  rsvpConformance	    OBJECT IDENTIFIER ::= { rsvp 4 } --	conformance



    RsvpEncapsulation ::= TEXTUAL-CONVENTION
	 STATUS	  current
	 DESCRIPTION
	   "This indicates the encapsulation that an  RSVP
	   Neighbor is perceived to be using."
	SYNTAX	 INTEGER {
		   ip (1),   --	IP Protocol 46
		   udp (2),  --	UDP Encapsulation
		   both	(3)  --	neighbor is using both encapsulations
		 }


    RefreshInterval ::=	TEXTUAL-CONVENTION
	 DISPLAY-HINT "d"
	 STATUS	  current
	 DESCRIPTION
	   "The	number of milliseconds that  are  expected
	   to	elapse	 between   refreshes  of  path	or
	   reservation	 state.	   Unrefreshed	 Path	or
	   reservation	state  is  removed  after  a small
	   multiple of this period."
	SYNTAX	 INTEGER (0..'7FFFFFFF'h)


--	The RSVP Session Statistics Database displays statistics
--	relating to the	number of senders and receivers	in each
--	session.


    rsvpSessionNewIndex	OBJECT-TYPE
	SYNTAX	    TestAndIncr
	MAX-ACCESS  read-write
	STATUS	    current
	DESCRIPTION
	   "This  object  is  used  to	assign	values	to
	   rsvpSessionNumber   as  described  in  'Textual
	   Conventions for SNMPv2'.  The  network  manager
	   reads  the  object,	and  then writes the value
	   back	in the SET that	creates	a new instance	of
	   rsvpSessionEntry.   If  the	SET fails with the
	   code	'inconsistentValue', then the process must
	   be  repeated;  If  the  SET	succeeds, then the
	   object is incremented, and the new instance	is
	   created according to	the manager's directions."
       ::= { rsvpGenObjects 5 }


    rsvpSessionTable OBJECT-TYPE
	SYNTAX	    SEQUENCE OF	RsvpSessionEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "A table  of	 all  sessions	seen  by  a  given
	   system."
       ::= { rsvpObjects 1 }


    rsvpSessionEntry OBJECT-TYPE
	SYNTAX	    RsvpSessionEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "A single session seen by a given system."
       INDEX { rsvpSessionNumber }
       ::= { rsvpSessionTable 1	}


    RsvpSessionEntry ::=
	SEQUENCE {
	rsvpSessionNumber	    SessionNumber,
	rsvpSessionType		    SessionType,
	rsvpSessionDestAddr	    OCTET STRING,
	rsvpSessionDestAddrLength   INTEGER,
	rsvpSessionProtocol	    Protocol,
	rsvpSessionPort		    Port,
	rsvpSessionSenders	    Gauge32,
	rsvpSessionReceivers	    Gauge32,
	rsvpSessionRequests	    Gauge32
	}


    rsvpSessionNumber OBJECT-TYPE
	SYNTAX	    SessionNumber
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "The	number of this session.	 This is for  SNMP
	   Indexing  purposes  only and	has no relation	to
	   any protocol	value."
       ::= { rsvpSessionEntry 1	}


    rsvpSessionType OBJECT-TYPE
	SYNTAX	    SessionType
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	type of	session	(IP4, IP6, IP6	with  flow
	   information,	etc)."
       ::= { rsvpSessionEntry 2	}


    rsvpSessionDestAddr	OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(4..16))
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	destination address used by all	senders	in
	   this	 session.   This object	may not	be changed
	   when	the  value  of	the  RowStatus	object	is
	   'active'."
       ::= { rsvpSessionEntry 3	}


    rsvpSessionDestAddrLength OBJECT-TYPE
	SYNTAX	    INTEGER(0..128)
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	CIDR prefix length of the session address,
	   which   is	32  for	 IP4  host  and	 multicast
	   addresses, and 128  for  IP6	 addresses.   This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpSessionEntry 4	}


    rsvpSessionProtocol	OBJECT-TYPE
	SYNTAX	    Protocol
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	IP Protocol used by  this  session.   This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpSessionEntry 5	}


    rsvpSessionPort OBJECT-TYPE
	SYNTAX	    Port
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	 UDP  or  TCP  port  number  used   as	 a
	   destination	 port  for  all	 senders  in  this
	   session.  If	the IP protocol	in use,	 specified
	   by  rsvpSenderProtocol, is 50 (ESP) or 51 (AH),
	   this	 represents  a	virtual	 destination  port
	   number.   A value of	zero indicates that the	IP
	   protocol in use  does  not  have  ports.   This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpSessionEntry 6	}


    rsvpSessionSenders OBJECT-TYPE
	SYNTAX	    Gauge32
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	number of distinct senders currently known
	   to be part of this session."
       ::= { rsvpSessionEntry 7	}


    rsvpSessionReceivers OBJECT-TYPE
	SYNTAX	    Gauge32
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	number of reservations being requested	of
	   this	system for this	session."
       ::= { rsvpSessionEntry 8	}

    rsvpSessionRequests	OBJECT-TYPE
	SYNTAX	    Gauge32
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	number of reservation requests this system
	   is sending upstream for this	session."
       ::= { rsvpSessionEntry 9	}
    
    rsvpBadPackets OBJECT-TYPE
	SYNTAX	    Gauge32
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "This object	keeps a	count of the number of bad
	   RSVP	packets	received."
       ::= { rsvpGenObjects 1 }


--	The RSVP Session Sender	Database contains the information
--	displayed by senders regarding their potential contribution
--	to session data	content. It is in essence a list of the
--	valid PATH messages that the RSVP Router or Host is receiving.


    rsvpSenderNewIndex OBJECT-TYPE
	SYNTAX	    TestAndIncr
	MAX-ACCESS  read-write
	STATUS	    current
	DESCRIPTION
	   "This  object  is  used  to	assign	values	to
	   rsvpSenderNumber   as   described  in  'Textual
	   Conventions for SNMPv2'.  The  network  manager
	   reads  the  object,	and  then writes the value
	   back	in the SET that	creates	a new instance	of
	   rsvpSenderEntry.   If  the  SET  fails with the
	   code	'inconsistentValue', then the process must
	   be  repeated;  If  the  SET	succeeds, then the
	   object is incremented, and the new instance	is
	   created according to	the manager's directions."
       ::= { rsvpGenObjects 2 }


    rsvpSenderTable OBJECT-TYPE
	SYNTAX	    SEQUENCE OF	RsvpSenderEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "Information	describing the	state  information
	   displayed by	senders	in PATH	messages."
       ::= { rsvpObjects 2 }


    rsvpSenderEntry OBJECT-TYPE
	SYNTAX	    RsvpSenderEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "Information	describing the	state  information
	   displayed by	a single sender's PATH message."
       INDEX { rsvpSessionNumber, rsvpSenderNumber }
       ::= { rsvpSenderTable 1 }

RsvpSenderEntry	::=

    SEQUENCE {
	rsvpSenderNumber			SessionNumber,
	rsvpSenderType				SessionType,
	rsvpSenderDestAddr			OCTET STRING,
	rsvpSenderAddr				OCTET STRING,
	rsvpSenderDestAddrLength		INTEGER,
	rsvpSenderAddrLength			INTEGER,
	rsvpSenderProtocol			Protocol,
	rsvpSenderDestPort			Port,
	rsvpSenderPort				Port,
	rsvpSenderFlowId			INTEGER,
	rsvpSenderHopAddr			OCTET STRING,
	rsvpSenderHopLih			Integer32,
	rsvpSenderInterface			InterfaceIndex,
	rsvpSenderTSpecRate			BitRate,
	rsvpSenderTSpecPeakRate			BitRate,
	rsvpSenderTSpecBurst			BurstSize,
	rsvpSenderTSpecMinTU			MessageSize,
	rsvpSenderTSpecMaxTU			MessageSize,
	rsvpSenderInterval			RefreshInterval,
	rsvpSenderRSVPHop			TruthValue,
	rsvpSenderLastChange			TimeStamp,
	rsvpSenderPolicy			OCTET STRING,
	rsvpSenderAdspecBreak			TruthValue,
	rsvpSenderAdspecHopCount		INTEGER,
	rsvpSenderAdspecPathBw			BitRate,
	rsvpSenderAdspecMinLatency		Integer32,
	rsvpSenderAdspecMtu			INTEGER,
	rsvpSenderAdspecGuaranteedSvc		TruthValue,
	rsvpSenderAdspecGuaranteedBreak		TruthValue,
	rsvpSenderAdspecGuaranteedCtot		Integer32,
	rsvpSenderAdspecGuaranteedDtot		Integer32,
	rsvpSenderAdspecGuaranteedCsum		Integer32,
	rsvpSenderAdspecGuaranteedDsum		Integer32,
	rsvpSenderAdspecGuaranteedHopCount	INTEGER,
	rsvpSenderAdspecGuaranteedPathBw	BitRate,
	rsvpSenderAdspecGuaranteedMinLatency	Integer32,
	rsvpSenderAdspecGuaranteedMtu		INTEGER,
	rsvpSenderAdspecCtrlLoadSvc		TruthValue,
	rsvpSenderAdspecCtrlLoadBreak		TruthValue,
	rsvpSenderAdspecCtrlLoadHopCount	INTEGER,
	rsvpSenderAdspecCtrlLoadPathBw		BitRate,
	rsvpSenderAdspecCtrlLoadMinLatency	Integer32,
	rsvpSenderAdspecCtrlLoadMtu		INTEGER,
	rsvpSenderStatus			RowStatus,
        rsvpSenderTTL			        INTEGER
    }

    rsvpSenderNumber OBJECT-TYPE
	SYNTAX	    SessionNumber
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "The	number of this sender.	This is	 for  SNMP
	   Indexing  purposes  only and	has no relation	to
	   any protocol	value."
       ::= { rsvpSenderEntry 1 }


    rsvpSenderType OBJECT-TYPE
	SYNTAX	    SessionType
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	type of	session	(IP4, IP6, IP6	with  flow
	   information,	etc)."
       ::= { rsvpSenderEntry 2 }


    rsvpSenderDestAddr OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(4..16))
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	destination address used by all	senders	in
	   this	 session.   This object	may not	be changed
	   when	the  value  of	the  RowStatus	object	is
	   'active'."
       ::= { rsvpSenderEntry 3 }


    rsvpSenderAddr OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(4..16))
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	source address used by this sender in this
	   session.   This  object may not be changed when
	   the value of	the RowStatus object is	'active'."
       ::= { rsvpSenderEntry 4 }


    rsvpSenderDestAddrLength OBJECT-TYPE
	SYNTAX	    INTEGER(0..128)
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	length of the destination address in bits.
	   This	 is  the CIDR Prefix Length, which for IP4
	   hosts and multicast addresses is 32 bits.  This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpSenderEntry 5 }


    rsvpSenderAddrLength OBJECT-TYPE
	SYNTAX	    INTEGER(0..128)
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	length of the sender's	address	 in  bits.
	   This	 is  the CIDR Prefix Length, which for IP4
	   hosts and multicast addresses is 32 bits.  This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpSenderEntry 6 }


    rsvpSenderProtocol OBJECT-TYPE
	SYNTAX	    Protocol
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	IP Protocol used by  this  session.   This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpSenderEntry 7 }


    rsvpSenderDestPort OBJECT-TYPE
	SYNTAX	    Port
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	 UDP  or  TCP  port  number  used   as	 a
	   destination	 port  for  all	 senders  in  this
	   session.  If	the IP protocol	in use,	 specified
	   by  rsvpSenderProtocol, is 50 (ESP) or 51 (AH),
	   this	 represents  a	virtual	 destination  port
	   number.   A value of	zero indicates that the	IP
	   protocol in use  does  not  have  ports.   This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpSenderEntry 8 }


    rsvpSenderPort OBJECT-TYPE
	SYNTAX	    Port
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	UDP or TCP port	number used  as	 a  source
	   port	 for  this sender in this session.  If the
	   IP	 protocol    in	   use,	   specified	by
	   rsvpSenderProtocol is 50 (ESP) or 51	(AH), this
	   represents a	generalized port identifier (GPI).
	   A  value of zero indicates that the IP protocol
	   in use does not have	ports.	 This  object  may
	   not	be changed when	the value of the RowStatus
	   object is 'active'."
       ::= { rsvpSenderEntry 9 }


    rsvpSenderFlowId OBJECT-TYPE
	SYNTAX	    INTEGER (0..16777215)
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	flow ID	that  this  sender  is	using,	if
	   this	 is  an	IPv6 session."
       ::= { rsvpSenderEntry 10	}


    rsvpSenderHopAddr OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(4..16))
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	address	used  by  the  previous	 RSVP  hop
	   (which may be the original sender)."
       ::= { rsvpSenderEntry 11	}


    rsvpSenderHopLih OBJECT-TYPE
	SYNTAX	    Integer32
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	 Logical  Interface  Handle  used  by  the
	   previous  RSVP  hop	(which may be the original
	   sender)."
       ::= { rsvpSenderEntry 12	}


    rsvpSenderInterface	OBJECT-TYPE
	SYNTAX	    InterfaceIndex
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	ifIndex	value of the  interface	 on  which
	   this	PATH message was most recently received."
       ::= { rsvpSenderEntry 13	}


    rsvpSenderTSpecRate	OBJECT-TYPE
	SYNTAX	    BitRate
	UNITS	    "bits per second"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	Average	Bit  Rate  of  the  sender's  data
	   stream.    Within  a	 transmission  burst,  the
	   arrival   rate    may    be	  as	fast	as
	   rsvpSenderTSpecPeakRate  (if	 supported  by the
	   service model); however, averaged across two	or
	   more	 burst	intervals,  the	 rate  should  not
	   exceed rsvpSenderTSpecRate.

	   Note	that this is a prediction, often based	on
	   the	general	 capability  of	a type of codec	or
	   particular encoding;	the measured average  rate
	   may be significantly	lower."
       ::= { rsvpSenderEntry 14	}


    rsvpSenderTSpecPeakRate OBJECT-TYPE
	SYNTAX	    BitRate
	UNITS	    "bits per second"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	Peak Bit Rate of the sender's data stream.
	   Traffic  arrival is not expected to exceed this
	   rate	at any time, apart  from  the  effects	of
	   jitter in the network.  If not specified in the
	   TSpec, this returns zero or noSuchValue."
       ::= { rsvpSenderEntry 15	}


    rsvpSenderTSpecBurst OBJECT-TYPE
	SYNTAX	    BurstSize
	UNITS	    "bytes"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	size of	the largest  burst  expected  from
	   the sender at a time."
       ::= { rsvpSenderEntry 16	}


    rsvpSenderTSpecMinTU OBJECT-TYPE
	SYNTAX	    MessageSize
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	minimum	message	size for  this	flow.  The
	   policing  algorithm will treat smaller messages
	   as though they are this size."
       ::= { rsvpSenderEntry 17	}


    rsvpSenderTSpecMaxTU OBJECT-TYPE
	SYNTAX	    MessageSize
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	maximum	message	size for  this	flow.  The
	   admission  algorithm	 will  reject TSpecs whose
	   Maximum Transmission	Unit, plus  the	 interface
	   headers, exceed the interface MTU."
       ::= { rsvpSenderEntry 18	}


    rsvpSenderInterval OBJECT-TYPE
	SYNTAX	    RefreshInterval
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	 interval  between  refresh  messages	as
	   advertised by the Previous Hop."
       ::= { rsvpSenderEntry 19	}


    rsvpSenderRSVPHop OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If TRUE, the node believes that  the  previous
	   IP  hop  is	an  RSVP  hop.	If FALSE, the node
	   believes that the previous IP hop may not be	an
	   RSVP	hop."
       ::= { rsvpSenderEntry 20	}


    rsvpSenderLastChange OBJECT-TYPE
	SYNTAX	    TimeStamp
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	time of	 the  last  change  in	this  PATH
	   message;  This  is either the first time it was
	   received or the time	of the most recent  change
	   in parameters."
       ::= { rsvpSenderEntry 21	}


    rsvpSenderPolicy OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(4..65536))
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	contents of the	policy	object,	 displayed
	   as an uninterpreted string of octets, including
	   the object header.  In the absence of  such	an
	   object, this	should be of zero length."
       ::= { rsvpSenderEntry 22	}


    rsvpSenderAdspecBreak OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	global break bit general  characterization
	   parameter  from  the	ADSPEC.	 If TRUE, at least
	   one non-IS hop was detected in  the	path.	If
	   FALSE, no non-IS hops were detected."
       ::= { rsvpSenderEntry 23	}


    rsvpSenderAdspecHopCount OBJECT-TYPE
	SYNTAX	    INTEGER (0..65535)
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	  hop	count	general	  characterization
	   parameter from the ADSPEC.  A return	of zero	or
	   noSuchValue	indicates  one	of  the	 following
	   conditions:

	      the invalid bit was set
	      the parameter was	not present"
       ::= { rsvpSenderEntry 24	}


    rsvpSenderAdspecPathBw OBJECT-TYPE
	SYNTAX	    BitRate
	UNITS	    "bits per second"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	  path	  bandwidth    estimate	   general
	   characterization  parameter from the	ADSPEC.	 A
	   return of zero or noSuchValue indicates one	of
	   the following conditions:

	      the invalid bit was set
	      the parameter was	not present"
       ::= { rsvpSenderEntry 25	}


    rsvpSenderAdspecMinLatency OBJECT-TYPE
	SYNTAX	    Integer32
	UNITS	    "microseconds"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	   minimum    path     latency	   general
	   characterization  parameter from the	ADSPEC.	 A
	   return of zero or noSuchValue indicates one	of
	   the following conditions:

	      the invalid bit was set
	      the parameter was	not present"
       ::= { rsvpSenderEntry 26	}


    rsvpSenderAdspecMtu	OBJECT-TYPE
	SYNTAX	    INTEGER (0..65535)
	UNITS	    "bytes"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	composed Maximum Transmission Unit general
	   characterization  parameter from the	ADSPEC.	 A
	   return of zero or noSuchValue indicates one	of
	   the following conditions:

	      the invalid bit was set
	      the parameter was	not present"
       ::= { rsvpSenderEntry 27	}


    rsvpSenderAdspecGuaranteedSvc OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If TRUE,  the  ADSPEC  contains  a	Guaranteed
	   Service  fragment.	If  FALSE, the ADSPEC does
	   not contain a Guaranteed Service fragment."
       ::= { rsvpSenderEntry 28	}


    rsvpSenderAdspecGuaranteedBreak OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If TRUE, the Guaranteed Service  fragment  has
	   its	'break'	 bit  set,  indicating that one	or
	   more	nodes along the	path do	 not  support  the
	   guaranteed	  service.     If    FALSE,    and
	   rsvpSenderAdspecGuaranteedSvc  is   TRUE,   the
	   'break' bit is not set.

	   If rsvpSenderAdspecGuaranteedSvc is FALSE, this
	   returns FALSE or noSuchValue."
       ::= { rsvpSenderEntry 29	}


    rsvpSenderAdspecGuaranteedCtot OBJECT-TYPE
	SYNTAX	    Integer32
	UNITS	    "bytes"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION

	   "If rsvpSenderAdspecGuaranteedSvc is	TRUE, this
	   is	the  end-to-end	 composed  value  for  the
	   guaranteed service 'C' parameter.  A	return	of
	   zero	  or  noSuchValue  indicates  one  of  the
	   following conditions:

	      the invalid bit was set
	      the parameter was	not present

	   If rsvpSenderAdspecGuaranteedSvc is FALSE, this
	   returns zero	or noSuchValue."
       ::= { rsvpSenderEntry 30	}


    rsvpSenderAdspecGuaranteedDtot OBJECT-TYPE
	SYNTAX	    Integer32
	UNITS	    "microseconds"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If rsvpSenderAdspecGuaranteedSvc is	TRUE, this
	   is	the  end-to-end	 composed  value  for  the
	   guaranteed service 'D' parameter.  A	return	of
	   zero	  or  noSuchValue  indicates  one  of  the
	   following conditions:

	      the invalid bit was set
	      the parameter was	not present

	   If rsvpSenderAdspecGuaranteedSvc is FALSE, this
	   returns zero	or noSuchValue."
       ::= { rsvpSenderEntry 31	}


    rsvpSenderAdspecGuaranteedCsum OBJECT-TYPE
	SYNTAX	    Integer32
	UNITS	    "bytes"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If rsvpSenderAdspecGuaranteedSvc is	TRUE, this
	   is	the  composed  value  for  the	guaranteed
	   service 'C' parameter since the last	 reshaping
	   point.    A	 return	 of  zero  or  noSuchValue
	   indicates one of the	following conditions:

	      the invalid bit was set
	      the parameter was	not present

	   If rsvpSenderAdspecGuaranteedSvc is FALSE, this
	   returns zero	or noSuchValue."
       ::= { rsvpSenderEntry 32	}


    rsvpSenderAdspecGuaranteedDsum OBJECT-TYPE
	SYNTAX	    Integer32
	UNITS	    "microseconds"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If rsvpSenderAdspecGuaranteedSvc is	TRUE, this
	   is	the  composed  value  for  the	guaranteed
	   service 'D' parameter since the last	 reshaping
	   point.    A	 return	 of  zero  or  noSuchValue
	   indicates one of the	following conditions:

	      the invalid bit was set
	      the parameter was	not present

	   If rsvpSenderAdspecGuaranteedSvc is FALSE, this
	   returns zero	or noSuchValue."
       ::= { rsvpSenderEntry 33	}


    rsvpSenderAdspecGuaranteedHopCount OBJECT-TYPE
	SYNTAX	    INTEGER (0..65535)
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION

	   "If rsvpSenderAdspecGuaranteedSvc is	TRUE, this
	   is  the  service-specific  override	of the hop
	   count general characterization  parameter  from
	   the	ADSPEC.	  A  return of zero or noSuchValue
	   indicates one of the	following conditions:

	      the invalid bit was set
	      the parameter was	not present

	   If rsvpSenderAdspecGuaranteedSvc is FALSE, this
	   returns zero	or noSuchValue."
       ::= { rsvpSenderEntry 34	}

    rsvpSenderAdspecGuaranteedPathBw OBJECT-TYPE
	SYNTAX	    BitRate
	UNITS	    "bits per second"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If rsvpSenderAdspecGuaranteedSvc is	TRUE, this
	   is  the  service-specific  override of the path
	   bandwidth  estimate	general	  characterization
	   parameter from the ADSPEC.  A return	of zero	or
	   noSuchValue	indicates  one	of  the	 following
	   conditions:

	      the invalid bit was set
	      the parameter was	not present

	   If rsvpSenderAdspecGuaranteedSvc is FALSE, this
	   returns zero	or noSuchValue."
       ::= { rsvpSenderEntry 35	}


    rsvpSenderAdspecGuaranteedMinLatency OBJECT-TYPE
	SYNTAX	    Integer32
	UNITS	    "microseconds"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If rsvpSenderAdspecGuaranteedSvc is	TRUE, this
	   is the service-specific override of the minimum
	   path	latency	general	characterization parameter
	   from	  the	ADSPEC.	   A  return  of  zero	or
	   noSuchValue	indicates  one	of  the	 following
	   conditions:

	      the invalid bit was set
	      the parameter was	not present

	   If rsvpSenderAdspecGuaranteedSvc is FALSE, this
	   returns zero	or noSuchValue."
       ::= { rsvpSenderEntry 36	}


    rsvpSenderAdspecGuaranteedMtu OBJECT-TYPE
	SYNTAX	    INTEGER (0..65535)
	UNITS	    "bytes"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If rsvpSenderAdspecGuaranteedSvc is	TRUE, this
	   is	the   service-specific	 override  of  the
	   composed  Maximum  Transmission  Unit   general
	   characterization  parameter from the	ADSPEC.	 A
	   return of zero or noSuchValue indicates one	of
	   the following conditions:

	      the invalid bit was set
	      the parameter was	not present

	   If rsvpSenderAdspecGuaranteedSvc is FALSE, this
	   returns zero	or noSuchValue."
       ::= { rsvpSenderEntry 37	}


    rsvpSenderAdspecCtrlLoadSvc	OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If TRUE, the ADSPEC	contains a Controlled Load
	   Service  fragment.	If  FALSE, the ADSPEC does
	   not	 contain   a   Controlled   Load   Service
	   fragment."
       ::= { rsvpSenderEntry 38	}


    rsvpSenderAdspecCtrlLoadBreak OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If TRUE, the Controlled Load Service  fragment
	   has its 'break' bit set, indicating that one	or
	   more	nodes along the	path do	 not  support  the
	   controlled	load   service.	   If  FALSE,  and
	   rsvpSenderAdspecCtrlLoadSvc	 is   TRUE,    the
	   'break' bit is not set.

	   If rsvpSenderAdspecCtrlLoadSvc is  FALSE,  this
	   returns FALSE or noSuchValue."
       ::= { rsvpSenderEntry 39	}


    rsvpSenderAdspecCtrlLoadHopCount OBJECT-TYPE
	SYNTAX	    INTEGER (0..65535)
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION

	   "If rsvpSenderAdspecCtrlLoadSvc is  TRUE,  this
	   is  the  service-specific  override	of the hop
	   count general characterization  parameter  from
	   the	ADSPEC.	  A  return of zero or noSuchValue
	   indicates one of the	following conditions:

	      the invalid bit was set
	      the parameter was	not present

	   If rsvpSenderAdspecCtrlLoadSvc is  FALSE,  this
	   returns zero	or noSuchValue."
       ::= { rsvpSenderEntry 40	}


    rsvpSenderAdspecCtrlLoadPathBw OBJECT-TYPE
	SYNTAX	    BitRate
	UNITS	    "bits per second"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If rsvpSenderAdspecCtrlLoadSvc is  TRUE,  this
	   is  the  service-specific  override of the path
	   bandwidth  estimate	general	  characterization
	   parameter from the ADSPEC.  A return	of zero	or
	   noSuchValue	indicates  one	of  the	 following
	   conditions:

	      the invalid bit was set
	      the parameter was	not present

	   If rsvpSenderAdspecCtrlLoadSvc is  FALSE,  this
	   returns zero	or noSuchValue."
       ::= { rsvpSenderEntry 41	}


    rsvpSenderAdspecCtrlLoadMinLatency OBJECT-TYPE
	SYNTAX	    Integer32
	UNITS	    "microseconds"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If rsvpSenderAdspecCtrlLoadSvc is  TRUE,  this
	   is the service-specific override of the minimum
	   path	latency	general	characterization parameter
	   from	  the	ADSPEC.	   A  return  of  zero	or
	   noSuchValue	indicates  one	of  the	 following
	   conditions:

	      the invalid bit was set
	      the parameter was	not present

	   If rsvpSenderAdspecCtrlLoadSvc is  FALSE,  this
	   returns zero	or noSuchValue."
       ::= { rsvpSenderEntry 42	}


    rsvpSenderAdspecCtrlLoadMtu	OBJECT-TYPE
	SYNTAX	    INTEGER (0..65535)
	UNITS	    "bytes"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If rsvpSenderAdspecCtrlLoadSvc is  TRUE,  this
	   is	the   service-specific	 override  of  the
	   composed  Maximum  Transmission  Unit   general
	   characterization  parameter from the	ADSPEC.	 A
	   return of zero or noSuchValue indicates one	of
	   the following conditions:

	      the invalid bit was set
	      the parameter was	not present

	   If rsvpSenderAdspecCtrlLoadSvc is  FALSE,  this
	   returns zero	or noSuchValue."
       ::= { rsvpSenderEntry 43	}


    rsvpSenderStatus OBJECT-TYPE
	SYNTAX	    RowStatus
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "'active' for all active PATH  messages.   This
	   object  may	be  used  to  install  static PATH
	   information or delete PATH information."
       ::= { rsvpSenderEntry 44	}


    rsvpSenderTTL OBJECT-TYPE
	SYNTAX	    INTEGER (0..255)
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	TTL value in the RSVP header that was last
	   received."
       ::= { rsvpSenderEntry 45	}


    rsvpSenderOutInterfaceTable	OBJECT-TYPE
	SYNTAX	    SEQUENCE OF	RsvpSenderOutInterfaceEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "List of outgoing interfaces	that PATH messages
	   use.	 The  ifIndex  is the ifIndex value of the
	   egress interface."
       ::= { rsvpObjects 3 }


    rsvpSenderOutInterfaceEntry	OBJECT-TYPE
	SYNTAX	    RsvpSenderOutInterfaceEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "List of outgoing interfaces	that a	particular
	   PATH	message	has."
       INDEX { rsvpSessionNumber, rsvpSenderNumber, ifIndex }
       ::= { rsvpSenderOutInterfaceTable 1 }

RsvpSenderOutInterfaceEntry ::=
    SEQUENCE {
	rsvpSenderOutInterfaceStatus		RowStatus
    }

    rsvpSenderOutInterfaceStatus OBJECT-TYPE
	SYNTAX	    RowStatus
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "'active' for all active PATH messages."
       ::= { rsvpSenderOutInterfaceEntry 1 }


--	The RSVP Reservation Requests Received Table contains the
--	information displayed by receivers regarding their needs with
--	respect	to sessions and	senders. It is in essence a list of the
--	valid RESV messages that the RSVP Router or Host is receiving.


    rsvpResvNewIndex OBJECT-TYPE
	SYNTAX	    TestAndIncr
	MAX-ACCESS  read-write
	STATUS	    current
	DESCRIPTION
	   "This  object  is  used  to	assign	values	to
	   rsvpResvNumber   as	 described   in	  'Textual
	   Conventions for SNMPv2'.  The  network  manager
	   reads  the  object,	and  then writes the value
	   back	in the SET that	creates	a new instance	of
	   rsvpResvEntry.   If the SET fails with the code
	   'inconsistentValue',	then the process  must	be
	   repeated;  If the SET succeeds, then	the object
	   is incremented, and the new instance	is created
	   according to	the manager's directions."
       ::= { rsvpGenObjects 3 }


    rsvpResvTable OBJECT-TYPE
	SYNTAX	    SEQUENCE OF	RsvpResvEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "Information	describing the	state  information
	   displayed by	receivers in RESV messages."
       ::= { rsvpObjects 4 }


    rsvpResvEntry OBJECT-TYPE
	SYNTAX	    RsvpResvEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "Information	describing the	state  information
	   displayed  by  a single receiver's RESV message
	   concerning a	single sender."
       INDEX { rsvpSessionNumber, rsvpResvNumber }
       ::= { rsvpResvTable 1 }


    RsvpResvEntry ::=
	SEQUENCE {
	    rsvpResvNumber		    SessionNumber,
	    rsvpResvType		    SessionType,
	    rsvpResvDestAddr		    OCTET STRING,
	    rsvpResvSenderAddr		    OCTET STRING,
	    rsvpResvDestAddrLength	    INTEGER,
	    rsvpResvSenderAddrLength	    INTEGER,
	    rsvpResvProtocol		    Protocol,
	    rsvpResvDestPort		    Port,
	    rsvpResvPort		    Port,
	    rsvpResvHopAddr		    OCTET STRING,
	    rsvpResvHopLih		    Integer32,
	    rsvpResvInterface		    InterfaceIndex,
	    rsvpResvService		    QosService,
	    rsvpResvTSpecRate		    BitRate,
	    rsvpResvTSpecPeakRate	    BitRate,
	    rsvpResvTSpecBurst		    BurstSize,
	    rsvpResvTSpecMinTU		    MessageSize,
	    rsvpResvTSpecMaxTU		    MessageSize,
	    rsvpResvRSpecRate		    BitRate,
	    rsvpResvRSpecSlack		    Integer32,
	    rsvpResvInterval		    RefreshInterval,
	    rsvpResvScope		    OCTET STRING,
	    rsvpResvShared		    TruthValue,
	    rsvpResvExplicit		    TruthValue,
	    rsvpResvRSVPHop		    TruthValue,
	    rsvpResvLastChange		    TimeStamp,
	    rsvpResvPolicy		    OCTET STRING,
	    rsvpResvStatus		    RowStatus,
	    rsvpResvTTL			    INTEGER,
	    rsvpResvFlowId		    INTEGER
	}


    rsvpResvNumber OBJECT-TYPE
	SYNTAX	    SessionNumber
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "The	number of this reservation request.   This
	   is  for  SNMP Indexing purposes only	and has	no
	   relation to any protocol value."
       ::= { rsvpResvEntry 1 }


    rsvpResvType OBJECT-TYPE
	SYNTAX	    SessionType
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	type of	session	(IP4, IP6, IP6	with  flow
	   information,	etc)."
       ::= { rsvpResvEntry 2 }


    rsvpResvDestAddr OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(4..16))
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	destination address used by all	senders	in
	   this	 session.   This object	may not	be changed
	   when	the  value  of	the  RowStatus	object	is
	   'active'."
       ::= { rsvpResvEntry 3 }


    rsvpResvSenderAddr OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(4..16))
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	source address of the sender  selected	by
	   this	 reservation.	The  value  of	all zeroes
	   indicates 'all senders'.  This object  may  not
	   be  changed	when  the  value  of the RowStatus
	   object is 'active'."
       ::= { rsvpResvEntry 4 }


    rsvpResvDestAddrLength OBJECT-TYPE
	SYNTAX	    INTEGER(0..128)
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	length of the destination address in bits.
	   This	 is  the CIDR Prefix Length, which for IP4
	   hosts and multicast addresses is 32 bits.  This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpResvEntry 5 }


    rsvpResvSenderAddrLength OBJECT-TYPE
	SYNTAX	    INTEGER(0..128)
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	length of the sender's	address	 in  bits.
	   This	 is  the CIDR Prefix Length, which for IP4
	   hosts and multicast addresses is 32 bits.  This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpResvEntry 6 }


    rsvpResvProtocol OBJECT-TYPE
	SYNTAX	    Protocol
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	IP Protocol used by  this  session.   This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpResvEntry 7 }


    rsvpResvDestPort OBJECT-TYPE
	SYNTAX	    Port
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	 UDP  or  TCP  port  number  used   as	 a
	   destination	 port  for  all	 senders  in  this
	   session.  If	the IP protocol	in use,	 specified
	   by  rsvpResvProtocol,  is  50 (ESP) or 51 (AH),
	   this	 represents  a	virtual	 destination  port
	   number.   A value of	zero indicates that the	IP
	   protocol in use  does  not  have  ports.   This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpResvEntry 8 }


    rsvpResvPort OBJECT-TYPE
	SYNTAX	    Port
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	UDP or TCP port	number used  as	 a  source
	   port	 for  this sender in this session.  If the
	   IP	 protocol    in	   use,	   specified	by
	   rsvpResvProtocol  is	 50 (ESP) or 51	(AH), this
	   represents a	generalized port identifier (GPI).
	   A  value of zero indicates that the IP protocol
	   in use does not have	ports.	 This  object  may
	   not	be changed when	the value of the RowStatus
	   object is 'active'."
       ::= { rsvpResvEntry 9 }


    rsvpResvHopAddr OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(4..16))
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	address	used by	the next RSVP  hop  (which
	   may be the ultimate receiver)."
       ::= { rsvpResvEntry 10 }


    rsvpResvHopLih OBJECT-TYPE
	SYNTAX	    Integer32
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	Logical	Interface Handle received from the
	   previous  RSVP  hop	(which may be the ultimate
	   receiver)."
       ::= { rsvpResvEntry 11 }


    rsvpResvInterface OBJECT-TYPE
	SYNTAX	    InterfaceIndex
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	ifIndex	value of the  interface	 on  which
	   this	RESV message was most recently received."
       ::= { rsvpResvEntry 12 }


    rsvpResvService OBJECT-TYPE
	SYNTAX	    QosService
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	QoS Service  classification  requested	by
	   the receiver."
       ::= { rsvpResvEntry 13 }


    rsvpResvTSpecRate OBJECT-TYPE
	SYNTAX	    BitRate
	UNITS	    "bits per second"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	Average	Bit  Rate  of  the  sender's  data
	   stream.    Within  a	 transmission  burst,  the
	   arrival   rate    may    be	  as	fast	as
	   rsvpResvTSpecPeakRate   (if	supported  by  the
	   service model); however, averaged across two	or
	   more	 burst	intervals,  the	 rate  should  not
	   exceed rsvpResvTSpecRate.

	   Note	that this is a prediction, often based	on
	   the	general	 capability  of	a type of codec	or
	   particular encoding;	the measured average  rate
	   may be significantly	lower."
       ::= { rsvpResvEntry 14 }


    rsvpResvTSpecPeakRate OBJECT-TYPE
	SYNTAX	    BitRate
	UNITS	    "bits per second"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	Peak Bit Rate of the sender's data stream.
	   Traffic  arrival is not expected to exceed this
	   rate	at any time, apart  from  the  effects	of
	   jitter in the network.  If not specified in the
	   TSpec, this returns zero or noSuchValue."
       ::= { rsvpResvEntry 15 }


    rsvpResvTSpecBurst OBJECT-TYPE
	SYNTAX	    BurstSize
	UNITS	    "bytes"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	size of	the largest  burst  expected  from
	   the sender at a time.

	   If this is less than	 the  sender's	advertised
	   burst  size,	the receiver is	asking the network
	   to provide flow pacing  beyond  what	 would	be
	   provided   under   normal  circumstances.  Such
	   pacing is at	the network's option."
       ::= { rsvpResvEntry 16 }


    rsvpResvTSpecMinTU OBJECT-TYPE
	SYNTAX	    MessageSize
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	minimum	message	size for  this	flow.  The
	   policing  algorithm will treat smaller messages
	   as though they are this size."
       ::= { rsvpResvEntry 17 }


    rsvpResvTSpecMaxTU OBJECT-TYPE
	SYNTAX	    MessageSize
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	maximum	message	size for  this	flow.  The
	   admission  algorithm	 will  reject TSpecs whose
	   Maximum Transmission	Unit, plus  the	 interface
	   headers, exceed the interface MTU."
       ::= { rsvpResvEntry 18 }


    rsvpResvRSpecRate OBJECT-TYPE
	SYNTAX	    BitRate
	UNITS	    "bits per second"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If the requested  service  is  Guaranteed,	as
	   specified   by  rsvpResvService,  this  is  the
	   clearing  rate   that   is	being	requested.
	   Otherwise,  it is zero, or the agent	may return
	   noSuchValue."
       ::= { rsvpResvEntry 19 }


    rsvpResvRSpecSlack OBJECT-TYPE
	SYNTAX	    Integer32
	UNITS	    "microseconds"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If the requested  service  is  Guaranteed,	as
	   specified by	rsvpResvService, this is the delay
	   slack.  Otherwise, it is zero, or the agent may
	   return noSuchValue."
       ::= { rsvpResvEntry 20 }


    rsvpResvInterval OBJECT-TYPE
	SYNTAX	    RefreshInterval
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	 interval  between  refresh  messages	as
	   advertised by the Next Hop."
       ::= { rsvpResvEntry 21 }


    rsvpResvScope OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(0..65536))
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION

	   "The	contents of the	scope object, displayed	as
	   an  uninterpreted  string  of octets, including
	   the object header.  In the absence of  such	an
	   object, this	should be of zero length.

	   If the length  is  non-zero,	 this  contains	 a
	   series of IP4 or IP6	addresses."
       ::= { rsvpResvEntry 22 }


    rsvpResvShared OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If TRUE, a reservation shared among	senders	is
	   requested.  If FALSE, a reservation specific	to
	   this	sender is requested."
       ::= { rsvpResvEntry 23 }


    rsvpResvExplicit OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If TRUE, individual	senders	are  listed  using
	   Filter  Specifications.   If	FALSE, all senders
	   are implicitly selected.  The Scope Object will
	   contain  a list of senders that need	to receive
	   this	reservation request  for  the  purpose	of
	   routing the RESV message."
       ::= { rsvpResvEntry 24 }


    rsvpResvRSVPHop OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If TRUE, the node believes that  the  previous
	   IP  hop  is	an  RSVP  hop.	If FALSE, the node
	   believes that the previous IP hop may not be	an
	   RSVP	hop."
       ::= { rsvpResvEntry 25 }


    rsvpResvLastChange OBJECT-TYPE
	SYNTAX	    TimeStamp
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	 time  of  the	 last	change	 in   this
	   reservation	request;  This is either the first
	   time	it was received	or the time  of	 the  most
	   recent change in parameters."
       ::= { rsvpResvEntry 26 }


    rsvpResvPolicy OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(0..65536))
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	contents of the	policy	object,	 displayed
	   as an uninterpreted string of octets, including
	   the object header.  In the absence of  such	an
	   object, this	should be of zero length."
       ::= { rsvpResvEntry 27 }


    rsvpResvStatus OBJECT-TYPE
	SYNTAX	    RowStatus
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "'active' for all active RESV  messages.   This
	   object  may	be  used  to  install  static RESV
	   information or delete RESV information."
       ::= { rsvpResvEntry 28 }


    rsvpResvTTL	OBJECT-TYPE
	SYNTAX	    INTEGER (0..255)
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	TTL value in the RSVP header that was last
	   received."
       ::= { rsvpResvEntry 29 }


    rsvpResvFlowId OBJECT-TYPE
	SYNTAX	    INTEGER (0..16777215)
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	flow ID	that this receiver  is	using,	if
	   this	 is  an	IPv6 session."
       ::= { rsvpResvEntry 30 }

--	The RSVP Reservation Requests Forwarded	Table contains the
--	information displayed by receivers regarding their needs with
--	respect	to sessions and	senders. It is in essence a list of the
--	valid RESV messages that the RSVP Router or Host is sending
--	to its upstream	neighbors.


    rsvpResvFwdNewIndex	OBJECT-TYPE
	SYNTAX	    TestAndIncr
	MAX-ACCESS  read-write
	STATUS	    current
	DESCRIPTION
	   "This  object  is  used  to	assign	values	to
	   rsvpResvFwdNumber   as  described  in  'Textual
	   Conventions for SNMPv2'.  The  network  manager
	   reads  the  object,	and  then writes the value
	   back	in the SET that	creates	a new instance	of
	   rsvpResvFwdEntry.   If  the	SET fails with the
	   code	'inconsistentValue', then the process must
	   be  repeated;  If  the  SET	succeeds, then the
	   object is incremented, and the new instance	is
	   created according to	the manager's directions."
       ::= { rsvpGenObjects 4 }


    rsvpResvFwdTable OBJECT-TYPE
	SYNTAX	    SEQUENCE OF	RsvpResvFwdEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "Information	describing the	state  information
	   displayed upstream in RESV messages."
       ::= { rsvpObjects 5 }


    rsvpResvFwdEntry OBJECT-TYPE
	SYNTAX	    RsvpResvFwdEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "Information	describing the	state  information
	   displayed   upstream	  in   an   RESV   message
	   concerning a	single sender."
       INDEX { rsvpSessionNumber, rsvpResvFwdNumber }
       ::= { rsvpResvFwdTable 1	}



    RsvpResvFwdEntry ::=
	SEQUENCE {
	    rsvpResvFwdNumber		    SessionNumber,
	    rsvpResvFwdType		    SessionType,
	    rsvpResvFwdDestAddr		    OCTET STRING,
	    rsvpResvFwdSenderAddr	    OCTET STRING,
	    rsvpResvFwdDestAddrLength	    INTEGER,
	    rsvpResvFwdSenderAddrLength	    INTEGER,
	    rsvpResvFwdProtocol		    Protocol,
	    rsvpResvFwdDestPort		    Port,
	    rsvpResvFwdPort		    Port,
	    rsvpResvFwdHopAddr		    OCTET STRING,
	    rsvpResvFwdHopLih		    Integer32,
	    rsvpResvFwdInterface	    InterfaceIndex,
	    rsvpResvFwdService		    QosService,
	    rsvpResvFwdTSpecRate	    BitRate,
	    rsvpResvFwdTSpecPeakRate	    BitRate,
	    rsvpResvFwdTSpecBurst	    BurstSize,
	    rsvpResvFwdTSpecMinTU	    MessageSize,
	    rsvpResvFwdTSpecMaxTU	    MessageSize,
	    rsvpResvFwdRSpecRate	    BitRate,
	    rsvpResvFwdRSpecSlack	    Integer32,
	    rsvpResvFwdInterval		    RefreshInterval,
	    rsvpResvFwdScope		    OCTET STRING,
	    rsvpResvFwdShared		    TruthValue,
	    rsvpResvFwdExplicit		    TruthValue,
	    rsvpResvFwdRSVPHop		    TruthValue,
	    rsvpResvFwdLastChange	    TimeStamp,
	    rsvpResvFwdPolicy		    OCTET STRING,
	    rsvpResvFwdStatus		    RowStatus,
	    rsvpResvFwdTTL		    INTEGER,
	    rsvpResvFwdFlowId		    INTEGER
	}


    rsvpResvFwdNumber OBJECT-TYPE
	SYNTAX	    SessionNumber
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "The	number of this reservation request.   This
	   is  for  SNMP Indexing purposes only	and has	no
	   relation to any protocol value."
       ::= { rsvpResvFwdEntry 1	}


    rsvpResvFwdType OBJECT-TYPE
	SYNTAX	    SessionType
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	type of	session	(IP4, IP6, IP6	with  flow
	   information,	etc)."
       ::= { rsvpResvFwdEntry 2	}


    rsvpResvFwdDestAddr	OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(4..16))
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	destination address used by all	senders	in
	   this	 session.   This object	may not	be changed
	   when	the  value  of	the  RowStatus	object	is
	   'active'."
       ::= { rsvpResvFwdEntry 3	}


    rsvpResvFwdSenderAddr OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(4..16))
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	source address of the sender  selected	by
	   this	 reservation.	The  value  of	all zeroes
	   indicates 'all senders'.  This object  may  not
	   be  changed	when  the  value  of the RowStatus
	   object is 'active'."
       ::= { rsvpResvFwdEntry 4	}

    rsvpResvFwdDestAddrLength OBJECT-TYPE
	SYNTAX	    INTEGER(0..128)
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	length of the destination address in bits.
	   This	 is  the CIDR Prefix Length, which for IP4
	   hosts and multicast addresses is 32 bits.  This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpResvFwdEntry 5	}


    rsvpResvFwdSenderAddrLength	OBJECT-TYPE
	SYNTAX	    INTEGER(0..128)
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	length of the sender's	address	 in  bits.
	   This	 is  the CIDR Prefix Length, which for IP4
	   hosts and multicast addresses is 32 bits.  This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpResvFwdEntry 6	}


    rsvpResvFwdProtocol	OBJECT-TYPE
	SYNTAX	    Protocol
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	IP Protocol used by a session. for  secure
	   sessions,  this  indicates  IP  Security.  This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpResvFwdEntry 7	}

    rsvpResvFwdDestPort	OBJECT-TYPE
	SYNTAX	    Port
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	 UDP  or  TCP  port  number  used   as	 a
	   destination	 port  for  all	 senders  in  this
	   session.  If	the IP protocol	in use,	 specified
	   by rsvpResvFwdProtocol, is 50 (ESP) or 51 (AH),
	   this	 represents  a	virtual	 destination  port
	   number.   A value of	zero indicates that the	IP
	   protocol in use  does  not  have  ports.   This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpResvFwdEntry 8	}


    rsvpResvFwdPort OBJECT-TYPE
	SYNTAX	    Port
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	UDP or TCP port	number used  as	 a  source
	   port	 for  this sender in this session.  If the
	   IP	 protocol    in	   use,	   specified	by
	   rsvpResvFwdProtocol	is  50	(ESP)  or 51 (AH),
	   this	represents a generalized  port	identifier
	   (GPI).   A  value of	zero indicates that the	IP
	   protocol in use  does  not  have  ports.   This
	   object may not be changed when the value of the
	   RowStatus object is 'active'."
       ::= { rsvpResvFwdEntry 9	}


    rsvpResvFwdHopAddr OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(4..16))
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	address	of the (previous) RSVP	that  will
	   receive this	message."
       ::= { rsvpResvFwdEntry 10 }


    rsvpResvFwdHopLih OBJECT-TYPE
	SYNTAX	    Integer32
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	 Logical  Interface  Handle  sent  to  the
	   (previous)	RSVP   that   will   receive  this
	   message."
       ::= { rsvpResvFwdEntry 11 }


    rsvpResvFwdInterface OBJECT-TYPE
	SYNTAX	    InterfaceIndex
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	ifIndex	value of the  interface	 on  which
	   this	RESV message was most recently sent."
       ::= { rsvpResvFwdEntry 12 }


    rsvpResvFwdService OBJECT-TYPE
	SYNTAX	    QosService
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	QoS Service classification requested."
       ::= { rsvpResvFwdEntry 13 }


    rsvpResvFwdTSpecRate OBJECT-TYPE
	SYNTAX	    BitRate
	UNITS	    "bits per second"
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	Average	Bit  Rate  of  the  sender's  data
	   stream.    Within  a	 transmission  burst,  the
	   arrival   rate    may    be	  as	fast	as
	   rsvpResvFwdTSpecPeakRate  (if  supported by the
	   service model); however, averaged across two	or
	   more	 burst	intervals,  the	 rate  should  not
	   exceed rsvpResvFwdTSpecRate.

	   Note	that this is a prediction, often based	on
	   the	general	 capability  of	a type of codec	or
	   particular encoding;	the measured average  rate
	   may be significantly	lower."
       ::= { rsvpResvFwdEntry 14 }


    rsvpResvFwdTSpecPeakRate OBJECT-TYPE
	SYNTAX	    BitRate
	UNITS	    "bits per second"
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	Peak Bit Rate of the sender's data  stream
	   Traffic  arrival is not expected to exceed this
	   rate	at any time, apart  from  the  effects	of
	   jitter in the network.  If not specified in the
	   TSpec, this returns zero or noSuchValue."
       ::= { rsvpResvFwdEntry 15 }


    rsvpResvFwdTSpecBurst OBJECT-TYPE
	SYNTAX	    BurstSize
	UNITS	    "bytes"
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	size of	the largest  burst  expected  from
	   the sender at a time.

	   If this is less than	 the  sender's	advertised
	   burst  size,	the receiver is	asking the network
	   to provide flow pacing  beyond  what	 would	be
	   provided   under   normal  circumstances.  Such
	   pacing is at	the network's option."
       ::= { rsvpResvFwdEntry 16 }


    rsvpResvFwdTSpecMinTU OBJECT-TYPE
	SYNTAX	    MessageSize
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	minimum	message	size for  this	flow.  The
	   policing  algorithm will treat smaller messages
	   as though they are this size."
       ::= { rsvpResvFwdEntry 17 }


    rsvpResvFwdTSpecMaxTU OBJECT-TYPE
	SYNTAX	    MessageSize
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	maximum	message	size for  this	flow.  The
	   admission  algorithm	 will  reject TSpecs whose
	   Maximum Transmission	Unit, plus  the	 interface
	   headers, exceed the interface MTU."
       ::= { rsvpResvFwdEntry 18 }


    rsvpResvFwdRSpecRate OBJECT-TYPE
	SYNTAX	    BitRate
	UNITS	    "bytes per second"
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "If the requested  service  is  Guaranteed,	as
	   specified   by  rsvpResvService,  this  is  the
	   clearing  rate   that   is	being	requested.
	   Otherwise,  it is zero, or the agent	may return
	   noSuchValue."
       ::= { rsvpResvFwdEntry 19 }


    rsvpResvFwdRSpecSlack OBJECT-TYPE
	SYNTAX	    Integer32
	UNITS	    "microseconds"
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "If the requested  service  is  Guaranteed,	as
	   specified by	rsvpResvService, this is the delay
	   slack.  Otherwise, it is zero, or the agent may
	   return noSuchValue."
       ::= { rsvpResvFwdEntry 20 }


    rsvpResvFwdInterval	OBJECT-TYPE
	SYNTAX	    RefreshInterval
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	  interval   between   refresh	  messages
	   advertised to the Previous Hop."
       ::= { rsvpResvFwdEntry 21 }


    rsvpResvFwdScope OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(0..65536))
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	contents of the	scope object, displayed	as
	   an  uninterpreted  string  of octets, including
	   the object header.  In the absence of  such	an
	   object, this	should be of zero length."
       ::= { rsvpResvFwdEntry 22 }


    rsvpResvFwdShared OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "If TRUE, a reservation shared among	senders	is
	   requested.  If FALSE, a reservation specific	to
	   this	sender is requested."
       ::= { rsvpResvFwdEntry 23 }


    rsvpResvFwdExplicit	OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "If TRUE, individual	senders	are  listed  using
	   Filter  Specifications.   If	FALSE, all senders
	   are implicitly selected.  The Scope Object will
	   contain  a list of senders that need	to receive
	   this	reservation request  for  the  purpose	of
	   routing the RESV message."
       ::= { rsvpResvFwdEntry 24 }

    rsvpResvFwdRSVPHop OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "If TRUE, the node believes that  the  next	IP
	   hop	is  an	RSVP  hop.   If	 FALSE,	 the  node
	   believes that the next IP hop  may  not  be	an
	   RSVP	hop."
       ::= { rsvpResvFwdEntry 25 }


    rsvpResvFwdLastChange OBJECT-TYPE
	SYNTAX	    TimeStamp
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	time of	the last change	in  this  request;
	   This	 is  either  the first time it was sent	or
	   the	time  of  the  most   recent   change	in
	   parameters."
       ::= { rsvpResvFwdEntry 26 }


    rsvpResvFwdPolicy OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(0..65536))
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	contents of the	policy	object,	 displayed
	   as an uninterpreted string of octets, including
	   the object header.  In the absence of  such	an
	   object, this	should be of zero length."
       ::= { rsvpResvFwdEntry 27 }


    rsvpResvFwdStatus OBJECT-TYPE
	SYNTAX	    RowStatus
	MAX-ACCESS  read-write
	STATUS	    current
	DESCRIPTION
	   "'active' for all active RESV  messages.   This
	   object may be used to delete	RESV information."
       ::= { rsvpResvFwdEntry 28 }


    rsvpResvFwdTTL OBJECT-TYPE
	SYNTAX	    INTEGER (0..255)
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	TTL value in the RSVP header that was last
	   received."
       ::= { rsvpResvFwdEntry 29 }


    rsvpResvFwdFlowId OBJECT-TYPE
	SYNTAX	    INTEGER (0..16777215)
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	flow ID	that this receiver  is	using,	if
	   this	 is  an	IPv6 session."
       ::= { rsvpResvFwdEntry 30 }


--	The RSVP Interface Attributes Database contains	the
--	RSVP-specific information for an interface. Information
--	that is	shared with other reservation procedures such
--	as ST-II is in the Integrated Interface	Attributes
--	Database.


    rsvpIfTable	OBJECT-TYPE
	SYNTAX	    SEQUENCE OF	RsvpIfEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "The	RSVP-specific attributes of  the  system's
	   interfaces."
       ::= { rsvpObjects 6 }


    rsvpIfEntry	OBJECT-TYPE
	SYNTAX	    RsvpIfEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "The	RSVP-specific attributes of  the  a  given
	   interface."
       INDEX { ifIndex }
       ::= { rsvpIfTable 1 }

RsvpIfEntry ::=
    SEQUENCE {
    rsvpIfUdpNbrs			Gauge32,
    rsvpIfIpNbrs			Gauge32,
    rsvpIfNbrs				Gauge32,
    rsvpIfEnabled			TruthValue,
    rsvpIfUdpRequired			TruthValue,
    rsvpIfRefreshBlockadeMultiple	INTEGER,
    rsvpIfRefreshMultiple		INTEGER,
    rsvpIfTTL				INTEGER,
    rsvpIfRefreshInterval		TimeInterval,
    rsvpIfRouteDelay			TimeInterval,
    rsvpIfStatus			RowStatus
    }


    rsvpIfUdpNbrs OBJECT-TYPE
	SYNTAX	    Gauge32
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	number of neighbors perceived to be  using
	   only	the RSVP UDP Encapsulation."
       ::= { rsvpIfEntry 1 }


    rsvpIfIpNbrs OBJECT-TYPE
	SYNTAX	    Gauge32
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	number of neighbors perceived to be  using
	   only	the RSVP IP Encapsulation."
       ::= { rsvpIfEntry 2 }


    rsvpIfNbrs OBJECT-TYPE
	SYNTAX	    Gauge32
	MAX-ACCESS  read-only
	STATUS	    current
	DESCRIPTION
	   "The	number of neighbors  currently	perceived;
	   this	 will  exceed rsvpIfIpNbrs + rsvpIfUdpNbrs
	   by  the  number   of	  neighbors   using   both
	   encapsulations."
       ::= { rsvpIfEntry 3 }


    rsvpIfRefreshBlockadeMultiple OBJECT-TYPE
	SYNTAX	    INTEGER (1..65536)
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	value of the RSVP value	'Kb', Which is the
	   minimum   number   of  refresh  intervals  that
	   blockade state will last once entered."
       DEFVAL	   { 4 }
       ::= { rsvpIfEntry 4 }



    rsvpIfRefreshMultiple OBJECT-TYPE
	SYNTAX	    INTEGER (1..65536)
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	value of the RSVP value	'K', which is  the
	   number  of  refresh intervals which must elapse
	   (minimum) before a PATH or RESV  message  which
	   is not being	refreshed will be aged out."
       DEFVAL	   { 3 }
       ::= { rsvpIfEntry 5 }


    rsvpIfTTL OBJECT-TYPE
	SYNTAX	    INTEGER (0..255)
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	value of SEND_TTL used on  this	 interface
	   for	messages  this node originates.	 If set	to
	   zero, the node determines  the  TTL	via  other
	   means."
       DEFVAL {	0 } -- which is	to say,	no override
       ::= { rsvpIfEntry 6 }


    rsvpIfRefreshInterval OBJECT-TYPE
	SYNTAX	    TimeInterval
	UNITS	    "milliseconds"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	value of the RSVP value	'R', which is  the
	   minimum period between refresh transmissions	of
	   a given PATH	or RESV	message	on an interface."
       DEFVAL	   { 3000 }	   -- 30 seconds
       ::= { rsvpIfEntry 7 }



    rsvpIfRouteDelay OBJECT-TYPE
	SYNTAX	    TimeInterval
	UNITS	    "hundredths	of a second"
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	approximate period from	the time  a  route
	   is  changed	to  the	 time  a resulting message
	   appears on the interface."
       DEFVAL	   { 200 } -- 2	seconds
       ::= { rsvpIfEntry 8 }


    rsvpIfEnabled OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If TRUE, RSVP is enabled  on  this	Interface.
	   If	FALSE,	 RSVP	is  not	 enabled  on  this
	   interface."
       ::= { rsvpIfEntry 9 }


    rsvpIfUdpRequired OBJECT-TYPE
	SYNTAX	    TruthValue
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "If TRUE, manual configuration forces  the  use
	   of  UDP  encapsulation  on  the  interface.	If
	   FALSE,  UDP	encapsulation  is  only	 used	if
	   rsvpIfUdpNbrs is not	zero."

       ::= { rsvpIfEntry 10 }


    rsvpIfStatus OBJECT-TYPE
	SYNTAX	    RowStatus
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "'active' on	interfaces that	are configured for
	   RSVP."
       ::= { rsvpIfEntry 11 }


--	The RSVP Neighbor Database lists the neighbors the RSVP
--	process	currently is receiving messages	from.


    rsvpNbrTable OBJECT-TYPE
	SYNTAX	    SEQUENCE OF	RsvpNbrEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "Information	describing  the	 Neighbors  of	an
	   RSVP	system."
       ::= { rsvpObjects 7 }


    rsvpNbrEntry OBJECT-TYPE
	SYNTAX	    RsvpNbrEntry
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "Information	  describing   a    single    RSVP
	   Neighbor."
       INDEX { ifIndex,	rsvpNbrAddress }
       ::= { rsvpNbrTable 1 }

RsvpNbrEntry ::=
    SEQUENCE {
    rsvpNbrAddress	OCTET STRING,
    rsvpNbrProtocol	RsvpEncapsulation,
    rsvpNbrStatus	RowStatus
    }

    rsvpNbrAddress OBJECT-TYPE
	SYNTAX	    OCTET STRING (SIZE(4..16))
	MAX-ACCESS  not-accessible
	STATUS	    current
	DESCRIPTION
	   "The	IP4 or IP6 Address used	by this	 neighbor.
	   This	 object	 may not be changed when the value
	   of the RowStatus object is 'active'."
       ::= { rsvpNbrEntry 1 }

    rsvpNbrProtocol OBJECT-TYPE
	SYNTAX	    RsvpEncapsulation
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "The	  encapsulation	  being	  used	 by   this
	   neighbor."
       ::= { rsvpNbrEntry 2 }


    rsvpNbrStatus OBJECT-TYPE
	SYNTAX	    RowStatus
	MAX-ACCESS  read-create
	STATUS	    current
	DESCRIPTION
	   "'active' for all neighbors.	 This  object  may
	   be	used   to  configure  neighbors.   In  the
	   presence   of   configured	 neighbors,    the
	   implementation  may	(but  is  not required to)
	   limit the  set  of  valid  neighbors	 to  those
	   configured."
       ::= { rsvpNbrEntry 3 }


--
--	Notifications used to signal events
--

    rsvpNotifications OBJECT IDENTIFIER	::= { rsvpNotificationsPrefix 0	}


    newFlow NOTIFICATION-TYPE
	OBJECTS	{
		    intSrvFlowStatus, rsvpSessionDestAddr,
		    rsvpResvFwdStatus, rsvpResvStatus, rsvpSenderStatus
		}
	STATUS	current
	DESCRIPTION
	   "The	  newFlow   trap   indicates   that    the
	   originating	system has installed a new flow	in
	   its	 classifier,	or    (when    reservation
	   authorization   is  in  view)  is  prepared	to
	   install such	a flow in the  classifier  and	is
	   requesting authorization.  The objects included
	   with	the  Notification  may	be  used  to  read
	   further   information   using   the	Integrated
	   Services and	RSVP MIBs.  Authorization or  non-
	   authorization  may be enacted by a write to the
	   variable intSrvFlowStatus."
       ::= { rsvpNotifications 1 }


    lostFlow NOTIFICATION-TYPE
	OBJECTS	{
		    intSrvFlowStatus, rsvpSessionDestAddr,
		    rsvpResvFwdStatus, rsvpResvStatus, rsvpSenderStatus
		}
	STATUS	current
	DESCRIPTION
	   "The	  lostFlow   trap   indicates	that   the
	   originating	system has removed a flow from its
	   classifier."
       ::= { rsvpNotifications 2 }


-- conformance information


rsvpGroups	OBJECT IDENTIFIER ::= {	rsvpConformance	1 }
rsvpCompliances	OBJECT IDENTIFIER ::= {	rsvpConformance	2 }

-- compliance statements


    rsvpCompliance MODULE-COMPLIANCE
	STATUS	current
	DESCRIPTION
	   "The	 compliance  statement.	  Note	that   the
	   implementation    of	  this	 module	  requires
	   implementation of the Integrated  Services  MIB
	   as well."
       MODULE  -- this module
       MANDATORY-GROUPS	{
	   rsvpSessionGroup, rsvpSenderGroup, rsvpResvGroup,
	   rsvpIfGroup,	rsvpNbrGroup,
	   rsvpGenObjectsGroup,	rsvpSenderOutInterfaceGroup
	   }

       GROUP rsvpResvFwdGroup
	 DESCRIPTION
	  "The Reservation Requests table  is  appropriate
	  in	implementations	   that	  store	  upstream
	  reservation messages,	 but  not  appropriate	in
	  implementations  which  calculate  them  on each
	  transmission."

      GROUP rsvpNotificationGroup
	DESCRIPTION
	 "The notifications in this module may be used	to
	 advise	a network management station of	changes	in
	 flow status, and are required when this use is	in
	 view."

     OBJECT	  rsvpSessionRequests
       MIN-ACCESS not-accessible
       DESCRIPTION
	"This object is	optional."

    OBJECT	 rsvpSenderType
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderDestAddr
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderAddr
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderDestAddrLength
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderAddrLength
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderProtocol
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderDestPort
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderPort
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderHopAddr
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderHopLih
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderInterface
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderTSpecRate
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderTSpecPeakRate
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderTSpecBurst
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderTSpecMinTU
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderTSpecMaxTU
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderInterval
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderRSVPHop
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderPolicy
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderAdspecBreak
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderAdspecHopCount
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderAdspecPathBw
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderAdspecMinLatency
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderAdspecMtu
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderAdspecGuaranteedSvc
      MIN-ACCESS not-accessible
      DESCRIPTION

       "This may be not-accessible if the system does  not
       support Guaranteed Service."

    OBJECT	 rsvpSenderAdspecGuaranteedBreak
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Guaranteed Service."

    OBJECT	 rsvpSenderAdspecGuaranteedCtot
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Guaranteed Service."

    OBJECT	 rsvpSenderAdspecGuaranteedDtot
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Guaranteed Service."

    OBJECT	 rsvpSenderAdspecGuaranteedCsum
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Guaranteed Service."

    OBJECT	 rsvpSenderAdspecGuaranteedDsum
      MIN-ACCESS read-only
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Guaranteed Service."

    OBJECT	 rsvpSenderAdspecGuaranteedHopCount
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Guaranteed Service."

    OBJECT	 rsvpSenderAdspecGuaranteedPathBw
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Guaranteed Service."


    OBJECT	 rsvpSenderAdspecGuaranteedMinLatency
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Guaranteed Service."

    OBJECT	 rsvpSenderAdspecGuaranteedMtu
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Guaranteed Service."

    OBJECT	 rsvpSenderAdspecCtrlLoadSvc
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Controlled Load."

    OBJECT	 rsvpSenderAdspecCtrlLoadBreak
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Controlled Load."

    OBJECT	 rsvpSenderAdspecCtrlLoadHopCount
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Controlled Load."

    OBJECT	 rsvpSenderAdspecCtrlLoadPathBw
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Controlled Load."

    OBJECT	 rsvpSenderAdspecCtrlLoadMinLatency
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This may be not-accessible if the system does  not
       support Controlled Load."

    OBJECT	 rsvpSenderAdspecCtrlLoadMtu
      MIN-ACCESS not-accessible
      DESCRIPTION

       "This may be not-accessible if the system does  not
       support Controlled Load."

    OBJECT	 rsvpSenderStatus
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpSenderFlowId
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This object  is	 needed	 only  in  a  system  that
       implements IPv6."


    OBJECT	 rsvpResvType
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvDestAddr
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvSenderAddr
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvDestAddrLength
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvSenderAddrLength
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvProtocol
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvDestPort
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvPort
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvHopAddr
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvHopLih
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvInterface
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvService
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvTSpecRate
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvTSpecPeakRate
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvTSpecBurst
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvTSpecMinTU
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvTSpecMaxTU
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvRSpecRate
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvRSpecSlack
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvInterval
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvScope
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvShared
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvExplicit
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvRSVPHop
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvPolicy
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvStatus
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvFlowId
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This object  is	 needed	 only  in  a  system  that
       implements IPv6."

    OBJECT	 rsvpResvFwdStatus
      MIN-ACCESS read-only
      DESCRIPTION
       "read-create access is not required.  This  may	be
       read-only."

    OBJECT	 rsvpResvFwdFlowId
      MIN-ACCESS not-accessible
      DESCRIPTION
       "This object  is	 needed	 only  in  a  system  that
       implements IPv6."

    ::=	{ rsvpCompliances 1 }


    rsvpSessionGroup OBJECT-GROUP
	 OBJECTS {
	    rsvpSessionType, rsvpSessionDestAddr,
	    rsvpSessionDestAddrLength, rsvpSessionProtocol,
	    rsvpSessionPort, rsvpSessionSenders, rsvpSessionReceivers,
	    rsvpSessionRequests, rsvpSessionNewIndex
	}
	STATUS	current
	DESCRIPTION
	   "These objects are required for RSVP	Systems."
       ::= { rsvpGroups	1 }


    rsvpSenderGroup OBJECT-GROUP
	 OBJECTS {
	    rsvpSenderType, rsvpSenderDestAddr,	rsvpSenderAddr,
	    rsvpSenderDestAddrLength, rsvpSenderAddrLength,
	    rsvpSenderProtocol,	rsvpSenderDestPort, rsvpSenderPort,
	    rsvpSenderFlowId, rsvpSenderTTL,
	    rsvpSenderHopAddr, rsvpSenderHopLih, rsvpSenderInterface,
	    rsvpSenderTSpecRate, rsvpSenderTSpecPeakRate,
	    rsvpSenderTSpecBurst, rsvpSenderTSpecMinTU,
	    rsvpSenderTSpecMaxTU, rsvpSenderInterval, rsvpSenderLastChange,
	    rsvpSenderStatus, rsvpSenderRSVPHop, rsvpSenderPolicy,
	    rsvpSenderAdspecBreak, rsvpSenderAdspecHopCount,
	    rsvpSenderAdspecPathBw, rsvpSenderAdspecMinLatency,
	    rsvpSenderAdspecMtu, rsvpSenderAdspecGuaranteedSvc,
	    rsvpSenderAdspecGuaranteedBreak,
	    rsvpSenderAdspecGuaranteedCtot, rsvpSenderAdspecGuaranteedDtot,
	    rsvpSenderAdspecGuaranteedCsum, rsvpSenderAdspecGuaranteedDsum,
	    rsvpSenderAdspecGuaranteedHopCount,
	    rsvpSenderAdspecGuaranteedPathBw,
	    rsvpSenderAdspecGuaranteedMinLatency,
	    rsvpSenderAdspecGuaranteedMtu, rsvpSenderAdspecCtrlLoadSvc,
	    rsvpSenderAdspecCtrlLoadBreak,
	    rsvpSenderAdspecCtrlLoadHopCount,
	    rsvpSenderAdspecCtrlLoadPathBw,
	    rsvpSenderAdspecCtrlLoadMinLatency,
	    rsvpSenderAdspecCtrlLoadMtu, rsvpSenderNewIndex
	}
	STATUS	current
	DESCRIPTION
	   "These objects are required for RSVP	Systems."
       ::= { rsvpGroups	2 }


    rsvpResvGroup OBJECT-GROUP
	 OBJECTS {
	    rsvpResvType, rsvpResvDestAddr, rsvpResvSenderAddr,
	    rsvpResvDestAddrLength, rsvpResvSenderAddrLength,
	    rsvpResvProtocol, rsvpResvDestPort,	rsvpResvPort,
	    rsvpResvHopAddr, rsvpResvHopLih, rsvpResvInterface,
	    rsvpResvService, rsvpResvTSpecRate,	rsvpResvTSpecBurst,
	    rsvpResvTSpecPeakRate, rsvpResvTSpecMinTU, rsvpResvTSpecMaxTU,
	    rsvpResvRSpecRate, rsvpResvRSpecSlack, rsvpResvInterval,
	    rsvpResvScope, rsvpResvShared, rsvpResvExplicit,
	    rsvpResvRSVPHop, rsvpResvLastChange, rsvpResvPolicy,
	    rsvpResvStatus, rsvpResvNewIndex, rsvpResvTTL, rsvpResvFlowId
	}
	STATUS	current
	DESCRIPTION
	   "These objects are required for RSVP	Systems."
       ::= { rsvpGroups	3 }


    rsvpResvFwdGroup OBJECT-GROUP
	 OBJECTS {
	    rsvpResvFwdType, rsvpResvFwdDestAddr, rsvpResvFwdSenderAddr,
	    rsvpResvFwdDestAddrLength, rsvpResvFwdSenderAddrLength,
	    rsvpResvFwdProtocol, rsvpResvFwdDestPort, rsvpResvFwdPort,
	    rsvpResvFwdHopAddr,	rsvpResvFwdHopLih, rsvpResvFwdInterface,
	    rsvpResvFwdNewIndex, rsvpResvFwdService,
	    rsvpResvFwdTSpecPeakRate, rsvpResvFwdTSpecMinTU,
	    rsvpResvFwdTSpecMaxTU, rsvpResvFwdTSpecRate,
	    rsvpResvFwdTSpecBurst, rsvpResvFwdRSpecRate,
	    rsvpResvFwdRSpecSlack, rsvpResvFwdInterval,	rsvpResvFwdScope,
	    rsvpResvFwdShared, rsvpResvFwdExplicit, rsvpResvFwdRSVPHop,
	    rsvpResvFwdLastChange, rsvpResvFwdPolicy, rsvpResvFwdStatus,
	    rsvpResvFwdTTL, rsvpResvFwdFlowId
	}
	STATUS	current
	DESCRIPTION
	   "These objects are optional,	used for some RSVP
	   Systems."
       ::= { rsvpGroups	4 }


    rsvpIfGroup	OBJECT-GROUP
	 OBJECTS {
	    rsvpIfUdpNbrs, rsvpIfIpNbrs, rsvpIfNbrs, rsvpIfEnabled,
	    rsvpIfUdpRequired, rsvpIfRefreshBlockadeMultiple,
	    rsvpIfRefreshMultiple, rsvpIfRefreshInterval, rsvpIfTTL,
	    rsvpIfRouteDelay, rsvpIfStatus
	}
	STATUS	current
	DESCRIPTION
	   "These objects are required for RSVP	Systems."
       ::= { rsvpGroups	5 }


    rsvpNbrGroup OBJECT-GROUP
	 OBJECTS {
	    rsvpNbrProtocol, rsvpNbrStatus
	}
	STATUS	current
	DESCRIPTION
	   "These objects are required for RSVP	Systems."
       ::= { rsvpGroups	6 }


    rsvpGenObjectsGroup	 OBJECT-GROUP
	OBJECTS	{
	   rsvpBadPackets
	}
	STATUS	current
	DESCRIPTION
	   "This objects are required for RSVP Systems."
       ::= { rsvpGroups	7 }



    rsvpSenderOutInterfaceGroup	OBJECT-GROUP
	OBJECTS	{
	    rsvpSenderOutInterfaceStatus
	}
	STATUS	current
	DESCRIPTION
	   "These objects are required for RSVP	Systems."
       ::= { rsvpGroups	8 }



    rsvpNotificationGroup NOTIFICATION-GROUP
	NOTIFICATIONS {	newFlow, lostFlow }
	STATUS	current
	DESCRIPTION
	   "This  notification	is  required  for  Systems
	   supporting the RSVP Policy Module using an SNMP
	   interface to	the Policy Manager."
       ::= { rsvpGroups	9 }


END

