-- *****************************************************************
-- CISCO-CAS-IF-MIB.my: Channel Associated Signal Interface MIB file
--
-- July 1997  Hongchi Shih   
-- Jan. 1999  Rick Chen
--
-- Copyright (c) 1997-1999, 2000, 2003, 2004 by cisco Systems, Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-CAS-IF-MIB DEFINITIONS ::= BEGIN

IMPORTS
        MODULE-IDENTITY,
        OBJECT-TYPE,
        Integer32 
                FROM SNMPv2-SMI
        RowStatus,
        TruthValue, 
        DisplayString
                FROM SNMPv2-TC
        MODULE-COMPLIANCE,
        OBJECT-GROUP
                FROM SNMPv2-CONF

        InterfaceIndex,
        ifIndex
                FROM IF-MIB

        CountryCode
                FROM CISCO-TC

        ciscoMgmt
                FROM CISCO-SMI;


ciscoCasIfMIB MODULE-IDENTITY
        LAST-UPDATED    "200410130000Z"
        ORGANIZATION    "Cisco Systems, Inc."
        CONTACT-INFO
                "       Cisco Systems
                        Customer Service

                Postal: 170 W. Tasman Drive
                        San Jose, CA  95134
                        USA

                Tel: +1 800 553-NETS

                E-mail: cs-voice@cisco.com"
        DESCRIPTION
                "Channel Associated Signal Interface MIB module.
                 This MIB manages the generic CAS (Channel Associated
                 Signal)or DS0 clear channel Interfaces in the router.
                "
        REVISION    "200410130000Z"
        DESCRIPTION
                "Extend CcasGrpEMTmEntry to include
                     ccasGrpEMTmPttXmt
                     ccasGrpEMTmPttRcv
                     ccasGrpEMTmDelayVoice
                 Extend CcasGrpEMCfgEntry to include  
                     ccasGrpEMCfgAutoGainControl
                 add ccasEMGroupRev2
                 add ccasIfMIBComplianceRev3
                "

        REVISION    "200409300000Z"
        DESCRIPTION
                "Extend ccasGrpCfgServiceType to include 
                 xgcp (11)"

        REVISION    "200401150000Z"
        DESCRIPTION
                "Deprecated ccasEMGroup
                 Add ccasEMGroupRev1         
                 Extend ccasGrpCfgType to include emLmr (27)
                 Extend CcasGrpEMCfgEntry to include 
                 ccasGrpEMCfgLmrMCap & ccasGrpEMCfgLmrECap
                 Extend CcasGrpEMTmEntry to include
                 ccasGrpEMTmVoiceHangover &
                 ccasGrpEMTmLmrTeardown
                "

        REVISION    "200304180000Z"
        DESCRIPTION
                "Extend ccasGrpCfgServiceType to include 
                 h248 (9) and ds0xconn (10)"

        REVISION    "200210020000Z"
        DESCRIPTION
                "Extend ccasGrpCfgServiceType to include 
                 trunkingService(8)."

        REVISION    "9901180000Z"
        DESCRIPTION
                "Add ccasXgcpCfgTable to configure continuity test
                 (COT) tone frequencies. 
                 Add object ccasGrpCfgServiceType for displaying service 
                 type.
                 Extend ccsaGrpCfgType to include fgdOS, fgdEANA and 
                 nullSignaling"

        ::= { ciscoMgmt 85 }

--
-- ifEntry for the all type of Channel Associated Signal channel (CAS)
-- supports the ifGeneralInformationGroup of Cisco IF-MIB.
-- 

-- ifTable           Comments
-- ==============    ==================================================
-- ifIndex           Each CAS channel is represented by an ifEntry.
-- ifDescr           Textual CAS channel description.
-- ifType            The IANA value of ds0(81)
--
-- ifSpeed           contains 64000 for CAS channel.
-- ifPhysAddress     contains an octet string of zero length.
--
-- ifAdminStatus     Only support the read-only ifAdminStatus.  
-- ifOperStatus      The current operational status of the CAS channel
--                   interface port. Note that dormant(5) is explicitly
--                   being used as defined in RFC 1573.
-- ifLastChange      Refer to RFC 1573.
-- ifLinkUpDownTrapEnable
--                   Only support the read-only ifLinkUpDownTrapEnable.
--                   It contains a 'disabled(2)' value.
-- ifConnectorPresent
--                   Refer to RFC 1573.
-- ifHighSpeed       contains a zero value.
-- ifName            Refer to RFC 1573.
-- ifAlias           Only support the read-only ifAlias. It contains an
--                   octet string of zero length.
--

             
--
-- Relationship to the IETF Dial Control MIB (RFC 2128)
--
-- Associating and disassociating a CAS channel interface with
-- a connection can be explicitly handled using an ifStack. If a
-- call connection is established, the managed system stacks the call
-- associated voice encapsulation interface on top of CAS channel of
-- T1/E1. 
-- Refer to the section 2.2.1 of RFC 2128 and the section 3.2.1 of
-- RFC 2127 for the detailed information.

--
-- Using ifStackTable
-- 
--   This section describes by example how to use ifStackTable to
--   represent the relationship of dial-up peer with ds0 and ds1
--   interfaces.
--   Examples given below are for illustration of active calls on
--   voice encapsulation peers via ds0 of DS1.
--
--   Example: A Voice Peer1 is being carried two active calls via two
--            ds0 interfaces and Voice Peer2 is being carried one active
--            call via one ds0 interface of the same DS1.
--
--       +=============+ +=====+
--       |     Voice   | |Voice|
--       |     Peer1   | |Peer2|
--       +=============+ +=====+
--          |       |       |    <==== appears active
--          |       |       |          when the dial-up peer
--          |       |       |          connects to CAS channel
--        +===+   +===+   +===+
--        |ds0|   |ds0|   |ds0|  <==== CAS channels
--        +===+   +===+   +===+
--          |       |       |
--       +=====================+
--       |         DS1         | 
--       +=====================+
--
--   The assignment of the index values could for example be:
--
--           ifIndex  Description
--           1        voice peer 1      (type 103)
--           2        voice peer 2      (type 103)
--           3        ds0 #1            (type 81)
--           4        ds0 #2            (type 81)
--           5        ds0 #3            (type 81)
--           7        ds1               (type 18)
--
--
--   The ifStackTable is then used to show the relationships between the
--   various interfaces.
--
--         ifStackTable Entries
--
--         HigherLayer   LowerLayer
--         0             1
--         0             2
--         1             3
--         1             4
--         2             5
--         3             7
--         4             7
--         5             7
--         7             0
--
--
--   The Signaling type of the DS0 group is enhanced to include null
--   signaling. When configured as null signaling, the DS0 group 
--   can provide voice/data path. 



ccasIfObjects          OBJECT IDENTIFIER ::= { ciscoCasIfMIB 1 }
ccasDS1Objects         OBJECT IDENTIFIER ::= { ccasIfObjects 1 }
ccasGrpObjects         OBJECT IDENTIFIER ::= { ccasIfObjects 2 }
ccasChannelObjects     OBJECT IDENTIFIER ::= { ccasIfObjects 3 }
ccasVoiceCfgObjects    OBJECT IDENTIFIER ::= { ccasIfObjects 4 }
ccasXgcpCfgObjects     OBJECT IDENTIFIER ::= { ccasIfObjects 5 }
ccasGrpGeneralObjects  OBJECT IDENTIFIER ::= { ccasGrpObjects 1 }
ccasGrpEMObjects       OBJECT IDENTIFIER ::= { ccasGrpObjects 2 }
ccasGrpLineObjects     OBJECT IDENTIFIER ::= { ccasGrpObjects 3 }
ccasGrpStaObjects      OBJECT IDENTIFIER ::= { ccasGrpObjects 4 }
ccasGrpABCDObjects     OBJECT IDENTIFIER ::= { ccasGrpObjects 5 }

--*********************************************************************
-- The CAS/DS0 Interface Groups
--*********************************************************************
-- [1] CAS/DS0 General Configuration for T1/E1
-- [2] CAS/DS0 General Configuration group
-- [3] CAS E&M group                
-- [4] CAS FXO/SAO group            
-- [5] CAS FXS/SAS group            
-- [6] CAS custom ABCD bits configuration group            
-- [7] CAS channel group          

--*********************************************************************
-- The CAS/DS0  General Configuration Table for T1/E1
--*********************************************************************
ccasDs1IfCfgTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CcasDs1IfCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "The CAS/DS0 General Configuration Table for T1/E1.  It
                 contains the CAS/DS0 related standard configuration 
                 information for T1/E1.
                "
        ::= { ccasDS1Objects 1 }

ccasDs1IfCfgEntry OBJECT-TYPE
        SYNTAX      CcasDs1IfCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An entry in the configuration table for each T1/E1.
                 The entry is created when a T1/E1 hardware is detected.
                "
        INDEX   { ifIndex }
        ::= { ccasDs1IfCfgTable 1 }

CcasDs1IfCfgEntry ::=
        SEQUENCE {
                ccasDs1IfCfgDs0ChannelsConfigurable OCTET STRING
        }

ccasDs1IfCfgDs0ChannelsConfigurable OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (0..4))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "This object contains the bit map of the available DS0
                 channel in the DS1.
                 The MSB (most significant bit) is DS0 channel number 1. 
                 The missing bytes is default to a value of 0.
                 A 1-bit indicates the channel is available for
                 configuration and a 0-bit indicates it isn't.
                 The length of this object is either 3 octets (for T1)
                 or 4 octets (for E1).
                 
                 The most significant bit is transmitted first.
                "
        ::= { ccasDs1IfCfgEntry 1 }



--*********************************************************************
-- The CAS/DS0 Group General Configuration Table
--*********************************************************************
ccasGrpCfgTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CcasGrpCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "The CAS/DS0 Group Standard Configuration Table.  It
                 contains the general configuration information for the
                 CAS/DS0 group of T1/E1 interfaces.
                "
        ::= { ccasGrpGeneralObjects 1 }

ccasGrpCfgEntry OBJECT-TYPE
        SYNTAX      CcasGrpCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "A CAS/DS0 group entry. Each entry consists of the CAS
                 group type and the CAS/DS0 group associated DS0
                 channels in a T1/E1.
                 The value of ccasGrpCfgDs0Channels must be specified
                 with at least one available DS0 channel in the CAS
                 group associated T1/E1 before a new row in this table
                 can become active(1).
                 The entry of this table can only be created if the
                 CAS/DS0 group associated DS1 ifEntry already exists.
                "
        INDEX   { ifIndex, ccasGrpCfgIndex }
        ::= { ccasGrpCfgTable 1 }

CcasGrpCfgEntry ::=
        SEQUENCE {
                ccasGrpCfgIndex            Integer32,
                ccasGrpCfgType             INTEGER,    
                ccasGrpCfgDs0Channels      OCTET STRING,
                ccasGrpCfgServiceType      INTEGER,
                ccasGrpCfgRowStatus        RowStatus
        }

ccasGrpCfgIndex OBJECT-TYPE
        SYNTAX      Integer32 (0..30)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An arbitrary index that uniquely identifies a DS0 group
                 in a T1/E1.
                "
        ::= { ccasGrpCfgEntry 1 }

ccasGrpCfgType OBJECT-TYPE
        SYNTAX      INTEGER {
            emWinkStart      (1),
            emWinkStartFgd   (2),
            emImmedStart     (3),
            emDelayDial      (4),
            fxsLoopStart     (5),  
            fxsGroundStart   (6),  
            sasLoopStart     (7),
            sasGroundStart   (8),
            r2Analog         (9),
            r2Digital        (10),
            r2Pulse          (11),
            p7               (12), 
            fxoLoopStart     (13),
            fxoGroundStart   (14), 
            fgdOS            (15),
            nullSignaling    (16),
            r1Itu            (17),
            r1Modified       (18),
            r1Turkey         (19),
            fgdEANA          (20),
            emMelImmedStart  (21),
            emMelWink        (22),
            emMelDelayDial   (23),
            fxsMelcas        (24),
            fxoMelcas        (25),
            extsig           (26),
            emLmr            (27)
        }         
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
                "The Signaling type of the DS0 group.
                 emWinkStart    - CAS E&M Wink Start.                   
                 emWinkStartFgd - CAS E&M Wink Start with Feature
                                  group D.
                 emImmedStart   - CAS E&M Immediate Start.     
                 emDelayDial    - CAS E&M Delay Dial.                   
                 fxsLoopStart   - CAS FXS Loop Start.
                 fxsGroundStart - CAS FXS Ground Start.
                 sasLoopStart   - CAS SAS Loop Start.
                 sasGroundStart - CAS SAS Ground Start.
                 r2Analog       - R2 ITU Q411.
                 r2Digital      - R2 ITU Q421.
                 r2Pulse        - R2 ITU Supplement 7. 
                 p7             - P7 switch.
                 fgdOS          - Bellcore Feature Group D : 
                                         Operator Services Signaling 
                 nullSignaling  - 64k clear channel
                 r1Itu          - R1 ITU.
                 r1Modified     - R1 Modified.
                 r1Turkey       - R1 Turkey.
                 fgdEANA        - FGD Exchange Access North American.
                 emMelImmedStart - CAS E&M Melcas Immediate Start
                 emMelWink      -  CAS E&M Melcas Wink Start
                 emMelDelayDial -  CAS E&M Melcas Delay Dial
                 fxsMelcas      -  CAS FXS Melcas
                 fxoMelcas      -  CAS FXO Melcas
                 extsig         -  External Signal 
                 emLmr          -  CAS E&M Land Mobil Radio(LMR)
                                   interface
                "
        REFERENCE
            "EIA/TIA-464B, chapter 6.2.1.1 Signaling Interface Types.
             ITU-T Q411 - Specifications of signalling system R2 line
                          signalling, analogue version.
             ITU-T Q421 - Specifications of signalling system R2 line
                          signalling, digital version. 
             ITU-T R2 Supplement 7 - Specifications of signalling system
                          R2 line signalling, pulsed version.
             Bellcore, TR-NPL-000258 -  Feature Group D
                       section 3.4 for Exchange Access North American 
                       section 3.6 for Operator Services Signaling 
            "
        DEFVAL      { emWinkStart }
        ::= { ccasGrpCfgEntry 2 }

ccasGrpCfgDs0Channels OBJECT-TYPE
        SYNTAX      OCTET STRING (SIZE (4))
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
                "This object contains the bit map of the selected DS0 
                 channels to be added into this group.
                 The MSB (most significant bit) is DS0 channel number 1.
                 For T1, only higher 24 bits are used to specify the
                 the CAS channels for the CAS group.
                 A 1-bit indicates the channel to be added into group
                 and a 0-bit indicates it isn't.
                "
        DEFVAL     { '00000000'H }
        ::= { ccasGrpCfgEntry 3 }

ccasGrpCfgServiceType OBJECT-TYPE
        SYNTAX      INTEGER {
                    none            (1),
                    casServSw56     (2), 
                    casServModem    (3),
                    casServAuto     (4),
                    sgcp            (5),
                    mgcp            (6),
                    other           (7),
                    trunkingService (8),
                    h248            (9),
                    ds0xconn        (10),
                    xgcp            (11)
                  }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
                "Specify the Service type of the CAS/DS0 group.
                 none - no service type 
                 casServSw56 -  sw56 service for CAS
                 casServModme -  modem service for CAS
                 casServAuto -  auto service for CAS
                 sgcp -  Simple Gateway Control Protocol
                         (SGCP) service. Used when DS0 is  
                         configured for null signaling.
                 mgcp -  Media Gateway Control Protocol 
                         (MGCP) service. Used when DS0 is  
                         configured for null signaling.
                 other - none of the above and the below.  
                 trunkingService - 
                         This DS0 group is handled by
                         trunking service application. 
                 h248 - ITU H.248 Media Gateway Control 
                        service. Used when DS0 is
                        configured for null signaling.
                 ds0xconn - Used for DS0 cross connection.
                 xgcp -  Media Gateway Control Protocol 
                         (MGCP) extension service including
                         TGCP (Trunking Gateway Control
                         Protocol) profiles feature. 
                         Used when DS0 is  configured for 
                         null signaling.
                "
        DEFVAL     { none }
        ::= { ccasGrpCfgEntry 5 }

ccasGrpCfgRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "This object is used to create a new row or modify
                 or delete an existing row in this table. The
                 corresponding instance of ccasGrpCfgType can not be
                 modified while this object has the value 'active'. 
                "
        ::= { ccasGrpCfgEntry 4 }
 


--*********************************************************************
-- The CAS Group E&M Standard Configuration Table
--*********************************************************************
ccasGrpEMCfgTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CcasGrpEMCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "The CAS Group E&M Standard Configuration Table. It
                 contains the CAS E&M group standard configuration
                 information of T1/E1.
                "
        ::= { ccasGrpEMObjects 1 }

ccasGrpEMCfgEntry OBJECT-TYPE
        SYNTAX      CcasGrpEMCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An entry in the configuration table for each CAS E&M
                 Group in the T1/E1.
                 The entry is created when the ccasGrpCfgType is
                 configured as 'em' on a T1/E1 via configuration
                 command.
                 The entry is deleted when the CAS Group is
                 de-configured from T1/E1.
                "
        INDEX   { ifIndex, ccasGrpCfgIndex }
        ::= { ccasGrpEMCfgTable 1 }

CcasGrpEMCfgEntry ::=
        SEQUENCE {
                ccasGrpEMCfgDialType         INTEGER,
                ccasGrpEMCfgDnisAni          BITS,
                ccasGrpEMCfgLmrMCap          INTEGER,
                ccasGrpEMCfgLmrECap          INTEGER,
                ccasGrpEMCfgAutoGainControl  TruthValue
        }


ccasGrpEMCfgDialType OBJECT-TYPE
        SYNTAX      INTEGER {
                    dtmf      (1),
                    pulse     (2),
                    mf        (3)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                "Specify the addressing type of the CAS group.
                 dtmf  - Dual Tone Multi-Frequency (DTMF) digit.
                 pulse - dial pulse.
                 mf    - Multi-Frequency (MF) digit.
                 The default value of this object is dtmf(1).
                "
        ::= { ccasGrpEMCfgEntry 1 }

ccasGrpEMCfgDnisAni OBJECT-TYPE
        SYNTAX      BITS {
                    incomingDnis       (0),
                    incomingAni        (1),
                    outgoingDnis       (2),
                    outgoingAni        (3)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                "Specify the type of Destination Number Identification
                 Service (DNIS) and Automatic Number Identification
                 (ANI) support.
                 MF tone supports both ANI and DNIS services. The DTMF
                 tone only supports both incoming and outgoing DNIS.
                 incomingDnis     - support incoming DNIS feature.
                 incomingAni      - support incoming ANI feature.
                 outgoingDnis     - support outgoing DNIS feature.
                 outgoingAni      - support outgoing ANI feature.
                 The default value of this object is '00'H.
                "
        ::= { ccasGrpEMCfgEntry 2 }

ccasGrpEMCfgLmrMCap OBJECT-TYPE
        SYNTAX      INTEGER {
                    inact     (1),
                    audio     (2),
                    dial      (3)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                "The M lead behavior of E&M LMR interface.
                 inact - The m-lead status should be ignored.
                 audio -  The m-lead status is used to control 
                          generating voice packet.
                 dial - The first m-lead off to on status indicates
                        call setup request. The following m-lead 
                        status change during the call should be
                        ignored.
                "
        DEFVAL { inact }
        ::= { ccasGrpEMCfgEntry 3 }

ccasGrpEMCfgLmrECap OBJECT-TYPE
        SYNTAX      INTEGER {
                    seize     (4),
                    voice     (5),
                    inactive  (6)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                "The E lead behavior of E&M LMR interface.
                 seize - The e-lead used as seize signal.
                 voice -  The e-lead status is used to indicate
                          voice packet received or not.
                 inactive -- e-lead is inactive.
                "
        DEFVAL { seize }
        ::= { ccasGrpEMCfgEntry 4 }

ccasGrpEMCfgAutoGainControl OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                "This object is used to enabling or disabling automatic 
                 gain control on this interface. AGC allows dsp to
                 adjust the input voice volume and avoid rapid
                 voice volume change.
                "
        DEFVAL { false }
        ::= { ccasGrpEMCfgEntry 5 }

--*********************************************************************
-- The CAS Group E&M Timing Parameters Table
--*********************************************************************

-- This table contains the CAS Group E&M timing parameters information.

ccasGrpEMTmTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CcasGrpEMTmEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "The E&M interface Timing Parameters table. It 
                 contains the configuration of the various E&M signaling
                 protocol timing parameters.
                "
        ::= { ccasGrpEMObjects 2 }

ccasGrpEMTmEntry OBJECT-TYPE
        SYNTAX      CcasGrpEMTmEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An entry in the E&M Timing Parameters Table for
                 each E&M interface."
        AUGMENTS   { ccasGrpEMCfgEntry }
        ::= { ccasGrpEMTmTable 1 }

CcasGrpEMTmEntry ::=
        SEQUENCE {
                ccasGrpEMTmClearWaitDuration        Integer32,
                ccasGrpEMTmMaxWinkWaitDuration      Integer32,
                ccasGrpEMTmMaxWinkDuration          Integer32,
                ccasGrpEMTmDelayStart               Integer32,
                ccasGrpEMTmMaxDelayDuration         Integer32,
                ccasGrpEMTmMinDelayPulseWidth       Integer32,
                ccasGrpEMTmDigitDuration            Integer32,
                ccasGrpEMTmInterDigitDuration       Integer32,
                ccasGrpEMTmPulseRate                Integer32,
                ccasGrpEMTmPulseInterDigitDuration  Integer32,
                ccasGrpEMTmVoiceHangover            Integer32,
                ccasGrpEMTmLmrTeardown              Integer32,
                ccasGrpEMTmPttXmt                   Integer32,
                ccasGrpEMTmPttRcv                   Integer32,
                ccasGrpEMTmDelayVoice               Integer32
        }


ccasGrpEMTmClearWaitDuration        OBJECT-TYPE
       SYNTAX     Integer32 (200..2000)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Time of Inactive incoming seizure signal to declare call
                cleared.
                This object is relevant to the interfaces in the CAS
                group if the ccasGrpCfgType object is emWinkStart(1) or
                emWinkStartFgd(2).
                The default value of this object is 400 milliseconds."
       ::= { ccasGrpEMTmEntry 1 }

ccasGrpEMTmMaxWinkWaitDuration        OBJECT-TYPE
       SYNTAX     Integer32 (100..5000)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Maximum wink wait duration for sending out wink start
                signaling. 
                This object is relevant to the interfaces in the CAS
                group if the ccasGrpCfgType object
                is emWinkStart(1) or emWinkStartFgd(2).
                The default value of this object is 200 milliseconds."
       ::= { ccasGrpEMTmEntry 2 }

ccasGrpEMTmMaxWinkDuration        OBJECT-TYPE
       SYNTAX     Integer32 (100..3000)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Maximum wink duration for sending out wink start
                signaling.
                This object is relevant to the interfaces in the CAS 
                group if the ccasGrpCfgType object is emWinkStart(1)
                or emWinkStartFgd(2).
                The default value of this object is 200 milliseconds."
       ::= { ccasGrpEMTmEntry 3 }

ccasGrpEMTmDelayStart        OBJECT-TYPE
       SYNTAX     Integer32 (20..2000)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Timing of generation of outgoing delayed start signal
                from detection of incoming seizure. 
                This object is relevant to the interfaces of the CAS
                group if the ccasGrpCfgType object is emDelayDial(4).
                The default value of this object is 300 milliseconds."
       ::= { ccasGrpEMTmEntry 4 }

ccasGrpEMTmMaxDelayDuration        OBJECT-TYPE
       SYNTAX     Integer32 (100..5000)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Maximum delay signal duration for sending out delay dial
                signaling. 
                This object is relevant to the interfaces in the CAS
                group if the ccasGrpCfgType object is emDelayDial(4).
                The default value of this object is 2000 milliseconds."
       ::= { ccasGrpEMTmEntry 5 }

ccasGrpEMTmMinDelayPulseWidth   OBJECT-TYPE
       SYNTAX     Integer32 (0 | 140..5000)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Minimum delay-dial pulse duration for incoming call.
                If the value of this object is 0, then no delay-dial
                is sent to the far end for the incoming call.
                This object is relevant to the interfaces in the CAS
                group if the ccasGrpCfgType object is emDelayDial(4).
                The default value of this object is 140 milliseconds."
       ::= { ccasGrpEMTmEntry 6 }

ccasGrpEMTmDigitDuration  OBJECT-TYPE
       SYNTAX     Integer32 (50..500)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Outgoing DTMF/MF digit duration in milliseconds.
                This object is not relevant to the addressing timing of
                the interfaces in the CAS group if ccasGrpCfgDialType
                is dtmf or R2 tone.
                The default value of this object is 100 milliseconds.
               " 
       ::= { ccasGrpEMTmEntry 7 }
 
ccasGrpEMTmInterDigitDuration  OBJECT-TYPE
       SYNTAX     Integer32 (50..500)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Outgoing DTMF/MF inter-digit duration in milliseconds.
                This object is not relevant to the addressing timing of
                the interfaces in the CAS group if ccasGrpCfgDialType
                is dtmf or R2 tone.
                The default value of this object is 100 milliseconds.
               " 
       ::= { ccasGrpEMTmEntry 8 }

ccasGrpEMTmPulseRate  OBJECT-TYPE
       SYNTAX     Integer32 (10..20)
       UNITS      "pulses per second"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Outgoing Pulse dialing rate in pulses per second (pps).
                This object is relevant to the addressing timing of the
                interfaces in the CAS group only if ccasGrpCfgDialType
                is pulse.
                The default value of this object is 10 pps.
               " 
       ::= { ccasGrpEMTmEntry 9 }
 
ccasGrpEMTmPulseInterDigitDuration  OBJECT-TYPE
       SYNTAX     Integer32 (100..1000)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Outgoing Pulse dialing inter-digit timing in
                milliseconds.
                This object is relevant to the addressing timing of the
                interfaces in the CAS group only if ccasGrpCfgDialType
                is pulse.
                The default value of this object is 500 milliseconds.
               " 
       ::= { ccasGrpEMTmEntry 10 }

ccasGrpEMTmVoiceHangover  OBJECT-TYPE
       SYNTAX     Integer32 (0..10000)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "The hangover time used to determine there is no more
                voice packet arrived.
                The default value of this object is 250 milliseconds.
               " 
       ::= { ccasGrpEMTmEntry 11 }

ccasGrpEMTmLmrTeardown  OBJECT-TYPE
       SYNTAX     Integer32 (-1 | 5..60000)
       UNITS      "seconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "LMR port tear down  timeout.
                This object is relevant to the waiting time of 
                teardown call on LMR port.
                If the value of this object is '-1', then the timeout
                is disable.
               " 
       DEFVAL { 1800 }
       ::= { ccasGrpEMTmEntry 12 }

ccasGrpEMTmPttXmt  OBJECT-TYPE
       SYNTAX     Integer32 (0..30)
       UNITS      "minutes"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "This object signifies LMR port maximum transmit time.
                This object is relevant to how long LMR port can
                continue transmit voice packet without pause.
               " 
       DEFVAL { 0 }
       ::= { ccasGrpEMTmEntry 13 }

ccasGrpEMTmPttRcv  OBJECT-TYPE
       SYNTAX     Integer32 (0..30)
       UNITS      "minutes"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "This object signifies LMR port maximum receive time.
                This object is relevant to how long LMR port can
                continue receive voice packet without pause.
               " 
       DEFVAL { 0 }
       ::= { ccasGrpEMTmEntry 14 }

ccasGrpEMTmDelayVoice  OBJECT-TYPE
       SYNTAX     Integer32 (0..1500)
       UNITS      "milliseconds"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "This object is relevant to how long LMR will delay
                sending the voice packet to the LMR port.
               " 
       DEFVAL { 0 }
       ::= { ccasGrpEMTmEntry 15 }

--*********************************************************************
-- The CAS Group FXS/SAS Standard Configuration Table
--*********************************************************************
ccasGrpLineCfgTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CcasGrpLineCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "The CAS Group FXS/SAS Standard Configuration Table.  It
                 contains the CAS FXS/SAS group standard configuration
                 information of T1/E1.
                "
        ::= { ccasGrpLineObjects 1 }

ccasGrpLineCfgEntry OBJECT-TYPE
        SYNTAX      CcasGrpLineCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An entry in the configuration table for each CAS
                 FXS/SAS Group in the T1/E1.
                 The entry is created when the ccasGrpCfgType is
                 configured as 'fxs' or 'sas' on a T1/E1 via
                 configuration command. The entry is deleted when the
                 CAS Group is de-configured from T1/E1.
                "
        INDEX   { ifIndex, ccasGrpCfgIndex }
        ::= { ccasGrpLineCfgTable 1 }

CcasGrpLineCfgEntry ::=
        SEQUENCE {
                ccasGrpLineCfgNumberRings      Integer32,    
                ccasGrpLineCfgSupDisconnect    TruthValue, 
                ccasGrpLineCfgDialType         INTEGER
        }


ccasGrpLineCfgNumberRings        OBJECT-TYPE
       SYNTAX     Integer32 (0..10)
       UNITS      "rings"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "The number of rings detected before closing loop.
                If the value of this object is 0, then the managed
                system answers immediately after the interface detects
                a incoming seizure if the ccasGrpCfgType is
                'fxsGroundStart' or 'sasGroundStart'.

                The default value of this object is 1 ring.
               "
       ::= { ccasGrpLineCfgEntry 1 }

ccasGrpLineCfgSupDisconnect OBJECT-TYPE
       SYNTAX  TruthValue
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               " Specifies whether a supervisory disconnect signal will 
                 be presented to the interface when the connected party
                 at the interface hangs up. this object is only relevant
                 to the ccasGrpCfgType is fxsLoopStart or sasLoopStart.
                 The default value of this object is 'true'.
               "
       ::= { ccasGrpLineCfgEntry 2 }

ccasGrpLineCfgDialType OBJECT-TYPE
        SYNTAX      INTEGER {
                    dtmf      (1),
                    pulse     (2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                "Specify the addressing type of the CAS group.
                 dtmf  - Dual Tone Multi-Frequency (DTMF) digit.
                 pulse - dial pulse.
                 The default value of this object is dtmf(1).
                "
        ::= { ccasGrpLineCfgEntry 3 }

--*********************************************************************
-- The FXS/SAS Timing Parameters Table
--*********************************************************************
-- This table contains the FXS/SAS interface timing parameters
-- information.

ccasGrpLineTmTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CcasGrpLineTmEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "The FXS/SAS interface Timing Parameters table. It
                 contains the configuration of the various FXS/SAS
                 signaling protocol timing parameters.
                "
        ::= { ccasGrpLineObjects 2 }

ccasGrpLineTmEntry OBJECT-TYPE
        SYNTAX      CcasGrpLineTmEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An entry in the FXS/SAS Timing Parameters Table for
                 each FXS/SAS interface."
        AUGMENTS   { ccasGrpLineCfgEntry }
        ::= { ccasGrpLineTmTable 1 }

CcasGrpLineTmEntry ::=
        SEQUENCE {
                ccasGrpLineTmDigitDuration               Integer32,
                ccasGrpLineTmInterDigitDuration          Integer32,
                ccasGrpLineTmPulseRate                   Integer32,
                ccasGrpLineTmPulseInterDigitDuration     Integer32
        }


ccasGrpLineTmDigitDuration  OBJECT-TYPE
       SYNTAX     Integer32 (50..500)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Outgoing DTMF digit duration in milliseconds.
                This object is not relevant to the addressing timing of
                the interfaces in the CAS group if ccasGrpLineCfgDialType
                is dtmf.
                The default value of this object is 100 milliseconds.
               " 
       ::= { ccasGrpLineTmEntry 1 }

ccasGrpLineTmInterDigitDuration  OBJECT-TYPE
       SYNTAX     Integer32 (50..500)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Outgoing DTMF inter-digit duration in milliseconds.
                This object is not relevant to the addressing timing
                of the interfaces in the CAS group if
                ccasGrpLineCfgDialType is dtmf.
                The default value of this object is 100 milliseconds.
               " 
       ::= { ccasGrpLineTmEntry 2 }

ccasGrpLineTmPulseRate  OBJECT-TYPE
       SYNTAX     Integer32 (10..20)
       UNITS      "pulses per second"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Outgoing Pulse dialing rate in pulses per second (pps).
                This object is relevant to the addressing timing of the
                interfaces in the CAS group only if ccasGrpStaCfgDialType
                is pulse.
                The default value of this object is 10 pps.
               " 
       ::= { ccasGrpLineTmEntry 3 }
 
ccasGrpLineTmPulseInterDigitDuration  OBJECT-TYPE
       SYNTAX     Integer32 (100..1000)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Outgoing Pulse dialing inter-digit timing in
                milliseconds. This object is relevant to the addressing
                timing of the interfaces in the CAS group only if
                ccasGrpStaCfgDialType is pulse.
                The default value of this object is 500 milliseconds.
               " 
       ::= { ccasGrpLineTmEntry 4 }


--*********************************************************************
-- The CAS Group FXO/SAO Standard Configuration Table
--*********************************************************************

-- This table contains the configuration information of FXO/SAO signal
-- interface.


ccasGrpStaCfgTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CcasGrpStaCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "The FXO/SAO standard configuration table. It contains
                 FXO/SAO configuration parameters, one entry per FXO/SAO
                 interface.
                 The configuration information of this table is set by 
                 its default setting when the CAS group is created by 
                 the configuration commands.
                "
        ::= { ccasGrpStaObjects 1 }

ccasGrpStaCfgEntry OBJECT-TYPE
        SYNTAX      CcasGrpStaCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An entry in the standard configuration table for
                 each FXO/SAO Group.
                 The entry is created when the ccasGrpCfgType is
                 configured as 'fxo' or 'sao' on a T1/E1 via
                 configuration command. The entry is deleted when the
                 CAS Group is de-configured from T1/E1.
                "
        INDEX   { ifIndex, ccasGrpCfgIndex }
        ::= { ccasGrpStaCfgTable 1 }

CcasGrpStaCfgEntry ::=
        SEQUENCE {
                ccasGrpStaCfgNumberRings       Integer32,
                ccasGrpStaCfgDialType          INTEGER
        }


ccasGrpStaCfgNumberRings        OBJECT-TYPE
       SYNTAX     Integer32 (0..1000)
       UNITS      "rings"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "The number of rings sent before sending reorder to the
                originator and releasing resources.
                If the value of this object is 0, then sending
                reorder to the originator is disabled. 
                The default value of this object is 20 rings.
               "
       ::= { ccasGrpStaCfgEntry 1 }

ccasGrpStaCfgDialType OBJECT-TYPE
        SYNTAX      INTEGER {
                    dtmf      (1),
                    pulse     (2)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                "Specify the addressing type of the CAS group.
                 dtmf  - Dual Tone Multi-Frequency (DTMF) digit.
                 pulse - dial pulse.
                 The default value of this object is dtmf(1).
                "
        ::= { ccasGrpStaCfgEntry 2 }
 

--*********************************************************************
-- The FXO/SAO Timing Parameters Table
--*********************************************************************
-- This table contains the FXO/SAO interface timing parameters
-- information.

ccasGrpStaTmTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CcasGrpStaTmEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "The FXO/SAO interface Timing Parameters table. It 
                 contains the configuration of the various FXO/SAO
                 signaling protocol timing parameters.
                "
        ::= { ccasGrpStaObjects 2 }

ccasGrpStaTmEntry OBJECT-TYPE
        SYNTAX      CcasGrpStaTmEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An entry in the FXO/SAO Timing Parameters Table for
                 each FXO/SAO interface."
        AUGMENTS   { ccasGrpStaCfgEntry }
        ::= { ccasGrpStaTmTable 1 }

CcasGrpStaTmEntry ::=
        SEQUENCE {
                ccasGrpStaTmDigitDuration               Integer32,
                ccasGrpStaTmInterDigitDuration          Integer32,
                ccasGrpStaTmPulseRate                   Integer32,
                ccasGrpStaTmPulseInterDigitDuration     Integer32
        }

ccasGrpStaTmDigitDuration  OBJECT-TYPE
       SYNTAX     Integer32 (50..500)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Outgoing DTMF digit duration in milliseconds.
                This object is not relevant to the addressing timing of
                the interfaces in the CAS group if ccasGrpStaCfgDialType
                is dtmf.
                The default value of this object is 100 milliseconds.
               " 
       ::= { ccasGrpStaTmEntry 1 }

ccasGrpStaTmInterDigitDuration  OBJECT-TYPE
       SYNTAX     Integer32 (50..500)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Outgoing DTMF inter-digit duration in milliseconds.
                This object is not relevant to the addressing timing of
                the interfaces in the CAS group if ccasGrpStaCfgDialType
                is dtmf.
                The default value of this object is 100 milliseconds.
               " 
       ::= { ccasGrpStaTmEntry 2 }

ccasGrpStaTmPulseRate  OBJECT-TYPE
       SYNTAX     Integer32 (10..20)
       UNITS      "pulses per second"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Outgoing Pulse dialing rate in pulses per second (pps).
                This object is relevant to the addressing timing of the
                interfaces in the CAS group only if ccasGrpStaCfgDialType
                is pulse.
                The default value of this object is 10 pps.
               " 
       ::= { ccasGrpStaTmEntry 3 }
 
ccasGrpStaTmPulseInterDigitDuration  OBJECT-TYPE
       SYNTAX     Integer32 (100..1000)
       UNITS      "milliseconds"
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Outgoing Pulse dialing inter-digit timing in
                milliseconds. This object is relevant to the addressing
                timing of the interfaces in the CAS group only if
                ccasGrpStaCfgDialType is pulse.
                The default value of this object is 500 milliseconds.
               " 
       ::= { ccasGrpStaTmEntry 4 }



--*********************************************************************
-- The CAS group associated custom ABCD bits configuration  Table
--*********************************************************************
-- This table contains the A/B/C/D bits handling parameters information.

ccasGrpABCDCfgTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CcasGrpABCDCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "The CAS group custom ABCD bits configuration table for
                 E1. It contains A/B/C/D bits handling objects, one
                 entry per CAS group on an E1 interface.
                "
        ::= { ccasGrpABCDObjects 1 }

ccasGrpABCDCfgEntry OBJECT-TYPE
        SYNTAX      CcasGrpABCDCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An entry in the custom ABCD configuration table for
                 each CAS Group on an E1 interface.
                 The entry is created when a CAS group is configured
                 on a E1. The entry is deleted when the CAS Group is 
                 de-configured from E1.
                "
        INDEX   { ifIndex, ccasGrpCfgIndex }
        ::= { ccasGrpABCDCfgTable 1 }

CcasGrpABCDCfgEntry ::=
        SEQUENCE {
                ccasGrpABCDCfgInvertBits         BITS,
                ccasGrpABCDCfgUnusedBits         BITS 
        }


ccasGrpABCDCfgInvertBits        OBJECT-TYPE
        SYNTAX      BITS {
                 dBit (0),
                 cBit (1), 
                 bBit (2),
                 aBit (3) 
        }
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Specify the A/B/C/D bit mask to invert the A/B/C/D bits
                value before the A/B/C/D bits are sent or
                after the A/B/C/D bits are received. 
                1-bit  - enable bit inversion.
                0-bit  - disable bit inversion.
                The default value of this object is '00'H.
               "
       ::= { ccasGrpABCDCfgEntry 1 }

ccasGrpABCDCfgUnusedBits OBJECT-TYPE
        SYNTAX      BITS {
                 dBit (0),
                 cBit (1), 
                 bBit (2),
                 aBit (3) 
        }
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
               "Specify the Unused A/B/C/D bit values to transmit.
                If any A/B/C/D bit is unused, the bit values in this
                object will be used to transmit for the unused 
                A/B/C/D bits.
                The default value of this object is '00'H 
               "
       ::= { ccasGrpABCDCfgEntry 2 }

--***********************************************************************
-- The CAS channel Standard Configuration Table
--***********************************************************************
ccasChannelCfgTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CcasChannelCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "The CAS channel Standard Configuration Table.  It
                 contains the standard configuration information of CAS
                 channel of T1/E1.
                "
        ::= { ccasChannelObjects 1 }

ccasChannelCfgEntry OBJECT-TYPE
        SYNTAX      CcasChannelCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An entry in the configuration table for each CAS
                 channel. The entry is created when a CAS channel is
                 configured on a T1/E1 via configuration command. The
                 entry is deleted when the CAS channel is de-configured
                 from T1/E1.
                "
        INDEX   { ifIndex }
        ::= { ccasChannelCfgTable 1 }

CcasChannelCfgEntry ::=
        SEQUENCE {
                ccasChannelCfgDS1IfIndex       InterfaceIndex,
                ccasChannelCfgGroup            Integer32,
                ccasChannelCfgTimeSlot         Integer32,
                ccasChannelCfgBusyOut          TruthValue         
        }

ccasChannelCfgDS1IfIndex OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "the ifIndex of this CAS channel associated T1/E1.     
                "
        ::= { ccasChannelCfgEntry 1 }

ccasChannelCfgGroup OBJECT-TYPE
        SYNTAX      Integer32 (0..30)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The CAS channel associated CAS group number.
                "
        ::= { ccasChannelCfgEntry 2 }

ccasChannelCfgTimeSlot OBJECT-TYPE
        SYNTAX      Integer32(1..31) 
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The CAS channel associated T1/E1 timeslot."
        ::= { ccasChannelCfgEntry 3 }

ccasChannelCfgBusyOut    OBJECT-TYPE
        SYNTAX      TruthValue         
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                "The CAS channel busyout configuration.
                 true  - the CAS channel is busied out.     
                 false - the CAS is normal.
                 The default value for this object is 'false'.
                "
        ::= { ccasChannelCfgEntry 4 }


--***********************************************************************
-- The CAS channel Status Table
--***********************************************************************
ccasChannelStatusTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CcasChannelStatusEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "The CAS channel Status Table.  It contains general 
                 information about the status of CAS channel.
                "
        ::= { ccasChannelObjects 2 }

ccasChannelStatusEntry OBJECT-TYPE
        SYNTAX      CcasChannelStatusEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An entry in the status table for each CAS channel. 
                "
        AUGMENTS   { ccasChannelCfgEntry }
        ::= { ccasChannelStatusTable 1 }

CcasChannelStatusEntry ::=
        SEQUENCE {
                ccasChannelStatusRecvSignalBits     BITS,
                ccasChannelStatusBusyOut            TruthValue,    
                ccasChannelStatusInfoType           INTEGER,
                ccasChannelStatusXmitSignalBits     BITS
        }

ccasChannelStatusRecvSignalBits OBJECT-TYPE
        SYNTAX      BITS {
                 dBit (0),
                 cBit (1), 
                 bBit (2),
                 aBit (3) 
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The receive ABCD signaling bits for the CAS channel.
                 aBit  - the signaling bit in the 6th frame
                 bBit  - the signaling bit in the 12th frame
                 cBit  - the signaling bit in the 18th frame
                 dBit  - the signaling bit in the 24th frame
                 the cBit and dBit are only valid for E1 or T1
                 interface is operating in extended superframe (ESF)
                 mode.
                "
        REFERENCE
            "EIA/TIA-464B, chapter 6.2 Digital Signaling and Supervision
            "
        ::= { ccasChannelStatusEntry 1 }

ccasChannelStatusBusyOut    OBJECT-TYPE
        SYNTAX      TruthValue         
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The CAS channel busyout state.
                 true  - the CAS channel is busied out.     
                 false - the CAS is normal.
                "
        ::= { ccasChannelStatusEntry 2 }

ccasChannelStatusInfoType              OBJECT-TYPE
        SYNTAX      INTEGER {
            unknown               (1),
            speech                (2),
            data56                (3),
            audio31               (4),
            audio7                (5),
            video                 (6),
            fax                   (7),
            modem                 (8)
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "The Information Transfer Capability for the current
             or last call.

             unknown  - If since system startup there has been no call
                        on this interface, this object has a value of
                        unknown(1).
             speech   - refers to a non-data connection
             data56   - 56k data.
             audio31  - audio 3.1 kHz; refers to data mode connections
             audio7   - audio 7 kHz; refer to data mode connections;
                        'Unrestricted digital information with tones/
                        announcements'.
             video    - as defined in Q.931
             fax      - Facsimile
             modem    - V.3x modem
            "
        REFERENCE
            "Q.931 [8], chapter 4.5.5, octet 3 of bearer capability
             information element, combined with the User Rate
             (as defined in octets 5 and 5a to 5d), if rate adoption
             is being used."
        ::= { ccasChannelStatusEntry 3 }

ccasChannelStatusXmitSignalBits OBJECT-TYPE
        SYNTAX      BITS {
                 dBit (0),
                 cBit (1), 
                 bBit (2),
                 aBit (3) 
        }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The transmit ABCD signaling bits for the CAS channel.
                 aBit  - the signaling bit in the 6th frame
                 bBit  - the signaling bit in the 12th frame
                 cBit  - the signaling bit in the 18th frame
                 dBit  - the signaling bit in the 24th frame
                 the cBit and dBit are only valid for E1 or T1 
                 interface is operating in extended superframe (ESF)
                 mode.
                "
        REFERENCE
            "EIA/TIA-464B, chapter 6.2 Digital Signaling and Supervision
            "
        ::= { ccasChannelStatusEntry 4 }


--  
-- Voice specific Configuration Table for a DS0 group 
--
ccasVoiceCfgTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CcasVoiceCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The voice specific configuration Table. It contains
             information about the voice related configuration
             parameters for a CAS group.
            "
       ::= { ccasVoiceCfgObjects 1 }

ccasVoiceCfgEntry OBJECT-TYPE
        SYNTAX      CcasVoiceCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry in the voice specific configuration table for each 
             CAS/DS0 group of a DS1.
             The entry is created if the associated CAS/DS0 group is
             created and the voice hardware is detected to support the
             voice capability for the CAS/DS0 group in the managed
             system.
             The entry is deleted when its associated CAS/DS0 group is
             deleted.
            "
        INDEX   { ifIndex, ccasGrpCfgIndex }
      ::= { ccasVoiceCfgTable 1 }

CcasVoiceCfgEntry ::=
        SEQUENCE {
            ccasVoiceCfgNoiseRegEnable         TruthValue, 
            ccasVoiceCfgNonLinearProcEnable    TruthValue, 
            ccasVoiceCfgMusicOnHoldThreshold   Integer32, 
            ccasVoiceCfgInGain                 Integer32,
            ccasVoiceCfgOutAttn                Integer32,
            ccasVoiceCfgEchoCancelEnable       TruthValue,
            ccasVoiceCfgEchoCancelCoverage     INTEGER,
            ccasVoiceCfgConnectionMode         INTEGER,
            ccasVoiceCfgConnectionNumber       DisplayString,
            ccasVoiceCfgInitialDigitTimeOut    Integer32,
            ccasVoiceCfgInterDigitTimeOut      Integer32,
            ccasVoiceCfgRegionalTone           CountryCode
        }

ccasVoiceCfgNoiseRegEnable OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The object indicates whether or not the background noise
             should be played to fill silence gaps if VAD is activated.
             The default value of this object is 'true'.
            "
        ::= { ccasVoiceCfgEntry 1 }


ccasVoiceCfgNonLinearProcEnable OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The object indicates whether or not the Nonlinear Processing
             is enabled for the interface.
             The default value of this object is 'true'.
            "
        ::= { ccasVoiceCfgEntry 2 }

ccasVoiceCfgMusicOnHoldThreshold OBJECT-TYPE
        SYNTAX      Integer32 (-70..-30)
        UNITS       "dBm" 
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The object specifies the Music On Hold Threshold for
             the interface.
             The default value of this object is -38 dBm.
            "
        ::= { ccasVoiceCfgEntry 3 }


ccasVoiceCfgInGain OBJECT-TYPE
       SYNTAX     Integer32 (-6..14)
       UNITS      "dB"
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
               "This object contains the amount of gain inserted at the
                receiver side of the interface. The input gain settings
                only define a gain/loss relative to the 0 dB setting.
                The absolute loss at the 0 dB setting could be
                implementation dependent based on the desired network
                loss plan.
                The default value of this object is 0 dB (decibel).
               "
        ::= { ccasVoiceCfgEntry 4 }

ccasVoiceCfgOutAttn OBJECT-TYPE
        SYNTAX      Integer32 (0..14)     
        UNITS      "dB"
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                "This object contains the amount of attenuation inserted
                 at the transmit side of the interface. 
                 The output attenuation settings only define a loss 
                 relative to the 0 dB setting.
                 The absolute loss at the 0 dB setting could be
                 implementation dependent based on the desired network
                 loss plan.
                 The default value of this object is 0 dB (decibel).
                "
        ::= { ccasVoiceCfgEntry 5 }

ccasVoiceCfgEchoCancelEnable OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The object specifies whether or not the Echo Cancellation 
             is enabled for the interface.
             The default value of this object is 'true'.
            "
        ::= { ccasVoiceCfgEntry 6 }

ccasVoiceCfgEchoCancelCoverage OBJECT-TYPE
        SYNTAX      INTEGER {
            echoCanceller8ms  (1),
            echoCanceller16ms (2),
            echoCanceller24ms (3),
            echoCanceller32ms (4),
            echoCanceller64ms (5),
            echoCanceller128ms(6)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The object specifies the Echo Canceller coverage for
             the interface. This object is valid if the
             ccasVoiceCfgEchoCancelEnable object is 'true'.
             echoCanceller8ms  -  8 milliseconds echo canceller coverage.
             echoCanceller16ms - 16 milliseconds echo canceller coverage.
             echoCanceller24ms - 24 milliseconds echo canceller coverage.
             echoCanceller32ms - 32 milliseconds echo canceller coverage.
             echoCanceller64ms -
                               64 milliseconds echo canceller coverage.
             echoCanceller128ms-
                              128 milliseconds echo canceller coverage.
             The default value of this object is echoCanceller8ms.
            "
        ::= { ccasVoiceCfgEntry 7 }

ccasVoiceCfgConnectionMode OBJECT-TYPE
        SYNTAX      INTEGER {
              normal  (1),
              trunk   (2),
              plar    (3)
        }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "The object indicates the connection mode of the interface.
             normal - the interface acts normally to handle incoming
                      and outgoing call.
             trunk  - the interface acts in trunking mode. trunking mode
                      causes two interfaces (on either the same or
                      different routers) to be always conferenced
                      together, and for telephony signaling to be
                      passed transparently through the VoIP system
                      rather than trapped and interpreted by the session
                      application on the router(s).
             plar   - the interface acts in PLAR (private line automatic
                      ringdown) mode. PLAR is handled by associating a
                      peer directly with an interface such that when the
                      interface goes off-hook, that peer is used to setup
                      the second call leg and conference them together
                      without the caller having to dial any digits.
            "
        ::= { ccasVoiceCfgEntry 8 }

ccasVoiceCfgConnectionNumber OBJECT-TYPE
        SYNTAX      DisplayString (SIZE (0..32))           
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "This is the E.164 phone number that is used to 
             establish connection with trunking mode or PLAR mode.
             If the ccasVoiceCfgConnectionMode is 'normal', then  this
             object will be a zero length string.
            "
        ::= { ccasVoiceCfgEntry 9 }

ccasVoiceCfgInitialDigitTimeOut OBJECT-TYPE
        SYNTAX      Integer32 (0..120)
        UNITS      "seconds"
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "This is the initial digit timeout that indicates the amount
             of time the managed system waits for an initial input digit
             from the caller. The timer is activated when the call is
             accepted and is deactivated upon digit input. If the timer
             expires, the caller is signaled through the appropriate
             tone and the call is abandoned. The value of zero disables
             the timer.
             The default value of this object is 10 seconds.
            "
        ::= { ccasVoiceCfgEntry 10 }

ccasVoiceCfgInterDigitTimeOut OBJECT-TYPE
        SYNTAX      Integer32 (0..120)
        UNITS      "seconds"
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
            "This is the inter-digit timeout that indicates the amount
             of time the managed system waits for a subsequent input
             digit from the caller. The timer is started upon receipt of
             an input digit and restarted as each digit is received
             until the destination address is identified. If the timer
             expires and no destination address is identified, the
             caller is signaled through the appropriate tone and the
             call is abandoned. The value of zero disables the timer.
             The default value of this object is 10 seconds.
            "
        ::= { ccasVoiceCfgEntry 11 }

ccasVoiceCfgRegionalTone OBJECT-TYPE
        SYNTAX      CountryCode      
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                "This object contains the current regional setting for
                 the call progress tone to be used by this CAS group.
                "
        ::= { ccasVoiceCfgEntry 12 }

--  
-- XGCP Configuration Table for a DS0 group 
--
ccasXgcpCfgTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF CcasXgcpCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "The XGCP configuration Table contains
             information about DS0 usage by XGCP(SGCP/MGCP).  
      
             XGCP is meant to represent both Simple Gateway Control
             Protocol (SGCP) and Media Gateway Control Protocol (MGCP).
            "
       ::= { ccasXgcpCfgObjects 1 }    

ccasXgcpCfgEntry OBJECT-TYPE
        SYNTAX      CcasXgcpCfgEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry in the configuration table for each 
             DS0 group of a DS1.

             The entry is created if the DS0 group is configured as   
             null-signaling and ccasGrpCfgServiceType is configured
             as either sgcp or mgcp.

             The entry is deleted when the signaling type is configured 
             as non null-signaling.
            "
        INDEX   { ifIndex, ccasGrpCfgIndex }
      ::= { ccasXgcpCfgTable 1 }


CcasXgcpCfgEntry ::=
        SEQUENCE {
            ccasXgcpCfgCotToneCo1             Integer32,
            ccasXgcpCfgCotToneCo2             Integer32
        }

ccasXgcpCfgCotToneCo1 OBJECT-TYPE
        SYNTAX      Integer32 (280..3800)
        UNITS       "hertz"
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                "This object specifies the continuity test tone
                 frequencies for co1. Co1 is the COT tone frequency from
                 the terminating switch in transponder mode and is from
                 the originating switch in loopback mode.
                "
        REFERENCE
            "Bellcore GR-317-CORE spec, Rev 3, Nov. 1996, section
             3.1.1.3. 
            "
        
        ::= { ccasXgcpCfgEntry 1 }
 
ccasXgcpCfgCotToneCo2 OBJECT-TYPE
        SYNTAX      Integer32 (280..3800)
        UNITS       "hertz"
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                "This object specifies the continuity test tone
                 frequencies for co2. Co2 is the COT tone frequency from
                 the originating switch only in transponder mode.  
                " 
        REFERENCE
            "Bellcore GR-317-CORE spec, Rev 3, Nov. 1996, section
             3.1.1.3. 
            "
        ::= { ccasXgcpCfgEntry 2 }



--***********************************************************************
-- Conformance and compliance statements
--***********************************************************************

-- conformance information

ccasIfMIBConformance
        OBJECT IDENTIFIER ::= { ciscoCasIfMIB 3 }
ccasIfMIBCompliances
        OBJECT IDENTIFIER ::= { ccasIfMIBConformance 1 }
ccasIfMIBGroups
        OBJECT IDENTIFIER ::= { ccasIfMIBConformance 2 }


-- compliance statements

ccasIfMIBCompliance MODULE-COMPLIANCE
        STATUS  obsolete   -- superseded by ccasIfMIBComplianceRev1 
        DESCRIPTION
                "The compliance statement for entities which implement
                 the Cisco Voice Digital interface MIB"
        MODULE  -- compliance to this module
                MANDATORY-GROUPS {
                   ccasIfDS1Group,
                   ccasGeneralInfoGroup
                }
                GROUP ccasEMGroup
                DESCRIPTION
                        "The CAS E&M group is mandatory for T1/E1 that
                         supports CAS E&M signal interface.
                        "
                GROUP ccasLineGroup
                DESCRIPTION
                        "The CAS Line group is mandatory for T1/E1 that
                         supports CAS FXO/SAO signal interfaces.
                        "
                GROUP ccasStaGroup
                DESCRIPTION
                        "The CAS Station group is mandatory for T1/E1
                         that supports CAS FXS/SAS signal interfaces.
                        "
                GROUP ccasCustomABCDGroup
                DESCRIPTION
                        "The CAS custom ABCD bits configuration group is
                         mandatory for E1 that supports CAS signal
                         interfaces.
                        "
                GROUP ccasVoiceGroup
                DESCRIPTION
                        "The CAS Voice group is mandatory for a CAS group
                         that supports voice/fax call capability.
                        "
                OBJECT  ccasGrpCfgType
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Create/Write access is not required."

                OBJECT   ccasGrpCfgDs0Channels
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Create/Write access is not required."

                OBJECT   ccasGrpCfgRowStatus
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Create/Write access is not required."

                OBJECT   ccasGrpEMCfgDialType
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasGrpEMCfgDnisAni
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."


                OBJECT   ccasGrpABCDCfgInvertBits
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasGrpABCDCfgUnusedBits
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."


                OBJECT   ccasVoiceCfgNoiseRegEnable
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasVoiceCfgNonLinearProcEnable
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasVoiceCfgMusicOnHoldThreshold
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasVoiceCfgInGain
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT    ccasVoiceCfgOutAttn
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasVoiceCfgEchoCancelEnable
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasVoiceCfgEchoCancelCoverage
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasVoiceCfgConnectionMode
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasVoiceCfgConnectionNumber
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasVoiceCfgInitialDigitTimeOut
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasVoiceCfgInterDigitTimeOut
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasVoiceCfgRegionalTone
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

        ::= { ccasIfMIBCompliances 1 }


ccasIfMIBComplianceRev1 MODULE-COMPLIANCE
        STATUS  deprecated   -- superseded by ccasIfMIBComplianceRev2
        DESCRIPTION
                "The compliance statement for entities which implement
                 the Cisco Voice Digital interface MIB"
        MODULE  -- compliance to this module
                MANDATORY-GROUPS {
                   ccasIfDS1Group,
                   ccasGeneralInfoGroupRev1
                }
                GROUP ccasEMGroupRev1
                DESCRIPTION
                        "The CAS E&M group is mandatory for T1/E1 that
                         supports CAS E&M signal interface.
                        "
                GROUP ccasLineGroup
                DESCRIPTION
                        "The CAS Line group is mandatory for T1/E1 that
                         supports CAS FXO/SAO signal interfaces.
                        "
                GROUP ccasStaGroup
                DESCRIPTION
                        "The CAS Station group is mandatory for T1/E1
                         that supports CAS FXS/SAS signal interfaces.
                        "
                GROUP ccasCustomABCDGroup
                DESCRIPTION
                        "The CAS custom ABCD bits configuration group is
                         mandatory for E1 that supports CAS signal
                         interfaces.
                        "
                GROUP ccasVoiceGroup
                DESCRIPTION
                        "The CAS Voice group is mandatory for a CAS
                         group that supports voice/fax call capability.
                        "
                GROUP ccasChannelInfoGroup
                DESCRIPTION
                        "The Channel Info group is mandatory for
                         providing channel signaling information
                         applicable to Channel Associated Signaling
                         interfaces.
                        "
                GROUP ccasXgcpCfgGroup 
                DESCRIPTION
                        "The XGCP Cfg group is mandatory for DS0 group
                         that supports XGCP protocol entity.
                        "
                OBJECT  ccasGrpCfgType
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Create/Write access is not required."

                OBJECT   ccasGrpCfgDs0Channels
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Create/Write access is not required."

                OBJECT   ccasGrpCfgRowStatus
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Create/Write access is not required."

                OBJECT   ccasGrpEMCfgDialType
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasGrpEMCfgDnisAni
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."


                OBJECT   ccasGrpABCDCfgInvertBits
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasGrpABCDCfgUnusedBits
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."


        ::= { ccasIfMIBCompliances 2 }

ccasIfMIBComplianceRev2 MODULE-COMPLIANCE
        STATUS  deprecated   -- superseded by ccasIfMIBComplianceRev3
        DESCRIPTION
                "The compliance statement for entities which implement
                 the Cisco Voice Digital interface MIB"
        MODULE  -- compliance to this module
                MANDATORY-GROUPS {
                   ccasIfDS1Group,
                   ccasGeneralInfoGroupRev1
                }
                GROUP ccasEMGroupRev1
                DESCRIPTION
                        "The CAS E&M group is mandatory for T1/E1 that
                         supports CAS E&M signal interface.
                        "
                GROUP ccasLineGroup
                DESCRIPTION
                        "The CAS Line group is mandatory for T1/E1 that
                         supports CAS FXO/SAO signal interfaces.
                        "
                GROUP ccasStaGroup
                DESCRIPTION
                        "The CAS Station group is mandatory for T1/E1
                         that supports CAS FXS/SAS signal interfaces.
                        "
                GROUP ccasCustomABCDGroup
                DESCRIPTION
                        "The CAS custom ABCD bits configuration group is
                         mandatory for E1 that supports CAS signal
                         interfaces.
                        "
                GROUP ccasVoiceGroup
                DESCRIPTION
                        "The CAS Voice group is mandatory for a CAS group
                         that supports voice/fax call capability.
                        "
                GROUP ccasChannelInfoGroup
                DESCRIPTION
                        "The Channel Info group is mandatory for
                         providing channel signaling information
                         applicable to Channel Associated Signaling
                         interfaces.
                        "
                GROUP ccasXgcpCfgGroup 
                DESCRIPTION
                        "The XGCP Cfg group is mandatory for DS0 group
                         that supports XGCP protocol entity.
                        "
                OBJECT  ccasGrpCfgType
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Create/Write access is not required."

                OBJECT   ccasGrpCfgDs0Channels
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Create/Write access is not required."

                OBJECT   ccasGrpCfgRowStatus
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Create/Write access is not required."

                OBJECT   ccasGrpEMCfgDialType
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasGrpEMCfgDnisAni
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."


                OBJECT   ccasGrpABCDCfgInvertBits
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasGrpABCDCfgUnusedBits
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."


        ::= { ccasIfMIBCompliances 3 }

ccasIfMIBComplianceRev3 MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
                "The compliance statement for entities which implement
                 the Cisco Voice Digital interface MIB"
        MODULE  -- compliance to this module
                MANDATORY-GROUPS {
                   ccasIfDS1Group,
                   ccasGeneralInfoGroupRev1
                }
                GROUP ccasEMGroupRev2
                DESCRIPTION
                        "The CAS E&M group is mandatory for T1/E1 that
                         supports CAS E&M signal interface.
                        "
                GROUP ccasLineGroup
                DESCRIPTION
                        "The CAS Line group is mandatory for T1/E1 that
                         supports CAS FXO/SAO signal interfaces.
                        "
                GROUP ccasStaGroup
                DESCRIPTION
                        "The CAS Station group is mandatory for T1/E1
                         that supports CAS FXS/SAS signal interfaces.
                        "
                GROUP ccasCustomABCDGroup
                DESCRIPTION
                        "The CAS custom ABCD bits configuration group is
                         mandatory for E1 that supports CAS signal
                         interfaces.
                        "
                GROUP ccasVoiceGroup
                DESCRIPTION
                        "The CAS Voice group is mandatory for a CAS
                         group that supports voice/fax call capability.
                        "
                GROUP ccasChannelInfoGroup
                DESCRIPTION
                        "The Channel Info group is mandatory for
                         providing channel signaling information
                         applicable to Channel Associated Signaling
                         interfaces.
                        "
                GROUP ccasXgcpCfgGroup 
                DESCRIPTION
                        "The XGCP Cfg group is mandatory for DS0 group
                         that supports XGCP protocol entity.
                        "
                OBJECT  ccasGrpCfgType
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Create/Write access is not required."

                OBJECT   ccasGrpCfgDs0Channels
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Create/Write access is not required."

                OBJECT   ccasGrpCfgRowStatus
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Create/Write access is not required."

                OBJECT   ccasGrpEMCfgDialType
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasGrpEMCfgDnisAni
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."


                OBJECT   ccasGrpABCDCfgInvertBits
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT   ccasGrpABCDCfgUnusedBits
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT  ccasGrpEMCfgLmrMCap
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT  ccasGrpEMCfgLmrECap
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."

                OBJECT  ccasGrpEMCfgAutoGainControl
                MIN-ACCESS  read-only
                DESCRIPTION
                        "Write access is not required."


        ::= { ccasIfMIBCompliances 4 }

-- units of conformance

ccasIfDS1Group OBJECT-GROUP
        OBJECTS {
                ccasDs1IfCfgDs0ChannelsConfigurable
        }
        STATUS  current
        DESCRIPTION
                "The collection of objects providing CAS/DS0 related 
                 T1/E1 information.
                "
        ::= { ccasIfMIBGroups 1 }

ccasGeneralInfoGroup OBJECT-GROUP
        OBJECTS {
                ccasGrpCfgType,
                ccasGrpCfgDs0Channels,
                ccasGrpCfgRowStatus,
                ccasChannelCfgDS1IfIndex,
                ccasChannelCfgGroup,
                ccasChannelCfgTimeSlot,
                ccasChannelCfgBusyOut,
                ccasChannelStatusRecvSignalBits,
                ccasChannelStatusBusyOut,
                ccasChannelStatusInfoType,
                ccasChannelStatusXmitSignalBits
        }
        STATUS  obsolete   -- superseded by ccasGeneralInfoGroupRev1
        DESCRIPTION
                "A collection of objects providing general information
                 applicable to Channel Associated Signaling interfaces.
                "
        ::= { ccasIfMIBGroups 2 }

ccasEMGroup OBJECT-GROUP
        OBJECTS {
                ccasGrpEMCfgDialType,
                ccasGrpEMCfgDnisAni,
                ccasGrpEMTmClearWaitDuration,
                ccasGrpEMTmMaxWinkWaitDuration,
                ccasGrpEMTmMaxWinkDuration,
                ccasGrpEMTmDelayStart,
                ccasGrpEMTmMaxDelayDuration,
                ccasGrpEMTmMinDelayPulseWidth,
                ccasGrpEMTmDigitDuration,
                ccasGrpEMTmInterDigitDuration,
                ccasGrpEMTmPulseRate,
                ccasGrpEMTmPulseInterDigitDuration
        }
        STATUS  deprecated  -- superceded by ccasEMGroupRev1
        DESCRIPTION
                "A collection of objects providing information applicable
                 to the CAS E&M signal interfaces.
                "
        ::= { ccasIfMIBGroups 3 }

ccasLineGroup OBJECT-GROUP
        OBJECTS {
                ccasGrpLineCfgNumberRings,    
                ccasGrpLineCfgSupDisconnect,
                ccasGrpLineCfgDialType,
                ccasGrpLineTmDigitDuration,
                ccasGrpLineTmInterDigitDuration,
                ccasGrpLineTmPulseRate,
                ccasGrpLineTmPulseInterDigitDuration
 
        }
        STATUS  current
        DESCRIPTION
                "A collection of objects providing information applicable
                 to the CAS FXS/SAS signal interfaces.
                "
        ::= { ccasIfMIBGroups 4 }

ccasStaGroup OBJECT-GROUP
        OBJECTS {
                ccasGrpStaCfgNumberRings,
                ccasGrpStaCfgDialType,
                ccasGrpStaTmDigitDuration,
                ccasGrpStaTmInterDigitDuration,
                ccasGrpStaTmPulseRate,
                ccasGrpStaTmPulseInterDigitDuration

        }
        STATUS  current
        DESCRIPTION
                "A collection of objects providing information applicable
                 to the CAS FXO/SAO signal interfaces.
                "
        ::= { ccasIfMIBGroups 5 }

ccasCustomABCDGroup OBJECT-GROUP
        OBJECTS {
                ccasGrpABCDCfgInvertBits, 
                ccasGrpABCDCfgUnusedBits
        }
        STATUS  current
        DESCRIPTION
                "A collection of objects providing ABCD bits
                 configuration information applicable to the CAS group
                 on E1 interface.
                "
        ::= { ccasIfMIBGroups 6 }

ccasVoiceGroup OBJECT-GROUP
        OBJECTS {
                ccasVoiceCfgNoiseRegEnable, 
                ccasVoiceCfgNonLinearProcEnable, 
                ccasVoiceCfgMusicOnHoldThreshold, 
                ccasVoiceCfgInGain,
                ccasVoiceCfgOutAttn,
                ccasVoiceCfgEchoCancelEnable,
                ccasVoiceCfgEchoCancelCoverage,
                ccasVoiceCfgConnectionMode,
                ccasVoiceCfgConnectionNumber,
                ccasVoiceCfgInitialDigitTimeOut,
                ccasVoiceCfgInterDigitTimeOut,
                ccasVoiceCfgRegionalTone

        }
        STATUS  current
        DESCRIPTION
                "A collection of objects providing information applicable
                 to the CAS/DS0 group that supports voice capability.
                "
        ::= { ccasIfMIBGroups 7 }

ccasGeneralInfoGroupRev1 OBJECT-GROUP
        OBJECTS {
                ccasGrpCfgType,
                ccasGrpCfgDs0Channels,
                ccasGrpCfgServiceType,
                ccasGrpCfgRowStatus
        }
        STATUS  current
        DESCRIPTION
                "A collection of objects providing general information
                 applicable to CAS/DS0 interfaces.
                "
        ::= { ccasIfMIBGroups 8 }

ccasChannelInfoGroup OBJECT-GROUP
        OBJECTS {
                ccasChannelCfgDS1IfIndex,
                ccasChannelCfgGroup,
                ccasChannelCfgTimeSlot,
                ccasChannelCfgBusyOut,
                ccasChannelStatusRecvSignalBits,
                ccasChannelStatusBusyOut,
                ccasChannelStatusInfoType,
                ccasChannelStatusXmitSignalBits
        }
        STATUS  current
        DESCRIPTION
                "A collection of objects providing channel signaling 
                 information applicable to Channel Associated Signaling 
                 interfaces.
                "
        ::= { ccasIfMIBGroups 9 }

ccasXgcpCfgGroup OBJECT-GROUP
        OBJECTS {
               ccasXgcpCfgCotToneCo1,
               ccasXgcpCfgCotToneCo2
        }
        STATUS  current
        DESCRIPTION
                "A collection of objects providing XGCP specific 
                 information applicable to DS0.
                "
        ::= { ccasIfMIBGroups 10 }

ccasEMGroupRev1 OBJECT-GROUP
        OBJECTS {
                ccasGrpEMCfgDialType,
                ccasGrpEMCfgDnisAni,
                ccasGrpEMTmClearWaitDuration,
                ccasGrpEMTmMaxWinkWaitDuration,
                ccasGrpEMTmMaxWinkDuration,
                ccasGrpEMTmDelayStart,
                ccasGrpEMTmMaxDelayDuration,
                ccasGrpEMTmMinDelayPulseWidth,
                ccasGrpEMTmDigitDuration,
                ccasGrpEMTmInterDigitDuration,
                ccasGrpEMTmPulseRate,
                ccasGrpEMTmPulseInterDigitDuration,
                ccasGrpEMCfgLmrMCap,
                ccasGrpEMCfgLmrECap,
                ccasGrpEMTmVoiceHangover,
                ccasGrpEMTmLmrTeardown
        }
        STATUS  deprecated  -- superceded by ccasEMGroupRev2
        DESCRIPTION
                "A collection of objects providing information
                 applicable to the CAS E&M signal interfaces.
                "
        ::= { ccasIfMIBGroups 11}

ccasEMGroupRev2 OBJECT-GROUP
        OBJECTS {
                ccasGrpEMCfgDialType,
                ccasGrpEMCfgDnisAni,
                ccasGrpEMTmClearWaitDuration,
                ccasGrpEMTmMaxWinkWaitDuration,
                ccasGrpEMTmMaxWinkDuration,
                ccasGrpEMTmDelayStart,
                ccasGrpEMTmMaxDelayDuration,
                ccasGrpEMTmMinDelayPulseWidth,
                ccasGrpEMTmDigitDuration,
                ccasGrpEMTmInterDigitDuration,
                ccasGrpEMTmPulseRate,
                ccasGrpEMTmPulseInterDigitDuration,
                ccasGrpEMCfgLmrMCap,
                ccasGrpEMCfgLmrECap,
                ccasGrpEMTmVoiceHangover,
                ccasGrpEMTmLmrTeardown,
                ccasGrpEMCfgAutoGainControl,
                ccasGrpEMTmPttXmt,
                ccasGrpEMTmPttRcv,
                ccasGrpEMTmDelayVoice
        }
        STATUS  current
        DESCRIPTION
                "A collection of objects providing information
                 applicable to the CAS E&M signal interfaces.
                "
        ::= { ccasIfMIBGroups 12}


END


