-- *******************************************************************
-- CISCO-LWAPP-MESH-LINKTEST-MIB.my
-- February 2007, Devesh Pujari
--   
-- Copyright (c) 2006, 2007, 2010 by Cisco Systems Inc.
-- All rights reserved.
-- *******************************************************************

CISCO-LWAPP-MESH-LINKTEST-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Unsigned32,
    Counter32,
    Integer32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    MacAddress,
    RowStatus
        FROM SNMPv2-TC
    ciscoMgmt
        FROM CISCO-SMI;


-- ********************************************************************
-- *  MODULE IDENTITY
-- ********************************************************************

ciscoLwappMeshLinkTestMIB MODULE-IDENTITY
    LAST-UPDATED    "201009300000Z"
    ORGANIZATION    "Cisco Systems Inc."
    CONTACT-INFO
            "Cisco Systems,
            Customer Service
            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA
            Tel: +1 800 553-NETS

            Email: cs-wnbu-snmp@cisco.com"
    DESCRIPTION
        "This MIB is intended to be implemented on all those
        devices operating as Central Controllers (CC) that
        terminate the Light Weight Access Point Protocol
        (LWAPP) tunnel from Light-weight  Access Points.

        Link Test is performed to learn the backhaul link 
        quality between two neighboring mesh nodes.

        The deployment of the controller 
        (referred to as CC in the diagram), mesh nodes 
        (RAP and MAP) LWAPP APs, client(MS) and NMS appear 
        as follows.

         +.......+                 +.......+
         +       +                 +       +
         +  NMS  +                 +  NMS  +
         +       +                 +       +
         +.......+                 +.......+
            .                         .
         .    .                     .   .
        .         .                .        .
        .            .             .            .
        +......+     +......+     +......+           +......+
        +      +     +      +     +      +           +      +
        +  CC  +     +  CC  +     +  CC  +           +  CC  +
        +      +     +      +     +      +           +      +
        +......+     +......+     +......+           +......+
        ..            .             .                 .
        ..            .             .                 .
        .  .            .             .                 .
        .    .            .             .                 .
        .      .            .             .                 .
        .        .            .             .                 .
        +......+ +......+     +......+      +......+          +......+
        +      + +      +     +      +      +      +          +      +
        +  RAP + +  RAP +     +  RAP  +     +  RAP +          +  RAP +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+
        .        .              .             .                 .
        .        .              .             .                 .
        .        .              .             .                 .
        .          .              .             .                 .
        .           .              .             .                 .
        +......+ +......+     +......+      +......+          +......+
        +      + +      +     +      +      +      +          +      +
        +  MAP + +  MS  +     +  MAP +      +  MAP +          +  MAP +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+
        .                    .                          ..    . 
        . .                  .                     ..        .
        .   .                .                  ..            .
        .     .              .              .                .
        +......+ +......+     +......+      +......+.         +......+
        +      + +      +     +      +      +      +          +      +
        +  MAP + +  MAP +     +  MAP +      +  MAP +          +  MS  +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+




        The LWAPP tunnel exists between the controller and
        the APs. The MNs communicate with the APs through
        the protocol defined by the 802.11 standard.

        LWAPP APs, upon bootup, discover and join one of the
        controllers and the controller pushes the 
        configuration, that includes the WLAN parameters to 
        the LWAPP APs. 
        The APs encapsulate all the 802.11 frames from
        wireless clients inside LWAPP frames and forward
        the LWAPP frames to the controller.

                           GLOSSARY

        Access Point ( AP )

        An entity that contains an 802.11 medium access
        control ( MAC ) and physical layer ( PHY ) interface
        and provides access to the distribution services via
        the wireless medium for associated clients.
        LWAPP APs encapsulate all the 802.11 frames in
        LWAPP frames and sends them to the controller to which
        it is logically connected.

        Central Controller ( CC )

        The central entity that terminates the LWAPP protocol
        tunnel from the LWAPP APs. Throughout this MIB,
        this entity is also referred to as 'controller'.

        Mobile Station ( MS )

        A roaming 802.11 wireless device in a wireless
        network associated with an access point. Mobile Station
        and client are used interchangeably. 

        Network Management System ( NMS )

        The station from which the administrator manages the
        wired and wireless networks.

        Mesh Node

        A mesh node is defined as a physical or logical entity
        in the mesh network participating in forming the mesh 
        backhaul. There are two types of mesh nodes supported 
        in Cisco mesh network:RAP and MAP.

        Root AP (RAP)

        The AP forming the bridge between a wired and a mesh
        network with an Ethernet interface to the wired 
        network and a 802.11 radio interface to the mesh 
        network

        Mesh AP (MAP).

        The AP extending wireless coverage similar to a 
        repeater in a mesh network and consists of a 802.11 
        uplink and a 802.11 downlink. On a single-radio 
        backhaul, both uplink and downlink exist on the same 
        radio and are logical links only. On a multi-radio 
        backhaul, they may exist on different radios.

        Mesh Network

        Network starting with the wireless backhaul downlink
        of the RAP and all the entities below except any 
        attached network to the Ethernet link of MAPs. A mesh 
        network below a single RAP is also referred to as a 
        'Mesh Sector'.A mesh network consists of mesh nodes. 
        A single mesh network is always augmented to a single 
        wired network.

        Mesh Link

        A logical 802.11 link between two mesh nodes. A single 
        link is point-to-point. All point-to-multipoint links 
        are considered as multiple mesh links. Often referred 
        to as mesh backhaul link.

        Mesh Backhaul

        A Mesh backhaul consists of mesh nodes and mesh links 
        terminating at a RAP. This necessarily creates a one-
        to-one relationship between a 'mesh network', 'mesh
        sector' and a 'mesh backhaul' where these terms can be 
        used interchangeably.

        SNR
        Signal to Noise ratio on the 802.11 radio.

        RSSI 
        Received Signal Strength Indication (RSSI), the IEEE 802.11 
        standard defines a mechanism by which RF energy is to be 
        measured by the circuitry on a wireless NIC. Its value is
        measured in dBm and ranges from -128 to 0.

        Bridged network 
        The bridged network is defined as the network(s)
        attached to the Ethernet port of any MAP. There can be
        multiple such networks attached to a single mesh 
        network.

        Mesh Node Roaming
        A mesh node may change its parent mesh node naturally 
        when the RF/network condition changes.Child Mesh node 
        will re-associate and re-authenticate to new parent 
        mesh node. Mesh Security supports two types of mesh 
        node roaming:
        Intra-controller roaming: LWAPP session remains and 
        no LWAPP session roam is necessary
        Inter-controller roaming: LWAPP session is lost and 
        LWAPP session roam may be necessary

        REFERENCE

        [1] Wireless LAN Medium Access Control ( MAC ) and
        Physical Layer ( PHY ) Specifications.

        [2] Draft-obara-capwap-lwapp-00.txt, IETF Light 
        Weight Access Point Protocol"
    REVISION        "201009300000Z"
    DESCRIPTION
        "Deprecated clMeshLtDataRate and replaced it with 
        clMeshLtDataRateValue.
        
        Deprecated ciscoLwappMeshLinkTestRunGroup and
        ciscoLwappMeshLinkTestMIBCompliance.
        
        Added ciscoLwappMeshLinkTestRunGroupRev1 and
        ciscoLwappMeshLinkTestMIBComplianceRev1."
    REVISION        "200702050000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 606 }


ciscoLwappMeshLinkTestMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshLinkTestMIB 0 }

ciscoLwappMeshLinkTestMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshLinkTestMIB 1 }

ciscoLwappMeshLinkTestMIBConform  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshLinkTestMIB 2 }

ciscoLwappMeshLinkTestConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshLinkTestMIBObjects 1 }

ciscoLwappMeshLinkTestRun  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshLinkTestMIBObjects 2 }

ciscoLwappMeshLinkTestStatus  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshLinkTestMIBObjects 3 }


-- ********************************************************************
-- *    Link Test global configurations
-- ********************************************************************

clMeshLtPurgeTime OBJECT-TYPE
    SYNTAX          Unsigned32 (15..1800)
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates the duration for which the
        results of a particular run of linktest is available
        in clMeshLtResultsTable from the time of completion 
        of that run of linktest.  At the expiry of this time, 
        after the completion of the linktest, the entries 
        corresponding to the linktest and the corresponding 
        results are removed from clMeshLtTable and 
        clMeshLtResultsTable respectively."
    DEFVAL          { 60 } 
    ::= { ciscoLwappMeshLinkTestConfig 1 }
-- ********************************************************************
-- * Mesh Link Test
-- ********************************************************************

clMeshLtTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF ClMeshLtEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table is used to initiate linktests between
        two neighbor mesh node AP.                

        With LinkTest support, the controller can test
        the backhaul link.

        User initiates one run of linktest by adding a
        row to this table through explicit management 
        action from the network manager.  A row is created
        by specifying clMeshLtIndex,
        clMeshLtSrcMacAddress and clMeshLtDestMacAddress 
        setting the RowStatus object to 'createAndGo'.
        This indicates the the request made to start the 
        linktest between two mesh nodes.

        The added row is deleted by setting the corresponding
        instance of the RowStatus object to 'destroy'.  In
        case if the agent finds that the time duration
        represented by clMeshLtPurgeTime has elapsed since
        the completion of the linktest, it proceeds to
        delete the row automatically, if the row exists at
        that point of time.

        The results of the linktest identified by 
        clMeshLtIndex can be obtained from the queries to 
        clMeshLtResultsTable."
    ::= { ciscoLwappMeshLinkTestRun 1 }

clMeshLtEntry OBJECT-TYPE
    SYNTAX          ClMeshLtEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents one instance
        of the linktest initiated by the user through
        a network manager."
    INDEX           { clMeshLtIndex } 
    ::= { clMeshLtTable 1 }

ClMeshLtEntry ::= SEQUENCE {
        clMeshLtIndex          Unsigned32,
        clMeshLtSrcMacAddress  MacAddress,
        clMeshLtDestMacAddress MacAddress,
        clMeshLtDataRate       Unsigned32,
        clMeshLtPktsPerSec     Unsigned32,
        clMeshLtPktSize        Unsigned32,
        clMeshLtDuration       Unsigned32,
        clMeshLtRowStatus      RowStatus,
        clMeshLtDataRateValue  INTEGER
}

clMeshLtIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..16)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies one particular
        run of the linktest initiated between the two mesh 
        node neighbors identified by clMeshLtSrcMacAddress 
        and clMeshLtDestMacAddress." 
    ::= { clMeshLtEntry 1 }

clMeshLtSrcMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the source mac address of AP
        which initiates the link test to 
        'clMeshLtDestMacAddress' involved in the particular run 
        of linktest. This object must be set to a valid value 
        when setting clMeshLtRowStatus to 'createAndGo' to 
        initiate a run of linktest." 
    ::= { clMeshLtEntry 2 }

clMeshLtDestMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the destination mac address of
        AP involved in the particular run of linktest. This
        object must be set to a valid value when setting
        clMeshLtRowStatus to 'createAndGo' to initiate a
        run of linktest." 
    ::= { clMeshLtEntry 3 }

clMeshLtDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "Mbps"
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "This object represents the data rate on backhaul link
        at which link test will be performed. Depending on the 
        backhaul radio type, data rate will vary. if the 
        backhaul radio is 802.11a, data rates can be 
        one of the following possible values. 
        Rates - 6,9,11,12,18,24,36,48,54,108 Mbps. If backhaul 
        link is 802.11b then data rate can be 1,2,5.5,6,9,11 
        If backhaul link is 802.11g 
        1,2,5.5,6,9,11,12,18,24,36,48,54,108. This
        object must be set to a valid value when setting
        clMeshLtRowStatus to 'createAndGo' to initiate a
        run of linktest. This object is deprecated and 
        superceded by clMeshLtDataRateValue object." 
    ::= { clMeshLtEntry 4 }

clMeshLtPktsPerSec OBJECT-TYPE
    SYNTAX          Unsigned32 (1..3000)
    UNITS           "packets"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the number of packets to be
        sent per sec during link test."
    DEFVAL          { 1000 } 
    ::= { clMeshLtEntry 5 }

clMeshLtPktSize OBJECT-TYPE
    SYNTAX          Unsigned32 (1..1500)
    UNITS           "bytes"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the size of packets to be sent
        during link test."
    DEFVAL          { 1500 } 
    ::= { clMeshLtEntry 6 }

clMeshLtDuration OBJECT-TYPE
    SYNTAX          Unsigned32 (15..60)
    UNITS           "seconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the duration, in seconds, of link
        test to be performed."
    DEFVAL          { 30 } 
    ::= { clMeshLtEntry 7 }

clMeshLtRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is the status column used for creating
        and deleting  instances of the columnar objects in
        this table." 
    ::= { clMeshLtEntry 8 }

clMeshLtDataRateValue OBJECT-TYPE
    SYNTAX          INTEGER  {
                        mbps1(1),
                        mbps2(2),
                        mbps5point5(3),
                        mbps6(4),
                        mbps9(5),
                        mbps11(6),
                        mbps12(7),
                        mbps18(8),
                        mbps24(9),
                        mbps36(10),
                        mbps48(11),
                        mbps54(12),
                        mbps108(13),
                        htMcs0(14),
                        htMcs1(15),
                        htMcs2(16),
                        htMcs3(17),
                        htMcs4(18),
                        htMcs5(19),
                        htMcs6(20),
                        htMcs7(21),
                        htMcs8(22),
                        htMcs9(23),
                        htMcs10(24),
                        htMcs11(25),
                        htMcs12(26),
                        htMcs13(27),
                        htMcs14(28),
                        htMcs15(29)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the data rate on backhaul link
        at which link test will be performed. Depending on the 
        backhaul radio type, data rate will vary. 

        If the value of clMeshNodeBackhaul object
        is 'dot11a', data rates can be one of the 
        following possible values. 
        mbps6(4)
        mbps9(5)
        mbps12(7)
        mbps18(8)
        mbps24(9)
        mbps36(10)
        mbps48(11)
        mbps54(12)
        mbps108(13)

        Additionally following data rates are supported if 802.11a 
        supports 11n.
        htMcs0(14)
        htMcs1(15)
        htMcs2(16)
        htMcs3(17)
        htMcs4(18)
        htMcs5(19)
        htMcs6(20)
        htMcs7(21)
        htMcs8(22)
        htMcs9(23)
        htMcs10(24)
        htMcs11(25)
        htMcs12(26)
        htMcs13(27)
        htMcs14(28)
        htMcs15(29)

        If the value of clMeshNodeBackhaul object
        is 'dot11b', then data rate can be one of 
        the following possible values.
        mbps1(1)
        mbps2(2)
        mbps5point5(3)
        mbps6(4)
        mbps9(5)
        mbps11(6)

        If the value of clMeshNodeBackhaul object
        is 'dot11g', then data rate can be one of
        the following possible values.

        mbps1(1)
        mbps2(2)
        mbps5point5(3)
        mbps6(4)
        mbps9(5)
        mbps11(6)
        mbps12(7)
        mbps18(8)
        mbps24(9)
        mbps36(10)
        mbps48(11)
        mbps54(12)
        mbps108(13)

        This object cannot be modified when the value 
        of clMeshLtRowStatus object in the same row is 'active'." 
    ::= { clMeshLtEntry 9 }
 

-- ********************************************************************
-- * Mesh Link Test Results
-- ********************************************************************

clMeshLtResultsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF ClMeshLtResultsEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table populates the results of the mesh
        linktests initiated by the user through the 
        clMeshLtTable.  

        This table has a sparse dependent relationship
        with clMeshLtEntry. There exists a row in this 
        table corresponding to each row in clMeshLtEntry 
        identified by clMeshLtIndex.  A row is added to this
        table when user, through the network manager, adds
        a row to clMeshLtEntry and initiates one run of 
        linktest. A row can be deleted by the agent when the 
        corresponding row of clMeshLtEntry is deleted or 
        it will get deleted when the clMeshLtPurgeTime expires.

        The manager is expected to poll clMeshLtStatus
        to check the status of the linktest."
    ::= { ciscoLwappMeshLinkTestStatus 1 }

clMeshLtResultsEntry OBJECT-TYPE
    SYNTAX          ClMeshLtResultsEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the results
        of the linktest identified by clMeshLtIndex."
    INDEX           { clMeshLtIndex } 
    ::= { clMeshLtResultsTable 1 }

ClMeshLtResultsEntry ::= SEQUENCE {
        clMeshLtTxPkts              Counter32,
        clMeshLtRxPkts              Counter32,
        clMeshLtRxGoodPkts          Counter32,
        clMeshLtRxDupPkts           Counter32,
        clMeshLtRxShortPkts         Counter32,
        clMeshLtRxBigPkts           Counter32,
        clMeshLtRxPhyErrPkts        Counter32,
        clMeshLtRxCRCErrPkts        Counter32,
        clMeshLtRxSeqErrPkts        Counter32,
        clMeshLtRxAvgSNR            Integer32,
        clMeshLtRxHighestSNR        Integer32,
        clMeshLtRxLowestSNR         Integer32,
        clMeshLtRxAvgNoiseFloor     Integer32,
        clMeshLtRxHighestNoiseFloor Integer32,
        clMeshLtRxLowestNoiseFloor  Integer32,
        clMeshLtRxAvgRSSI           Integer32,
        clMeshLtRxHighestRSSI       Integer32,
        clMeshLtRxLowestRSSI        Integer32,
        clMeshLtStatus              INTEGER
}

clMeshLtTxPkts OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of packets sent to the destination
        mesh node specified by clMeshLtDestMacAddress from AP 
        specified by clMeshLtSrcMacAddress." 
    ::= { clMeshLtResultsEntry 1 }

clMeshLtRxPkts OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of packets received by mesh
        node specified by clMeshLtDestMacAddress from mesh 
        node specified by clMeshLtSrcMacAddress." 
    ::= { clMeshLtResultsEntry 2 }

clMeshLtRxGoodPkts OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of packets received without any
        errors by mesh node specified by clMeshLtDestMacAddress 
        from mesh node AP specified by clMeshLtSrcMacAddress ." 
    ::= { clMeshLtResultsEntry 3 }

clMeshLtRxDupPkts OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of packets received with same
        sequence number by mesh node specified by 
        clMeshLtDestMacAddress from mesh node specified by 
        clMeshLtSrcMacAddress." 
    ::= { clMeshLtResultsEntry 4 }

clMeshLtRxShortPkts OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of packets received that were
        shorter than the 802.11 frame size by mesh node specified 
        by clMeshLtDestMacAddress from mesh node specified by 
        clMeshLtSrcMacAddress." 
    ::= { clMeshLtResultsEntry 5 }

clMeshLtRxBigPkts OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of packets received that were
        larger than the 802.11 frame size by mesh node specified 
        by clMeshLtDestMacAddress from mesh node specified by 
        clMeshLtSrcMacAddress." 
    ::= { clMeshLtResultsEntry 6 }

clMeshLtRxPhyErrPkts OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of packets with error detected at
        physical layer received by mesh node specified by 
        clMeshLtDestMacAddress from mesh node specified by 
        clMeshLtSrcMacAddress." 
    ::= { clMeshLtResultsEntry 7 }

clMeshLtRxCRCErrPkts OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of packets with CRC error
        received by mesh node specified by 
        clMeshLtDestMacAddress from mesh node specified 
        by clMeshLtSrcMacAddress." 
    ::= { clMeshLtResultsEntry 8 }

clMeshLtRxSeqErrPkts OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "packets"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of packets that were received with
        sequence number out of order by mesh node specified by 
        clMeshLtDestMacAddress from mesh node specified by 
        clMeshLtSrcMacAddress." 
    ::= { clMeshLtResultsEntry 9 }

clMeshLtRxAvgSNR OBJECT-TYPE
    SYNTAX          Integer32
    UNITS           "dB"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The average SNR value observed at the mesh node
        specified by clMeshLtDestMacAddress." 
    ::= { clMeshLtResultsEntry 10 }

clMeshLtRxHighestSNR OBJECT-TYPE
    SYNTAX          Integer32
    UNITS           "dB"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The highest SNR value observed at the mesh node
        specified by clMeshLtDestMacAddress." 
    ::= { clMeshLtResultsEntry 11 }

clMeshLtRxLowestSNR OBJECT-TYPE
    SYNTAX          Integer32
    UNITS           "dB"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The lowest SNR value observed at the mesh node specified
        by clMeshLtDestMacAddress." 
    ::= { clMeshLtResultsEntry 12 }

clMeshLtRxAvgNoiseFloor OBJECT-TYPE
    SYNTAX          Integer32
    UNITS           "dB"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The average noise floor value observed at the
        mesh node specified by clMeshLtDestMacAddress. 
        The noise floor is the measure of the signal created 
        from the sum of all the noise sources and unwanted 
        signals within a measurement system." 
    ::= { clMeshLtResultsEntry 13 }

clMeshLtRxHighestNoiseFloor OBJECT-TYPE
    SYNTAX          Integer32
    UNITS           "dB"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The highest Noise Floor value observed at the mesh node
        specified by clMeshLtDestMacAddress. The noise floor is the 
        measure of the signal created from the sum of all the 
        noise sources and unwanted signals within a 
        measurement system." 
    ::= { clMeshLtResultsEntry 14 }

clMeshLtRxLowestNoiseFloor OBJECT-TYPE
    SYNTAX          Integer32
    UNITS           "dB"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The lowest Noise Floor value observed at the mesh node
        specified by clMeshLtDestMacAddress. The noise floor is the 
        measure of the signal created from the sum of all the
        noise sources and unwanted signals within a 
        measurement system." 
    ::= { clMeshLtResultsEntry 15 }

clMeshLtRxAvgRSSI OBJECT-TYPE
    SYNTAX          Integer32
    UNITS           "dBm"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The average RSSI value observed at the mesh node
        specified by clMeshLtDestMacAddress." 
    ::= { clMeshLtResultsEntry 16 }

clMeshLtRxHighestRSSI OBJECT-TYPE
    SYNTAX          Integer32
    UNITS           "dBm"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The highest RSSI value observed at the mesh node
        specified by clMeshLtDestMacAddress." 
    ::= { clMeshLtResultsEntry 17 }

clMeshLtRxLowestRSSI OBJECT-TYPE
    SYNTAX          Integer32
    UNITS           "dBm"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The lowest RSSI value as observed at the mesh node
        specified by clMeshLtDestMacAddress." 
    ::= { clMeshLtResultsEntry 18 }

clMeshLtStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        clMeshLtStatusFailed(1),
                        clMeshLtStatusInProgress(2),
                        clMeshLtStatusSuccess(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the status of the linktest
        this particular entry corresponds to.

        The semantics as follows.

        'clMeshLtStatusFailed' - This value indicates that
        this particular linktest has failed. 

        'clMeshLtStatusInProgress' - This value indicates
        that the linktest is in progress.

        'clMeshLtStatusSuccess' - This value indicates
        that linktest has succeeded." 
    ::= { clMeshLtResultsEntry 19 }
 

-- ********************************************************************
-- *    Compliance statements
-- ********************************************************************

ciscoLwappMeshLinkTestMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshLinkTestMIBConform 1 }

ciscoLwappMeshLinkTestMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoLwappMeshLinkTestMIBConform 2 }


ciscoLwappMeshLinkTestMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappMeshLinkTestMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappMeshLinkTestConfigGroup,
                        ciscoLwappMeshLinkTestRunGroup
                    }
    ::= { ciscoLwappMeshLinkTestMIBCompliances 1 }

ciscoLwappMeshLinkTestMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappMeshLinkTestMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappMeshLinkTestConfigGroup,
                        ciscoLwappMeshLinkTestRunGroupRev1
                    }
    ::= { ciscoLwappMeshLinkTestMIBCompliances 2 }

-- ********************************************************************
-- *    Units of conformance
-- ********************************************************************

ciscoLwappMeshLinkTestConfigGroup OBJECT-GROUP
    OBJECTS         { clMeshLtPurgeTime }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the linktest
        parameters for configuration and result."
    ::= { ciscoLwappMeshLinkTestMIBGroups 1 }

ciscoLwappMeshLinkTestRunGroup OBJECT-GROUP
    OBJECTS         {
                        clMeshLtSrcMacAddress,
                        clMeshLtDestMacAddress,
                        clMeshLtDataRate,
                        clMeshLtPktsPerSec,
                        clMeshLtPktSize,
                        clMeshLtDuration,
                        clMeshLtRowStatus,
                        clMeshLtTxPkts,
                        clMeshLtRxPkts,
                        clMeshLtRxGoodPkts,
                        clMeshLtRxDupPkts,
                        clMeshLtRxShortPkts,
                        clMeshLtRxBigPkts,
                        clMeshLtRxPhyErrPkts,
                        clMeshLtRxCRCErrPkts,
                        clMeshLtRxSeqErrPkts,
                        clMeshLtRxAvgSNR,
                        clMeshLtRxHighestSNR,
                        clMeshLtRxLowestSNR,
                        clMeshLtRxAvgNoiseFloor,
                        clMeshLtRxHighestNoiseFloor,
                        clMeshLtRxLowestNoiseFloor,
                        clMeshLtRxAvgRSSI,
                        clMeshLtRxHighestRSSI,
                        clMeshLtRxLowestRSSI,
                        clMeshLtStatus
                    }
    STATUS          deprecated
    DESCRIPTION
        "This collection of objects is used to initiate
        linktests and retrieve the results of the respective
        runs of the link test."
    ::= { ciscoLwappMeshLinkTestMIBGroups 2 }
    
ciscoLwappMeshLinkTestRunGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        clMeshLtSrcMacAddress,
                        clMeshLtDestMacAddress,
                        clMeshLtDataRateValue,
                        clMeshLtPktsPerSec,
                        clMeshLtPktSize,
                        clMeshLtDuration,
                        clMeshLtRowStatus,
                        clMeshLtTxPkts,
                        clMeshLtRxPkts,
                        clMeshLtRxGoodPkts,
                        clMeshLtRxDupPkts,
                        clMeshLtRxShortPkts,
                        clMeshLtRxBigPkts,
                        clMeshLtRxPhyErrPkts,
                        clMeshLtRxCRCErrPkts,
                        clMeshLtRxSeqErrPkts,
                        clMeshLtRxAvgSNR,
                        clMeshLtRxHighestSNR,
                        clMeshLtRxLowestSNR,
                        clMeshLtRxAvgNoiseFloor,
                        clMeshLtRxHighestNoiseFloor,
                        clMeshLtRxLowestNoiseFloor,
                        clMeshLtRxAvgRSSI,
                        clMeshLtRxHighestRSSI,
                        clMeshLtRxLowestRSSI,
                        clMeshLtStatus
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects is used to initiate
        linktests and retrieve the results of the respective
        runs of the link test."
    ::= { ciscoLwappMeshLinkTestMIBGroups 3 }


END





