-- *******************************************************************
-- CISCO-LWAPP-ROGUE-MIB.my
-- February 2007, Devesh Pujari, Srinath Candadai
--   
-- Copyright (c) 2007, 2010-2014 by Cisco Systems Inc.
-- All rights reserved.
-- *******************************************************************

CISCO-LWAPP-ROGUE-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    NOTIFICATION-TYPE,
    OBJECT-TYPE,
    Integer32,
    Unsigned32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    NOTIFICATION-GROUP,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    StorageType,
    RowStatus,
    MacAddress,
    TruthValue,
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    cLApName
        FROM CISCO-LWAPP-AP-MIB
    ciscoMgmt
        FROM CISCO-SMI;


ciscoLwappRogueMIB MODULE-IDENTITY
    LAST-UPDATED    "201407140000Z"
    ORGANIZATION    "Cisco Systems Inc."
    CONTACT-INFO
            "Cisco Systems,
            Customer Service
            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA
            Tel: +1 800 553-NETS

            Email: cs-wnbu-snmp@cisco.com"
    DESCRIPTION
        "This MIB is intended to be implemented on all those
        devices operating as Central Controllers, that
        terminate the Light Weight Access Point Protocol
        tunnel from Cisco Light-weight LWAPP Access Points.

        This MIB provides information about the Rogue APs
        and Clients that are detected by the controller.

        The relationship between CC and the LWAPP APs
        can be depicted as follows:

              +......+     +......+     +......+
              +      +     +      +     +      +
              +  CC  +     +  CC  +     +  CC  +
              +      +     +      +     +      +
              +......+     +......+     +......+
                ..            .             .
                ..            .             .
               .  .            .             .
              .    .            .             .
             .      .            .             .
            .        .            .             .
        +......+ +......+     +......+      +......+
        +      + +      +     +      +      +      +
        +  AP  + +  AP  +     +  AP  +      +  AP  +
        +      + +      +     +      +      +      +
        +......+ +......+     +......+      +......+
                   .              .             .
                 .  .              .             .
                .    .              .             .
               .      .              .             .
              .        .              .             .
           +......+ +......+     +......+      +......+
           +      + +      +     +      +      +      +
           +  MN  + +  MN  +     +  MN  +      +  MN  +
           +      + +      +     +      +      +      +
           +......+ +......+     +......+      +......+


        The LWAPP tunnel exists between the controller and
        the APs.  The MNs communicate with the APs through
        the protocol defined by the 802.11 standard.

        LWAPP APs, upon bootup, discover and join one of the
        controllers and the controller pushes the configuration,
        that includes the WLAN parameters, to the LWAPP APs.
        The APs then encapsulate all the 802.11 frames from
        wireless clients inside LWAPP frames and forward
        the LWAPP frames to the controller.

                           GLOSSARY

        Access Point ( AP )

        An entity that contains an 802.11 medium access
        control ( MAC ) and physical layer ( PHY ) interface
        and provides access to the distribution services via
        the wireless medium for associated clients.  

        LWAPP APs encapsulate all the 802.11 frames in
        LWAPP frames and sends them to the controller to which
        it is logically connected.

        Light Weight Access Point Protocol ( LWAPP )

        This is a generic protocol that defines the 
        communication between the Access Points and the
        Central Controller. 

        Mobile Node ( MN )

        A roaming 802.11 wireless device in a wireless
        network associated with an access point. Mobile Node 
        and client are used interchangeably. 

        Rogue

        Any 802.11 device which is not part of the RF network 
        is a Rogue device.

        Ad-hoc Network 

        A set of mobile devices within direct communication 
        range establishing a network among themselves for 
        transmitting data, without the use of a Access point 
        is called a ad-hoc network. 

        Rogue Ad-hoc Client

        Any 802.11 client which is part of that ad-hoc network, 
        but not in the trusted list.

        Service Set Identifier ( SSID )

        SSID is a unique identifier that APs and clients
        use to identify with each other.  SSID is a simple
        means of access control and is not for security.
        The SSID can be any alphanumeric entry up to 32
        characters.

        RSSI

        Received Signal Strength Indication (RSSI), the IEEE 802.11
        standard defines a mechanism by which RF energy is to be
        measured by the circuitry on a wireless NIC. Its value is
        measured in dBm and ranges from -128 to 0.

        Rogue Location Detection Protocol (RLDP)

        RLDP is a protocol to detect and automatically 
        contain rogue devices. When the controller discovers 
        a rogue access point, it uses the Rogue Location 
        Discovery Protocol (RLDP) to determine if the 
        rogue is attached to your network.
        RLDP can be enabled/disabled per controller level.

        LRAD (LWAPP RADIO)

        Light Weight Access Point Protocol Radio 
        basically ones own AP.       

        REFERENCE

        [1] Wireless LAN Medium Access Control ( MAC ) and
            Physical Layer ( PHY ) Specifications.

        [2] Draft-obara-capwap-lwapp-00.txt, IETF Light 
            Weight Access Point Protocol."
    REVISION        "201407140000Z"
    DESCRIPTION
        "Added new object group
        - ciscoLwappRogueConfigSup4Group
        Added new compliance
        - ciscoLwappRogueMIBComplianceRev4."
    REVISION        "201109070000Z"
    DESCRIPTION
        "Added following objects:

        cLRogueReportInterval
        cLRogueMinimumRssi
        cLRogueTransientInterval.

        Deprecated ciscoLwappRogueMIBComplianceRev2 and
        added ciscoLwappRogueMIBComplianceRev3."
    REVISION        "201103110000Z"
    DESCRIPTION
        "Added following objects:

        cLRldpAutoContainLevel
        cLRldpAutoContainOnlyforMonitorModeAps.

        Deprecated ciscoLwappRogueMIBComplianceRev1 and
        added ciscoLwappRogueMIBComplianceRev2."
    REVISION        "201007170000Z"
    DESCRIPTION
        "Added following tables:

        cLRogueIgnoreListTable
        cLRuleConfigTable
        cLConditionConfigTable
        cLConditionSsidConfigTable

        Added following objects:

        cLRldpAutoContainFeatureOnWiredNetwork
        cLRldpAutoContainRoguesAdvertisingSsid
        cLRldpAutoContainAdhocNetworks
        cLRldpAutoContainTrustedClientsOnRogueAps

        Deprecated ciscoLwappRogueMIBCompliance and 
        added ciscoLwappRogueMIBComplianceRev1."
    REVISION        "200702060000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 610 }


ciscoLwappRogueMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoLwappRogueMIB 0 }

ciscoLwappRogueMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappRogueMIB 1 }

ciscoLwappRogueMIBConform  OBJECT IDENTIFIER
    ::= { ciscoLwappRogueMIB 2 }

cLRogueConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappRogueMIBObjects 1 }

cLRoguePolicyConfig  OBJECT IDENTIFIER
    ::= { cLRogueConfig 1 }

cLRogueRuleConfig  OBJECT IDENTIFIER
    ::= { cLRogueConfig 3 }

cLRogueIgnoreListConfig  OBJECT IDENTIFIER
    ::= { cLRogueConfig 4 }

cLRldpAutoContainConfig  OBJECT IDENTIFIER
    ::= { cLRogueConfig 5 }

cLRogueApConfig  OBJECT IDENTIFIER
    ::= { cLRogueConfig 6 }


CLAutoContainActions ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This textual convention represents the action that should be
        taken with respect to auto containment feature when any of the
        following are detected by the switch:
        rogue adhoc network 
        rogues APs that are advertising our SSID
        trusted clients that are associated to rogue APs

        alarmOnly(1) - only an alarm will be generated
        contain(2)   - contain automatically"
    SYNTAX          INTEGER  {
                        alarmOnly(1),
                        contain(2)
                    }

cLRogueAdhocRogueReportEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object is used to turn on and off ad-hoc
        rogue reporting.  Setting this object to 'true' 
        will enable ad-hoc rogue reporting. Setting to 
        'false' will disable ad-hoc rogue reporting."
    DEFVAL          { true } 
    ::= { cLRoguePolicyConfig 1 }

cLRogueReportInterval OBJECT-TYPE
    SYNTAX          Unsigned32 (10..300)
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the rogue report interval,
        which is the interval that monitor mode APs send 
        rogue detection details to the controller." 
    ::= { cLRoguePolicyConfig 2 }

cLRogueMinimumRssi OBJECT-TYPE
    SYNTAX          Integer32 (-128..-70)
    UNITS           "dBm"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the minimum value of RSSI
        considered for detection of rogues." 
    ::= { cLRoguePolicyConfig 3 }

cLRogueTransientInterval OBJECT-TYPE
    SYNTAX          Unsigned32 (0 | 120..1800)
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the rogue transient
        interval. 

        A value of '0' specifies that an AP sends 
        rogue detection details to the controller 
        as soon as it detects a rogue. 

        A non-zero value specifies that an AP sends 
        rogue detection details to the controller if 
        it hears the rogue more than once in the specified 
        interval." 
    ::= { cLRoguePolicyConfig 4 }

cLRogueClientNumThreshold OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the number of clients the Rogue AP
        can have. A value of zero indicates no limitation on 
        the number of clients the Rogue AP can have." 
    ::= { cLRoguePolicyConfig 5 }

cLRogueDetectionSecurityLevel OBJECT-TYPE
    SYNTAX          INTEGER  {
                        low(1),
                        high(2),
                        critical(3),
                        custom(4)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the rogue detection security level.
        When the object has value of 'low', 'high' or 'critical', 
        controller uses pre-defined rogue detection parameters for 
        the specified security level. 
        When the object has value of 'custom', controller uses the 
        user configured rogue detection parameters. 

        low      - security level is low 
        high     - security level is high 
        critical - security level is critical 
        custom   - customized security level" 
    ::= { cLRoguePolicyConfig 6 }

cLRogueValidateRogueClientsAgainstMse OBJECT-TYPE
    SYNTAX          INTEGER  {
                        disable(1),
                        enable(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object specifies whether the controller validates
        'valid' clients which are associating with rogue AP, 
        against MSE. A value of 'enable' indicates that the 
        controller does validates 'valid'clients which are 
        associating with rogue AP, against MSE. A value of 
        'disable' indicates that the controller does not 
        validates 'valid' clients which are associating 
        with rogue AP, against MSE." 
    ::= { cLRoguePolicyConfig 7 }

cLRogueAdhocRogueNotifEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object to control the generation of
        cLRogueAdhocDetected notification.

        A value of 'true' indicates that the agent generates
        cLRogueAdhocDetected notification.

        A value of 'false' indicates that the agent doesn't
        generate cLRogueAdhocDetected notification."
    DEFVAL          { false } 
    ::= { cLRogueConfig 2 }

cLRogueAdhocRogueDetected NOTIFICATION-TYPE
    OBJECTS         { cLApName }
    STATUS          current
    DESCRIPTION
        "This notification is generated by the controller when a
        a rogue is detected.  The name of the AP that  
        detected this rogue is sent in the notification."
   ::= { ciscoLwappRogueMIBNotifs 1 }
-- ********************************************************************
-- Rule configuration
-- ********************************************************************

cLRuleConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLRuleConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides the configuration needed
        by the controller for classifying rogue APs. 
        The user defines the custom rules which are 
        used to classify the APs under different 
        classification types. When a new rule is created 
        priority will be assigned automatically by controller, 
        highest priority given to rule which are created first. 
        Also if user is changing the priority of a rule manually, 
        the new priority should not be used by any other existing rule."
    ::= { cLRogueRuleConfig 1 }

cLRuleConfigEntry OBJECT-TYPE
    SYNTAX          CLRuleConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row
        (as identified by a rule name)in cLRuleConfigTable."
    INDEX           { cLRuleName } 
    ::= { cLRuleConfigTable 1 }

CLRuleConfigEntry ::= SEQUENCE {
        cLRuleName            SnmpAdminString,
        cLRuleRogueType       INTEGER,
        cLRuleConditionsMatch INTEGER,
        cLRulePriority        Unsigned32,
        cLRuleEnable          TruthValue,
        cLRuleStorageType     StorageType,
        cLRuleRowStatus       RowStatus
}

cLRuleName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the rule name to identify
        this entry." 
    ::= { cLRuleConfigEntry 1 }

cLRuleRogueType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        friendly(1),
                        malicious(2),
                        unclassified(3),
                        custom(4)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object determines the classification applied
        to the rogue AP that matches this rule.

        friendly     - known and acknowledged rogue AP.
        malicious    - unknown AP that matches user defined 
                       malicious rules.
        unclassified - an unknown AP that did not match malicious 
                       or friendly rules.
        custom       - user can configure rogue detection parameters."
    DEFVAL          { custom } 
    ::= { cLRuleConfigEntry 2 }

cLRuleConditionsMatch OBJECT-TYPE
    SYNTAX          INTEGER  {
                        all(1),
                        any(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents how the conditions
        defined by corresponding instances of 
        cLConditionType, are matched under each rule.
        all - all the conditions defined per rule should be matched
        any - any conditions defined per rule can be matched." 
    ::= { cLRuleConfigEntry 3 }

cLRulePriority OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to define the order in which the
        rules will be applied. The rules will be applied from 
        lowest to highest and gaps are allowed.  
        Each rule must have and unique value for this object." 
    ::= { cLRuleConfigEntry 4 }

cLRuleEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies whether this rule is enabled or not.
        A value of 'true' specifies this rule is enabled.
        A value of 'false' specifies this rule is disabled." 
    ::= { cLRuleConfigEntry 5 }

cLRuleStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the storage type for this conceptual
        row."
    DEFVAL          { nonVolatile } 
    ::= { cLRuleConfigEntry 6 }

cLRuleRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the status column for a
        conceptual row in this table. All writable objects 
        in this row may be modified when the row is active." 
    ::= { cLRuleConfigEntry 7 }
 

-- ********************************************************************
-- Rule/Condition name configuration
-- ********************************************************************

cLConditionConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLConditionConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the configuration of
        conditions that can be applied to a rule."
    ::= { cLRogueRuleConfig 2 }

cLConditionConfigEntry OBJECT-TYPE
    SYNTAX          CLConditionConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row in
        cLConditionConfigTable, as identified by a 
        specific condition name to be applied on a 
        specific rule name."
    INDEX           {
                        cLRuleName,
                        cLConditionName
                    } 
    ::= { cLConditionConfigTable 1 }

CLConditionConfigEntry ::= SEQUENCE {
        cLConditionName                SnmpAdminString,
        cLConditionType                INTEGER,
        cLConditionValue               Integer32,
        cLConditionEnable              TruthValue,
        cLConditionStorageType         StorageType,
        cLConditionRowStatus           RowStatus,
        cLConditionRssi                Integer32,
        cLConditionClientCount         Unsigned32,
        cLConditionNoEncryptionEnabled TruthValue,
        cLConditionManagedSsidEnabled  TruthValue,
        cLConditionDuration            Unsigned32
}

cLConditionName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..64))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the condition name." 
    ::= { cLConditionConfigEntry 1 }

cLConditionType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        managedSsid(1),
                        rssi(2),
                        duration(3),
                        clientCount(4),
                        noEncryption(5),
                        userConfigSsid(6)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the condition type
        for this condition associated with a rule.
             managedSsid    - matches managed SSID
             rssi           - required minimum RSSI 
             duration       - limited to this time duration
             clientCount    - number of associated clients
             noEncryption   - no encryption rule
             userConfigSsid - matches user configured SSID" 
    ::= { cLConditionConfigEntry 2 }

cLConditionValue OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the value associated
        with the condition type as specified by 
        the corresponding cLConditionType instance.
        If cLConditionType is 'userConfigSsid', 
        then corresponding 'cLConditionValue' can 
        only take on the value of zero." 
    ::= { cLConditionConfigEntry 3 }

cLConditionEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates whether matching against
        this condition is enabled or not. A value of 'true' 
        indicates matching against this condition is enabled.
        A value of 'false' indicates matching against 
        this condition is disabled." 
    ::= { cLConditionConfigEntry 4 }

cLConditionStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the storage type for this conceptual
        row."
    DEFVAL          { nonVolatile } 
    ::= { cLConditionConfigEntry 5 }

cLConditionRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the status column for a
        conceptual row in this table. All writable objects 
        except cLConditionType in this row may be 
        modified when the row is active." 
    ::= { cLConditionConfigEntry 6 }

cLConditionRssi OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the minimum value of RSSI that
        a rogue AP must have in order to match cLConditionType
        of 'rssi'."
    DEFVAL          { 0 } 
    ::= { cLConditionConfigEntry 7 }

cLConditionClientCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the minimum value of client count
        that a rogue AP must have in order to match cLConditionType
        of 'clientCount'."
    DEFVAL          { 0 } 
    ::= { cLConditionConfigEntry 8 }

cLConditionNoEncryptionEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies whether or not encryption is enabled.
        A value of 'true' indicates that encryption is not enabled.
        A value of 'false' indicates that encryption is enabled
        for this condition."
    DEFVAL          { true } 
    ::= { cLConditionConfigEntry 9 }

cLConditionManagedSsidEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies whether or not managed SSID is enabled.
        A value of 'true' indicates managed SSID is enabled.
        A value of 'false' indicates managed SSID is not enabled
        for this condition."
    DEFVAL          { true } 
    ::= { cLConditionConfigEntry 10 }

cLConditionDuration OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the minimum value of duration,
        in seconds, a rogue AP must be present in order to match 
        cLConditionType of 'duration'."
    DEFVAL          { 0 } 
    ::= { cLConditionConfigEntry 11 }
 

-- ********************************************************************
-- Rule/Condition SSID configuration
-- ********************************************************************

cLConditionSsidConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLConditionSsidConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the configuration of
        SSID for a rule. This is applicable to 
        conditions within a rule which has the 
        corresponding cLConditionType taking on the value 
        of 'userConfigSsid'."
    ::= { cLRogueRuleConfig 3 }

cLConditionSsidConfigEntry OBJECT-TYPE
    SYNTAX          CLConditionSsidConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row in
        cLConditionSsidConfigTable."
    INDEX           {
                        cLRuleName,
                        cLConditionName,
                        cLConditionSsidValue
                    } 
    ::= { cLConditionSsidConfigTable 1 }

CLConditionSsidConfigEntry ::= SEQUENCE {
        cLConditionSsidValue       SnmpAdminString,
        cLConditionSsidStorageType StorageType,
        cLConditionSsidRowStatus   RowStatus
}

cLConditionSsidValue OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the SSID value for this
        condition associated with a rule." 
    ::= { cLConditionSsidConfigEntry 1 }

cLConditionSsidStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the storage
        type for this conceptual row."
    DEFVAL          { nonVolatile } 
    ::= { cLConditionSsidConfigEntry 2 }

cLConditionSsidRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the status column for a
        conceptual row in this table. All writable objects 
        in this row may not be modified when the row is active." 
    ::= { cLConditionSsidConfigEntry 3 }
 

-- ********************************************************************
-- Rogue Ignore List Configuration
-- ********************************************************************

cLRogueIgnoreListTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLRogueIgnoreListEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table lists the APs, as identified by the AP's mac address,
        which should not be treated as rogue by the controller.
        These APs are the autonomous access points that have been 
        manually added to WCS."
    ::= { cLRogueIgnoreListConfig 1 }

cLRogueIgnoreListEntry OBJECT-TYPE
    SYNTAX          CLRogueIgnoreListEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row in this table.
        There will be a row for each entry of the autonomous 
        APs which are manually added to WCS. When the autonomous
        AP is no longer managed by WCS, the corresponding row 
        entry will be removed."
    INDEX           { cLRogueIgnoreListMACAddress } 
    ::= { cLRogueIgnoreListTable 1 }

CLRogueIgnoreListEntry ::= SEQUENCE {
        cLRogueIgnoreListMACAddress  MacAddress,
        cLRogueIgnoreListStorageType StorageType,
        cLRogueIgnoreListRowStatus   RowStatus
}

cLRogueIgnoreListMACAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This is the MAC Address of the AP to be put in the
        rogue ignore list." 
    ::= { cLRogueIgnoreListEntry 1 }

cLRogueIgnoreListStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the storage type for this
        conceptual row."
    DEFVAL          { nonVolatile } 
    ::= { cLRogueIgnoreListEntry 2 }

cLRogueIgnoreListRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status of the conceptual row.
        All writable objects in this row may not be 
        modified when the row is active." 
    ::= { cLRogueIgnoreListEntry 3 }
 


-- ********************************************************************
-- Auto Containment configuration
-- ********************************************************************

cLRldpAutoContainFeatureOnWiredNetwork OBJECT-TYPE
    SYNTAX          INTEGER  {
                        disable(1),
                        enable(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the RLDP Auto contain feature status.

        disable - automatic containment of rogues on wired network 
                  is disabled
        enable  - automatic containment of rogues on wired network
                  is enabled

        NOTE: Using this feature may have legal consequences!!!"
    DEFVAL          { disable } 
    ::= { cLRldpAutoContainConfig 1 }

cLRldpAutoContainRoguesAdvertisingSsid OBJECT-TYPE
    SYNTAX          CLAutoContainActions
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This is the action with respect to auto containment feature,
        that should be taken when switch detects rogues that are 
        advertising our SSID.

        NOTE: Using this feature may have legal consequences!!!"
    DEFVAL          { alarmOnly } 
    ::= { cLRldpAutoContainConfig 2 }

cLRldpAutoContainAdhocNetworks OBJECT-TYPE
    SYNTAX          CLAutoContainActions
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This is the action with respect to auto containment feature,
        that should be taken when adhoc networks are
        detected by the switch. 

        NOTE: Using this feature may have legal consequences!!!"
    DEFVAL          { alarmOnly } 
    ::= { cLRldpAutoContainConfig 3 }

cLRldpAutoContainTrustedClientsOnRogueAps OBJECT-TYPE
    SYNTAX          CLAutoContainActions
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This is the action with respect to auto containment feature,
        that should be taken when trusted clients that
        are associated to rogue APs are detected by the switch. 

        NOTE: Using this feature may have legal consequences!!!"
    DEFVAL          { alarmOnly } 
    ::= { cLRldpAutoContainConfig 4 }

cLRldpAutoContainLevel OBJECT-TYPE
    SYNTAX          Integer32 (1..4)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object is used to specify the level of auto containment.
        The level actually denotes the number of APs that should be 
        used by the controller for auto containment."
    DEFVAL          { 1 } 
    ::= { cLRldpAutoContainConfig 5 }

cLRldpAutoContainOnlyforMonitorModeAps OBJECT-TYPE
    SYNTAX          INTEGER  {
                        disable(1),
                        enable(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object is used to specify if auto containment should be
        done only using monitor mode APs or not.

        disable - auto containment will be done using all APs 
                  irrespective of the mode
        enable  - auto containment will be done only using monitor
                  mode APs."
    DEFVAL          { disable } 
    ::= { cLRldpAutoContainConfig 6 }
-- ********************************************************************
-- Rogue AP List Configuration
-- ********************************************************************

cLRogueApTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLRogueApEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table lists the configured rogue APs in the system."
    ::= { cLRogueApConfig 1 }

cLRogueApEntry OBJECT-TYPE
    SYNTAX          CLRogueApEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing contains management information
        of a particular rogue AP. 

        An entry can be created, or deleted by using
        cLRogueApRowStatus."
    INDEX           { cLRogueApMACAddress } 
    ::= { cLRogueApTable 1 }

CLRogueApEntry ::= SEQUENCE {
        cLRogueApMACAddress  MacAddress,
        cLRogueApClassType   INTEGER,
        cLRogueApState       INTEGER,
        cLRogueApStorageType StorageType,
        cLRogueApRowStatus   RowStatus
}

cLRogueApMACAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "MAC Address of a rogue AP." 
    ::= { cLRogueApEntry 1 }

cLRogueApClassType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        friendly(1),
                        malicious(2),
                        unclassified(3),
                        custom(4)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the type of a rogue AP.

        friendly     - existing known, Acknowledge, and Trust missing
                       rogue states are classified as Friendly.
        malicious    - unknown AP that could be a threat.
        unclassified - an unknown AP or rogue AP is identified
                       but it does not belong to Friendly or
                       Malicious rogue types.
        custom       - AP that matches user defined custom rules."
    DEFVAL          { custom } 
    ::= { cLRogueApEntry 2 }

cLRogueApState OBJECT-TYPE
    SYNTAX          INTEGER  {
                        pending(1),
                        alert(2),
                        detectedLrad(3),
                        known(4),
                        acknowledge(5),
                        contained(6),
                        threat(7),
                        containedPending(8),
                        knownContained(9),
                        trustedMissing(10),
                        initializing(11)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This objects specifies the state in which
        the rogue AP is.

        pending          - a read-only value indicates that rogue AP
                           can not be state to any of the following
                           type.
        alert            - rogue AP can be a potential threat.
                           Trap will be sent out to trap recipients.
        detectedLrad     - a read-only value indicates that a LRAD
                           that got detected as rogue.
        known            - a read-only value indicates that an internal
                           AP which is not on the same switch.
        acknowledge      - a read-only value indicates that an external
                           AP whose existence is acceptable and not a
                           threat(probably from vendor other than
                           cisco).
        contained        - containment is initiated and ongoing.
        threat           - rogue AP is found on wired network.
        containedPending - a read-only value indicates that no AP
                           resources available for containment.
        knownContained   - a read-only value indicates that no longer
                           used.
        trustedMissing   - rogue AP is friendly but there is no slot
                           for friendly AP.
        initializing     - a read-only value indicates that rogue
                           AP is being initialized.

        For a friendly rogue AP, only two states are valid:
        'known' and 'acknowledge'.

        'known', 'knownContained' and 'trustedMissing'
        can appear in known rogue list.

        Known rogues can be pre-provisioned and known rogues
        state can be changed to 'alert'."
    DEFVAL          { alert } 
    ::= { cLRogueApEntry 3 }

cLRogueApStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the storage type for this
        conceptual row."
    DEFVAL          { nonVolatile } 
    ::= { cLRogueApEntry 4 }

cLRogueApRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The status of the conceptual row.
        All writable objects in this row may be modified when
        the row is active." 
    ::= { cLRogueApEntry 5 }
 

-- ********************************************************************
-- MIB Compliance Statements
-- ********************************************************************

ciscoLwappRogueMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoLwappRogueMIBConform 1 }

ciscoLwappRogueMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoLwappRogueMIBConform 2 }


ciscoLwappRogueMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappRogueMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappRogueConfigGroup,
                        ciscoLwappRogueNotifsGroup
                    }
    ::= { ciscoLwappRogueMIBCompliances 1 }

ciscoLwappRogueMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappRogueMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappRogueConfigGroup,
                        ciscoLwappRogueNotifsGroup,
                        ciscoLwappRogueConfigSup1Group
                    }

    OBJECT          cLRogueIgnoreListRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLRuleRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLConditionRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLConditionSsidRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLRogueIgnoreListStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLRuleStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLConditionStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLConditionSsidStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."
    ::= { ciscoLwappRogueMIBCompliances 2 }

ciscoLwappRogueMIBComplianceRev2 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappRogueMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappRogueConfigGroup,
                        ciscoLwappRogueNotifsGroup,
                        ciscoLwappRogueConfigSup2Group
                    }

    OBJECT          cLRogueIgnoreListRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLRuleRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLConditionRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLConditionSsidRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLRogueIgnoreListStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLRuleStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLConditionStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLConditionSsidStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."
    ::= { ciscoLwappRogueMIBCompliances 3 }

ciscoLwappRogueMIBComplianceRev3 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappRogueMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappRogueConfigGroup,
                        ciscoLwappRogueNotifsGroup,
                        ciscoLwappRogueConfigSup3Group
                    }

    OBJECT          cLRogueIgnoreListRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLRuleRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLConditionRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLConditionSsidRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLRogueIgnoreListStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLRuleStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLConditionStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLConditionSsidStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."
    ::= { ciscoLwappRogueMIBCompliances 4 }

ciscoLwappRogueMIBComplianceRev4 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappRogueMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappRogueConfigGroup,
                        ciscoLwappRogueNotifsGroup,
                        ciscoLwappRogueConfigSup3Group
                    }

    GROUP           ciscoLwappRogueConfigSup4Group
    DESCRIPTION
        "This group is mandatory for platforms which support
        rogue functionality."

    OBJECT          cLRogueIgnoreListRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLRuleRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLConditionRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLConditionSsidRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLRogueIgnoreListStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLRuleStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLConditionStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLConditionSsidStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLRogueClientNumThreshold
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLRogueDetectionSecurityLevel
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLRogueValidateRogueClientsAgainstMse
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLConditionRssi
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLConditionClientCount
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLConditionNoEncryptionEnabled
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLConditionManagedSsidEnabled
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLConditionDuration
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLRogueApClassType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLRogueApState
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLRogueApStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cLRogueApRowStatus
    SYNTAX          INTEGER  {
                        active(1)
                    }
    WRITE-SYNTAX    INTEGER  {
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required.
        Support for createAndWait and notInService
        is not required."
    ::= { ciscoLwappRogueMIBCompliances 5 }

-- Units of Conformance

ciscoLwappRogueConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLRogueAdhocRogueReportEnable,
                        cLRogueAdhocRogueNotifEnabled
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        rogue configuration on the controller."
    ::= { ciscoLwappRogueMIBGroups 1 }

ciscoLwappRogueNotifsGroup NOTIFICATION-GROUP
   NOTIFICATIONS    { cLRogueAdhocRogueDetected }
    STATUS          current
    DESCRIPTION
        "This collection of objects specifies the
        notifications for rogue detection."
    ::= { ciscoLwappRogueMIBGroups 2 }

ciscoLwappRogueConfigSup1Group OBJECT-GROUP
    OBJECTS         {
                        cLRogueIgnoreListStorageType,
                        cLRogueIgnoreListRowStatus,
                        cLRuleRogueType,
                        cLRuleConditionsMatch,
                        cLRulePriority,
                        cLRuleEnable,
                        cLRuleStorageType,
                        cLRuleRowStatus,
                        cLConditionType,
                        cLConditionValue,
                        cLConditionEnable,
                        cLConditionStorageType,
                        cLConditionRowStatus,
                        cLConditionSsidStorageType,
                        cLConditionSsidRowStatus,
                        cLRldpAutoContainFeatureOnWiredNetwork,
                        cLRldpAutoContainRoguesAdvertisingSsid,
                        cLRldpAutoContainAdhocNetworks,
                        cLRldpAutoContainTrustedClientsOnRogueAps
                    }
    STATUS          deprecated
    DESCRIPTION
        "This collection of objects represent the
        rogue configuration on the controller.
        ciscoLwappRogueConfigSup1Group object is superseded
        by ciscoLwappRogueConfigSup2Group."
    ::= { ciscoLwappRogueMIBGroups 3 }

ciscoLwappRogueConfigSup2Group OBJECT-GROUP
    OBJECTS         {
                        cLRogueIgnoreListStorageType,
                        cLRogueIgnoreListRowStatus,
                        cLRuleRogueType,
                        cLRuleConditionsMatch,
                        cLRulePriority,
                        cLRuleEnable,
                        cLRuleStorageType,
                        cLRuleRowStatus,
                        cLConditionType,
                        cLConditionValue,
                        cLConditionEnable,
                        cLConditionStorageType,
                        cLConditionRowStatus,
                        cLConditionSsidStorageType,
                        cLConditionSsidRowStatus,
                        cLRldpAutoContainFeatureOnWiredNetwork,
                        cLRldpAutoContainRoguesAdvertisingSsid,
                        cLRldpAutoContainAdhocNetworks,
                        cLRldpAutoContainTrustedClientsOnRogueAps,
                        cLRldpAutoContainLevel,
                        cLRldpAutoContainOnlyforMonitorModeAps
                    }
    STATUS          deprecated
    DESCRIPTION
        "This collection of objects represent the
        rogue configuration on the controller.
        ciscoLwappRogueConfigSup2Group object is
        superseded by ciscoLwappRogueConfigSup3Group."
    ::= { ciscoLwappRogueMIBGroups 4 }

ciscoLwappRogueConfigSup3Group OBJECT-GROUP
    OBJECTS         {
                        cLRogueIgnoreListStorageType,
                        cLRogueIgnoreListRowStatus,
                        cLRuleRogueType,
                        cLRuleConditionsMatch,
                        cLRulePriority,
                        cLRuleEnable,
                        cLRuleStorageType,
                        cLRuleRowStatus,
                        cLConditionType,
                        cLConditionValue,
                        cLConditionEnable,
                        cLConditionStorageType,
                        cLConditionRowStatus,
                        cLConditionSsidStorageType,
                        cLConditionSsidRowStatus,
                        cLRldpAutoContainFeatureOnWiredNetwork,
                        cLRldpAutoContainRoguesAdvertisingSsid,
                        cLRldpAutoContainAdhocNetworks,
                        cLRldpAutoContainTrustedClientsOnRogueAps,
                        cLRldpAutoContainLevel,
                        cLRldpAutoContainOnlyforMonitorModeAps,
                        cLRogueReportInterval,
                        cLRogueMinimumRssi,
                        cLRogueTransientInterval
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        rogue configuration on the controller."
    ::= { ciscoLwappRogueMIBGroups 5 }

ciscoLwappRogueConfigSup4Group OBJECT-GROUP
    OBJECTS         {
                        cLRogueApClassType,
                        cLRogueApState,
                        cLRogueApStorageType,
                        cLRogueApRowStatus,
                        cLRogueClientNumThreshold,
                        cLRogueDetectionSecurityLevel,
                        cLRogueValidateRogueClientsAgainstMse,
                        cLConditionRssi,
                        cLConditionClientCount,
                        cLConditionNoEncryptionEnabled,
                        cLConditionManagedSsidEnabled,
                        cLConditionDuration
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        rogue configuration on the controller."
    ::= { ciscoLwappRogueMIBGroups 6 }

END





































