-- *******************************************************************
-- CISCO-GSLB-SYSTEM-MIB.my:  Global Server Load Balancing
-- Platform and System Status
--   
-- Dec 2006, Pawan N
--   
-- Copyright (c) 2006, 2010-2011 by Cisco Systems Inc.
-- All rights reserved.
-- *******************************************************************

CISCO-GSLB-SYSTEM-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    NOTIFICATION-TYPE,
    Counter32,
    Unsigned32,
    Gauge32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    NOTIFICATION-GROUP,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    RowStatus,
    StorageType,
    TruthValue
        FROM SNMPv2-TC
    InetAddressType,
    InetAddress,
    InetAddressDNS
        FROM INET-ADDRESS-MIB
    sysName
        FROM SNMPv2-MIB
    InterfaceIndexOrZero
        FROM IF-MIB
    CiscoGslbNodeServices,
    CiscoGslbPeerStatus
        FROM CISCO-GSLB-TC-MIB
    ciscoMgmt
        FROM CISCO-SMI;


ciscoGslbSystemMIB MODULE-IDENTITY
    LAST-UPDATED    "201106060000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-slb@cisco.com"
    DESCRIPTION
        "This MIB module defines objects for network and system
        information of Global Server Load Balancer(GSLB) as a
        network device.  A GSLB device is used to allocate the
        least-loaded and proximate resource to the requester.
        The MIB objects define information about GLSB status,
        GSLB's peers (other GSLB devices available on its
        network with which it interacts) information & status,
        GSLB's proximity information related statistics, etc.
        Further it defines related notifications.

        Acronyms and their description:

        DNS          : Domain Name Service (RFC1035).

        D-proxy      : Local DNS name server of the client.

        Proximity    : Refers to the distance or delay, in terms
                       of network topology and not geographic
                       distance, between the requesting client's
                       D-proxy and the resources corresponding
                       to that request.

        Proximity    : To respond to DNS requests with the most
        probing        proximate answers, the GSLB device
                       communicates with a probing device located
                       in each proximity zone to gather round-trip
                       time (RTT) metric information measured
                       between the requesting client's D-proxy 
                       and the zone.  The GSLB device then directs
                       client requests to an available resource
                       with the lowest RTT value.

        Probed       : This is the device to which the GSLB device
        device         sends a proximity probe. This is done to
                       learn the proximity of the device.

        DRP          : Director Response Protocol (DRP) is a
                       simple User Datagram Protocol (UDP)
                       based application developed by
                       Cisco Systems, Inc.  DRP enables
                       Cisco Distributed-Director product to
                       perform global load distribution and
                       content routing in a sophisticated manner
                       that accounts for server availability,
                       relative client-to-server topological
                       proximities, and client-to-server link
                       latency to determine the best server.
                       Using routing table intelligence in the
                       network infrastructure, Distributed-Director
                       transparently redirects end-user service
                       requests to the closest server, as
                       determined by client-to-server topological
                       proximity or client-to-server link latency,
                       resulting in increased access performance
                       seen by the end user.

        Region       : Higher-level geographical groupings that
                       may contain one or more locations.  Each
                       location should be assigned to a region.

        Location     : Grouping for devices with common
                       geographical attributes.  A location is
                       assigned to a region.
                       A location is also assigned to a zone,
                       which is used for proximity probing.

        Zone         : A network can be logically partioned into
                       zones based on the arrangement of devices
                       and network partion characteristics.
                       A zone can be geographically related to
                       data centers in a continent, a country,
                       or a major city.  All devices, such as web
                       servers in a data center, that are located
                       in the same zone have the same proximity
                       value when communicating with other areas
                       of the Internet.  Within each zone, there
                       is an active probing device that is
                       configured to accept probing instructions
                       from any GSLB device.  Probing here refers
                       to the process of measuring RTT from one
                       probing device to a requesting D-proxy."
    REVISION        "201106060000Z"
    DESCRIPTION
        "-Deprecated cgsRegionTable and replaced it with
        cgsRegionIdTable

        -Deprecated ciscoGslbSystemMIBCompliance and replaced it with
        ciscoGslbSystemMIBComplianceRev1

        -Deprecated ciscoGslbSystemResourceGroup and replaced it with
        ciscoGslbSystemResourceLocationGroup and 
        ciscoGslbSystemResourceRegionGroup"
    REVISION        "200612040000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 589 }


ciscoGslbSystemMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoGslbSystemMIB 0 }

ciscoGslbSystemMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoGslbSystemMIB 1 }

ciscoGslbSystemMIBConform  OBJECT IDENTIFIER
    ::= { ciscoGslbSystemMIB 2 }

-- Objects for Notification Control

cgsNotifControl  OBJECT IDENTIFIER
    ::= { ciscoGslbSystemMIBObjects 1 }

-- Objects for Notification

cgsNotifObjects  OBJECT IDENTIFIER
    ::= { ciscoGslbSystemMIBObjects 2 }

-- Objects for general status

cgsGeneral  OBJECT IDENTIFIER
    ::= { ciscoGslbSystemMIBObjects 3 }

-- Objects for status of GSLB peers

cgsPeer  OBJECT IDENTIFIER
    ::= { ciscoGslbSystemMIBObjects 4 }

-- Objects for Proximity Probes statistics

cgsProxZoneStats  OBJECT IDENTIFIER
    ::= { ciscoGslbSystemMIBObjects 5 }

-- Objects for Resources

cgsResources  OBJECT IDENTIFIER
    ::= { ciscoGslbSystemMIBObjects 6 }


-- General Status Objects

cgsNodeService OBJECT-TYPE
    SYNTAX          CiscoGslbNodeServices
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the type of role of the GSLB
        device amongst its peers." 
    ::= { cgsGeneral 1 }

cgsNodeCommIfName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the textual name of the interface
        used by the GSLB device to communicate with peer GSLB
        devices.  The value of this object must be same as the
        ifName reported by IF-MIB  for the interface instance." 
    ::= { cgsGeneral 2 }

cgsNodeCommIfIndex OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object is used as an identifier for the interface
        used by the GSLB device to communicate with peer GSLB
        devices.  The value of this object must be same as the
        ifIndex reported by IF-MIB for the interface identified
        by cgsNodeCommIfName." 
    ::= { cgsGeneral 3 }

cgsNodeStatus OBJECT-TYPE
    SYNTAX          CiscoGslbPeerStatus
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the status of the GSLB device as
        known on the GSLB network of peers." 
    ::= { cgsGeneral 4 }

cgsNodeLocation OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..80))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the administratively assigned
        location for the GSLB device." 
    ::= { cgsGeneral 5 }

cgsNodeRegion OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..80))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the administratively assigned
        region for the GSLB device.  This value corresponds to
        an instance of cgsLocationRegion from cgsLocationTable." 
    ::= { cgsGeneral 6 }

cgsPeerTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CgsPeerEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table lists the information on peers in the GSLB
        network of devices."
    ::= { cgsPeer 1 }

cgsPeerEntry OBJECT-TYPE
    SYNTAX          CgsPeerEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cgsPeerEntryTable.  Each entry contains
        information on the GSLB peers.  Entries are
        added/deleted when a GSLB peer device is added/deleted
        in GSLB network of peers."
    INDEX           {
                        cgsPeerAddressType,
                        cgsPeerAddress
                    } 
    ::= { cgsPeerTable 1 }

CgsPeerEntry ::= SEQUENCE {
        cgsPeerAddressType InetAddressType,
        cgsPeerAddress     InetAddress,
        cgsPeerLocation    SnmpAdminString,
        cgsPeerDnsName     InetAddressDNS,
        cgsPeerService     CiscoGslbNodeServices,
        cgsPeerStatus      CiscoGslbPeerStatus,
        cgsPeerVersion     SnmpAdminString
}

cgsPeerAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the IP address type of the
        GSLB peer." 
    ::= { cgsPeerEntry 1 }

cgsPeerAddress OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (1..16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the GSLB peer IP address.
        The type of IP address is identified by
        cgsPeerAddressType." 
    ::= { cgsPeerEntry 2 }

cgsPeerLocation OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..80))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the administratively assigned
        location of the GSLB peer.  Its value must be same as
        the value configured in cgsLocationTable." 
    ::= { cgsPeerEntry 3 }

cgsPeerDnsName OBJECT-TYPE
    SYNTAX          InetAddressDNS
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the host name assigned uniquely
        to a GSLB peer.  Its value is same as the value of
        sysName of the GSLB peer." 
    ::= { cgsPeerEntry 4 }

cgsPeerService OBJECT-TYPE
    SYNTAX          CiscoGslbNodeServices
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the type of role the GSLB peer
        has in a GSLB network of peers.  Its value is same as
        value of cgsNodeService of the GSLB peer." 
    ::= { cgsPeerEntry 5 }

cgsPeerStatus OBJECT-TYPE
    SYNTAX          CiscoGslbPeerStatus
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the status of GSLB peer as
        known to the reporting GSLB device." 
    ::= { cgsPeerEntry 6 }

cgsPeerVersion OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the software version installed
        on the GSLB peer." 
    ::= { cgsPeerEntry 7 }
 


cgsProxZoneTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CgsProxZoneEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table is used for configuring proximity zones.
        It consists a  list of proximity probing statistics
        for each configured proximity zone."
    ::= { cgsProxZoneStats 1 }

cgsProxZoneEntry OBJECT-TYPE
    SYNTAX          CgsProxZoneEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cgsProxZoneTable.  Each entry contains
        information on proximity zones and probing statistics.
        Entries can be added/deleted/modified by administrator
        action."
    INDEX           { cgsProxZoneName } 
    ::= { cgsProxZoneTable 1 }

CgsProxZoneEntry ::= SEQUENCE {
        cgsProxZoneName             SnmpAdminString,
        cgsProxPrimaryAddressType   InetAddressType,
        cgsProxPrimaryAddress       InetAddress,
        cgsProxSecondaryAddressType InetAddressType,
        cgsProxSecondaryAddress     InetAddress,
        cgsProxEchoSentReqs         Counter32,
        cgsProxEchoRcvdResps        Counter32,
        cgsProxSentMeasureReqs      Counter32,
        cgsProxRcvdMeasureResps     Counter32,
        cgsProxTotalSentReqs        Counter32,
        cgsProxTotalRcvdResps       Counter32,
        cgsProxSendRate             Unsigned32,
        cgsProxRcvdRate             Unsigned32,
        cgsProxPeakSendRate         Unsigned32,
        cgsProxPeakRcvdRate         Unsigned32,
        cgsProxStorageType          StorageType,
        cgsProxRowStatus            RowStatus
}

cgsProxZoneName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..80))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies a name given uniquely for
        a proximity zone." 
    ::= { cgsProxZoneEntry 1 }

cgsProxPrimaryAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the IP address type of the
        primary device being probed in the proximity zone."
    DEFVAL          { ipv4 } 
    ::= { cgsProxZoneEntry 2 }

cgsProxPrimaryAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the IP address of the primary
        device being probed  in the proximity zone.  The type of
        IP address is identified by cgsProxPrimaryAddressType.
        This object is mandatory for row creation." 
    ::= { cgsProxZoneEntry 3 }

cgsProxSecondaryAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the IP address type of the
        secondary device that may be probed in the
        proximity zone."
    DEFVAL          { ipv4 } 
    ::= { cgsProxZoneEntry 4 }

cgsProxSecondaryAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the IP address of the secondary
        device that may be probed for proximity in the proximity
        zone.  The type of IP address is identified by
        cgsProxSecondaryAddressType."
    DEFVAL          { "" } 
    ::= { cgsProxZoneEntry 5 }

cgsProxEchoSentReqs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "requests"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of DRP echo requests
        sent by GSLB to all probed devices." 
    ::= { cgsProxZoneEntry 6 }

cgsProxEchoRcvdResps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "responses"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of DRP echo responses
        received by GLSB from all probed devices." 
    ::= { cgsProxZoneEntry 7 }

cgsProxSentMeasureReqs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "requests"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of DRP measured
        requests sent by GSLB to all probed devices." 
    ::= { cgsProxZoneEntry 8 }

cgsProxRcvdMeasureResps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "responses"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of DRP measured
        responses received by GSLB from all probed devices." 
    ::= { cgsProxZoneEntry 9 }

cgsProxTotalSentReqs OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "requests"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total of DRP requests sent
        by GSLB to probed device in the proximity zone." 
    ::= { cgsProxZoneEntry 10 }

cgsProxTotalRcvdResps OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "responses"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total of DRP responses
        received by GSLB from all probed devices in the
        proximity zone." 
    ::= { cgsProxZoneEntry 11 }

cgsProxSendRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "rate per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the current transmitted DRP
        request rate per second." 
    ::= { cgsProxZoneEntry 12 }

cgsProxRcvdRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "rate per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the current received DRP response
        rate per second." 
    ::= { cgsProxZoneEntry 13 }

cgsProxPeakSendRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "rate per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the peak transmitted DRP request
        rate per second." 
    ::= { cgsProxZoneEntry 14 }

cgsProxPeakRcvdRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "rate per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the peak received DRP response
        rate per second." 
    ::= { cgsProxZoneEntry 15 }

cgsProxStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the storage type for this
        conceptual row."
    DEFVAL          { nonVolatile } 
    ::= { cgsProxZoneEntry 16 }

cgsProxRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to create/delete an entry in the
        cgsProxZoneTable." 
    ::= { cgsProxZoneEntry 17 }
 


cgsRegionTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CgsRegionEntry 
    MAX-ACCESS      not-accessible
    STATUS          deprecated
    DESCRIPTION
        "This table is used to configure regions on the device.
        It consists a list of regions configured on the GSLB
        device."
    ::= { cgsResources 1 }

cgsRegionEntry OBJECT-TYPE
    SYNTAX          CgsRegionEntry
    MAX-ACCESS      not-accessible
    STATUS          deprecated
    DESCRIPTION
        "An entry in cgsRegionTable.  Each entry contains the
        information about a region.  Entries can be
        added/deleted/modified by administrator action."
    INDEX           { cgsRegionName } 
    ::= { cgsRegionTable 1 }

CgsRegionEntry ::= SEQUENCE {
        cgsRegionName        SnmpAdminString,
        cgsRegionComments    SnmpAdminString,
        cgsRegionStorageType StorageType,
        cgsRegionRowStatus   RowStatus
}

cgsRegionName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..80))
    MAX-ACCESS      not-accessible
    STATUS          deprecated
    DESCRIPTION
        "This object specifies the name given uniquely for a
        region." 
    ::= { cgsRegionEntry 1 }

cgsRegionComments OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "This object specifies the comments associated with the
        region."
    DEFVAL          { "" } 
    ::= { cgsRegionEntry 2 }

cgsRegionStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "This object specifies the storage type for this
        conceptual row."
    DEFVAL          { nonVolatile } 
    ::= { cgsRegionEntry 3 }

cgsRegionRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "This object is used to create/delete an entry in the
        cgsRegionTable" 
    ::= { cgsRegionEntry 4 }
 


cgsLocationTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CgsLocationEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table is used to configure locations on the device.
        It consists a list of locations configured on the GSLB
        device."
    ::= { cgsResources 2 }

cgsLocationEntry OBJECT-TYPE
    SYNTAX          CgsLocationEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cgsLocationTable.  Each entry contains the
        information about a location.  Entries can be
        added/deleted/modified by administrator action."
    INDEX           { cgsLocationName } 
    ::= { cgsLocationTable 1 }

CgsLocationEntry ::= SEQUENCE {
        cgsLocationName        SnmpAdminString,
        cgsLocationRegion      SnmpAdminString,
        cgsLocationZone        SnmpAdminString,
        cgsLocationComments    SnmpAdminString,
        cgsLocationStorageType StorageType,
        cgsLocationRowStatus   RowStatus
}

cgsLocationName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..80))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the name given uniquely for a
        location." 
    ::= { cgsLocationEntry 1 }

cgsLocationRegion OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies a region to which this location
        instance is associated.
        This object is mandatory for a row creation." 
    ::= { cgsLocationEntry 2 }

cgsLocationZone OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies a zone to which this location
        instance is associated."
    DEFVAL          { "" } 
    ::= { cgsLocationEntry 3 }

cgsLocationComments OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the comments associated with the
        location."
    DEFVAL          { "" } 
    ::= { cgsLocationEntry 4 }

cgsLocationStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the storage type for this
        conceptual row"
    DEFVAL          { nonVolatile } 
    ::= { cgsLocationEntry 5 }

cgsLocationRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to create/delete an entry in the
        cgsLocationTable" 
    ::= { cgsLocationEntry 6 }
 


cgsRegionIdTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CgsRegionIdEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table is used to configure regions on the device.
        It consists a list of regions configured on the GSLB
        device."
    ::= { cgsResources 3 }

cgsRegionIdEntry OBJECT-TYPE
    SYNTAX          CgsRegionIdEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cgsRegionIdTable.Each entry contains the
        information about a region.  Entries can be
        added/deleted/modified by administrator action."
    INDEX           { cgsRegionId } 
    ::= { cgsRegionIdTable 1 }

CgsRegionIdEntry ::= SEQUENCE {
        cgsRegionId                          Unsigned32,
        cgsRegionIdName                      SnmpAdminString,
        cgsRegionIdComments                  SnmpAdminString,
        cgsReqCountPerRegionId               Counter32,
        cgsReqCountRatePerRegionId1Min       Gauge32,
        cgsReqCountRatePerRegionId5Min       Gauge32,
        cgsReqCountRatePerRegionId30Min      Gauge32,
        cgsReqCountRatePerRegionId4Hr        Gauge32,
        cgsAnswerCountPerRegionId            Counter32,
        cgsAnswerCountRatePerRegionId1Min    Gauge32,
        cgsAnswerCountRatePerRegionId5Min    Gauge32,
        cgsAnswerCountRatePerRegionId30Min   Gauge32,
        cgsAnswerCountRatePerRegionId4Hr     Gauge32,
        cgsUnAnswerCountPerRegionId          Counter32,
        cgsUnAnswerCountRatePerRegionId1Min  Gauge32,
        cgsUnAnswerCountRatePerRegionId5Min  Gauge32,
        cgsUnAnswerCountRatePerRegionId30Min Gauge32,
        cgsUnAnswerCountRatePerRegionId4Hr   Gauge32,
        cgsRegionIdStorageType               StorageType,
        cgsRegionIdRowStatus                 RowStatus
}

cgsRegionId OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4294967295)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies a region." 
    ::= { cgsRegionIdEntry 1 }

cgsRegionIdName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..80))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the name given uniquely for a
        region." 
    ::= { cgsRegionIdEntry 2 }

cgsRegionIdComments OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the comments associated with the
        region."
    DEFVAL          { "" } 
    ::= { cgsRegionIdEntry 3 }

cgsReqCountPerRegionId OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "number of hits"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of DNS requests
        received from this region since the GSLB device was last
        started." 
    ::= { cgsRegionIdEntry 4 }

cgsReqCountRatePerRegionId1Min OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "hits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the average per second DNS requests
        received from this region, calculated during the last one 
        minute interval." 
    ::= { cgsRegionIdEntry 5 }

cgsReqCountRatePerRegionId5Min OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "hits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the average per second DNS requests
        received from this region , calculated during the last 5 
        minute interval." 
    ::= { cgsRegionIdEntry 6 }

cgsReqCountRatePerRegionId30Min OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "hits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the average per second DNS requests
        received from this region , calculated during the last 30
        minute interval." 
    ::= { cgsRegionIdEntry 7 }

cgsReqCountRatePerRegionId4Hr OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "hits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the average per second DNS requests
        received from this region , calculated during the last 4
        hour interval." 
    ::= { cgsRegionIdEntry 8 }

cgsAnswerCountPerRegionId OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "number of hits"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of times answers in
        this region are used in replying for DNS queries, since the 
        GSLB device was last started." 
    ::= { cgsRegionIdEntry 9 }

cgsAnswerCountRatePerRegionId1Min OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "hits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the average per second hit count for
        answers in this region, calculated during the last 1 minute
        interval." 
    ::= { cgsRegionIdEntry 10 }

cgsAnswerCountRatePerRegionId5Min OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "hits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the average per second hit count for
        answers in this region, calculated during the last 5 minute
        interval." 
    ::= { cgsRegionIdEntry 11 }

cgsAnswerCountRatePerRegionId30Min OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "hits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the average per second hit count for
        answers in this region, calculated during the last 30 minute
        interval." 
    ::= { cgsRegionIdEntry 12 }

cgsAnswerCountRatePerRegionId4Hr OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "hits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the average per second hit count for
        answers in this region, calculated during the last 4 hour
        interval." 
    ::= { cgsRegionIdEntry 13 }

cgsUnAnswerCountPerRegionId OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "number of hits"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of times DNS requests
        from this region have not been answered, since the GSLB device
        was last started." 
    ::= { cgsRegionIdEntry 14 }

cgsUnAnswerCountRatePerRegionId1Min OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "hits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the average per second unanswered
        DNS requests from this region, calculated during the last
        one minute." 
    ::= { cgsRegionIdEntry 15 }

cgsUnAnswerCountRatePerRegionId5Min OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "hits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the average per second unanswered
        DNS requests from this region, calculated during the
        last 5 minute interval." 
    ::= { cgsRegionIdEntry 16 }

cgsUnAnswerCountRatePerRegionId30Min OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "hits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the average per second unanswered
        DNS requests from this region, calculated during the 
        last 30 minute interval." 
    ::= { cgsRegionIdEntry 17 }

cgsUnAnswerCountRatePerRegionId4Hr OBJECT-TYPE
    SYNTAX          Gauge32
    UNITS           "hits per second"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the average per second unanswered
        DNS requests from this region, calculated during the 
        last 4 hour interval." 
    ::= { cgsRegionIdEntry 18 }

cgsRegionIdStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the storage type for this
        conceptual row."
    DEFVAL          { nonVolatile } 
    ::= { cgsRegionIdEntry 19 }

cgsRegionIdRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to create/delete an entry in the
        cgsRegionIdTable. Users can modify all writable objects
        in this row when this object value is 'active'. The 
        cgsRegionIdName object need to be set to valid value
        by the users before user can activate the row." 
    ::= { cgsRegionIdEntry 20 }
 


-- Notification Control Group

cgsPeerEventNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object defines the administrative state of sending
        notifications to signal a GSLB peer status change."
    DEFVAL          { false } 
    ::= { cgsNotifControl 1 }

-- Objects for Notification

cgsPeerPrevStatus OBJECT-TYPE
    SYNTAX          CiscoGslbPeerStatus
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object is used for sending the value of cgsPeerStatus
        before transitioning to new state." 
    ::= { cgsNotifObjects 1 }

-- Notifications

ciscoGslbSystemPeerEventStatus NOTIFICATION-TYPE
    OBJECTS         {
                        sysName,
                        cgsPeerDnsName,
                        cgsPeerService,
                        cgsPeerPrevStatus,
                        cgsPeerStatus
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent when the value of
        cgsPeerStatus changes from one state to another.
        This notification is reported only by a GSLB device
        with cgsNodeService value of 'primary'."
   ::= { ciscoGslbSystemMIBNotifs 1 }
-- Conformance

ciscoGslbSystemMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoGslbSystemMIBConform 1 }

ciscoGslbSystemMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoGslbSystemMIBConform 2 }


-- Compliance

ciscoGslbSystemMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "Compliance statement for entities which implement
        the Cisco GSLB System MIB"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoGslbSystemGeneralGroup,
                        ciscoGslbSystemPeerGroup,
                        ciscoGslbSystemProxZoneGroup,
                        ciscoGslbSystemResourceGroup,
                        ciscoGslbSystemNotifControlGroup,
                        ciscoGslbSystemNotifObjectsGroup,
                        ciscoGslbSystemNotifGroup
                    }
    ::= { ciscoGslbSystemMIBCompliances 1 }

ciscoGslbSystemMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "Compliance statement for entities which implement
        the Cisco GSLB System MIB"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoGslbSystemGeneralGroup,
                        ciscoGslbSystemPeerGroup,
                        ciscoGslbSystemProxZoneGroup,
                        ciscoGslbSystemNotifControlGroup,
                        ciscoGslbSystemNotifObjectsGroup,
                        ciscoGslbSystemNotifGroup,
                        ciscoGslbSystemResourceLocationGroup,
                        ciscoGslbSystemResourceRegionGroup
                    }
    ::= { ciscoGslbSystemMIBCompliances 2 }

-- Units of Conformance

ciscoGslbSystemGeneralGroup OBJECT-GROUP
    OBJECTS         {
                        cgsNodeService,
                        cgsNodeCommIfName,
                        cgsNodeCommIfIndex,
                        cgsNodeStatus,
                        cgsNodeLocation,
                        cgsNodeRegion
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing general GSLB status."
    ::= { ciscoGslbSystemMIBGroups 1 }

ciscoGslbSystemPeerGroup OBJECT-GROUP
    OBJECTS         {
                        cgsPeerLocation,
                        cgsPeerDnsName,
                        cgsPeerService,
                        cgsPeerStatus,
                        cgsPeerVersion
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing GSLB peer status."
    ::= { ciscoGslbSystemMIBGroups 2 }

ciscoGslbSystemProxZoneGroup OBJECT-GROUP
    OBJECTS         {
                        cgsProxPrimaryAddressType,
                        cgsProxPrimaryAddress,
                        cgsProxSecondaryAddressType,
                        cgsProxSecondaryAddress,
                        cgsProxEchoSentReqs,
                        cgsProxEchoRcvdResps,
                        cgsProxSentMeasureReqs,
                        cgsProxRcvdMeasureResps,
                        cgsProxTotalSentReqs,
                        cgsProxTotalRcvdResps,
                        cgsProxSendRate,
                        cgsProxRcvdRate,
                        cgsProxPeakSendRate,
                        cgsProxPeakRcvdRate,
                        cgsProxStorageType,
                        cgsProxRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing GSLB proximity
        zone statistics."
    ::= { ciscoGslbSystemMIBGroups 3 }

ciscoGslbSystemResourceGroup OBJECT-GROUP
    OBJECTS         {
                        cgsRegionComments,
                        cgsRegionStorageType,
                        cgsRegionRowStatus,
                        cgsLocationRegion,
                        cgsLocationZone,
                        cgsLocationComments,
                        cgsLocationStorageType,
                        cgsLocationRowStatus
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects providing GSLB resource
        configurations."
    ::= { ciscoGslbSystemMIBGroups 4 }

ciscoGslbSystemNotifControlGroup OBJECT-GROUP
    OBJECTS         { cgsPeerEventNotifEnable }
    STATUS          current
    DESCRIPTION
        "This group of objects controls the sending of
        notifications defined in this MIB module."
    ::= { ciscoGslbSystemMIBGroups 5 }

ciscoGslbSystemNotifObjectsGroup OBJECT-GROUP
    OBJECTS         { cgsPeerPrevStatus }
    STATUS          current
    DESCRIPTION
        "A collection of objects that convey information for
        notifications defined in this MIB module."
    ::= { ciscoGslbSystemMIBGroups 6 }

ciscoGslbSystemNotifGroup NOTIFICATION-GROUP
   NOTIFICATIONS    { ciscoGslbSystemPeerEventStatus }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing GSLB System events."
    ::= { ciscoGslbSystemMIBGroups 7 }

ciscoGslbSystemResourceLocationGroup OBJECT-GROUP
    OBJECTS         {
                        cgsLocationRegion,
                        cgsLocationZone,
                        cgsLocationComments,
                        cgsLocationStorageType,
                        cgsLocationRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing GSLB location resource
        configurations."
    ::= { ciscoGslbSystemMIBGroups 8 }

ciscoGslbSystemResourceRegionGroup OBJECT-GROUP
    OBJECTS         {
                        cgsRegionIdName,
                        cgsRegionIdComments,
                        cgsReqCountPerRegionId,
                        cgsReqCountRatePerRegionId1Min,
                        cgsReqCountRatePerRegionId5Min,
                        cgsReqCountRatePerRegionId30Min,
                        cgsReqCountRatePerRegionId4Hr,
                        cgsAnswerCountPerRegionId,
                        cgsAnswerCountRatePerRegionId1Min,
                        cgsAnswerCountRatePerRegionId5Min,
                        cgsAnswerCountRatePerRegionId30Min,
                        cgsAnswerCountRatePerRegionId4Hr,
                        cgsUnAnswerCountPerRegionId,
                        cgsUnAnswerCountRatePerRegionId1Min,
                        cgsUnAnswerCountRatePerRegionId5Min,
                        cgsUnAnswerCountRatePerRegionId30Min,
                        cgsUnAnswerCountRatePerRegionId4Hr,
                        cgsRegionIdStorageType,
                        cgsRegionIdRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing GSLB region resource
        configurations."
    ::= { ciscoGslbSystemMIBGroups 9 }

END














