-- *****************************************************************
-- CISCO-VIDEO-SESSION-CAPABILITY.my
--   
-- Copyright (c) 2010-2011 by cisco Systems Inc.
-- All rights reserved.
--   
-- *****************************************************************

CISCO-VIDEO-SESSION-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoVideoSessionCapability MODULE-IDENTITY
    LAST-UPDATED    "201105240000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-video@cisco.com"
    DESCRIPTION
        "Agent capabilities for CISCO-VIDEO-SESSION-MIB."
    REVISION        "201105240000Z"
    DESCRIPTION
        "Added ciscoVideoSessionCapabilityV152T02."
    REVISION        "201011110000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 599 }



ciscoVideoSessionCapabilityV15R01 AGENT-CAPABILITIES
    PRODUCT-RELEASE "OS=IOS
                     OSVERSION=15.1
                     PLATFORM=c29xx,c3925,c3945,c3925E,c3945E
                     INTERFACE=None"
    STATUS          current
    DESCRIPTION
        "Cisco Video Session MIB capabilities."

    SUPPORTS        CISCO-VIDEO-SESSION-MIB
    INCLUDES        {
                        cVideoSessionHistoryGroup,
                        cVideoSessionActiveGroup
                    }
    ::= { ciscoVideoSessionCapability 1 }

ciscoVideoSessionCapabilityV152T02 AGENT-CAPABILITIES
    PRODUCT-RELEASE "OS=IOS
                     OSVERSION=15.2(2)T
                     PLATFORM=c29xx,c3925,c3945,c3925E,c3945E
                     INTERFACE=None"
    STATUS          current
    DESCRIPTION
        "Cisco Video Session MIB capabilities.
        Some objects are not implemented due to DSP statistics reporting
        capabilities."

    SUPPORTS        CISCO-VIDEO-SESSION-MIB
    INCLUDES        {
                        cVideoSessionCommonStatusGroup,
                        cVideoSessionCommonStatisticsGroup,
                        cVideoSessionCallStatisticsGroup,
                        cVideoSessionConfereeStatisticsGroup
                    }
    VARIATION       cVideoCommonStatsHistoryTxMaxJitter
    DESCRIPTION
        "This object is only supported for video conference call."

    VARIATION       cVideoCommonStatsHistoryTxMaxDelay
    DESCRIPTION
        "This object is only supported for video conference call."

    VARIATION       cVideoCommonStatsHistoryTxPercentLostPackets
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not implemented."

    VARIATION       cVideoCommonStatsHistoryTxAvgJitter
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not implemented."

    VARIATION       cVideoCommonStatsHistoryTxAvgDelay
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not implemented."

    VARIATION       cVideoCommonStatsHistoryRxTotalLostPackets
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not implemented."

    VARIATION       cVideoCommonStatsHistoryRxPercentLostPackets
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not implemented."

    VARIATION       cVideoCommonStatsActiveTxActualBitrate
    DESCRIPTION
        "This object is only supported for video conference call."

    VARIATION       cVideoCommonStatsActiveTxCurrentLostPackets
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not implemented."

    VARIATION       cVideoCommonStatsActiveTxCurrentOutOfOrderPackets
    DESCRIPTION
        "This object is only supported for video conference call."

    VARIATION       cVideoCommonStatsActiveTxMaxJitter
    DESCRIPTION
        "This object is only supported for video conference call."

    VARIATION       cVideoCommonStatsActiveTxCurrentJitter
    DESCRIPTION
        "This object is only supported for video conference call."

    VARIATION       cVideoCommonStatsActiveTxMaxDelay
    DESCRIPTION
        "This object is only supported for video conference call."

    VARIATION       cVideoCommonStatsActiveTxCurrentDelay
    DESCRIPTION
        "This object is only supported for video conference call."

    VARIATION       cVideoCommonStatsActiveTxPercentLostPackets
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not implemented."

    VARIATION       cVideoCommonStatsActiveTxAvgJitter
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not implemented."

    VARIATION       cVideoCommonStatsActiveTxAvgDelay
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not implemented."

    VARIATION       cVideoCommonStatsActiveRxCurrentLostPackets
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not implemented."

    VARIATION       cVideoCommonStatsActiveRxActualBitrate
    DESCRIPTION
        "This object is only supported for point-to-point video
        transcoding call."

    VARIATION       cVideoCommonStatsActiveRxTotalLostPackets
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not implemented."

    VARIATION       cVideoCommonStatsActiveRxPercentLostPackets
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not implemented."

    ::= { ciscoVideoSessionCapability 2 }

END

















