-- *****************************************************************
-- IPV6-FLOW-LABEL-MIB.my:  Textual Conventions for IPv6 Flow Labels
--
-- July 2006, Vishnu Kant Varma
--
-- Copyright (c) 2006-2008 by cisco Systems, Inc.
-- All rights reserved.
--
-- *****************************************************************

IPV6-FLOW-LABEL-MIB DEFINITIONS ::= BEGIN 
 
   IMPORTS 
 
       MODULE-IDENTITY, mib-2, Integer32           FROM SNMPv2-SMI 
       TEXTUAL-CONVENTION                          FROM SNMPv2-TC; 
 
   ipv6FlowLabelMIB   MODULE-IDENTITY 
 
       LAST-UPDATED  "200308280000Z"  -- 28 August 2003 
       ORGANIZATION  "IETF Operations and Management Area" 
       CONTACT-INFO  "Bert Wijnen (Editor) 
                      Lucent Technologies 
                      Schagen 33 
                      3461 GL Linschoten 
                      Netherlands 
                      Phone: +31 348-407-775 
                      EMail: bwijnen@lucent.com 
 
                      Send comments to <mibs@ops.ietf.org>. 
                     " 
       DESCRIPTION   "This MIB module provides commonly used textual 
                      conventions for IPv6 Flow Labels. 
 
                      Copyright (C) The Internet Society (2003).  This 
                      version of this MIB module is part of RFC 3595, 
                      see the RFC itself for full legal notices. 
                     " 
       -- Revision History 
 
       REVISION      "200308280000Z"  -- 28 August 2003 
       DESCRIPTION   "Initial version, published as RFC 3595." 
 
       ::= { mib-2 103 } 
 
   IPv6FlowLabel      ::= TEXTUAL-CONVENTION 
       DISPLAY-HINT  "d" 
       STATUS         current 
       DESCRIPTION   "The flow identifier or Flow Label in an IPv6 
                      packet header that may be used to discriminate 
                      traffic flows. 
                     " 
       REFERENCE     "Internet Protocol, Version 6 (IPv6) specification, 
                      section 6.  RFC 2460. 
                     " 
       SYNTAX         Integer32 (0..1048575) 
 
   IPv6FlowLabelOrAny ::= TEXTUAL-CONVENTION 
       DISPLAY-HINT  "d" 
       STATUS         current 
       DESCRIPTION   "The flow identifier or Flow Label in an IPv6 
                      packet header that may be used to discriminate 
                      traffic flows.  The value of -1 is used to 
                      indicate a wildcard, i.e. any value. 
                     " 
       SYNTAX         Integer32 (-1 | 0..1048575) 
 
   END 
 
