-- *****************************************************************
-- CISCO-IF-EXTENSION-CAPABILITY.my:
-- Cisco CISCO-IF-EXTENSION-MIB AGENT-CAPABILITIES
--   
-- Jan 2004, Liwei Lue
--   
-- Copyright (c) 2004-2015 by Cisco Systems Inc.
-- All rights reserved.
-- ****************************************************************

CISCO-IF-EXTENSION-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    Integer32,
    Unsigned32
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoIfExtensionCapability MODULE-IDENTITY
    LAST-UPDATED    "201506030000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "The capabilities description of
        CISCO-IF-EXTENSION-MIB."
    REVISION        "201506030000Z"
    DESCRIPTION
        "Added ciscoIfExtensionTableIntfGroup3SupR02 and
        VARIATIONs for cieIfTransceiverFrequencyConfig,
        cieIfFillPatternConfig, cieIfIgnoreBitErrorsConfig and
        cieIfIgnoreInterruptThresholdConfig
        in capability statement ciscoIfExtCapNxOSV06R0201PMDS9000
        and ciscoIfExtCapNxOSV06R0202PN7K."
    REVISION        "201309050000Z"
    DESCRIPTION
        "Added agent capability statement
        ciscoIfExtCapNxOSV06R0201PMDS9000 and 
        ciscoIfExtCapNxOSV06R0202PN7K."
    REVISION        "201203010000Z"
    DESCRIPTION
        "Added ciscoIfExtCapV15R0002SGPCat4K agent
        capability statement."
    REVISION        "201103210000Z"
    DESCRIPTION
        "Added ciscoIfExtCapNXOSV52R1MDS9000 agent
        capability statement."
    REVISION        "200803240000Z"
    DESCRIPTION
        "Added ciscoIfExtCapCatOSV08R0701PCat6K agent
        capability statement."
    REVISION        "200711050000Z"
    DESCRIPTION
        "Added ciscoIfExtCapc4710aceVA1R700
        agent capabilities for ACE 4710 Application 
        Control Engine Appliance."
    REVISION        "200708300000Z"
    DESCRIPTION
        "Added ciscoIfExtCapV12R0233SXHPCat6K
        capability statement."
    REVISION        "200704190000Z"
    DESCRIPTION
        "Added ciscoIfExtCapV12R0229SM1 and
        ciscoIfExtCapV12R0412MR1 capability statements."
    REVISION        "200602210000Z"
    DESCRIPTION
        "Added capability statement
        ciscoIfExtCapabilityACSWV03R000 for 
        Application Control Engine (ACE)."
    REVISION        "200504140000Z"
    DESCRIPTION
        "Added capability statement
        ciscoIfExtCapSanOSV30R1MDS9000."
    REVISION        "200503040000Z"
    DESCRIPTION
        "Added capability statement
        ciscoIfExtCapV12R0217bSXAPCat6K."
    REVISION        "200401260000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 395 }



ciscoIfExtensionCapV08R0301 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.3(1) on Catalyst 6000/6500 and
                         Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-IF-EXTENSION-MIB capabilities."

    SUPPORTS        CISCO-IF-EXTENSION-MIB
    INCLUDES        {
                        ciscoIfExtDot1qEtherTypeGroup,
                        ciscoIfExtUtilizationGroup,
                        ciscoIfExtDot1dBaseMappingGroup
                    }
    ::= { ciscoIfExtensionCapability 1 }

ciscoIfExtCapV12R0217bSXAPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(17b)SXA on Catalyst 6000/6500
                        and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-IF-EXTENSION-MIB capabilities."

    SUPPORTS        CISCO-IF-EXTENSION-MIB
    INCLUDES        {
                        ciscoIfExtensionTablePacketGroup,
                        ciscoIfExtensionTableIntfGroup,
                        ciscoIfExtDot1qEtherTypeGroup,
                        ciscoIfExtDot1dBaseMappingGroup
                    }
    ::= { ciscoIfExtensionCapability 2 }

ciscoIfExtCapSanOSV30R1MDS9000 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco SanOS 3.0 on Cisco MDS 9000
                          series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-IF-EXTENSION-MIB capabilities."

    SUPPORTS        CISCO-IF-EXTENSION-MIB
    INCLUDES        {
                        ciscoIfExtensionTableIntfGroup2,
                        ciscoIfExtUtilizationGroup,
                        ciscoIfExtDot1dBaseMappingGroup,
                        ciscoIfExtIfNameMappingGroup,
                        cieIfStatusListGroup
                    }
    VARIATION       cieIfDhcpMode
    SYNTAX          INTEGER  {
                        false(2)
                    }
    ACCESS          read-only
    DESCRIPTION
        "Implementation supports only read-only access for
        this object. Support for true(1) is only required
        on interfaces which support DHCP."

    VARIATION       cieIfMtu
    ACCESS          read-only
    DESCRIPTION
        "Implementation support only read-only access for
        this object."

    ::= { ciscoIfExtensionCapability 3 }

ciscoIfExtCapabilityACSWV03R000 AGENT-CAPABILITIES
    PRODUCT-RELEASE "ACSW (Application Control Software) 3.0"
    STATUS          current
    DESCRIPTION
        "CISCO-IF-EXTENSION-MIB capabilities."

    SUPPORTS        CISCO-IF-EXTENSION-MIB
    INCLUDES        { ciscoIfExtIfNameMappingGroup }
    ::= { ciscoIfExtensionCapability 4 }

ciscoIfExtCapV12R0229SM1 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(29)SM1"
    STATUS          current
    DESCRIPTION
        "IOS 12.2(29)SM1 Cisco CISCO-IF-EXTENSION-MIB User Agent MIB
        capabilities."

    SUPPORTS        CISCO-IF-EXTENSION-MIB
    INCLUDES        {
                        ciscoIfExtensionTablePacketGroup,
                        ciscoIfExtensionTableIntfGroup
                    }
    VARIATION       cieIfMtu
    SYNTAX          Integer32 (40..2147483647)
    WRITE-SYNTAX    Integer32 (40..2147483647)
    ACCESS          read-only
    DESCRIPTION
        "Image only support for cieIfMtu not other objects in
        ciscoIfExtensionTableIntfGroup1."

    ::= { ciscoIfExtensionCapability 5 }

ciscoIfExtCapV12R0412MR1 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.4(2)MR1"
    STATUS          current
    DESCRIPTION
        "IOS 12.4(2)MR1 Cisco CISCO-IF-EXTENSION-MIB User Agent MIB
        capabilities."

    SUPPORTS        CISCO-IF-EXTENSION-MIB
    INCLUDES        {
                        ciscoIfExtensionTablePacketGroup,
                        ciscoIfExtensionTableIntfGroup,
                        ciscoIfExtensionAsymmetricalSpeedGroup
                    }
    ::= { ciscoIfExtensionCapability 6 }

ciscoIfExtCapV12R0233SXHPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(33)SXH on Catalyst 6000/6500
                    and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-IF-EXTENSION-MIB agent capabilities."

    SUPPORTS        CISCO-IF-EXTENSION-MIB
    INCLUDES        {
                        ciscoIfExtensionTablePacketGroup,
                        ciscoIfExtensionTableIntfGroup,
                        ciscoIfExtDot1qEtherTypeGroup,
                        ciscoIfExtDot1dBaseMappingGroup,
                        ciscoIfExtUtilizationGroup,
                        ciscoIfExtIfNameMappingGroup
                    }
    ::= { ciscoIfExtensionCapability 7 }

ciscoIfExtCapc4710aceVA1R700 AGENT-CAPABILITIES
    PRODUCT-RELEASE "ACSW (Application Control Software) A1(7)
                     for ACE 4710 Application Control Engine 
                     Appliance"
    STATUS          current
    DESCRIPTION
        "CISCO-IF-EXTENSION-MIB capabilities."

    SUPPORTS        CISCO-IF-EXTENSION-MIB
    INCLUDES        { ciscoIfExtIfNameMappingGroup }
    ::= { ciscoIfExtensionCapability 8 }

ciscoIfExtCapCatOSV08R0701PCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.7(1) on Catalyst 6000/6500 and
                     Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-IF-EXTENSION-MIB capabilities."

    SUPPORTS        CISCO-IF-EXTENSION-MIB
    INCLUDES        {
                        ciscoIfExtDot1qEtherTypeGroup,
                        ciscoIfExtUtilizationGroup,
                        ciscoIfExtDot1dBaseMappingGroup,
                        ciscoIfExtUtilIntervalGroup
                    }
    VARIATION       cieIfInterval
    SYNTAX          Unsigned32 (30 | 300)
    DESCRIPTION
        "Only limited set of values are supported.
        Changes on the value of one instance of this
        object will be applied to all the instance values
        of this object."

    ::= { ciscoIfExtensionCapability 9 }

ciscoIfExtCapNXOSV52R1MDS9000 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco NXOS 5.2(1) on MDS 9000."
    STATUS          current
    DESCRIPTION
        "CISCO-IF-EXTENSION-MIB capabilities."

    SUPPORTS        CISCO-IF-EXTENSION-MIB
    INCLUDES        {
                        ciscoIfExtDot1qEtherTypeGroup,
                        ciscoIfExtUtilizationGroup,
                        ciscoIfExtDot1dBaseMappingGroup,
                        ciscoIfExtUtilIntervalGroup
                    }
    VARIATION       cieIfInterval
    ACCESS          read-only
    DESCRIPTION
        "Implementation support only read-only access for
        this object."

    ::= { ciscoIfExtensionCapability 10 }

ciscoIfExtCapV15R0002SGPCat4K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 15.0(2)SG on Catalyst 4000 family
                    switches."
    STATUS          current
    DESCRIPTION
        "CISCO-IF-EXTENSION-MIB agent capabilities."

    SUPPORTS        CISCO-IF-EXTENSION-MIB
    INCLUDES        {
                        ciscoIfExtensionTablePacketGroup,
                        ciscoIfExtensionTableIntfGroup,
                        ciscoIfExtDot1dBaseMappingGroup,
                        ciscoIfExtIfNameMappingGroup
                    }
    ::= { ciscoIfExtensionCapability 11 }

ciscoIfExtCapNxOSV06R0201PMDS9000 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco NX-OS 6.2(1) on MDS 9000 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-IF-EXTENSION-MIB agent capabilities."

    SUPPORTS        CISCO-IF-EXTENSION-MIB
    INCLUDES        {
                        ciscoIfExtensionTablePacketGroup,
                        ciscoIfExtensionTableIntfGroup,
                        ciscoIfExtUtilizationGroup,
                        ciscoIfExtIfNameMappingGroup,
                        cieIfStatusListGroup,
                        cieLinkUpDownNotifEnableGroup,
                        cieLinkUpDownNotifGroup,
                        cieDelayedLinkUpDownNotifNotifEnableGroup,
                        cieDelayedLinkUpDownNotifNotifGroup,
                        ciscoIfExtensionTableIntfGroup3,
                        cieIfStatusListGroupSup1,
                        cieIfVlStatsGroup,
                        ciscoIfExtensionTableIntfGroup3SupR01,
                        cieLinkUpDownNotifConfigGroup,
                        ciscoIfExtensionTableIntfGroup3SupR02
                    }
    VARIATION       cieIfKeepAliveEnabled
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       cieIfDhcpMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cieIfOwner
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       cieIfTransceiverFrequencyConfig
    DESCRIPTION
        "Write access is only supported for Fiber Channel interfaces."

    VARIATION       cieIfFillPatternConfig
    DESCRIPTION
        "Write access is only supported for Fiber Channel interfaces."

    VARIATION       cieIfIgnoreBitErrorsConfig
    DESCRIPTION
        "Write access is only supported for Fiber Channel interfaces."

    VARIATION       cieIfIgnoreInterruptThresholdConfig
    DESCRIPTION
        "Write access is only supported for Fiber Channel interfaces."

    ::= { ciscoIfExtensionCapability 12 }

ciscoIfExtCapNxOSV06R0202PN7K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco NX-OS 6.2(2) on Nexus 7000 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-IF-EXTENSION-MIB agent capabilities."

    SUPPORTS        CISCO-IF-EXTENSION-MIB
    INCLUDES        {
                        ciscoIfExtensionTablePacketGroup,
                        ciscoIfExtensionTableIntfGroup,
                        ciscoIfExtIfNameMappingGroup,
                        ciscoIfExtDot1dBaseMappingGroup,
                        cieIfStatusListGroup,
                        cieLinkUpDownNotifEnableGroup,
                        cieLinkUpDownNotifGroup,
                        cieDelayedLinkUpDownNotifNotifEnableGroup,
                        cieDelayedLinkUpDownNotifNotifGroup,
                        ciscoIfExtensionTableIntfGroup3,
                        cieIfStatusListGroupSup1,
                        cieIfVlStatsGroup,
                        ciscoIfExtensionTableIntfGroup3SupR01,
                        cieLinkUpDownNotifConfigGroup,
                        ciscoIfExtensionTableIntfGroup3SupR02
                    }
    VARIATION       cieIfKeepAliveEnabled
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       cieIfDhcpMode
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cieIfOwner
    ACCESS          not-implemented
    DESCRIPTION
        "This object is not supported."

    VARIATION       cieIfTransceiverFrequencyConfig
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cieIfFillPatternConfig
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cieIfIgnoreBitErrorsConfig
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    VARIATION       cieIfIgnoreInterruptThresholdConfig
    ACCESS          read-only
    DESCRIPTION
        "Write access is not supported."

    ::= { ciscoIfExtensionCapability 13 }

END




