-- *****************************************************************
-- CISCO-PAGP-CAPABILITY.my:
-- Cisco CISCO-PAGP-MIB AGENT-CAPABILITIES
--   
-- March 2004, Liwei Lue
--   
-- Copyright (c) 2004, 2010, 2011 by Cisco Systems Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-PAGP-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    Unsigned32
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoPagpCapability MODULE-IDENTITY
    LAST-UPDATED    "201109270000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-lan-switch-snmp@cisco.com
            cs-etherchan@cisco.com"
    DESCRIPTION
        "The capabilities description of CISCO-PAGP-MIB."
    REVISION        "201109270000Z"
    DESCRIPTION
        "Add ciscoPagpCapV15R0001SYPCat6k agent capability
         statement.

         Added VARIATION for pagpDistributionProtocol object
         in ciscoPagpCapCatOSV08R0101 agent capabilty statement."
    REVISION        "201011170000Z"
    DESCRIPTION
        "Added capability statement
        ciscoPagpCapV12R0250SYPCat6K."
    REVISION        "201005060000Z"
    DESCRIPTION
        "Add ciscoPagpCapV12R0254SGPCat4K agent capability
        statement.

        Add VARIATION for pagpDistributionProtocol object
        in ciscoPagpCapV12R0217aSXCat6k agent capability
        statement."
    REVISION        "200403300000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 391 }



ciscoPagpCapV12R0111bEXCat6k AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.1(11b)EX on Catalyst 6000/6500
                         and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-PAGP-MIB capabilities."

    SUPPORTS        CISCO-PAGP-MIB
    INCLUDES        {
                        ciscoPagpEthcGroupV2R2,
                        ciscoPagpPagpGroupV1R1
                    }
    VARIATION       pagpDistributionProtocol
    SYNTAX          INTEGER  {
                        ip(1),
                        mac(2),
                        port(3)
                    }
    DESCRIPTION
        "Only a limited set of values is supported."

    ::= { ciscoPagpCapability 1 }

ciscoPagpCapV12R0217aSXCat6k AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(17a)SX on Catalyst 6000/6500
                         and Cisco 7600 series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-PAGP-MIB capabilities."

    SUPPORTS        CISCO-PAGP-MIB
    INCLUDES        {
                        ciscoPagpEthcGroupV2R2,
                        ciscoPagpPagpGroupV1R1
                    }
    VARIATION       pagpDistributionProtocol
    SYNTAX          INTEGER  {
                        ip(1),
                        mac(2),
                        port(3)
                    }
    DESCRIPTION
        "Only a limited set of values is supported."

    ::= { ciscoPagpCapability 2 }

ciscoPagpCapCatOSV08R0101 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco CatOS 8.1(1)."
    STATUS          current
    DESCRIPTION
        "CISCO-PAGP-MIB capabilities."

    SUPPORTS        CISCO-PAGP-MIB
    INCLUDES        {
                        ciscoPagpEthcGroupV2R2,
                        ciscoPagpPagpGroupV1R1
                    }
    VARIATION       pagpDistributionProtocol
    SYNTAX          INTEGER {
                        ip(1),
                        mac(2),
                        port(3),
                        vlanIpPort(4)
                    }
    DESCRIPTION
        "The enumerated values supported are all those
        defined at the time this clause was written."

    ::= { ciscoPagpCapability 3 }

ciscoPagpCapV12R0254SGPCat4K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(54)SG on Cat4K family switches."
    STATUS          current
    DESCRIPTION
        "CISCO-PAGP-MIB capabilities."

    SUPPORTS        CISCO-PAGP-MIB
    INCLUDES        {
                        ciscoPagpEthcGroupV2R2,
                        ciscoPagpPagpGroupV1R1,
                        ciscoPagpRateAndTimeOutGroup
                    }
    VARIATION       pagpDistributionProtocol
    SYNTAX          INTEGER  {
                        ip(1),
                        mac(2),
                        port(3)
                    }
    DESCRIPTION
        "Only a limited set of values is supported."

    VARIATION       pagpInPacketTimeout
    SYNTAX          Unsigned32 (45..90)
    DESCRIPTION
        "Only a limited set of values is supported."

    ::= { ciscoPagpCapability 4 }

ciscoPagpCapV12R0250SYPCat6K AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 12.2(50)SY on Catalyst 6000/6500
                    series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-PAGP-MIB capabilities."

    SUPPORTS        CISCO-PAGP-MIB
    INCLUDES        {
                        ciscoPagpEthcGroupV2R2,
                        ciscoPagpPagpGroupV1R1,
                        ciscoPagpRateAndTimeOutGroup
                    }
    VARIATION       pagpInPacketTimeout
    SYNTAX          Unsigned32 (45..90)
    DESCRIPTION
        "Only a limited set of values is supported."

    VARIATION       pagpDistributionProtocol
    SYNTAX          INTEGER  {
                        ip(1),
                        mac(2),
                        port(3)
                    }
    DESCRIPTION
        "Only a limited set of values is supported."

    ::= { ciscoPagpCapability 5 }

ciscoPagpCapV15R0001SYPCat6k AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco IOS 15.0(1)SY on Catalyst 6000/6500
                    series devices."
    STATUS          current
    DESCRIPTION
        "CISCO-PAGP-MIB capabilities."

    SUPPORTS        CISCO-PAGP-MIB
    INCLUDES        {
                        ciscoPagpEthcGroupV2R2,
                        ciscoPagpPagpGroupV1R1,
                        ciscoPagpRateAndTimeOutGroup
                    }

    VARIATION       pagpInPacketTimeout
    SYNTAX          Unsigned32 (45..90)
    DESCRIPTION
        "Only a limited set of values is supported."

    VARIATION       pagpDistributionProtocol
    SYNTAX          INTEGER  {
                        ip(1),
                        mac(2),
                        port(3),
                        vlanIpPort(4),
                        vlanIp(5),
                        pPort(6)
                    }
    DESCRIPTION
        "The enumerated values supported are all those
        defined at the time this clause was written."

    ::= { ciscoPagpCapability 6 }

END




