-- *-------------------------------------------------------------------------
-- * CISCO-AUTHORIZATION-STATS-MIB.my:  The CISCO Authorization Status MIB.
-- *
-- * Jan 2003, Brian D. Steven
-- *
-- * Copyright (c) 2003-2006 by Cisco Systems, Inc.
--   
-- * All rights reserved.
-- *
-- *------------------------------------------------------------------------

CISCO-AUTHORIZATION-STATS-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Counter32,
    Integer32,
    Gauge32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    TimeInterval
        FROM SNMPv2-TC
    InetAddressType,
    InetAddress
        FROM INET-ADDRESS-MIB
    CiscoPort
        FROM CISCO-TC
    ciscoMgmt
        FROM CISCO-SMI;


ciscoAuthorizationStatsMibModule MODULE-IDENTITY
    LAST-UPDATED    "200611080000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            170 W Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS
            E-mail: cs-cvpn3000@cisco.com"
    DESCRIPTION
        "The Cisco User Authorization Statistics MIB models
        counters and objects that are of management 
        interest.
        "
    REVISION        "200611080000Z"
    DESCRIPTION
        "The initial version of this MIB."
          ::= { ciscoMgmt 343 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- MIB Objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++
cStatsAuthorization  OBJECT IDENTIFIER
    ::= { ciscoAuthorizationStatsMibModule 1 }

cAuthorizationGlobal  OBJECT IDENTIFIER
    ::= { cStatsAuthorization 1 }


cAuthorizationStatsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CAuthorizationStatsEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The list of servers that may be queried for authorization
        attributes for connecting IPSec tunnel users."
    ::= { cStatsAuthorization 2 }

cAuthorizationStatsEntry OBJECT-TYPE
    SYNTAX          CAuthorizationStatsEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in the cAuthorizationStatsTable. These entries are
        created or destroyed whenever an authorization server 
        connection is added or removed via one of the management 
        interfaces to the tunnel server."
    INDEX           { cAuthorizServerIndex } 
    ::= { cAuthorizationStatsTable 1 }

CAuthorizationStatsEntry ::= SEQUENCE {
        cAuthorizServerIndex            Integer32,
        cAuthorizServerAddressType      InetAddressType,
        cAuthorizServerAddress          InetAddress,
        cAuthorizClientServerPortNum    CiscoPort,
        cAuthorizClientRoundTripTime    TimeInterval,
        cAuthorizClientAccessRequests   Counter32,
        cAuthorizClientAccessRetrans    Counter32,
        cAuthorizClientAccessAccepts    Counter32,
        cAuthorizClientAccessRejects    Counter32,
        cAuthorizClientAccessChallenges Counter32,
        cAuthorizClientMalAccessResps   Counter32,
        cAuthorizClientBadAuthenticates Counter32,
        cAuthorizClientPendingRequests  Gauge32,
        cAuthorizClientTimeouts         Counter32,
        cAuthorizClientUnknownTypes     Counter32,
        cAuthorizServerGroupId          Integer32
}

cAuthorizServerIndex OBJECT-TYPE
    SYNTAX          Integer32 (1..65535 )
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "The unique number used as the index for this row." 
    ::= { cAuthorizationStatsEntry 1 }

cAuthorizServerAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION     "The type of Internet address used by this entry." 
    ::= { cAuthorizationStatsEntry 2 }

cAuthorizServerAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP address of the authorization server whose
        statistics are being reported." 
    ::= { cAuthorizationStatsEntry 3 }

cAuthorizClientServerPortNum OBJECT-TYPE
    SYNTAX          CiscoPort
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The UDP The port on the server to which authorization
        requests are directed." 
    ::= { cAuthorizationStatsEntry 4 }

cAuthorizClientRoundTripTime OBJECT-TYPE
    SYNTAX          TimeInterval
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The time interval between the most recent
        Access-Reply/Access-Challenge and the Access-Request." 
    ::= { cAuthorizationStatsEntry 5 }

-- Request/Response statistics
-- Ignoring Unknown Types, then
-- AccessRequests + AccesssRetransmissions = AccessAccepts +
-- AccessRejects + AccessChallenges + PendingRequests + Timeouts
cAuthorizClientAccessRequests OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of  Access-Request packets sent to
        authorization server since client start-up. 
        This does not include retransmissions." 
    ::= { cAuthorizationStatsEntry 6 }

cAuthorizClientAccessRetrans OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of  Access-Request packets retransmitted
        to authorization server since client start-up." 
    ::= { cAuthorizationStatsEntry 7 }

cAuthorizClientAccessAccepts OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of  Access-Accept packets received by
        authorization server since client start-up." 
    ::= { cAuthorizationStatsEntry 8 }

cAuthorizClientAccessRejects OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of  Access-Reject packets received by
        authorization server since client start-up." 
    ::= { cAuthorizationStatsEntry 9 }

cAuthorizClientAccessChallenges OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of  Access-Challenge packets received by
        authorization server since client start-up." 
    ::= { cAuthorizationStatsEntry 10 }

-- "Access-Response" includes an Access-Accept, Access-Challenge
-- or Access-Reject
cAuthorizClientMalAccessResps OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of malformed Access-Response packets
        received by authoriztion server since client start-up. 
        Malformed packets include packets with an invalid length. 
        Bad authenticators or Signature attributes are not included 
        as malformed access responses." 
    ::= { cAuthorizationStatsEntry 11 }

cAuthorizClientBadAuthenticates OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of Access-Response packets containing
        invalid authenticators or Signature attributes received by 
        authorization server since client start-up." 
    ::= { cAuthorizationStatsEntry 12 }

cAuthorizClientPendingRequests OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of  Access-Request packets destined for
        authorization server that have not yet timed out or received 
        a response. This variable is incremented when an 
        Access-Request is sent and decremented due to receipt of an 
        Access-Reply or Access-Challenge, a timeout or 
        retransmission." 
    ::= { cAuthorizationStatsEntry 13 }

cAuthorizClientTimeouts OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of timeouts to authorization server since
        client startup. After a timeout the client may retry to the 
        same server, send to a different server, or give up. A retry 
        to the same server is counted as a retransmit as well as a 
        timeout. A send to a different server is counted as a Request 
        as well as a timeout." 
    ::= { cAuthorizationStatsEntry 14 }

cAuthorizClientUnknownTypes OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of unknown type packets received by
        authorization server since client start-up." 
    ::= { cAuthorizationStatsEntry 15 }

cAuthorizServerGroupId OBJECT-TYPE
    SYNTAX          Integer32 (0..65535 )
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The Id of user group associated with authorization
        server. The group ID is an integer value assigned by 
        the tunnel server. Group ID 0 is a special value used 
        to refer all gorups." 
    ::= { cAuthorizationStatsEntry 16 }
 

-- conformance information
cAuthorizationMIBConformance  OBJECT IDENTIFIER
    ::= { ciscoAuthorizationStatsMibModule 2 }

cAuthorizationMIBCompliances  OBJECT IDENTIFIER
    ::= { cAuthorizationMIBConformance 1 }

cAuthorizationGroup  OBJECT IDENTIFIER
    ::= { cAuthorizationMIBConformance 2 }


-- compliance statements
cAuthorizationMIBCompliance MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for authorization clients
        implementing the Authorization Client MIB."
    MODULE          -- this module
    MANDATORY-GROUPS { cAuthorizationClientMIBGroup }
    ::= { cAuthorizationMIBCompliances 1 }

cAuthorizationClientMIBGroup OBJECT-GROUP
    OBJECTS         {
                        cAuthorizServerAddressType,
                        cAuthorizServerAddress,
                        cAuthorizClientServerPortNum,
                        cAuthorizClientRoundTripTime,
                        cAuthorizClientAccessRequests,
                        cAuthorizClientAccessRetrans,
                        cAuthorizClientAccessAccepts,
                        cAuthorizClientAccessRejects,
                        cAuthorizClientAccessChallenges,
                        cAuthorizClientMalAccessResps,
                        cAuthorizClientBadAuthenticates,
                        cAuthorizClientPendingRequests,
                        cAuthorizClientTimeouts,
                        cAuthorizClientUnknownTypes,
                        cAuthorizServerGroupId
                    }
    STATUS          current
    DESCRIPTION
        "The basic collection of objects providing management of
        Authorization Clients."
    ::= { cAuthorizationGroup 1 }

END




