-- *****************************************************************
-- CISCO-RMON-CAPABILITY.my:
-- Cisco RMON-MIB AGENT-CAPABILITIES
--   
-- April 2004, Padma Pullela
--   
-- Copyright (c) 2004, 2006, 2008 by Cisco Systems Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-RMON-CAPABILITY DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    ciscoAgentCapability
        FROM CISCO-SMI;


ciscoRmonCapability MODULE-IDENTITY
    LAST-UPDATED    "200808040000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-lan-switch-snmp@cisco.com
            cs-rmon@cisco.com"
    DESCRIPTION
        "The capabilities description of
        RMON-MIB."
    REVISION        "200808040000Z"
    DESCRIPTION
        "Added capability statement ciscoRmonCapNXOSV04R0101PMDS9000."
    REVISION        "200603090000Z"
    DESCRIPTION
        "Add VARIATIONs for notifications
        fallingAlarm and risingAlarm in 
        ciscoRmonCapCatOSV08R0101."
    REVISION        "200404020000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoAgentCapability 357 }

ciscoRmonCapCatOSV08R0101  AGENT-CAPABILITIES
    PRODUCT-RELEASE     "Cisco CatOS 8.1(1)." 
    STATUS              current
    DESCRIPTION         "RMON-MIB capabilities."

    SUPPORTS            RMON-MIB
       INCLUDES         { rmonEtherStatsGroup,
                          rmonHistoryControlGroup,
                          rmonEthernetHistoryGroup,
                          rmonAlarmGroup,
                          rmonEventGroup,
                          rmonNotificationGroup
                        }

        VARIATION        fallingAlarm -- NOTIFICATION-TYPE
--          OBJECTS      { alarmIndex, alarmVariable, 
--                         alarmSampleType, alarmValue, 
--                         alarmFallingThreshold, ifName
--                       }
            DESCRIPTION
                    "In addition to the regular varbinds, the
                     instance values of ifName is appended 
                     to this notification."

        VARIATION        risingAlarm -- NOTIFICATION-TYPE
--          OBJECTS      { alarmIndex, alarmVariable, 
--                         alarmSampleType, alarmValue, 
--                         alarmRisingThreshold, ifName
--                       }
            DESCRIPTION
                    "In addition to the regular varbinds, the
                     instance values of ifName is appended
                     to this notification."

    ::= { ciscoRmonCapability 1 }


ciscoRmonCapNXOSV04R0101PMDS9000 AGENT-CAPABILITIES
    PRODUCT-RELEASE "Cisco NX-OS 4.1(1) on MDS9000 Storage Switches."
    STATUS          current
    DESCRIPTION
        "RMON-MIB capabilities."

    SUPPORTS        RMON-MIB
    INCLUDES        {
                        rmonAlarmGroup,
                        rmonEventGroup,
                        rmonNotificationGroup
                    }
    VARIATION       fallingAlarm -- NOTIFICATION-TYPE
--     OBJECTS      { alarmIndex, alarmVariable, 
--                    alarmSampleType, alarmValue, 
--                    alarmFallingThreshold, ifDescr
--                  }
    DESCRIPTION
        "In addition to the regular varbinds, the
        instance values of ifDescr is appended
        to this notification."

    VARIATION        risingAlarm -- NOTIFICATION-TYPE
--      OBJECTS      { alarmIndex, alarmVariable, 
--                     alarmSampleType, alarmValue, 
--                     alarmRisingThreshold, ifDescr
--                   }
    DESCRIPTION
        "In addition to the regular varbinds, the
        instance values of ifDescr is appended
        to this notification."

    ::= { ciscoRmonCapability 2 }

END





